{"text_format":"2","workbook":"xlsx","n_sheets":20,"sheets":["빅데이터분석DB 테이블스페이스관리","신호최적화 테이블스페이스관리","변경이력","DB사용자 계정","글로벌브릿지(스마트교차로)","동인(신호정보)","센터(시스템운영)","센터-네트워크가공","SUMO-현시,네트워크","SUMO-출력","SUMO-최적화","센터(집계,통계,화면표출용 등)","글로벌브릿지(백업용)","코드테이블 정의","센터(SUMO) 질의","데이터 구성참조 설문자료","테이블 보관주기동기화","물리타입 변환 안내","VOLT DB","테이블 인덱스 목록"],"not_rendered":{"charts":0,"images":4,"macros":0,"external_links":0,"defined_names":0,"comments":7,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"빅데이터분석DB 테이블스페이스관리","index":0,"n_rows":280,"n_cols":12,"rows_kept":280,"cut":false,"hidden":false,"merged":[[165,2,166,2],[167,2,168,2],[182,2,189,2],[199,2,218,2],[220,2,228,2],[230,2,234,2],[278,0,278,5],[279,0,303,5],[28,1,29,1],[31,2,32,2],[76,1,275,1],[139,2,143,2],[144,2,148,2],[149,2,150,2],[151,2,152,2],[236,2,275,2],[31,3,32,3],[153,2,154,2],[155,2,156,2],[157,2,158,2],[159,2,160,2],[63,3,69,3],[71,2,73,2],[71,3,73,3],[33,7,41,7],[31,7,32,7],[33,2,41,2],[33,3,41,3],[42,3,50,3],[42,7,50,7],[161,2,162,2],[163,2,164,2],[0,0,14,9],[16,0,16,2],[23,0,23,9],[24,0,24,9],[26,0,29,0],[26,1,27,1],[51,7,62,7],[63,7,69,7],[71,7,73,7],[30,1,75,1],[42,2,50,2],[51,2,62,2],[51,3,62,3],[63,2,69,2]]}
["TAC 설치 확인서 및 raw device 맵 송부드립니다. \n설치에 사용한 raw device 정보는 기재해 두었으며, 해당 자료 참고하시어 현재 사용 중인 raw device를 제외한 raw device를 통해 테이블스페이스 생성 작업 진행하시면 됩니다. \n\n* 설치 시 사용한 raw device /dev/raw/raw1~/dev/raw/raw28 \n\n* 테이블스페이스 추가 생성시 사용 가능한 raw device /dev/raw/raw29 부터 사용 가능 \n\n* 테이블스페이스 TBS_TEST 생성 예시 SQL> CREATE TABLESPACE TBS_TEST DATAFILE '/dev/raw/raw29' SIZE 30700M AUTOEXTEND OFF; \n\n업무에 참조바랍니다. 감사합니다. \n\n\n■사이트 기술지원 접수 및 요청 – Call Center 1544-8629 ( Tmax 기술서비스센터 ) \n■\"제품 매뉴얼/기술문서/데모라이센스신청\" 관련 검색 : http://technet.tmaxsoft.com"]
{"$rows_empty":15}
["테이블스페이스 "]
["전체",1600,"개"]
["티베로",50,"개","1~50",null,"DBMS 점유 영역"]
["예비",50,"개","51~100",null,"예비 영역"]
["신호최적화시스템",900,"개","101~1000",null,"DATA : 101~700 / INDEX : 701~1000"]
["교통정책시스템",600,"개","1001~1600"]
[]
["TAC TABLESPACE MAP"]
["* 참고 : 절대적인 값은 아니며 상황에 따라 조정 가능합니다. 할당 크기의 경우 고객사 환경에 맞도록 구성하시면 됩니다."]
["구분","영역","용도/사용자","테이블스페이스명","LV명","경로명","할당크기(MB)","합계(MB)","Node간 Share","Node간\n Concurrent접근"]
["File System","Tibero Engine\n / DBLog","Node1의\n Tibero Engine \n DBMS/Trace Log 등","-","-","/app/tibero7","-","-","N","N"]
[null,null,"Node2의\n Tibero Engine \n DBMS/Trace Log 등","-","-","/app/tibero7","-","-","N","N"]
[null,"Archive Log","Node1의 \n Archive File저장\n (업무에 따라 산정)","-","-","/logs/tbarch/biganlydb1","-","-","Y","N"]
[null,null,"Node2의\n Archive File저장\n (업무에 따라 산정)","-","-","/logs/tbarch/biganlydb2","-","-","Y","N"]
["Raw Device","System영역","Cluster","cfile",null,"/dev/raw/raw1\n/dev/raw/raw2",30700,30700,"Y","Y"]
[null,null,"Control File","Control File",null,"/dev/raw/raw3",30700,61400,"Y","Y"]
[{"$nulls":5},"/dev/raw/raw4",30700,null,"Y","Y"]
[null,null,"Node0의 Redo Log","Redo Log",null,"/dev/raw/raw5",30700,276300,"Y","Y"]
[{"$nulls":5},"/dev/raw/raw6",30700,null,"Y","Y"]
[{"$nulls":5},"/dev/raw/raw7",30700,null,"Y","Y"]
[{"$nulls":5},"/dev/raw/raw8",30700,null,"Y","Y"]
[{"$nulls":5},"/dev/raw/raw9",30700,null,"Y","Y"]
[{"$nulls":5},"/dev/raw/raw10",30700,null,"Y","Y"]
[{"$nulls":5},"/dev/raw/raw11",30700,null,"Y","Y"]
[{"$nulls":5},"/dev/raw/raw12",30700,null,"Y","Y"]
[{"$nulls":5},"/dev/raw/raw13",30700,null,"Y","Y"]
[null,null,"Node1의 Redo Log","Redo Log",null,"/dev/raw/raw14",30700,276300,"Y","Y"]
[{"$nulls":5},"/dev/raw/raw15",30700,null,"Y","Y"]
[{"$nulls":5},"/dev/raw/raw16",30700,null,"Y","Y"]
[{"$nulls":5},"/dev/raw/raw17",30700,null,"Y","Y"]
[{"$nulls":5},"/dev/raw/raw18",30700,null,"Y","Y"]
[{"$nulls":5},"/dev/raw/raw19",30700,null,"Y","Y"]
[{"$nulls":5},"/dev/raw/raw20",30700,null,"Y","Y"]
[{"$nulls":5},"/dev/raw/raw21",30700,null,"Y","Y"]
[{"$nulls":5},"/dev/raw/raw22",30700,null,"Y","Y"]
[null,null,"Node0의\n UNDO0 Tablespace\n (업무에 따라 산정)","UNDO0",null,"/dev/raw/raw23",30700,30700,"Y","Y"]
[{"$nulls":5},"/dev/raw/raw29",null,null,"Y","Y",null,{"$f":"\"ALTER TABLESPACE \"&$D$52&\" ADD DATAFILE '\" & F53 & \"' SIZE 30700M AUTOEXTEND OFF;\"","v":"ALTER TABLESPACE UNDO0 ADD DATAFILE '/dev/raw/raw29' SIZE 30700M AUTOEXTEND OFF;"}]
[{"$nulls":5},"/dev/raw/raw30",null,null,"Y","Y",null,"ALTER TABLESPACE UNDO0 ADD DATAFILE '/dev/raw/raw30' SIZE 30700M AUTOEXTEND OFF;"]
[{"$nulls":5},"/dev/raw/raw31",null,null,"Y","Y",null,"ALTER TABLESPACE UNDO0 ADD DATAFILE '/dev/raw/raw31' SIZE 30700M AUTOEXTEND OFF;"]
[{"$nulls":5},"/dev/raw/raw32",null,null,"Y","Y",null,"ALTER TABLESPACE UNDO0 ADD DATAFILE '/dev/raw/raw32' SIZE 30700M AUTOEXTEND OFF;"]
[{"$nulls":5},"/dev/raw/raw33",null,null,"Y","Y",null,"ALTER TABLESPACE UNDO0 ADD DATAFILE '/dev/raw/raw33' SIZE 30700M AUTOEXTEND OFF;"]
[{"$nulls":5},"/dev/raw/raw34",null,null,"Y","Y",null,"ALTER TABLESPACE UNDO0 ADD DATAFILE '/dev/raw/raw34' SIZE 30700M AUTOEXTEND OFF;"]
[{"$nulls":5},"/dev/raw/raw41",null,null,"Y","Y",null,"ALTER TABLESPACE UNDO0 ADD DATAFILE '/dev/raw/raw41' SIZE 30700M AUTOEXTEND OFF;"]
[{"$nulls":5},"/dev/raw/raw42",null,null,"Y","Y",null,"ALTER TABLESPACE UNDO0 ADD DATAFILE '/dev/raw/raw42' SIZE 30700M AUTOEXTEND OFF;"]
[{"$nulls":5},"/dev/raw/raw43",null,null,"Y","Y",null,"ALTER TABLESPACE UNDO0 ADD DATAFILE '/dev/raw/raw43' SIZE 30700M AUTOEXTEND OFF;"]
[{"$nulls":5},"/dev/raw/raw44",null,null,"Y","Y",null,"ALTER TABLESPACE UNDO0 ADD DATAFILE '/dev/raw/raw44' SIZE 30700M AUTOEXTEND OFF;"]
[{"$nulls":5},"/dev/raw/raw45",null,null,"Y","Y",null,"ALTER TABLESPACE UNDO0 ADD DATAFILE '/dev/raw/raw45' SIZE 30700M AUTOEXTEND OFF;"]
[null,null,"Node1의\n UNDO1 Tablespace\n (업무에 따라 산정)","UNDO1",null,"/dev/raw/raw24",30700,30700,"Y","Y"]
[{"$nulls":5},"/dev/raw/raw35",null,null,"Y","Y",null,{"$f":"\"ALTER TABLESPACE \"&$D$64&\" ADD DATAFILE '\" & F65 & \"' SIZE 30700M AUTOEXTEND OFF;\"","v":"ALTER TABLESPACE UNDO1 ADD DATAFILE '/dev/raw/raw35' SIZE 30700M AUTOEXTEND OFF;"}]
[{"$nulls":5},"/dev/raw/raw36",null,null,"Y","Y",null,"ALTER TABLESPACE UNDO1 ADD DATAFILE '/dev/raw/raw36' SIZE 30700M AUTOEXTEND OFF;"]
[{"$nulls":5},"/dev/raw/raw37",null,null,"Y","Y",null,"ALTER TABLESPACE UNDO1 ADD DATAFILE '/dev/raw/raw37' SIZE 30700M AUTOEXTEND OFF;"]
[{"$nulls":5},"/dev/raw/raw38",{"$nulls":5},"ALTER TABLESPACE UNDO1 ADD DATAFILE '/dev/raw/raw38' SIZE 30700M AUTOEXTEND OFF;"]
[{"$nulls":5},"/dev/raw/raw39",{"$nulls":5},"ALTER TABLESPACE UNDO1 ADD DATAFILE '/dev/raw/raw39' SIZE 30700M AUTOEXTEND OFF;"]
[{"$nulls":5},"/dev/raw/raw40",null,null,"Y","Y",null,"ALTER TABLESPACE UNDO1 ADD DATAFILE '/dev/raw/raw40' SIZE 30700M AUTOEXTEND OFF;"]
[null,null,"SYSTEM Tablespace","SYSTEM",null,"/dev/raw/raw25",30700,30700,"Y","Y"]
[null,null,"TEMP Tablespace\n (업무에 따라 산정)","TEMP",null,"/dev/raw/raw26",30700,30700,"Y","Y"]
[{"$nulls":8},"Y","Y"]
[{"$nulls":8},"Y","Y"]
[null,null,"USR Tablespace","USR",null,"/dev/raw/raw27",30700,30700,"Y","Y"]
[null,null,"APM Tablespace","_APM_TS",null,"/dev/raw/raw28",30700,30700,"Y","Y"]
[null,"User영역","사용자 Tablespace","User Tablespace \n (DB생성 시 임의 지정)",null,"관리 필요",null,"30700 * n","Y","Y"]
[null,null,"신호최적화시스템","soit_d08","001","/dev/raw/raw101",{"$nulls":5},{"$f":"\"CREATE TABLESPACE \"&D78&\" DATAFILE '\" & F78 & \"' SIZE 30700M AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE soit_d08 DATAFILE '/dev/raw/raw101' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"soit_d08","002","/dev/raw/raw102",{"$nulls":5},{"$f":"\"ALTER TABLESPACE \"&D79&\" ADD DATAFILE '\" & F79 & \"' SIZE 30700M AUTOEXTEND OFF;\"","v":"ALTER TABLESPACE soit_d08 ADD DATAFILE '/dev/raw/raw102' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"soit_d08","003","/dev/raw/raw103",{"$nulls":5},"ALTER TABLESPACE soit_d08 ADD DATAFILE '/dev/raw/raw103' SIZE 30700M AUTOEXTEND OFF;"]
[null,null,null,"soit_d08","004","/dev/raw/raw104",{"$nulls":5},"ALTER TABLESPACE soit_d08 ADD DATAFILE '/dev/raw/raw104' SIZE 30700M AUTOEXTEND OFF;"]
[null,null,null,"soit_d08","005","/dev/raw/raw105",{"$nulls":5},"ALTER TABLESPACE soit_d08 ADD DATAFILE '/dev/raw/raw105' SIZE 30700M AUTOEXTEND OFF;"]
[null,null,null,"soit_d08","006","/dev/raw/raw106",{"$nulls":5},"ALTER TABLESPACE soit_d08 ADD DATAFILE '/dev/raw/raw106' SIZE 30700M AUTOEXTEND OFF;"]
[null,null,null,"soit_d08","007","/dev/raw/raw107",{"$nulls":5},"ALTER TABLESPACE soit_d08 ADD DATAFILE '/dev/raw/raw107' SIZE 30700M AUTOEXTEND OFF;"]
[null,null,null,"soit_d08","008","/dev/raw/raw108",{"$nulls":5},"ALTER TABLESPACE soit_d08 ADD DATAFILE '/dev/raw/raw108' SIZE 30700M AUTOEXTEND OFF;"]
[null,null,null,"soit_d08","009","/dev/raw/raw109",{"$nulls":5},"ALTER TABLESPACE soit_d08 ADD DATAFILE '/dev/raw/raw109' SIZE 30700M AUTOEXTEND OFF;"]
[null,null,null,"soit_d08","010","/dev/raw/raw110",{"$nulls":5},"ALTER TABLESPACE soit_d08 ADD DATAFILE '/dev/raw/raw110' SIZE 30700M AUTOEXTEND OFF;"]
[null,null,null,"soit_d08","011","/dev/raw/raw111",{"$nulls":5},"ALTER TABLESPACE SOIT_D08 ADD DATAFILE '/dev/raw/raw111' SIZE 30700M,"]
[null,null,null,"soit_d08","012","/dev/raw/raw112",{"$nulls":5},"'/dev/raw/raw112' SIZE 30700M,"]
[null,null,null,"soit_d08","013","/dev/raw/raw113",{"$nulls":5},"'/dev/raw/raw113' SIZE 30700M,"]
[null,null,null,"soit_d08","014","/dev/raw/raw114",{"$nulls":5},"'/dev/raw/raw114' SIZE 30700M,"]
[null,null,null,"soit_d08","015","/dev/raw/raw115",{"$nulls":5},"'/dev/raw/raw115' SIZE 30700M,"]
[null,null,null,"soit_d08","016","/dev/raw/raw116",{"$nulls":5},"'/dev/raw/raw116' SIZE 30700M,"]
[null,null,null,"soit_d08","017","/dev/raw/raw117",{"$nulls":5},"'/dev/raw/raw117' SIZE 30700M,"]
[null,null,null,"soit_d08","018","/dev/raw/raw118",{"$nulls":5},"'/dev/raw/raw118' SIZE 30700M,"]
[null,null,null,"soit_d08","019","/dev/raw/raw119",{"$nulls":5},"'/dev/raw/raw119' SIZE 30700M,"]
[null,null,null,"soit_d08","020","/dev/raw/raw120",{"$nulls":5},"'/dev/raw/raw120' SIZE 30700M;"]
[null,null,null,"soit_d08","021","/dev/raw/raw121",{"$nulls":5},"ALTER TABLESPACE SOIT_D08 ADD DATAFILE '/dev/raw/raw121' SIZE 30700M,"]
[null,null,null,"soit_d08","022","/dev/raw/raw122",{"$nulls":5},"/dev/raw/raw122' SIZE 30700M,"]
[null,null,null,"soit_d08","023","/dev/raw/raw123",{"$nulls":5},"/dev/raw/raw123' SIZE 30700M,"]
[null,null,null,"soit_d08","024","/dev/raw/raw124",{"$nulls":5},"/dev/raw/raw124' SIZE 30700M,"]
[null,null,null,"soit_d08","025","/dev/raw/raw125",{"$nulls":5},"/dev/raw/raw125' SIZE 30700M,"]
[null,null,null,"soit_d08","026","/dev/raw/raw126",{"$nulls":5},"/dev/raw/raw126' SIZE 30700M,"]
[null,null,null,"soit_d08","027","/dev/raw/raw127",{"$nulls":5},"/dev/raw/raw127' SIZE 30700M,"]
[null,null,null,"soit_d08","028","/dev/raw/raw128",{"$nulls":5},"/dev/raw/raw128' SIZE 30700M,"]
[null,null,null,"soit_d08","029","/dev/raw/raw129",{"$nulls":5},"/dev/raw/raw129' SIZE 30700M,"]
[null,null,null,"soit_d08","030","/dev/raw/raw130",{"$nulls":5},"/dev/raw/raw130' SIZE 30700M,"]
[null,null,null,"soit_d08","031","/dev/raw/raw131",{"$nulls":5},"/dev/raw/raw131' SIZE 30700M,"]
[null,null,null,"soit_d08","032","/dev/raw/raw132",{"$nulls":5},"/dev/raw/raw132' SIZE 30700M,"]
[null,null,null,"soit_d08","033","/dev/raw/raw133",{"$nulls":5},"/dev/raw/raw133' SIZE 30700M,"]
[null,null,null,"soit_d08","034","/dev/raw/raw134",{"$nulls":5},"/dev/raw/raw134' SIZE 30700M,"]
[null,null,null,"soit_d08","035","/dev/raw/raw135",{"$nulls":5},"/dev/raw/raw135' SIZE 30700M,"]
[null,null,null,"soit_d08","036","/dev/raw/raw136",{"$nulls":5},"/dev/raw/raw136' SIZE 30700M,"]
[null,null,null,"soit_d08","037","/dev/raw/raw137",{"$nulls":5},"/dev/raw/raw137' SIZE 30700M,"]
[null,null,null,"soit_d08","038","/dev/raw/raw138",{"$nulls":5},"/dev/raw/raw138' SIZE 30700M,"]
[null,null,null,"soit_d08","039","/dev/raw/raw139",{"$nulls":5},"/dev/raw/raw139' SIZE 30700M,"]
[null,null,null,"soit_d08","040","/dev/raw/raw140",{"$nulls":5},"/dev/raw/raw140' SIZE 30700M;"]
[null,null,null,"soit_d08","041","/dev/raw/raw141",{"$nulls":5},{"$f":"\"ALTER TABLESPACE \"&D118&\" ADD DATAFILE '\" & F118 & \"' SIZE 30700M,\"","v":"ALTER TABLESPACE soit_d08 ADD DATAFILE '/dev/raw/raw141' SIZE 30700M,"}]
[null,null,null,"soit_d08","042","/dev/raw/raw142",{"$nulls":5},{"$f":"\"'\" & F119 & \"' SIZE 30700M,\"","v":"'/dev/raw/raw142' SIZE 30700M,"}]
[null,null,null,"soit_d08","043","/dev/raw/raw143",{"$nulls":5},"'/dev/raw/raw143' SIZE 30700M,"]
[null,null,null,"soit_d08","044","/dev/raw/raw144",{"$nulls":5},"'/dev/raw/raw144' SIZE 30700M,"]
[null,null,null,"soit_d08","045","/dev/raw/raw145",{"$nulls":5},"'/dev/raw/raw145' SIZE 30700M,"]
[null,null,null,"soit_d08","046","/dev/raw/raw146",{"$nulls":5},"'/dev/raw/raw146' SIZE 30700M,"]
[null,null,null,"soit_d08","047","/dev/raw/raw147",{"$nulls":5},"'/dev/raw/raw147' SIZE 30700M,"]
[null,null,null,"soit_d08","048","/dev/raw/raw148",{"$nulls":5},"'/dev/raw/raw148' SIZE 30700M,"]
[null,null,null,"soit_d08","049","/dev/raw/raw149",{"$nulls":5},"'/dev/raw/raw149' SIZE 30700M,"]
[null,null,null,"soit_d08","050","/dev/raw/raw150",{"$nulls":5},"'/dev/raw/raw150' SIZE 30700M,"]
[null,null,null,"soit_d08","051","/dev/raw/raw151",{"$nulls":5},"'/dev/raw/raw151' SIZE 30700M,"]
[null,null,null,"soit_d08","052","/dev/raw/raw152",{"$nulls":5},"'/dev/raw/raw152' SIZE 30700M,"]
[null,null,null,"soit_d08","053","/dev/raw/raw153",{"$nulls":5},"'/dev/raw/raw153' SIZE 30700M,"]
[null,null,null,"soit_d08","054","/dev/raw/raw154",{"$nulls":5},"'/dev/raw/raw154' SIZE 30700M,"]
[null,null,null,"soit_d08","055","/dev/raw/raw155",{"$nulls":5},"'/dev/raw/raw155' SIZE 30700M,"]
[null,null,null,"soit_d08","056","/dev/raw/raw156",{"$nulls":5},"'/dev/raw/raw156' SIZE 30700M,"]
[null,null,null,"soit_d08","057","/dev/raw/raw157",{"$nulls":5},"'/dev/raw/raw157' SIZE 30700M,"]
[null,null,null,"soit_d08","058","/dev/raw/raw158",{"$nulls":5},"'/dev/raw/raw158' SIZE 30700M,"]
[null,null,null,"soit_d08","059","/dev/raw/raw159",{"$nulls":5},"'/dev/raw/raw159' SIZE 30700M,"]
[null,null,null,"soit_d08","060","/dev/raw/raw160",{"$nulls":5},"'/dev/raw/raw160' SIZE 30700M,"]
[]
[]
[null,null,"신호변경이력용 테이블스페이스","soit_d08_02","001","/dev/raw/raw400",{"$nulls":5},{"$f":"\"CREATE TABLESPACE \"&D140&\" DATAFILE '\" & F140 & \"' SIZE 30700M AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE soit_d08_02 DATAFILE '/dev/raw/raw400' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"soit_d08_02","002","/dev/raw/raw401",{"$nulls":5},{"$f":"\"ALTER TABLESPACE \"&D141&\" ADD DATAFILE '\" & F141 & \"' SIZE 30700M,\"","v":"ALTER TABLESPACE soit_d08_02 ADD DATAFILE '/dev/raw/raw401' SIZE 30700M,"}]
[null,null,null,"soit_d08_02","003","/dev/raw/raw402",{"$nulls":5},{"$f":"\"'\" & F142 & \"' SIZE 30700M,\"","v":"'/dev/raw/raw402' SIZE 30700M,"}]
[null,null,null,"soit_d08_02","004","/dev/raw/raw403",{"$nulls":5},"'/dev/raw/raw403' SIZE 30700M,"]
[null,null,null,"soit_d08_02","005","/dev/raw/raw404",{"$nulls":5},{"$f":"\"'\" & F144 & \"' SIZE 30700M;\"","v":"'/dev/raw/raw404' SIZE 30700M;"}]
[null,null,"차량이동궤적용 테이블스페이스","soit_d08_01","001","/dev/raw/raw500",{"$nulls":5},{"$f":"\"CREATE TABLESPACE \"&D145&\" DATAFILE '\" & F145 & \"' SIZE 30700M AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE soit_d08_01 DATAFILE '/dev/raw/raw500' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"soit_d08_01","002","/dev/raw/raw501",{"$nulls":5},{"$f":"\"ALTER TABLESPACE \"&D146&\" ADD DATAFILE '\" & F146 & \"' SIZE 30700M,\"","v":"ALTER TABLESPACE soit_d08_01 ADD DATAFILE '/dev/raw/raw501' SIZE 30700M,"}]
[null,null,null,"soit_d08_01","003","/dev/raw/raw502",{"$nulls":5},{"$f":"\"'\" & F147 & \"' SIZE 30700M,\"","v":"'/dev/raw/raw502' SIZE 30700M,"}]
[null,null,null,"soit_d08_01","004","/dev/raw/raw503",{"$nulls":5},"'/dev/raw/raw503' SIZE 30700M,"]
[null,null,null,"soit_d08_01","005","/dev/raw/raw504",{"$nulls":5},{"$f":"\"'\" & F149 & \"' SIZE 30700M;\"","v":"'/dev/raw/raw504' SIZE 30700M;"}]
[null,null,"이동궤적-1지역","soit_d08_011","001","/dev/raw/raw505",{"$nulls":5},{"$f":"\"CREATE TABLESPACE \"&D150&\" DATAFILE '\" & F150 & \"' SIZE 30700M AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE soit_d08_011 DATAFILE '/dev/raw/raw505' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"soit_d08_011","002","/dev/raw/raw506",{"$nulls":5},{"$f":"\"ALTER TABLESPACE \"&D151&\" ADD DATAFILE '\" & F151 & \"' SIZE 30700M;\"","v":"ALTER TABLESPACE soit_d08_011 ADD DATAFILE '/dev/raw/raw506' SIZE 30700M;"}]
[null,null,"이동궤적-2지역","soit_d08_012","001","/dev/raw/raw507",{"$nulls":5},{"$f":"\"CREATE TABLESPACE \"&D152&\" DATAFILE '\" & F152 & \"' SIZE 30700M AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE soit_d08_012 DATAFILE '/dev/raw/raw507' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"soit_d08_012","002","/dev/raw/raw508",{"$nulls":5},{"$f":"\"ALTER TABLESPACE \"&D153&\" ADD DATAFILE '\" & F153 & \"' SIZE 30700M;\"","v":"ALTER TABLESPACE soit_d08_012 ADD DATAFILE '/dev/raw/raw508' SIZE 30700M;"}]
[null,null,"이동궤적-3지역","soit_d08_013","001","/dev/raw/raw509",{"$nulls":5},{"$f":"\"CREATE TABLESPACE \"&D154&\" DATAFILE '\" & F154 & \"' SIZE 30700M AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE soit_d08_013 DATAFILE '/dev/raw/raw509' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"soit_d08_013","002","/dev/raw/raw510",{"$nulls":5},{"$f":"\"ALTER TABLESPACE \"&D155&\" ADD DATAFILE '\" & F155 & \"' SIZE 30700M;\"","v":"ALTER TABLESPACE soit_d08_013 ADD DATAFILE '/dev/raw/raw510' SIZE 30700M;"}]
[null,null,"이동궤적-4지역","soit_d08_014","001","/dev/raw/raw511",{"$nulls":5},{"$f":"\"CREATE TABLESPACE \"&D156&\" DATAFILE '\" & F156 & \"' SIZE 30700M AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE soit_d08_014 DATAFILE '/dev/raw/raw511' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"soit_d08_014","002","/dev/raw/raw512",{"$nulls":5},{"$f":"\"ALTER TABLESPACE \"&D157&\" ADD DATAFILE '\" & F157 & \"' SIZE 30700M;\"","v":"ALTER TABLESPACE soit_d08_014 ADD DATAFILE '/dev/raw/raw512' SIZE 30700M;"}]
[null,null,"이동궤적-5지역","soit_d08_015","001","/dev/raw/raw513",{"$nulls":5},{"$f":"\"CREATE TABLESPACE \"&D158&\" DATAFILE '\" & F158 & \"' SIZE 30700M AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE soit_d08_015 DATAFILE '/dev/raw/raw513' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"soit_d08_015","002","/dev/raw/raw514",{"$nulls":5},{"$f":"\"ALTER TABLESPACE \"&D159&\" ADD DATAFILE '\" & F159 & \"' SIZE 30700M;\"","v":"ALTER TABLESPACE soit_d08_015 ADD DATAFILE '/dev/raw/raw514' SIZE 30700M;"}]
[null,null,"이동궤적-6지역","soit_d08_016","001","/dev/raw/raw515",{"$nulls":5},{"$f":"\"CREATE TABLESPACE \"&D160&\" DATAFILE '\" & F160 & \"' SIZE 30700M AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE soit_d08_016 DATAFILE '/dev/raw/raw515' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"soit_d08_016","002","/dev/raw/raw516",{"$nulls":5},{"$f":"\"ALTER TABLESPACE \"&D161&\" ADD DATAFILE '\" & F161 & \"' SIZE 30700M;\"","v":"ALTER TABLESPACE soit_d08_016 ADD DATAFILE '/dev/raw/raw516' SIZE 30700M;"}]
[null,null,"이동궤적-7지역","soit_d08_017","001","/dev/raw/raw517",{"$nulls":5},{"$f":"\"CREATE TABLESPACE \"&D162&\" DATAFILE '\" & F162 & \"' SIZE 30700M AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE soit_d08_017 DATAFILE '/dev/raw/raw517' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"soit_d08_017","002","/dev/raw/raw518",{"$nulls":5},{"$f":"\"ALTER TABLESPACE \"&D163&\" ADD DATAFILE '\" & F163 & \"' SIZE 30700M;\"","v":"ALTER TABLESPACE soit_d08_017 ADD DATAFILE '/dev/raw/raw518' SIZE 30700M;"}]
[null,null,"이동궤적-8지역","soit_d08_018","001","/dev/raw/raw519",{"$nulls":5},{"$f":"\"CREATE TABLESPACE \"&D164&\" DATAFILE '\" & F164 & \"' SIZE 30700M AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE soit_d08_018 DATAFILE '/dev/raw/raw519' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"soit_d08_018","002","/dev/raw/raw520",{"$nulls":5},{"$f":"\"ALTER TABLESPACE \"&D165&\" ADD DATAFILE '\" & F165 & \"' SIZE 30700M;\"","v":"ALTER TABLESPACE soit_d08_018 ADD DATAFILE '/dev/raw/raw520' SIZE 30700M;"}]
[null,null,"이동궤적-9지역","soit_d08_019","001","/dev/raw/raw521",{"$nulls":5},{"$f":"\"CREATE TABLESPACE \"&D166&\" DATAFILE '\" & F166 & \"' SIZE 30700M AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE soit_d08_019 DATAFILE '/dev/raw/raw521' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"soit_d08_019","002","/dev/raw/raw522",{"$nulls":5},{"$f":"\"ALTER TABLESPACE \"&D167&\" ADD DATAFILE '\" & F167 & \"' SIZE 30700M;\"","v":"ALTER TABLESPACE soit_d08_019 ADD DATAFILE '/dev/raw/raw522' SIZE 30700M;"}]
[null,null,"대기행렬-실시간","soit_d08_031","001","/dev/raw/raw550",{"$nulls":5},{"$f":"\"CREATE TABLESPACE \"&D168&\" DATAFILE '\" & F168 & \"' SIZE 30700M AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE soit_d08_031 DATAFILE '/dev/raw/raw550' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"soit_d08_031","002","/dev/raw/raw551",{"$nulls":5},{"$f":"\"ALTER TABLESPACE \"&D169&\" ADD DATAFILE '\" & F169 & \"' SIZE 30700M;\"","v":"ALTER TABLESPACE soit_d08_031 ADD DATAFILE '/dev/raw/raw551' SIZE 30700M;"}]
[]
[null,null,"BI 집계","soit_d08_041","001","/dev/raw/raw555",{"$nulls":5},{"$f":"\"CREATE TABLESPACE \"&D171&\" DATAFILE '\" & F171 & \"' SIZE 30700M AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE soit_d08_041 DATAFILE '/dev/raw/raw555' SIZE 30700M AUTOEXTEND OFF;"}]
[]
[null,null,null,"soit_i08","001","/dev/raw/raw701",{"$nulls":5},{"$f":"\"CREATE TABLESPACE \"&D173&\" DATAFILE '\" & F173 & \"' SIZE 30700M AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE soit_i08 DATAFILE '/dev/raw/raw701' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"soit_i08","002","/dev/raw/raw702",{"$nulls":5},{"$f":"\"ALTER TABLESPACE \"&D174&\" ADD DATAFILE '\" & F174 & \"' SIZE 30700M AUTOEXTEND OFF;\"","v":"ALTER TABLESPACE soit_i08 ADD DATAFILE '/dev/raw/raw702' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"soit_i08","003","/dev/raw/raw703",{"$nulls":5},"ALTER TABLESPACE soit_i08 ADD DATAFILE '/dev/raw/raw703' SIZE 30700M AUTOEXTEND OFF;"]
[null,null,null,"soit_i08","004","/dev/raw/raw704",{"$nulls":5},"ALTER TABLESPACE soit_i08 ADD DATAFILE '/dev/raw/raw704' SIZE 30700M AUTOEXTEND OFF;"]
[null,null,null,"soit_i08","005","/dev/raw/raw705",{"$nulls":5},"ALTER TABLESPACE soit_i08 ADD DATAFILE '/dev/raw/raw705' SIZE 30700M AUTOEXTEND OFF;"]
[null,null,null,"soit_i08","006","/dev/raw/raw706",{"$nulls":5},"ALTER TABLESPACE soit_i08 ADD DATAFILE '/dev/raw/raw706' SIZE 30700M AUTOEXTEND OFF;"]
[null,null,null,"soit_i08","007","/dev/raw/raw707",{"$nulls":5},"ALTER TABLESPACE soit_i08 ADD DATAFILE '/dev/raw/raw707' SIZE 30700M AUTOEXTEND OFF;"]
[null,null,null,"soit_i08","008","/dev/raw/raw708",{"$nulls":5},"ALTER TABLESPACE soit_i08 ADD DATAFILE '/dev/raw/raw708' SIZE 30700M AUTOEXTEND OFF;"]
[]
[]
[null,null,"교통정책지원시스템(TPSSA*)","TPSS_D08_01","001","/dev/raw/raw1001",{"$nulls":5},"CREATE TABLESPACE TPSS_D08_01 DATAFILE '/dev/raw/raw1001' SIZE 30700M AUTOEXTEND OFF, '/dev/raw/raw1002' SIZE 30700M AUTOEXTEND OFF; "]
[{"$nulls":4},"002","/dev/raw/raw1002"]
[]
[null,null,null,"TPSS_I08_01",null,"/dev/raw/raw1100"]
[{"$nulls":5},"/dev/raw/raw1099"]
[{"$nulls":5},"/dev/raw/raw1098"]
[{"$nulls":5},"/dev/raw/raw1097"]
[{"$nulls":5},"/dev/raw/raw1096"]
[]
[null,null,"교통정책지원시스템(TPSSB*)","TPSS_D08_02","001","/dev/raw/raw1101",{"$nulls":5},"CREATE TABLESPACE TPSS_D08_02 DATAFILE '/dev/raw/raw1101' SIZE 30700M AUTOEXTEND OFF; "]
[]
[null,null,"교통정책지원시스템(TPSSD*)","TPSS_D08_04","001","/dev/raw/raw1111",{"$nulls":5},"CREATE TABLESPACE TPSS_D08_04 DATAFILE '/dev/raw/raw1111' SIZE 30700M AUTOEXTEND OFF; "]
[]
[null,null,"교통정책지원시스템(TPSSX*)","TPSS_D08_24","001","/dev/raw/raw1521",{"$nulls":5},"CREATE TABLESPACE TPSS_D08_24 DATAFILE '/dev/raw/raw1521' SIZE 30700M AUTOEXTEND OFF; "]
[]
[null,null,"교통정책지원시스템(TPSSZ*)","TPSS_D08_26","001","/dev/raw/raw1571",{"$nulls":5},"CREATE TABLESPACE TPSS_D08_26 DATAFILE '/dev/raw/raw1571' SIZE 30700M AUTOEXTEND OFF; "]
[]
[null,null,"교통정책지원시스템(TPSSG*)","TPSS_D08_07",null,"/dev/raw/raw1171"]
[null,null,null,"TPSS_D08_07",null,"/dev/raw/raw1172"]
[null,null,null,"TPSS_D08_07",null,"/dev/raw/raw1173"]
[null,null,null,"TPSS_D08_07",null,"/dev/raw/raw1174"]
[null,null,null,"TPSS_D08_07",null,"/dev/raw/raw1175"]
[null,null,null,"TPSS_D08_07",null,"/dev/raw/raw1176"]
[null,null,null,"TPSS_D08_07",null,"/dev/raw/raw1177"]
[null,null,null,"TPSS_D08_07",null,"/dev/raw/raw1178"]
[null,null,null,"TPSS_D08_07",null,"/dev/raw/raw1179"]
[null,null,null,"TPSS_D08_07",null,"/dev/raw/raw1180"]
[null,null,null,"TPSS_D08_07",null,"/dev/raw/raw1181"]
[null,null,null,"TPSS_D08_07",null,"/dev/raw/raw1182"]
[null,null,null,"TPSS_D08_07",null,"/dev/raw/raw1183"]
[null,null,null,"TPSS_D08_07",null,"/dev/raw/raw1184"]
[null,null,null,"TPSS_D08_07",null,"/dev/raw/raw1185"]
[null,null,null,"TPSS_D08_07",null,"/dev/raw/raw1186"]
[null,null,null,"TPSS_D08_07",null,"/dev/raw/raw1187"]
[null,null,null,"TPSS_D08_07",null,"/dev/raw/raw1188"]
[null,null,null,"TPSS_D08_07",null,"/dev/raw/raw1189"]
[null,null,null,"TPSS_D08_07",null,"/dev/raw/raw1190"]
[]
[null,null,"교통정책지원시스템(TPSSG*)","TPSS_I08_07",null,"/dev/raw/raw1210"]
[null,null,null,"TPSS_I08_07",null,"/dev/raw/raw1209"]
[null,null,null,"TPSS_I08_07",null,"/dev/raw/raw1208",{"$nulls":5},"ALTER TABLESPACE TPSS_I08_07 ADD DATAFILE '/dev/raw/raw1208' SIZE 30700M AUTOEXTEND OFF,\n                                          '/dev/raw/raw1207' SIZE 30700M AUTOEXTEND OFF,\n                                          '/dev/raw/raw1206' SIZE 30700M AUTOEXTEND OFF,\n                                          '/dev/raw/raw1205' SIZE 30700M AUTOEXTEND OFF,\n                                          '/dev/raw/raw1204' SIZE 30700M AUTOEXTEND OFF,\n                                          '/dev/raw/raw1203' SIZE 30700M AUTOEXTEND OFF,\n                                          '/dev/raw/raw1202' SIZE 30700M AUTOEXTEND OFF"]
[null,null,null,"TPSS_I08_07",null,"/dev/raw/raw1207"]
[null,null,null,"TPSS_I08_07",null,"/dev/raw/raw1206"]
[null,null,null,"TPSS_I08_07",null,"/dev/raw/raw1205"]
[null,null,null,"TPSS_I08_07",null,"/dev/raw/raw1204"]
[null,null,null,"TPSS_I08_07",null,"/dev/raw/raw1203"]
[null,null,null,"TPSS_I08_07",null,"/dev/raw/raw1202"]
[]
[null,null,"교통정책지원시스템(TPSSM*)","TPSS_D08_13",null,"/dev/raw/raw1221"]
[{"$nulls":5},"/dev/raw/raw1222"]
[]
[null,null,null,"TPSS_I08_13",null,"/dev/raw/raw1250"]
[{"$nulls":5},"/dev/raw/raw1249"]
[]
[null,null,"교통정책지원시스템 연계데이터(SCDT)","SCDT_D08_20","001","/dev/raw/raw1441"]
[null,null,null,"SCDT_D08_20","002","/dev/raw/raw1442"]
[null,null,null,"SCDT_D08_20","003","/dev/raw/raw1443"]
[null,null,null,"SCDT_D08_20","004","/dev/raw/raw1444"]
[null,null,null,"SCDT_D08_20","005","/dev/raw/raw1445"]
[null,null,null,"SCDT_D08_20","006","/dev/raw/raw1446",{"$nulls":5},"ALTER TABLESPACE SCDT_D08_20 ADD DATAFILE '/dev/raw/raw1446' SIZE 30700M,"]
[null,null,null,"SCDT_D08_20","007","/dev/raw/raw1447",{"$nulls":5},"/dev/raw/raw1447' SIZE 30700M,"]
[null,null,null,"SCDT_D08_20","008","/dev/raw/raw1448",{"$nulls":5},"/dev/raw/raw1448' SIZE 30700M,"]
[null,null,null,"SCDT_D08_20","009","/dev/raw/raw1449",{"$nulls":5},"/dev/raw/raw1449' SIZE 30700M,"]
[null,null,null,"SCDT_D08_20","010","/dev/raw/raw1450",{"$nulls":5},"/dev/raw/raw1450' SIZE 30700M,"]
[null,null,null,"SCDT_D08_20","011","/dev/raw/raw1451",{"$nulls":5},"/dev/raw/raw1451' SIZE 30700M,"]
[null,null,null,"SCDT_D08_20","012","/dev/raw/raw1452",{"$nulls":5},"/dev/raw/raw1452' SIZE 30700M,"]
[null,null,null,"SCDT_D08_20","013","/dev/raw/raw1453",{"$nulls":5},"/dev/raw/raw1453' SIZE 30700M,"]
[null,null,null,"SCDT_D08_20","014","/dev/raw/raw1454",{"$nulls":5},"/dev/raw/raw1454' SIZE 30700M,"]
[null,null,null,"SCDT_D08_20","015","/dev/raw/raw1455",{"$nulls":5},"/dev/raw/raw1455' SIZE 30700M;"]
[null,null,null,"SCDT_D08_20","016","/dev/raw/raw1456"]
[null,null,null,"SCDT_D08_20","017","/dev/raw/raw1457"]
[null,null,null,"SCDT_D08_20","018","/dev/raw/raw1458"]
[null,null,null,"SCDT_D08_20","019","/dev/raw/raw1459"]
[null,null,null,"SCDT_D08_20","020","/dev/raw/raw1460"]
[null,null,null,"SCDT_D08_20","021","/dev/raw/raw1461"]
[null,null,null,"SCDT_D08_20","022","/dev/raw/raw1462"]
[null,null,null,"SCDT_D08_20","023","/dev/raw/raw1463"]
[null,null,null,"SCDT_D08_20","024","/dev/raw/raw1464"]
[null,null,null,"SCDT_D08_20","025","/dev/raw/raw1465"]
[null,null,null,"SCDT_D08_20","026","/dev/raw/raw1466"]
[null,null,null,"SCDT_D08_20","027","/dev/raw/raw1467"]
[null,null,null,"SCDT_D08_20","028","/dev/raw/raw1468"]
[null,null,null,"SCDT_D08_20","029","/dev/raw/raw1469"]
[null,null,null,"SCDT_D08_20","030","/dev/raw/raw1470"]
[null,null,null,"SCDT_D08_20","031","/dev/raw/raw1471"]
[null,null,null,"SCDT_D08_20","032","/dev/raw/raw1472"]
[null,null,null,"SCDT_D08_20","033","/dev/raw/raw1473"]
[null,null,null,"SCDT_D08_20","034","/dev/raw/raw1474"]
[null,null,null,"SCDT_D08_20","035","/dev/raw/raw1475"]
[null,null,null,"SCDT_D08_20","036","/dev/raw/raw1476"]
[null,null,null,"SCDT_D08_20","037","/dev/raw/raw1477"]
[null,null,null,"SCDT_D08_20","038","/dev/raw/raw1478"]
[null,null,null,"SCDT_D08_20","039","/dev/raw/raw1479"]
[null,null,null,"SCDT_D08_20","040","/dev/raw/raw1480"]
[]
[]
["테이블 스페이스 사용량 확인 조회 쿼리"]
["    SELECT SUBSTR(T1.TABLESPACE_NAME,1,30) \"TS_NM\"\n               , ROUND(SUM(T1.TOTAL1)/1024/1024,1) \"TOTAL(MB)\"\n               , ROUND(SUM(T1.TOTAL1)/1024/1024,1)-ROUND(SUM(T1.SUM1)/1024/1024,1) \"USED(MB)\"\n               , ROUND(SUM(T1.SUM1)/1024/1024,1) \"FREE(MB)\"\n               , ROUND((ROUND(SUM(T1.TOTAL1)/1024/1024,1)-ROUND(SUM(T1.SUM1)/1024/1024,1))/ROUND(SUM(T1.TOTAL1)/1024/1024,1)*100,2) \"USED(%)\"\n     FROM\n      ( SELECT   TABLESPACE_NAME\n                        , 0 TOTAL1\n                        , SUM(BYTES) SUM1\n                        , MAX(BYTES) MAXB\n                        , COUNT(BYTES) CNT\n        FROM  DBA_FREE_SPACE\n        GROUP BY TABLESPACE_NAME\n        UNION\n        SELECT   TABLESPACE_NAME\n                      , SUM(BYTES) TOTAL1\n                      , 0\n                      , 0\n                      , 0\n        FROM     DBA_DATA_FILES\n        GROUP BY TABLESPACE_NAME) T1\n      GROUP BY T1.TABLESPACE_NAME\n      ORDER BY 1"]

{"sheet":"신호최적화 테이블스페이스관리","index":1,"n_rows":208,"n_cols":11,"rows_kept":208,"cut":false,"hidden":false,"merged":[[6,0,6,7],[7,0,22,0],[7,1,15,1],[8,2,12,2],[13,2,14,2],[16,1,22,1],[17,2,19,2],[30,2,34,2],[36,2,37,2],[20,2,21,2],[23,0,23,7],[24,0,43,0],[24,1,35,1],[24,2,26,2],[27,2,29,2],[36,1,43,1],[38,2,39,2],[40,2,42,2],[44,0,44,7],[152,1,176,1],[171,2,176,2],[178,1,207,1],[198,2,207,2],[45,0,150,0],[45,1,107,1],[108,1,150,1],[151,0,151,7],[152,0,207,0]]}
["구분","영역","용도/사용자","테이블스페이스명","LV명","경로명","할당크기(MB)","합계(MB)","갱신일","경로","/data/soit/"]
[null,null,null,"REDO",null,"?"]
[null,null,null,"UNDO"]
[null,null,null,"SYSTEM"]
[null,null,null,"TEMP"]
[null,null,null,"USER"]
["글로벌브릿지 스마트교차로 테이블스페이스"]
["글로벌브릿지","DATA","신호최적화-글로벌","SOIT_D08_G001","001",{"$f":"D8&\"_\"&E8","v":"SOIT_D08_G001_001"},"100M",null,null,{"$f":"\"CREATE TABLESPACE \"&D8&\" DATAFILE '\" & $K$1 & F8 & \".dbf' SIZE \"&G8&\" AUTOEXTEND ON;\"","v":"CREATE TABLESPACE SOIT_D08_G001 DATAFILE '/data/soit/SOIT_D08_G001_001.dbf' SIZE 100M AUTOEXTEND ON;"}]
[null,null,"신호최적화-글로벌(실시간)","SOIT_D08_G002","001","SOIT_D08_G002_001","30700M",null,null,{"$f":"\"CREATE TABLESPACE \"&D9&\" DATAFILE '\" & $K$1 & F9 & \".dbf' SIZE \"&G9&\" AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE SOIT_D08_G002 DATAFILE '/data/soit/SOIT_D08_G002_001.dbf' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"SOIT_D08_G002","002","SOIT_D08_G002_002","30700M",null,null,{"$f":"\"ALTER TABLESPACE \" & D10 & \" ADD DATAFILE '\" & $K$1 &F10&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_D08_G002 ADD DATAFILE '/data/soit/SOIT_D08_G002_002.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_D08_G002","003","SOIT_D08_G002_003","30700M",null,null,{"$f":"\"'\"&$K$1&F11&\".dbf' SIZE \"& G11 &\",\"","v":"'/data/soit/SOIT_D08_G002_003.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_D08_G002","004","SOIT_D08_G002_004","30700M",null,null,"'/data/soit/SOIT_D08_G002_004.dbf' SIZE 30700M,"]
[null,null,null,"SOIT_D08_G002","005","SOIT_D08_G002_005","30700M",null,null,{"$f":"\"'\"&$K$1&F13&\".dbf' SIZE \"& G13 &\";\"","v":"'/data/soit/SOIT_D08_G002_005.dbf' SIZE 30700M;"}]
[null,null,"신호최적화-글로벌(통계/상태)","SOIT_D08_G003","001","SOIT_D08_G003_001","30700M",null,null,{"$f":"\"CREATE TABLESPACE \"&D14&\" DATAFILE '\" & $K$1 & F14 & \".dbf' SIZE \"&G14&\" AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE SOIT_D08_G003 DATAFILE '/data/soit/SOIT_D08_G003_001.dbf' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"SOIT_D08_G003","002","SOIT_D08_G003_002","30700M",null,null,{"$f":"\"ALTER TABLESPACE \" & D15 & \" ADD DATAFILE '\" & $K$1 &F15&\".dbf' SIZE 30700M;\"","v":"ALTER TABLESPACE SOIT_D08_G003 ADD DATAFILE '/data/soit/SOIT_D08_G003_002.dbf' SIZE 30700M;"}]
[]
[null,"INDEX","신호최적화-글로벌","SOIT_I08_G001","001",{"$f":"D17&\"_\"&E17","v":"SOIT_I08_G001_001"},"100M",null,null,{"$f":"\"CREATE TABLESPACE \"&D17&\" DATAFILE '\" & $K$1 & F17 & \".dbf' SIZE \"&G17&\" AUTOEXTEND ON;\"","v":"CREATE TABLESPACE SOIT_I08_G001 DATAFILE '/data/soit/SOIT_I08_G001_001.dbf' SIZE 100M AUTOEXTEND ON;"}]
[null,null,"신호최적화-글로벌(실시간)","SOIT_I08_G002","001","SOIT_I08_G002_001","30700M",null,null,{"$f":"\"CREATE TABLESPACE \"&D18&\" DATAFILE '\" & $K$1 & F18 & \".dbf' SIZE \"&G18&\" AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE SOIT_I08_G002 DATAFILE '/data/soit/SOIT_I08_G002_001.dbf' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"SOIT_I08_G002","002","SOIT_I08_G002_002","30700M",null,null,{"$f":"\"ALTER TABLESPACE \" & D19 & \" ADD DATAFILE '\" & $K$1 &F19&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_I08_G002 ADD DATAFILE '/data/soit/SOIT_I08_G002_002.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_I08_G002","003","SOIT_I08_G002_003","30700M",null,null,{"$f":"\"'\"&$K$1&F20&\".dbf' SIZE \"& G20 &\";\"","v":"'/data/soit/SOIT_I08_G002_003.dbf' SIZE 30700M;"}]
[null,null,"신호최적화-글로벌(통계/상태)","SOIT_I08_G003","001","SOIT_I08_G003_001","30700M",null,null,{"$f":"\"CREATE TABLESPACE \"&D21&\" DATAFILE '\" & $K$1 & F21 & \".dbf' SIZE \"&G21&\" AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE SOIT_I08_G003 DATAFILE '/data/soit/SOIT_I08_G003_001.dbf' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"SOIT_I08_G003","002","SOIT_I08_G003_002","30700M",null,null,{"$f":"\"ALTER TABLESPACE \" & D22 & \" ADD DATAFILE '\" & $K$1 &F22&\".dbf' SIZE 30700M;\"","v":"ALTER TABLESPACE SOIT_I08_G003 ADD DATAFILE '/data/soit/SOIT_I08_G003_002.dbf' SIZE 30700M;"}]
[]
["동인시스템 신호현시/긴급차량 테이블스페이스"]
["동인시스템","DATA","신호최적화-동인(TOD정보)","SOIT_D08_D001","001",{"$f":"D25&\"_\"&E25","v":"SOIT_D08_D001_001"},"30700M",null,null,{"$f":"\"CREATE TABLESPACE \"&D25&\" DATAFILE '\" & $K$1 & F25 & \".dbf' SIZE \"&G25&\" AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE SOIT_D08_D001 DATAFILE '/data/soit/SOIT_D08_D001_001.dbf' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"SOIT_D08_D001","002","SOIT_D08_D001_002","30700M",null,null,{"$f":"\"ALTER TABLESPACE \" & D26 & \" ADD DATAFILE '\" & $K$1 &F26&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_D08_D001 ADD DATAFILE '/data/soit/SOIT_D08_D001_002.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_D08_D001","003","SOIT_D08_D001_003","30700M",null,null,{"$f":"\"'\"&$K$1&F27&\".dbf' SIZE \"& G27 &\";\"","v":"'/data/soit/SOIT_D08_D001_003.dbf' SIZE 30700M;"}]
[null,null,"신호최적화-동인(긴급차량)","SOIT_D08_D002","001","SOIT_D08_D002_001","30700M",null,null,{"$f":"\"CREATE TABLESPACE \"&D28&\" DATAFILE '\" & $K$1 & F28 & \".dbf' SIZE \"&G28&\" AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE SOIT_D08_D002 DATAFILE '/data/soit/SOIT_D08_D002_001.dbf' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"SOIT_D08_D002","002","SOIT_D08_D002_002","30700M",null,null,{"$f":"\"ALTER TABLESPACE \" & D29 & \" ADD DATAFILE '\" & $K$1 &F29&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_D08_D002 ADD DATAFILE '/data/soit/SOIT_D08_D002_002.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_D08_D002","003","SOIT_D08_D002_003","30700M",null,null,{"$f":"\"'\"&$K$1&F30&\".dbf' SIZE \"& G30 &\";\"","v":"'/data/soit/SOIT_D08_D002_003.dbf' SIZE 30700M;"}]
[null,null,"신호최적화-동인(실시간)","SOIT_D08_D003","001","SOIT_D08_D003_001","30700M",null,null,{"$f":"\"CREATE TABLESPACE \"&D31&\" DATAFILE '\" & $K$1 & F31 & \".dbf' SIZE \"&G31&\" AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE SOIT_D08_D003 DATAFILE '/data/soit/SOIT_D08_D003_001.dbf' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"SOIT_D08_D003","002","SOIT_D08_D003_002","30700M",null,null,{"$f":"\"ALTER TABLESPACE \" & D32 & \" ADD DATAFILE '\" & $K$1 &F32&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_D08_D003 ADD DATAFILE '/data/soit/SOIT_D08_D003_002.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_D08_D003","003","SOIT_D08_D003_003","30700M",null,null,{"$f":"\"'\"&$K$1&F33&\".dbf' SIZE \"& G33 &\",\"","v":"'/data/soit/SOIT_D08_D003_003.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_D08_D003","004","SOIT_D08_D003_004","30700M",null,null,"'/data/soit/SOIT_D08_D003_004.dbf' SIZE 30700M,"]
[null,null,null,"SOIT_D08_D003","005","SOIT_D08_D003_005","30700M",null,null,{"$f":"\"'\"&$K$1&F35&\".dbf' SIZE \"& G35 &\";\"","v":"'/data/soit/SOIT_D08_D003_005.dbf' SIZE 30700M;"}]
[]
[null,"INDEX","신호최적화-동인(TOD정보)","SOIT_I08_D001","001",{"$f":"D37&\"_\"&E37","v":"SOIT_I08_D001_001"},"30700M",null,null,{"$f":"\"CREATE TABLESPACE \"&D37&\" DATAFILE '\" & $K$1 & F37 & \".dbf' SIZE \"&G37&\" AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE SOIT_I08_D001 DATAFILE '/data/soit/SOIT_I08_D001_001.dbf' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"SOIT_I08_D001","002","SOIT_I08_D001_002","30700M",null,null,{"$f":"\"ALTER TABLESPACE \" & D38 & \" ADD DATAFILE '\" & $K$1 &F38&\".dbf' SIZE 30700M;\"","v":"ALTER TABLESPACE SOIT_I08_D001 ADD DATAFILE '/data/soit/SOIT_I08_D001_002.dbf' SIZE 30700M;"}]
[null,null,"신호최적화-동인(긴급차량)","SOIT_I08_D002","001","SOIT_I08_D002_001","30700M",null,null,{"$f":"\"CREATE TABLESPACE \"&D39&\" DATAFILE '\" & $K$1 & F39 & \".dbf' SIZE \"&G39&\" AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE SOIT_I08_D002 DATAFILE '/data/soit/SOIT_I08_D002_001.dbf' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"SOIT_I08_D002","002","SOIT_I08_D002_002","30700M",null,null,{"$f":"\"ALTER TABLESPACE \" & D40 & \" ADD DATAFILE '\" & $K$1 &F40&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_I08_D002 ADD DATAFILE '/data/soit/SOIT_I08_D002_002.dbf' SIZE 30700M,"}]
[null,null,"신호최적화-동인(실시간)","SOIT_I08_D003","001","SOIT_I08_D003_001","30700M",null,null,{"$f":"\"'\"&$K$1&F41&\".dbf' SIZE \"& G41 &\";\"","v":"'/data/soit/SOIT_I08_D003_001.dbf' SIZE 30700M;"}]
[null,null,null,"SOIT_I08_D003","002","SOIT_I08_D003_002","30700M",null,null,{"$f":"\"CREATE TABLESPACE \"&D42&\" DATAFILE '\" & $K$1 & F42 & \".dbf' SIZE \"&G42&\" AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE SOIT_I08_D003 DATAFILE '/data/soit/SOIT_I08_D003_002.dbf' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"SOIT_I08_D003","003","SOIT_I08_D003_003","30700M",null,null,{"$f":"\"ALTER TABLESPACE \" & D43 & \" ADD DATAFILE '\" & $K$1 &F43&\".dbf' SIZE 30700M;\"","v":"ALTER TABLESPACE SOIT_I08_D003 ADD DATAFILE '/data/soit/SOIT_I08_D003_003.dbf' SIZE 30700M;"}]
[]
["신호최적화 운영정보/시뮬레이션 테이블스페이스"]
[null,"DATA","신호최적화-시스템운영/기반정보(현시, 네트워크)","SOIT_D08_M001","001",{"$f":"D46&\"_\"&E46","v":"SOIT_D08_M001_001"},"100M",null,null,{"$f":"\"CREATE TABLESPACE \"&D46&\" DATAFILE '\" & $K$1 & F46 & \".dbf' SIZE \"&G46&\" AUTOEXTEND ON;\"","v":"CREATE TABLESPACE SOIT_D08_M001 DATAFILE '/data/soit/SOIT_D08_M001_001.dbf' SIZE 100M AUTOEXTEND ON;"}]
[null,null,"신호최적화-궤적-1지역","SOIT_D08_C001","001","SOIT_D08_C001_001","30700M",null,null,{"$f":"\"CREATE TABLESPACE \"&D47&\" DATAFILE '\" & $K$1 & F47 & \".dbf' SIZE \"&G47&\" AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE SOIT_D08_C001 DATAFILE '/data/soit/SOIT_D08_C001_001.dbf' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"SOIT_D08_C001","002","SOIT_D08_C001_002","30700M",null,null,{"$f":"\"ALTER TABLESPACE \" & D48 & \" ADD DATAFILE '\" & $K$1 &F48&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_D08_C001 ADD DATAFILE '/data/soit/SOIT_D08_C001_002.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_D08_C001","003","SOIT_D08_C001_003","30700M",null,null,{"$f":"\"'\"&$K$1&F49&\".dbf' SIZE \"& G49 &\",\"","v":"'/data/soit/SOIT_D08_C001_003.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_D08_C001","004","SOIT_D08_C001_004","30700M",null,null,"'/data/soit/SOIT_D08_C001_004.dbf' SIZE 30700M,"]
[null,null,null,"SOIT_D08_C001","005","SOIT_D08_C001_005","30700M",null,null,{"$f":"\"'\"&$K$1&F51&\".dbf' SIZE \"& G51 &\";\"","v":"'/data/soit/SOIT_D08_C001_005.dbf' SIZE 30700M;"}]
[null,null,"신호최적화-궤적-2지역","SOIT_D08_C002","001","SOIT_D08_C002_001","30700M",null,null,{"$f":"\"CREATE TABLESPACE \"&D52&\" DATAFILE '\" & $K$1 & F52 & \".dbf' SIZE \"&G52&\" AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE SOIT_D08_C002 DATAFILE '/data/soit/SOIT_D08_C002_001.dbf' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"SOIT_D08_C002","002","SOIT_D08_C002_002","30700M",null,null,{"$f":"\"ALTER TABLESPACE \" & D53 & \" ADD DATAFILE '\" & $K$1 &F53&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_D08_C002 ADD DATAFILE '/data/soit/SOIT_D08_C002_002.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_D08_C002","003","SOIT_D08_C002_003","30700M",null,null,{"$f":"\"'\"&$K$1&F54&\".dbf' SIZE \"& G54 &\",\"","v":"'/data/soit/SOIT_D08_C002_003.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_D08_C002","004","SOIT_D08_C002_004","30700M",null,null,"'/data/soit/SOIT_D08_C002_004.dbf' SIZE 30700M,"]
[null,null,null,"SOIT_D08_C002","005","SOIT_D08_C002_005","30700M",null,null,{"$f":"\"'\"&$K$1&F56&\".dbf' SIZE \"& G56 &\";\"","v":"'/data/soit/SOIT_D08_C002_005.dbf' SIZE 30700M;"}]
[null,null,null,"SOIT_D08_C002","006","SOIT_D08_C002_006","30700M",null,"2023-03-13",{"$f":"\"ALTER TABLESPACE \" & D57 & \" ADD DATAFILE '\" & $K$1 &F57&\".dbf' SIZE 30700M;\"","v":"ALTER TABLESPACE SOIT_D08_C002 ADD DATAFILE '/data/soit/SOIT_D08_C002_006.dbf' SIZE 30700M;"}]
[null,null,"신호최적화-궤적-3지역","SOIT_D08_C003","001","SOIT_D08_C003_001","30700M",null,null,{"$f":"\"CREATE TABLESPACE \"&D58&\" DATAFILE '\" & $K$1 & F58 & \".dbf' SIZE \"&G58&\" AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE SOIT_D08_C003 DATAFILE '/data/soit/SOIT_D08_C003_001.dbf' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"SOIT_D08_C003","002","SOIT_D08_C003_002","30700M",null,null,{"$f":"\"ALTER TABLESPACE \" & D59 & \" ADD DATAFILE '\" & $K$1 &F59&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_D08_C003 ADD DATAFILE '/data/soit/SOIT_D08_C003_002.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_D08_C003","003","SOIT_D08_C003_003","30700M",null,null,{"$f":"\"'\"&$K$1&F60&\".dbf' SIZE \"& G60 &\",\"","v":"'/data/soit/SOIT_D08_C003_003.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_D08_C003","004","SOIT_D08_C003_004","30700M",null,null,"'/data/soit/SOIT_D08_C003_004.dbf' SIZE 30700M,"]
[null,null,null,"SOIT_D08_C003","005","SOIT_D08_C003_005","30700M",null,null,{"$f":"\"'\"&$K$1&F62&\".dbf' SIZE \"& G62 &\";\"","v":"'/data/soit/SOIT_D08_C003_005.dbf' SIZE 30700M;"}]
[null,null,null,"SOIT_D08_C003","006","SOIT_D08_C003_006","30700M",null,"2023-03-13",{"$f":"\"ALTER TABLESPACE \" & D63 & \" ADD DATAFILE '\" & $K$1 &F63&\".dbf' SIZE 30700M;\"","v":"ALTER TABLESPACE SOIT_D08_C003 ADD DATAFILE '/data/soit/SOIT_D08_C003_006.dbf' SIZE 30700M;"}]
[null,null,"신호최적화-궤적-4지역","SOIT_D08_C004","001","SOIT_D08_C004_001","30700M",null,null,{"$f":"\"CREATE TABLESPACE \"&D64&\" DATAFILE '\" & $K$1 & F64 & \".dbf' SIZE \"&G64&\" AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE SOIT_D08_C004 DATAFILE '/data/soit/SOIT_D08_C004_001.dbf' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"SOIT_D08_C004","002","SOIT_D08_C004_002","30700M",null,null,{"$f":"\"ALTER TABLESPACE \" & D65 & \" ADD DATAFILE '\" & $K$1 &F65&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_D08_C004 ADD DATAFILE '/data/soit/SOIT_D08_C004_002.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_D08_C004","003","SOIT_D08_C004_003","30700M",null,null,{"$f":"\"'\"&$K$1&F66&\".dbf' SIZE \"& G66 &\",\"","v":"'/data/soit/SOIT_D08_C004_003.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_D08_C004","004","SOIT_D08_C004_004","30700M",null,null,"'/data/soit/SOIT_D08_C004_004.dbf' SIZE 30700M,"]
[null,null,null,"SOIT_D08_C004","005","SOIT_D08_C004_005","30700M",null,null,{"$f":"\"'\"&$K$1&F68&\".dbf' SIZE \"& G68 &\";\"","v":"'/data/soit/SOIT_D08_C004_005.dbf' SIZE 30700M;"}]
[null,null,null,"SOIT_D08_C004","006","SOIT_D08_C004_006","30700M",null,"2023-03-13",{"$f":"\"ALTER TABLESPACE \" & D69 & \" ADD DATAFILE '\" & $K$1 &F69&\".dbf' SIZE 30700M;\"","v":"ALTER TABLESPACE SOIT_D08_C004 ADD DATAFILE '/data/soit/SOIT_D08_C004_006.dbf' SIZE 30700M;"}]
[null,null,"신호최적화-궤적-5지역","SOIT_D08_C005","001","SOIT_D08_C005_001","30700M",null,null,{"$f":"\"CREATE TABLESPACE \"&D70&\" DATAFILE '\" & $K$1 & F70 & \".dbf' SIZE \"&G70&\" AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE SOIT_D08_C005 DATAFILE '/data/soit/SOIT_D08_C005_001.dbf' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"SOIT_D08_C005","002","SOIT_D08_C005_002","30700M",null,null,{"$f":"\"ALTER TABLESPACE \" & D71 & \" ADD DATAFILE '\" & $K$1 &F71&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_D08_C005 ADD DATAFILE '/data/soit/SOIT_D08_C005_002.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_D08_C005","003","SOIT_D08_C005_003","30700M",null,null,{"$f":"\"'\"&$K$1&F72&\".dbf' SIZE \"& G72 &\",\"","v":"'/data/soit/SOIT_D08_C005_003.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_D08_C005","004","SOIT_D08_C005_004","30700M",null,null,"'/data/soit/SOIT_D08_C005_004.dbf' SIZE 30700M,"]
[null,null,null,"SOIT_D08_C005","005","SOIT_D08_C005_005","30700M",null,null,{"$f":"\"'\"&$K$1&F74&\".dbf' SIZE \"& G74 &\";\"","v":"'/data/soit/SOIT_D08_C005_005.dbf' SIZE 30700M;"}]
[null,null,"신호최적화-궤적-6지역","SOIT_D08_C006","001","SOIT_D08_C006_001","30700M",null,null,{"$f":"\"CREATE TABLESPACE \"&D75&\" DATAFILE '\" & $K$1 & F75 & \".dbf' SIZE \"&G75&\" AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE SOIT_D08_C006 DATAFILE '/data/soit/SOIT_D08_C006_001.dbf' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"SOIT_D08_C006","002","SOIT_D08_C006_002","30700M",null,null,{"$f":"\"ALTER TABLESPACE \" & D76 & \" ADD DATAFILE '\" & $K$1 &F76&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_D08_C006 ADD DATAFILE '/data/soit/SOIT_D08_C006_002.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_D08_C006","003","SOIT_D08_C006_003","30700M",null,null,{"$f":"\"'\"&$K$1&F77&\".dbf' SIZE \"& G77 &\",\"","v":"'/data/soit/SOIT_D08_C006_003.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_D08_C006","004","SOIT_D08_C006_004","30700M",null,null,"'/data/soit/SOIT_D08_C006_004.dbf' SIZE 30700M,"]
[null,null,null,"SOIT_D08_C006","005","SOIT_D08_C006_005","30700M",null,null,{"$f":"\"'\"&$K$1&F79&\".dbf' SIZE \"& G79 &\";\"","v":"'/data/soit/SOIT_D08_C006_005.dbf' SIZE 30700M;"}]
[null,null,null,"SOIT_D08_C006","006","SOIT_D08_C006_006","30700M",null,"2023-03-13",{"$f":"\"ALTER TABLESPACE \" & D80 & \" ADD DATAFILE '\" & $K$1 &F80&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_D08_C006 ADD DATAFILE '/data/soit/SOIT_D08_C006_006.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_D08_C006","007","SOIT_D08_C006_007","30700M",null,"2023-03-13",{"$f":"\"'\"&$K$1&F81&\".dbf' SIZE \"& G81 &\";\"","v":"'/data/soit/SOIT_D08_C006_007.dbf' SIZE 30700M;"}]
[null,null,null,"SOIT_D08_C006","008","SOIT_D08_C006_008","30700M",null,"2023-03-13",{"$f":"\"ALTER TABLESPACE \" & D82 & \" ADD DATAFILE '\" & $K$1 &F82&\".dbf' SIZE 30700M;\"","v":"ALTER TABLESPACE SOIT_D08_C006 ADD DATAFILE '/data/soit/SOIT_D08_C006_008.dbf' SIZE 30700M;"}]
[null,null,"신호최적화-궤적-7지역","SOIT_D08_C007","001","SOIT_D08_C007_001","30700M",null,null,{"$f":"\"CREATE TABLESPACE \"&D83&\" DATAFILE '\" & $K$1 & F83 & \".dbf' SIZE \"&G83&\" AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE SOIT_D08_C007 DATAFILE '/data/soit/SOIT_D08_C007_001.dbf' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"SOIT_D08_C007","002","SOIT_D08_C007_002","30700M",null,null,{"$f":"\"ALTER TABLESPACE \" & D84 & \" ADD DATAFILE '\" & $K$1 &F84&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_D08_C007 ADD DATAFILE '/data/soit/SOIT_D08_C007_002.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_D08_C007","003","SOIT_D08_C007_003","30700M",null,null,{"$f":"\"'\"&$K$1&F85&\".dbf' SIZE \"& G85 &\",\"","v":"'/data/soit/SOIT_D08_C007_003.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_D08_C007","004","SOIT_D08_C007_004","30700M",null,null,"'/data/soit/SOIT_D08_C007_004.dbf' SIZE 30700M,"]
[null,null,null,"SOIT_D08_C007","005","SOIT_D08_C007_005","30700M",null,null,{"$f":"\"'\"&$K$1&F87&\".dbf' SIZE \"& G87 &\";\"","v":"'/data/soit/SOIT_D08_C007_005.dbf' SIZE 30700M;"}]
[null,null,"신호최적화-궤적-8지역","SOIT_D08_C008","001","SOIT_D08_C008_001","30700M",null,null,{"$f":"\"CREATE TABLESPACE \"&D88&\" DATAFILE '\" & $K$1 & F88 & \".dbf' SIZE \"&G88&\" AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE SOIT_D08_C008 DATAFILE '/data/soit/SOIT_D08_C008_001.dbf' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"SOIT_D08_C008","002","SOIT_D08_C008_002","30700M",null,null,{"$f":"\"ALTER TABLESPACE \" & D89 & \" ADD DATAFILE '\" & $K$1 &F89&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_D08_C008 ADD DATAFILE '/data/soit/SOIT_D08_C008_002.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_D08_C008","003","SOIT_D08_C008_003","30700M",null,null,{"$f":"\"'\"&$K$1&F90&\".dbf' SIZE \"& G90 &\",\"","v":"'/data/soit/SOIT_D08_C008_003.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_D08_C008","004","SOIT_D08_C008_004","30700M",null,null,"'/data/soit/SOIT_D08_C008_004.dbf' SIZE 30700M,"]
[null,null,null,"SOIT_D08_C008","005","SOIT_D08_C008_005","30700M",null,null,{"$f":"\"'\"&$K$1&F92&\".dbf' SIZE \"& G92 &\";\"","v":"'/data/soit/SOIT_D08_C008_005.dbf' SIZE 30700M;"}]
[null,null,"신호최적화-궤적-9지역","SOIT_D08_C009","001","SOIT_D08_C009_001","30700M",null,null,{"$f":"\"CREATE TABLESPACE \"&D93&\" DATAFILE '\" & $K$1 & F93 & \".dbf' SIZE \"&G93&\" AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE SOIT_D08_C009 DATAFILE '/data/soit/SOIT_D08_C009_001.dbf' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"SOIT_D08_C009","002","SOIT_D08_C009_002","30700M",null,null,{"$f":"\"ALTER TABLESPACE \" & D94 & \" ADD DATAFILE '\" & $K$1 &F94&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_D08_C009 ADD DATAFILE '/data/soit/SOIT_D08_C009_002.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_D08_C009","003","SOIT_D08_C009_003","30700M",null,null,{"$f":"\"'\"&$K$1&F95&\".dbf' SIZE \"& G95 &\",\"","v":"'/data/soit/SOIT_D08_C009_003.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_D08_C009","004","SOIT_D08_C009_004","30700M",null,null,"'/data/soit/SOIT_D08_C009_004.dbf' SIZE 30700M,"]
[null,null,null,"SOIT_D08_C009","005","SOIT_D08_C009_005","30700M",null,null,{"$f":"\"'\"&$K$1&F97&\".dbf' SIZE \"& G97 &\";\"","v":"'/data/soit/SOIT_D08_C009_005.dbf' SIZE 30700M;"}]
[null,null,"신호최적화-실측신호이력","SOIT_D08_S001","001","SOIT_D08_S001_001","30700M",null,null,{"$f":"\"CREATE TABLESPACE \"&D98&\" DATAFILE '\" & $K$1 & F98 & \".dbf' SIZE \"&G98&\" AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE SOIT_D08_S001 DATAFILE '/data/soit/SOIT_D08_S001_001.dbf' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"SOIT_D08_S001","002","SOIT_D08_S001_002","30700M",null,null,{"$f":"\"ALTER TABLESPACE \" & D99 & \" ADD DATAFILE '\" & $K$1 &F99&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_D08_S001 ADD DATAFILE '/data/soit/SOIT_D08_S001_002.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_D08_S001","003","SOIT_D08_S001_003","30700M",null,null,{"$f":"\"'\"&$K$1&F100&\".dbf' SIZE \"& G100 &\",\"","v":"'/data/soit/SOIT_D08_S001_003.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_D08_S001","004","SOIT_D08_S001_004","30700M",null,null,"'/data/soit/SOIT_D08_S001_004.dbf' SIZE 30700M,"]
[null,null,null,"SOIT_D08_S001","005","SOIT_D08_S001_005","30700M",null,null,{"$f":"\"'\"&$K$1&F102&\".dbf' SIZE \"& G102 &\";\"","v":"'/data/soit/SOIT_D08_S001_005.dbf' SIZE 30700M;"}]
[null,null,"신호최적화-예측신호이력","SOIT_D08_S002","001","SOIT_D08_S002_001","30700M",null,null,{"$f":"\"CREATE TABLESPACE \"&D103&\" DATAFILE '\" & $K$1 & F103 & \".dbf' SIZE \"&G103&\" AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE SOIT_D08_S002 DATAFILE '/data/soit/SOIT_D08_S002_001.dbf' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"SOIT_D08_S002","002","SOIT_D08_S002_002","30700M",null,null,{"$f":"\"ALTER TABLESPACE \" & D104 & \" ADD DATAFILE '\" & $K$1 &F104&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_D08_S002 ADD DATAFILE '/data/soit/SOIT_D08_S002_002.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_D08_S002","003","SOIT_D08_S002_003","30700M",null,null,{"$f":"\"'\"&$K$1&F105&\".dbf' SIZE \"& G105 &\",\"","v":"'/data/soit/SOIT_D08_S002_003.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_D08_S002","004","SOIT_D08_S002_004","30700M",null,null,"'/data/soit/SOIT_D08_S002_004.dbf' SIZE 30700M,"]
[null,null,null,"SOIT_D08_S002","005","SOIT_D08_S002_005","30700M",null,null,{"$f":"\"'\"&$K$1&F107&\".dbf' SIZE \"& G107 &\";\"","v":"'/data/soit/SOIT_D08_S002_005.dbf' SIZE 30700M;"}]
[]
[null,"INDEX","신호최적화-시스템운영/기반정보(현시, 네트워크)","SOIT_I08_M001","001",{"$f":"D109&\"_\"&E109","v":"SOIT_I08_M001_001"},"100M",null,null,{"$f":"\"CREATE TABLESPACE \"&D109&\" DATAFILE '\" & $K$1 & F109 & \".dbf' SIZE \"&G109&\" AUTOEXTEND ON;\"","v":"CREATE TABLESPACE SOIT_I08_M001 DATAFILE '/data/soit/SOIT_I08_M001_001.dbf' SIZE 100M AUTOEXTEND ON;"}]
[null,null,"신호최적화-궤적-1지역","SOIT_I08_C001","001","SOIT_I08_C001_001","30700M",null,null,{"$f":"\"CREATE TABLESPACE \"&D110&\" DATAFILE '\" & $K$1 & F110 & \".dbf' SIZE \"&G110&\" AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE SOIT_I08_C001 DATAFILE '/data/soit/SOIT_I08_C001_001.dbf' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"SOIT_I08_C001","002","SOIT_I08_C001_002","30700M",null,null,{"$f":"\"ALTER TABLESPACE \" & D111 & \" ADD DATAFILE '\" & $K$1 &F111&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_I08_C001 ADD DATAFILE '/data/soit/SOIT_I08_C001_002.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_I08_C001","003","SOIT_I08_C001_003","30700M",null,null,{"$f":"\"'\"&$K$1&F112&\".dbf' SIZE \"& G112 &\";\"","v":"'/data/soit/SOIT_I08_C001_003.dbf' SIZE 30700M;"}]
[null,null,"신호최적화-궤적-2지역","SOIT_I08_C002","001","SOIT_I08_C002_001","30700M",null,null,{"$f":"\"CREATE TABLESPACE \"&D113&\" DATAFILE '\" & $K$1 & F113 & \".dbf' SIZE \"&G113&\" AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE SOIT_I08_C002 DATAFILE '/data/soit/SOIT_I08_C002_001.dbf' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"SOIT_I08_C002","002","SOIT_I08_C002_002","30700M",null,null,{"$f":"\"ALTER TABLESPACE \" & D114 & \" ADD DATAFILE '\" & $K$1 &F114&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_I08_C002 ADD DATAFILE '/data/soit/SOIT_I08_C002_002.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_I08_C002","003","SOIT_I08_C002_003","30700M",null,null,{"$f":"\"'\"&$K$1&F115&\".dbf' SIZE \"& G115 &\";\"","v":"'/data/soit/SOIT_I08_C002_003.dbf' SIZE 30700M;"}]
[null,null,null,"SOIT_I08_C002","004","SOIT_I08_C002_004","30700M",null,"2023-03-13",{"$f":"\"ALTER TABLESPACE \" & D116 & \" ADD DATAFILE '\" & $K$1 &F116&\".dbf' SIZE 30700M;\"","v":"ALTER TABLESPACE SOIT_I08_C002 ADD DATAFILE '/data/soit/SOIT_I08_C002_004.dbf' SIZE 30700M;"}]
[null,null,"신호최적화-궤적-3지역","SOIT_I08_C003","001","SOIT_I08_C003_001","30700M",null,null,{"$f":"\"CREATE TABLESPACE \"&D117&\" DATAFILE '\" & $K$1 & F117 & \".dbf' SIZE \"&G117&\" AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE SOIT_I08_C003 DATAFILE '/data/soit/SOIT_I08_C003_001.dbf' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"SOIT_I08_C003","002","SOIT_I08_C003_002","30700M",null,null,{"$f":"\"ALTER TABLESPACE \" & D118 & \" ADD DATAFILE '\" & $K$1 &F118&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_I08_C003 ADD DATAFILE '/data/soit/SOIT_I08_C003_002.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_I08_C003","003","SOIT_I08_C003_003","30700M",null,null,{"$f":"\"'\"&$K$1&F119&\".dbf' SIZE \"& G119 &\";\"","v":"'/data/soit/SOIT_I08_C003_003.dbf' SIZE 30700M;"}]
[null,null,null,"SOIT_I08_C003","004","SOIT_I08_C003_004","30700M",null,"2023-03-13",{"$f":"\"ALTER TABLESPACE \" & D120 & \" ADD DATAFILE '\" & $K$1 &F120&\".dbf' SIZE 30700M;\"","v":"ALTER TABLESPACE SOIT_I08_C003 ADD DATAFILE '/data/soit/SOIT_I08_C003_004.dbf' SIZE 30700M;"}]
[null,null,null,"SOIT_I08_C003","005","SOIT_I08_C003_005","30700M",null,"2023-03-13","ALTER TABLESPACE SOIT_I08_C003 ADD DATAFILE '/data/soit/SOIT_I08_C003_005.dbf' SIZE 30700M;"]
[null,null,"신호최적화-궤적-4지역","SOIT_I08_C004","001","SOIT_I08_C004_001","30700M",null,null,{"$f":"\"CREATE TABLESPACE \"&D122&\" DATAFILE '\" & $K$1 & F122 & \".dbf' SIZE \"&G122&\" AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE SOIT_I08_C004 DATAFILE '/data/soit/SOIT_I08_C004_001.dbf' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"SOIT_I08_C004","002","SOIT_I08_C004_002","30700M",null,null,{"$f":"\"ALTER TABLESPACE \" & D123 & \" ADD DATAFILE '\" & $K$1 &F123&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_I08_C004 ADD DATAFILE '/data/soit/SOIT_I08_C004_002.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_I08_C004","003","SOIT_I08_C004_003","30700M",null,null,{"$f":"\"'\"&$K$1&F124&\".dbf' SIZE \"& G124 &\";\"","v":"'/data/soit/SOIT_I08_C004_003.dbf' SIZE 30700M;"}]
[null,null,null,"SOIT_I08_C004","004","SOIT_I08_C004_004","30700M",null,"2023-03-13",{"$f":"\"ALTER TABLESPACE \" & D125 & \" ADD DATAFILE '\" & $K$1 &F125&\".dbf' SIZE 30700M;\"","v":"ALTER TABLESPACE SOIT_I08_C004 ADD DATAFILE '/data/soit/SOIT_I08_C004_004.dbf' SIZE 30700M;"}]
[null,null,"신호최적화-궤적-5지역","SOIT_I08_C005","001","SOIT_I08_C005_001","30700M",null,null,{"$f":"\"CREATE TABLESPACE \"&D126&\" DATAFILE '\" & $K$1 & F126 & \".dbf' SIZE \"&G126&\" AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE SOIT_I08_C005 DATAFILE '/data/soit/SOIT_I08_C005_001.dbf' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"SOIT_I08_C005","002","SOIT_I08_C005_002","30700M",null,null,{"$f":"\"ALTER TABLESPACE \" & D127 & \" ADD DATAFILE '\" & $K$1 &F127&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_I08_C005 ADD DATAFILE '/data/soit/SOIT_I08_C005_002.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_I08_C005","003","SOIT_I08_C005_003","30700M",null,null,{"$f":"\"'\"&$K$1&F128&\".dbf' SIZE \"& G128 &\";\"","v":"'/data/soit/SOIT_I08_C005_003.dbf' SIZE 30700M;"}]
[null,null,null,"SOIT_I08_C005","004","SOIT_I08_C005_004","30700M",null,"2023-03-13",{"$f":"\"ALTER TABLESPACE \" & D129 & \" ADD DATAFILE '\" & $K$1 &F129&\".dbf' SIZE 30700M;\"","v":"ALTER TABLESPACE SOIT_I08_C005 ADD DATAFILE '/data/soit/SOIT_I08_C005_004.dbf' SIZE 30700M;"}]
[null,null,"신호최적화-궤적-6지역","SOIT_I08_C006","001","SOIT_I08_C006_001","30700M",null,null,{"$f":"\"CREATE TABLESPACE \"&D130&\" DATAFILE '\" & $K$1 & F130 & \".dbf' SIZE \"&G130&\" AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE SOIT_I08_C006 DATAFILE '/data/soit/SOIT_I08_C006_001.dbf' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"SOIT_I08_C006","002","SOIT_I08_C006_002","30700M",null,null,{"$f":"\"ALTER TABLESPACE \" & D131 & \" ADD DATAFILE '\" & $K$1 &F131&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_I08_C006 ADD DATAFILE '/data/soit/SOIT_I08_C006_002.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_I08_C006","003","SOIT_I08_C006_003","30700M",null,null,{"$f":"\"'\"&$K$1&F132&\".dbf' SIZE \"& G132 &\";\"","v":"'/data/soit/SOIT_I08_C006_003.dbf' SIZE 30700M;"}]
[null,null,null,"SOIT_I08_C006","004","SOIT_I08_C006_004","30700M",null,"2023-03-13",{"$f":"\"ALTER TABLESPACE \" & D133 & \" ADD DATAFILE '\" & $K$1 &F133&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_I08_C006 ADD DATAFILE '/data/soit/SOIT_I08_C006_004.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_I08_C006","005","SOIT_I08_C006_005","30700M",null,"2023-03-13",{"$f":"\"'\"&$K$1&F134&\".dbf' SIZE \"& G134 &\";\"","v":"'/data/soit/SOIT_I08_C006_005.dbf' SIZE 30700M;"}]
[null,null,null,"SOIT_I08_C006","006","SOIT_I08_C006_006","30700M",null,"2023-03-13",{"$f":"\"ALTER TABLESPACE \" & D135 & \" ADD DATAFILE '\" & $K$1 &F135&\".dbf' SIZE 30700M;\"","v":"ALTER TABLESPACE SOIT_I08_C006 ADD DATAFILE '/data/soit/SOIT_I08_C006_006.dbf' SIZE 30700M;"}]
[null,null,"신호최적화-궤적-7지역","SOIT_I08_C007","001","SOIT_I08_C007_001","30700M",null,null,{"$f":"\"CREATE TABLESPACE \"&D136&\" DATAFILE '\" & $K$1 & F136 & \".dbf' SIZE \"&G136&\" AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE SOIT_I08_C007 DATAFILE '/data/soit/SOIT_I08_C007_001.dbf' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"SOIT_I08_C007","002","SOIT_I08_C007_002","30700M",null,null,{"$f":"\"ALTER TABLESPACE \" & D137 & \" ADD DATAFILE '\" & $K$1 &F137&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_I08_C007 ADD DATAFILE '/data/soit/SOIT_I08_C007_002.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_I08_C007","003","SOIT_I08_C007_003","30700M",null,null,{"$f":"\"'\"&$K$1&F138&\".dbf' SIZE \"& G138 &\";\"","v":"'/data/soit/SOIT_I08_C007_003.dbf' SIZE 30700M;"}]
[null,null,"신호최적화-궤적-8지역","SOIT_I08_C008","001","SOIT_I08_C008_001","30700M",null,null,{"$f":"\"CREATE TABLESPACE \"&D139&\" DATAFILE '\" & $K$1 & F139 & \".dbf' SIZE \"&G139&\" AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE SOIT_I08_C008 DATAFILE '/data/soit/SOIT_I08_C008_001.dbf' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"SOIT_I08_C008","002","SOIT_I08_C008_002","30700M",null,null,{"$f":"\"ALTER TABLESPACE \" & D140 & \" ADD DATAFILE '\" & $K$1 &F140&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_I08_C008 ADD DATAFILE '/data/soit/SOIT_I08_C008_002.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_I08_C008","003","SOIT_I08_C008_003","30700M",null,null,{"$f":"\"'\"&$K$1&F141&\".dbf' SIZE \"& G141 &\";\"","v":"'/data/soit/SOIT_I08_C008_003.dbf' SIZE 30700M;"}]
[null,null,"신호최적화-궤적-9지역","SOIT_I08_C009","001","SOIT_I08_C009_001","30700M",null,null,{"$f":"\"CREATE TABLESPACE \"&D142&\" DATAFILE '\" & $K$1 & F142 & \".dbf' SIZE \"&G142&\" AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE SOIT_I08_C009 DATAFILE '/data/soit/SOIT_I08_C009_001.dbf' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"SOIT_I08_C009","002","SOIT_I08_C009_002","30700M",null,null,{"$f":"\"ALTER TABLESPACE \" & D143 & \" ADD DATAFILE '\" & $K$1 &F143&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_I08_C009 ADD DATAFILE '/data/soit/SOIT_I08_C009_002.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_I08_C009","003","SOIT_I08_C009_003","30700M",null,null,{"$f":"\"'\"&$K$1&F144&\".dbf' SIZE \"& G144 &\";\"","v":"'/data/soit/SOIT_I08_C009_003.dbf' SIZE 30700M;"}]
[null,null,"신호최적화-실측신호이력","SOIT_I08_S001","001","SOIT_I08_S001_001","30700M",null,null,{"$f":"\"CREATE TABLESPACE \"&D145&\" DATAFILE '\" & $K$1 & F145 & \".dbf' SIZE \"&G145&\" AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE SOIT_I08_S001 DATAFILE '/data/soit/SOIT_I08_S001_001.dbf' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"SOIT_I08_S001","002","SOIT_I08_S001_002","30700M",null,null,{"$f":"\"ALTER TABLESPACE \" & D146 & \" ADD DATAFILE '\" & $K$1 &F146&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_I08_S001 ADD DATAFILE '/data/soit/SOIT_I08_S001_002.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_I08_S001","003","SOIT_I08_S001_003","30700M",null,null,{"$f":"\"'\"&$K$1&F147&\".dbf' SIZE \"& G147 &\";\"","v":"'/data/soit/SOIT_I08_S001_003.dbf' SIZE 30700M;"}]
[null,null,"신호최적화-예측신호이력","SOIT_I08_S002","001","SOIT_I08_S002_001","30700M",null,null,{"$f":"\"CREATE TABLESPACE \"&D148&\" DATAFILE '\" & $K$1 & F148 & \".dbf' SIZE \"&G148&\" AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE SOIT_I08_S002 DATAFILE '/data/soit/SOIT_I08_S002_001.dbf' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"SOIT_I08_S002","002","SOIT_I08_S002_002","30700M",null,null,{"$f":"\"ALTER TABLESPACE \" & D149 & \" ADD DATAFILE '\" & $K$1 &F149&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_I08_S002 ADD DATAFILE '/data/soit/SOIT_I08_S002_002.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_I08_S002","003","SOIT_I08_S002_003","30700M",null,null,{"$f":"\"'\"&$K$1&F150&\".dbf' SIZE \"& G150 &\";\"","v":"'/data/soit/SOIT_I08_S002_003.dbf' SIZE 30700M;"}]
[]
["신호최적화 집계/최적화분석 테이블스페이스"]
[null,"DATA","신호최적화-실시간 시뮬레이션 집계","SOIT_D08_T001","001",{"$f":"D153&\"_\"&E153","v":"SOIT_D08_T001_001"},"30700M",null,null,{"$f":"\"CREATE TABLESPACE \"&D153&\" DATAFILE '\" & $K$1 & F153 & \".dbf' SIZE \"&G153&\" AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE SOIT_D08_T001 DATAFILE '/data/soit/SOIT_D08_T001_001.dbf' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"SOIT_D08_T001","002","SOIT_D08_T001_002","30700M",null,null,{"$f":"\"ALTER TABLESPACE \" & D154 & \" ADD DATAFILE '\" & $K$1 &F154&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_D08_T001 ADD DATAFILE '/data/soit/SOIT_D08_T001_002.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_D08_T001","003","SOIT_D08_T001_003","30700M",null,null,{"$f":"\"'\"&$K$1&F155&\".dbf' SIZE \"& G155 &\";\"","v":"'/data/soit/SOIT_D08_T001_003.dbf' SIZE 30700M;"}]
[null,null,null,"SOIT_D08_T001","004","SOIT_D08_T001_004","30700M",null,null,{"$f":"\"ALTER TABLESPACE \" & D156 & \" ADD DATAFILE '\" & $K$1 &F156&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_D08_T001 ADD DATAFILE '/data/soit/SOIT_D08_T001_004.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_D08_T001","005","SOIT_D08_T001_005","30700M",null,null,{"$f":"\"'\"&$K$1&F157&\".dbf' SIZE \"& G157 &\",\"","v":"'/data/soit/SOIT_D08_T001_005.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_D08_T001","006","SOIT_D08_T001_006","30700M",null,null,{"$f":"\"'\"&$K$1&F158&\".dbf' SIZE \"& G158 &\";\"","v":"'/data/soit/SOIT_D08_T001_006.dbf' SIZE 30700M;"}]
[null,null,null,"SOIT_D08_T001","007","SOIT_D08_T001_007","30700M",null,"2023-03-06",{"$f":"\"ALTER TABLESPACE \" & D159 & \" ADD DATAFILE '\" & $K$1 &F159&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_D08_T001 ADD DATAFILE '/data/soit/SOIT_D08_T001_007.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_D08_T001","008","SOIT_D08_T001_008","30700M",null,"2023-03-06",{"$f":"\"'\"&$K$1&F160&\".dbf' SIZE \"& G160 &\";\"","v":"'/data/soit/SOIT_D08_T001_008.dbf' SIZE 30700M;"}]
[null,null,null,"SOIT_D08_T001","009","SOIT_D08_T001_009","30700M",null,"2023-03-13",{"$f":"\"ALTER TABLESPACE \" & D161 & \" ADD DATAFILE '\" & $K$1 &F161&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_D08_T001 ADD DATAFILE '/data/soit/SOIT_D08_T001_009.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_D08_T001","010","SOIT_D08_T001_010","30700M",null,"2023-03-13",{"$f":"\"'\"&$K$1&F162&\".dbf' SIZE \"& G162 &\";\"","v":"'/data/soit/SOIT_D08_T001_010.dbf' SIZE 30700M;"}]
[null,null,"신호최적화-배치 시뮬레이션/BI 집계","SOIT_D08_T002","001","SOIT_D08_T002_001","30700M",null,null,{"$f":"\"CREATE TABLESPACE \"&D163&\" DATAFILE '\" & $K$1 & F163 & \".dbf' SIZE \"&G163&\" AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE SOIT_D08_T002 DATAFILE '/data/soit/SOIT_D08_T002_001.dbf' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"SOIT_D08_T002","002","SOIT_D08_T002_002","30700M",null,null,{"$f":"\"ALTER TABLESPACE \" & D164 & \" ADD DATAFILE '\" & $K$1 &F164&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_D08_T002 ADD DATAFILE '/data/soit/SOIT_D08_T002_002.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_D08_T002","003","SOIT_D08_T002_003","30700M",null,null,{"$f":"\"'\"&$K$1&F165&\".dbf' SIZE \"& G165 &\";\"","v":"'/data/soit/SOIT_D08_T002_003.dbf' SIZE 30700M;"}]
[null,null,null,"SOIT_D08_T002","004","SOIT_D08_T002_004","30700M",null,"2023-03-06",{"$f":"\"ALTER TABLESPACE \" & D166 & \" ADD DATAFILE '\" & $K$1 &F166&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_D08_T002 ADD DATAFILE '/data/soit/SOIT_D08_T002_004.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_D08_T002","005","SOIT_D08_T002_005","30700M",null,"2023-03-06",{"$f":"\"'\"&$K$1&F167&\".dbf' SIZE \"& G167 &\";\"","v":"'/data/soit/SOIT_D08_T002_005.dbf' SIZE 30700M;"}]
[null,null,null,"SOIT_D08_T002","006","SOIT_D08_T002_006","30700M",null,"2023-03-13",{"$f":"\"ALTER TABLESPACE \" & D168 & \" ADD DATAFILE '\" & $K$1 &F168&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_D08_T002 ADD DATAFILE '/data/soit/SOIT_D08_T002_006.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_D08_T002","007","SOIT_D08_T002_007","30700M",null,"2023-03-13",{"$f":"\"'\"&$K$1&F169&\".dbf' SIZE \"& G169 &\";\"","v":"'/data/soit/SOIT_D08_T002_007.dbf' SIZE 30700M;"}]
[null,null,"신호최적화-최적화분석 ","SOIT_D08_A001","001","SOIT_D08_A001_001","30700M",null,null,{"$f":"\"CREATE TABLESPACE \"&D170&\" DATAFILE '\" & $K$1 & F170 & \".dbf' SIZE \"&G170&\" AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE SOIT_D08_A001 DATAFILE '/data/soit/SOIT_D08_A001_001.dbf' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"SOIT_D08_A001","002","SOIT_D08_A001_002","30700M",null,null,{"$f":"\"ALTER TABLESPACE \" & D171 & \" ADD DATAFILE '\" & $K$1 &F171&\".dbf' SIZE 30700M;\"","v":"ALTER TABLESPACE SOIT_D08_A001 ADD DATAFILE '/data/soit/SOIT_D08_A001_002.dbf' SIZE 30700M;"}]
[null,null,"신호최적화-실시간 시뮬레이션 집계-대기행렬","SOIT_D08_T003","001","SOIT_D08_T003_001","30700M",null,null,{"$f":"\"CREATE TABLESPACE \"&D172&\" DATAFILE '\" & $K$1 & F172 & \".dbf' SIZE \"&G172&\" AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE SOIT_D08_T003 DATAFILE '/data/soit/SOIT_D08_T003_001.dbf' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"SOIT_D08_T003","002","SOIT_D08_T003_002","30700M",null,null,{"$f":"\"ALTER TABLESPACE \" & D173 & \" ADD DATAFILE '\" & $K$1 &F173&\".dbf' SIZE 30700M;\"","v":"ALTER TABLESPACE SOIT_D08_T003 ADD DATAFILE '/data/soit/SOIT_D08_T003_002.dbf' SIZE 30700M;"}]
[null,null,null,"SOIT_D08_T003","003","SOIT_D08_T003_003","30700M",null,"2023-02-22",{"$f":"\"ALTER TABLESPACE \" & D174 & \" ADD DATAFILE '\" & $K$1 &F174&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_D08_T003 ADD DATAFILE '/data/soit/SOIT_D08_T003_003.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_D08_T003","004","SOIT_D08_T003_004","30700M",null,"2023-02-22",{"$f":"\"'\"&$K$1&F175&\".dbf' SIZE \"& G175 &\";\"","v":"'/data/soit/SOIT_D08_T003_004.dbf' SIZE 30700M;"}]
[null,null,null,"SOIT_D08_T003","005","SOIT_D08_T003_005","30700M",null,"2023-02-28",{"$f":"\"ALTER TABLESPACE \" & D176 & \" ADD DATAFILE '\" & $K$1 &F176&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_D08_T003 ADD DATAFILE '/data/soit/SOIT_D08_T003_005.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_D08_T003","006","SOIT_D08_T003_006","30700M",null,"2023-02-28",{"$f":"\"'\"&$K$1&F177&\".dbf' SIZE \"& G177 &\";\"","v":"'/data/soit/SOIT_D08_T003_006.dbf' SIZE 30700M;"}]
[]
[null,"INDEX","신호최적화-실시간 시뮬레이션 집계","SOIT_I08_T001","001",{"$f":"D179&\"_\"&E179","v":"SOIT_I08_T001_001"},"30700M",null,null,{"$f":"\"CREATE TABLESPACE \"&D179&\" DATAFILE '\" & $K$1 & F179 & \".dbf' SIZE \"&G179&\" AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE SOIT_I08_T001 DATAFILE '/data/soit/SOIT_I08_T001_001.dbf' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"SOIT_I08_T001","002","SOIT_I08_T001_002","30700M",null,null,{"$f":"\"ALTER TABLESPACE \" & D180 & \" ADD DATAFILE '\" & $K$1 &F180&\".dbf' SIZE 30700M;\"","v":"ALTER TABLESPACE SOIT_I08_T001 ADD DATAFILE '/data/soit/SOIT_I08_T001_002.dbf' SIZE 30700M;"}]
[null,null,null,"SOIT_I08_T001","003","SOIT_I08_T001_003","30700M",null,null,{"$f":"\"ALTER TABLESPACE \" & D181 & \" ADD DATAFILE '\" & $K$1 &F181&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_I08_T001 ADD DATAFILE '/data/soit/SOIT_I08_T001_003.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_I08_T001","004","SOIT_I08_T001_004","30700M",null,null,{"$f":"\"'\"&$K$1&F182&\".dbf' SIZE \"& G182 &\";\"","v":"'/data/soit/SOIT_I08_T001_004.dbf' SIZE 30700M;"}]
[null,null,null,"SOIT_I08_T001","005","SOIT_I08_T001_005","30700M",null,null,{"$f":"\"ALTER TABLESPACE \" & D183 & \" ADD DATAFILE '\" & $K$1 &F183&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_I08_T001 ADD DATAFILE '/data/soit/SOIT_I08_T001_005.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_I08_T001","006","SOIT_I08_T001_006","30700M",null,null,{"$f":"\"'\"&$K$1&F184&\".dbf' SIZE \"& G184 &\";\"","v":"'/data/soit/SOIT_I08_T001_006.dbf' SIZE 30700M;"}]
[null,null,null,"SOIT_I08_T001","007","SOIT_I08_T001_007","30700M",null,"2023-03-01",{"$f":"\"ALTER TABLESPACE \" & D185 & \" ADD DATAFILE '\" & $K$1 &F185&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_I08_T001 ADD DATAFILE '/data/soit/SOIT_I08_T001_007.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_I08_T001","008","SOIT_I08_T001_008","30700M",null,"2023-03-01",{"$f":"\"'\"&$K$1&F186&\".dbf' SIZE \"& G186 &\";\"","v":"'/data/soit/SOIT_I08_T001_008.dbf' SIZE 30700M;"}]
[null,null,null,"SOIT_I08_T001","009","SOIT_I08_T001_009","30700M",null,"2023-03-06",{"$f":"\"ALTER TABLESPACE \" & D187 & \" ADD DATAFILE '\" & $K$1 &F187&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_I08_T001 ADD DATAFILE '/data/soit/SOIT_I08_T001_009.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_I08_T001","010","SOIT_I08_T001_010","30700M",null,"2023-03-06",{"$f":"\"'\"&$K$1&F188&\".dbf' SIZE \"& G188 &\";\"","v":"'/data/soit/SOIT_I08_T001_010.dbf' SIZE 30700M;"}]
[null,null,null,"SOIT_I08_T001","011","SOIT_I08_T001_011","30700M",null,"2023-03-14",{"$f":"\"ALTER TABLESPACE \" & D189 & \" ADD DATAFILE '\" & $K$1 &F189&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_I08_T001 ADD DATAFILE '/data/soit/SOIT_I08_T001_011.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_I08_T001","012","SOIT_I08_T001_012","30700M",null,"2023-03-14",{"$f":"\"'\"&$K$1&F190&\".dbf' SIZE \"& G190 &\";\"","v":"'/data/soit/SOIT_I08_T001_012.dbf' SIZE 30700M;"}]
[null,null,"신호최적화-배치 시뮬레이션/BI 집계","SOIT_I08_T002","001","SOIT_I08_T002_001","30700M",null,null,{"$f":"\"CREATE TABLESPACE \"&D191&\" DATAFILE '\" & $K$1 & F191 & \".dbf' SIZE \"&G191&\" AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE SOIT_I08_T002 DATAFILE '/data/soit/SOIT_I08_T002_001.dbf' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"SOIT_I08_T002","002","SOIT_I08_T002_002","30700M",null,null,{"$f":"\"ALTER TABLESPACE \" & D192 & \" ADD DATAFILE '\" & $K$1 &F192&\".dbf' SIZE 30700M;\"","v":"ALTER TABLESPACE SOIT_I08_T002 ADD DATAFILE '/data/soit/SOIT_I08_T002_002.dbf' SIZE 30700M;"}]
[null,null,null,"SOIT_I08_T002","003","SOIT_I08_T002_003","30700M",null,"2023-02-28",{"$f":"\"ALTER TABLESPACE \" & D193 & \" ADD DATAFILE '\" & $K$1 &F193&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_I08_T002 ADD DATAFILE '/data/soit/SOIT_I08_T002_003.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_I08_T002","004","SOIT_I08_T002_004","30700M",null,"2023-02-28",{"$f":"\"'\"&$K$1&F194&\".dbf' SIZE \"& G194 &\";\"","v":"'/data/soit/SOIT_I08_T002_004.dbf' SIZE 30700M;"}]
[null,null,null,"SOIT_I08_T002","005","SOIT_I08_T002_005","30700M",null,"2023-03-13",{"$f":"\"ALTER TABLESPACE \" & D195 & \" ADD DATAFILE '\" & $K$1 &F195&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_I08_T002 ADD DATAFILE '/data/soit/SOIT_I08_T002_005.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_I08_T002","006","SOIT_I08_T002_006","30700M",null,"2023-03-13",{"$f":"\"'\"&$K$1&F196&\".dbf' SIZE \"& G196 &\";\"","v":"'/data/soit/SOIT_I08_T002_006.dbf' SIZE 30700M;"}]
[null,null,"신호최적화-최적화분석 ","SOIT_I08_A001","001","SOIT_I08_A001_001","30700M",null,null,{"$f":"\"CREATE TABLESPACE \"&D197&\" DATAFILE '\" & $K$1 & F197 & \".dbf' SIZE \"&G197&\" AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE SOIT_I08_A001 DATAFILE '/data/soit/SOIT_I08_A001_001.dbf' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"SOIT_I08_A001","002","SOIT_I08_A001_002","30700M",null,null,{"$f":"\"ALTER TABLESPACE \" & D198 & \" ADD DATAFILE '\" & $K$1 &F198&\".dbf' SIZE 30700M;\"","v":"ALTER TABLESPACE SOIT_I08_A001 ADD DATAFILE '/data/soit/SOIT_I08_A001_002.dbf' SIZE 30700M;"}]
[null,null,"신호최적화-실시간 시뮬레이션 집계-대기행렬","SOIT_I08_T003","001","SOIT_I08_T003_001","30700M",null,null,{"$f":"\"CREATE TABLESPACE \"&D199&\" DATAFILE '\" & $K$1 & F199 & \".dbf' SIZE \"&G199&\" AUTOEXTEND OFF;\"","v":"CREATE TABLESPACE SOIT_I08_T003 DATAFILE '/data/soit/SOIT_I08_T003_001.dbf' SIZE 30700M AUTOEXTEND OFF;"}]
[null,null,null,"SOIT_I08_T003","002","SOIT_I08_T003_002","30700M",null,null,{"$f":"\"ALTER TABLESPACE \" & D200 & \" ADD DATAFILE '\" & $K$1 &F200&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_I08_T003 ADD DATAFILE '/data/soit/SOIT_I08_T003_002.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_I08_T003","003","SOIT_I08_T003_003","30700M",null,null,{"$f":"\"'\"&$K$1&F201&\".dbf' SIZE \"& G201 &\";\"","v":"'/data/soit/SOIT_I08_T003_003.dbf' SIZE 30700M;"}]
[null,null,null,"SOIT_I08_T003","004","SOIT_I08_T003_004","30700M",null,"2023-02-21",{"$f":"\"ALTER TABLESPACE \" & D202 & \" ADD DATAFILE '\" & $K$1 &F202&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_I08_T003 ADD DATAFILE '/data/soit/SOIT_I08_T003_004.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_I08_T003","005","SOIT_I08_T003_005","30700M",null,"2023-02-21",{"$f":"\"'\"&$K$1&F203&\".dbf' SIZE \"& G203 &\";\"","v":"'/data/soit/SOIT_I08_T003_005.dbf' SIZE 30700M;"}]
[null,null,null,"SOIT_I08_T003","006","SOIT_I08_T003_006","30700M",null,"2023-02-21",{"$f":"\"ALTER TABLESPACE \" & D204 & \" ADD DATAFILE '\" & $K$1 &F204&\".dbf' SIZE 30700M,\"","v":"ALTER TABLESPACE SOIT_I08_T003 ADD DATAFILE '/data/soit/SOIT_I08_T003_006.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_I08_T003","007","SOIT_I08_T003_007","30700M",null,"2023-02-21",{"$f":"\"'\"&$K$1&F205&\".dbf' SIZE \"& G205 &\",\"","v":"'/data/soit/SOIT_I08_T003_007.dbf' SIZE 30700M,"}]
[null,null,null,"SOIT_I08_T003","008","SOIT_I08_T003_008","30700M",null,"2023-02-21","'/data/soit/SOIT_I08_T003_008.dbf' SIZE 30700M,"]
[null,null,null,"SOIT_I08_T003","009","SOIT_I08_T003_009","30700M",null,"2023-02-21","'/data/soit/SOIT_I08_T003_009.dbf' SIZE 30700M,"]
[null,null,null,"SOIT_I08_T003","010","SOIT_I08_T003_010","30700M",null,"2023-02-21",{"$f":"\"'\"&$K$1&F208&\".dbf' SIZE \"& G208 &\";\"","v":"'/data/soit/SOIT_I08_T003_010.dbf' SIZE 30700M;"}]

{"sheet":"변경이력","index":2,"n_rows":7,"n_cols":5,"rows_kept":7,"cut":false,"hidden":false,"merged":[]}
["번호","글로벌브릿지","동인","SUMO","신호시스템"]
[1," - 22.06.09\n - 아래 테이블에 대해 컬럼추가요청에 의해 센터기준으로 물리명 변경해서 전달\n > soitgcamrinfo\n > soitgcamrsttsinfo"," - 22.06.24\n - 우선신호운영교차로 추가 적용"," - 22.06.24 (박산하)\n - 센터(sumo 관련) 시트 → 최적화 결과 신호운영 테이블 추가"," - 22.06.24 (김한빈)\n - BI용 공해차량단속집계 테이블 추가"]
[2," - 22.06.17\n - 아래 테이블에 대해 컬럼추가요청에 의해 센터기준으로 물리명 변경해서 전달\n  > soitgcamrinfo, soitgvhcldtrtstats, soitgturndtrtstats, soitgcamrsttsinfo\n  > 현장카메라방향ID, 오토바이검지수\n - 코드 정보 추가","- 22.07.14\n- 1. 모든 테이블은 insert 형태로 제공함.\n2. insert 형태로 변경됨에 따라 일시 컬럼들 추가\n3. 가능하면 모든 테이블은 volt db 로 전송(동인시스템 확인 필)\n4. tod 구성정보는 기존 테이블 유지하고 별도로 tod plan 정보와 time plan 정보를 추가적으로 제공\n5. 특수일시각제어, 주간시각제어 테이블은 신호 교차로 번호 기준으로 정보를 제공하는 방식으로 변경\n6. 신호교차로상태 테이블에 a,b링 이동류 번호 컬럼 및 시각계획번호, 교차로 현시 운영계획번호 정보를 제공\n7. 신호 교차로 운영이력 테이블에 2010년도에 해당하는 보행이력 정보(보행신호 현시, 보행신호 방향) 정보를 제공"," - 22.06.24 (김한빈)\n - 최적화테이블 질의사항 정리 및 결과 업데이트"]
[3," - 22.06.23\n - realtime_detections 테이블에 차적조회여부 컬럼 추가 \n  -> 유아이 관리용 컬럼, 글로벌에서는 빈 컬럼으로 입력\n - 숫자로 시작되는 컬럼명 수정",null," - 22.07.11 (김한빈)\n - 1차 SUMO테이블 도메인 작업 완료 (네트워크, 신호, 시뮬레이션)"]
[4," - 22.06.30\n - 코드 라고 적혀있는 컬럼들 중 실제 코드가 아닌 컬럼들 용어 변경\n - 테이블 정의서 형태로 데이터 업데이트\n - 트래킹ID -> 추적ID 변경하여 컬럼명 유지\n    종료유닉스시각 -> 컬럼 추가",null," - 22.07.27 (김종성)\n - 신호최적화 부분 테이블 일부 수정(tb_program 테이블 정규화)"]
[5," - 22.07.04\n - 돌발이벤트 테이블 처리유닉스시각 컬럼 추가\n - 보행자 검지정보 pk 추가"]
[6,"- 22.07.15\n- 코드값 추가\n- 차로정보 : 회전유형코드를 회전유형명 으로 변경"]

{"sheet":"DB사용자 계정","index":3,"n_rows":10,"n_cols":10,"rows_kept":10,"cut":false,"hidden":false,"merged":[[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,4,0,8],[0,9,1,9]]}
[null,"DB서버명","사용자명","대상 DB","부여된 권한",{"$nulls":4},"비고"]
[{"$nulls":4},"관리자","테이블참조","테이블수정","함수/프로시저 실행","함수/프로시저 수정"]
[null,"통합운영","SOIT","IOMS","X","O(일부)","O(일부)","X","X","신호최적화에서 사용자 및 메뉴권한관리 위하여 통합운영 접속용 계정"]
[]
[]
[null,"빅데이터","iomsu01","SOIT","X","O(전체)","X","O","X","상황판에서 신호최적화 및 스마트교차로 데이터 접근 위한 계정"]
[null,"빅데이터","globalu02","SOIT","X","O(일부)","O(일부)","X","X","글로벌브릿지 스마트교차로 테이블 접근 계정"]
[null,"빅데이터","donginu03","SOIT","X","O(일부)","O(일부)","X","X","동인시스템에서 교차로신호상태 및 긴급차량 데이터 제공 위한 계정"]
[null,"빅데이터","TPSS","SOIT","O","O(전체)","X","O","X","정책지원시스템에서 신호최적화 및 스마트교차로 데이터 접근 위한 계정"]
[null,"빅데이터","itcoresu05","SOIT","X","O(일부)","X","X","X","아이티코어스에서 스마트교차로 데이터 조회 위한 계정"]

{"sheet":"글로벌브릿지(스마트교차로)","index":4,"n_rows":344,"n_cols":44,"rows_kept":344,"cut":false,"hidden":false,"merged":[[3,25,3,34],[3,35,3,40],[1,1,1,2],[1,3,1,10],[2,1,2,2],[2,3,2,10],[3,1,3,2],[3,3,3,10],[3,16,3,21],[14,1,14,2],[14,3,14,10],[15,1,15,2],[15,3,15,10],[16,1,16,2],[16,3,16,10],[33,3,33,10],[33,1,33,2],[34,1,34,2],[34,3,34,10],[35,1,35,2],[43,1,43,2],[44,1,44,2],[45,1,45,2],[52,1,52,2],[93,1,93,2],[102,1,102,2],[103,1,103,2],[104,1,104,2],[53,1,53,2],[54,1,54,2],[76,1,76,2],[77,1,77,2],[78,1,78,2],[91,1,91,2],[92,1,92,2],[198,3,198,10],[245,3,245,10],[102,3,102,10],[103,3,103,10],[104,3,104,10],[129,3,129,10],[130,3,130,10],[143,3,143,10],[144,3,144,10],[145,3,145,10],[161,3,161,10],[128,3,128,10],[293,1,293,2],[294,1,294,2],[246,3,246,10],[276,14,290,14],[293,3,293,10],[294,3,294,10],[295,3,295,10],[297,14,307,14],[215,3,215,10],[216,3,216,10],[217,3,217,10],[229,3,229,10],[230,3,230,10],[231,3,231,10],[244,3,244,10],[295,1,295,2],[215,1,215,2],[216,1,216,2],[217,1,217,2],[229,1,229,2],[230,1,230,2],[231,1,231,2],[272,3,272,10],[273,3,273,10],[35,3,35,10],[43,3,43,10],[44,3,44,10],[45,3,45,10],[52,3,52,10],[53,3,53,10],[54,3,54,10],[76,3,76,10],[77,3,77,10],[78,3,78,10],[91,3,91,10],[92,3,92,10],[93,3,93,10],[114,1,114,2],[114,3,114,10],[115,1,115,2],[115,3,115,10],[116,1,116,2],[116,3,116,10],[128,1,128,2],[129,1,129,2],[130,1,130,2],[143,1,143,2],[144,1,144,2],[145,1,145,2],[161,1,161,2],[261,1,261,2],[261,3,261,10],[162,1,162,2],[163,1,163,2],[181,1,181,2],[182,1,182,2],[183,1,183,2],[196,1,196,2],[197,1,197,2],[198,1,198,2],[162,3,162,10],[163,3,163,10],[181,3,181,10],[182,3,182,10],[183,3,183,10],[196,3,196,10],[197,3,197,10],[274,3,274,10],[244,1,244,2],[245,1,245,2],[246,1,246,2],[259,1,259,2],[259,3,259,10],[260,1,260,2],[260,3,260,10],[272,1,272,2],[273,1,273,2],[274,1,274,2]]}
[]
[null,"테이블명",null,"soitgintsinfo"]
[null,"테이블설명",null,"교차로 정보"]
[null,"참고사항",{"$nulls":14},"VOLT DDL",{"$nulls":8},"TIBERO DDL",{"$nulls":9},"COMMENTS"]
[null,"NO","PK","논리명","물리명","VoltDB 타입","Tibero 타입","길이","NULL","기본값","비고",null,"형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE","soitgintsinfo",null," IS ",{"$f":"\"'\"&D3&\"'\"","v":"'교차로 정보'"},";"]
[null,1,"PK","현장 교차로 ID","spot_ints_id","SMALLINT","NUMBER",5,"N",0,"현장 교차로 ID",null,"NUMBER(5)","SMALLINT","NUMBER(5)",null,"CREATE TABLE ",{"$f":"D2&\" (\"","v":"soitgintsinfo ("},{"$f":"E6&\" \"","v":"spot_ints_id "},{"$f":"N6&\" \"","v":"SMALLINT "},{"$f":"IF(I6=\"N\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(C6=\"PK\", C6=\"PK/FK\"), E6, \"\")","v":"spot_ints_id"},"));","CREATE TABLE ",{"$f":"D2&\" (\"","v":"soitgintsinfo ("},{"$f":"E6&\" \"","v":"spot_ints_id "},{"$f":"O6&\" \"","v":"NUMBER(5) "},{"$f":"IF(I6=\"N\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","CONSTRAINT ",{"$f":"\"PK_\"&D2&\" PRIMARY KEY (\"","v":"PK_soitgintsinfo PRIMARY KEY ("},{"$f":"IF(OR(C6=\"PK\", C6=\"PK/FK\"), E6, \"\")","v":"spot_ints_id"},{"$f":"\") using index tablespace \" & AA14 & \") TABLESPACE \" & Z14&\";\"","v":") using index tablespace SOIT_I08_G001) TABLESPACE SOIT_D08_G001;"},"COMMENT ON COLUMN  ","soitgintsinfo.",{"$f":"E6","v":"spot_ints_id"}," IS ",{"$f":"\"'\"&K6&\"'\"","v":"'현장 교차로 ID'"},";"]
[null,2,null,"교차로명","ints_nm","VARCHAR","VARCHAR2",40,"N",null,"교차로명",null,"VARCHAR2(50)","VARCHAR(50)","VARCHAR2(50)",null,null,null,"ints_nm ","VARCHAR(50) ","NOT NULL",",",null,"",null,null,null,"ints_nm ","VARCHAR2(50) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitgintsinfo.","ints_nm"," IS ","'교차로명'",";"]
[null,3,null,"시군구명","sgg_nm","VARCHAR","VARCHAR2",40,"N",null,"시군구명",null,"VARCHAR2(40)","VARCHAR(40)","VARCHAR2(40)",null,null,null,"sgg_nm ","VARCHAR(40) ","NOT NULL",",",null,"",null,null,null,"sgg_nm ","VARCHAR2(40) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitgintsinfo.","sgg_nm"," IS ","'시군구명'",";"]
[null,4,null,"행정동명","dong_nm","VARCHAR","VARCHAR2",40,"N",null,"행정동명",null,"VARCHAR2(40)","VARCHAR(40)","VARCHAR2(40)",null,null,null,"dong_nm ","VARCHAR(40) ","NOT NULL",",",null,"",null,null,null,"dong_nm ","VARCHAR2(40) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitgintsinfo.","dong_nm"," IS ","'행정동명'",";"]
[null,5,null,"교차로활성여부","ints_vtlt_yn","VARCHAR","VARCHAR2",1,"N","N","교차로활성여부",null,"CHAR(1)","VARCHAR(1)","VARCHAR2(1)",null,null,null,"ints_vtlt_yn ","VARCHAR(1) ","NOT NULL",",",null,"",null,null,null,"ints_vtlt_yn ","VARCHAR2(1) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitgintsinfo.","ints_vtlt_yn"," IS ","'교차로활성여부'",";"]
[null,6,null,"함체교체여부","encl_rplc_yn","VARCHAR","CHAR",1,"N","N","함체교체여부(Y:교체, N:미교체)",null,"CHAR(1)","VARCHAR(1)","VARCHAR2(1)",null,null,null,"encl_rplc_yn ","VARCHAR(1) ","NOT NULL",",",{"$nulls":5},"encl_rplc_yn ","VARCHAR2(1) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitgintsinfo.","encl_rplc_yn"," IS ","'함체교체여부(Y:교체, N:미교체)'",";"]
[null,7,null,"비고","rmrk","VARCHAR","VARCHAR2",2000,"Y",null,"비고",null,"VARCHAR2(2000)","VARCHAR(2000)","VARCHAR2(2000)",null,null,null,"rmrk ","VARCHAR(2000) ","",",",null,{"$f":"IF(OR(C12=\"PK\", C12=\"PK/FK\"), E12, \"\")","v":""},null,null,null,"rmrk ","VARCHAR2(2000) ","",",",null,null,{"$f":"IF(OR(C12=\"PK\", C12=\"PK/FK\"), E12, \"\")","v":""},null,"COMMENT ON COLUMN ","soitgintsinfo.","rmrk"," IS ","'비고'",";"]
[{"$nulls":18},{"$f":"CONCATENATE(W6:Y13)","v":{"$error":"#VALUE!"}},{"$f":"M14&\" \"","v":" "},{"$f":"IF(J14=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},null,null,{"$f":"IF(OR(I14=\"PK\", I14=\"PK/FK\"), K14, \"\")","v":""},null,null,null,{"$f":"CONCATENATE(AF6:AI13)","v":{"$error":"#VALUE!"}},{"$f":"N14&\" \"","v":" "},{"$f":"IF(J14=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},null,null,null,"",{"$nulls":9},{"$f":"IF(LEFT(AB13, 13) = \"CONSTRAINT PK\", AB13, \"\")","v":{"$error":"#VALUE!"}}]
[{"$nulls":25},"SOIT_D08_G001","SOIT_I08_G001",{"$nulls":16},""]
[null,"테이블명",null,"soitgcamrinfo",{"$nulls":39},""]
[null,"테이블설명",null,"현장서버 정보",{"$nulls":39},""]
[null,"참고사항",{"$nulls":41},""]
[null,"NO","PK","논리명","물리명","VoltDB 타입","Tibero 타입","길이","NULL","기본값","비고",null,"형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE","soitgcamrinfo",null," IS ",{"$f":"\"'\"&D16&\"'\"","v":"'현장서버 정보'"},";",null,null,""]
[null,1,"PK","현장교차로ID","spot_ints_id","SMALLINT","NUMBER",5,"N",0,"현장교차로ID",null,"NUMBER(5)","SMALLINT","NUMBER(5)",null,"CREATE TABLE ",{"$f":"D15&\" (\"","v":"soitgcamrinfo ("},{"$f":"E19&\" \"","v":"spot_ints_id "},{"$f":"N19&\" \"","v":"SMALLINT "},{"$f":"IF(I19=\"N\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(C19=\"PK\", C19=\"PK/FK\"), E19, \"\")","v":"spot_ints_id"},{"$f":"IF(OR(C20=\"PK\", C20=\"PK/FK\"), \",\", \"\")","v":""},"CREATE TABLE ",{"$f":"D15&\" (\"","v":"soitgcamrinfo ("},{"$f":"E19&\" \"","v":"spot_ints_id "},{"$f":"O19&\" \"","v":"NUMBER(5) "},{"$f":"IF(I19=\"N\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","CONSTRAINT ",{"$f":"\"PK_\"&D15&\" PRIMARY KEY (\"","v":"PK_soitgcamrinfo PRIMARY KEY ("},{"$f":"IF(OR(C19=\"PK\", C19=\"PK/FK\"), E19, \"\")","v":"spot_ints_id"},{"$f":"IF(OR(C20=\"PK\", C20=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitgcamrinfo.",{"$f":"E19","v":"spot_ints_id"}," IS ",{"$f":"\"'\"&K19&\"'\"","v":"'현장교차로ID'"},";",null,null,""]
[null,2,"UK","현장카메라위치ID","spot_camr_locn_id","VARCHAR","VARCHAR2",64,"N",null,"현장카메라위치ID",null,"VARCHAR2(64)","VARCHAR(64)","VARCHAR2(64)",null,null,null,"spot_camr_locn_id ","VARCHAR(64) ","NOT NULL",",",null,"",",",null,null,"spot_camr_locn_id ","VARCHAR2(64) ","NOT NULL",",",null,null,"",",","COMMENT ON COLUMN ","soitgcamrinfo.","spot_camr_locn_id"," IS ","'현장카메라위치ID'",";",null,null,""]
[null,3,"PK","현장카메라ID","spot_camr_id","VARCHAR","VARCHAR2",10,"N",null,"현장카메라ID(교차로 ID + \"_\" + 이동류번호)",null,"VARCHAR2(10)","VARCHAR(10)","VARCHAR2(10)",null,null,null,"spot_camr_id ","VARCHAR(10) ","NOT NULL",",",null,"spot_camr_id","",null,null,"spot_camr_id ","VARCHAR2(10) ","NOT NULL",",",null,null,"spot_camr_id","","COMMENT ON COLUMN ","soitgcamrinfo.","spot_camr_id"," IS ","'현장카메라ID(교차로 ID + \"_\" + 이동류번호)'",";",null,null,""]
[null,4,null,"현장서버명","spot_srvr_nm","VARCHAR","VARCHAR2",256,"Y",null,"현장서버명",null,"VARCHAR2(256)","VARCHAR(256)","VARCHAR2(256)",null,null,null,"spot_srvr_nm ","VARCHAR(256) ","",",",null,"","",null,null,"spot_srvr_nm ","VARCHAR2(256) ","",",",null,null,"","","COMMENT ON COLUMN ","soitgcamrinfo.","spot_srvr_nm"," IS ","'현장서버명'",";",null,null,""]
[null,5,null,"2K카메라IP","camr_2k_ip","VARCHAR","VARCHAR2",15,"Y",null,"2K카메라IP",null,"VARCHAR2(15)","VARCHAR(15)","VARCHAR2(15)",null,null,null,"camr_2k_ip ","VARCHAR(15) ","",",",null,"","",null,null,"camr_2k_ip ","VARCHAR2(15) ","",",",null,null,"","","COMMENT ON COLUMN ","soitgcamrinfo.","camr_2k_ip"," IS ","'2K카메라IP'",";",null,null,""]
[null,6,null,"2K엣지시스템IP","edge_sys_2k_ip","VARCHAR","VARCHAR2",15,"Y",null,"2K엣지시스템IP",null,"VARCHAR2(15)","VARCHAR(15)","VARCHAR2(15)",null,null,null,"edge_sys_2k_ip ","VARCHAR(15) ","",",",null,"","",null,null,"edge_sys_2k_ip ","VARCHAR2(15) ","",",",null,null,"","","COMMENT ON COLUMN ","soitgcamrinfo.","edge_sys_2k_ip"," IS ","'2K엣지시스템IP'",";",null,null,""]
[null,7,null,"4K카메라IP","camr_4k_ip","VARCHAR","VARCHAR2",15,"Y",null,"4K카메라IP",null,"VARCHAR2(15)","VARCHAR(15)","VARCHAR2(15)",null,null,null,"camr_4k_ip ","VARCHAR(15) ","",",",null,"","",null,null,"camr_4k_ip ","VARCHAR2(15) ","",",",null,null,"","","COMMENT ON COLUMN ","soitgcamrinfo.","camr_4k_ip"," IS ","'4K카메라IP'",";",null,null,""]
[null,8,null,"4K엣지시스템IP","edge_sys_4k_ip","VARCHAR","VARCHAR2",15,"Y",null,"4K엣지시스템IP",null,"VARCHAR2(15)","VARCHAR(15)","VARCHAR2(15)",null,null,null,"edge_sys_4k_ip ","VARCHAR(15) ","",",",null,"","",null,null,"edge_sys_4k_ip ","VARCHAR2(15) ","",",",null,null,"","","COMMENT ON COLUMN ","soitgcamrinfo.","edge_sys_4k_ip"," IS ","'4K엣지시스템IP'",";",null,null,""]
[null,9,null,"검지거리","dttn_dstn","DECIMAL","NUMBER","19,9","Y",0,"검지거리(미터)",null,"NUMBER(19,9)","DECIMAL(19,9)","NUMBER(19,9)",null,null,null,"dttn_dstn ","DECIMAL(19,9) ","",",",null,"",",",null,null,"dttn_dstn ","NUMBER(19,9) ","",",",null,null,"",",","COMMENT ON COLUMN ","soitgcamrinfo.","dttn_dstn"," IS ","'검지거리(미터)'",";",null,null,""]
[null,10,"PK","설치위치번호","instl_locn_no","VARCHAR","VARCHAR2",2,"N",null,"설치위치번호",null,"CHAR(2)","VARCHAR(2)","VARCHAR2(2)",null,null,null,"instl_locn_no ","VARCHAR(2) ","NOT NULL",",",null,"instl_locn_no","));",null,null,"instl_locn_no ","VARCHAR2(2) ","NOT NULL",",",null,null,"instl_locn_no",{"$f":"\") using index tablespace \" &AG33  & \") TABLESPACE \" & AF33&\";\"","v":") using index tablespace SOIT_I08_G001) TABLESPACE SOIT_D08_G001;"},"COMMENT ON COLUMN ","soitgcamrinfo.","instl_locn_no"," IS ","'설치위치번호'",";",null,null,""]
[null,11,null,"관리일련번호","mng_sn","VARCHAR","VARCHAR2",50,"Y",null,"관리일련번호",null,"VARCHAR2(50)","VARCHAR(50)","VARCHAR2(50)",null,null,null,"mng_sn ","VARCHAR(50) ","",",",null,"",null,null,null,"mng_sn ","VARCHAR2(50) ","",",",null,null,"",{"$f":"IF(OR(C30=\"PK\", C30=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitgcamrinfo.","mng_sn"," IS ","'관리일련번호'",";",null,null,""]
[null,12,null,"ECU정보전송여부","ecu_info_trsm_yn","VARCHAR","VARCHAR2",1,"N","N","전송여부(014)","Y:전송, N:미전송","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",null,null,null,"ecu_info_trsm_yn ","VARCHAR(1) ","NOT NULL",",",null,"",null,null,null,"ecu_info_trsm_yn ","VARCHAR2(1) ","NOT NULL",",",null,null,"","","COMMENT ON COLUMN ","soitgcamrinfo.","ecu_info_trsm_yn"," IS ","'전송여부(014)'",";",null,null,""]
[null,13,null,"카메라활성여부","camr_vtlt_yn","VARCHAR","VARCHAR2",1,"N","Y","카메라활성여부",null,"CHAR(1)","VARCHAR(1)","VARCHAR2(1)",null,null,null,"camr_vtlt_yn ","VARCHAR(1) ","NOT NULL",",",null,"",null,null,null,"camr_vtlt_yn ","VARCHAR2(1) ","NOT NULL",",",null,null,"",{"$f":"IF(OR(M32=\"PK\", M32=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitgcamrinfo.","camr_vtlt_yn"," IS ","'카메라활성여부'",";",null,null,""]
[{"$nulls":18},{"$f":"CONCATENATE(W19:Y31)","v":{"$error":"#VALUE!"}},{"$f":"M26&\" \"","v":"VARCHAR2(15) "},null,null,null,"",null,null,null,{"$f":"CONCATENATE(AF19:AI32)","v":{"$error":"#VALUE!"}},{"$nulls":5},"",{"$nulls":9},{"$error":"#VALUE!"}]
[{"$nulls":31},"SOIT_D08_G001","SOIT_I08_G001",{"$nulls":10},""]
[null,"테이블명",null,"soitglaneinfo",{"$nulls":39},""]
[null,"테이블설명",null,"차로정보",{"$nulls":39},""]
[null,"참고사항",{"$nulls":41},""]
[null,"NO","PK","논리명","물리명","VoltDB 타입","Tibero 타입","길이","NULL","기본값","비고",null,"형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE","soitglaneinfo",null," IS ",{"$f":"\"'\"&D35&\"'\"","v":"'차로정보'"},";",null,null,""]
[null,1,"PK","현장카메라ID","spot_camr_id","VARCHAR","VARCHAR2",10,"N",null,"현장카메라ID",null,"VARCHAR2(10)","VARCHAR(10)","VARCHAR2(10)",null,"CREATE TABLE ",{"$f":"D34&\" (\"","v":"soitglaneinfo ("},{"$f":"E38&\" \"","v":"spot_camr_id "},{"$f":"N38&\" \"","v":"VARCHAR(10) "},{"$f":"IF(I38=\"N\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(C38=\"PK\", C38=\"PK/FK\"), E38, \"\")","v":"spot_camr_id"},{"$f":"IF(OR(C39=\"PK\", C39=\"PK/FK\"), \",\", \"\")","v":","},"CREATE TABLE ",{"$f":"D34&\" (\"","v":"soitglaneinfo ("},{"$f":"E38&\" \"","v":"spot_camr_id "},{"$f":"O38&\" \"","v":"VARCHAR2(10) "},{"$f":"IF(I38=\"N\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","CONSTRAINT ",{"$f":"\"PK_\"&D34&\" PRIMARY KEY (\"","v":"PK_soitglaneinfo PRIMARY KEY ("},{"$f":"IF(OR(C38=\"PK\", C38=\"PK/FK\"), E38, \"\")","v":"spot_camr_id"},{"$f":"IF(OR(C39=\"PK\", C39=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ","soitglaneinfo.",{"$f":"E38","v":"spot_camr_id"}," IS ",{"$f":"\"'\"&K38&\"'\"","v":"'현장카메라ID'"},";",null,null,""]
[null,2,"PK","차로번호","lane_no","TINYINT","NUMBER",2,"N",1,"차로번호",null,"NUMBER(2)","TINYINT","NUMBER(2)",null,null,null,"lane_no ","TINYINT ","NOT NULL",",",null,"lane_no","));",null,null,"lane_no ","NUMBER(2) ","NOT NULL",",",null,null,"lane_no",{"$f":"\") using index tablespace \" &AG43  & \") TABLESPACE \" & AF43&\";\"","v":") using index tablespace SOIT_I08_G001) TABLESPACE SOIT_D08_G001;"},"COMMENT ON COLUMN ","soitglaneinfo.","lane_no"," IS ","'차로번호'",";",null,null,""]
[null,3,null,"회전유형명","turn_type_nm","VARCHAR","VARCHAR2",30,"Y",null,"회전유형명",null,"VARCHAR2(30)","VARCHAR(30)","VARCHAR2(30)",null,null,null,"turn_type_nm ","VARCHAR(30) ","",",",null,"",{"$f":"IF(OR(C41=\"PK\", C41=\"PK/FK\"), \",\", \"\")","v":""},null,null,"turn_type_nm ","VARCHAR2(30) ","",",",null,null,"",{"$f":"IF(OR(C41=\"PK\", C41=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitglaneinfo.","turn_type_nm"," IS ","'회전유형명'",";",null,null,""]
[null,4,null,"차량번호4K검지여부","vhno_4k_dttn_yn","VARCHAR","VARCHAR2",1,"N","N","검지여부(021)","Y:검지, N:미검지","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",null,null,null,"vhno_4k_dttn_yn ","VARCHAR(1) ","NOT NULL",",",null,"","",null,null,"vhno_4k_dttn_yn ","VARCHAR2(1) ","NOT NULL",",",null,null,"","","COMMENT ON COLUMN ","soitglaneinfo.","vhno_4k_dttn_yn"," IS ","'검지여부(021)'",";",null,null,""]
[{"$nulls":18},{"$f":"CONCATENATE(W38:Y41)","v":{"$error":"#VALUE!"}},{"$nulls":4},"","",null,null,{"$f":"CONCATENATE(AF38:AI42)","v":{"$error":"#VALUE!"}},{"$nulls":15},{"$error":"#VALUE!"}]
[{"$nulls":23},"","",{"$nulls":6},"SOIT_D08_G001","SOIT_I08_G001",{"$nulls":10},""]
[null,"테이블명",null,"soitgspotcdinfo",{"$nulls":19},"","",{"$nulls":18},""]
[null,"테이블설명",null,"코드정보",{"$nulls":19},"","",{"$nulls":18},""]
[null,"참고사항",{"$nulls":41},""]
[null,"NO","PK","논리명","물리명","VoltDB 타입","Tibero 타입","길이","NULL","기본값","비고",null,"형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE","soitgspotcdinfo",null," IS ",{"$f":"\"'\"&D45&\"'\"","v":"'코드정보'"},";",null,null,""]
[null,1,"PK","코드유형ID","cd_type_id","VARCHAR","VARCHAR2",20,"N",null,"코드유형명",null,"VARCHAR2(10)","VARCHAR(10)","VARCHAR(10)",null,"CREATE TABLE ",{"$f":"D44&\" (\"","v":"soitgspotcdinfo ("},{"$f":"E48&\" \"","v":"cd_type_id "},{"$f":"N48&\" \"","v":"VARCHAR(10) "},{"$f":"IF(I48=\"N\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(C48=\"PK\", C48=\"PK/FK\"), E48, \"\")","v":"cd_type_id"},{"$f":"IF(OR(C49=\"PK\", C49=\"PK/FK\"), \",\", \"\")","v":","},"CREATE TABLE ",{"$f":"D44&\" (\"","v":"soitgspotcdinfo ("},{"$f":"E48&\" \"","v":"cd_type_id "},{"$f":"O48&\" \"","v":"VARCHAR(10) "},{"$f":"IF(I48=\"N\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","CONSTRAINT ",{"$f":"\"PK_\"&D44&\" PRIMARY KEY (\"","v":"PK_soitgspotcdinfo PRIMARY KEY ("},{"$f":"IF(OR(C48=\"PK\", C48=\"PK/FK\"), E48, \"\")","v":"cd_type_id"},{"$f":"IF(OR(C49=\"PK\", C49=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ","soitgspotcdinfo.",{"$f":"E48","v":"cd_type_id"}," IS ",{"$f":"\"'\"&K48&\"'\"","v":"'코드유형명'"},";",null,null,""]
[null,2,"PK","코드유형명","cd_type_nm","VARCHAR","VARCHAR2",10,"N",null,"코드이름",null,"VARCHAR2(20)","VARCHAR(20)","VARCHAR(20)",null,null,null,"cd_type_nm ","VARCHAR(20) ","NOT NULL",",",null,"cd_type_nm","));",null,null,"cd_type_nm ","VARCHAR(20) ","NOT NULL",",",null,null,"cd_type_nm",{"$f":"\") using index tablespace \" &AG52  & \") TABLESPACE \" &AF52&\";\"","v":") using index tablespace SOIT_I08_G001) TABLESPACE SOIT_D08_G001;"},"COMMENT ON COLUMN ","soitgspotcdinfo.","cd_type_nm"," IS ","'코드이름'",";",null,null,""]
[null,3,null,"비고","rmrk","VARCHAR","VARCHAR2",2000,"Y",null,"비고",null,"VARCHAR2(2000)","VARCHAR(2000)","VARCHAR(2000)",null,null,null,"rmrk ","VARCHAR(2000) ","",",",{"$nulls":5},"rmrk ","VARCHAR(2000) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitgspotcdinfo.","rmrk"," IS ","'비고'",";",null,null,""]
[{"$nulls":18},{"$f":"CONCATENATE(W48:Y50)","v":{"$error":"#VALUE!"}}," ",{"$nulls":7},{"$f":"CONCATENATE(AF48:AI49)","v":{"$error":"#VALUE!"}}," ","",{"$nulls":13},{"$error":"#VALUE!"}]
[{"$nulls":31},"SOIT_D08_G001","SOIT_I08_G001",{"$nulls":10},""]
[null,"테이블명",null,"soitgrtmdtinfo",{"$nulls":7},1440,{"$nulls":31},""]
[null,"테이블설명",null,"실시간 차량검지 정보",{"$nulls":39},""]
[null,"참고사항",{"$nulls":41},""]
[null,"NO","PK","논리명","물리명","VoltDB 타입","Tibero 타입","길이","NULL","기본값","비고",null,"형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE","soitgrtmdtinfo",null," IS ",{"$f":"\"'\"&D54&\"'\"","v":"'실시간 차량검지 정보'"},";",null,null,""]
[null,1,"PK","현장카메라ID","spot_camr_id","VARCHAR","VARCHAR2",10,"N",null,"현장카메라ID",null,"VARCHAR2(10)","VARCHAR(10)","VARCHAR2(10)",null,"CREATE TABLE ",{"$f":"D53&\" (\"","v":"soitgrtmdtinfo ("},{"$f":"E57&\" \"","v":"spot_camr_id "},{"$f":"N57&\" \"","v":"VARCHAR(10) "},{"$f":"IF(I57=\"N\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(C57=\"PK\", C57=\"PK/FK\"), E57, \"\")","v":"spot_camr_id"},{"$f":"IF(OR(C58=\"PK\", C58=\"PK/FK\"), \",\", \"\")","v":","},"CREATE TABLE ",{"$f":"D53&\" (\"","v":"soitgrtmdtinfo ("},{"$f":"E57&\" \"","v":"spot_camr_id "},{"$f":"O57&\" \"","v":"VARCHAR2(10) "},{"$f":"IF(I57=\"N\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(C57=\"PK\", C57=\"PK/FK\"), E57, \"\")","v":"spot_camr_id"},{"$f":"IF(OR(C58=\"PK\", C58=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ","soitgrtmdtinfo.",{"$f":"E57","v":"spot_camr_id"}," IS ",{"$f":"\"'\"&K57&\"'\"","v":"'현장카메라ID'"},";",null,null,""]
[null,2,"PK","차종코드","kncr_cd","VARCHAR","VARCHAR2",10,"N",null,"차종(008)"," LBUS:대형버스, LTRUCK:대형트럭(4.5T이상), MBUS:미니버스,\nMOTOR:오토바이, MTRUCK:트럭(4.5T미만), PCAR:승용차 ","CHAR(10)","VARCHAR(10)","VARCHAR2(10)",null,null,null,"kncr_cd ","VARCHAR(10) ","NOT NULL",",",null,"kncr_cd",",",null,null,"kncr_cd ","VARCHAR2(10) ","NOT NULL",",",null,null,"kncr_cd",",","COMMENT ON COLUMN ","soitgrtmdtinfo.","kncr_cd"," IS ","'차종(008)'",";",null,null,""]
[null,3,"PK","차로번호","lane_no","TINYINT","NUMBER",2,"N","1","차로번호",null,"NUMBER(2)","TINYINT","NUMBER(2)",null,null,null,"lane_no ","TINYINT ","NOT NULL",",",null,"lane_no",",",null,null,"lane_no ","NUMBER(2) ","NOT NULL",",",null,null,"lane_no",",","COMMENT ON COLUMN ","soitgrtmdtinfo.","lane_no"," IS ","'차로번호'",";",null,null,""]
[null,4,"PK","회전유형코드","turn_type_cd","VARCHAR","VARCHAR2",10,"N",null,"회전유형(700)"," 11:직진, 21:작은좌회전, 22:큰좌회전, 31:작은우회전, 32:큰우회전, 41:유턴","CHAR(10)","VARCHAR(10)","VARCHAR2(10)",null,null,null,"turn_type_cd ","VARCHAR(10) ","NOT NULL",",",null,"turn_type_cd",",",null,null,"turn_type_cd ","VARCHAR2(10) ","NOT NULL",",",null,null,"turn_type_cd",",","COMMENT ON COLUMN ","soitgrtmdtinfo.","turn_type_cd"," IS ","'회전유형(700)'",";",null,null,""]
[null,5,"PK","회전검지유닉스시각","turn_dttn_unix_tm","INT","NUMBER",10,"N","0","회전검지유닉스시각",null,"NUMBER(10)","INT","NUMBER(10)",null,null,null,"turn_dttn_unix_tm ","INT ","NOT NULL",",",null,"turn_dttn_unix_tm","",null,null,"turn_dttn_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"turn_dttn_unix_tm","","COMMENT ON COLUMN ","soitgrtmdtinfo.","turn_dttn_unix_tm"," IS ","'회전검지유닉스시각'",";",null,null,""]
[null,6,null,"회전검지속도","turn_dttn_sped","FLOAT","NUMBER","10,2","Y","0.00","회전검지속도",null,"NUMBER(10,2)","NUMBER(10,2)","NUMBER(10,2)",null,null,null,"turn_dttn_sped ","NUMBER(10,2) ","",",",null,"",",",null,null,"turn_dttn_sped ","NUMBER(10,2) ","",",",null,null,"",",","COMMENT ON COLUMN ","soitgrtmdtinfo.","turn_dttn_sped"," IS ","'회전검지속도'",";",null,null,""]
[null,7,"PK","정지선통과유닉스시각","stln_pasg_unix_tm","INT","NUMBER",10,"N","0","정지선통과유닉스시각",null,"NUMBER(10)","INT","NUMBER(10)",null,null,null,"stln_pasg_unix_tm ","INT ","NOT NULL",",",null,"stln_pasg_unix_tm","",null,null,"stln_pasg_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"stln_pasg_unix_tm","","COMMENT ON COLUMN ","soitgrtmdtinfo.","stln_pasg_unix_tm"," IS ","'정지선통과유닉스시각'",";",null,null,""]
[null,8,null,"정지선검지속도","stln_dttn_sped","FLOAT","NUMBER","10,2","Y","0.00","정지선검지속도",null,"NUMBER(10,2)","NUMBER(10,2)","NUMBER(10,2)",null,null,null,"stln_dttn_sped ","NUMBER(10,2) ","",",",null,"","",null,null,"stln_dttn_sped ","NUMBER(10,2) ","",",",null,null,"","","COMMENT ON COLUMN ","soitgrtmdtinfo.","stln_dttn_sped"," IS ","'정지선검지속도'",";",null,null,""]
[null,9,null,"차량구간속도","vhcl_sect_sped","FLOAT","NUMBER","10,2","Y","0.00","차량구간속도",null,"NUMBER(10,2)","NUMBER(10,2)","NUMBER(10,2)",null,null,null,"vhcl_sect_sped ","NUMBER(10,2) ","",",",null,"",",",null,null,"vhcl_sect_sped ","NUMBER(10,2) ","",",",null,null,"",",","COMMENT ON COLUMN ","soitgrtmdtinfo.","vhcl_sect_sped"," IS ","'차량구간속도'",";",null,null,""]
[null,10,"PK","최초관측유닉스시각","frst_obsrvn_unix_tm","INT","NUMBER",10,"N","0","최초관측유닉스시각",null,"NUMBER(10)","VARCHAR(10)","VARCHAR(10)",null,null,null,"frst_obsrvn_unix_tm ","VARCHAR(10) ","NOT NULL",",",null,"frst_obsrvn_unix_tm","));",null,null,"frst_obsrvn_unix_tm ","VARCHAR(10) ","NOT NULL",",",null,null,"frst_obsrvn_unix_tm",")","COMMENT ON COLUMN ","soitgrtmdtinfo.","frst_obsrvn_unix_tm"," IS ","'최초관측유닉스시각'",";",null,null,""]
[null,11,null,"차량관측시간","vhcl_obsrvn_hr","INT","NUMBER",10,"Y","1","차량관측시간",null,"NUMBER(3)","NUMBER(3)","NUMBER(3)",null,null,null,"vhcl_obsrvn_hr ","NUMBER(3) ","",",",null,"",null,null,null,"vhcl_obsrvn_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitgrtmdtinfo.","vhcl_obsrvn_hr"," IS ","'차량관측시간'",";",null,null,""]
[null,12,null,"차량번호명","vhno_nm","VARCHAR","VARCHAR2",20,"Y",null,"차량 번호",null,"VARCHAR2(20)","VARCHAR(20)","VARCHAR2(50)",null,null,null,"vhno_nm ","VARCHAR(20) ","",",",null,"",null,null,null,"vhno_nm ","VARCHAR2(50) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitgrtmdtinfo.","vhno_nm"," IS ","'차량 번호'",";",null,null,""]
[null,13,null,"차량번호검지여부","vhno_dttn_yn","VARCHAR","VARCHAR2",1,"Y",null,"정검지 여부(507)"," (Y:정검지 N:미검지 F:오검지)","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",null,null,null,"vhno_dttn_yn ","VARCHAR(1) ","",",",null,"",null,null,null,"vhno_dttn_yn ","VARCHAR2(1) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitgrtmdtinfo.","vhno_dttn_yn"," IS ","'정검지 여부(507)'",";",null,null,""]
[null,14,null,"이미지경로명","img_path_nm","VARCHAR","VARCHAR2",80,"Y",null,"이미지경로명",null,"VARCHAR2(80)","VARCHAR(80)","VARCHAR2(80)",null,null,null,"img_path_nm ","VARCHAR(80) ","",",",null,"",null,null,null,"img_path_nm ","VARCHAR2(80) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitgrtmdtinfo.","img_path_nm"," IS ","'이미지경로명'",";",null,null,""]
[null,15,null,"차량이미지파일명","vhcl_img_file_nm","VARCHAR","VARCHAR2",80,"Y",null,"차량이미지파일명",null,"VARCHAR2(80)","VARCHAR(80)","VARCHAR2(80)",null,null,null,"vhcl_img_file_nm ","VARCHAR(80) ","",",",null,"",null,null,null,"vhcl_img_file_nm ","VARCHAR2(80) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitgrtmdtinfo.","vhcl_img_file_nm"," IS ","'차량이미지파일명'",";",null,null,""]
[null,16,null,"번호판이미지파일명","nopl_img_file_nm","VARCHAR","VARCHAR2",80,"Y",null,"번호판이미지파일명",null,"VARCHAR2(80)","VARCHAR(80)","VARCHAR2(80)",null,null,null,"nopl_img_file_nm ","VARCHAR(80) ","",",",null,"",null,null,null,"nopl_img_file_nm ","VARCHAR2(80) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitgrtmdtinfo.","nopl_img_file_nm"," IS ","'번호판이미지파일명'",";",null,null,""]
[null,17,"UK","차량_검지_ID","vhcl_dttn_id","VARCHAR","VARCHAR2",256,"Y",null,"차량검지정보 ID",null,"VARCHAR2(256)","VARCHAR(256)","VARCHAR2(256)",null,null,null,"vhcl_dttn_id ","VARCHAR(256) ","",",",null,"",null,null,null,"vhcl_dttn_id ","VARCHAR2(256) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitgrtmdtinfo.","vhcl_dttn_id"," IS ","'차량검지정보 ID'",";",null,null,""]
[null,18,null,"생성유닉스시각","crt_unix_tm","INT","NUMBER",10,"Y","0","생성유닉스시각",null,"NUMBER(10)","INT","NUMBER(10)",null,null,null,"crt_unix_tm ","INT ","",",",null,"",null,null,null,"crt_unix_tm ","NUMBER(10) ","",{"$f":"\") TABLESPACE \"&AF76&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_G002 NOLOGGING"},{"$nulls":4},"COMMENT ON COLUMN ","soitgrtmdtinfo.","crt_unix_tm"," IS ","'생성유닉스시각'",";",null,null,""]
[{"$nulls":18},{"$f":"CONCATENATE(W57:Y74)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AF75:AH75)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (stln_pasg_unix_tm) INTERVAL (86400) STORE IN (\"&AF76&\") (PARTITION BFR_\" & D53 & \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AF76&\");\"","v":"PARTITION BY RANGE (stln_pasg_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_G002) (PARTITION BFR_soitgrtmdtinfo_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_G002);"},{"$f":"\"CREATE INDEX PK_\" & D53 & \" ON \" & D53 & CONCATENATE(AG57:AI74) & \" LOCAL (PARTITION BFR_\" & D53 & \"_20221101 TABLESPACE \"&AG76&\") TABLESPACE \"&AG76&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & D53 & \" ADD CONSTRAINT PK_\" & D53 & \" PRIMARY KEY \" & CONCATENATE(AG57:AI74) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":9},{"$error":"#VALUE!"}]
[{"$nulls":31},"SOIT_D08_G002","SOIT_I08_G002",{"$nulls":10},""]
[null,"테이블명",null,"soitgunacevet",{"$nulls":39},""]
[null,"테이블설명",null,"돌발 이벤트",{"$nulls":39},""]
[null,"참고사항",{"$nulls":41},""]
[null,"NO","PK","논리명","물리명","VoltDB 타입","Tibero 타입","길이","NULL","기본값","비고",null,"형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE","soitgunacevet",null," IS ",{"$f":"\"'\"&D78&\"'\"","v":"'돌발 이벤트'"},";",null,null,""]
[null,1,"PK","현장카메라ID","spot_camr_id","VARCHAR","VARCHAR2",10,"N",null,"현장카메라ID",null,"VARCHAR2(10)","VARCHAR(10)","VARCHAR2(10)",null,"CREATE TABLE ",{"$f":"D77&\" (\"","v":"soitgunacevet ("},{"$f":"E81&\" \"","v":"spot_camr_id "},{"$f":"N81&\" \"","v":"VARCHAR(10) "},{"$f":"IF(I81=\"N\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(C81=\"PK\", C81=\"PK/FK\"), E81, \"\")","v":"spot_camr_id"},{"$f":"IF(OR(C82=\"PK\", C82=\"PK/FK\"), \",\", \"\")","v":","},"CREATE TABLE ",{"$f":"D77&\" (\"","v":"soitgunacevet ("},{"$f":"E81&\" \"","v":"spot_camr_id "},{"$f":"O81&\" \"","v":"VARCHAR2(10) "},{"$f":"IF(I81=\"N\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(C81=\"PK\", C81=\"PK/FK\"), E81, \"\")","v":"spot_camr_id"},{"$f":"IF(OR(C82=\"PK\", C82=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ","soitgunacevet.",{"$f":"E81","v":"spot_camr_id"}," IS ",{"$f":"\"'\"&K81&\"'\"","v":"'현장카메라ID'"},";",null,null,""]
[null,2,"PK","트래킹 ID","trce_id","INT","NUMBER",10,"N",null,"객체 트래킹 ID",null,"NUMBER(10)","INT","NUMBER(10)",null,null,null,"trce_id ","INT ","NOT NULL",",",null,"trce_id",",",null,null,"trce_id ","NUMBER(10) ","NOT NULL",",",null,null,"trce_id",",","COMMENT ON COLUMN ","soitgunacevet.","trce_id"," IS ","'객체 트래킹 ID'",";",null,null,""]
[null,3,"PK","발생유닉스시각","ocrn_unix_tm","INT","NUMBER",10,"N",0,"발생유닉스시각",null,"NUMBER(10)","INT","NUMBER(10)",null,null,null,"ocrn_unix_tm ","INT ","NOT NULL",",",null,"ocrn_unix_tm","));",null,null,"ocrn_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"ocrn_unix_tm",")","COMMENT ON COLUMN ","soitgunacevet.","ocrn_unix_tm"," IS ","'발생유닉스시각'",";",null,null,""]
[null,4,null,"종료유닉스시작","end_unix_tm","INT","NUMBER",10,"Y",null,"종료유닉스시각",null,"NUMBER(10)","INT","NUMBER(10)",null,null,null,"end_unix_tm ","INT ","",",",null,"",null,null,null,"end_unix_tm ","NUMBER(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitgunacevet.","end_unix_tm"," IS ","'종료유닉스시각'",";",null,null,""]
[null,5,null,"이벤트유형코드","evet_type_cd","VARCHAR","VARCHAR2",1,"Y",null,"돌발유형(012)","(1:차량정지, 2:꼬리물기, 3:보행자횡단;인도이탈, 4:역주행)","CHAR(10)","VARCHAR(10)","VARCHAR2(10)",null,null,null,"evet_type_cd ","VARCHAR(10) ","",",",null,"",null,null,null,"evet_type_cd ","VARCHAR2(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitgunacevet.","evet_type_cd"," IS ","'돌발유형(012)'",";",null,null,""]
[null,6,null,"이미지경로명","img_path_nm","VARCHAR","VARCHAR2",80,"Y",null,"이미지경로명",null,"VARCHAR2(80)","VARCHAR(80)","VARCHAR2(80)",null,null,null,"img_path_nm ","VARCHAR(80) ","",",",null,"",null,null,null,"img_path_nm ","VARCHAR2(80) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitgunacevet.","img_path_nm"," IS ","'이미지경로명'",";",null,null,""]
[null,7,null,"이미지파일명","img_file_nm","VARCHAR","VARCHAR2",80,"Y",null,"이미지파일명",null,"VARCHAR2(80)","VARCHAR(80)","VARCHAR2(80)",null,null,null,"img_file_nm ","VARCHAR(80) ","",",",null,"",null,null,null,"img_file_nm ","VARCHAR2(80) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitgunacevet.","img_file_nm"," IS ","'이미지파일명'",";",null,null,""]
[null,8,null,"처리유닉스시각","prcs_unix_tm","INT","NUMBER",10,"Y",0,"처리유닉스시각(돌발이벤트가 종료되기전까지 일정주기로 업데이드 됨)",null,"NUMBER(10)","INT","NUMBER(10)",null,null,null,"prcs_unix_tm ","INT ","",",",null,"",null,null,null,"prcs_unix_tm ","NUMBER(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitgunacevet.","prcs_unix_tm"," IS ","'처리유닉스시각(돌발이벤트가 종료되기전까지 일정주기로 업데이드 됨)'",";",null,null,""]
[null,9,null,"생성유닉스시각","crt_unix_tm","INT","NUMBER",10,"Y",0,"생성유닉스시각",null,"NUMBER(10)","INT","NUMBER(10)",null,null,null,"crt_unix_tm ","INT ","",",",null,"",null,null,null,"crt_unix_tm ","NUMBER(10) ","",{"$f":"\") TABLESPACE \"&AF91&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_G002 NOLOGGING"},null,null,"",null,"COMMENT ON COLUMN ","soitgunacevet.","crt_unix_tm"," IS ","'생성유닉스시각'",";",null,null,""]
[{"$nulls":18},{"$f":"CONCATENATE(W81:Y89)","v":{"$error":"#VALUE!"}},{"$nulls":4},"",null,null,null,{"$f":"CONCATENATE(AF90:AH90)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (ocrn_unix_tm) INTERVAL (3600) STORE IN (\"&AF91&\") (PARTITION BFR_\" & D77 & \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AF91&\");\"","v":"PARTITION BY RANGE (ocrn_unix_tm) INTERVAL (3600) STORE IN (SOIT_D08_G002) (PARTITION BFR_soitgunacevet_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_G002);"},{"$f":"\"CREATE INDEX PK_\" & D77 & \" ON \" & D77 & CONCATENATE(AG81:AI89) & \" LOCAL (PARTITION BFR_\" & D77 & \"_20221101 TABLESPACE \"&AG91&\") TABLESPACE \"&AG91&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & D77 & \" ADD CONSTRAINT PK_\" & D77 & \" PRIMARY KEY \" & CONCATENATE(AG81:AI89) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":9},{"$error":"#VALUE!"}]
[{"$nulls":23},"",{"$nulls":7},"SOIT_D08_G002","SOIT_I08_G002",{"$nulls":10},""]
[null,"테이블명",null,"soitgcwdtinfo",{"$nulls":19},"",{"$nulls":19},""]
[null,"테이블설명",null,"실시간 보행자 검지 정보",{"$nulls":19},"",{"$nulls":19},""]
[null,"참고사항",{"$nulls":21},"",{"$nulls":19},""]
[null,"NO","PK","논리명","물리명","VoltDB 타입","Tibero 타입","길이","NULL","기본값","비고",null,"형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE","soitgcwdtinfo",null," IS ",{"$f":"\"'\"&D93&\"'\"","v":"'실시간 보행자 검지 정보'"},";",null,null,""]
[null,1,"PK","현장카메라ID","spot_camr_id","VARCHAR","VARCHAR2",10,"N",null,"현장카메라ID",null,"VARCHAR2(10)","VARCHAR(10)","VARCHAR2(10)",null,"CREATE TABLE ",{"$f":"D92&\" (\"","v":"soitgcwdtinfo ("},{"$f":"E96&\" \"","v":"spot_camr_id "},{"$f":"N96&\" \"","v":"VARCHAR(10) "},{"$f":"IF(I96=\"N\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(C96=\"PK\", C96=\"PK/FK\"), E96, \"\")","v":"spot_camr_id"},{"$f":"IF(OR(C97=\"PK\", C97=\"PK/FK\"), \",\", \"\")","v":","},"CREATE TABLE ",{"$f":"D92&\" (\"","v":"soitgcwdtinfo ("},{"$f":"E96&\" \"","v":"spot_camr_id "},{"$f":"O96&\" \"","v":"VARCHAR2(10) "},{"$f":"IF(I96=\"N\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(C96=\"PK\", C96=\"PK/FK\"), E96, \"\")","v":"spot_camr_id"},{"$f":"IF(OR(C97=\"PK\", C97=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ","soitgcwdtinfo.",{"$f":"E96","v":"spot_camr_id"}," IS ",{"$f":"\"'\"&K96&\"'\"","v":"'현장카메라ID'"},";",null,null,""]
[null,2,"PK","추적 ID","trce_id","INT","NUMBER",10,"N",0,"객체 트래킹 ID",null,"NUMBER(10)","INT","NUMBER(10)",null,null,null,"trce_id ","INT ","NOT NULL",",",null,"trce_id",",",null,null,"trce_id ","NUMBER(10) ","NOT NULL",",",null,null,"trce_id",",","COMMENT ON COLUMN ","soitgcwdtinfo.","trce_id"," IS ","'객체 트래킹 ID'",";",null,null,""]
[null,3,"PK","검지유닉스시각","dttn_unix_tm","INT","NUMBER",10,"N",0,"검지유닉스시각",null,"NUMBER(10)","INT","NUMBER(10)",null,null,null,"dttn_unix_tm ","INT ","NOT NULL",",",null,"dttn_unix_tm","));",null,null,"dttn_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"dttn_unix_tm",")","COMMENT ON COLUMN ","soitgcwdtinfo.","dttn_unix_tm"," IS ","'검지유닉스시각'",";",null,null,""]
[null,4,null,"방향구분코드","drct_se_cd","VARCHAR","VARCHAR2",1,"N","L","보행자 방향구분(013)","(왼쪽:L, 오른쪽:R)","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",null,null,null,"drct_se_cd ","VARCHAR(1) ","NOT NULL",",",null,"",null,null,null,"drct_se_cd ","VARCHAR2(1) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitgcwdtinfo.","drct_se_cd"," IS ","'보행자 방향구분(013)'",";",null,null,""]
[null,5,null,"생성유닉스시각","crt_unix_tm","INT","NUMBER",10,"Y",0,"생성유닉스시각",null,"NUMBER(10)","INT","NUMBER(10)",null,null,null,"crt_unix_tm ","INT ","",",",null,"",null,null,null,"crt_unix_tm ","NUMBER(10) ","",{"$f":"\") TABLESPACE \"&AF102&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_G002 NOLOGGING"},null,null,"",null,"COMMENT ON COLUMN ","soitgcwdtinfo.","crt_unix_tm"," IS ","'생성유닉스시각'",";",null,null,""]
[{"$nulls":18},{"$f":"CONCATENATE(W96:Y100)","v":{"$error":"#VALUE!"}},{"$nulls":4},"",null,null,null,{"$f":"CONCATENATE(AF101:AH101)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (dttn_unix_tm) INTERVAL (3600) STORE IN (\"&AF102&\") (PARTITION BFR_\" & D92 & \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AF102&\");\"","v":"PARTITION BY RANGE (dttn_unix_tm) INTERVAL (3600) STORE IN (SOIT_D08_G002) (PARTITION BFR_soitgcwdtinfo_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_G002);"},{"$f":"\"CREATE INDEX PK_\" & D92 & \" ON \" & D92 & CONCATENATE(AG96:AI100) & \" LOCAL (PARTITION BFR_\" & D92 & \"_20221101 TABLESPACE \"&AG102&\") TABLESPACE \"&AG102&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & D92 & \" ADD CONSTRAINT PK_\" & D92 & \" PRIMARY KEY \" & CONCATENATE(AG96:AI100) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":9},{"$error":"#VALUE!"}]
[{"$nulls":23},"",{"$nulls":7},"SOIT_D08_G002","SOIT_I08_G002",{"$nulls":10},""]
[null,"테이블명",null,"soitgvhcltrce",{"$nulls":19},"",{"$nulls":19},""]
[null,"테이블설명",null,"차량 트래킹 정보",{"$nulls":19},"",{"$nulls":19},""]
[null,"참고사항",{"$nulls":41},""]
[null,"NO","PK","논리명","물리명","VoltDB 타입","Tibero 타입","길이","NULL","기본값","비고",null,"형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE","soitgvhcltrce",null," IS ",{"$f":"\"'\"&D104&\"'\"","v":"'차량 트래킹 정보'"},";",null,null,""]
[null,1,"PK","현장카메라ID","spot_camr_id","VARCHAR","VARCHAR2",10,"N",null,"현장카메라ID",null,"VARCHAR2(10)","VARCHAR(10)","VARCHAR2(10)",null,"CREATE TABLE ",{"$f":"D103&\" (\"","v":"soitgvhcltrce ("},{"$f":"E107&\" \"","v":"spot_camr_id "},{"$f":"N107&\" \"","v":"VARCHAR(10) "},{"$f":"IF(I107=\"N\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(C107=\"PK\", C107=\"PK/FK\"), E107, \"\")","v":"spot_camr_id"},{"$f":"IF(OR(C108=\"PK\", C108=\"PK/FK\"), \",\", \"\")","v":","},"CREATE TABLE ",{"$f":"D103&\" (\"","v":"soitgvhcltrce ("},{"$f":"E107&\" \"","v":"spot_camr_id "},{"$f":"O107&\" \"","v":"VARCHAR2(10) "},{"$f":"IF(I107=\"N\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(C107=\"PK\", C107=\"PK/FK\"), E107, \"\")","v":"spot_camr_id"},{"$f":"IF(OR(C108=\"PK\", C108=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ","soitgvhcltrce.",{"$f":"E107","v":"spot_camr_id"}," IS ",{"$f":"\"'\"&K107&\"'\"","v":"'현장카메라ID'"},";",null,null,""]
[null,2,"PK","추적시작유닉스시각","trce_bgng_unix_tm","INT","NUMBER",10,"N",0,"추적시작유닉스시각",null,"NUMBER(10)","INT","NUMBER(10)",null,null,null,"trce_bgng_unix_tm ","INT ","NOT NULL",",",null,"trce_bgng_unix_tm",",",null,null,"trce_bgng_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"trce_bgng_unix_tm",",","COMMENT ON COLUMN ","soitgvhcltrce.","trce_bgng_unix_tm"," IS ","'추적시작유닉스시각'",";",null,null,""]
[null,3,"PK","추적종료유닉스시각","trce_end_unix_tm","INT","NUMBER",10,"N",0,"추적종료유닉스시각",null,"NUMBER(10)","INT","NUMBER(10)",null,null,null,"trce_end_unix_tm ","INT ","NOT NULL",",",null,"trce_end_unix_tm","));",null,null,"trce_end_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"trce_end_unix_tm",")","COMMENT ON COLUMN ","soitgvhcltrce.","trce_end_unix_tm"," IS ","'추적종료유닉스시각'",";",null,null,""]
[null,4,null,"이미지경로명","img_path_nm","VARCHAR","VARCHAR2",80,"Y",null,"이미지경로명",null,"VARCHAR2(80)","VARCHAR(80)","VARCHAR2(80)",null,null,null,"img_path_nm ","VARCHAR(80) ","",",",null,"",null,null,null,"img_path_nm ","VARCHAR2(80) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitgvhcltrce.","img_path_nm"," IS ","'이미지경로명'",";",null,null,""]
[null,5,null,"이미지파일명","img_file_nm","VARCHAR","VARCHAR2",80,"Y",null,"이미지파일명",null,"VARCHAR2(80)","VARCHAR(80)","VARCHAR2(80)",null,null,null,"img_file_nm ","VARCHAR(80) ","",",",null,"",null,null,null,"img_file_nm ","VARCHAR2(80) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitgvhcltrce.","img_file_nm"," IS ","'이미지파일명'",";",null,null,""]
[null,6,null,"생성유닉스시각","crt_unix_tm","INT","NUMBER",10,"Y",0,"생성유닉스시각",null,"NUMBER(10)","INT","NUMBER(10)",null,null,null,"crt_unix_tm ","INT ","",",",null,"",null,null,null,"crt_unix_tm ","NUMBER(10) ","",{"$f":"\") TABLESPACE \"&AF114&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_G002 NOLOGGING"},null,null,{"$f":"IF(OR(C112=\"PK\", C112=\"PK/FK\"), E112, \"\")","v":""},null,"COMMENT ON COLUMN ","soitgvhcltrce.","crt_unix_tm"," IS ","'생성유닉스시각'",";",null,null,""]
[{"$nulls":18},{"$f":"CONCATENATE(W107:Y112)","v":{"$error":"#VALUE!"}},{"$nulls":4},"",null,null,null,{"$f":"CONCATENATE(AF113:AH113)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (trce_bgng_unix_tm) INTERVAL (3600) STORE IN (\"&AF114&\") (PARTITION BFR_\" & D103 & \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AF114&\");\"","v":"PARTITION BY RANGE (trce_bgng_unix_tm) INTERVAL (3600) STORE IN (SOIT_D08_G002) (PARTITION BFR_soitgvhcltrce_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_G002);"},{"$f":"\"CREATE INDEX PK_\" & D103 & \" ON \" & D103 & CONCATENATE(AG107:AI112) & \" LOCAL (PARTITION BFR_\" & D103 & \"_20221101 TABLESPACE \"&AG114&\") TABLESPACE \"&AG114&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & D103 & \" ADD CONSTRAINT PK_\" & D103 & \" PRIMARY KEY \" & CONCATENATE(AG107:AI112) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":9},{"$error":"#VALUE!"}]
[{"$nulls":23},"",{"$nulls":7},"SOIT_D08_G002","SOIT_I08_G002",{"$nulls":10},""]
[null,"테이블명",null,"soitgvhcldtrtstats",{"$nulls":19},"",{"$nulls":19},""]
[null,"테이블설명",null,"번호판 검지 통계",{"$nulls":19},"",{"$nulls":19},""]
[null,"참고사항",{"$nulls":21},"",{"$nulls":19},""]
[null,"NO","PK","논리명","물리명","VoltDB 타입","Tibero 타입","길이","NULL","기본값","비고",null,"형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE","soitgvhcldtrtstats",null," IS ",{"$f":"\"'\"&D116&\"'\"","v":"'번호판 검지 통계'"},";",null,null,""]
[null,1,"PK","현장카메라ID","spot_camr_id","VARCHAR","VARCHAR2",10,"N",null,"현장카메라ID",null,"VARCHAR2(10)","VARCHAR(10)","VARCHAR2(10)",null,"CREATE TABLE ",{"$f":"D115&\" (\"","v":"soitgvhcldtrtstats ("},{"$f":"E119&\" \"","v":"spot_camr_id "},{"$f":"N119&\" \"","v":"VARCHAR(10) "},{"$f":"IF(I119=\"N\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(C119=\"PK\", C119=\"PK/FK\"), E119, \"\")","v":"spot_camr_id"},{"$f":"IF(OR(C120=\"PK\", C120=\"PK/FK\"), \",\", \"\")","v":","},"CREATE TABLE ",{"$f":"D115&\" (\"","v":"soitgvhcldtrtstats ("},{"$f":"E119&\" \"","v":"spot_camr_id "},{"$f":"O119&\" \"","v":"VARCHAR2(10) "},{"$f":"IF(I119=\"N\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(C119=\"PK\", C119=\"PK/FK\"), E119, \"\")","v":"spot_camr_id"},{"$f":"IF(OR(C120=\"PK\", C120=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ","soitgvhcldtrtstats.",{"$f":"E119","v":"spot_camr_id"}," IS ",{"$f":"\"'\"&K119&\"'\"","v":"'현장카메라ID'"},";",null,null,""]
[null,2,"PK","통계시작유닉스시각","stats_bgng_unix_tm","INT","NUMBER",10,"N",null,"통계시작유닉스시각",null,"NUMBER(10)","INT","NUMBER(10)",null,null,null,"stats_bgng_unix_tm ","INT ","NOT NULL",",",null,"stats_bgng_unix_tm",",",null,null,"stats_bgng_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"stats_bgng_unix_tm",",","COMMENT ON COLUMN ","soitgvhcldtrtstats.","stats_bgng_unix_tm"," IS ","'통계시작유닉스시각'",";",null,null,""]
[null,3,"PK","통계종료유닉스시각","stats_end_unix_tm","INT","NUMBER",10,"N",null,"통계종료유닉스시각",null,"NUMBER(10)","INT","NUMBER(10)",null,null,null,"stats_end_unix_tm ","INT ","NOT NULL",",",null,"stats_end_unix_tm","));",null,null,"stats_end_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"stats_end_unix_tm",")","COMMENT ON COLUMN ","soitgvhcldtrtstats.","stats_end_unix_tm"," IS ","'통계종료유닉스시각'",";",null,null,""]
[null,4,null,"정검지수","nrdt_cnt","SMALLINT","NUMBER",5,"Y",0,"정검지수",null,"NUMBER(5)","SMALLINT","NUMBER(5)",null,null,null,"nrdt_cnt ","SMALLINT ","",",",null,"",null,null,null,"nrdt_cnt ","NUMBER(5) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitgvhcldtrtstats.","nrdt_cnt"," IS ","'정검지수'",";",null,null,""]
[null,5,null,"오검지수","abdt_cnt","SMALLINT","NUMBER",5,"Y",0,"오검지수",null,"NUMBER(5)","SMALLINT","NUMBER(5)",null,null,null,"abdt_cnt ","SMALLINT ","",",",null,"",null,null,null,"abdt_cnt ","NUMBER(5) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitgvhcldtrtstats.","abdt_cnt"," IS ","'오검지수'",";",null,null,""]
[null,6,null,"미검지수","undt_cnt","SMALLINT","NUMBER",5,"Y",0,"미검지수",null,"NUMBER(5)","SMALLINT","NUMBER(5)",null,null,null,"undt_cnt ","SMALLINT ","",",",null,"",null,null,null,"undt_cnt ","NUMBER(5) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitgvhcldtrtstats.","undt_cnt"," IS ","'미검지수'",";",null,null,""]
[null,7,null,"오토바이수","mtcl_dttn_cnt","SMALLINT","NUMBER",5,"Y",0,"오토바이수",null,"NUMBER(5)","SMALLINT","NUMBER(5)",null,null,null,"mtcl_dttn_cnt ","SMALLINT ","",",",null,"",null,null,null,"mtcl_dttn_cnt ","NUMBER(5) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitgvhcldtrtstats.","mtcl_dttn_cnt"," IS ","'오토바이수'",";",null,null,""]
[null,8,null,"생성유닉스시각","crt_unix_tm","INT","NUMBER",10,"Y",0,"생성유닉스시각",null,"NUMBER(10)","INT","NUMBER(10)",null,null,null,"crt_unix_tm ","INT ","",",",null,"",null,null,null,"crt_unix_tm ","NUMBER(10) ","",{"$f":"\") TABLESPACE \"&AF128&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_G003 NOLOGGING"},null,null,{"$f":"IF(OR(C126=\"PK\", C126=\"PK/FK\"), E126, \"\")","v":""},null,"COMMENT ON COLUMN ","soitgvhcldtrtstats.","crt_unix_tm"," IS ","'생성유닉스시각'",";",null,null,""]
[{"$nulls":18},{"$f":"CONCATENATE(W119:Y126)","v":{"$error":"#VALUE!"}},{"$nulls":4},"",null,null,null,{"$f":"CONCATENATE(AF127:AH127)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (stats_bgng_unix_tm) INTERVAL (86400) STORE IN (\"&AF128&\") (PARTITION BFR_\" & D115 & \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AF128&\");\"","v":"PARTITION BY RANGE (stats_bgng_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_G003) (PARTITION BFR_soitgvhcldtrtstats_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_G003);"},{"$f":"\"CREATE INDEX PK_\" & D115 & \" ON \" & D115 & CONCATENATE(AG119:AI126) & \" LOCAL (PARTITION BFR_\" & D117 & \"_20221101 TABLESPACE \"&AG128&\") TABLESPACE \"&AG128&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & D115 & \" ADD CONSTRAINT PK_\" & D115 & \" PRIMARY KEY \" & CONCATENATE(AG119:AI126) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":9},{"$error":"#VALUE!"}]
[{"$nulls":23},"",{"$nulls":7},"SOIT_D08_G003","SOIT_I08_G003",{"$nulls":10},""]
[null,"테이블명",null,"soitgturndtrtstats",{"$nulls":19},"",{"$nulls":19},""]
[null,"테이블설명",null,"회전별 번호판 검지 통계",{"$nulls":19},"",{"$nulls":19},""]
[null,"참고사항",{"$nulls":21},"",{"$nulls":19},""]
[null,"NO","PK","논리명","물리명","VoltDB 타입","Tibero 타입","길이","NULL","기본값","비고",null,"형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE","soitgturndtrtstats",null," IS ",{"$f":"\"'\"&D130&\"'\"","v":"'회전별 번호판 검지 통계'"},";",null,null,""]
[null,1,"PK","현장카메라ID","spot_camr_id","VARCHAR","VARCHAR2",10,"N",null,"현장카메라ID",null,"VARCHAR2(10)","VARCHAR(10)","VARCHAR2(10)",null,"CREATE TABLE ",{"$f":"D129&\" (\"","v":"soitgturndtrtstats ("},{"$f":"E133&\" \"","v":"spot_camr_id "},{"$f":"N133&\" \"","v":"VARCHAR(10) "},{"$f":"IF(I133=\"N\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(C133=\"PK\", C133=\"PK/FK\"), E133, \"\")","v":"spot_camr_id"},{"$f":"IF(OR(C134=\"PK\", C134=\"PK/FK\"), \",\", \"\")","v":","},"CREATE TABLE ",{"$f":"D129&\" (\"","v":"soitgturndtrtstats ("},{"$f":"E133&\" \"","v":"spot_camr_id "},{"$f":"O133&\" \"","v":"VARCHAR2(10) "},{"$f":"IF(I133=\"N\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(C133=\"PK\", C133=\"PK/FK\"), E133, \"\")","v":"spot_camr_id"},{"$f":"IF(OR(C134=\"PK\", C134=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ","soitgturndtrtstats.",{"$f":"E133","v":"spot_camr_id"}," IS ",{"$f":"\"'\"&K133&\"'\"","v":"'현장카메라ID'"},";",null,null,""]
[null,2,"PK","통계시작유닉스시각","stats_bgng_unix_tm","INT","NUMBER",10,"N",0,"통계시작유닉스시각",null,"NUMBER(10)","INT","NUMBER(10)",null,null,null,"stats_bgng_unix_tm ","INT ","NOT NULL",",",null,"stats_bgng_unix_tm",",",null,null,"stats_bgng_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"stats_bgng_unix_tm",",","COMMENT ON COLUMN ","soitgturndtrtstats.","stats_bgng_unix_tm"," IS ","'통계시작유닉스시각'",";",null,null,""]
[null,3,"PK","통계종료유닉스시각","stats_end_unix_tm","INT","NUMBER",10,"N",0,"통계종료유닉스시각",null,"NUMBER(10)","INT","NUMBER(10)",null,null,null,"stats_end_unix_tm ","INT ","NOT NULL",",",null,"stats_end_unix_tm",",",null,null,"stats_end_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"stats_end_unix_tm",",","COMMENT ON COLUMN ","soitgturndtrtstats.","stats_end_unix_tm"," IS ","'통계종료유닉스시각'",";",null,null,""]
[null,4,"PK","회전유형코드","turn_type_cd","VARCHAR","VARCHAR2",10,"N",null,"회전유형(700)","( 11:직진, 21:작은좌회전, 22:큰좌회전, 31:작은우회전, 32:큰우회전, 41:유턴)","CHAR(10)","VARCHAR(10)","VARCHAR2(10)",null,null,null,"turn_type_cd ","VARCHAR(10) ","NOT NULL",",",null,"turn_type_cd","));",null,null,"turn_type_cd ","VARCHAR2(10) ","NOT NULL",",",null,null,"turn_type_cd",")","COMMENT ON COLUMN ","soitgturndtrtstats.","turn_type_cd"," IS ","'회전유형(700)'",";",null,null,""]
[null,5,null,"정검지수","nrdt_cnt","SMALLINT","NUMBER",5,"Y",0,"정검지수",null,"NUMBER(5)","SMALLINT","NUMBER(5)",null,null,null,"nrdt_cnt ","SMALLINT ","",",",null,"",{"$f":"IF(OR(C138=\"PK\", C138=\"PK/FK\"), \",\", \"\")","v":""},null,null,"nrdt_cnt ","NUMBER(5) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitgturndtrtstats.","nrdt_cnt"," IS ","'정검지수'",";",null,null,""]
[null,6,null,"오검지수","abdt_cnt","SMALLINT","NUMBER",5,"Y",0,"오검지수",null,"NUMBER(5)","SMALLINT","NUMBER(5)",null,null,null,"abdt_cnt ","SMALLINT ","",",",null,"","",null,null,"abdt_cnt ","NUMBER(5) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitgturndtrtstats.","abdt_cnt"," IS ","'오검지수'",";",null,null,""]
[null,7,null,"미검지수","undt_cnt","SMALLINT","NUMBER",5,"Y",0,"미검지수",null,"NUMBER(5)","SMALLINT","NUMBER(5)",null,null,null,"undt_cnt ","SMALLINT ","",",",null,"","",null,null,"undt_cnt ","NUMBER(5) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitgturndtrtstats.","undt_cnt"," IS ","'미검지수'",";",null,null,""]
[null,8,null,"오토바이수","mtcl_dttn_cnt","SMALLINT","NUMBER",5,"Y",0,"오토바이수",null,"NUMBER(5)","SMALLINT","NUMBER(5)",null,null,null,"mtcl_dttn_cnt ","SMALLINT ","",",",null,"","",null,null,"mtcl_dttn_cnt ","NUMBER(5) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitgturndtrtstats.","mtcl_dttn_cnt"," IS ","'오토바이수'",";",null,null,""]
[null,9,null,"생성유닉스시각","crt_unix_tm","INT","NUMBER",10,"Y",0,"생성유닉스시각",null,"NUMBER(10)","INT","NUMBER(10)",null,null,null,"crt_unix_tm ","INT ","",",",null,"","",null,null,"crt_unix_tm ","NUMBER(10) ","",{"$f":"\") TABLESPACE \"&AF143&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_G003 NOLOGGING"},null,null,"",null,"COMMENT ON COLUMN ","soitgturndtrtstats.","crt_unix_tm"," IS ","'생성유닉스시각'",";",null,null,""]
[{"$nulls":18},{"$f":"CONCATENATE(W133:Y141)","v":{"$error":"#VALUE!"}},{"$nulls":4},"","",null,null,{"$f":"CONCATENATE(AF142:AH142)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (stats_bgng_unix_tm) INTERVAL (86400) STORE IN (\"&AF143&\") (PARTITION BFR_\" & D129 & \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AF143&\");\"","v":"PARTITION BY RANGE (stats_bgng_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_G003) (PARTITION BFR_soitgturndtrtstats_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_G003);"},{"$f":"\"CREATE INDEX PK_\" & D129 & \" ON \" & D129 & CONCATENATE(AG133:AI140) & \" LOCAL (PARTITION BFR_\" & D132 & \"_20221101 TABLESPACE \"&AG143&\") TABLESPACE \"&AG143&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & D129 & \" ADD CONSTRAINT PK_\" & D129 & \" PRIMARY KEY \" & CONCATENATE(AG133:AI141) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":9},{"$error":"#VALUE!"}]
[{"$nulls":23},"",{"$nulls":7},"SOIT_D08_G003","SOIT_I08_G003",{"$nulls":10},""]
[null,"테이블명",null,"soitgaprdstats",{"$nulls":19},"",{"$nulls":19},""]
[null,"테이블설명",null,"접근로별 통계",{"$nulls":19},"",{"$nulls":19},""]
[null,"참고사항",{"$nulls":21},"",{"$nulls":19},""]
[null,"NO","PK","논리명","물리명","VoltDB 타입","Tibero 타입","길이","NULL","기본값","비고",null,"형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE","soitgaprdstats",null," IS ",{"$f":"\"'\"&D145&\"'\"","v":"'접근로별 통계'"},";",null,null,""]
[null,1,"PK","현장카메라ID","spot_camr_id","VARCHAR","VARCHAR2",10,"N",null,"현장카메라ID",null,"VARCHAR2(10)","VARCHAR(10)","VARCHAR2(10)",null,"CREATE TABLE ",{"$f":"D144&\" (\"","v":"soitgaprdstats ("},{"$f":"E148&\" \"","v":"spot_camr_id "},{"$f":"N148&\" \"","v":"VARCHAR(10) "},{"$f":"IF(I148=\"N\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(C148=\"PK\", C148=\"PK/FK\"), E148, \"\")","v":"spot_camr_id"},{"$f":"IF(OR(C149=\"PK\", C149=\"PK/FK\"), \",\", \"\")","v":","},"CREATE TABLE ",{"$f":"D144&\" (\"","v":"soitgaprdstats ("},{"$f":"E148&\" \"","v":"spot_camr_id "},{"$f":"O148&\" \"","v":"VARCHAR2(10) "},{"$f":"IF(I148=\"N\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(C148=\"PK\", C148=\"PK/FK\"), E148, \"\")","v":"spot_camr_id"},{"$f":"IF(OR(C149=\"PK\", C149=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ","soitgaprdstats.",{"$f":"E148","v":"spot_camr_id"}," IS ",{"$f":"\"'\"&K148&\"'\"","v":"'현장카메라ID'"},";",null,null,""]
[null,2,"PK","시간유형코드","hr_type_cd","VARCHAR","VARCHAR2",10,"N",null,"시간구분(011)","(1:신호현시, 2:1분단위, 3:5분단위)","CHAR(10)","VARCHAR(10)","VARCHAR2(10)",null,null,null,"hr_type_cd ","VARCHAR(10) ","NOT NULL",",",null,"hr_type_cd",",",null,null,"hr_type_cd ","VARCHAR2(10) ","NOT NULL",",",null,null,"hr_type_cd",",","COMMENT ON COLUMN ","soitgaprdstats.","hr_type_cd"," IS ","'시간구분(011)'",";",null,null,""]
[null,3,"PK","통계시작유닉스시각","stats_bgng_unix_tm","INT","NUMBER",10,"N","0","통계시작유닉스시각",null,"NUMBER(10)","INT","NUMBER(10)",null,null,null,"stats_bgng_unix_tm ","INT ","NOT NULL",",",null,"stats_bgng_unix_tm",",",null,null,"stats_bgng_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"stats_bgng_unix_tm",",","COMMENT ON COLUMN ","soitgaprdstats.","stats_bgng_unix_tm"," IS ","'통계시작유닉스시각'",";",null,null,""]
[null,4,"PK","통계종료유닉스시각","stats_end_unix_tm","INT","NUMBER",10,"N","0","통계종료유닉스시각",null,"NUMBER(10)","INT","NUMBER(10)",null,null,null,"stats_end_unix_tm ","INT ","NOT NULL",",",null,"stats_end_unix_tm","));",null,null,"stats_end_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"stats_end_unix_tm",")","COMMENT ON COLUMN ","soitgaprdstats.","stats_end_unix_tm"," IS ","'통계종료유닉스시각'",";",null,null,""]
[null,5,null,"총교통량","totl_trvl","INT","NUMBER",10,"Y","0","총교통량",null,"NUMBER(10)","INT","NUMBER(10)",null,null,null,"totl_trvl ","INT ","",",",null,"",null,null,null,"totl_trvl ","NUMBER(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitgaprdstats.","totl_trvl"," IS ","'총교통량'",";",null,null,""]
[null,6,null,"평균정지선검지속도","avg_stln_dttn_sped","FLOAT","NUMBER","10,2","Y","0.00","평균정지선검지속도",null,"NUMBER(10,2)","FLOAT","NUMBER(10,2)",null,null,null,"avg_stln_dttn_sped ","FLOAT ","",",",null,"",null,null,null,"avg_stln_dttn_sped ","NUMBER(10,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitgaprdstats.","avg_stln_dttn_sped"," IS ","'평균정지선검지속도'",";",null,null,""]
[null,7,null,"평균구간속도","avg_sect_sped","FLOAT","NUMBER","10,2","Y","0.00","평균구간속도","roi ","NUMBER(10,2)","FLOAT","NUMBER(10,2)",null,null,null,"avg_sect_sped ","FLOAT ","",",",null,"",null,null,null,"avg_sect_sped ","NUMBER(10,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitgaprdstats.","avg_sect_sped"," IS ","'평균구간속도'",";",null,null,""]
[null,8,null,"평균교통밀도","avg_trfc_dnst","SMALLINT","NUMBER",5,"Y","0","평균교통밀도(단위:대/km)",null,"NUMBER(5)","SMALLINT","NUMBER(5)",null,null,null,"avg_trfc_dnst ","SMALLINT ","",",",null,"",null,null,null,"avg_trfc_dnst ","NUMBER(5) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitgaprdstats.","avg_trfc_dnst"," IS ","'평균교통밀도(단위:대/km)'",";",null,null,""]
[null,9,null,"최소교통밀도","min_trfc_dnst","SMALLINT","NUMBER",5,"Y","0","최소교통밀도(단위:대/km)",null,"NUMBER(5)","SMALLINT","NUMBER(5)",null,null,null,"min_trfc_dnst ","SMALLINT ","",",",null,"",null,null,null,"min_trfc_dnst ","NUMBER(5) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitgaprdstats.","min_trfc_dnst"," IS ","'최소교통밀도(단위:대/km)'",";",null,null,""]
[null,10,null,"최대교통밀도","max_trfc_dnst","SMALLINT","NUMBER",5,"Y","0","최대교통밀도(단위:대/km)",null,"NUMBER(5)","SMALLINT","NUMBER(5)",null,null,null,"max_trfc_dnst ","SMALLINT ","",",",null,"",null,null,null,"max_trfc_dnst ","NUMBER(5) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitgaprdstats.","max_trfc_dnst"," IS ","'최대교통밀도(단위:대/km)'",";",null,null,""]
[null,11,null,"평균차로점유율","avg_lane_ocpn_rt","DECIMAL","NUMBER","12,9","Y",0,"평균차로점유율",null,"NUMBER(12,9)","DECIMAL(12,9)","NUMBER(12,9)",null,null,null,"avg_lane_ocpn_rt ","DECIMAL(12,9) ","",",",null,"",null,null,null,"avg_lane_ocpn_rt ","NUMBER(12,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitgaprdstats.","avg_lane_ocpn_rt"," IS ","'평균차로점유율'",";",null,null,""]
[null,12,null,"생성유닉스시각","crt_unix_tm","INT","NUMBER",10,"Y",0,"생성유닉스시각",null,"NUMBER(10)","INT","NUMBER(10)",null,null,null,"crt_unix_tm ","INT ","",",",null,"",null,null,null,"crt_unix_tm ","NUMBER(10) ","",{"$f":"\") TABLESPACE \"&AF161&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_G003 NOLOGGING"},null,null,{"$f":"IF(OR(C159=\"PK\", C159=\"PK/FK\"), E159, \"\")","v":""},null,"COMMENT ON COLUMN ","soitgaprdstats.","crt_unix_tm"," IS ","'생성유닉스시각'",";",null,null,""]
[{"$nulls":18},{"$f":"CONCATENATE(W148:Y159)","v":{"$error":"#VALUE!"}},{"$nulls":4},"",null,null,null,{"$f":"CONCATENATE(AF160:AH160)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (stats_bgng_unix_tm) INTERVAL (86400) STORE IN (\"&AF161&\") (PARTITION BFR_\" & D144 & \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AF161&\");\"","v":"PARTITION BY RANGE (stats_bgng_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_G003) (PARTITION BFR_soitgaprdstats_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_G003);"},{"$f":"\"CREATE INDEX PK_\" & D144 & \" ON \" & D144 & CONCATENATE(AG148:AI158) & \" LOCAL (PARTITION BFR_\" & D150 & \"_20221101 TABLESPACE \"&AG161&\") TABLESPACE \"&AG161&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & D144 & \" ADD CONSTRAINT PK_\" & D144 & \" PRIMARY KEY \" & CONCATENATE(AG148:AI158) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":9},{"$error":"#VALUE!"}]
[{"$nulls":23},"",{"$nulls":7},"SOIT_D08_G003","SOIT_I08_G003",{"$nulls":10},""]
[null,"테이블명",null,"soitgturntypestats",{"$nulls":19},"",{"$nulls":19},""]
[null,"테이블설명",null,"회전별 통계",{"$nulls":19},"",{"$nulls":19},""]
[null,"참고사항",{"$nulls":21},"",{"$nulls":19},""]
[null,"NO","PK","논리명","물리명","VoltDB 타입","Tibero 타입","길이","NULL","기본값","비고",null,"형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE","soitgturntypestats",null," IS ",{"$f":"\"'\"&D163&\"'\"","v":"'회전별 통계'"},";",null,null,""]
[null,1,"PK","현장카메라ID","spot_camr_id","VARCHAR","VARCHAR2",10,"N",null,"현장카메라ID",null,"VARCHAR2(10)","VARCHAR(10)","VARCHAR2(10)",null,"CREATE TABLE ",{"$f":"D162&\" (\"","v":"soitgturntypestats ("},{"$f":"E166&\" \"","v":"spot_camr_id "},{"$f":"N166&\" \"","v":"VARCHAR(10) "},{"$f":"IF(I166=\"N\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(C166=\"PK\", C166=\"PK/FK\"), E166, \"\")","v":"spot_camr_id"},{"$f":"IF(OR(C167=\"PK\", C167=\"PK/FK\"), \",\", \"\")","v":","},"CREATE TABLE ",{"$f":"D162&\" (\"","v":"soitgturntypestats ("},{"$f":"E166&\" \"","v":"spot_camr_id "},{"$f":"O166&\" \"","v":"VARCHAR2(10) "},{"$f":"IF(I166=\"N\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(C166=\"PK\", C166=\"PK/FK\"), E166, \"\")","v":"spot_camr_id"},{"$f":"IF(OR(C167=\"PK\", C167=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ","soitgturntypestats.",{"$f":"E166","v":"spot_camr_id"}," IS ",{"$f":"\"'\"&K166&\"'\"","v":"'현장카메라ID'"},";",null,null,""]
[null,2,"PK","회전유형코드","turn_type_cd","VARCHAR","VARCHAR2",10,"N",null,"회전유형코드(700)","( 11:직진, 21:작은좌회전, 22:큰좌회전, 31:작은우회전, 32:큰우회전, 41:유턴)","CHAR(10)","VARCHAR(10)","VARCHAR2(10)",null,null,null,"turn_type_cd ","VARCHAR(10) ","NOT NULL",",",null,"turn_type_cd",",",null,null,"turn_type_cd ","VARCHAR2(10) ","NOT NULL",",",null,null,"turn_type_cd",",","COMMENT ON COLUMN ","soitgturntypestats.","turn_type_cd"," IS ","'회전유형코드(700)'",";",null,null,""]
[null,3,"PK","시간유형코드","hr_type_cd","VARCHAR","VARCHAR2",10,"N",null,"시간구분(011)","(1:신호현시, 2:1분단위, 3:5분단위)","CHAR(10)","VARCHAR(10)","VARCHAR2(10)",null,null,null,"hr_type_cd ","VARCHAR(10) ","NOT NULL",",",null,"hr_type_cd",",",null,null,"hr_type_cd ","VARCHAR2(10) ","NOT NULL",",",null,null,"hr_type_cd",",","COMMENT ON COLUMN ","soitgturntypestats.","hr_type_cd"," IS ","'시간구분(011)'",";",null,null,""]
[null,4,"PK","통계시작유닉스시각","stats_bgng_unix_tm","INT","NUMBER",10,"N","0","통계시작유닉스시각",null,"NUMBER(10)","INT","NUMBER(10)",null,null,null,"stats_bgng_unix_tm ","INT ","NOT NULL",",",null,"stats_bgng_unix_tm",",",null,null,"stats_bgng_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"stats_bgng_unix_tm",",","COMMENT ON COLUMN ","soitgturntypestats.","stats_bgng_unix_tm"," IS ","'통계시작유닉스시각'",";",null,null,""]
[null,5,"PK","통계종료유닉스시각","stats_end_unix_tm","INT","NUMBER",10,"N","0","통계종료유닉스시각",null,"NUMBER(10)","INT","NUMBER(10)",null,null,null,"stats_end_unix_tm ","INT ","NOT NULL",",",null,"stats_end_unix_tm","));",null,null,"stats_end_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"stats_end_unix_tm",")","COMMENT ON COLUMN ","soitgturntypestats.","stats_end_unix_tm"," IS ","'통계종료유닉스시각'",";",null,null,""]
[null,6,null,"차종1_교통량","kncr1_trvl","INT","NUMBER",10,"Y","0","차종1_교통량","MBUS","NUMBER(10)","INT","NUMBER(10)",null,null,null,"kncr1_trvl ","INT ","",",",null,"",null,null,null,"kncr1_trvl ","NUMBER(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitgturntypestats.","kncr1_trvl"," IS ","'차종1_교통량'",";",null,null,""]
[null,7,null,"차종2_교통량","kncr2_trvl","INT","NUMBER",10,"Y","0","차종2_교통량","LBUS","NUMBER(10)","INT","NUMBER(10)",null,null,null,"kncr2_trvl ","INT ","",",",null,"",null,null,null,"kncr2_trvl ","NUMBER(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitgturntypestats.","kncr2_trvl"," IS ","'차종2_교통량'",";",null,null,""]
[null,8,null,"차종3_교통량","kncr3_trvl","INT","NUMBER",10,"Y","0","차종3_교통량","PCAR","NUMBER(10)","INT","NUMBER(10)",null,null,null,"kncr3_trvl ","INT ","",",",null,"",null,null,null,"kncr3_trvl ","NUMBER(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitgturntypestats.","kncr3_trvl"," IS ","'차종3_교통량'",";",null,null,""]
[null,9,null,"차종4_교통량","kncr4_trvl","INT","NUMBER",10,"Y","0","차종4_교통량","MOTOR","NUMBER(10)","INT","NUMBER(10)",null,null,null,"kncr4_trvl ","INT ","",",",null,"",null,null,null,"kncr4_trvl ","NUMBER(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitgturntypestats.","kncr4_trvl"," IS ","'차종4_교통량'",";",null,null,""]
[null,10,null,"차종5_교통량","kncr5_trvl","INT","NUMBER",10,"Y","0","차종5_교통량","MTRUCK","NUMBER(10)","INT","NUMBER(10)",null,null,null,"kncr5_trvl ","INT ","",",",null,"",null,null,null,"kncr5_trvl ","NUMBER(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitgturntypestats.","kncr5_trvl"," IS ","'차종5_교통량'",";",null,null,""]
[null,11,null,"차종6_교통량","kncr6_trvl","INT","NUMBER",10,"Y","0","차종6_교통량","LTRUCK","NUMBER(10)","INT","NUMBER(10)",null,null,null,"kncr6_trvl ","INT ","",",",null,"",null,null,null,"kncr6_trvl ","NUMBER(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitgturntypestats.","kncr6_trvl"," IS ","'차종6_교통량'",";",null,null,""]
[null,12,null,"평균정지선검지속도","avg_stln_dttn_sped","FLOAT","NUMBER","10,2","Y","0.00","평균정지선검지속도",null,"NUMBER(10,2)","FLOAT","NUMBER(10,2)",null,null,null,"avg_stln_dttn_sped ","FLOAT ","",",",null,"",null,null,null,"avg_stln_dttn_sped ","NUMBER(10,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitgturntypestats.","avg_stln_dttn_sped"," IS ","'평균정지선검지속도'",";",null,null,""]
[null,13,null,"평균구간속도","avg_sect_sped","FLOAT","NUMBER","10,2","Y",0,"평균구간속도",null,"NUMBER(10,2)","FLOAT","NUMBER(10,2)",null,null,null,"avg_sect_sped ","FLOAT ","",",",null,"",null,null,null,"avg_sect_sped ","NUMBER(10,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitgturntypestats.","avg_sect_sped"," IS ","'평균구간속도'",";",null,null,""]
[null,14,null,"생성유닉스시각","crt_unix_tm","INT","NUMBER",10,"Y",0,"생성유닉스시각",null,"NUMBER(10)","INT","NUMBER(10)",null,null,null,"crt_unix_tm ","INT ","",",",null,"",null,null,null,"crt_unix_tm ","NUMBER(10) ","",{"$f":"\") TABLESPACE \"&AF181&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_G003 NOLOGGING"},null,null,"",null,"COMMENT ON COLUMN ","soitgturntypestats.","crt_unix_tm"," IS ","'생성유닉스시각'",";",null,null,""]
[{"$nulls":18},{"$f":"CONCATENATE(W166:Y179)","v":{"$error":"#VALUE!"}},{"$nulls":4},"",null,null,null,{"$f":"CONCATENATE(AF180:AH180)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (stats_bgng_unix_tm) INTERVAL (86400) STORE IN (\"&AF181&\") (PARTITION BFR_\" & D162 & \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AF181&\");\"","v":"PARTITION BY RANGE (stats_bgng_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_G003) (PARTITION BFR_soitgturntypestats_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_G003);"},{"$f":"\"CREATE INDEX PK_\" & D162 & \" ON \" & D162 & CONCATENATE(AG166:AI177) & \" LOCAL (PARTITION BFR_\" & D170 & \"_20221101 TABLESPACE \"&AG181&\") TABLESPACE \"&AG181&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & D162 & \" ADD CONSTRAINT PK_\" & D162 & \" PRIMARY KEY \" & CONCATENATE(AG166:AI177) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":9},{"$error":"#VALUE!"}]
[{"$nulls":23},"",{"$nulls":7},"SOIT_D08_G003","SOIT_I08_G003",{"$nulls":10},""]
[null,"테이블명",null,"soitgkncrstats",{"$nulls":19},"",{"$nulls":19},""]
[null,"테이블설명",null,"차종별 통계",{"$nulls":19},"",{"$nulls":19},""]
[null,"참고사항",{"$nulls":21},"",{"$nulls":19},""]
[null,"NO","PK","논리명","물리명","VoltDB 타입","Tibero 타입","길이","NULL","기본값","비고",null,"형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE","soitgkncrstats",null," IS ",{"$f":"\"'\"&D183&\"'\"","v":"'차종별 통계'"},";",null,null,""]
[null,1,"PK","현장카메라ID","spot_camr_id","VARCHAR","VARCHAR2",10,"N",null,"현장카메라ID",null,"VARCHAR2(10)","VARCHAR(10)","VARCHAR2(10)",null,"CREATE TABLE ",{"$f":"D182&\" (\"","v":"soitgkncrstats ("},{"$f":"E186&\" \"","v":"spot_camr_id "},{"$f":"N186&\" \"","v":"VARCHAR(10) "},{"$f":"IF(I186=\"N\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(C186=\"PK\", C186=\"PK/FK\"), E186, \"\")","v":"spot_camr_id"},{"$f":"IF(OR(C187=\"PK\", C187=\"PK/FK\"), \",\", \"\")","v":","},"CREATE TABLE ",{"$f":"D182&\" (\"","v":"soitgkncrstats ("},{"$f":"E186&\" \"","v":"spot_camr_id "},{"$f":"O186&\" \"","v":"VARCHAR2(10) "},{"$f":"IF(I186=\"N\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(C186=\"PK\", C186=\"PK/FK\"), E186, \"\")","v":"spot_camr_id"},{"$f":"IF(OR(C187=\"PK\", C187=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ","soitgkncrstats.",{"$f":"E186","v":"spot_camr_id"}," IS ",{"$f":"\"'\"&K186&\"'\"","v":"'현장카메라ID'"},";",null,null,""]
[null,2,"PK","차종코드","kncr_cd","VARCHAR","VARCHAR2",10,"N",null,"차종(008)","( LBUS:대형버스, LTRUCK:대형트럭(4.5T이상), MBUS:미니버스,\nMOTOR:오토바이, MTRUCK:트럭(4.5T미만), PCAR:승용차 )","CHAR(10)","VARCHAR(10)","VARCHAR2(10)",null,null,null,"kncr_cd ","VARCHAR(10) ","NOT NULL",",",null,"kncr_cd",",",null,null,"kncr_cd ","VARCHAR2(10) ","NOT NULL",",",null,null,"kncr_cd",",","COMMENT ON COLUMN ","soitgkncrstats.","kncr_cd"," IS ","'차종(008)'",";",null,null,""]
[null,3,"PK","시간유형코드","hr_type_cd","VARCHAR","VARCHAR2",10,"N",null,"시간구분(011)","(1:신호현시, 2:1분단위, 3:5분단위)","CHAR(10)","VARCHAR(10)","VARCHAR2(10)",null,null,null,"hr_type_cd ","VARCHAR(10) ","NOT NULL",",",null,"hr_type_cd",",",null,null,"hr_type_cd ","VARCHAR2(10) ","NOT NULL",",",null,null,"hr_type_cd",",","COMMENT ON COLUMN ","soitgkncrstats.","hr_type_cd"," IS ","'시간구분(011)'",";",null,null,""]
[null,4,"PK","통계시작유닉스시각","stats_bgng_unix_tm","INT","NUMBER",10,"N","0","통계시작유닉스시각",null,"NUMBER(10)","INT","NUMBER(10)",null,null,null,"stats_bgng_unix_tm ","INT ","NOT NULL",",",null,"stats_bgng_unix_tm",",",null,null,"stats_bgng_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"stats_bgng_unix_tm",",","COMMENT ON COLUMN ","soitgkncrstats.","stats_bgng_unix_tm"," IS ","'통계시작유닉스시각'",";",null,null,""]
[null,5,"PK","통계종료유닉스시각","stats_end_unix_tm","INT","NUMBER",10,"N","0","통계종료유닉스시각",null,"NUMBER(10)","INT","NUMBER(10)",null,null,null,"stats_end_unix_tm ","INT ","NOT NULL",",",null,"stats_end_unix_tm","));",null,null,"stats_end_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"stats_end_unix_tm",")","COMMENT ON COLUMN ","soitgkncrstats.","stats_end_unix_tm"," IS ","'통계종료유닉스시각'",";",null,null,""]
[null,6,null,"총교통량","totl_trvl","INT","NUMBER",10,"Y","0","총교통량",null,"NUMBER(10)","INT","NUMBER(10)",null,null,null,"totl_trvl ","INT ","",",",null,"",null,null,null,"totl_trvl ","NUMBER(10) ","",",",null,null,"",{"$f":"IF(OR(C192=\"PK\", C192=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitgkncrstats.","totl_trvl"," IS ","'총교통량'",";",null,null,""]
[null,7,null,"평균정지선검지속도","avg_stln_dttn_sped","FLOAT","NUMBER","10,2","Y","0.00","평균정지선검지속도",null,"NUMBER(10,2)","FLOAT","NUMBER(10,2)",null,null,null,"avg_stln_dttn_sped ","FLOAT ","",",",null,"",null,null,null,"avg_stln_dttn_sped ","NUMBER(10,2) ","",",",null,null,"","","COMMENT ON COLUMN ","soitgkncrstats.","avg_stln_dttn_sped"," IS ","'평균정지선검지속도'",";",null,null,""]
[null,8,null,"평균구간속도","avg_sect_sped","FLOAT","NUMBER","10,2","Y",0,"평균구간속도",null,"NUMBER(10,2)","FLOAT","NUMBER(10,2)",null,null,null,"avg_sect_sped ","FLOAT ","",",",null,"",null,null,null,"avg_sect_sped ","NUMBER(10,2) ","",",",null,null,"","","COMMENT ON COLUMN ","soitgkncrstats.","avg_sect_sped"," IS ","'평균구간속도'",";",null,null,""]
[null,9,null,"생성유닉스시각","crt_unix_tm","INT","NUMBER",10,"Y",0,"생성유닉스시각",null,"NUMBER(10)","INT","NUMBER(10)",null,null,null,"crt_unix_tm ","INT ","",",",null,"",null,null,null,"crt_unix_tm ","NUMBER(10) ","",{"$f":"\") TABLESPACE \"&AF196&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_G003 NOLOGGING"},null,null,"",null,"COMMENT ON COLUMN ","soitgkncrstats.","crt_unix_tm"," IS ","'생성유닉스시각'",";",null,null,""]
[{"$nulls":18},{"$f":"CONCATENATE(W186:Y194)","v":{"$error":"#VALUE!"}}," ","",null,null,"",null,null,null,{"$f":"CONCATENATE(AF195:AH195)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (stats_bgng_unix_tm) INTERVAL (86400) STORE IN (\"&AF196&\") (PARTITION BFR_\" & D182 & \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AF196&\");\"","v":"PARTITION BY RANGE (stats_bgng_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_G003) (PARTITION BFR_soitgkncrstats_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_G003);"},{"$f":"\"CREATE INDEX PK_\" & D182 & \" ON \" & D182 & CONCATENATE(AG186:AI193) & \" LOCAL (PARTITION BFR_\" & D185 & \"_20221101 TABLESPACE \"&AG196&\") TABLESPACE \"&AG196&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & D182 & \" ADD CONSTRAINT PK_\" & D182 & \" PRIMARY KEY \" & CONCATENATE(AG186:AI193) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":9},{"$error":"#VALUE!"}]
[{"$nulls":23},"",{"$nulls":7},"SOIT_D08_G003","SOIT_I08_G003",{"$nulls":10},""]
[null,"테이블명",null,"soitglanestats",{"$nulls":19},"",{"$nulls":19},""]
[null,"테이블설명",null,"차로별 통계",{"$nulls":19},"",{"$nulls":19},""]
[null,"참고사항",{"$nulls":21},"",{"$nulls":19},""]
[null,"NO","PK","논리명","물리명","VoltDB 타입","Tibero 타입","길이","NULL","기본값","비고",null,"형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE","soitglanestats",null," IS ",{"$f":"\"'\"&D198&\"'\"","v":"'차로별 통계'"},";",null,null,""]
[null,1,"PK","현장카메라ID","spot_camr_id","VARCHAR","VARCHAR2",10,"N",null,"현장카메라ID",null,"VARCHAR2(10)","VARCHAR(10)","VARCHAR2(10)",null,"CREATE TABLE ",{"$f":"D197&\" (\"","v":"soitglanestats ("},{"$f":"E201&\" \"","v":"spot_camr_id "},{"$f":"N201&\" \"","v":"VARCHAR(10) "},{"$f":"IF(I201=\"N\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(C201=\"PK\", C201=\"PK/FK\"), E201, \"\")","v":"spot_camr_id"},{"$f":"IF(OR(C202=\"PK\", C202=\"PK/FK\"), \",\", \"\")","v":","},"CREATE TABLE ",{"$f":"D197&\" (\"","v":"soitglanestats ("},{"$f":"E201&\" \"","v":"spot_camr_id "},{"$f":"O201&\" \"","v":"VARCHAR2(10) "},{"$f":"IF(I201=\"N\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(C201=\"PK\", C201=\"PK/FK\"), E201, \"\")","v":"spot_camr_id"},{"$f":"IF(OR(C202=\"PK\", C202=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ","soitglanestats.",{"$f":"E201","v":"spot_camr_id"}," IS ",{"$f":"\"'\"&K201&\"'\"","v":"'현장카메라ID'"},";",null,null,""]
[null,2,"PK","차로번호","lane_no","TINYINT","NUMBER",2,"N","1","차로번호(중앙선으로부터 1, 2, 3) 글로벌브릿지 재확인필요",null,"NUMBER(2)","TINYINT","NUMBER(2)",null,null,null,"lane_no ","TINYINT ","NOT NULL",",",null,"lane_no",",",null,null,"lane_no ","NUMBER(2) ","NOT NULL",",",null,null,"lane_no",",","COMMENT ON COLUMN ","soitglanestats.","lane_no"," IS ","'차로번호(중앙선으로부터 1, 2, 3) 글로벌브릿지 재확인필요'",";",null,null,""]
[null,3,"PK","시간유형코드","hr_type_cd","VARCHAR","VARCHAR2",10,"N",null,"시간구분(011)","5분단위","CHAR(10)","VARCHAR(10)","VARCHAR2(10)",null,null,null,"hr_type_cd ","VARCHAR(10) ","NOT NULL",",",null,"hr_type_cd",",",null,null,"hr_type_cd ","VARCHAR2(10) ","NOT NULL",",",null,null,"hr_type_cd",",","COMMENT ON COLUMN ","soitglanestats.","hr_type_cd"," IS ","'시간구분(011)'",";",null,null,""]
[null,4,"PK","통계시작유닉스시각","stats_bgng_unix_tm","INT","NUMBER",10,"N","0","통계시작유닉스시각",null,"NUMBER(10)","INT","NUMBER(10)",null,null,null,"stats_bgng_unix_tm ","INT ","NOT NULL",",",null,"stats_bgng_unix_tm",",",null,null,"stats_bgng_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"stats_bgng_unix_tm",",","COMMENT ON COLUMN ","soitglanestats.","stats_bgng_unix_tm"," IS ","'통계시작유닉스시각'",";",null,null,""]
[null,5,"PK","통계종료유닉스시각","stats_end_unix_tm","INT","NUMBER",10,"N","0","통계종료유닉스시각",null,"NUMBER(10)","INT","NUMBER(10)",null,null,null,"stats_end_unix_tm ","INT ","NOT NULL",",",null,"stats_end_unix_tm","));",null,null,"stats_end_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"stats_end_unix_tm",")","COMMENT ON COLUMN ","soitglanestats.","stats_end_unix_tm"," IS ","'통계종료유닉스시각'",";",null,null,""]
[null,6,null,"총교통량","totl_trvl","INT","NUMBER",10,"Y","0","총교통량",null,"NUMBER(10)","INT","NUMBER(10)",null,null,null,"totl_trvl ","INT ","",",",null,"",null,null,null,"totl_trvl ","NUMBER(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitglanestats.","totl_trvl"," IS ","'총교통량'",";",null,null,""]
[null,7,null,"평균정지선검지속도","avg_stln_dttn_sped","FLOAT","NUMBER","10,2","Y","0.00","평균정지선검지속도",null,"NUMBER(10,2)","FLOAT","NUMBER(10,2)",null,null,null,"avg_stln_dttn_sped ","FLOAT ","",",",null,"",null,null,null,"avg_stln_dttn_sped ","NUMBER(10,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitglanestats.","avg_stln_dttn_sped"," IS ","'평균정지선검지속도'",";",null,null,""]
[null,8,null,"평균구간속도","avg_sect_sped","FLOAT","NUMBER","10,2","Y","0.00","평균구간속도",null,"NUMBER(10,2)","FLOAT","NUMBER(10,2)",null,null,null,"avg_sect_sped ","FLOAT ","",",",null,"",null,null,null,"avg_sect_sped ","NUMBER(10,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitglanestats.","avg_sect_sped"," IS ","'평균구간속도'",";",null,null,""]
[null,9,null,"평균교통밀도","avg_trfc_dnst","SMALLINT","NUMBER",5,"Y","0","평균교통밀도(단위:대/km/차선)",null,"NUMBER(5)","SMALLINT","NUMBER(5)",null,null,null,"avg_trfc_dnst ","SMALLINT ","",",",null,"",null,null,null,"avg_trfc_dnst ","NUMBER(5) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitglanestats.","avg_trfc_dnst"," IS ","'평균교통밀도(단위:대/km/차선)'",";",null,null,""]
[null,10,null,"최소교통밀도","min_trfc_dnst","SMALLINT","NUMBER",5,"Y","0","최소교통밀도(단위:대/km/차선)",null,"NUMBER(5)","SMALLINT","NUMBER(5)",null,null,null,"min_trfc_dnst ","SMALLINT ","",",",null,"",null,null,null,"min_trfc_dnst ","NUMBER(5) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitglanestats.","min_trfc_dnst"," IS ","'최소교통밀도(단위:대/km/차선)'",";",null,null,""]
[null,11,null,"최대교통밀도","max_trfc_dnst","SMALLINT","NUMBER",5,"Y","0","최대교통밀도(단위:대/km/차선)",null,"NUMBER(5)","SMALLINT","NUMBER(5)",null,null,null,"max_trfc_dnst ","SMALLINT ","",",",null,"",null,null,null,"max_trfc_dnst ","NUMBER(5) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitglanestats.","max_trfc_dnst"," IS ","'최대교통밀도(단위:대/km/차선)'",";",null,null,""]
[null,12,null,"점유율","ocpn_rt","DECIMAL","NUMBER","12,9","Y",0,"점유율(전체차량점유시간/단위시간/차로)",null,"NUMBER(12,9)","DECIMAL(12,9)","NUMBER(12,9)",null,null,null,"ocpn_rt ","DECIMAL(12,9) ","",",",null,"",null,null,null,"ocpn_rt ","NUMBER(12,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitglanestats.","ocpn_rt"," IS ","'점유율(전체차량점유시간/단위시간/차로)'",";",null,null,""]
[null,13,null,"생성유닉스시각","crt_unix_tm","INT","NUMBER",10,"Y",0,"생성유닉스시각",null,"NUMBER(10)","INT","NUMBER(10)",null,null,null,"crt_unix_tm ","INT ","",",",null,"",null,null,null,"crt_unix_tm ","NUMBER(10) ","",{"$f":"\") TABLESPACE \"&AF215&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_G003 NOLOGGING"},null,null,{"$f":"IF(OR(C213=\"PK\", C213=\"PK/FK\"), E213, \"\")","v":""},null,"COMMENT ON COLUMN ","soitglanestats.","crt_unix_tm"," IS ","'생성유닉스시각'",";",null,null,""]
[{"$nulls":18},{"$f":"CONCATENATE(W201:Y213)","v":{"$error":"#VALUE!"}}," ","",null,null,"",null,null,null,{"$f":"CONCATENATE(AF214:AH214)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (stats_bgng_unix_tm) INTERVAL (86400) STORE IN (\"&AF215&\") (PARTITION BFR_\" & D197 & \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AF215&\");\"","v":"PARTITION BY RANGE (stats_bgng_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_G003) (PARTITION BFR_soitglanestats_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_G003);"},{"$f":"\"CREATE INDEX PK_\" & D197 & \" ON \" & D197 & CONCATENATE(AG201:AI209) & \" LOCAL (PARTITION BFR_\" & D197 & \"_20221101 TABLESPACE \"&AG215&\") TABLESPACE \"&AG215&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & D197 & \" ADD CONSTRAINT PK_\" & D197 & \" PRIMARY KEY \" & CONCATENATE(AG201:AI210) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":9},{"$error":"#VALUE!"}]
[{"$nulls":23},"",{"$nulls":7},"SOIT_D08_G003","SOIT_I08_G003",{"$nulls":10},""]
[null,"테이블명",null,"soitgaprdqueu",{"$nulls":19},"",{"$nulls":19},""]
[null,"테이블설명",null,"접근로별 대기행렬(신호 1주기)",{"$nulls":19},"",{"$nulls":19},""]
[null,"참고사항",{"$nulls":21},"",{"$nulls":19},""]
[null,"NO","PK","논리명","물리명","VoltDB 타입","Tibero 타입","길이","NULL","기본값","비고",null,"형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE","soitgaprdqueu",null," IS ",{"$f":"\"'\"&D217&\"'\"","v":"'접근로별 대기행렬(신호 1주기)'"},";",null,null,""]
[null,1,"PK","현장카메라ID","spot_camr_id","VARCHAR","VARCHAR2",10,"N",null,"현장카메라ID",null,"VARCHAR2(10)","VARCHAR(10)","VARCHAR2(10)",null,"CREATE TABLE ",{"$f":"D216&\" (\"","v":"soitgaprdqueu ("},{"$f":"E220&\" \"","v":"spot_camr_id "},{"$f":"N220&\" \"","v":"VARCHAR(10) "},{"$f":"IF(I220=\"N\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(C220=\"PK\", C220=\"PK/FK\"), E220, \"\")","v":"spot_camr_id"},{"$f":"IF(OR(C221=\"PK\", C221=\"PK/FK\"), \",\", \"\")","v":","},"CREATE TABLE ",{"$f":"D216&\" (\"","v":"soitgaprdqueu ("},{"$f":"E220&\" \"","v":"spot_camr_id "},{"$f":"O220&\" \"","v":"VARCHAR2(10) "},{"$f":"IF(I220=\"N\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(C220=\"PK\", C220=\"PK/FK\"), E220, \"\")","v":"spot_camr_id"},{"$f":"IF(OR(C221=\"PK\", C221=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ","soitgaprdqueu.",{"$f":"E220","v":"spot_camr_id"}," IS ",{"$f":"\"'\"&K220&\"'\"","v":"'현장카메라ID'"},";",null,null,""]
[null,2,"PK","통계시작유닉스시각","stats_bgng_unix_tm","INT","NUMBER",10,"N",0,"통계시작유닉스시각",null,"NUMBER(10)","INT","NUMBER(10)",null,null,null,"stats_bgng_unix_tm ","INT ","NOT NULL",",",null,"stats_bgng_unix_tm",",",null,null,"stats_bgng_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"stats_bgng_unix_tm",",","COMMENT ON COLUMN ","soitgaprdqueu.","stats_bgng_unix_tm"," IS ","'통계시작유닉스시각'",";",null,null,""]
[null,3,"PK","통계종료유닉스시각","stats_end_unix_tm","INT","NUMBER",10,"N",0,"통계종료유닉스시각",null,"NUMBER(10)","INT","NUMBER(10)",null,null,null,"stats_end_unix_tm ","INT ","NOT NULL",",",null,"stats_end_unix_tm","));",null,null,"stats_end_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"stats_end_unix_tm",")","COMMENT ON COLUMN ","soitgaprdqueu.","stats_end_unix_tm"," IS ","'통계종료유닉스시각'",";",null,null,""]
[null,4,null,"잔여대기행렬길이","rmnn_queu_lngt","DECIMAL","NUMBER","19,9","Y",0,"잔여대기행렬길이",null,"NUMBER(19,9)","DECIMAL(19,9)","NUMBER(19,9)",null,null,null,"rmnn_queu_lngt ","DECIMAL(19,9) ","",",",null,"",null,null,null,"rmnn_queu_lngt ","NUMBER(19,9) ","",",",null,null,"",{"$f":"IF(OR(C224=\"PK\", C224=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitgaprdqueu.","rmnn_queu_lngt"," IS ","'잔여대기행렬길이'",";",null,null,""]
[null,5,null,"최대대기행렬길이","max_queu_lngt","DECIMAL","NUMBER","19,9","Y",0,"최대대기행렬길이",null,"NUMBER(19,9)","DECIMAL(19,9)","NUMBER(19,9)",null,null,null,"max_queu_lngt ","DECIMAL(19,9) ","",",",null,"",null,null,null,"max_queu_lngt ","NUMBER(19,9) ","",",",null,null,"",{"$f":"IF(OR(C227=\"PK\", C227=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitgaprdqueu.","max_queu_lngt"," IS ","'최대대기행렬길이'",";",null,null,""]
[null,6,null,"이미지경로명","img_path_nm","VARCHAR","VARCHAR2",80,"Y",null,"이미지경로명",null,"VARCHAR2(80)","VARCHAR(80)","VARCHAR2(80)",null,null,null,"img_path_nm ","VARCHAR(80) ","",",",{"$nulls":5},"img_path_nm ","VARCHAR2(80) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitgaprdqueu.","img_path_nm"," IS ","'이미지경로명'",";",null,null,""]
[null,7,null,"이미지파일명","img_file_nm","VARCHAR","VARCHAR2",80,"Y",null,"이미지파일명",null,"VARCHAR2(80)","VARCHAR(80)","VARCHAR2(80)",null,null,null,"img_file_nm ","VARCHAR(80) ","",",",{"$nulls":5},"img_file_nm ","VARCHAR2(80) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitgaprdqueu.","img_file_nm"," IS ","'이미지파일명'",";",null,null,""]
[null,8,null,"생성유닉스시각","crt_unix_tm","INT","NUMBER",10,"Y",0,"생성유닉스시각",null,"NUMBER(10)","INT","NUMBER(10)",null,null,null,"crt_unix_tm ","INT ","",",",null,{"$f":"IF(OR(C227=\"PK\", C227=\"PK/FK\"), E227, \"\")","v":""},null,null,null,"crt_unix_tm ","NUMBER(10) ","",{"$f":"\") TABLESPACE \"&AF229&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_G003 NOLOGGING"},null,null,{"$f":"IF(OR(C227=\"PK\", C227=\"PK/FK\"), E227, \"\")","v":""},null,"COMMENT ON COLUMN ","soitgaprdqueu.","crt_unix_tm"," IS ","'생성유닉스시각'",";",null,null,""]
[{"$nulls":18},{"$f":"CONCATENATE(W219:Y227)","v":{"$error":"#VALUE!"}}," ",null,null,null,"",null,null,null,{"$f":"CONCATENATE(AF228:AH228)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (stats_bgng_unix_tm) INTERVAL (86400) STORE IN (\"&AF229&\") (PARTITION BFR_\" & D216 & \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AF229&\");\"","v":"PARTITION BY RANGE (stats_bgng_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_G003) (PARTITION BFR_soitgaprdqueu_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_G003);"},{"$f":"\"CREATE INDEX PK_\" & D216 & \" ON \" & D216 & CONCATENATE(AG220:AI226) & \" LOCAL (PARTITION BFR_\" & D216 & \"_20221101 TABLESPACE \"&AG229&\") TABLESPACE \"&AG229&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & D216 & \" ADD CONSTRAINT PK_\" & D216 & \" PRIMARY KEY \" & CONCATENATE(AG220:AI226) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":9},{"$error":"#VALUE!"}]
[{"$nulls":18},{"$f":"E229&\" \"","v":" "}," ",null,null,null,"",{"$nulls":7},"SOIT_D08_G003","SOIT_I08_G003",{"$f":"IF(OR(C229=\"PK\", C229=\"PK/FK\"), E229, \"\")","v":""},{"$nulls":9},""]
[null,"테이블명",null,"soitglanequeu",{"$nulls":19},"",{"$nulls":9},"",{"$nulls":9},""]
[null,"테이블설명",null,"차로별 대기행렬(신호 1주기)",{"$nulls":19},"",{"$nulls":19},""]
[null,"참고사항",{"$nulls":21},"",{"$nulls":19},""]
[null,"NO","PK","논리명","물리명","VoltDB 타입","Tibero 타입","길이","NULL","기본값","비고",null,"형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE","soitgaprdqueu",null," IS ",{"$f":"\"'\"&D231&\"'\"","v":"'차로별 대기행렬(신호 1주기)'"},";",null,null,""]
[null,1,"PK","현장카메라ID","spot_camr_id","VARCHAR","VARCHAR2",10,"N",null,"현장카메라ID",null,"VARCHAR2(10)","VARCHAR(10)","VARCHAR2(10)",null,"CREATE TABLE ",{"$f":"D230&\" (\"","v":"soitglanequeu ("},{"$f":"E234&\" \"","v":"spot_camr_id "},{"$f":"N234&\" \"","v":"VARCHAR(10) "},{"$f":"IF(I234=\"N\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(C234=\"PK\", C234=\"PK/FK\"), E234, \"\")","v":"spot_camr_id"},{"$f":"IF(OR(C235=\"PK\", C235=\"PK/FK\"), \",\", \"\")","v":","},"CREATE TABLE ",{"$f":"D230&\" (\"","v":"soitglanequeu ("},{"$f":"E234&\" \"","v":"spot_camr_id "},{"$f":"O234&\" \"","v":"VARCHAR2(10) "},{"$f":"IF(I234=\"N\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(C234=\"PK\", C234=\"PK/FK\"), E234, \"\")","v":"spot_camr_id"},{"$f":"IF(OR(C235=\"PK\", C235=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ","soitglanequeu.",{"$f":"E234","v":"spot_camr_id"}," IS ",{"$f":"\"'\"&K234&\"'\"","v":"'현장카메라ID'"},";",null,null,""]
[null,2,"PK","차로번호","lane_no","TINYINT","NUMBER",2,"N",1,"차로번호(중앙선으로부터 1, 2, 3) 글로벌브릿지 재확인필요",null,"NUMBER(2)","TINYINT","NUMBER(2)",null,null,null,"lane_no ","TINYINT ","NOT NULL",",",null,"lane_no",",",null,null,"lane_no ","NUMBER(2) ","NOT NULL",",",null,null,"lane_no",",","COMMENT ON COLUMN ","soitglanequeu.","lane_no"," IS ","'차로번호(중앙선으로부터 1, 2, 3) 글로벌브릿지 재확인필요'",";",null,null,""]
[null,3,"PK","통계시작유닉스시각","stats_bgng_unix_tm","INT","NUMBER",10,"N",0,"통계시작유닉스시각",null,"NUMBER(10)","INT","NUMBER(10)",null,null,null,"stats_bgng_unix_tm ","INT ","NOT NULL",",",null,"stats_bgng_unix_tm",",",null,null,"stats_bgng_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"stats_bgng_unix_tm",",","COMMENT ON COLUMN ","soitglanequeu.","stats_bgng_unix_tm"," IS ","'통계시작유닉스시각'",";",null,null,""]
[null,4,"PK","통계종료유닉스시각","stats_end_unix_tm","INT","NUMBER",10,"N",0,"통계종료유닉스시각",null,"NUMBER(10)","INT","NUMBER(10)",null,null,null,"stats_end_unix_tm ","INT ","NOT NULL",",",null,"stats_end_unix_tm","));",null,null,"stats_end_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"stats_end_unix_tm",")","COMMENT ON COLUMN ","soitglanequeu.","stats_end_unix_tm"," IS ","'통계종료유닉스시각'",";",null,null,""]
[null,5,null,"잔여대기행렬길이","rmnn_queu_lngt","DECIMAL","NUMBER","19,9","Y",0,"잔여대기행렬길이",null,"NUMBER(19,9)","DECIMAL(19,9)","NUMBER(19,9)",null,null,null,"rmnn_queu_lngt ","DECIMAL(19,9) ","",",",null,"",{"$f":"IF(OR(C239=\"PK\", C239=\"PK/FK\"), \",\", \"\")","v":""},null,null,"rmnn_queu_lngt ","NUMBER(19,9) ","",",",null,null,null,{"$f":"IF(OR(C239=\"PK\", C239=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitglanequeu.","rmnn_queu_lngt"," IS ","'잔여대기행렬길이'",";",null,null,""]
[null,6,null,"최대대기행렬길이","max_queu_lngt","DECIMAL","NUMBER","19,9","Y",0,"최대대기행렬길이",null,"NUMBER(19,9)","DECIMAL(19,9)","NUMBER(19,9)",null,null,null,"max_queu_lngt ","DECIMAL(19,9) ","",",",null,"",{"$f":"IF(OR(C242=\"PK\", C242=\"PK/FK\"), \",\", \"\")","v":""},null,null,"max_queu_lngt ","NUMBER(19,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitglanequeu.","max_queu_lngt"," IS ","'최대대기행렬길이'",";",null,null,""]
[null,7,null,"이미지경로명","img_path_nm","VARCHAR","VARCHAR2",80,"Y",null,"이미지경로명",null,"VARCHAR2(80)","VARCHAR(80)","VARCHAR2(80)",null,null,null,"img_path_nm ","VARCHAR(80) ","",",",{"$nulls":5},"img_path_nm ","VARCHAR2(80) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitglanequeu.","img_path_nm"," IS ","'이미지경로명'",";",null,null,""]
[null,8,null,"이미지파일명","img_file_nm","VARCHAR","VARCHAR2",80,"Y",null,"이미지파일명",null,"VARCHAR2(80)","VARCHAR(80)","VARCHAR2(80)",null,null,null,"img_file_nm ","VARCHAR(80) ","",",",{"$nulls":5},"img_file_nm ","VARCHAR2(80) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitglanequeu.","img_file_nm"," IS ","'이미지파일명'",";",null,null,""]
[null,9,null,"생성유닉스시각","crt_unix_tm","INT","NUMBER",10,"Y",0,"생성유닉스시각",null,"NUMBER(10)","INT","NUMBER(10)",null,null,null,"crt_unix_tm ","INT ","",",",null,{"$f":"IF(OR(C242=\"PK\", C242=\"PK/FK\"), E242, \"\")","v":""},{"$f":"IF(OR(C243=\"PK\", C243=\"PK/FK\"), \",\", \"\")","v":""},null,null,"crt_unix_tm ","NUMBER(10) ","",{"$f":"\") TABLESPACE \"&AF244&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_G003 NOLOGGING"},null,null,{"$f":"IF(OR(C242=\"PK\", C242=\"PK/FK\"), E242, \"\")","v":""},null,"COMMENT ON COLUMN ","soitglanequeu.","crt_unix_tm"," IS ","'생성유닉스시각'",";",null,null,""]
[{"$nulls":18},{"$f":"CONCATENATE(W234:Y242)","v":{"$error":"#VALUE!"}}," ","",null,null,"","",null,null,{"$f":"CONCATENATE(AF243:AH243)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (stats_bgng_unix_tm) INTERVAL (86400) STORE IN (\"&AF244&\") (PARTITION BFR_\" & D230 & \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AF244&\");\"","v":"PARTITION BY RANGE (stats_bgng_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_G003) (PARTITION BFR_soitglanequeu_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_G003);"},{"$f":"\"CREATE INDEX PK_\" & D230 & \" ON \" & D230 & CONCATENATE(AG234:AI241) & \" LOCAL (PARTITION BFR_\" & D230 & \"_20221101 TABLESPACE \"&AG244&\") TABLESPACE \"&AG244&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & D230 & \" ADD CONSTRAINT PK_\" & D230 & \" PRIMARY KEY \" & CONCATENATE(AG234:AI241) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":9},{"$error":"#VALUE!"}]
[{"$nulls":23},"",{"$nulls":7},"SOIT_D08_G003","SOIT_I08_G003",{"$nulls":10},""]
[null,"테이블명",null,"soitgenclsttsinfo",{"$nulls":19},"",{"$nulls":19},""]
[null,"테이블설명",null,"함체 상태정보",{"$nulls":19},"",{"$nulls":19},""]
[null,"참고사항",null,"5분 주기로 INSERT 한다.",{"$nulls":19},"",{"$nulls":19},""]
[null,"NO","PK","논리명","물리명","VoltDB 타입","Tibero 타입","길이","NULL","기본값","비고",null,"형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE","soitgenclsttsinfo",null," IS ",{"$f":"\"'\"&D246&\"'\"","v":"'함체 상태정보'"},";",null,null,""]
[null,1,"PK","현장교차로ID","spot_ints_id","SMALLINT","NUMBER",5,"N",0,"현장교차로ID",null,"NUMBER(5)","SMALLINT","NUMBER(5)",null,"CREATE TABLE ",{"$f":"D245&\" (\"","v":"soitgenclsttsinfo ("},{"$f":"E249&\" \"","v":"spot_ints_id "},{"$f":"N249&\" \"","v":"SMALLINT "},{"$f":"IF(I249=\"N\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(C249=\"PK\", C249=\"PK/FK\"), E249, \"\")","v":"spot_ints_id"},{"$f":"IF(OR(C250=\"PK\", C250=\"PK/FK\"), \",\", \"\")","v":","},"CREATE TABLE ",{"$f":"D245&\" (\"","v":"soitgenclsttsinfo ("},{"$f":"E249&\" \"","v":"spot_ints_id "},{"$f":"O249&\" \"","v":"NUMBER(5) "},{"$f":"IF(I249=\"N\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(C249=\"PK\", C249=\"PK/FK\"), E249, \"\")","v":"spot_ints_id"},{"$f":"IF(OR(C250=\"PK\", C250=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ","soitgenclsttsinfo.",{"$f":"E249","v":"spot_ints_id"}," IS ",{"$f":"\"'\"&K249&\"'\"","v":"'현장교차로ID'"},";",null,null,""]
[null,2,"PK","처리유닉스시각","prcs_unix_tm","INT","NUMBER",10,"Y",0,"처리유닉스시각",null,"NUMBER(10)","INT","NUMBER(10)",null,null,null,"prcs_unix_tm ","INT ","",",",null,"prcs_unix_tm","));",null,null,"prcs_unix_tm ","NUMBER(10) ","",",",null,null,"prcs_unix_tm",")","COMMENT ON COLUMN ","soitgenclsttsinfo.","prcs_unix_tm"," IS ","'처리유닉스시각'",";",null,null,""]
[null,3,null,"통신상태코드","cmnc_stts_cd","VARCHAR","VARCHAR2",1,"Y",0,"통신상태코드(701)","(0:정상 1:통신두절 2:통신없음)","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",null,null,null,"cmnc_stts_cd ","VARCHAR(1) ","",",",null,"",{"$f":"IF(OR(C252=\"PK\", C252=\"PK/FK\"), \",\", \"\")","v":""},null,null,"cmnc_stts_cd ","VARCHAR2(1) ","",",",null,null,"",{"$f":"IF(OR(C252=\"PK\", C252=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitgenclsttsinfo.","cmnc_stts_cd"," IS ","'통신상태코드(701)'",";",null,null,""]
[null,4,null,"장비상태코드","eqpm_stts_cd","VARCHAR","VARCHAR2",1,"Y",0,"장비상태코드(702)","(0:정상 1:카메라 이상 3:엣지모듈이상 4:기타오류)","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",null,null,null,"eqpm_stts_cd ","VARCHAR(1) ","",",",null,"",null,null,null,"eqpm_stts_cd ","VARCHAR2(1) ",null,",",null,null,"",null,"COMMENT ON COLUMN ","soitgenclsttsinfo.","eqpm_stts_cd"," IS ","'장비상태코드(702)'",";",null,null,""]
[null,5,null,"장비온도","eqpm_tmpt","SMALLINT","NUMBER",5,"Y",0,"장비온도(-40 ~ +80)",null,"NUMBER(3)","SMALLINT","NUMBER(3)",null,null,null,"eqpm_tmpt ","SMALLINT ","",",",null,"",null,null,null,"eqpm_tmpt ","NUMBER(3) ",null,",",null,null,"",null,"COMMENT ON COLUMN ","soitgenclsttsinfo.","eqpm_tmpt"," IS ","'장비온도(-40 ~ +80)'",";",null,null,""]
[null,6,null,"팬상태코드","pann_stts_cd","VARCHAR","VARCHAR2",1,"Y",0,"상태코드(015)","(0:정상 1: 이상)","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",null,null,null,"pann_stts_cd ","VARCHAR(1) ","",",",null,"",null,null,null,"pann_stts_cd ","VARCHAR2(1) ",null,",",null,null,"",null,"COMMENT ON COLUMN ","soitgenclsttsinfo.","pann_stts_cd"," IS ","'상태코드(015)'",";",null,null,""]
[null,7,null,"히터상태코드","hetr_stts_cd","VARCHAR","VARCHAR2",1,"Y",0,"히터상태코드(703)","(0:가동 1:중지 3:정보없음)","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",null,null,null,"hetr_stts_cd ","VARCHAR(1) ","",",",null,"",null,null,null,"hetr_stts_cd ","VARCHAR2(1) ",null,",",{"$nulls":4},"COMMENT ON COLUMN ","soitgenclsttsinfo.","hetr_stts_cd"," IS ","'히터상태코드(703)'",";",null,null,""]
[null,8,null,"함체개방여부","encl_open_yn","VARCHAR","VARCHAR2",1,"Y",0,"함체개방여부(704)","(0:닫힘 1:열림 3:정보없음)","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",null,null,null,"encl_open_yn ","VARCHAR(1) ","",",",null,"",null,null,null,"encl_open_yn ","VARCHAR2(1) ",null,",",{"$nulls":4},"COMMENT ON COLUMN ","soitgenclsttsinfo.","encl_open_yn"," IS ","'함체개방여부(704)'",";",null,null,""]
[null,9,null,"함체교체여부","encl_rplc_yn","VARCHAR","VARCHAR2",1,"N","Y","교체여부(016)","(Y:교체, N:미교체)","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",null,null,null,"encl_rplc_yn ","VARCHAR(1) ","NOT NULL",",",null,"",null,null,null,"encl_rplc_yn ","VARCHAR2(1) ",null,{"$f":"\") TABLESPACE \"&AF259&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_G003 NOLOGGING"},null,null,{"$f":"IF(OR(C257=\"PK\", C257=\"PK/FK\"), E257, \"\")","v":""},null,"COMMENT ON COLUMN ","soitgenclsttsinfo.","encl_rplc_yn"," IS ","'교체여부(016)'",";",null,null,""]
[{"$nulls":18},{"$f":"CONCATENATE(W249:Y257)","v":{"$error":"#VALUE!"}}," ","",null,null,"",null,null,null,{"$f":"CONCATENATE(AF258:AH258)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (prcs_unix_tm) INTERVAL (3600) STORE IN (\"&AF259&\") (PARTITION BFR_\" & D245 & \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AF259&\");\"","v":"PARTITION BY RANGE (prcs_unix_tm) INTERVAL (3600) STORE IN (SOIT_D08_G003) (PARTITION BFR_soitgenclsttsinfo_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_G003);"},{"$f":"\"CREATE INDEX PK_\" & D245 & \" ON \" & D245 & CONCATENATE(AG249:AI256) & \" LOCAL (PARTITION BFR_\" & D245 & \"_20221101 TABLESPACE \"&AG259&\") TABLESPACE \"&AG259&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & D245 & \" ADD CONSTRAINT PK_\" & D245 & \" PRIMARY KEY \" & CONCATENATE(AG249:AI256) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":9},{"$error":"#VALUE!"}]
[{"$nulls":23},{"$f":"IF(OR(C259=\"PK\", C259=\"PK/FK\"),#REF!, \"\")","v":""},{"$nulls":7},"SOIT_D08_G003","SOIT_I08_G003",{"$nulls":10},""]
[null,"테이블명",null,"soitgcamrsttsinfo",{"$nulls":19},{"$f":"IF(OR(C260=\"PK\", C260=\"PK/FK\"), E260, \"\")","v":""},{"$nulls":19},""]
[null,"테이블설명",null,"카메라 상태 정보",{"$nulls":19},"",{"$nulls":19},""]
[null,"참고사항",null,"5분 주기로 INSERT 한다.",{"$nulls":19},"",{"$nulls":19},""]
[null,"NO","PK","논리명","물리명","VoltDB 타입","Tibero 타입","길이","NULL","기본값","비고",null,"형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE","soitgcamrsttsinfo",null," IS ",{"$f":"\"'\"&D261&\"'\"","v":"'카메라 상태 정보'"},";",null,null,""]
[null,1,"PK","현장카메라ID","spot_camr_id","VARCHAR","VARCHAR2",10,"N",null,"현장카메라ID",null,"VARCHAR2(10)","VARCHAR(10)","VARCHAR2(10)",null,"CREATE TABLE ",{"$f":"D260&\" (\"","v":"soitgcamrsttsinfo ("},{"$f":"E264&\" \"","v":"spot_camr_id "},{"$f":"N264&\" \"","v":"VARCHAR(10) "},{"$f":"IF(I264=\"N\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(C264=\"PK\", C264=\"PK/FK\"), E264, \"\")","v":"spot_camr_id"},{"$f":"IF(OR(C265=\"PK\", C265=\"PK/FK\"), \",\", \"\")","v":","},"CREATE TABLE ",{"$f":"D260&\" (\"","v":"soitgcamrsttsinfo ("},{"$f":"E264&\" \"","v":"spot_camr_id "},{"$f":"O264&\" \"","v":"VARCHAR2(10) "},{"$f":"IF(I264=\"N\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(C264=\"PK\", C264=\"PK/FK\"), E264, \"\")","v":"spot_camr_id"},{"$f":"IF(OR(C265=\"PK\", C265=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ","soitgcamrsttsinfo.",{"$f":"E264","v":"spot_camr_id"}," IS ",{"$f":"\"'\"&K264&\"'\"","v":"'현장카메라ID'"},";",null,null,""]
[null,2,"PK","설치위치번호","instl_locn_no","VARCHAR","CHAR",2,"Y",null,"설치위치번호",null,"VARCHAR2(64)","VARCHAR(64)","VARCHAR2(64)",null,null,null,"instl_locn_no ","VARCHAR(64) ","",",",null,"instl_locn_no",",",null,null,"instl_locn_no ","VARCHAR2(64) ","",",",null,null,"instl_locn_no",",","COMMENT ON COLUMN ","soitgcamrsttsinfo.","instl_locn_no"," IS ","'설치위치번호'",";",null,null,""]
[null,3,"PK","처리유닉스시각","prcs_unix_tm","INT","NUMBER",10,"N",null,"처리유닉스시각",null,"NUMBER(10)","INT","NUMBER(10)",null,null,null,"prcs_unix_tm ","INT ","NOT NULL",",",null,"prcs_unix_tm","));",null,null,"prcs_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"prcs_unix_tm",")","COMMENT ON COLUMN ","soitgcamrsttsinfo.","prcs_unix_tm"," IS ","'처리유닉스시각'",";",null,null,""]
[null,4,null,"2K카메라 상태코드","camr_2k_stts_cd","VARCHAR","VARCHAR2",1,"Y",0,"2K카메라상태코드(705)","(0:정상 1:이상 3:통신단절 4:기타오류)","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",null,null,null,"camr_2k_stts_cd ","VARCHAR(1) ","",",",null,"",{"$f":"IF(OR(C268=\"PK\", C268=\"PK/FK\"), \",\", \"\")","v":""},null,null,"camr_2k_stts_cd ","VARCHAR2(1) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitgcamrsttsinfo.","camr_2k_stts_cd"," IS ","'2K카메라상태코드(705)'",";",null,null,""]
[null,5,null,"2Ke카메라 상태코드","ecamr_2k_stts_cd","VARCHAR","VARCHAR2",1,"Y",0,"2Ke카메라상태코드(705)","(0:정상 1:이상 3:통신단절 4:기타오류)","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",null,null,null,"ecamr_2k_stts_cd ","VARCHAR(1) ","",",",null,"","",null,null,"ecamr_2k_stts_cd ","VARCHAR2(1) ","",",",null,null,"",{"$f":"IF(OR(C269=\"PK\", C269=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitgcamrsttsinfo.","ecamr_2k_stts_cd"," IS ","'2Ke카메라상태코드(705)'",";",null,null,{"$f":"IF(LEFT(AB268, 13) = \"CONSTRAINT PK\", AB268, \"\")","v":""}]
[null,6,null,"4K카메라 상태코드","camr_4k_stts_cd","VARCHAR","VARCHAR2",1,"Y",0,"4K카메라상태코드(705)","(0:정상 1:이상 3:통신단절 4:기타오류)","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",null,null,null,"camr_4k_stts_cd ","VARCHAR(1) ","",",",null,"","",null,null,"camr_4k_stts_cd ","VARCHAR2(1) ","",",",null,null,"","","COMMENT ON COLUMN ","soitgcamrsttsinfo.","camr_4k_stts_cd"," IS ","'4K카메라상태코드(705)'",";",null,null,""]
[null,7,null,"4Ke카메라 상태코드","ecamr_4k_stts_cd","VARCHAR","VARCHAR2",1,"Y",0,"4Ke카메라상태코드(705)","(0:정상 1:이상 3:통신단절 4:기타오류)","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",null,null,null,"ecamr_4k_stts_cd ","VARCHAR(1) ","",",",null,"",null,null,null,"ecamr_4k_stts_cd ","VARCHAR2(1) ","",{"$f":"\") TABLESPACE \"&AF272&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_G003 NOLOGGING"},null,null,"",null,"COMMENT ON COLUMN ","soitgcamrsttsinfo.","ecamr_4k_stts_cd"," IS ","'4Ke카메라상태코드(705)'",";",null,null,""]
[{"$nulls":18},{"$f":"CONCATENATE(W298:Y308)","v":{"$error":"#VALUE!"}}," ",null,null,null,"",null,null,null,{"$f":"CONCATENATE(AF271:AH271)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (prcs_unix_tm) INTERVAL (3600) STORE IN (\"&AF272&\") (PARTITION BFR_\" & D260 & \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AF272&\");\"","v":"PARTITION BY RANGE (prcs_unix_tm) INTERVAL (3600) STORE IN (SOIT_D08_G003) (PARTITION BFR_soitgcamrsttsinfo_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_G003);"},{"$f":"\"CREATE INDEX PK_\" & D260 & \" ON \" & D260 & CONCATENATE(AG264:AI269) & \" LOCAL (PARTITION BFR_\" & D258 & \"_20221101 TABLESPACE \"&AG272&\") TABLESPACE \"&AG272&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & D260 & \" ADD CONSTRAINT PK_\" & D260 & \" PRIMARY KEY \" & CONCATENATE(AG264:AI269) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":9},{"$error":"#VALUE!"}]
[{"$nulls":18},{"$f":"E272&\" \"","v":" "}," ",null,null,null,"",{"$nulls":7},"SOIT_D08_G003","SOIT_I08_G003",{"$nulls":10},""]
[null,"테이블명",null,"soitgrtmdtinfo_2K",{"$nulls":19},"",{"$nulls":19},""]
[null,"테이블설명",null,"2K 실시간 차량검지 정보",{"$nulls":19},"",{"$nulls":19},""]
[null,"참고사항",{"$nulls":21},"",{"$nulls":19},""]
[null,"NO","PK","논리명","물리명","VoltDB 타입","Tibero 타입","길이","NULL","기본값","비고",null,"형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE","soitgrtmdtinfo_2k",null," IS ",{"$f":"\"'\"&D274&\"'\"","v":"'2K 실시간 차량검지 정보'"},";",null,null,""]
[null,1,"PK","현장카메라ID","spot_camr_id","VARCHAR","VARCHAR2",10,"N",null,"현장카메라ID",null,"VARCHAR2(10)","VARCHAR(10)","티베로 안씀",null,"CREATE TABLE ",{"$f":"D273&\" (\"","v":"soitgrtmdtinfo_2K ("},{"$f":"E277&\" \"","v":"spot_camr_id "},{"$f":"N277&\" \"","v":"VARCHAR(10) "},{"$f":"IF(I277=\"N\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(C277=\"PK\", C277=\"PK/FK\"), E277, \"\")","v":"spot_camr_id"},{"$f":"IF(OR(C278=\"PK\", C278=\"PK/FK\"), \",\", \"\")","v":","},{"$nulls":10},"COMMENT ON COLUMN ","soitgrtmdtinfo_2k.",{"$f":"E277","v":"spot_camr_id"}," IS ",{"$f":"\"'\"&K277&\"'\"","v":"'현장카메라ID'"},";",null,null,""]
[null,2,"PK","차종코드","kncr_cd","VARCHAR","CHAR",10,"N",null,"차종(008)","( LBUS:대형버스, LTRUCK:대형트럭(4.5T이상), MBUS:미니버스,\nMOTOR:오토바이, MTRUCK:트럭(4.5T미만), PCAR:승용차 )","CHAR(10)","VARCHAR(10)",{"$nulls":4},"kncr_cd ","VARCHAR(10) ","NOT NULL",",",null,"kncr_cd",",",{"$nulls":10},"COMMENT ON COLUMN ","soitgrtmdtinfo_2k.","kncr_cd"," IS ","'차종(008)'",";",null,null,""]
[null,3,"PK","차로번호","lane_no","TINYINT","NUMBER",2,"N",1,"차로번호",null,"NUMBER(2)","TINYINT",{"$nulls":4},"lane_no ","TINYINT ","NOT NULL",",",null,"lane_no",",",{"$nulls":10},"COMMENT ON COLUMN ","soitgrtmdtinfo_2k.","lane_no"," IS ","'차로번호'",";",null,null,""]
[null,4,"PK","회전유형코드","turn_type_cd","VARCHAR","CHAR",10,"N",null,"회전유형코드(700)","( 11:직진, 21:작은좌회전, 22:큰좌회전, 31:작은우회전, 32:큰우회전, 41:유턴)","CHAR(10)","VARCHAR(10)",{"$nulls":4},"turn_type_cd ","VARCHAR(10) ","NOT NULL",",",null,"turn_type_cd",",",{"$nulls":10},"COMMENT ON COLUMN ","soitgrtmdtinfo_2k.","turn_type_cd"," IS ","'회전유형코드(700)'",";",null,null,""]
[null,5,"PK","회전검지유닉스시각","turn_dttn_unix_tm","INT","NUMBER",10,"N",0,"회전검지유닉스시각",null,"NUMBER(10)","INT",{"$nulls":4},"turn_dttn_unix_tm ","INT ","NOT NULL",",",null,"turn_dttn_unix_tm","",{"$nulls":10},"COMMENT ON COLUMN ","soitgrtmdtinfo_2k.","turn_dttn_unix_tm"," IS ","'회전검지유닉스시각'",";",null,null,""]
[null,6,null,"회전검지속도","turn_dttn_sped","FLOAT","NUMBER","10,2","Y",0,"회전검지속도",null,"NUMBER(10,2)","FLOAT",{"$nulls":4},"turn_dttn_sped ","FLOAT ","",",",null,"",",",{"$nulls":10},"COMMENT ON COLUMN ","soitgrtmdtinfo_2k.","turn_dttn_sped"," IS ","'회전검지속도'",";",null,null,""]
[null,7,"PK","정지선통과유닉스시각","stln_pasg_unix_tm","INT","NUMBER",10,"N",0,"정지선통과유닉스시각",null,"NUMBER(10)","INT",{"$nulls":4},"stln_pasg_unix_tm ","INT ","NOT NULL",",",null,"stln_pasg_unix_tm","",{"$nulls":10},"COMMENT ON COLUMN ","soitgrtmdtinfo_2k.","stln_pasg_unix_tm"," IS ","'정지선통과유닉스시각'",";",null,null,""]
[null,8,null,"정지선검지속도","stln_dttn_sped","FLOAT","NUMBER","10,2","Y",0,"정지선검지속도",null,"NUMBER(10,2)","FLOAT",{"$nulls":4},"stln_dttn_sped ","FLOAT ","",",",null,"","",{"$nulls":10},"COMMENT ON COLUMN ","soitgrtmdtinfo_2k.","stln_dttn_sped"," IS ","'정지선검지속도'",";",null,null,""]
[null,9,null,"차량구간속도","vhcl_sect_sped","FLOAT","NUMBER","10,2","Y",0,"차량구간속도",null,"NUMBER(10,2)","FLOAT",{"$nulls":4},"vhcl_sect_sped ","FLOAT ","",",",null,"",",",{"$nulls":10},"COMMENT ON COLUMN ","soitgrtmdtinfo_2k.","vhcl_sect_sped"," IS ","'차량구간속도'",";",null,null,""]
[null,10,"PK","최초관측유닉스시각","frst_obsrvn_unix_tm","INT","NUMBER",10,"N",0,"최초관측유닉스시각",null,"NUMBER(10)","INT",{"$nulls":4},"frst_obsrvn_unix_tm ","INT ","NOT NULL",",",null,"frst_obsrvn_unix_tm","));",{"$nulls":10},"COMMENT ON COLUMN ","soitgrtmdtinfo_2k.","frst_obsrvn_unix_tm"," IS ","'최초관측유닉스시각'",";",null,null,""]
[null,11,null,"차량관측시간","vhcl_obsrvn_hr","INT","NUMBER",10,"Y",1,"차량관측시간",null,"NUMBER(3)","INT",{"$nulls":4},"vhcl_obsrvn_hr ","INT ","",",",null,"",{"$nulls":11},"COMMENT ON COLUMN ","soitgrtmdtinfo_2k.","vhcl_obsrvn_hr"," IS ","'차량관측시간'",";",null,null,""]
[null,12,null,"이미지경로명","img_path_nm","VARCHAR","VARCHAR2",80,"Y",null,"이미지경로명",null,"VARCHAR2(80)","VARCHAR(80)",{"$nulls":4},"img_path_nm ","VARCHAR(80) ","",",",null,"",{"$nulls":11},"COMMENT ON COLUMN ","soitgrtmdtinfo_2k.","img_path_nm"," IS ","'이미지경로명'",";",null,null,""]
[null,13,null,"차량이미지파일명","vhcl_img_file_nm","VARCHAR","VARCHAR2",80,"Y",null,"차량이미지파일명",null,"VARCHAR2(80)","VARCHAR(80)",{"$nulls":4},"vhcl_img_file_nm ","VARCHAR(80) ","",",",null,"",{"$nulls":11},"COMMENT ON COLUMN ","soitgrtmdtinfo_2k.","vhcl_img_file_nm"," IS ","'차량이미지파일명'",";",null,null,""]
[null,14,"UK","차량검지_2K_ID","vhcl_dttn_2k_id","VARCHAR","VARCHAR2",256,"Y",null,"2K 차량검지정보 ID",null,"VARCHAR2(256)","VARCHAR(256)",{"$nulls":4},"vhcl_dttn_2k_id ","VARCHAR(256) ","",",",null,"",{"$nulls":11},"COMMENT ON COLUMN ","soitgrtmdtinfo_2k.","vhcl_dttn_2k_id"," IS ","'2K 차량검지정보 ID'",";",null,null,""]
[null,15,null,"생성유닉스시각","crt_unix_tm","INT","NUMBER",10,"Y",0,"생성유닉스시각",null,"NUMBER(10)","INT",{"$nulls":4},"crt_unix_tm ","INT ","",",",null,"",{"$nulls":11},"COMMENT ON COLUMN ","soitgrtmdtinfo_2k.","crt_unix_tm"," IS ","'생성유닉스시각'",";",null,null,""]
[{"$nulls":18},{"$f":"CONCATENATE(W277:Y291)","v":{"$error":"#VALUE!"}},{"$nulls":4},"",{"$nulls":19},""]
[{"$nulls":23},"",{"$nulls":19},""]
[null,"테이블명",null,"soitgrtmdtinfo_4K",{"$nulls":19},"",{"$nulls":19},""]
[null,"테이블설명",null,"4K 실시간 차량 검지정보",{"$nulls":19},"",{"$nulls":19},""]
[null,"참고사항",{"$nulls":21},"",{"$nulls":19},""]
[null,"NO","PK","논리명","물리명","VoltDB 타입","Tibero 타입","길이","NULL","기본값","비고",null,"형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE","soitgrtmdtinfo_4k",null," IS ",{"$f":"\"'\"&D295&\"'\"","v":"'4K 실시간 차량 검지정보'"},";",null,null,""]
[null,1,"PK","현장카메라ID","spot_camr_id","VARCHAR","VARCHAR2",10,"N",null,"현장카메라ID",null,"VARCHAR2(10)","VARCHAR(10)","티베로 안씀",null,"CREATE TABLE ",{"$f":"D294&\" (\"","v":"soitgrtmdtinfo_4K ("},{"$f":"E298&\" \"","v":"spot_camr_id "},{"$f":"N298&\" \"","v":"VARCHAR(10) "},{"$f":"IF(I298=\"N\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(C298=\"PK\", C298=\"PK/FK\"), E298, \"\")","v":"spot_camr_id"},{"$f":"IF(OR(C299=\"PK\", C299=\"PK/FK\"), \",\", \"\")","v":","},{"$nulls":10},"COMMENT ON COLUMN ","soitgrtmdtinfo_4k.",{"$f":"E298","v":"spot_camr_id"}," IS ",{"$f":"\"'\"&K298&\"'\"","v":"'현장카메라ID'"},";",null,null,""]
[null,2,"PK","차종코드","kncr_cd","VARCHAR","CHAR",10,"N",null,"차종","차종(008)","CHAR(10)","VARCHAR(10)",{"$nulls":4},"kncr_cd ","VARCHAR(10) ","NOT NULL",",",null,"kncr_cd",",",{"$nulls":10},"COMMENT ON COLUMN ","soitgrtmdtinfo_4k.","kncr_cd"," IS ","'차종'",";",null,null,""]
[null,3,"PK","차로번호","lane_no","TINYINT","NUMBER",2,"N",1,"차로번호",null,"NUMBER(2)","TINYINT",{"$nulls":4},"lane_no ","TINYINT ","NOT NULL",",",null,"lane_no",",",{"$nulls":10},"COMMENT ON COLUMN ","soitgrtmdtinfo_4k.","lane_no"," IS ","'차로번호'",";",null,null,""]
[null,4,"PK","정지선통과유닉스시각","stln_pasg_unix_tm","INT","NUMBER",10,"N",0,"정지선통과유닉스시각",null,"NUMBER(10)","INT",{"$nulls":4},"stln_pasg_unix_tm ","INT ","NOT NULL",",",null,"stln_pasg_unix_tm","));",{"$nulls":10},"COMMENT ON COLUMN ","soitgrtmdtinfo_4k.","stln_pasg_unix_tm"," IS ","'정지선통과유닉스시각'",";",null,null,""]
[null,5,null,"차량번호명","vhno_nm","VARCHAR","VARCHAR2",20,"Y",null,"차량 번호",null,"VARCHAR2(20)","VARCHAR(20)",{"$nulls":4},"vhno_nm ","VARCHAR(20) ","",",",null,"",{"$nulls":11},"COMMENT ON COLUMN ","soitgrtmdtinfo_4k.","vhno_nm"," IS ","'차량 번호'",";",null,null,""]
[null,6,null,"차량번호검지여부","vhno_dttn_yn","VARCHAR","CHAR",1,"Y",null,"정검지 여부(507)","(Y:정검지 N:미검지 F:오검지)","CHAR(1)","VARCHAR(1)",{"$nulls":4},"vhno_dttn_yn ","VARCHAR(1) ","",",",null,"",{"$nulls":11},"COMMENT ON COLUMN ","soitgrtmdtinfo_4k.","vhno_dttn_yn"," IS ","'정검지 여부(507)'",";",null,null,""]
[null,7,null,"이미지경로명","img_path_nm","VARCHAR","VARCHAR2",80,"Y",null,"이미지경로명",null,"VARCHAR2(80)","VARCHAR(80)",{"$nulls":4},"img_path_nm ","VARCHAR(80) ","",",",null,"",{"$nulls":11},"COMMENT ON COLUMN ","soitgrtmdtinfo_4k.","img_path_nm"," IS ","'이미지경로명'",";",null,null,""]
[null,8,null,"차량이미지파일명","vhcl_img_file_nm","VARCHAR","VARCHAR2",80,"Y",null,"차량이미지파일명",null,"VARCHAR2(80)","VARCHAR(80)",{"$nulls":4},"vhcl_img_file_nm ","VARCHAR(80) ","",",",null,"",{"$nulls":11},"COMMENT ON COLUMN ","soitgrtmdtinfo_4k.","vhcl_img_file_nm"," IS ","'차량이미지파일명'",";",null,null,""]
[null,9,null,"번호판이미지파일명","nopl_img_file_nm","VARCHAR","VARCHAR2",80,"Y",null,"번호판이미지파일명",null,"VARCHAR2(80)","VARCHAR(80)",{"$nulls":4},"nopl_img_file_nm ","VARCHAR(80) ","",",",null,"",{"$nulls":11},"COMMENT ON COLUMN ","soitgrtmdtinfo_4k.","nopl_img_file_nm"," IS ","'번호판이미지파일명'",";",null,null,""]
[null,10,"UK","차량검지_4K_ID","vhcl_dttn_4k_id","VARCHAR","VARCHAR2",256,"Y",null,"4K 차량검지정보 ID",null,"VARCHAR2(256)","VARCHAR(256)",{"$nulls":4},"vhcl_dttn_4k_id ","VARCHAR(256) ","",",",null,"",{"$nulls":11},"COMMENT ON COLUMN ","soitgrtmdtinfo_4k.","vhcl_dttn_4k_id"," IS ","'4K 차량검지정보 ID'",";",null,null,""]
[null,11,null,"생성유닉스시각","crt_unix_tm","INT","NUMBER",10,"Y",0,"생성유닉스시각",null,"NUMBER(10)","INT",{"$nulls":4},"crt_unix_tm ","INT ","",",",null,"",{"$nulls":11},"COMMENT ON COLUMN ","soitgrtmdtinfo_4k.","crt_unix_tm"," IS ","'생성유닉스시각'",";",null,null,""]
{"$rows_empty":22}
[{"$nulls":23},{"$f":"IF(OR(C331=\"PK\", C331=\"PK/FK\"), E331, \"\")","v":""},{"$nulls":19},{"$f":"IF(LEFT(AB331, 13) = \"CONSTRAINT PK\", AB331, \"\")","v":""}]
[{"$nulls":23},""]
[{"$nulls":23},""]
[{"$nulls":23},""]
[{"$nulls":23},""]
[{"$nulls":23},""]
[{"$nulls":23},""]
[{"$nulls":23},""]
[{"$nulls":23},""]
[{"$nulls":23},""]
[{"$nulls":23},""]
[{"$nulls":23},""]
[{"$nulls":23},""]
[{"$nulls":23},""]

{"sheet":"동인(신호정보)","index":5,"n_rows":513,"n_cols":43,"rows_kept":513,"cut":false,"hidden":false,"merged":[[0,0,0,4],[21,7,21,11],[29,0,29,5],[29,7,29,11],[29,16,29,21],[29,25,29,34],[29,35,29,40],[83,7,83,11],[83,16,83,21],[41,0,41,5],[41,7,41,11],[41,16,41,21],[70,0,70,5],[70,7,70,11],[70,16,70,21],[83,0,83,5],[192,7,192,11],[192,16,192,21],[111,0,111,5],[111,7,111,11],[111,16,111,21],[183,0,183,5],[183,7,183,11],[183,16,183,21],[192,0,192,5],[263,7,263,11],[263,16,263,21],[204,0,204,5],[204,7,204,11],[204,16,204,21],[225,0,225,5],[225,7,225,11],[225,16,225,21],[263,0,263,5],[306,0,306,5],[306,7,306,11],[306,16,306,21],[315,0,315,5],[315,7,315,11],[315,16,315,21],[346,5,361,5],[372,5,387,5],[393,0,393,5],[393,7,393,11],[393,16,393,21],[364,0,364,5],[364,7,364,11],[364,16,364,21],[333,0,333,5],[335,0,335,5],[339,0,339,5],[339,7,339,11],[339,16,339,21],[401,5,416,5],[422,0,422,5],[501,0,501,5],[501,7,501,11],[501,16,501,21],[456,7,456,11],[456,16,456,21],[456,0,456,5],[493,7,493,11],[493,16,493,21],[473,0,473,5],[473,7,473,11],[473,16,473,21],[482,0,482,5],[432,0,432,5],[432,7,432,11],[482,7,482,11],[482,16,482,21],[493,0,493,5],[422,7,422,11],[422,16,422,21],[432,16,432,21],[443,0,443,5],[443,7,443,11],[443,16,443,21]]}
["동인 신호연계정보_220714_동인_유아이네트웍스 수정.hwp"]
[]
["3.1 테이블 정보"]
["구분","연계 정보","설명","전송주기","비고","구분"]
["신호","신호교차로관리","신호 교차로 정보","일 한번 24시 0분,변경 시","INSERT","VoltDB","3,000건/일"]
["신호","TOD구성","TOD 구성 정보","일 한번 24시 0분,변경 시","INSERT","VoltDB","500,000건/일"]
["신호","시각계획","TOD PLAN","일 한번 24시 0분,변경 시","INSERT","VoltDB","500,000건/일"]
["신호","시간계획","TIME PLAN","일 한번 24시 0분,변경 시","INSERT","VoltDB","500,000건/일"]
["신호","교차로현시","교차로 현시 정보","일 한번 24시 0분,변경 시","INSERT","VoltDB","20,000건/일"]
["신호","교차로그룹관리","교차로 그룹 정보","일 한번 24시 0분,변경 시","INSERT","VoltDB","20,000건/일"]
["신호","특수일시각제어","교차로별 특수일 시각제어 정보","일 한번 24시 0분,변경 시","INSERT","VoltDB","100,000건/일"]
["신호","주간시각제어","교차로 별 주간시각제어 정보","일 한번 24시 0분,변경 시","INSERT","VoltDB","3,000건/일"]
["신호","신호교차로상태","신호교차로 상태 정보","1초","INSERT","VoltDB / Tibero","5,000,000건/시간"]
["신호","신호교차로\n운영이력","신호교차로 운영이력정보","운영이력 발생 시","INSERT","VoltDB","1,500,000건/일"]
["신호","소속교차로관리","교차로 그룹 소속교차로","일 한번 24시 0분,변경 시","INSERT","VoltDB","20,000건/일"]
["신호","교차로예약","교차로 예약","일 한번 24시 0분,변경 시","INSERT","VoltDB","30,000건/일"]
["신호","신호제어기","신호교차로의 좌표, 현시코드","일 한번 24시 0분,변경 시","INSERT","VoltDB","3,000건/일"]
["신호","신호 운영 맵3","신호운영 맵정보(2010년규격)","일 한번 24시 0분,변경 시","INSERT","VoltDB","400,000건/일"]
["신호","신호 운영 맵4","신호운영 맵정보(2004년규격)","일 한번 24시 0분,변경 시","INSERT","VoltDB","300,000건/일"]
["신호","신호출력","신호출력정보","일 한번 24시 0분,변경 시","2010년 규격만 정보 올라옴\nINSERT","VoltDB","10,000건/일"]
["긴급","긴급차량운영이력","긴급차량운영이력정보","앱 실행 시 1초","INSERT","VoltDB"]
["긴급","우선신호요청정보","우선신호요청정보","긴급차량 발생 시","INSERT","VoltDB",null,"변경후(센터 도메인 및 용어기준)"]
["긴급","긴급차량정보","긴급차량정보","일 한번 24시 0분,변경 시","INSERT","VoltDB","25건/일"]
["긴급","우선신호\n운영교차로","우선신호운영교차로","긴급차량 운영 시","INSERT","VoltDB"]
["긴급","긴급차량 목적지\n마스터 정보","긴급차량 목적지 마스터 정보","긴급차량 운영 시","INSERT","VoltDB"]
["긴급","우선신호 안내경로 정보","우선신호 안내경로 정보","긴급차량 운영 시","INSERT","Tibero"]
["긴급","긴급차량 기관정보","긴급차량 기관정보","일 한번 24시 0분,변경 시","INSERT","VoltDB"]
[]
[]
["- 신호교차로관리(SGNL_IXR_MNGM)",{"$nulls":6},"soitdspotintsinfo",{"$nulls":17},"TIBERO DDL",{"$nulls":9},"COMMENTS"]
["NO","속성명","컬럼명","형태","길이","비고",null,"논리명","PK/FK","NULL","물리명","형태","VOLT","TIBERO","COMMENT",{"$nulls":20},"COMMENT ON TABLE",{"$f":"H30&\" \"","v":"soitdspotintsinfo "},null," IS ",{"$f":"\"'\"&A30&\"'\"","v":"'- 신호교차로관리(SGNL_IXR_MNGM)'"},";"]
[1,"신호 교차로 번호","SGNL_IXR_NMBR","NUMBER",4,null,null,"현장교차로ID","PK","NOT NULL","spot_ints_id","NUMBER(5)","INTEGER","NUMBER(5)","현장교차로ID",null,"CREATE TABLE ",{"$f":"H30&\" (\"","v":"soitdspotintsinfo ("},{"$f":"K32&\" \"","v":"spot_ints_id "},{"$f":"M32&\" \"","v":"INTEGER "},{"$f":"IF(J32=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(I32=\"PK\", I32=\"PK/FK\"), K32, \"\")","v":"spot_ints_id"},",","CREATE TABLE ",{"$f":"H30&\" (\"","v":"soitdspotintsinfo ("},{"$f":"K32&\" \"","v":"spot_ints_id "},{"$f":"N32&\" \"","v":"NUMBER(5) "},{"$f":"IF(J32=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(I32=\"PK\", I32=\"PK/FK\"), K32, \"\")","v":"spot_ints_id"},",","COMMENT ON COLUMN ",{"$f":"$H30&\".\"","v":"soitdspotintsinfo."},{"$f":"K32","v":"spot_ints_id"}," IS ",{"$f":"\"'\"&O32&\"'\"","v":"'현장교차로ID'"},";"]
[2,"수집 일시","CLCT_DT","INTEGER","UTC",null,null,"수집유닉스시각","PK","NOT NULL","clct_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)","수집유닉스시각",null,null,null,{"$f":"K33","v":"clct_unix_tm"},"INTEGER ","NOT NULL",",",null,"clct_unix_tm","));",null,null,"clct_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"clct_unix_tm",")","COMMENT ON COLUMN ",{"$f":"$H30&\".\"","v":"soitdspotintsinfo."},"clct_unix_tm"," IS ","'수집유닉스시각'",";"]
[2,"수집일","CLCT_DATE","VARHCAR2",8,"YYYYMMDD",null,"수집일시",null,"NOT NULL","clct_dt","VARCHAR2(8)","VARCHAR(8)","VARCHAR2(8)","수집일시(yyyyMMdd)",null,null,null,"clct_dt","VARCHAR(8) ","NOT NULL",",",null,"",null,null,null,"clct_dt ","VARCHAR2(8) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ",{"$f":"$H30&\".\"","v":"soitdspotintsinfo."},"clct_dt"," IS ","'수집일시(yyyyMMdd)'",";"]
[3,"교차로 그룹","IXR_GROP","NUMBER",3,null,null,"교차로군ID","FK","NULL","ints_grop_id","NUMBER(5)","INTEGER","NUMBER(5)","교차로군ID",null,null,null,"ints_grop_id","INTEGER ","",",",null,"",null,null,null,"ints_grop_id ","NUMBER(5) ","",",",{"$nulls":4},"COMMENT ON COLUMN ",{"$f":"H30&\".\"","v":"soitdspotintsinfo."},"ints_grop_id"," IS ","'교차로군ID'",";"]
[4,"교차로 명","IXR_NM","VARCHAR2",50,null,null,"교차로명",null,"NULL","ints_nm","VARCHAR2(50)","VARCHAR(50)","VARCHAR2(50)","교차로명",null,null,null,"ints_nm","VARCHAR(50) ","",",",null,"",null,null,null,"ints_nm ","VARCHAR2(50) ","",",",{"$nulls":4},"COMMENT ON COLUMN ",{"$f":"H30&\".\"","v":"soitdspotintsinfo."},"ints_nm"," IS ","'교차로명'",";"]
[5,"등록 유무","RGST_EN","NUMBER",1,"0:미등록 \n1:등록","등록여부(017)","등록구분코드",null,"NOT NULL","reg_se_cd","CHAR(3)","VARCHAR(3)","VARCHAR2(3)","등록구분코드(017)","등록구분코드 (0:미등록, 1:등록)",null,null,"reg_se_cd","VARCHAR(3) ","NOT NULL",",",null,"",null,null,null,"reg_se_cd ","VARCHAR2(3) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ",{"$f":"H30&\".\"","v":"soitdspotintsinfo."},"reg_se_cd"," IS ","'등록구분코드(017)'",";"]
[6,"주현시","MAIN_PHAS","NUMBER",1,null,null,"주현시번호",null,"NOT NULL","majr_phas_no","NUMBER(2)","INTEGER","NUMBER(2)","주현시번호","주현시번호",null,null,"majr_phas_no","INTEGER ","NOT NULL",",",null,"",null,null,null,"majr_phas_no ","NUMBER(2) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ",{"$f":"H30&\".\"","v":"soitdspotintsinfo."},"majr_phas_no"," IS ","'주현시번호'",";"]
[7,"교차로 구분","IXR_DVSN","NUMBER",1,"0:2004년\n1:2010년","교차로연도구분(800)","교차로연도구분코드",null,"NOT NULL","ints_yr_se_cd","CHAR(3)","VARCHAR(3)","VARCHAR2(3)","교차로연도구분코드(800)","교차로연도구분코드 (0:2004, 1:2010)",null,null,"ints_yr_se_cd","VARCHAR(3) ","NOT NULL",",",null,"",null,null,null,"ints_yr_se_cd ","VARCHAR2(3) ","NOT NULL",{"$f":"\") TABLESPACE \"&AF41&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_D001 NOLOGGING"},null,null,{"$f":"IF(OR(C39=\"PK\", C39=\"PK/FK\"), E39, \"\")","v":""},null,"COMMENT ON COLUMN ",{"$f":"H30&\".\"","v":"soitdspotintsinfo."},"ints_yr_se_cd"," IS ","'교차로연도구분코드(800)'",";"]
[{"$nulls":18},{"$f":"CONCATENATE(W32:Y39)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AF40:AH40)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (clct_unix_tm) INTERVAL (86400) STORE IN (\"&AF41&\") (PARTITION BFR_\" & H30 & \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AF41&\");\"","v":"PARTITION BY RANGE (clct_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_D001) (PARTITION BFR_soitdspotintsinfo_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_D001);"},{"$f":"\"CREATE INDEX PK_\" & H30 & \" ON \" & H30 & CONCATENATE(AG32:AI38) & \" LOCAL (PARTITION BFR_\" & H30 & \"_20221101 TABLESPACE \"&AG41&\") TABLESPACE \"&AG41&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & H30 & \" ADD CONSTRAINT PK_\" & H30 & \" PRIMARY KEY \" & CONCATENATE(AG32:AI38) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"IF(LEFT(AB40, 13) = \"CONSTRAINT PK\", AB40, \"\")","v":{"$error":"#VALUE!"}}]
[{"$nulls":31},"SOIT_D08_D001","SOIT_I08_D001",{"$nulls":9},""]
["- TOD구성(TOD_CNFG)",{"$nulls":6},"soitdtodcnfg",{"$nulls":34},""]
["NO","속성명","컬럼명","형태","길이","비고",null,"논리명","PK/FK","NULL","물리명","형태","VOLT","TIBERO","COMMENT",{"$nulls":20},"COMMENT ON TABLE",{"$f":"H42&\" \"","v":"soitdtodcnfg "},null," IS ",{"$f":"\"'\"&A42&\"'\"","v":"'- TOD구성(TOD_CNFG)'"},";",null,""]
[1,"신호 교차로 번호","SGNL_IXR_NMBR","NUMBER",4,null,null,"현장교차로ID","PK/FK","NOT NULL","spot_ints_id","NUMBER(5)","INTEGER","NUMBER(5)","현장교차로ID",null,"CREATE TABLE ",{"$f":"H42&\" (\"","v":"soitdtodcnfg ("},{"$f":"K44&\" \"","v":"spot_ints_id "},{"$f":"M44&\" \"","v":"INTEGER "},{"$f":"IF(J44=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(I44=\"PK\", I44=\"PK/FK\"), K44, \"\")","v":"spot_ints_id"},",","CREATE TABLE ",{"$f":"H42&\" (\"","v":"soitdtodcnfg ("},{"$f":"K44&\" \"","v":"spot_ints_id "},{"$f":"N44&\" \"","v":"NUMBER(5) "},{"$f":"IF(J44=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(I44=\"PK\", I44=\"PK/FK\"), K44, \"\")","v":"spot_ints_id"},",","COMMENT ON COLUMN ",{"$f":"$H42&\".\"","v":"soitdtodcnfg."},{"$f":"K44","v":"spot_ints_id"}," IS ",{"$f":"\"'\"&O44&\"'\"","v":"'현장교차로ID'"},";",null,""]
[2,"수집 일시","CLCT_DT","INTEGER","UTC",null,null,"수집유닉스시각","PK","NOT NULL","clct_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)","수집유닉스시각",null,null,null,"clct_unix_tm ","INTEGER ","NOT NULL",",",null,"clct_unix_tm",",",null,null,"clct_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"clct_unix_tm",",","COMMENT ON COLUMN ",{"$f":"$H$42&\".\"","v":"soitdtodcnfg."},"clct_unix_tm"," IS ","'수집유닉스시각'",";",null,""]
[2,"수집일","CLCT_DATE","VARHCAR2",8,"YYYYMMDD",null,"수집일시",null,"NOT NULL","clct_dt","VARCHAR2(8)","VARCHAR(8)","VARCHAR2(8)","수집일시(yyyyMMdd)",null,null,null,{"$f":"K46","v":"clct_dt"},"VARCHAR(8) ","NOT NULL",",",null,"",null,null,null,"clct_dt ","VARCHAR2(8) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitdtodcnfg.","clct_dt"," IS ","'수집일시(yyyyMMdd)'",";"]
[3,"시각계획번호","HMS_PLAN_NMBR","NUMBER",2,"1~10",null,"시각계획번호","PK","NOT NULL","tm_plan_no","NUMBER(2)","INTEGER","NUMBER(2)","시각계획번호 (tod plan구분, 1~10)",null,null,null,{"$f":"K47&\" \"","v":"tm_plan_no "},"INTEGER ","NOT NULL",",",null,"tm_plan_no",",",null,null,"tm_plan_no ","NUMBER(2) ","NOT NULL",",",null,null,"tm_plan_no",",","COMMENT ON COLUMN ","soitdtodcnfg.","tm_plan_no"," IS ","'시각계획번호 (tod plan구분, 1~10)'",";",null,{"$f":"IF(LEFT(AB47, 13) = \"CONSTRAINT PK\", AB47, \"\")","v":""}]
[4,"교차로 현시 운영 계획 번호","IXR_PHAS_OPER_PLAN_NMBR","NUMBER",2,"1~16",null,"현시운영계획번호","PK","NOT NULL","phas_oper_plan_no","NUMBER(2)","INTEGER","NUMBER(2)","현시운영계획번호 (time plan ID, 1~16)",null,null,null,"phas_oper_plan_no ","INTEGER ","NOT NULL",",",null,"phas_oper_plan_no","));",null,null,"phas_oper_plan_no ","NUMBER(2) ","NOT NULL",",",null,null,"phas_oper_plan_no",")","COMMENT ON COLUMN ","soitdtodcnfg.","phas_oper_plan_no"," IS ","'현시운영계획번호 (time plan ID, 1~16)'",";",null,""]
[5,"시간","HH","NUMBER",2,null,null,"시작시",null,"NOT NULL","bgng_hh","NUMBER(2)","INTEGER","NUMBER(2)","시작시 (HH)",null,null,null,"bgng_hh ","INTEGER ","NOT NULL",",",null,"",null,null,null,"bgng_hh ","NUMBER(2) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitdtodcnfg.","bgng_hh"," IS ","'시작시 (HH)'",";",null,""]
[6,"분","MM","NUMBER",2,null,null,"시작분",null,"NOT NULL","bgng_mi","NUMBER(2)","INTEGER","NUMBER(2)","시작분 (mm)",null,null,null,"bgng_mi ","INTEGER ","NOT NULL",",",null,"",null,null,null,"bgng_mi ","NUMBER(2) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitdtodcnfg.","bgng_mi"," IS ","'시작분 (mm)'",";",null,""]
[7,"주기","CYCL","NUMBER",3,"초",null,"주기시간",null,"NOT NULL","cycl_hr","NUMBER(3)","INTEGER","NUMBER(3)","주기시간 (sec)",null,null,null,"cycl_hr ","INTEGER ","NOT NULL",",",null,"",null,null,null,"cycl_hr ","NUMBER(3) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitdtodcnfg.","cycl_hr"," IS ","'주기시간 (sec)'",";",null,""]
[8,"옵셋","OFST","NUMBER",3,"초",null,"옵셋시간",null,"NOT NULL","ofst_hr","NUMBER(3)","INTEGER","NUMBER(3)","옵셋시간 (sec)",null,null,null,"ofst_hr ","INTEGER ","NOT NULL",",",null,"",null,null,null,"ofst_hr ","NUMBER(3) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitdtodcnfg.","ofst_hr"," IS ","'옵셋시간 (sec)'",";",null,""]
[9,"A링 1현시","ARING_1PHAS","NUMBER",3,"초",null,"A링1현시시간",null,"NULL","A_ring_1_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링1현시시간 (sec)",null,null,null,"A_ring_1_phas_hr ","INTEGER ","",",",null,"",null,null,null,"A_ring_1_phas_hr ","NUMBER(3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitdtodcnfg.","A_ring_1_phas_hr"," IS ","'A링1현시시간 (sec)'",";",null,""]
[10,"A링 2현시","ARING_2PHAS","NUMBER",3,"초",null,"A링2현시시간",null,"NULL","A_ring_2_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링2현시시간 (sec)",null,null,null,"A_ring_2_phas_hr ","INTEGER ","",",",null,"",null,null,null,"A_ring_2_phas_hr ","NUMBER(3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitdtodcnfg.","A_ring_2_phas_hr"," IS ","'A링2현시시간 (sec)'",";",null,""]
[11,"A링 3현시","ARING_3PHAS","NUMBER",3,"초",null,"A링3현시시간",null,"NULL","A_ring_3_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링3현시시간 (sec)",null,null,null,"A_ring_3_phas_hr ","INTEGER ","",",",null,"",null,null,null,"A_ring_3_phas_hr ","NUMBER(3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitdtodcnfg.","A_ring_3_phas_hr"," IS ","'A링3현시시간 (sec)'",";",null,""]
[12,"A링 4현시","ARING_4PHAS","NUMBER",3,"초",null,"A링4현시시간",null,"NULL","A_ring_4_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링4현시시간 (sec)",null,null,null,"A_ring_4_phas_hr ","INTEGER ","",",",null,"",null,null,null,"A_ring_4_phas_hr ","NUMBER(3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitdtodcnfg.","A_ring_4_phas_hr"," IS ","'A링4현시시간 (sec)'",";",null,""]
[13,"A링 5현시","ARING_5PHAS","NUMBER",3,"초",null,"A링5현시시간",null,"NULL","A_ring_5_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링5현시시간 (sec)",null,null,null,"A_ring_5_phas_hr ","INTEGER ","",",",null,"",null,null,null,"A_ring_5_phas_hr ","NUMBER(3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitdtodcnfg.","A_ring_5_phas_hr"," IS ","'A링5현시시간 (sec)'",";",null,""]
[14,"A링 6현시","ARING_6PHAS","NUMBER",3,"초",null,"A링6현시시간",null,"NULL","A_ring_6_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링6현시시간 (sec)",null,null,null,"A_ring_6_phas_hr ","INTEGER ","",",",null,"",null,null,null,"A_ring_6_phas_hr ","NUMBER(3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitdtodcnfg.","A_ring_6_phas_hr"," IS ","'A링6현시시간 (sec)'",";",null,""]
[15,"A링 7현시","ARING_7PHAS","NUMBER",3,"초",null,"A링7현시시간",null,"NULL","A_ring_7_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링7현시시간 (sec)",null,null,null,"A_ring_7_phas_hr ","INTEGER ","",",",null,"",null,null,null,"A_ring_7_phas_hr ","NUMBER(3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitdtodcnfg.","A_ring_7_phas_hr"," IS ","'A링7현시시간 (sec)'",";",null,""]
[16,"A링 8현시","ARING_8PHAS","NUMBER",3,"초",null,"A링8현시시간",null,"NULL","A_ring_8_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링8현시시간 (sec)",null,null,null,"A_ring_8_phas_hr ","INTEGER ","",",",null,"",null,null,null,"A_ring_8_phas_hr ","NUMBER(3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitdtodcnfg.","A_ring_8_phas_hr"," IS ","'A링8현시시간 (sec)'",";",null,""]
[17,"B링 1현시","BRING_1PHAS","NUMBER",3,"초",null,"B링1현시시간",null,"NULL","B_ring_1_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링1현시시간 (sec)",null,null,null,"B_ring_1_phas_hr ","INTEGER ","",",",null,"",null,null,null,"B_ring_1_phas_hr ","NUMBER(3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitdtodcnfg.","B_ring_1_phas_hr"," IS ","'B링1현시시간 (sec)'",";",null,""]
[18,"B링 2현시","BRING_2PHAS","NUMBER",3,"초",null,"B링2현시시간",null,"NULL","B_ring_2_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링2현시시간 (sec)",null,null,null,"B_ring_2_phas_hr ","INTEGER ","",",",null,"",null,null,null,"B_ring_2_phas_hr ","NUMBER(3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitdtodcnfg.","B_ring_2_phas_hr"," IS ","'B링2현시시간 (sec)'",";",null,""]
[19,"B링 3현시","BRING_3PHAS","NUMBER",3,"초",null,"B링3현시시간",null,"NULL","B_ring_3_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링3현시시간 (sec)",null,null,null,"B_ring_3_phas_hr ","INTEGER ","",",",null,"",null,null,null,"B_ring_3_phas_hr ","NUMBER(3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitdtodcnfg.","B_ring_3_phas_hr"," IS ","'B링3현시시간 (sec)'",";",null,""]
[20,"B링 4현시","BRING_4PHAS","NUMBER",3,"초",null,"B링4현시시간",null,"NULL","B_ring_4_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링4현시시간 (sec)",null,null,null,"B_ring_4_phas_hr ","INTEGER ","",",",null,"",null,null,null,"B_ring_4_phas_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdtodcnfg.","B_ring_4_phas_hr"," IS ","'B링4현시시간 (sec)'",";",null,""]
[21,"B링 5현시","BRING_5PHAS","NUMBER",3,"초",null,"B링5현시시간",null,"NULL","B_ring_5_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링5현시시간 (sec)",null,null,null,"B_ring_5_phas_hr ","INTEGER ","",",",null,"",null,null,null,"B_ring_5_phas_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdtodcnfg.","B_ring_5_phas_hr"," IS ","'B링5현시시간 (sec)'",";",null,""]
[22,"B링 6현시","BRING_6PHAS","NUMBER",3,"초",null,"B링6현시시간",null,"NULL","B_ring_6_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링6현시시간 (sec)",null,null,null,"B_ring_6_phas_hr ","INTEGER ","",",",null,"",null,null,null,"B_ring_6_phas_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdtodcnfg.","B_ring_6_phas_hr"," IS ","'B링6현시시간 (sec)'",";",null,""]
[23,"B링 7현시","BRING_7PHAS","NUMBER",3,"초",null,"B링7현시시간",null,"NULL","B_ring_7_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링7현시시간 (sec)",null,null,null,"B_ring_7_phas_hr ","INTEGER ","",",",null,"",null,null,null,"B_ring_7_phas_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdtodcnfg.","B_ring_7_phas_hr"," IS ","'B링7현시시간 (sec)'",";",null,""]
[24,"B링 8현시","BRING_8PHAS","NUMBER",3,"초",null,"B링8현시시간",null,"NULL","B_ring_8_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링8현시시간 (sec)",null,null,null,"B_ring_8_phas_hr ","INTEGER ","",",",null,"",null,null,null,"B_ring_8_phas_hr ","NUMBER(3) ","",{"$f":"\") TABLESPACE \"&AF70&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_D001 NOLOGGING"},{"$nulls":4},"COMMENT ON COLUMN ","soitdtodcnfg.","B_ring_8_phas_hr"," IS ","'B링8현시시간 (sec)'",";",null,""]
[{"$nulls":18},{"$f":"CONCATENATE(W44:Y68)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AF69:AH69)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (clct_unix_tm) INTERVAL (86400) STORE IN (\"&AF70&\") (PARTITION BFR_\" & H42 & \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AF70&\");\"","v":"PARTITION BY RANGE (clct_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_D001) (PARTITION BFR_soitdtodcnfg_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_D001);"},{"$f":"\"CREATE INDEX PK_\" & H42 & \" ON \" & H42 & CONCATENATE(AG44:AI48) & \" LOCAL (PARTITION BFR_\" & H42 & \"_20221101 TABLESPACE \"&AG70&\") TABLESPACE \"&AG70&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & H42 & \" ADD CONSTRAINT PK_\" & H42 & \" PRIMARY KEY \" & CONCATENATE(AG44:AI48) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$error":"#VALUE!"}]
[{"$nulls":31},"SOIT_D08_D001","SOIT_I08_D001"]
["- 시각 계획 (HMS_PLAN)  TOD PLAN",{"$nulls":6},"soitdtodplan",{"$nulls":34},{"$f":"IF(LEFT(AB71, 13) = \"CONSTRAINT PK\", AB71, \"\")","v":""}]
["NO","속성명","컬럼명","형태","길이","비고",null,"논리명","PK/FK","NULL","물리명","형태","VOLT","TIBERO","COMMENT",{"$nulls":20},"COMMENT ON TABLE",{"$f":"H71&\" \"","v":"soitdtodplan "},null," IS ",{"$f":"\"'\"&A71&\"'\"","v":"'- 시각 계획 (HMS_PLAN)  TOD PLAN'"},";",null,""]
[1,"신호 교차로 번호","SGNL_IXR_NMBR","NUMBER",4,null,null,"현장교차로ID","PK/FK","NOT NULL","spot_ints_id","NUMBER(5)","INTEGER","NUMBER(5)","현장교차로ID",null,"CREATE TABLE ",{"$f":"H71&\" (\"","v":"soitdtodplan ("},{"$f":"K73&\" \"","v":"spot_ints_id "},{"$f":"M73&\" \"","v":"INTEGER "},{"$f":"IF(J73=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(I73=\"PK\", I73=\"PK/FK\"), K73, \"\")","v":"spot_ints_id"},{"$f":"IF(OR(I73=\"PK\", I73=\"PK/FK\"), \",\", \"\")","v":","},"CREATE TABLE ",{"$f":"H71&\" (\"","v":"soitdtodplan ("},{"$f":"K73&\" \"","v":"spot_ints_id "},{"$f":"N73&\" \"","v":"NUMBER(5) "},{"$f":"IF(J73=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(I73=\"PK\", I73=\"PK/FK\"), K73, \"\")","v":"spot_ints_id"},{"$f":"IF(OR(I73=\"PK\", I73=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$H$71&\".\"","v":"soitdtodplan."},{"$f":"K73","v":"spot_ints_id"}," IS ",{"$f":"\"'\"&O73&\"'\"","v":"'현장교차로ID'"},";",null,""]
[2,"시각계획번호","HMS_PLAN_NMBR","NUMBER",2,"tod plan\n구분\n1~10",null,"시각계획번호","PK","NOT NULL","tm_plan_no","NUMBER(2)","INTEGER","NUMBER(2)","시각계획번호 (tod plan구분, 1~10)",null,null,null,"tm_plan_no ","INTEGER ","NOT NULL",",",null,"tm_plan_no",",",null,null,"tm_plan_no ","NUMBER(2) ","NOT NULL",",",null,null,"tm_plan_no",",","COMMENT ON COLUMN ","soitdtodplan.","tm_plan_no"," IS ","'시각계획번호 (tod plan구분, 1~10)'",";",null,""]
[3,"시각운영번호","HMS_OPER_NMBR","NUMBER",2,"tod plan 번호\n1~16",null,"시각운영번호","PK","NOT NULL","tm_oper_no","NUMBER(2)","INTEGER","NUMBER(2)","시각운영번호 (tod plan 번호, 1~16)",null,null,null,"tm_oper_no ","INTEGER ","NOT NULL",",",null,"tm_oper_no",",",null,null,"tm_oper_no ","NUMBER(2) ","NOT NULL",",",null,null,"tm_oper_no",",","COMMENT ON COLUMN ","soitdtodplan.","tm_oper_no"," IS ","'시각운영번호 (tod plan 번호, 1~16)'",";",null,""]
[4,"수집 일시","CLCT_DT","INTEGER","UTC",null,null,"수집유닉스시각","PK","NOT NULL","clct_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)","수집유닉스시각",null,null,null,"clct_unix_tm ","INTEGER ","NOT NULL",",",null,"clct_unix_tm","));",null,null,"clct_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"clct_unix_tm",")","COMMENT ON COLUMN ","soitdtodplan.","clct_unix_tm"," IS ","'수집유닉스시각'",";",null,""]
[2,"수집일","CLCT_DATE","VARHCAR2",8,"YYYYMMDD",null,"수집일시",null,"NOT NULL","clct_dt","VARCHAR2(8)","VARCHAR(8)","VARCHAR2(8)","수집일시(yyyyMMdd)",null,null,null,{"$f":"K77","v":"clct_dt"},"VARCHAR(8) ","NOT NULL",",",null,"",null,null,null,"clct_dt ","VARCHAR2(8) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitdtodplan.","clct_dt"," IS ","'수집일시(yyyyMMdd)'",";"]
[5,"시간","HH","NUMBER",2,null,null,"시작시",null,"NOT NULL","bgng_hh","NUMBER(2)","INTEGER","NUMBER(2)","시작시 (HH)",null,null,null,{"$f":"K78&\" \"","v":"bgng_hh "},"INTEGER ","NOT NULL",",",null,"",{"$f":"IF(OR(I78=\"PK\", I78=\"PK/FK\"), \",\", \"\")","v":""},null,null,"bgng_hh ","NUMBER(2) ","NOT NULL",",",null,null,"",{"$f":"IF(OR(I78=\"PK\", I78=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitdtodplan.","bgng_hh"," IS ","'시작시 (HH)'",";",null,{"$f":"IF(LEFT(AB78, 13) = \"CONSTRAINT PK\", AB78, \"\")","v":""}]
[6,"분","MM","NUMBER",2,null,null,"시작분",null,"NOT NULL","bgng_mi","NUMBER(2)","INTEGER","NUMBER(2)","시작분 (mm)",null,null,null,"bgng_mi ","INTEGER ","NOT NULL",",",null,"","",null,null,"bgng_mi ","NUMBER(2) ","NOT NULL",",",null,null,"","","COMMENT ON COLUMN ","soitdtodplan.","bgng_mi"," IS ","'시작분 (mm)'",";",null,""]
[7,"교차로 현시 운영 번호","IXR_PHAS_OPER_NMBR","NUMBER",2,"time plan \n수준\n1~6",null,"현시운영번호",null,"NOT NULL","phas_oper_no","NUMBER(2)","INTEGER","NUMBER(2)","현시운영번호 (time plan 수준, 1~6)",null,null,null,"phas_oper_no ","INTEGER ","NOT NULL",",",null,"","",null,null,"phas_oper_no ","NUMBER(2) ","NOT NULL",",",null,null,"","","COMMENT ON COLUMN ","soitdtodplan.","phas_oper_no"," IS ","'현시운영번호 (time plan 수준, 1~6)'",";",null,""]
[8,"교차로 현시 운영 계획 번호","IXR_PHAS_OPER_PLAN_NMBR","NUMBER",2,"time paln\nID\n1~16",null,"현시운영계획번호",null,"NOT NULL","phas_oper_plan_no","NUMBER(2)","INTEGER","NUMBER(2)","현시운영계획번호 (time plan ID, 1~16)",null,null,null,"phas_oper_plan_no ","INTEGER ","NOT NULL",",",null,"","",null,null,"phas_oper_plan_no ","NUMBER(2) ","NOT NULL",{"$f":"\") TABLESPACE \"&AF83&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_D001 NOLOGGING"},null,null,{"$f":"IF(OR(C81=\"PK\", C81=\"PK/FK\"), E81, \"\")","v":""},null,"COMMENT ON COLUMN ","soitdtodplan.","phas_oper_plan_no"," IS ","'현시운영계획번호 (time plan ID, 1~16)'",";",null,""]
[{"$nulls":18},{"$f":"CONCATENATE(W73:Y81)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AF82:AH82)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (clct_unix_tm) INTERVAL (86400) STORE IN (\"&AF83&\") (PARTITION BFR_\" & H71 & \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AF83&\");\"","v":"PARTITION BY RANGE (clct_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_D001) (PARTITION BFR_soitdtodplan_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_D001);"},{"$f":"\"CREATE INDEX PK_\" & H71& \" ON \" & H71 & CONCATENATE(AG73:AI80) & \" LOCAL (PARTITION BFR_\" & H71 & \"_20221101 TABLESPACE \"&AG83&\") TABLESPACE \"&AG83&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & H71 & \" ADD CONSTRAINT PK_\" & H71 & \" PRIMARY KEY \" & CONCATENATE(AG73:AI80) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$error":"#VALUE!"}]
[{"$nulls":31},"SOIT_D08_D001","SOIT_I08_D001"]
["- 시간 계획 (HH_PLAN)  TIME PLAN",{"$nulls":6},"soitdtimeplan",{"$nulls":34},{"$f":"IF(LEFT(AB84, 13) = \"CONSTRAINT PK\", AB84, \"\")","v":""}]
["NO","속성명","컬럼명","형태","길이","비고",null,"논리명","PK/FK","NULL","물리명","형태","VOLT","TIBERO","COMMENT",{"$nulls":20},"COMMENT ON TABLE",{"$f":"H84&\" \"","v":"soitdtimeplan "},null," IS ",{"$f":"\"'\"&A84&\"'\"","v":"'- 시간 계획 (HH_PLAN)  TIME PLAN'"},";",null,""]
[1,"신호 교차로 번호","SGNL_IXR_NMBR","NUMBER",4,null,null,"현장교차로ID","PK/FK","NOT NULL","spot_ints_id","NUMBER(5)","INTEGER","NUMBER(5)","현장교차로ID",null,"CREATE TABLE ",{"$f":"H84&\" (\"","v":"soitdtimeplan ("},{"$f":"K86&\" \"","v":"spot_ints_id "},{"$f":"M86&\" \"","v":"INTEGER "},{"$f":"IF(J86=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(I86=\"PK\", I86=\"PK/FK\"), K86, \"\")","v":"spot_ints_id"},{"$f":"IF(OR(I86=\"PK\", I86=\"PK/FK\"), \",\", \"\")","v":","},"CREATE TABLE ",{"$f":"H84&\" (\"","v":"soitdtimeplan ("},{"$f":"K86&\" \"","v":"spot_ints_id "},{"$f":"N86&\" \"","v":"NUMBER(5) "},{"$f":"IF(J86=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(I86=\"PK\", I86=\"PK/FK\"), K86, \"\")","v":"spot_ints_id"},{"$f":"IF(OR(I86=\"PK\", I86=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$H$84&\".\"","v":"soitdtimeplan."},{"$f":"K86","v":"spot_ints_id"}," IS ",{"$f":"\"'\"&O86&\"'\"","v":"'현장교차로ID'"},";",null,""]
[2,"시간 계획 번호","HH_PLAN_NMBR","NUMBER",2,"1~10     1만 쓰는걸로 보임",null,"시간계획번호","PK","NOT NULL","hr_plan_no","NUMBER(2)","INTEGER","NUMBER(2)","시간계획번호 (1~10)",null,null,null,"hr_plan_no ","INTEGER ","NOT NULL",",",null,"hr_plan_no",",",null,null,"hr_plan_no ","NUMBER(2) ","NOT NULL",",",null,null,"hr_plan_no",",","COMMENT ON COLUMN ","soitdtimeplan.","hr_plan_no"," IS ","'시간계획번호 (1~10)'",";",null,""]
[3,"교차로 현시 운영 번호","IXR_PHAS_OPER_NMBR","NUMBER",2,"time plan 수준\n1~10",null,"현시운영번호",null,"NOT NULL","phas_oper_no","NUMBER(2)","INTEGER","NUMBER(2)","현시운영번호 (time plan 수준, 1~6)",null,null,null,"phas_oper_no ","INTEGER ","NOT NULL",",",null,"","",null,null,"phas_oper_no ","NUMBER(2) ","NOT NULL",",",null,null,"","","COMMENT ON COLUMN ","soitdtimeplan.","phas_oper_no"," IS ","'현시운영번호 (time plan 수준, 1~6)'",";",null,""]
[4,"교차로 현시 운영 계획 번호","IXR_PHAS_OPER_PLAN_NMBR","NUMBER",2,"time paln\nID\n1~16",null,"현시운영계획번호","PK","NOT NULL","phas_oper_plan_no","NUMBER(2)","INTEGER","NUMBER(2)","현시운영계획번호 (time plan ID, 1~16)",null,null,null,"phas_oper_plan_no ","INTEGER ","NOT NULL",",",null,"phas_oper_plan_no",",",null,null,"phas_oper_plan_no ","NUMBER(2) ","NOT NULL",",",null,null,"phas_oper_plan_no",",","COMMENT ON COLUMN ","soitdtimeplan.","phas_oper_plan_no"," IS ","'현시운영계획번호 (time plan ID, 1~16)'",";",null,""]
[5,"수집 일시","CLCT_DT","DATE","DATE","sysdate",null,"수집유닉스시각","PK","NOT NULL","clct_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)","수집유닉스시각",null,null,null,"clct_unix_tm ","INTEGER ","NOT NULL",",",null,"clct_unix_tm","));",null,null,"clct_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"clct_unix_tm",")","COMMENT ON COLUMN ","soitdtimeplan.","clct_unix_tm"," IS ","'수집유닉스시각'",";",null,""]
[2,"수집일","CLCT_DATE","VARHCAR2",8,"YYYYMMDD",null,"수집일시",null,"NOT NULL","clct_dt","VARCHAR2(8)","VARCHAR(8)","VARCHAR2(8)","수집일시(yyyyMMdd)",null,null,null,{"$f":"K91","v":"clct_dt"},"VARCHAR(8) ","NOT NULL",",",null,"",null,null,null,"clct_dt ","VARCHAR2(8) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitdtimeplan.","clct_dt"," IS ","'수집일시(yyyyMMdd)'",";"]
[6,"주기","CYCL","NUMBER",3,null,null,"주기시간",null,"NOT NULL","cycl_hr","NUMBER(3)","INTEGER","NUMBER(3)","주기시간 (sec)",null,null,null,{"$f":"K92&\" \"","v":"cycl_hr "},"INTEGER ","NOT NULL",",",null,"",{"$f":"IF(OR(I92=\"PK\", I92=\"PK/FK\"), \",\", \"\")","v":""},null,null,"cycl_hr ","NUMBER(3) ","NOT NULL",",",null,null,"",{"$f":"IF(OR(I92=\"PK\", I92=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitdtimeplan.","cycl_hr"," IS ","'주기시간 (sec)'",";",null,{"$f":"IF(LEFT(AB92, 13) = \"CONSTRAINT PK\", AB92, \"\")","v":""}]
[7,"옵셋","OFST","NUMBER",3,null,null,"옵셋시간",null,"NOT NULL","ofst_hr","NUMBER(3)","INTEGER","NUMBER(3)","옵셋시간 (sec)",null,null,null,"ofst_hr ","INTEGER ","NOT NULL",",",null,"","",null,null,"ofst_hr ","NUMBER(3) ","NOT NULL",",",null,null,"","","COMMENT ON COLUMN ","soitdtimeplan.","ofst_hr"," IS ","'옵셋시간 (sec)'",";",null,""]
[8,"A링 1현시","ARING_1PHAS","NUMBER",3,null,null,"A링1현시시간",null,"NULL","A_ring_1_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링1현시시간 (sec)",null,null,null,"A_ring_1_phas_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_1_phas_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdtimeplan.","A_ring_1_phas_hr"," IS ","'A링1현시시간 (sec)'",";",null,""]
[9,"A링 2현시","ARING_2PHAS","NUMBER",3,null,null,"A링2현시시간",null,"NULL","A_ring_2_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링2현시시간 (sec)",null,null,null,"A_ring_2_phas_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_2_phas_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdtimeplan.","A_ring_2_phas_hr"," IS ","'A링2현시시간 (sec)'",";",null,""]
[10,"A링 3현시","ARING_3PHAS","NUMBER",3,null,null,"A링3현시시간",null,"NULL","A_ring_3_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링3현시시간 (sec)",null,null,null,"A_ring_3_phas_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_3_phas_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdtimeplan.","A_ring_3_phas_hr"," IS ","'A링3현시시간 (sec)'",";",null,""]
[11,"A링 4현시","ARING_4PHAS","NUMBER",3,null,null,"A링4현시시간",null,"NULL","A_ring_4_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링4현시시간 (sec)",null,null,null,"A_ring_4_phas_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_4_phas_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdtimeplan.","A_ring_4_phas_hr"," IS ","'A링4현시시간 (sec)'",";",null,""]
[12,"A링 5현시","ARING_5PHAS","NUMBER",3,null,null,"A링5현시시간",null,"NULL","A_ring_5_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링5현시시간 (sec)",null,null,null,"A_ring_5_phas_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_5_phas_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdtimeplan.","A_ring_5_phas_hr"," IS ","'A링5현시시간 (sec)'",";",null,""]
[13,"A링 6현시","ARING_6PHAS","NUMBER",3,null,null,"A링6현시시간",null,"NULL","A_ring_6_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링6현시시간 (sec)",null,null,null,"A_ring_6_phas_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_6_phas_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdtimeplan.","A_ring_6_phas_hr"," IS ","'A링6현시시간 (sec)'",";",null,""]
[14,"A링 7현시","ARING_7PHAS","NUMBER",3,null,null,"A링7현시시간",null,"NULL","A_ring_7_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링7현시시간 (sec)",null,null,null,"A_ring_7_phas_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_7_phas_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdtimeplan.","A_ring_7_phas_hr"," IS ","'A링7현시시간 (sec)'",";",null,""]
[15,"A링 8현시","ARING_8PHAS","NUMBER",3,null,null,"A링8현시시간",null,"NULL","A_ring_8_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링8현시시간 (sec)",null,null,null,"A_ring_8_phas_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_8_phas_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdtimeplan.","A_ring_8_phas_hr"," IS ","'A링8현시시간 (sec)'",";",null,""]
[16,"B링 1현시","BRING_1PHAS","NUMBER",3,null,null,"B링1현시시간",null,"NULL","B_ring_1_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링1현시시간 (sec)",null,null,null,"B_ring_1_phas_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_1_phas_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdtimeplan.","B_ring_1_phas_hr"," IS ","'B링1현시시간 (sec)'",";",null,""]
[17,"B링 2현시","BRING_2PHAS","NUMBER",3,null,null,"B링2현시시간",null,"NULL","B_ring_2_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링2현시시간 (sec)",null,null,null,"B_ring_2_phas_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_2_phas_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdtimeplan.","B_ring_2_phas_hr"," IS ","'B링2현시시간 (sec)'",";",null,""]
[18,"B링 3현시","BRING_3PHAS","NUMBER",3,null,null,"B링3현시시간",null,"NULL","B_ring_3_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링3현시시간 (sec)",null,null,null,"B_ring_3_phas_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_3_phas_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdtimeplan.","B_ring_3_phas_hr"," IS ","'B링3현시시간 (sec)'",";",null,""]
[19,"B링 4현시","BRING_4PHAS","NUMBER",3,null,null,"B링4현시시간",null,"NULL","B_ring_4_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링4현시시간 (sec)",null,null,null,"B_ring_4_phas_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_4_phas_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdtimeplan.","B_ring_4_phas_hr"," IS ","'B링4현시시간 (sec)'",";",null,""]
[20,"B링 5현시","BRING_5PHAS","NUMBER",3,null,null,"B링5현시시간",null,"NULL","B_ring_5_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링5현시시간 (sec)",null,null,null,"B_ring_5_phas_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_5_phas_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdtimeplan.","B_ring_5_phas_hr"," IS ","'B링5현시시간 (sec)'",";",null,""]
[21,"B링 6현시","BRING_6PHAS","NUMBER",3,null,null,"B링6현시시간",null,"NULL","B_ring_6_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링6현시시간 (sec)",null,null,null,"B_ring_6_phas_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_6_phas_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdtimeplan.","B_ring_6_phas_hr"," IS ","'B링6현시시간 (sec)'",";",null,""]
[22,"B링 7현시","BRING_7PHAS","NUMBER",3,null,null,"B링7현시시간",null,"NULL","B_ring_7_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링7현시시간 (sec)",null,null,null,"B_ring_7_phas_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_7_phas_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdtimeplan.","B_ring_7_phas_hr"," IS ","'B링7현시시간 (sec)'",";",null,""]
[23,"B링 8현시","BRING_8PHAS","NUMBER",3,null,null,"B링8현시시간",null,"NULL","B_ring_8_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링8현시시간 (sec)",null,null,null,"B_ring_8_phas_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_8_phas_hr ","NUMBER(3) ","",{"$f":"\") TABLESPACE \"&AF111&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_D001 NOLOGGING"},null,null,{"$f":"IF(OR(C109=\"PK\", C109=\"PK/FK\"), E109, \"\")","v":""},null,"COMMENT ON COLUMN ","soitdtimeplan.","B_ring_8_phas_hr"," IS ","'B링8현시시간 (sec)'",";",null,""]
[{"$nulls":18},{"$f":"CONCATENATE(W86:Y90)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AF110:AH110)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (clct_unix_tm) INTERVAL (86400) STORE IN (\"&AF111&\") (PARTITION BFR_\" & H84 & \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AF111&\");\"","v":"PARTITION BY RANGE (clct_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_D001) (PARTITION BFR_soitdtimeplan_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_D001);"},{"$f":"\"CREATE INDEX PK_\" & H84& \" ON \" & H84 & CONCATENATE(AG86:AI95) & \" LOCAL (PARTITION BFR_\" & H84 & \"_20221101 TABLESPACE \"&AG111&\") TABLESPACE \"&AG111&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & H84 & \" ADD CONSTRAINT PK_\" & H84 & \" PRIMARY KEY \" & CONCATENATE(AG86:AI97) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$error":"#VALUE!"}]
[{"$nulls":31},"SOIT_D08_D001","SOIT_I08_D001",{"$nulls":9},""]
["- 교차로현시(IXR_PHAS)",{"$nulls":6},"soitdintsphasinfo",{"$nulls":34},""]
["NO","속성명","컬럼명","형태","길이","비고",null,"논리명","PK/FK","NULL","물리명","형태","VOLT","TIBERO","COMMENT",{"$nulls":20},"COMMENT ON TABLE",{"$f":"H112&\" \"","v":"soitdintsphasinfo "},null," IS ",{"$f":"\"'\"&A112&\"'\"","v":"'- 교차로현시(IXR_PHAS)'"},";",null,""]
[1,"신호 교차로 번호","SGNL_IXR_NMBR","NUMBER",4,null,null,"현장교차로ID","PK/FK","NOT NULL","spot_ints_id","NUMBER(5)","INTEGER","NUMBER(5)","현장교차로ID",null,"CREATE TABLE ",{"$f":"H112&\" (\"","v":"soitdintsphasinfo ("},{"$f":"K114&\" \"","v":"spot_ints_id "},{"$f":"M114&\" \"","v":"INTEGER "},{"$f":"IF(J114=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(I114=\"PK\", I114=\"PK/FK\"), K114, \"\")","v":"spot_ints_id"},{"$f":"IF(OR(I114=\"PK\", I114=\"PK/FK\"), \",\", \"\")","v":","},"CREATE TABLE ",{"$f":"H112&\" (\"","v":"soitdintsphasinfo ("},{"$f":"K114&\" \"","v":"spot_ints_id "},{"$f":"N114&\" \"","v":"NUMBER(5) "},{"$f":"IF(J114=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(I114=\"PK\", I114=\"PK/FK\"), K114, \"\")","v":"spot_ints_id"},{"$f":"IF(OR(I114=\"PK\", I114=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$H$112&\".\"","v":"soitdintsphasinfo."},{"$f":"K114","v":"spot_ints_id"}," IS ",{"$f":"\"'\"&O114&\"'\"","v":"'현장교차로ID'"},";",null,""]
[2,"수집 일시","CLCT_DT","INTEGER","UTC",null,null,"수집유닉스시각","PK","NOT NULL","clct_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)","수집유닉스시각",null,null,null,"clct_unix_tm ","INTEGER ","NOT NULL",",",null,"clct_unix_tm",",",null,null,"clct_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"clct_unix_tm",",","COMMENT ON COLUMN ","soitdintsphasinfo.","clct_unix_tm"," IS ","'수집유닉스시각'",";",null,""]
[2,"수집일","CLCT_DATE","VARHCAR2",8,"YYYYMMDD",null,"수집일시",null,"NOT NULL","clct_dt","VARCHAR2(8)","VARCHAR(8)","VARCHAR2(8)","수집일시(yyyyMMdd)",null,null,null,{"$f":"K116","v":"clct_dt"},"VARCHAR(8) ","NOT NULL",",",null,"",null,null,null,"clct_dt ","VARCHAR2(8) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitdintsphasinfo.","clct_dt"," IS ","'수집일시(yyyyMMdd)'",";"]
[3,"교차로 운영 모드","IXR_OPER_MODE","NUMBER",2,"0:일반 , 1:시차1, 2: 시차2, 3:시차3, 4:시차4, 5:시차5","운영구분코드(801)","운영구분코드","PK","NOT NULL","oper_se_cd","CHAR(3)","VARCHAR(3)","VARCHAR2(3)","운영구분코드(801)","운영구분코드 (0:일반 , 1:시차1, 2: 시차2, 3:시차3, 4:시차4, 5:시차5)",null,null,{"$f":"K117&\" \"","v":"oper_se_cd "},"VARCHAR(3) ","NOT NULL",",",null,"oper_se_cd","));",null,null,"oper_se_cd ","VARCHAR2(3) ","NOT NULL",",",null,null,"oper_se_cd",")","COMMENT ON COLUMN ","soitdintsphasinfo.","oper_se_cd"," IS ","'운영구분코드(801)'",";",null,{"$f":"IF(LEFT(AB117, 13) = \"CONSTRAINT PK\", AB117, \"\")","v":""}]
[4,"A링 1현시 이동류 번호","ARING_1PHAS_CRFL_NMBR","NUMBER",2,null,null,"A링1현시이동류번호",null,"NULL","A_ring_1_phas_mvmt_no","NUMBER(2)","INTEGER","NUMBER(2)","A링1현시이동류번호",null,null,null,"A_ring_1_phas_mvmt_no ","INTEGER ","",",",null,"",{"$f":"IF(OR(I118=\"PK\", I118=\"PK/FK\"), \",\", \"\")","v":""},null,null,"A_ring_1_phas_mvmt_no ","NUMBER(2) ","",",",null,null,"",{"$f":"IF(OR(I118=\"PK\", I118=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitdintsphasinfo.","A_ring_1_phas_mvmt_no"," IS ","'A링1현시이동류번호'",";",null,""]
[5,"A링 2현시 이동류 번호","ARING_2PHAS_CRFL_NMBR","NUMBER",2,null,null,"A링2현시이동류번호",null,"NULL","A_ring_2_phas_mvmt_no","NUMBER(2)","INTEGER","NUMBER(2)","A링2현시이동류번호",null,null,null,"A_ring_2_phas_mvmt_no ","INTEGER ","",",",null,"","",null,null,"A_ring_2_phas_mvmt_no ","NUMBER(2) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","A_ring_2_phas_mvmt_no"," IS ","'A링2현시이동류번호'",";",null,""]
[6,"A링 3현시 이동류 번호","ARING_3PHAS_CRFL_NMBR","NUMBER",2,null,null,"A링3현시이동류번호",null,"NULL","A_ring_3_phas_mvmt_no","NUMBER(2)","INTEGER","NUMBER(2)","A링3현시이동류번호",null,null,null,"A_ring_3_phas_mvmt_no ","INTEGER ","",",",null,"","",null,null,"A_ring_3_phas_mvmt_no ","NUMBER(2) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","A_ring_3_phas_mvmt_no"," IS ","'A링3현시이동류번호'",";",null,""]
[7,"A링 4현시 이동류 번호","ARING_4PHAS_CRFL_NMBR","NUMBER",2,null,null,"A링4현시이동류번호",null,"NULL","A_ring_4_phas_mvmt_no","NUMBER(2)","INTEGER","NUMBER(2)","A링4현시이동류번호",null,null,null,"A_ring_4_phas_mvmt_no ","INTEGER ","",",",null,"","",null,null,"A_ring_4_phas_mvmt_no ","NUMBER(2) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","A_ring_4_phas_mvmt_no"," IS ","'A링4현시이동류번호'",";",null,""]
[8,"A링 5현시 이동류 번호","ARING_5PHAS_CRFL_NMBR","NUMBER",2,null,null,"A링5현시이동류번호",null,"NULL","A_ring_5_phas_mvmt_no","NUMBER(2)","INTEGER","NUMBER(2)","A링5현시이동류번호",null,null,null,"A_ring_5_phas_mvmt_no ","INTEGER ","",",",null,"","",null,null,"A_ring_5_phas_mvmt_no ","NUMBER(2) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","A_ring_5_phas_mvmt_no"," IS ","'A링5현시이동류번호'",";",null,""]
[9,"A링 6현시 이동류 번호","ARING_6PHAS_CRFL_NMBR","NUMBER",2,null,null,"A링6현시이동류번호",null,"NULL","A_ring_6_phas_mvmt_no","NUMBER(2)","INTEGER","NUMBER(2)","A링6현시이동류번호",null,null,null,"A_ring_6_phas_mvmt_no ","INTEGER ","",",",null,"","",null,null,"A_ring_6_phas_mvmt_no ","NUMBER(2) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","A_ring_6_phas_mvmt_no"," IS ","'A링6현시이동류번호'",";",null,""]
[10,"A링 7현시 이동류 번호","ARING_7PHAS_CRFL_NMBR","NUMBER",2,null,null,"A링7현시이동류번호",null,"NULL","A_ring_7_phas_mvmt_no","NUMBER(2)","INTEGER","NUMBER(2)","A링7현시이동류번호",null,null,null,"A_ring_7_phas_mvmt_no ","INTEGER ","",",",null,"","",null,null,"A_ring_7_phas_mvmt_no ","NUMBER(2) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","A_ring_7_phas_mvmt_no"," IS ","'A링7현시이동류번호'",";",null,""]
[11,"A링 8현시 이동류 번호","ARING_8PHAS_CRFL_NMBR","NUMBER",2,null,null,"A링8현시이동류번호",null,"NULL","A_ring_8_phas_mvmt_no","NUMBER(2)","INTEGER","NUMBER(2)","A링8현시이동류번호",null,null,null,"A_ring_8_phas_mvmt_no ","INTEGER ","",",",null,"","",null,null,"A_ring_8_phas_mvmt_no ","NUMBER(2) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","A_ring_8_phas_mvmt_no"," IS ","'A링8현시이동류번호'",";",null,""]
[12,"B링 1현시 이동류 번호","BRING_1PHAS_CRFL_NMBR","NUMBER",2,null,null,"B링1현시이동류번호",null,"NULL","B_ring_1_phas_mvmt_no","NUMBER(2)","INTEGER","NUMBER(2)","B링1현시이동류번호",null,null,null,"B_ring_1_phas_mvmt_no ","INTEGER ","",",",null,"","",null,null,"B_ring_1_phas_mvmt_no ","NUMBER(2) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","B_ring_1_phas_mvmt_no"," IS ","'B링1현시이동류번호'",";",null,""]
[13,"B링 2현시 이동류 번호","BRING_2PHAS_CRFL_NMBR","NUMBER",2,null,null,"B링2현시이동류번호",null,"NULL","B_ring_2_phas_mvmt_no","NUMBER(2)","INTEGER","NUMBER(2)","B링2현시이동류번호",null,null,null,"B_ring_2_phas_mvmt_no ","INTEGER ","",",",null,"","",null,null,"B_ring_2_phas_mvmt_no ","NUMBER(2) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","B_ring_2_phas_mvmt_no"," IS ","'B링2현시이동류번호'",";",null,""]
[14,"B링 3현시 이동류 번호","BRING_3PHAS_CRFL_NMBR","NUMBER",2,null,null,"B링3현시이동류번호",null,"NULL","B_ring_3_phas_mvmt_no","NUMBER(2)","INTEGER","NUMBER(2)","B링3현시이동류번호",null,null,null,"B_ring_3_phas_mvmt_no ","INTEGER ","",",",null,"","",null,null,"B_ring_3_phas_mvmt_no ","NUMBER(2) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","B_ring_3_phas_mvmt_no"," IS ","'B링3현시이동류번호'",";",null,""]
[15,"B링 4현시 이동류 번호","BRING_4PHAS_CRFL_NMBR","NUMBER",2,null,null,"B링4현시이동류번호",null,"NULL","B_ring_4_phas_mvmt_no","NUMBER(2)","INTEGER","NUMBER(2)","B링4현시이동류번호",null,null,null,"B_ring_4_phas_mvmt_no ","INTEGER ","",",",null,"","",null,null,"B_ring_4_phas_mvmt_no ","NUMBER(2) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","B_ring_4_phas_mvmt_no"," IS ","'B링4현시이동류번호'",";",null,""]
[16,"B링 5현시 이동류 번호","BRING_5PHAS_CRFL_NMBR","NUMBER",2,null,null,"B링5현시이동류번호",null,"NULL","B_ring_5_phas_mvmt_no","NUMBER(2)","INTEGER","NUMBER(2)","B링5현시이동류번호",null,null,null,"B_ring_5_phas_mvmt_no ","INTEGER ","",",",null,"","",null,null,"B_ring_5_phas_mvmt_no ","NUMBER(2) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","B_ring_5_phas_mvmt_no"," IS ","'B링5현시이동류번호'",";",null,""]
[17,"B링 6현시 이동류 번호","BRING_6PHAS_CRFL_NMBR","NUMBER",2,null,null,"B링6현시이동류번호",null,"NULL","B_ring_6_phas_mvmt_no","NUMBER(2)","INTEGER","NUMBER(2)","B링6현시이동류번호",null,null,null,"B_ring_6_phas_mvmt_no ","INTEGER ","",",",null,"","",null,null,"B_ring_6_phas_mvmt_no ","NUMBER(2) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","B_ring_6_phas_mvmt_no"," IS ","'B링6현시이동류번호'",";",null,""]
[18,"B링 7현시 이동류 번호","BRING_7PHAS_CRFL_NMBR","NUMBER",2,null,null,"B링7현시이동류번호",null,"NULL","B_ring_7_phas_mvmt_no","NUMBER(2)","INTEGER","NUMBER(2)","B링7현시이동류번호",null,null,null,"B_ring_7_phas_mvmt_no ","INTEGER ","",",",null,"","",null,null,"B_ring_7_phas_mvmt_no ","NUMBER(2) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","B_ring_7_phas_mvmt_no"," IS ","'B링7현시이동류번호'",";",null,""]
[19,"B링 8현시 이동류 번호","BRING_8PHAS_CRFL_NMBR","NUMBER",2,null,null,"B링8현시이동류번호",null,"NULL","B_ring_8_phas_mvmt_no","NUMBER(2)","INTEGER","NUMBER(2)","B링8현시이동류번호",null,null,null,"B_ring_8_phas_mvmt_no ","INTEGER ","",",",null,"","",null,null,"B_ring_8_phas_mvmt_no ","NUMBER(2) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","B_ring_8_phas_mvmt_no"," IS ","'B링8현시이동류번호'",";",null,""]
[20,"A링 1현시 최소 녹색 시간","ARING_1PHAS_MIN_GREN_HH","NUMBER",3,"초",null,"A링1현시최소녹색시간",null,"NULL","A_ring_1_phas_min_gren_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링1현시최소녹색시간 (sec)",null,null,null,"A_ring_1_phas_min_gren_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_1_phas_min_gren_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","A_ring_1_phas_min_gren_hr"," IS ","'A링1현시최소녹색시간 (sec)'",";",null,""]
[21,"A링 2현시 최소 녹색 시간","ARING_2PHAS_MIN_GREN_HH","NUMBER",3,"초",null,"A링2현시최소녹색시간",null,"NULL","A_ring_2_phas_min_gren_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링2현시최소녹색시간 (sec)",null,null,null,"A_ring_2_phas_min_gren_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_2_phas_min_gren_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","A_ring_2_phas_min_gren_hr"," IS ","'A링2현시최소녹색시간 (sec)'",";",null,""]
[22,"A링 3현시 최소 녹색 시간","ARING_3PHAS_MIN_GREN_HH","NUMBER",3,"초",null,"A링3현시최소녹색시간",null,"NULL","A_ring_3_phas_min_gren_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링3현시최소녹색시간 (sec)",null,null,null,"A_ring_3_phas_min_gren_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_3_phas_min_gren_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","A_ring_3_phas_min_gren_hr"," IS ","'A링3현시최소녹색시간 (sec)'",";",null,""]
[23,"A링 4현시 최소 녹색 시간","ARING_4PHAS_MIN_GREN_HH","NUMBER",3,"초",null,"A링4현시최소녹색시간",null,"NULL","A_ring_4_phas_min_gren_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링4현시최소녹색시간 (sec)",null,null,null,"A_ring_4_phas_min_gren_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_4_phas_min_gren_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","A_ring_4_phas_min_gren_hr"," IS ","'A링4현시최소녹색시간 (sec)'",";",null,""]
[24,"A링 5현시 최소 녹색 시간","ARING_5PHAS_MIN_GREN_HH","NUMBER",3,"초",null,"A링5현시최소녹색시간",null,"NULL","A_ring_5_phas_min_gren_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링5현시최소녹색시간 (sec)",null,null,null,"A_ring_5_phas_min_gren_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_5_phas_min_gren_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","A_ring_5_phas_min_gren_hr"," IS ","'A링5현시최소녹색시간 (sec)'",";",null,""]
[25,"A링 6현시 최소 녹색 시간","ARING_6PHAS_MIN_GREN_HH","NUMBER",3,"초",null,"A링6현시최소녹색시간",null,"NULL","A_ring_6_phas_min_gren_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링6현시최소녹색시간 (sec)",null,null,null,"A_ring_6_phas_min_gren_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_6_phas_min_gren_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","A_ring_6_phas_min_gren_hr"," IS ","'A링6현시최소녹색시간 (sec)'",";",null,""]
[26,"A링 7현시 최소 녹색 시간","ARING_7PHAS_MIN_GREN_HH","NUMBER",3,"초",null,"A링7현시최소녹색시간",null,"NULL","A_ring_7_phas_min_gren_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링7현시최소녹색시간 (sec)",null,null,null,"A_ring_7_phas_min_gren_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_7_phas_min_gren_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","A_ring_7_phas_min_gren_hr"," IS ","'A링7현시최소녹색시간 (sec)'",";",null,""]
[27,"A링 8현시 최소 녹색 시간","ARING_8PHAS_MIN_GREN_HH","NUMBER",3,"초",null,"A링8현시최소녹색시간",null,"NULL","A_ring_8_phas_min_gren_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링8현시최소녹색시간 (sec)",null,null,null,"A_ring_8_phas_min_gren_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_8_phas_min_gren_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","A_ring_8_phas_min_gren_hr"," IS ","'A링8현시최소녹색시간 (sec)'",";",null,""]
[28,"B링 1현시 최소 녹색 시간","BRING_1PHAS_MIN_GREN_HH","NUMBER",3,"초",null,"B링1현시최소녹색시간",null,"NULL","B_ring_1_phas_min_gren_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링1현시최소녹색시간 (sec)",null,null,null,"B_ring_1_phas_min_gren_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_1_phas_min_gren_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","B_ring_1_phas_min_gren_hr"," IS ","'B링1현시최소녹색시간 (sec)'",";",null,""]
[29,"B링 2현시 최소 녹색 시간","BRING_2PHAS_MIN_GREN_HH","NUMBER",3,"초",null,"B링2현시최소녹색시간",null,"NULL","B_ring_2_phas_min_gren_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링2현시최소녹색시간 (sec)",null,null,null,"B_ring_2_phas_min_gren_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_2_phas_min_gren_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","B_ring_2_phas_min_gren_hr"," IS ","'B링2현시최소녹색시간 (sec)'",";",null,""]
[30,"B링 3현시 최소 녹색 시간","BRING_3PHAS_MIN_GREN_HH","NUMBER",3,"초",null,"B링3현시최소녹색시간",null,"NULL","B_ring_3_phas_min_gren_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링3현시최소녹색시간 (sec)",null,null,null,"B_ring_3_phas_min_gren_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_3_phas_min_gren_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","B_ring_3_phas_min_gren_hr"," IS ","'B링3현시최소녹색시간 (sec)'",";",null,""]
[31,"B링 4현시 최소 녹색 시간","BRING_4PHAS_MIN_GREN_HH","NUMBER",3,"초",null,"B링4현시최소녹색시간",null,"NULL","B_ring_4_phas_min_gren_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링4현시최소녹색시간 (sec)",null,null,null,"B_ring_4_phas_min_gren_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_4_phas_min_gren_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","B_ring_4_phas_min_gren_hr"," IS ","'B링4현시최소녹색시간 (sec)'",";",null,""]
[32,"B링 5현시 최소 녹색 시간","BRING_5PHAS_MIN_GREN_HH","NUMBER",3,"초",null,"B링5현시최소녹색시간",null,"NULL","B_ring_5_phas_min_gren_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링5현시최소녹색시간 (sec)",null,null,null,"B_ring_5_phas_min_gren_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_5_phas_min_gren_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","B_ring_5_phas_min_gren_hr"," IS ","'B링5현시최소녹색시간 (sec)'",";",null,""]
[33,"B링 6현시 최소 녹색 시간","BRING_6PHAS_MIN_GREN_HH","NUMBER",3,"초",null,"B링6현시최소녹색시간",null,"NULL","B_ring_6_phas_min_gren_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링6현시최소녹색시간 (sec)",null,null,null,"B_ring_6_phas_min_gren_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_6_phas_min_gren_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","B_ring_6_phas_min_gren_hr"," IS ","'B링6현시최소녹색시간 (sec)'",";",null,""]
[34,"B링 7현시 최소 녹색 시간","BRING_7PHAS_MIN_GREN_HH","NUMBER",3,"초",null,"B링7현시최소녹색시간",null,"NULL","B_ring_7_phas_min_gren_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링7현시최소녹색시간 (sec)",null,null,null,"B_ring_7_phas_min_gren_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_7_phas_min_gren_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","B_ring_7_phas_min_gren_hr"," IS ","'B링7현시최소녹색시간 (sec)'",";",null,""]
[35,"B링 8현시 최소 녹색 시간","BRING_8PHAS_MIN_GREN_HH","NUMBER",3,"초",null,"B링8현시최소녹색시간",null,"NULL","B_ring_8_phas_min_gren_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링8현시최소녹색시간 (sec)",null,null,null,"B_ring_8_phas_min_gren_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_8_phas_min_gren_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","B_ring_8_phas_min_gren_hr"," IS ","'B링8현시최소녹색시간 (sec)'",";",null,""]
[36,"A링 1현시 최대 녹색 시간","ARING_1PHAS_MAX_GREN_HH","NUMBER",3,"초",null,"A링1현시최대녹색시간",null,"NULL","A_ring_1_phas_max_gren_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링1현시최대녹색시간 (sec)",null,null,null,"A_ring_1_phas_max_gren_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_1_phas_max_gren_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","A_ring_1_phas_max_gren_hr"," IS ","'A링1현시최대녹색시간 (sec)'",";",null,""]
[37,"A링 2현시 최대 녹색 시간","ARING_2PHAS_MAX_GREN_HH","NUMBER",3,"초",null,"A링2현시최대녹색시간",null,"NULL","A_ring_2_phas_max_gren_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링2현시최대녹색시간 (sec)",null,null,null,"A_ring_2_phas_max_gren_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_2_phas_max_gren_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","A_ring_2_phas_max_gren_hr"," IS ","'A링2현시최대녹색시간 (sec)'",";",null,""]
[38,"A링 3현시 최대 녹색 시간","ARING_3PHAS_MAX_GREN_HH","NUMBER",3,"초",null,"A링3현시최대녹색시간",null,"NULL","A_ring_3_phas_max_gren_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링3현시최대녹색시간 (sec)",null,null,null,"A_ring_3_phas_max_gren_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_3_phas_max_gren_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","A_ring_3_phas_max_gren_hr"," IS ","'A링3현시최대녹색시간 (sec)'",";",null,""]
[39,"A링 4현시 최대 녹색 시간","ARING_4PHAS_MAX_GREN_HH","NUMBER",3,"초",null,"A링4현시최대녹색시간",null,"NULL","A_ring_4_phas_max_gren_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링4현시최대녹색시간 (sec)",null,null,null,"A_ring_4_phas_max_gren_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_4_phas_max_gren_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","A_ring_4_phas_max_gren_hr"," IS ","'A링4현시최대녹색시간 (sec)'",";",null,""]
[40,"A링 5현시 최대 녹색 시간","ARING_5PHAS_MAX_GREN_HH","NUMBER",3,"초",null,"A링5현시최대녹색시간",null,"NULL","A_ring_5_phas_max_gren_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링5현시최대녹색시간 (sec)",null,null,null,"A_ring_5_phas_max_gren_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_5_phas_max_gren_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","A_ring_5_phas_max_gren_hr"," IS ","'A링5현시최대녹색시간 (sec)'",";",null,""]
[41,"A링 6현시 최대 녹색 시간","ARING_6PHAS_MAX_GREN_HH","NUMBER",3,"초",null,"A링6현시최대녹색시간",null,"NULL","A_ring_6_phas_max_gren_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링6현시최대녹색시간 (sec)",null,null,null,"A_ring_6_phas_max_gren_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_6_phas_max_gren_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","A_ring_6_phas_max_gren_hr"," IS ","'A링6현시최대녹색시간 (sec)'",";",null,""]
[42,"A링 7현시 최대 녹색 시간","ARING_7PHAS_MAX_GREN_HH","NUMBER",3,"초",null,"A링7현시최대녹색시간",null,"NULL","A_ring_7_phas_max_gren_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링7현시최대녹색시간 (sec)",null,null,null,"A_ring_7_phas_max_gren_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_7_phas_max_gren_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","A_ring_7_phas_max_gren_hr"," IS ","'A링7현시최대녹색시간 (sec)'",";",null,""]
[43,"A링 8현시 최대 녹색 시간","ARING_8PHAS_MAX_GREN_HH","NUMBER",3,"초",null,"A링8현시최대녹색시간",null,"NULL","A_ring_8_phas_max_gren_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링8현시최대녹색시간 (sec)",null,null,null,"A_ring_8_phas_max_gren_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_8_phas_max_gren_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","A_ring_8_phas_max_gren_hr"," IS ","'A링8현시최대녹색시간 (sec)'",";",null,""]
[44,"B링 1현시 최대 녹색 시간","BRING_1PHAS_MAX_GREN_HH","NUMBER",3,"초",null,"B링1현시최대녹색시간",null,"NULL","B_ring_1_phas_max_gren_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링1현시최대녹색시간 (sec)",null,null,null,"B_ring_1_phas_max_gren_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_1_phas_max_gren_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","B_ring_1_phas_max_gren_hr"," IS ","'B링1현시최대녹색시간 (sec)'",";",null,""]
[45,"B링 2현시 최대 녹색 시간","BRING_2PHAS_MAX_GREN_HH","NUMBER",3,"초",null,"B링2현시최대녹색시간",null,"NULL","B_ring_2_phas_max_gren_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링2현시최대녹색시간 (sec)",null,null,null,"B_ring_2_phas_max_gren_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_2_phas_max_gren_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","B_ring_2_phas_max_gren_hr"," IS ","'B링2현시최대녹색시간 (sec)'",";",null,""]
[46,"B링 3현시 최대 녹색 시간","BRING_3PHAS_MAX_GREN_HH","NUMBER",3,"초",null,"B링3현시최대녹색시간",null,"NULL","B_ring_3_phas_max_gren_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링3현시최대녹색시간 (sec)",null,null,null,"B_ring_3_phas_max_gren_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_3_phas_max_gren_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","B_ring_3_phas_max_gren_hr"," IS ","'B링3현시최대녹색시간 (sec)'",";",null,""]
[47,"B링 4현시 최대 녹색 시간","BRING_4PHAS_MAX_GREN_HH","NUMBER",3,"초",null,"B링4현시최대녹색시간",null,"NULL","B_ring_4_phas_max_gren_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링4현시최대녹색시간 (sec)",null,null,null,"B_ring_4_phas_max_gren_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_4_phas_max_gren_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","B_ring_4_phas_max_gren_hr"," IS ","'B링4현시최대녹색시간 (sec)'",";",null,""]
[48,"B링 5현시 최대 녹색 시간","BRING_5PHAS_MAX_GREN_HH","NUMBER",3,"초",null,"B링5현시최대녹색시간",null,"NULL","B_ring_5_phas_max_gren_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링5현시최대녹색시간 (sec)",null,null,null,"B_ring_5_phas_max_gren_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_5_phas_max_gren_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","B_ring_5_phas_max_gren_hr"," IS ","'B링5현시최대녹색시간 (sec)'",";",null,""]
[49,"B링 6현시 최대 녹색 시간","BRING_6PHAS_MAX_GREN_HH","NUMBER",3,"초",null,"B링6현시최대녹색시간",null,"NULL","B_ring_6_phas_max_gren_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링6현시최대녹색시간 (sec)",null,null,null,"B_ring_6_phas_max_gren_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_6_phas_max_gren_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","B_ring_6_phas_max_gren_hr"," IS ","'B링6현시최대녹색시간 (sec)'",";",null,""]
[50,"B링 7현시 최대 녹색 시간","BRING_7PHAS_MAX_GREN_HH","NUMBER",3,"초",null,"B링7현시최대녹색시간",null,"NULL","B_ring_7_phas_max_gren_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링7현시최대녹색시간 (sec)",null,null,null,"B_ring_7_phas_max_gren_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_7_phas_max_gren_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","B_ring_7_phas_max_gren_hr"," IS ","'B링7현시최대녹색시간 (sec)'",";",null,""]
[51,"B링 8현시 최대 녹색 시간","BRING_8PHAS_MAX_GREN_HH","NUMBER",3,"초",null,"B링8현시최대녹색시간",null,"NULL","B_ring_8_phas_max_gren_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링8현시최대녹색시간 (sec)",null,null,null,"B_ring_8_phas_max_gren_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_8_phas_max_gren_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","B_ring_8_phas_max_gren_hr"," IS ","'B링8현시최대녹색시간 (sec)'",";",null,""]
[52,"A링 1현시 황색 시간","ARING_1PHAS_YELW_HH","NUMBER",2,"초",null,"A링1현시황색시간",null,"NULL","A_ring_1_phas_yelw_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링1현시황색시간 (sec)",null,null,null,"A_ring_1_phas_yelw_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_1_phas_yelw_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","A_ring_1_phas_yelw_hr"," IS ","'A링1현시황색시간 (sec)'",";",null,""]
[53,"A링 2현시 황색 시간","ARING_2PHAS_YELW_HH","NUMBER",2,"초",null,"A링2현시황색시간",null,"NULL","A_ring_2_phas_yelw_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링2현시황색시간 (sec)",null,null,null,"A_ring_2_phas_yelw_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_2_phas_yelw_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","A_ring_2_phas_yelw_hr"," IS ","'A링2현시황색시간 (sec)'",";",null,""]
[54,"A링 3현시 황색 시간","ARING_3PHAS_YELW_HH","NUMBER",2,"초",null,"A링3현시황색시간",null,"NULL","A_ring_3_phas_yelw_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링3현시황색시간 (sec)",null,null,null,"A_ring_3_phas_yelw_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_3_phas_yelw_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","A_ring_3_phas_yelw_hr"," IS ","'A링3현시황색시간 (sec)'",";",null,""]
[55,"A링 4현시 황색 시간","ARING_4PHAS_YELW_HH","NUMBER",2,"초",null,"A링4현시황색시간",null,"NULL","A_ring_4_phas_yelw_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링4현시황색시간 (sec)",null,null,null,"A_ring_4_phas_yelw_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_4_phas_yelw_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","A_ring_4_phas_yelw_hr"," IS ","'A링4현시황색시간 (sec)'",";",null,""]
[56,"A링 5현시 황색 시간","ARING_5PHAS_YELW_HH","NUMBER",2,"초",null,"A링5현시황색시간",null,"NULL","A_ring_5_phas_yelw_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링5현시황색시간 (sec)",null,null,null,"A_ring_5_phas_yelw_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_5_phas_yelw_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","A_ring_5_phas_yelw_hr"," IS ","'A링5현시황색시간 (sec)'",";",null,""]
[57,"A링 6현시 황색 시간","ARING_6PHAS_YELW_HH","NUMBER",2,"초",null,"A링6현시황색시간",null,"NULL","A_ring_6_phas_yelw_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링6현시황색시간 (sec)",null,null,null,"A_ring_6_phas_yelw_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_6_phas_yelw_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","A_ring_6_phas_yelw_hr"," IS ","'A링6현시황색시간 (sec)'",";",null,""]
[58,"A링 7현시 황색 시간","ARING_7PHAS_YELW_HH","NUMBER",2,"초",null,"A링7현시황색시간",null,"NULL","A_ring_7_phas_yelw_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링7현시황색시간 (sec)",null,null,null,"A_ring_7_phas_yelw_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_7_phas_yelw_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","A_ring_7_phas_yelw_hr"," IS ","'A링7현시황색시간 (sec)'",";",null,""]
[59,"A링 8현시 황색 시간","ARING_8PHAS_YELW_HH","NUMBER",2,"초",null,"A링8현시황색시간",null,"NULL","A_ring_8_phas_yelw_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링8현시황색시간 (sec)",null,null,null,"A_ring_8_phas_yelw_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_8_phas_yelw_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","A_ring_8_phas_yelw_hr"," IS ","'A링8현시황색시간 (sec)'",";",null,""]
[60,"B링 1현시 황색 시간","BRING_1PHAS_YELW_HH","NUMBER",2,"초",null,"B링1현시황색시간",null,"NULL","B_ring_1_phas_yelw_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링1현시황색시간 (sec)",null,null,null,"B_ring_1_phas_yelw_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_1_phas_yelw_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","B_ring_1_phas_yelw_hr"," IS ","'B링1현시황색시간 (sec)'",";",null,""]
[61,"B링 2현시 황색 시간","BRING_2PHAS_YELW_HH","NUMBER",2,"초",null,"B링2현시황색시간",null,"NULL","B_ring_2_phas_yelw_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링2현시황색시간 (sec)",null,null,null,"B_ring_2_phas_yelw_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_2_phas_yelw_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","B_ring_2_phas_yelw_hr"," IS ","'B링2현시황색시간 (sec)'",";",null,""]
[62,"B링 3현시 황색 시간","BRING_3PHAS_YELW_HH","NUMBER",2,"초",null,"B링3현시황색시간",null,"NULL","B_ring_3_phas_yelw_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링3현시황색시간 (sec)",null,null,null,"B_ring_3_phas_yelw_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_3_phas_yelw_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","B_ring_3_phas_yelw_hr"," IS ","'B링3현시황색시간 (sec)'",";",null,""]
[63,"B링 4현시 황색 시간","BRING_4PHAS_YELW_HH","NUMBER",2,"초",null,"B링4현시황색시간",null,"NULL","B_ring_4_phas_yelw_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링4현시황색시간 (sec)",null,null,null,"B_ring_4_phas_yelw_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_4_phas_yelw_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","B_ring_4_phas_yelw_hr"," IS ","'B링4현시황색시간 (sec)'",";",null,""]
[64,"B링 5현시 황색 시간","BRING_5PHAS_YELW_HH","NUMBER",2,"초",null,"B링5현시황색시간",null,"NULL","B_ring_5_phas_yelw_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링5현시황색시간 (sec)",null,null,null,"B_ring_5_phas_yelw_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_5_phas_yelw_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","B_ring_5_phas_yelw_hr"," IS ","'B링5현시황색시간 (sec)'",";",null,""]
[65,"B링 6현시 황색 시간","BRING_6PHAS_YELW_HH","NUMBER",2,"초",null,"B링6현시황색시간",null,"NULL","B_ring_6_phas_yelw_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링6현시황색시간 (sec)",null,null,null,"B_ring_6_phas_yelw_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_6_phas_yelw_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","B_ring_6_phas_yelw_hr"," IS ","'B링6현시황색시간 (sec)'",";",null,""]
[66,"B링 7현시 황색 시간","BRING_7PHAS_YELW_HH","NUMBER",2,"초",null,"B링7현시황색시간",null,"NULL","B_ring_7_phas_yelw_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링7현시황색시간 (sec)",null,null,null,"B_ring_7_phas_yelw_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_7_phas_yelw_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdintsphasinfo.","B_ring_7_phas_yelw_hr"," IS ","'B링7현시황색시간 (sec)'",";",null,""]
[67,"B링 8현시 황색 시간","BRING_8PHAS_YELW_HH","NUMBER",2,"초",null,"B링8현시황색시간",null,"NULL","B_ring_8_phas_yelw_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링8현시황색시간 (sec)",null,null,null,"B_ring_8_phas_yelw_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_8_phas_yelw_hr ","NUMBER(3) ","",{"$f":"\") TABLESPACE \"&AF183&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_D001 NOLOGGING"},null,null,{"$f":"IF(OR(C181=\"PK\", C181=\"PK/FK\"), E181, \"\")","v":""},null,"COMMENT ON COLUMN ","soitdintsphasinfo.","B_ring_8_phas_yelw_hr"," IS ","'B링8현시황색시간 (sec)'",";",null,""]
[{"$nulls":18},{"$f":"CONCATENATE(W114:Y117)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AF182:AH182)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (clct_unix_tm) INTERVAL (86400) STORE IN (\"&AF183&\") (PARTITION BFR_\" & H112 & \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AF183&\");\"","v":"PARTITION BY RANGE (clct_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_D001) (PARTITION BFR_soitdintsphasinfo_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_D001);"},{"$f":"\"CREATE INDEX PK_\" & H112& \" ON \" & H112 & CONCATENATE(AG114:AI122) & \" LOCAL (PARTITION BFR_\" & H112 & \"_20221101 TABLESPACE \"&AG183&\") TABLESPACE \"&AG183&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & H112 & \" ADD CONSTRAINT PK_\" & H112 & \" PRIMARY KEY \" & CONCATENATE(AG114:AI130) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$error":"#VALUE!"}]
[{"$nulls":31},"SOIT_D08_D001","SOIT_I08_D001",{"$nulls":9},""]
["- 교차로그룹관리(IXR_GROP_MNGM)",{"$nulls":6},"soitdintsgrp",{"$nulls":34},""]
["NO","속성명","컬럼명","형태","길이","비고",null,"논리명","PK/FK","NULL","물리명","형태","VOLT","TIBERO","COMMENT",{"$nulls":20},"COMMENT ON TABLE",{"$f":"H184&\" \"","v":"soitdintsgrp "},null," IS ",{"$f":"\"'\"&A184&\"'\"","v":"'- 교차로그룹관리(IXR_GROP_MNGM)'"},";",null,""]
[1,"교차로 그룹","IXR_GROP","NUMBER",3,null,null,"교차로군ID","PK","NOT NULL","ints_grop_id","NUMBER(5)","INTEGER","NUMBER(5)","교차로군ID",null,"CREATE TABLE ",{"$f":"H184&\" (\"","v":"soitdintsgrp ("},{"$f":"K186&\" \"","v":"ints_grop_id "},{"$f":"M186&\" \"","v":"INTEGER "},{"$f":"IF(J186=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(I186=\"PK\", I186=\"PK/FK\"), K186, \"\")","v":"ints_grop_id"},{"$f":"IF(OR(I186=\"PK\", I186=\"PK/FK\"), \",\", \"\")","v":","},"CREATE TABLE ",{"$f":"H184&\" (\"","v":"soitdintsgrp ("},{"$f":"K186&\" \"","v":"ints_grop_id "},{"$f":"N186&\" \"","v":"NUMBER(5) "},{"$f":"IF(J186=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(I186=\"PK\", I186=\"PK/FK\"), K186, \"\")","v":"ints_grop_id"},{"$f":"IF(OR(I186=\"PK\", I186=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$H$184&\".\"","v":"soitdintsgrp."},{"$f":"K186","v":"ints_grop_id"}," IS ",{"$f":"\"'\"&O186&\"'\"","v":"'교차로군ID'"},";",null,""]
[2,"수집 일시","CLCT_DT","INTEGER","UTC",null,null,"수집유닉스시각","PK","NOT NULL","clct_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)","수집유닉스시각",null,null,null,"clct_unix_tm ","INTEGER ","NOT NULL",",",null,"clct_unix_tm","));",null,null,"clct_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"clct_unix_tm",")","COMMENT ON COLUMN ","soitdintsgrp.","clct_unix_tm"," IS ","'수집유닉스시각'",";",null,""]
[2,"수집일","CLCT_DATE","VARHCAR2",8,"YYYYMMDD",null,"수집일시",null,"NOT NULL","clct_dt","VARCHAR2(8)","VARCHAR(8)","VARCHAR2(8)","수집일시(yyyyMMdd)",null,null,null,{"$f":"K188","v":"clct_dt"},"VARCHAR(8) ","NOT NULL",",",null,"",null,null,null,"clct_dt ","VARCHAR2(8) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitdintsgrp.","clct_dt"," IS ","'수집일시(yyyyMMdd)'",";"]
[3,"교차로 그룹 명","IXR_GROP_NM","VARCHAR2",50,null,null,"교차로군명",null,"NULL","ints_grop_nm","VARCHAR2(50)","VARCHAR(50)","VARCHAR2(50)","교차로군명",null,null,null,{"$f":"K189&\" \"","v":"ints_grop_nm "},"VARCHAR(50) ","",",",null,"",{"$f":"IF(OR(I189=\"PK\", I189=\"PK/FK\"), \",\", \"\")","v":""},null,null,"ints_grop_nm ","VARCHAR2(50) ","",",",null,null,"",{"$f":"IF(OR(I189=\"PK\", I189=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitdintsgrp.","ints_grop_nm"," IS ","'교차로군명'",";",null,{"$f":"IF(LEFT(AB189, 13) = \"CONSTRAINT PK\", AB189, \"\")","v":""}]
[4,"등록 유무","RGST_EN","NUMBER",1,"0:미등록 \n1:등록","등록여부(017)","등록구분코드",null,"NOT NULL","reg_se_cd","CHAR(3)","VARCHAR(3)","VARCHAR2(3)","등록여부(017)","등록구분코드 (0:미등록,1:등록)",null,null,"reg_se_cd ","VARCHAR(3) ","NOT NULL",",",null,"","",null,null,"reg_se_cd ","VARCHAR2(3) ","NOT NULL",{"$f":"\") TABLESPACE \"&AF192&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_D001 NOLOGGING"},null,null,{"$f":"IF(OR(C190=\"PK\", C190=\"PK/FK\"), E190, \"\")","v":""},null,"COMMENT ON COLUMN ","soitdintsgrp.","reg_se_cd"," IS ","'등록여부(017)'",";",null,""]
[{"$nulls":18},{"$f":"CONCATENATE(W186:Y187)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AF191:AH191)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (clct_unix_tm) INTERVAL (86400) STORE IN (\"&AF192&\") (PARTITION BFR_\" & H184 & \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AF192&\");\"","v":"PARTITION BY RANGE (clct_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_D001) (PARTITION BFR_soitdintsgrp_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_D001);"},{"$f":"\"CREATE INDEX PK_\" & H184& \" ON \" & H184 & CONCATENATE(AG186:AI189) & \" LOCAL (PARTITION BFR_\" & H184 & \"_20221101 TABLESPACE \"&AG192&\") TABLESPACE \"&AG192&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & H184 & \" ADD CONSTRAINT PK_\" & H184 & \" PRIMARY KEY \" & CONCATENATE(AG186:AI189) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$error":"#VALUE!"}]
[{"$nulls":31},"SOIT_D08_D001","SOIT_I08_D001",{"$nulls":9},""]
["- 특수일시각제어(SPCL_DD_HMS_CNTL)",{"$nulls":6},"soitdspdydayplan",{"$nulls":34},""]
["NO","속성명","컬럼명","형태","길이","비고",null,"논리명","PK/FK","NULL","물리명","형태","VOLT","TIBERO","COMMENT",{"$nulls":20},"COMMENT ON TABLE",{"$f":"H193&\" \"","v":"soitdspdydayplan "},null," IS ",{"$f":"\"'\"&A193&\"'\"","v":"'- 특수일시각제어(SPCL_DD_HMS_CNTL)'"},";",null,""]
[1,"신호 교차로 번호","SGNL_IXR_NMBR","NUMBER",4,null,null,"현장교차로ID","PK/FK","NOT NULL","spot_ints_id","NUMBER(5)","INTEGER","NUMBER(5)","현장교차로ID",null,"CREATE TABLE ",{"$f":"H193&\" (\"","v":"soitdspdydayplan ("},{"$f":"K195&\" \"","v":"spot_ints_id "},{"$f":"M195&\" \"","v":"INTEGER "},{"$f":"IF(J195=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(I195=\"PK\", I195=\"PK/FK\"), K195, \"\")","v":"spot_ints_id"},{"$f":"IF(OR(I195=\"PK\", I195=\"PK/FK\"), \",\", \"\")","v":","},"CREATE TABLE ",{"$f":"H193&\" (\"","v":"soitdspdydayplan ("},{"$f":"K195&\" \"","v":"spot_ints_id "},{"$f":"N195&\" \"","v":"NUMBER(5) "},{"$f":"IF(J195=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(I195=\"PK\", I195=\"PK/FK\"), K195, \"\")","v":"spot_ints_id"},{"$f":"IF(OR(I195=\"PK\", I195=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$H$193&\".\"","v":"soitdspdydayplan."},{"$f":"K195","v":"spot_ints_id"}," IS ",{"$f":"\"'\"&O195&\"'\"","v":"'현장교차로ID'"},";",null,""]
[2,"수집 일시","CLCT_DT","INTEGER","UTC",null,null,"수집유닉스시각","PK","NOT NULL","clct_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)","수집유닉스시각",null,null,null,"clct_unix_tm ","INTEGER ","NOT NULL",",",null,"clct_unix_tm",",",null,null,"clct_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"clct_unix_tm",",","COMMENT ON COLUMN ","soitdspdydayplan.","clct_unix_tm"," IS ","'수집유닉스시각'",";",null,""]
[2,"수집일","CLCT_DATE","VARHCAR2",8,"YYYYMMDD",null,"수집일시",null,"NOT NULL","clct_dt","VARCHAR2(8)","VARCHAR(8)","VARCHAR2(8)","수집일시(yyyyMMdd)",null,null,null,{"$f":"K197","v":"clct_dt"},"VARCHAR(8) ","NOT NULL",",",null,"",null,null,null,"clct_dt ","VARCHAR2(8) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitdspdydayplan.","clct_dt"," IS ","'수집일시(yyyyMMdd)'",";"]
[3,"특수 일 일련번호","SPCL_DD_SEQ","NUMBER",2,null,null,"특수일 일련번호","PK","NOT NULL","spdy_sn","NUMBER(2)","INTEGER","NUMBER(2)","특수일 일련번호",null,null,null,{"$f":"K198&\" \"","v":"spdy_sn "},"INTEGER ","NOT NULL",",",null,"spdy_sn","));",null,null,"spdy_sn ","NUMBER(2) ","NOT NULL",",",null,null,"spdy_sn",")","COMMENT ON COLUMN ","soitdspdydayplan.","spdy_sn"," IS ","'특수일 일련번호'",";",null,{"$f":"IF(LEFT(AB198, 13) = \"CONSTRAINT PK\", AB198, \"\")","v":""}]
[4,"특수 일 월","SPCL_DD_MN","NUMBER",2,null,null,"특수일 월",null,"NOT NULL","spdy_mm","NUMBER(2)","INTEGER","NUMBER(2)","특수일 월 (MM)",null,null,null,"spdy_mm ","INTEGER ","NOT NULL",",",null,"",{"$f":"IF(OR(I199=\"PK\", I199=\"PK/FK\"), \",\", \"\")","v":""},null,null,"spdy_mm ","NUMBER(2) ","NOT NULL",",",null,null,"",{"$f":"IF(OR(I199=\"PK\", I199=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitdspdydayplan.","spdy_mm"," IS ","'특수일 월 (MM)'",";",null,""]
[5,"특수 일 일","SPCL_DD_DD","NUMBER",2,null,null,"특수일 일",null,"NOT NULL","spdy_day","NUMBER(2)","INTEGER","NUMBER(2)","특수일 일 (dd)",null,null,null,"spdy_day ","INTEGER ","NOT NULL",",",null,"","",null,null,"spdy_day ","NUMBER(2) ","NOT NULL",",",null,null,"","","COMMENT ON COLUMN ","soitdspdydayplan.","spdy_day"," IS ","'특수일 일 (dd)'",";",null,""]
[6,"시각 계획 번호","HMS_PLAN_NMBR","NUMBER",2,"1~10",null,"시각계획번호",null,"NOT NULL","tm_plan_no","NUMBER(2)","INTEGER","NUMBER(2)","시각계획번호 (tod plan구분, 1~10)",null,null,null,"tm_plan_no ","INTEGER ","NOT NULL",",",null,"","",null,null,"tm_plan_no ","NUMBER(2) ","NOT NULL",",",null,null,"","","COMMENT ON COLUMN ","soitdspdydayplan.","tm_plan_no"," IS ","'시각계획번호 (tod plan구분, 1~10)'",";",null,""]
[7,"시간 계획 번호","HH_PLAN_NMBR","NUMBER",2,"1~10",null,"시간계획번호",null,"NOT NULL","hr_plan_no","NUMBER(2)","INTEGER","NUMBER(2)","시간계획번호 (1~10)",null,null,null,"hr_plan_no ","INTEGER ","NOT NULL",",",null,"","",null,null,"hr_plan_no ","NUMBER(2) ","NOT NULL",{"$f":"\") TABLESPACE \"&AF204&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_D001 NOLOGGING"},null,null,{"$f":"IF(OR(C202=\"PK\", C202=\"PK/FK\"), E202, \"\")","v":""},null,"COMMENT ON COLUMN ","soitdspdydayplan.","hr_plan_no"," IS ","'시간계획번호 (1~10)'",";",null,""]
[{"$nulls":18},{"$f":"CONCATENATE(W195:Y198)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AF203:AH203)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (clct_unix_tm) INTERVAL (86400) STORE IN (\"&AF204&\") (PARTITION BFR_\" & H193 & \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AF204&\");\"","v":"PARTITION BY RANGE (clct_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_D001) (PARTITION BFR_soitdspdydayplan_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_D001);"},{"$f":"\"CREATE INDEX PK_\" & H193& \" ON \" & H193 & CONCATENATE(AG195:AI201) & \" LOCAL (PARTITION BFR_\" & H193 & \"_20221101 TABLESPACE \"&AG204&\") TABLESPACE \"&AG204&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & H193 & \" ADD CONSTRAINT PK_\" & H193 & \" PRIMARY KEY \" & CONCATENATE(AG195:AI201) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$error":"#VALUE!"}]
[{"$nulls":31},"SOIT_D08_D001","SOIT_I08_D001"]
["- 주간시각제어(WEEK_HMS_CNTL)",{"$nulls":6},"soitdwklyplan",{"$nulls":34},{"$f":"IF(LEFT(AB205, 13) = \"CONSTRAINT PK\", AB205, \"\")","v":""}]
["NO","속성명","컬럼명","형태","길이","비고",null,"논리명","PK/FK","NULL","물리명","형태","VOLT","TIBERO","COMMENT",{"$nulls":20},"COMMENT ON TABLE",{"$f":"H205&\" \"","v":"soitdwklyplan "},null," IS ",{"$f":"\"'\"&A205&\"'\"","v":"'- 주간시각제어(WEEK_HMS_CNTL)'"},";",null,""]
[1,"신호 교차로 번호","SGNL_IXR_NMBR","NUMBER",4,null,null,"현장교차로ID","PK/FK","NOT NULL","spot_ints_id","NUMBER(5)","INTEGER","NUMBER(5)","교차로군ID",null,"CREATE TABLE ",{"$f":"H205&\" (\"","v":"soitdwklyplan ("},{"$f":"K207&\" \"","v":"spot_ints_id "},{"$f":"M207&\" \"","v":"INTEGER "},{"$f":"IF(J207=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(I207=\"PK\", I207=\"PK/FK\"), K207, \"\")","v":"spot_ints_id"},{"$f":"IF(OR(I207=\"PK\", I207=\"PK/FK\"), \",\", \"\")","v":","},"CREATE TABLE ",{"$f":"H205&\" (\"","v":"soitdwklyplan ("},{"$f":"K207&\" \"","v":"spot_ints_id "},{"$f":"N207&\" \"","v":"NUMBER(5) "},{"$f":"IF(J207=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(I207=\"PK\", I207=\"PK/FK\"), K207, \"\")","v":"spot_ints_id"},{"$f":"IF(OR(I207=\"PK\", I207=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$H$205&\".\"","v":"soitdwklyplan."},{"$f":"K207","v":"spot_ints_id"}," IS ",{"$f":"\"'\"&O207&\"'\"","v":"'교차로군ID'"},";",null,""]
[2,"수집 일시","CLCT_DT","INTEGER","UTC",null,null,"수집유닉스시각","PK","NOT NULL","clct_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)","수집유닉스시각",null,null,null,"clct_unix_tm ","INTEGER ","NOT NULL",",",null,"clct_unix_tm","));",null,null,"clct_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"clct_unix_tm",")","COMMENT ON COLUMN ","soitdwklyplan.","clct_unix_tm"," IS ","'수집유닉스시각'",";",null,""]
[2,"수집일","CLCT_DATE","VARHCAR2",8,"YYYYMMDD",null,"수집일시",null,"NOT NULL","clct_dt","VARCHAR2(8)","VARCHAR(8)","VARCHAR2(8)","수집일시(yyyyMMdd)",null,null,null,{"$f":"K209","v":"clct_dt"},"VARCHAR(8) ","NOT NULL",",",null,"",null,null,null,"clct_dt ","VARCHAR2(8) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitdwklyplan.","clct_dt"," IS ","'수집일시(yyyyMMdd)'",";"]
[3,"일요일 시각 계획","SUN_HMS_PLAN","NUMBER",2,"1~10","TOD_PLAN","일요일시각계획번호",null,"NULL","sun_tm_plan_no","NUMBER(2)","INTEGER","NUMBER(2)","일요일시각계획번호 (1~10)",null,null,null,{"$f":"K210&\" \"","v":"sun_tm_plan_no "},"INTEGER ","",",",null,"",{"$f":"IF(OR(I210=\"PK\", I210=\"PK/FK\"), \",\", \"\")","v":""},null,null,"sun_tm_plan_no ","NUMBER(2) ","",",",null,null,"",{"$f":"IF(OR(I210=\"PK\", I210=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitdwklyplan.","sun_tm_plan_no"," IS ","'일요일시각계획번호 (1~10)'",";",null,{"$f":"IF(LEFT(AB210, 13) = \"CONSTRAINT PK\", AB210, \"\")","v":""}]
[4,"월요일 시각 계획","MON_HMS_PLAN","NUMBER",2,"1~10",null,"월요일시각계획번호",null,"NULL","mon_tm_plan_no","NUMBER(2)","INTEGER","NUMBER(2)","월요일시각계획번호 (1~10)",null,null,null,"mon_tm_plan_no ","INTEGER ","",",",null,"","",null,null,"mon_tm_plan_no ","NUMBER(2) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdwklyplan.","mon_tm_plan_no"," IS ","'월요일시각계획번호 (1~10)'",";",null,""]
[5,"화요일 시각 계획","TUE_HMS_PLAN","NUMBER",2,"1~10",null,"화요일시각계획번호",null,"NULL","tue_tm_plan_no","NUMBER(2)","INTEGER","NUMBER(2)","화요일시각계획번호 (1~10)",null,null,null,"tue_tm_plan_no ","INTEGER ","",",",null,"","",null,null,"tue_tm_plan_no ","NUMBER(2) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdwklyplan.","tue_tm_plan_no"," IS ","'화요일시각계획번호 (1~10)'",";",null,""]
[6,"수요일 시각 계획","WED_HMS_PLAN","NUMBER",2,"1~10",null,"수요일시각계획번호",null,"NULL","wed_tm_plan_no","NUMBER(2)","INTEGER","NUMBER(2)","수요일시각계획번호 (1~10)",null,null,null,"wed_tm_plan_no ","INTEGER ","",",",null,"","",null,null,"wed_tm_plan_no ","NUMBER(2) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdwklyplan.","wed_tm_plan_no"," IS ","'수요일시각계획번호 (1~10)'",";",null,""]
[7,"목요일 시각 계획","THU_HMS_PLAN","NUMBER",2,"1~10",null,"목요일시각계획번호",null,"NULL","thu_tm_plan_no","NUMBER(2)","INTEGER","NUMBER(2)","목요일시각계획번호 (1~10)",null,null,null,"thu_tm_plan_no ","INTEGER ","",",",null,"","",null,null,"thu_tm_plan_no ","NUMBER(2) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdwklyplan.","thu_tm_plan_no"," IS ","'목요일시각계획번호 (1~10)'",";",null,""]
[8,"금요일 시각 계획","FRI_HMS_PLAN","NUMBER",2,"1~10",null,"금요일시각계획번호",null,"NULL","fri_tm_plan_no","NUMBER(2)","INTEGER","NUMBER(2)","금요일시각계획번호 (1~10)",null,null,null,"fri_tm_plan_no ","INTEGER ","",",",null,"","",null,null,"fri_tm_plan_no ","NUMBER(2) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdwklyplan.","fri_tm_plan_no"," IS ","'금요일시각계획번호 (1~10)'",";",null,""]
[9,"토요일 시각 계획","SAT_HMS_PLAN","NUMBER",2,"1~10",null,"토요일시각계획번호",null,"NULL","sat_tm_plan_no","NUMBER(2)","INTEGER","NUMBER(2)","토요일시각계획번호 (1~10)",null,null,null,"sat_tm_plan_no ","INTEGER ","",",",null,"","",null,null,"sat_tm_plan_no ","NUMBER(2) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdwklyplan.","sat_tm_plan_no"," IS ","'토요일시각계획번호 (1~10)'",";",null,""]
[10,"일요일 시간 계획","SUN_HH_PLAN","NUMBER",2,"1~10","TIME_PLAN","일요일시간계획번호",null,"NULL","sun_hr_plan_no","NUMBER(2)","INTEGER","NUMBER(2)","일요일시간계획번호 (1~10)",null,null,null,"sun_hr_plan_no ","INTEGER ","",",",null,"","",null,null,"sun_hr_plan_no ","NUMBER(2) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdwklyplan.","sun_hr_plan_no"," IS ","'일요일시간계획번호 (1~10)'",";",null,""]
[11,"월요일 시간 계획","MON_HH_PLAN","NUMBER",2,"1~10",null,"월요일시간계획번호",null,"NULL","mon_hr_plan_no","NUMBER(2)","INTEGER","NUMBER(2)","월요일시간계획번호 (1~10)",null,null,null,"mon_hr_plan_no ","INTEGER ","",",",null,"","",null,null,"mon_hr_plan_no ","NUMBER(2) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdwklyplan.","mon_hr_plan_no"," IS ","'월요일시간계획번호 (1~10)'",";",null,""]
[12,"화요일 시간 계획","TUE_HH_PLAN","NUMBER",2,"1~10",null,"화요일시간계획번호",null,"NULL","tue_hr_plan_no","NUMBER(2)","INTEGER","NUMBER(2)","화요일시간계획번호 (1~10)",null,null,null,"tue_hr_plan_no ","INTEGER ","",",",null,"","",null,null,"tue_hr_plan_no ","NUMBER(2) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdwklyplan.","tue_hr_plan_no"," IS ","'화요일시간계획번호 (1~10)'",";",null,""]
[13,"수요일 시간 계획","WED_HH_PLAN","NUMBER",2,"1~10",null,"수요일시간계획번호",null,"NULL","wed_hr_plan_no","NUMBER(2)","INTEGER","NUMBER(2)","수요일시간계획번호 (1~10)",null,null,null,"wed_hr_plan_no ","INTEGER ","",",",null,"","",null,null,"wed_hr_plan_no ","NUMBER(2) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdwklyplan.","wed_hr_plan_no"," IS ","'수요일시간계획번호 (1~10)'",";",null,""]
[14,"목요일 시간 계획","THU_HH_PLAN","NUMBER",2,"1~10",null,"목요일시간계획번호",null,"NULL","thu_hr_plan_no","NUMBER(2)","INTEGER","NUMBER(2)","목요일시간계획번호 (1~10)",null,null,null,"thu_hr_plan_no ","INTEGER ","",",",null,"","",null,null,"thu_hr_plan_no ","NUMBER(2) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdwklyplan.","thu_hr_plan_no"," IS ","'목요일시간계획번호 (1~10)'",";",null,""]
[15,"금요일 시간 계획","FRI_HH_PLAN","NUMBER",2,"1~10",null,"금요일시간계획번호",null,"NULL","fri_hr_plan_no","NUMBER(2)","INTEGER","NUMBER(2)","금요일시간계획번호 (1~10)",null,null,null,"fri_hr_plan_no ","INTEGER ","",",",null,"","",null,null,"fri_hr_plan_no ","NUMBER(2) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdwklyplan.","fri_hr_plan_no"," IS ","'금요일시간계획번호 (1~10)'",";",null,""]
[16,"토요일 시간 계획","SAT_HH_PLAN","NUMBER",2,"1~10",null,"토요일시간계획번호",null,"NULL","sat_hr_plan_no","NUMBER(2)","INTEGER","NUMBER(2)","토요일시간계획번호 (1~10)",null,null,null,"sat_hr_plan_no ","INTEGER ","",",",null,"","",null,null,"sat_hr_plan_no ","NUMBER(2) ","",{"$f":"\") TABLESPACE \"&AF225&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_D001 NOLOGGING"},null,null,{"$f":"IF(OR(C223=\"PK\", C223=\"PK/FK\"), E223, \"\")","v":""},null,"COMMENT ON COLUMN ","soitdwklyplan.","sat_hr_plan_no"," IS ","'토요일시간계획번호 (1~10)'",";",null,""]
[{"$nulls":18},{"$f":"CONCATENATE(W207:Y208)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AF224:AH224)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (clct_unix_tm) INTERVAL (86400) STORE IN (\"&AF225&\") (PARTITION BFR_\" & H205 & \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AF225&\");\"","v":"PARTITION BY RANGE (clct_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_D001) (PARTITION BFR_soitdwklyplan_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_D001);"},{"$f":"\"CREATE INDEX PK_\" & H205& \" ON \" & H205 & CONCATENATE(AG207:AI220) & \" LOCAL (PARTITION BFR_\" & H205 & \"_20221101 TABLESPACE \"&AG225&\") TABLESPACE \"&AG225&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & H205 & \" ADD CONSTRAINT PK_\" & H205 & \" PRIMARY KEY \" & CONCATENATE(AG207:AI214) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$error":"#VALUE!"}]
[{"$nulls":31},"SOIT_D08_D001","SOIT_I08_D001",{"$nulls":9},""]
["- 신호교차로상태(SGNL_IXR_STTS)",{"$nulls":6},"soitdspotintsstts",{"$nulls":34},""]
["NO","속성명","컬럼명","형태","길이","비고",null,"논리명","PK/FK","NULL","물리명","형태","VOLT","TIBERO","COMMENT",{"$nulls":20},"COMMENT ON TABLE",{"$f":"H226&\" \"","v":"soitdspotintsstts "},null," IS ",{"$f":"\"'\"&A226&\"'\"","v":"'- 신호교차로상태(SGNL_IXR_STTS)'"},";",null,""]
[1,"신호 교차로 번호","SGNL_IXR_NMBR","NUMBER",4,null,null,"현장교차로ID","PK/FK","NOT NULL","spot_ints_id","NUMBER(5)","INTEGER","NUMBER(5)","현장교차로ID",null,"CREATE TABLE ",{"$f":"H226&\" (\"","v":"soitdspotintsstts ("},{"$f":"K228&\" \"","v":"spot_ints_id "},{"$f":"M228&\" \"","v":"INTEGER "},{"$f":"IF(J228=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(I228=\"PK\", I228=\"PK/FK\"), K228, \"\")","v":"spot_ints_id"},{"$f":"IF(OR(I228=\"PK\", I228=\"PK/FK\"), \",\", \"\")","v":","},"CREATE TABLE ",{"$f":"H226&\" (\"","v":"soitdspotintsstts ("},{"$f":"K228&\" \"","v":"spot_ints_id "},{"$f":"N228&\" \"","v":"NUMBER(5) "},{"$f":"IF(J228=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(I228=\"PK\", I228=\"PK/FK\"), K228, \"\")","v":"spot_ints_id"},{"$f":"IF(OR(I228=\"PK\", I228=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$H$226&\".\"","v":"soitdspotintsstts."},{"$f":"K228","v":"spot_ints_id"}," IS ",{"$f":"\"'\"&O228&\"'\"","v":"'현장교차로ID'"},";",null,""]
[2,"수집 일시","CLCT_DT","INTEGER","UTC",null,null,"수집유닉스시각","PK","NOT NULL","clct_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)","수집유닉스시각",null,null,null,"clct_unix_tm ","INTEGER ","NOT NULL",",",null,"clct_unix_tm","));",null,null,"clct_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"clct_unix_tm",")","COMMENT ON COLUMN ","soitdspotintsstts.","clct_unix_tm"," IS ","'수집유닉스시각'",";",null,""]
[2,"수집일","CLCT_DATE","VARHCAR2",8,"YYYYMMDD",null,"수집일시",null,"NOT NULL","clct_dt","VARCHAR2(8)","VARCHAR(8)","VARCHAR2(8)","수집일시(yyyyMMdd)",null,null,null,{"$f":"K230","v":"clct_dt"},"VARCHAR(8) ","NOT NULL",",",null,"",null,null,null,"clct_dt ","VARCHAR2(8) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsstts.","clct_dt"," IS ","'수집일시(yyyyMMdd)'",";"]
[3,"LC 카운트","LC_CNT","NUMBER",3,"초",null,"LC수",null,"NOT NULL","lc_cnt","NUMBER(3)","INTEGER","NUMBER(3)","LC수",null,null,null,{"$f":"K231&\" \"","v":"lc_cnt "},"INTEGER ","NOT NULL",",",null,"",{"$f":"IF(OR(I231=\"PK\", I231=\"PK/FK\"), \",\", \"\")","v":""},null,null,"lc_cnt ","NUMBER(3) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsstts.","lc_cnt"," IS ","'LC수'",";",null,{"$f":"IF(LEFT(AB231, 13) = \"CONSTRAINT PK\", AB231, \"\")","v":""}]
[4,"제어 모드","CNTL_MODE","NUMBER",1,"0:TRC\n1:TOD\n2:MAN","제어구분코드(009)","제어구분코드",null,"NOT NULL","ctrl_se_cd","CHAR(3)","VARCHAR(3)","VARCHAR2(3)","제어구분코드(009)","제어구분코드 (0:TRC, 1:TOD, 2:MAN)",null,null,"ctrl_se_cd ","VARCHAR(3) ","NOT NULL",",",null,"","",null,null,"ctrl_se_cd ","VARCHAR2(3) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsstts.","ctrl_se_cd"," IS ","'제어구분코드(009)'",";",null,""]
[5,"제어 상태","CNTL_STTS","NUMBER",1,"0:오프라인\n1:온라인\n2:트랜스\n3:통신장애","제어상태코드(010)","제어상태코드",null,"NOT NULL","ctrl_stts_cd","CHAR(3)","VARCHAR(3)","VARCHAR2(3)","제어상태코드(010)","제어상태코드 (0:오프라인, 1:온라인, 2:트랜스, 3:통신장애)",null,null,"ctrl_stts_cd ","VARCHAR(3) ","NOT NULL",",",null,"","",null,null,"ctrl_stts_cd ","VARCHAR2(3) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsstts.","ctrl_stts_cd"," IS ","'제어상태코드(010)'",";",null,""]
[6,"특수 제어","SPCL_CNTL","NUMBER",2,"0:없음\n1:점멸\n2:소등\n3:수종\n4:감응","특수제어코드(802)","특수제어구분코드",null,"NOT NULL","spcn_ctrl_se_cd","CHAR(3)","VARCHAR(3)","VARCHAR2(3)","특수제어코드(802)","특수제어구분코드 (0:없음, 1:점멸, 2:소등, 3:수종, 4:감응)",null,null,"spcn_ctrl_se_cd ","VARCHAR(3) ","NOT NULL",",",null,"","",null,null,"spcn_ctrl_se_cd ","VARCHAR2(3) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsstts.","spcn_ctrl_se_cd"," IS ","'특수제어코드(802)'",";",null,""]
[7,"주기","CYCL","NUMBER",3,"초",null,"주기시간",null,"NOT NULL","cycl_hr","NUMBER(3)","INTEGER","NUMBER(3)","주기시간 (sec)",null,null,null,"cycl_hr ","INTEGER ","NOT NULL",",",null,"","",null,null,"cycl_hr ","NUMBER(3) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsstts.","cycl_hr"," IS ","'주기시간 (sec)'",";",null,""]
[8,"옵셋","OFST","NUMBER",3,"초",null,"옵셋시간",null,"NOT NULL","ofst_hr","NUMBER(3)","INTEGER","NUMBER(3)","옵셋시간 (sec)",null,null,null,"ofst_hr ","INTEGER ","NOT NULL",",",null,"","",null,null,"ofst_hr ","NUMBER(3) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsstts.","ofst_hr"," IS ","'옵셋시간 (sec)'",";",null,""]
[9,"A링 1현시","ARING_1PHAS","NUMBER",3,"초",null,"A링1현시시간",null,"NULL","A_ring_1_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링1현시시간 (sec)",null,null,null,"A_ring_1_phas_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_1_phas_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsstts.","A_ring_1_phas_hr"," IS ","'A링1현시시간 (sec)'",";",null,""]
[10,"A링 2현시","ARING_2PHAS","NUMBER",3,"초",null,"A링2현시시간",null,"NULL","A_ring_2_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링2현시시간 (sec)",null,null,null,"A_ring_2_phas_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_2_phas_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsstts.","A_ring_2_phas_hr"," IS ","'A링2현시시간 (sec)'",";",null,""]
[11,"A링 3현시","ARING_3PHAS","NUMBER",3,"초",null,"A링3현시시간",null,"NULL","A_ring_3_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링3현시시간 (sec)",null,null,null,"A_ring_3_phas_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_3_phas_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsstts.","A_ring_3_phas_hr"," IS ","'A링3현시시간 (sec)'",";",null,""]
[12,"A링 4현시","ARING_4PHAS","NUMBER",3,"초",null,"A링4현시시간",null,"NULL","A_ring_4_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링4현시시간 (sec)",null,null,null,"A_ring_4_phas_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_4_phas_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsstts.","A_ring_4_phas_hr"," IS ","'A링4현시시간 (sec)'",";",null,""]
[13,"A링 5현시","ARING_5PHAS","NUMBER",3,"초",null,"A링5현시시간",null,"NULL","A_ring_5_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링5현시시간 (sec)",null,null,null,"A_ring_5_phas_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_5_phas_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsstts.","A_ring_5_phas_hr"," IS ","'A링5현시시간 (sec)'",";",null,""]
[14,"A링 6현시","ARING_6PHAS","NUMBER",3,"초",null,"A링6현시시간",null,"NULL","A_ring_6_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링6현시시간 (sec)",null,null,null,"A_ring_6_phas_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_6_phas_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsstts.","A_ring_6_phas_hr"," IS ","'A링6현시시간 (sec)'",";",null,""]
[15,"A링 7현시","ARING_7PHAS","NUMBER",3,"초",null,"A링7현시시간",null,"NULL","A_ring_7_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링7현시시간 (sec)",null,null,null,"A_ring_7_phas_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_7_phas_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsstts.","A_ring_7_phas_hr"," IS ","'A링7현시시간 (sec)'",";",null,""]
[16,"A링 8현시","ARING_8PHAS","NUMBER",3,"초",null,"A링8현시시간",null,"NULL","A_ring_8_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링8현시시간 (sec)",null,null,null,"A_ring_8_phas_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_8_phas_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsstts.","A_ring_8_phas_hr"," IS ","'A링8현시시간 (sec)'",";",null,""]
[17,"B링 1현시","BRING_1PHAS","NUMBER",3,"초",null,"B링1현시시간",null,"NULL","B_ring_1_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링1현시시간 (sec)",null,null,null,"B_ring_1_phas_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_1_phas_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsstts.","B_ring_1_phas_hr"," IS ","'B링1현시시간 (sec)'",";",null,""]
[18,"B링 2현시","BRING_2PHAS","NUMBER",3,"초",null,"B링2현시시간",null,"NULL","B_ring_2_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링2현시시간 (sec)",null,null,null,"B_ring_2_phas_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_2_phas_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsstts.","B_ring_2_phas_hr"," IS ","'B링2현시시간 (sec)'",";",null,""]
[19,"B링 3현시","BRING_3PHAS","NUMBER",3,"초",null,"B링3현시시간",null,"NULL","B_ring_3_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링3현시시간 (sec)",null,null,null,"B_ring_3_phas_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_3_phas_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsstts.","B_ring_3_phas_hr"," IS ","'B링3현시시간 (sec)'",";",null,""]
[20,"B링 4현시","BRING_4PHAS","NUMBER",3,"초",null,"B링4현시시간",null,"NULL","B_ring_4_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링4현시시간 (sec)",null,null,null,"B_ring_4_phas_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_4_phas_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsstts.","B_ring_4_phas_hr"," IS ","'B링4현시시간 (sec)'",";",null,""]
[21,"B링 5현시","BRING_5PHAS","NUMBER",3,"초",null,"B링5현시시간",null,"NULL","B_ring_5_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링5현시시간 (sec)",null,null,null,"B_ring_5_phas_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_5_phas_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsstts.","B_ring_5_phas_hr"," IS ","'B링5현시시간 (sec)'",";",null,""]
[22,"B링 6현시","BRING_6PHAS","NUMBER",3,"초",null,"B링6현시시간",null,"NULL","B_ring_6_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링6현시시간 (sec)",null,null,null,"B_ring_6_phas_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_6_phas_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsstts.","B_ring_6_phas_hr"," IS ","'B링6현시시간 (sec)'",";",null,""]
[23,"B링 7현시","BRING_7PHAS","NUMBER",3,"초",null,"B링7현시시간",null,"NULL","B_ring_7_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링7현시시간 (sec)",null,null,null,"B_ring_7_phas_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_7_phas_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsstts.","B_ring_7_phas_hr"," IS ","'B링7현시시간 (sec)'",";",null,""]
[24,"B링 8현시","BRING_8PHAS","NUMBER",3,"초",null,"B링8현시시간",null,"NULL","B_ring_8_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링8현시시간 (sec)",null,null,null,"B_ring_8_phas_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_8_phas_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsstts.","B_ring_8_phas_hr"," IS ","'B링8현시시간 (sec)'",";",null,""]
[25,"현재 A링 현시","PRST_ARING_PHAS","NUMBER",1,"진행 현시번호",null,"현재A링현시번호",null,"NOT NULL","psnt_A_ring_phas_no","NUMBER(2)","INTEGER","NUMBER(2)","현재A링현시번호",null,null,null,"psnt_A_ring_phas_no ","INTEGER ","NOT NULL",",",null,"","",null,null,"psnt_A_ring_phas_no ","NUMBER(2) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsstts.","psnt_A_ring_phas_no"," IS ","'현재A링현시번호'",";",null,""]
[26,"현재 B링 현시","PRST_BRING_PHAS","NUMBER",1,"진행 현시번호",null,"현재B링현시번호",null,"NOT NULL","psnt_B_ring_phas_no","NUMBER(2)","INTEGER","NUMBER(2)","현재B링현시번호",null,null,null,"psnt_B_ring_phas_no ","INTEGER ","NOT NULL",",",null,"","",null,null,"psnt_B_ring_phas_no ","NUMBER(2) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsstts.","psnt_B_ring_phas_no"," IS ","'현재B링현시번호'",";",null,""]
[27,"현재 A링 스텝","PRST_ARING_STEP","NUMBER",2,"진행 스텝번호",null,"현재A링스탭번호",null,"NOT NULL","psnt_A_ring_step_no","NUMBER(2)","INTEGER","NUMBER(2)","현재A링스탭번호",null,null,null,"psnt_A_ring_step_no ","INTEGER ","NOT NULL",",",null,"","",null,null,"psnt_A_ring_step_no ","NUMBER(2) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsstts.","psnt_A_ring_step_no"," IS ","'현재A링스탭번호'",";",null,""]
[28,"현재 B링 스텝","PRST_BRING_STEP","NUMBER",2,"진행 스텝번호",null,"현재B링스탭번호",null,"NOT NULL","psnt_B_ring_step_no","NUMBER(2)","INTEGER","NUMBER(2)","현재B링스탭번호",null,null,null,"psnt_B_ring_step_no ","INTEGER ","NOT NULL",",",null,"","",null,null,"psnt_B_ring_step_no ","NUMBER(2) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsstts.","psnt_B_ring_step_no"," IS ","'현재B링스탭번호'",";",null,""]
[29,"맵 번호","MAP_NMBR","NUMBER",1,"0:일반\n1~5:시차","운영구분코드(801)","신호맵번호",null,"NOT NULL","sgnl_map_no","NUMBER(2)","INTEGER","NUMBER(2)","운영구분코드(801, 0:일반, 1~5:시차) ","0:일반\n1~5:시차",null,null,"sgnl_map_no ","INTEGER ","NOT NULL",",",null,"","",null,null,"sgnl_map_no ","NUMBER(2) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsstts.","sgnl_map_no"," IS ","'운영구분코드(801, 0:일반, 1~5:시차) '",";",null,""]
[30,"A링 이동류 번호","ARING_CRFL_NMBR","NUMBER",2,null,null,"A링이동류번호",null,"NOT NULL","A_ring_mvmt_no","NUMBER(2)","INTEGER","NUMBER(2)","A링이동류번호",null,null,null,"A_ring_mvmt_no ","INTEGER ","NOT NULL",",",null,"","",null,null,"A_ring_mvmt_no ","NUMBER(2) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsstts.","A_ring_mvmt_no"," IS ","'A링이동류번호'",";",null,""]
[31,"B링 이동류 번호","BRING_CRFL_NMBR","NUMBER",2,null,null,"B링이동류번호",null,"NOT NULL","B_ring_mvmt_no","NUMBER(2)","INTEGER","NUMBER(2)","B링이동류번호",null,null,null,"B_ring_mvmt_no ","INTEGER ","NOT NULL",",",null,"","",null,null,"B_ring_mvmt_no ","NUMBER(2) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsstts.","B_ring_mvmt_no"," IS ","'B링이동류번호'",";",null,""]
[32,"시각계획번호","HMS_PLAN_NMBR","NUMBER",2,"tod plan\n구분\n1~10",null,"시간계획번호",null,"NOT NULL","hr_plan_no","NUMBER(2)","INTEGER","NUMBER(2)","시각계획번호 (tod plan구분, 1~10)",null,null,null,"hr_plan_no ","INTEGER ","NOT NULL",",",null,"","",null,null,"hr_plan_no ","NUMBER(2) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsstts.","hr_plan_no"," IS ","'시각계획번호 (tod plan구분, 1~10)'",";",null,""]
[33,"시각운영번호","HMS_OPER_NMBR","NUMBER",2,"tod plan 번호\n1~16",null,"시각운영번호",null,"NOT NULL","tm_oper_no","NUMBER(2)","INTEGER","NUMBER(2)","시각운영번호 (tod plan 번호, 1~16)",null,null,null,"tm_oper_no ","INTEGER ","NOT NULL",",",null,"","",null,null,"tm_oper_no ","NUMBER(2) ","NOT NULL",{"$f":"\") TABLESPACE \"&AF263&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_D003 NOLOGGING"},null,null,{"$f":"IF(OR(C261=\"PK\", C261=\"PK/FK\"), E261, \"\")","v":""},null,"COMMENT ON COLUMN ","soitdspotintsstts.","tm_oper_no"," IS ","'시각운영번호 (tod plan 번호, 1~16)'",";",null,""]
[{"$nulls":18},{"$f":"CONCATENATE(W228:Y261)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AF262:AH262)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (clct_unix_tm) INTERVAL (3600) STORE IN (\"&AF263&\") (PARTITION BFR_\" & H226 & \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AF263&\");\"","v":"PARTITION BY RANGE (clct_unix_tm) INTERVAL (3600) STORE IN (SOIT_D08_D003) (PARTITION BFR_soitdspotintsstts_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_D003);"},{"$f":"\"CREATE INDEX PK_\" & H226& \" ON \" & H226 & CONCATENATE(AG228:AI234) & \" LOCAL (PARTITION BFR_\" & H226 & \"_20221101 TABLESPACE \"&AG263&\") TABLESPACE \"&AG263&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & H226 & \" ADD CONSTRAINT PK_\" & H226 & \" PRIMARY KEY \" & CONCATENATE(AG228:AI234) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$error":"#VALUE!"}]
[{"$nulls":31},"SOIT_D08_D003","SOIT_I08_D003"]
["- 신호교차로운영이력(SGNL_IXR_OPER_HS)",{"$nulls":6},"soitdspotintsoperhstr",{"$nulls":4},{"$f":"LEN(H264)","v":21},{"$nulls":29},{"$f":"IF(LEFT(AB264, 13) = \"CONSTRAINT PK\", AB264, \"\")","v":""}]
["NO","속성명","컬럼명","형태","길이","비고",null,"논리명","PK/FK","NULL","물리명","형태","VOLT","TIBERO","COMMENT",{"$nulls":20},"COMMENT ON TABLE",{"$f":"H264&\" \"","v":"soitdspotintsoperhstr "},null," IS ",{"$f":"\"'\"&A264&\"'\"","v":"'- 신호교차로운영이력(SGNL_IXR_OPER_HS)'"},";",null,""]
[1,"신호 교차로 번호","SGNL_IXR_NMBR","NUMBER",4,null,null,"현장교차로ID","PK/FK","NOT NULL","spot_ints_id","NUMBER(5)","INTEGER","NUMBER(5)","현장교차로ID",null,"CREATE TABLE ",{"$f":"H264&\" (\"","v":"soitdspotintsoperhstr ("},{"$f":"K266&\" \"","v":"spot_ints_id "},{"$f":"M266&\" \"","v":"INTEGER "},{"$f":"IF(J266=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(I266=\"PK\", I266=\"PK/FK\"), K266, \"\")","v":"spot_ints_id"},{"$f":"IF(OR(I266=\"PK\", I266=\"PK/FK\"), \",\", \"\")","v":","},"CREATE TABLE ",{"$f":"H264&\" (\"","v":"soitdspotintsoperhstr ("},{"$f":"K266&\" \"","v":"spot_ints_id "},{"$f":"N266&\" \"","v":"NUMBER(5) "},{"$f":"IF(J266=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(I266=\"PK\", I266=\"PK/FK\"), K266, \"\")","v":"spot_ints_id"},{"$f":"IF(OR(I266=\"PK\", I266=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$H$264&\".\"","v":"soitdspotintsoperhstr."},{"$f":"K266","v":"spot_ints_id"}," IS ",{"$f":"\"'\"&O266&\"'\"","v":"'현장교차로ID'"},";",null,""]
[2,"수집 일시","CLCT_DT","INTEGER","UTC",null,null,"수집유닉스시각","PK","NOT NULL","clct_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)","수집유닉스시각",null,null,null,"clct_unix_tm ","INTEGER ","NOT NULL",",",null,"clct_unix_tm","));",null,null,"clct_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"clct_unix_tm",")","COMMENT ON COLUMN ","soitdspotintsoperhstr.","clct_unix_tm"," IS ","'수집유닉스시각'",";",null,""]
[2,"수집일","CLCT_DATE","VARHCAR2",8,"YYYYMMDD",null,"수집일시",null,"NOT NULL","clct_dt","VARCHAR2(8)","VARCHAR(8)","VARCHAR2(8)","수집일시(yyyyMMdd)",null,null,null,{"$f":"K268","v":"clct_dt"},"VARCHAR(8) ","NOT NULL",",",null,"",null,null,null,"clct_dt ","VARCHAR2(8) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitdspotintsoperhstr.","clct_dt"," IS ","'수집일시(yyyyMMdd)'",";"]
[3,"제어 모드","CNTL_MODE","NUMBER",1,"0: 비감응 지역제어\n1: 감응 지역제어\n2: 감응 중앙제어\n3: 비감응 중앙제어","제어모드코드(803)","제어구분코드",null,"NOT NULL","ctrl_se_cd","CHAR(3)","VARCHAR(3)","VARCHAR2(3)","제어모드구분코드(803)","제어구분코드 (0: 비감응 지역제어, 1: 감응 지역제어, 2: 감응 중앙제어, 3: 비감응 중앙제어)",null,null,{"$f":"K269&\" \"","v":"ctrl_se_cd "},"VARCHAR(3) ","NOT NULL",",",null,"",{"$f":"IF(OR(I269=\"PK\", I269=\"PK/FK\"), \",\", \"\")","v":""},null,null,"ctrl_se_cd ","VARCHAR2(3) ","NOT NULL",",",null,null,"",{"$f":"IF(OR(I269=\"PK\", I269=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitdspotintsoperhstr.","ctrl_se_cd"," IS ","'제어모드구분코드(803)'",";",null,{"$f":"IF(LEFT(AB269, 13) = \"CONSTRAINT PK\", AB269, \"\")","v":""}]
[4,"제어 상태","CNTL_STTS","NUMBER",1,"0:오프라인\n1:온라인\n2:트랜스\n3:통신장애\n4:수동","제어상태코드(010)","제어상태코드",null,"NOT NULL","ctrl_stts_cd","CHAR(3)","VARCHAR(3)","VARCHAR2(3)","제어상태코드(010)","제어상태코드 (0:오프라인, 1:온라인, 2:트랜스, 3:통신장애, 4:수동)",null,null,"ctrl_stts_cd ","VARCHAR(3) ","NOT NULL",",",null,"","",null,null,"ctrl_stts_cd ","VARCHAR2(3) ","NOT NULL",",",null,null,"","","COMMENT ON COLUMN ","soitdspotintsoperhstr.","ctrl_stts_cd"," IS ","'제어상태코드(010)'",";",null,""]
[5," ","CYCL","NUMBER",3,"초",null,"주기시간",null,"NOT NULL","cycl_hr","NUMBER(3)","INTEGER","NUMBER(3)","주기시간 (sec)",null,null,null,"cycl_hr ","INTEGER ","NOT NULL",",",null,"","",null,null,"cycl_hr ","NUMBER(3) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsoperhstr.","cycl_hr"," IS ","'주기시간 (sec)'",";",null,""]
[6,"옵셋","OFST","NUMBER",3,"초",null,"옵셋시간",null,"NOT NULL","ofst_hr","NUMBER(3)","INTEGER","NUMBER(3)","옵셋시간 (sec)",null,null,null,"ofst_hr ","INTEGER ","NOT NULL",",",null,"","",null,null,"ofst_hr ","NUMBER(3) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsoperhstr.","ofst_hr"," IS ","'옵셋시간 (sec)'",";",null,""]
[7,"A링 1현시","ARING_1PHAS","NUMBER",3,"초",null,"A링1현시시간",null,"NULL","A_ring_1_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링1현시시간 (sec)",null,null,null,"A_ring_1_phas_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_1_phas_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsoperhstr.","A_ring_1_phas_hr"," IS ","'A링1현시시간 (sec)'",";",null,""]
[8,"A링 2현시","ARING_2PHAS","NUMBER",3,"초",null,"A링2현시시간",null,"NULL","A_ring_2_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링2현시시간 (sec)",null,null,null,"A_ring_2_phas_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_2_phas_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsoperhstr.","A_ring_2_phas_hr"," IS ","'A링2현시시간 (sec)'",";",null,""]
[9,"A링 3현시","ARING_3PHAS","NUMBER",3,"초",null,"A링3현시시간",null,"NULL","A_ring_3_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링3현시시간 (sec)",null,null,null,"A_ring_3_phas_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_3_phas_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsoperhstr.","A_ring_3_phas_hr"," IS ","'A링3현시시간 (sec)'",";",null,""]
[10,"A링 4현시","ARING_4PHAS","NUMBER",3,"초",null,"A링4현시시간",null,"NULL","A_ring_4_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링4현시시간 (sec)",null,null,null,"A_ring_4_phas_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_4_phas_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsoperhstr.","A_ring_4_phas_hr"," IS ","'A링4현시시간 (sec)'",";",null,""]
[11,"A링 5현시","ARING_5PHAS","NUMBER",3,"초",null,"A링5현시시간",null,"NULL","A_ring_5_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링5현시시간 (sec)",null,null,null,"A_ring_5_phas_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_5_phas_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsoperhstr.","A_ring_5_phas_hr"," IS ","'A링5현시시간 (sec)'",";",null,""]
[12,"A링 6현시","ARING_6PHAS","NUMBER",3,"초",null,"A링6현시시간",null,"NULL","A_ring_6_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링6현시시간 (sec)",null,null,null,"A_ring_6_phas_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_6_phas_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsoperhstr.","A_ring_6_phas_hr"," IS ","'A링6현시시간 (sec)'",";",null,""]
[13,"A링 7현시","ARING_7PHAS","NUMBER",3,"초",null,"A링7현시시간",null,"NULL","A_ring_7_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링7현시시간 (sec)",null,null,null,"A_ring_7_phas_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_7_phas_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsoperhstr.","A_ring_7_phas_hr"," IS ","'A링7현시시간 (sec)'",";",null,""]
[14,"A링 8현시","ARING_8PHAS","NUMBER",3,"초",null,"A링8현시시간",null,"NULL","A_ring_8_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링8현시시간 (sec)",null,null,null,"A_ring_8_phas_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_8_phas_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsoperhstr.","A_ring_8_phas_hr"," IS ","'A링8현시시간 (sec)'",";",null,""]
[15,"B링 1현시","BRING_1PHAS","NUMBER",3,"초",null,"B링1현시시간",null,"NULL","B_ring_1_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링1현시시간 (sec)",null,null,null,"B_ring_1_phas_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_1_phas_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsoperhstr.","B_ring_1_phas_hr"," IS ","'B링1현시시간 (sec)'",";",null,""]
[16,"B링 2현시","BRING_2PHAS","NUMBER",3,"초",null,"B링2현시시간",null,"NULL","B_ring_2_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링2현시시간 (sec)",null,null,null,"B_ring_2_phas_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_2_phas_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsoperhstr.","B_ring_2_phas_hr"," IS ","'B링2현시시간 (sec)'",";",null,""]
[17,"B링 3현시","BRING_3PHAS","NUMBER",3,"초",null,"B링3현시시간",null,"NULL","B_ring_3_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링3현시시간 (sec)",null,null,null,"B_ring_3_phas_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_3_phas_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsoperhstr.","B_ring_3_phas_hr"," IS ","'B링3현시시간 (sec)'",";",null,""]
[18,"B링 4현시","BRING_4PHAS","NUMBER",3,"초",null,"B링4현시시간",null,"NULL","B_ring_4_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링4현시시간 (sec)",null,null,null,"B_ring_4_phas_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_4_phas_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsoperhstr.","B_ring_4_phas_hr"," IS ","'B링4현시시간 (sec)'",";",null,""]
[19,"B링 5현시","BRING_5PHAS","NUMBER",3,"초",null,"B링5현시시간",null,"NULL","B_ring_5_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링5현시시간 (sec)",null,null,null,"B_ring_5_phas_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_5_phas_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsoperhstr.","B_ring_5_phas_hr"," IS ","'B링5현시시간 (sec)'",";",null,""]
[20,"B링 6현시","BRING_6PHAS","NUMBER",3,"초",null,"B링6현시시간",null,"NULL","B_ring_6_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링6현시시간 (sec)",null,null,null,"B_ring_6_phas_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_6_phas_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsoperhstr.","B_ring_6_phas_hr"," IS ","'B링6현시시간 (sec)'",";",null,""]
[21,"B링 7현시","BRING_7PHAS","NUMBER",3,"초",null,"B링7현시시간",null,"NULL","B_ring_7_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링7현시시간 (sec)",null,null,null,"B_ring_7_phas_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_7_phas_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsoperhstr.","B_ring_7_phas_hr"," IS ","'B링7현시시간 (sec)'",";",null,""]
[22,"B링 8현시","BRING_8PHAS","NUMBER",3,"초",null,"B링8현시시간",null,"NULL","B_ring_8_phas_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링8현시시간 (sec)",null,null,null,"B_ring_8_phas_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_8_phas_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsoperhstr.","B_ring_8_phas_hr"," IS ","'B링8현시시간 (sec)'",";",null,""]
[23,"A링 1현시 보행","ARING_1PHAS_WALK","NUMBER",3,"2010년",null,"A링1현시보행시간",null,"NULL","A_ring_1_phas_ambl_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링1현시보행시간 (sec)",null,null,null,"A_ring_1_phas_ambl_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_1_phas_ambl_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsoperhstr.","A_ring_1_phas_ambl_hr"," IS ","'A링1현시보행시간 (sec)'",";",null,""]
[24,"A링 2현시 보행","ARING_2PHAS_WALK","NUMBER",3,"2010년",null,"A링2현시보행시간",null,"NULL","A_ring_2_phas_ambl_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링2현시보행시간 (sec)",null,null,null,"A_ring_2_phas_ambl_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_2_phas_ambl_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsoperhstr.","A_ring_2_phas_ambl_hr"," IS ","'A링2현시보행시간 (sec)'",";",null,""]
[25,"A링 3현시 보행","ARING_3PHAS_WALK","NUMBER",3,"2010년",null,"A링3현시보행시간",null,"NULL","A_ring_3_phas_ambl_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링3현시보행시간 (sec)",null,null,null,"A_ring_3_phas_ambl_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_3_phas_ambl_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsoperhstr.","A_ring_3_phas_ambl_hr"," IS ","'A링3현시보행시간 (sec)'",";",null,""]
[26,"A링 4현시 보행","ARING_4PHAS_WALK","NUMBER",3,"2010년",null,"A링4현시보행시간",null,"NULL","A_ring_4_phas_ambl_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링4현시보행시간 (sec)",null,null,null,"A_ring_4_phas_ambl_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_4_phas_ambl_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsoperhstr.","A_ring_4_phas_ambl_hr"," IS ","'A링4현시보행시간 (sec)'",";",null,""]
[27,"A링 5현시 보행","ARING_5PHAS_WALK","NUMBER",3,"2010년",null,"A링5현시보행시간",null,"NULL","A_ring_5_phas_ambl_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링5현시보행시간 (sec)",null,null,null,"A_ring_5_phas_ambl_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_5_phas_ambl_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsoperhstr.","A_ring_5_phas_ambl_hr"," IS ","'A링5현시보행시간 (sec)'",";",null,""]
[28,"A링 6현시 보행","ARING_6PHAS_WALK","NUMBER",3,"2010년",null,"A링6현시보행시간",null,"NULL","A_ring_6_phas_ambl_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링6현시보행시간 (sec)",null,null,null,"A_ring_6_phas_ambl_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_6_phas_ambl_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsoperhstr.","A_ring_6_phas_ambl_hr"," IS ","'A링6현시보행시간 (sec)'",";",null,""]
[29,"A링 7현시 보행","ARING_7PHAS_WALK","NUMBER",3,"2010년",null,"A링7현시보행시간",null,"NULL","A_ring_7_phas_ambl_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링7현시보행시간 (sec)",null,null,null,"A_ring_7_phas_ambl_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_7_phas_ambl_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsoperhstr.","A_ring_7_phas_ambl_hr"," IS ","'A링7현시보행시간 (sec)'",";",null,""]
[30,"A링 8현시 보행","ARING_8PHAS_WALK","NUMBER",3,"2010년",null,"A링8현시보행시간",null,"NULL","A_ring_8_phas_ambl_hr","NUMBER(3)","INTEGER","NUMBER(3)","A링8현시보행시간 (sec)",null,null,null,"A_ring_8_phas_ambl_hr ","INTEGER ","",",",null,"","",null,null,"A_ring_8_phas_ambl_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsoperhstr.","A_ring_8_phas_ambl_hr"," IS ","'A링8현시보행시간 (sec)'",";",null,""]
[31,"B링 1현시 보행","BRING_1PHAS_WALK","NUMBER",3,"2010년",null,"B링1현시보행시간",null,"NULL","B_ring_1_phas_ambl_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링1현시보행시간 (sec)",null,null,null,"B_ring_1_phas_ambl_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_1_phas_ambl_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsoperhstr.","B_ring_1_phas_ambl_hr"," IS ","'B링1현시보행시간 (sec)'",";",null,""]
[32,"B링 2현시 보행","BRING_2PHAS_WALK","NUMBER",3,"2010년",null,"B링2현시보행시간",null,"NULL","B_ring_2_phas_ambl_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링2현시보행시간 (sec)",null,null,null,"B_ring_2_phas_ambl_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_2_phas_ambl_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsoperhstr.","B_ring_2_phas_ambl_hr"," IS ","'B링2현시보행시간 (sec)'",";",null,""]
[33,"B링 3현시 보행","BRING_3PHAS_WALK","NUMBER",3,"2010년",null,"B링3현시보행시간",null,"NULL","B_ring_3_phas_ambl_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링3현시보행시간 (sec)",null,null,null,"B_ring_3_phas_ambl_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_3_phas_ambl_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsoperhstr.","B_ring_3_phas_ambl_hr"," IS ","'B링3현시보행시간 (sec)'",";",null,""]
[34,"B링 4현시 보행","BRING_4PHAS_WALK","NUMBER",3,"2010년",null,"B링4현시보행시간",null,"NULL","B_ring_4_phas_ambl_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링4현시보행시간 (sec)",null,null,null,"B_ring_4_phas_ambl_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_4_phas_ambl_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsoperhstr.","B_ring_4_phas_ambl_hr"," IS ","'B링4현시보행시간 (sec)'",";",null,""]
[35,"B링 5현시 보행","BRING_5PHAS_WALK","NUMBER",3,"2010년",null,"B링5현시보행시간",null,"NULL","B_ring_5_phas_ambl_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링5현시보행시간 (sec)",null,null,null,"B_ring_5_phas_ambl_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_5_phas_ambl_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsoperhstr.","B_ring_5_phas_ambl_hr"," IS ","'B링5현시보행시간 (sec)'",";",null,""]
[36,"B링 6현시 보행","BRING_6PHAS_WALK","NUMBER",3,"2010년",null,"B링6현시보행시간",null,"NULL","B_ring_6_phas_ambl_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링6현시보행시간 (sec)",null,null,null,"B_ring_6_phas_ambl_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_6_phas_ambl_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsoperhstr.","B_ring_6_phas_ambl_hr"," IS ","'B링6현시보행시간 (sec)'",";",null,""]
[37,"B링 7현시 보행","BRING_7PHAS_WALK","NUMBER",3,"2010년",null,"B링7현시보행시간",null,"NULL","B_ring_7_phas_ambl_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링7현시보행시간 (sec)",null,null,null,"B_ring_7_phas_ambl_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_7_phas_ambl_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdspotintsoperhstr.","B_ring_7_phas_ambl_hr"," IS ","'B링7현시보행시간 (sec)'",";",null,""]
[38,"B링 8현시 보행","BRING_8PHAS_WALK","NUMBER",3,"2010년",null,"B링8현시보행시간",null,"NULL","B_ring_8_phas_ambl_hr","NUMBER(3)","INTEGER","NUMBER(3)","B링8현시보행시간 (sec)",null,null,null,"B_ring_8_phas_ambl_hr ","INTEGER ","",",",null,"","",null,null,"B_ring_8_phas_ambl_hr ","NUMBER(3) ","",{"$f":"\") TABLESPACE \"&AF306&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_D003 NOLOGGING"},null,null,{"$f":"IF(OR(C304=\"PK\", C304=\"PK/FK\"), E304, \"\")","v":""},null,"COMMENT ON COLUMN ","soitdspotintsoperhstr.","B_ring_8_phas_ambl_hr"," IS ","'B링8현시보행시간 (sec)'",";",null,""]
[{"$nulls":18},{"$f":"CONCATENATE(W266:Y304)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AF305:AH305)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (clct_unix_tm) INTERVAL (3600) STORE IN (\"&AF306&\") (PARTITION BFR_\" & H264 & \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AF306&\");\"","v":"PARTITION BY RANGE (clct_unix_tm) INTERVAL (3600) STORE IN (SOIT_D08_D003) (PARTITION BFR_soitdspotintsoperhstr_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_D003);"},{"$f":"\"CREATE INDEX PK_\" & H264& \" ON \" & H264 & CONCATENATE(AG266:AI273) & \" LOCAL (PARTITION BFR_\" & H264 & \"_20221101 TABLESPACE \"&AG306&\") TABLESPACE \"&AG306&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & H264 & \" ADD CONSTRAINT PK_\" & H264 & \" PRIMARY KEY \" & CONCATENATE(AG266:AI274) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$error":"#VALUE!"}]
[{"$nulls":31},"SOIT_D08_D003","SOIT_I08_D003"]
["- 소속교차로관리(PSTN_IXR_MNGM)",{"$nulls":6},"soitdintsgrpinfo",{"$nulls":4},{"$f":"LEN(H307)","v":16},{"$nulls":29},{"$f":"IF(LEFT(AB307, 13) = \"CONSTRAINT PK\", AB307, \"\")","v":""}]
["NO","속성명","컬럼명","형태","길이","비고",null,"논리명","PK/FK","NULL","물리명","형태","VOLT","TIBERO","COMMENT",{"$nulls":20},"COMMENT ON TABLE",{"$f":"H307&\" \"","v":"soitdintsgrpinfo "},null," IS ",{"$f":"\"'\"&A307&\"'\"","v":"'- 소속교차로관리(PSTN_IXR_MNGM)'"},";",null,""]
[1,"교차로 그룹","IXR_GROP","NUMBER",3,null,null,"교차로군ID","PK/FK","NOT NULL","ints_grop_id","NUMBER(5)","INTEGER","NUMBER(5)","교차로군ID",null,"CREATE TABLE ",{"$f":"H307&\" (\"","v":"soitdintsgrpinfo ("},{"$f":"K309&\" \"","v":"ints_grop_id "},{"$f":"M309&\" \"","v":"INTEGER "},{"$f":"IF(J309=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(I309=\"PK\", I309=\"PK/FK\"), K309, \"\")","v":"ints_grop_id"},{"$f":"IF(OR(I309=\"PK\", I309=\"PK/FK\"), \",\", \"\")","v":","},"CREATE TABLE ",{"$f":"H307&\" (\"","v":"soitdintsgrpinfo ("},{"$f":"K309&\" \"","v":"ints_grop_id "},{"$f":"N309&\" \"","v":"NUMBER(5) "},{"$f":"IF(J309=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(I309=\"PK\", I309=\"PK/FK\"), K309, \"\")","v":"ints_grop_id"},{"$f":"IF(OR(I309=\"PK\", I309=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$H$307&\".\"","v":"soitdintsgrpinfo."},{"$f":"K309","v":"ints_grop_id"}," IS ",{"$f":"\"'\"&O309&\"'\"","v":"'교차로군ID'"},";",null,""]
[2,"수집 일시","CLCT_DT","INTEGER","UTC",null,null,"수집유닉스시각","PK","NOT NULL","clct_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)","수집유닉스시각",null,null,null,"clct_unix_tm ","INTEGER ","NOT NULL",",",null,"clct_unix_tm",",",null,null,"clct_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"clct_unix_tm",",","COMMENT ON COLUMN ","soitdintsgrpinfo.","clct_unix_tm"," IS ","'수집유닉스시각'",";",null,""]
[2,"수집일","CLCT_DATE","VARHCAR2",8,"YYYYMMDD",null,"수집일시",null,"NOT NULL","clct_dt","VARCHAR2(8)","VARCHAR(8)","VARCHAR2(8)","수집일시(yyyyMMdd)",null,null,null,{"$f":"K311","v":"clct_dt"},"VARCHAR(8) ","NOT NULL",",",null,"",null,null,null,"clct_dt ","VARCHAR2(8) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitdintsgrpinfo.","clct_dt"," IS ","'수집일시(yyyyMMdd)'",";"]
[3,"일련번호","SEQ","NUMBER",2,"1~20",null,"그룹일련번호","PK","NOT NULL","grup_sn","NUMBER(2)","INTEGER","NUMBER(2)","그룹일련번호",null,null,null,{"$f":"K312&\" \"","v":"grup_sn "},"INTEGER ","NOT NULL",",",null,"grup_sn","));",null,null,"grup_sn ","NUMBER(2) ","NOT NULL",",",null,null,"grup_sn",")","COMMENT ON COLUMN ","soitdintsgrpinfo.","grup_sn"," IS ","'그룹일련번호'",";",null,{"$f":"IF(LEFT(AB312, 13) = \"CONSTRAINT PK\", AB312, \"\")","v":""}]
[4,"소속 교차로 번호","PSTN_IXR_NMBR","NUMBER",4,null,null,"현장교차로ID","FK","NULL","spot_ints_id","NUMBER(5)","INTEGER","NUMBER(5)","소속 현장교차로ID",null,null,null,"spot_ints_id ","INTEGER ","",",",null,"",{"$f":"IF(OR(I313=\"PK\", I313=\"PK/FK\"), \",\", \"\")","v":""},null,null,"spot_ints_id ","NUMBER(5) ","",{"$f":"\") TABLESPACE \"&AF315&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_D001 NOLOGGING"},null,null,{"$f":"IF(OR(C313=\"PK\", C313=\"PK/FK\"), E313, \"\")","v":""},null,"COMMENT ON COLUMN ","soitdintsgrpinfo.","spot_ints_id"," IS ","'소속 현장교차로ID'",";",null,""]
[{"$nulls":18},{"$f":"CONCATENATE(W309:Y313)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AF314:AH314)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (clct_unix_tm) INTERVAL (86400) STORE IN (\"&AF315&\") (PARTITION BFR_\" & H307 & \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AF315&\");\"","v":"PARTITION BY RANGE (clct_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_D001) (PARTITION BFR_soitdintsgrpinfo_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_D001);"},{"$f":"\"CREATE INDEX PK_\" & H307& \" ON \" & H307 & CONCATENATE(AG309:AI312) & \" LOCAL (PARTITION BFR_\" & H307 & \"_20221101 TABLESPACE \"&AG315&\") TABLESPACE \"&AG315&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & H307 & \" ADD CONSTRAINT PK_\" & H307 & \" PRIMARY KEY \" & CONCATENATE(AG309:AI312) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$error":"#VALUE!"}]
[{"$nulls":31},"SOIT_D08_D001","SOIT_I08_D001"]
["- 교차로예약(IXR_APNT)",{"$nulls":6},"soitdphasrevt",{"$nulls":4},{"$f":"LEN(H316)","v":13},{"$nulls":29},{"$f":"IF(LEFT(AB316, 13) = \"CONSTRAINT PK\", AB316, \"\")","v":""}]
["NO","속성명","컬럼명","형태","길이","비고",null,"논리명","PK/FK","NULL","물리명","형태","VOLT","TIBERO","COMMENT",{"$nulls":20},"COMMENT ON TABLE",{"$f":"H316&\" \"","v":"soitdphasrevt "},null," IS ",{"$f":"\"'\"&A316&\"'\"","v":"'- 교차로예약(IXR_APNT)'"},";",null,""]
[1,"신호 교차로 번호","SGNL_IXR_NMBR","NUMBER",4,null,null,"현장교차로ID","PK/FK","NOT NULL","spot_ints_id","NUMBER(5)","INTEGER","NUMBER(5)","현장교차로ID",null,"CREATE TABLE ",{"$f":"H316&\" (\"","v":"soitdphasrevt ("},{"$f":"K318&\" \"","v":"spot_ints_id "},{"$f":"M318&\" \"","v":"INTEGER "},{"$f":"IF(J318=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(I318=\"PK\", I318=\"PK/FK\"), K318, \"\")","v":"spot_ints_id"},{"$f":"IF(OR(I318=\"PK\", I318=\"PK/FK\"), \",\", \"\")","v":","},"CREATE TABLE ",{"$f":"H316&\" (\"","v":"soitdphasrevt ("},{"$f":"K318&\" \"","v":"spot_ints_id "},{"$f":"N318&\" \"","v":"NUMBER(5) "},{"$f":"IF(J318=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(I318=\"PK\", I318=\"PK/FK\"), K318, \"\")","v":"spot_ints_id"},{"$f":"IF(OR(I318=\"PK\", I318=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$H$316&\".\"","v":"soitdphasrevt."},{"$f":"K318","v":"spot_ints_id"}," IS ",{"$f":"\"'\"&O318&\"'\"","v":"'현장교차로ID'"},";",null,""]
[2,"수집 일시","CLCT_DATE","INTEGER","UTC",null,null,"수집유닉스시각","PK","NOT NULL","clct_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)","수집유닉스시각",null,null,null,"clct_unix_tm ","INTEGER ","NOT NULL",",",null,"clct_unix_tm",",",null,null,"clct_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"clct_unix_tm",",","COMMENT ON COLUMN ","soitdphasrevt.","clct_unix_tm"," IS ","'수집유닉스시각'",";",null,""]
[2,"수집일",null,"VARHCAR2",8,"YYYYMMDD",null,"수집일시",null,"NOT NULL","clct_dt","VARCHAR2(8)","VARCHAR(8)","VARCHAR2(8)","수집일시(yyyyMMdd)",null,null,null,{"$f":"K320","v":"clct_dt"},"VARCHAR(8) ","NOT NULL",",",null,"",null,null,null,"clct_dt ","VARCHAR2(8) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitdphasrevt.","clct_dt"," IS ","'수집일시(yyyyMMdd)'",";"]
[3,"교차로 예약 계획 번호","IXR_APNT_PLAN_NMBR","NUMBER",2,null,null,"예약계획번호","PK","NOT NULL","rsvt_plan_no","NUMBER(2)","INTEGER","NUMBER(2)","예약계획번호",null,null,null,{"$f":"K321&\" \"","v":"rsvt_plan_no "},"INTEGER ","NOT NULL",",",null,"rsvt_plan_no","));",null,null,"rsvt_plan_no ","NUMBER(2) ","NOT NULL",",",null,null,"rsvt_plan_no",")","COMMENT ON COLUMN ","soitdphasrevt.","rsvt_plan_no"," IS ","'예약계획번호'",";",null,{"$f":"IF(LEFT(AB321, 13) = \"CONSTRAINT PK\", AB321, \"\")","v":""}]
[4,"수행 여부","ACTV_YN","NUMBER",1,"0:수행하지않음\n1:수행 ->Y/N변경요청필요","수행여부(019)","예약수행여부",null,"NOT NULL","rsvt_flfmt_yn","CHAR(1)","VARCHAR(1)","VARCHAR2(1)","예약수행여부(019)","예약수행여부 (Y/N)",null,null,"rsvt_flfmt_yn ","VARCHAR(1) ","NOT NULL",",",null,"",{"$f":"IF(OR(I322=\"PK\", I322=\"PK/FK\"), \",\", \"\")","v":""},null,null,"rsvt_flfmt_yn ","VARCHAR2(1) ","NOT NULL",",",null,null,"",{"$f":"IF(OR(I322=\"PK\", I322=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitdphasrevt.","rsvt_flfmt_yn"," IS ","'예약수행여부(019)'",";",null,""]
[5,"월","MN","NUMBER",2,null,null,"예약설정월",null,"NOT NULL","rsvt_stng_mm","NUMBER(2)","INTEGER","NUMBER(2)","예약설정월",null,null,null,"rsvt_stng_mm ","INTEGER ","NOT NULL",",",null,"","",null,null,"rsvt_stng_mm ","NUMBER(2) ","NOT NULL",",",null,null,"","","COMMENT ON COLUMN ","soitdphasrevt.","rsvt_stng_mm"," IS ","'예약설정월'",";",null,""]
[6,"일","DD","NUMBER",2,null,null,"예약설정일",null,"NOT NULL","rsvt_stng_day","NUMBER(2)","INTEGER","NUMBER(2)","예약설정일",null,null,null,"rsvt_stng_day ","INTEGER ","NOT NULL",",",null,"","",null,null,"rsvt_stng_day ","NUMBER(2) ","NOT NULL",",",null,null,"","","COMMENT ON COLUMN ","soitdphasrevt.","rsvt_stng_day"," IS ","'예약설정일'",";",null,""]
[7,"요일","DAY","NUMBER",2,"요일코드참조",null,"예약설정요일코드",null,"NOT NULL","rsvt_stng_dotw_cd","CHAR(3)","VARCHAR(3)","VARCHAR2(3)","예약설정요일코드 (0:없음, 1:일, 2:월, 3:화, 4:수, 5:목, 6: 금, 7:토, 8:평일, 9:토+일) (0:없음, 1:일, 2:월, 3:화, 4:수, 5:목, 6: 금, 7:토, 8:공휴일, 9:평일, 10:토+일, 11:격주토1)",null,null,null,"rsvt_stng_dotw_cd ","VARCHAR(3) ","NOT NULL",",",null,"","",null,null,"rsvt_stng_dotw_cd ","VARCHAR2(3) ","NOT NULL",",",null,null,"","","COMMENT ON COLUMN ","soitdphasrevt.","rsvt_stng_dotw_cd"," IS ","'예약설정요일코드 (0:없음, 1:일, 2:월, 3:화, 4:수, 5:목, 6: 금, 7:토, 8:평일, 9:토+일) (0:없음, 1:일, 2:월, 3:화, 4:수, 5:목, 6: 금, 7:토, 8:공휴일, 9:평일, 10:토+일, 11:격주토1)'",";",null,""]
[8,"시작 시간","STRT_HH","NUMBER",2,null,null,"예약설정시",null,"NOT NULL","rsvt_stng_hh","NUMBER(2)","INTEGER","NUMBER(2)","예약설정시",null,null,null,"rsvt_stng_hh ","INTEGER ","NOT NULL",",",null,"","",null,null,"rsvt_stng_hh ","NUMBER(2) ","NOT NULL",",",null,null,"","","COMMENT ON COLUMN ","soitdphasrevt.","rsvt_stng_hh"," IS ","'예약설정시'",";",null,""]
[9,"시작 분","STRT_MM","NUMBER",2,null,null,"예약설정분",null,"NOT NULL","rsvt_stng_mi","NUMBER(2)","INTEGER","NUMBER(2)","예약설정분",null,null,null,"rsvt_stng_mi ","INTEGER ","NOT NULL",",",null,"","",null,null,"rsvt_stng_mi ","NUMBER(2) ","NOT NULL",",",null,null,"","","COMMENT ON COLUMN ","soitdphasrevt.","rsvt_stng_mi"," IS ","'예약설정분'",";",null,""]
[10,"종료 시간","END_HH","NUMBER",2,null,null,"예약종료시",null,"NOT NULL","rsvt_end_hh","NUMBER(2)","INTEGER","NUMBER(2)","예약종료시",null,null,null,"rsvt_end_hh ","INTEGER ","NOT NULL",",",null,"","",null,null,"rsvt_end_hh ","NUMBER(2) ","NOT NULL",",",null,null,"","","COMMENT ON COLUMN ","soitdphasrevt.","rsvt_end_hh"," IS ","'예약종료시'",";",null,""]
[11,"종료 분","END_MM","NUMBER",2,null,null,"예약종료분",null,"NOT NULL","rsvt_end_mi","NUMBER(2)","INTEGER","NUMBER(2)","예약종료분",null,null,null,"rsvt_end_mi ","INTEGER ","NOT NULL",",",null,"","",null,null,"rsvt_end_mi ","NUMBER(2) ","NOT NULL",",",null,null,"","","COMMENT ON COLUMN ","soitdphasrevt.","rsvt_end_mi"," IS ","'예약종료분'",";",null,""]
[12,"예약 명령","APNT_CMND","NUMBER",2,"0: 없음\n1: 조광제어\n2: 점멸제어\n3: 소등제어\n4: 시차제어\n5: 감응제어\n6:보행자버튼활성","예약명령코드(804)","예약명령구분코드",null,"NOT NULL","rsvt_cmd_se_cd","CHAR(3)","VARCHAR(3)","VARCHAR2(3)","예약명령구분코드(804)","예약명령구분코드 (0: 없음, 1: 조광제어, 2: 점멸제어, 3: 소등제어, 4: 시차제어, 5: 감응제어, 6:보행자버튼활성)",null,null,"rsvt_cmd_se_cd ","VARCHAR(3) ","NOT NULL",",",null,"","",null,null,"rsvt_cmd_se_cd ","VARCHAR2(3) ","NOT NULL",{"$f":"\") TABLESPACE \"&AF332&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_D001 NOLOGGING"},null,null,{"$f":"IF(OR(C330=\"PK\", C330=\"PK/FK\"), E330, \"\")","v":""},null,"COMMENT ON COLUMN ","soitdphasrevt.","rsvt_cmd_se_cd"," IS ","'예약명령구분코드(804)'",";",null,""]
[{"$nulls":18},{"$f":"CONCATENATE(W318:Y330)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AF331:AH331)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (clct_unix_tm) INTERVAL (86400) STORE IN (\"&AF332&\") (PARTITION BFR_\" & H316 & \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AF332&\");\"","v":"PARTITION BY RANGE (clct_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_D001) (PARTITION BFR_soitdphasrevt_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_D001);"},{"$f":"\"CREATE INDEX PK_\" & H316& \" ON \" & H316 & CONCATENATE(AG318:AI329) & \" LOCAL (PARTITION BFR_\" & H316 & \"_20221101 TABLESPACE \"&AG332&\") TABLESPACE \"&AG332&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & H316 & \" ADD CONSTRAINT PK_\" & H316 & \" PRIMARY KEY \" & CONCATENATE(AG318:AI327) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$error":"#VALUE!"}]
["요일 코드",{"$nulls":30},"SOIT_D08_D001","SOIT_I08_D001",{"$nulls":9},""]
["- 2004년 규격",{"$nulls":41},""]
["0 : 없음, 1:일, 2:월, 3:화, 4:수, 5:목, 6: 금, 7:토, 8:평일, 9:토+일",{"$nulls":41},""]
["- 2010년 규격",{"$nulls":41},""]
["0 : 없음, 1:일, 2:월, 3:화, 4:수, 5:목, 6: 금, 7:토, 8:공휴일, 9:평일, 10:토+일, 11:격주토1",{"$nulls":41},""]
[{"$nulls":42},""]
[{"$nulls":42},""]
[{"$nulls":42},""]
["- 신호제어기(SGNL_CTLR)",{"$nulls":6},"soitdsgnlctrr",{"$nulls":4},{"$f":"LEN(H340)","v":13},{"$nulls":29},""]
["NO","속성명","컬럼명","형태","길이","비고",null,"논리명","PK/FK","NULL","물리명","형태","VOLT","TIBERO","COMMENT",{"$nulls":20},"COMMENT ON TABLE",{"$f":"H340&\" \"","v":"soitdsgnlctrr "},null," IS ",{"$f":"\"'\"&A340&\"'\"","v":"'- 신호제어기(SGNL_CTLR)'"},";",null,""]
[1,"신호 교차로 번호","SGNL_IXR_NMBR","NUMBER",4,null,null,"현장교차로ID","PK/FK","NOT NULL","spot_ints_id","NUMBER(5)","INTEGER","NUMBER(5)","현장교차로ID",null,"CREATE TABLE ",{"$f":"H340&\" (\"","v":"soitdsgnlctrr ("},{"$f":"K342&\" \"","v":"spot_ints_id "},{"$f":"M342&\" \"","v":"INTEGER "},{"$f":"IF(J342=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(I342=\"PK\", I342=\"PK/FK\"), K342, \"\")","v":"spot_ints_id"},{"$f":"IF(OR(I342=\"PK\", I342=\"PK/FK\"), \",\", \"\")","v":","},"CREATE TABLE ",{"$f":"H340&\" (\"","v":"soitdsgnlctrr ("},{"$f":"K342&\" \"","v":"spot_ints_id "},{"$f":"N342&\" \"","v":"NUMBER(5) "},{"$f":"IF(J342=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(I342=\"PK\", I342=\"PK/FK\"), K342, \"\")","v":"spot_ints_id"},{"$f":"IF(OR(I342=\"PK\", I342=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$H$340&\".\"","v":"soitdsgnlctrr."},{"$f":"K342","v":"spot_ints_id"}," IS ",{"$f":"\"'\"&O342&\"'\"","v":"'현장교차로ID'"},";",null,""]
[2,"수집 일시","CLCT_DT","INTEGER","UTC",null,null,"수집유닉스시각","PK","NOT NULL","clct_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)","수집유닉스시각",null,null,null,"clct_unix_tm ","INTEGER ","NOT NULL",",",null,"clct_unix_tm","));",null,null,"clct_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"clct_unix_tm",")","COMMENT ON COLUMN ","soitdsgnlctrr.","clct_unix_tm"," IS ","'수집유닉스시각'",";",null,""]
[2,"수집일","CLCT_DATE","VARHCAR2",8,"YYYYMMDD",null,"수집일시",null,"NOT NULL","clct_dt","VARCHAR2(8)","VARCHAR(8)","VARCHAR2(8)","수집일시(yyyyMMdd)",null,null,null,{"$f":"K344","v":"clct_dt"},"VARCHAR(8) ","NOT NULL",",",null,"",null,null,null,"clct_dt ","VARCHAR2(8) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitdsgnlctrr.","clct_dt"," IS ","'수집일시(yyyyMMdd)'",";"]
[2,"X 좌표","X_CRDN","NUMBER",10,null,null,"제어기경도",null,"NULL","ctrr_lot","NUMBER(13,10)","FLOAT","NUMBER(13,10)","제어기경도",null,null,null,{"$f":"K345&\" \"","v":"ctrr_lot "},"FLOAT ","",",",null,"",{"$f":"IF(OR(I345=\"PK\", I345=\"PK/FK\"), \",\", \"\")","v":""},null,null,"ctrr_lot ","NUMBER(13,10) ","",",",null,null,"",{"$f":"IF(OR(I345=\"PK\", I345=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitdsgnlctrr.","ctrr_lot"," IS ","'제어기경도'",";",null,{"$f":"IF(LEFT(AB345, 13) = \"CONSTRAINT PK\", AB345, \"\")","v":""}]
[3,"Y 좌표","Y_CRDN","NUMBER",10,null,null,"제어기위도",null,"NULL","ctrr_lat","NUMBER(12,10)","FLOAT","NUMBER(12,10)","제어기위도",null,null,null,"ctrr_lat ","FLOAT ","",",",null,"","",null,null,"ctrr_lat ","NUMBER(12,10) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdsgnlctrr.","ctrr_lat"," IS ","'제어기위도'",";",null,""]
[4,"A링 1현시 코드","ARING_1PHAS_CD","NUMBER",7,"현시코드\n참조",null,"A링1현시코드",null,"NULL","A_ring_1_phas_cd","CHAR(7)","VARCHAR(7)","VARCHAR2(7)","A링1현시코드 (구분자(1:직,좌, 2:보행)+진입방위각(3)+진출방위각(3))",null,null,null,"A_ring_1_phas_cd ","VARCHAR(7) ","",",",null,"","",null,null,"A_ring_1_phas_cd ","VARCHAR2(7) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdsgnlctrr.","A_ring_1_phas_cd"," IS ","'A링1현시코드 (구분자(1:직,좌, 2:보행)+진입방위각(3)+진출방위각(3))'",";",null,""]
[5,"A링 2현시 코드","ARING_2PHAS_CD","NUMBER",7,null,null,"A링2현시코드",null,"NULL","A_ring_2_phas_cd","CHAR(7)","VARCHAR(7)","VARCHAR2(7)","A링2현시코드 (구분자(1:직,좌, 2:보행)+진입방위각(3)+진출방위각(3))",null,null,null,"A_ring_2_phas_cd ","VARCHAR(7) ","",",",null,"","",null,null,"A_ring_2_phas_cd ","VARCHAR2(7) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdsgnlctrr.","A_ring_2_phas_cd"," IS ","'A링2현시코드 (구분자(1:직,좌, 2:보행)+진입방위각(3)+진출방위각(3))'",";",null,""]
[6,"A링 3현시 코드","ARING_3PHAS_CD","NUMBER",7,null,null,"A링3현시코드",null,"NULL","A_ring_3_phas_cd","CHAR(7)","VARCHAR(7)","VARCHAR2(7)","A링3현시코드 (구분자(1:직,좌, 2:보행)+진입방위각(3)+진출방위각(3))",null,null,null,"A_ring_3_phas_cd ","VARCHAR(7) ","",",",null,"","",null,null,"A_ring_3_phas_cd ","VARCHAR2(7) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdsgnlctrr.","A_ring_3_phas_cd"," IS ","'A링3현시코드 (구분자(1:직,좌, 2:보행)+진입방위각(3)+진출방위각(3))'",";",null,""]
[7,"A링 4현시 코드","ARING_4PHAS_CD","NUMBER",7,null,null,"A링4현시코드",null,"NULL","A_ring_4_phas_cd","CHAR(7)","VARCHAR(7)","VARCHAR2(7)","A링4현시코드 (구분자(1:직,좌, 2:보행)+진입방위각(3)+진출방위각(3))",null,null,null,"A_ring_4_phas_cd ","VARCHAR(7) ","",",",null,"","",null,null,"A_ring_4_phas_cd ","VARCHAR2(7) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdsgnlctrr.","A_ring_4_phas_cd"," IS ","'A링4현시코드 (구분자(1:직,좌, 2:보행)+진입방위각(3)+진출방위각(3))'",";",null,""]
[8,"A링 5현시 코드","ARING_5PHAS_CD","NUMBER",7,null,null,"A링5현시코드",null,"NULL","A_ring_5_phas_cd","CHAR(7)","VARCHAR(7)","VARCHAR2(7)","A링5현시코드 (구분자(1:직,좌, 2:보행)+진입방위각(3)+진출방위각(3))",null,null,null,"A_ring_5_phas_cd ","VARCHAR(7) ","",",",null,"","",null,null,"A_ring_5_phas_cd ","VARCHAR2(7) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdsgnlctrr.","A_ring_5_phas_cd"," IS ","'A링5현시코드 (구분자(1:직,좌, 2:보행)+진입방위각(3)+진출방위각(3))'",";",null,""]
[9,"A링 6현시 코드","ARING_6PHAS_CD","NUMBER",7,null,null,"A링6현시코드",null,"NULL","A_ring_6_phas_cd","CHAR(7)","VARCHAR(7)","VARCHAR2(7)","A링6현시코드 (구분자(1:직,좌, 2:보행)+진입방위각(3)+진출방위각(3))",null,null,null,"A_ring_6_phas_cd ","VARCHAR(7) ","",",",null,"","",null,null,"A_ring_6_phas_cd ","VARCHAR2(7) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdsgnlctrr.","A_ring_6_phas_cd"," IS ","'A링6현시코드 (구분자(1:직,좌, 2:보행)+진입방위각(3)+진출방위각(3))'",";",null,""]
[10,"A링 7현시 코드","ARING_7PHAS_CD","NUMBER",7,null,null,"A링7현시코드",null,"NULL","A_ring_7_phas_cd","CHAR(7)","VARCHAR(7)","VARCHAR2(7)","A링7현시코드 (구분자(1:직,좌, 2:보행)+진입방위각(3)+진출방위각(3))",null,null,null,"A_ring_7_phas_cd ","VARCHAR(7) ","",",",null,"","",null,null,"A_ring_7_phas_cd ","VARCHAR2(7) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdsgnlctrr.","A_ring_7_phas_cd"," IS ","'A링7현시코드 (구분자(1:직,좌, 2:보행)+진입방위각(3)+진출방위각(3))'",";",null,""]
[11,"A링 8현시 코드","ARING_8PHAS_CD","NUMBER",7,null,null,"A링8현시코드",null,"NULL","A_ring_8_phas_cd","CHAR(7)","VARCHAR(7)","VARCHAR2(7)","A링8현시코드 (구분자(1:직,좌, 2:보행)+진입방위각(3)+진출방위각(3))",null,null,null,"A_ring_8_phas_cd ","VARCHAR(7) ","",",",null,"","",null,null,"A_ring_8_phas_cd ","VARCHAR2(7) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdsgnlctrr.","A_ring_8_phas_cd"," IS ","'A링8현시코드 (구분자(1:직,좌, 2:보행)+진입방위각(3)+진출방위각(3))'",";",null,""]
[12,"B링 1현시 코드","BRING_1PHAS_CD","NUMBER",7,null,null,"B링1현시코드",null,"NULL","B_ring_1_phas_cd","CHAR(7)","VARCHAR(7)","VARCHAR2(7)","B링1현시코드 (구분자(1:직,좌, 2:보행)+진입방위각(3)+진출방위각(3))",null,null,null,"B_ring_1_phas_cd ","VARCHAR(7) ","",",",null,"","",null,null,"B_ring_1_phas_cd ","VARCHAR2(7) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdsgnlctrr.","B_ring_1_phas_cd"," IS ","'B링1현시코드 (구분자(1:직,좌, 2:보행)+진입방위각(3)+진출방위각(3))'",";",null,""]
[13,"B링 2현시 코드","BRING_2PHAS_CD","NUMBER",7,null,null,"B링2현시코드",null,"NULL","B_ring_2_phas_cd","CHAR(7)","VARCHAR(7)","VARCHAR2(7)","B링2현시코드 (구분자(1:직,좌, 2:보행)+진입방위각(3)+진출방위각(3))",null,null,null,"B_ring_2_phas_cd ","VARCHAR(7) ","",",",null,"","",null,null,"B_ring_2_phas_cd ","VARCHAR2(7) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdsgnlctrr.","B_ring_2_phas_cd"," IS ","'B링2현시코드 (구분자(1:직,좌, 2:보행)+진입방위각(3)+진출방위각(3))'",";",null,""]
[14,"B링 3현시 코드","BRING_3PHAS_CD","NUMBER",7,null,null,"B링3현시코드",null,"NULL","B_ring_3_phas_cd","CHAR(7)","VARCHAR(7)","VARCHAR2(7)","B링3현시코드 (구분자(1:직,좌, 2:보행)+진입방위각(3)+진출방위각(3))",null,null,null,"B_ring_3_phas_cd ","VARCHAR(7) ","",",",null,"","",null,null,"B_ring_3_phas_cd ","VARCHAR2(7) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdsgnlctrr.","B_ring_3_phas_cd"," IS ","'B링3현시코드 (구분자(1:직,좌, 2:보행)+진입방위각(3)+진출방위각(3))'",";",null,""]
[15,"B링 4현시 코드","BRING_4PHAS_CD","NUMBER",7,null,null,"B링4현시코드",null,"NULL","B_ring_4_phas_cd","CHAR(7)","VARCHAR(7)","VARCHAR2(7)","B링4현시코드 (구분자(1:직,좌, 2:보행)+진입방위각(3)+진출방위각(3))",null,null,null,"B_ring_4_phas_cd ","VARCHAR(7) ","",",",null,"","",null,null,"B_ring_4_phas_cd ","VARCHAR2(7) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdsgnlctrr.","B_ring_4_phas_cd"," IS ","'B링4현시코드 (구분자(1:직,좌, 2:보행)+진입방위각(3)+진출방위각(3))'",";",null,""]
[16,"B링 5현시 코드","BRING_5PHAS_CD","NUMBER",7,null,null,"B링5현시코드",null,"NULL","B_ring_5_phas_cd","CHAR(7)","VARCHAR(7)","VARCHAR2(7)","B링5현시코드 (구분자(1:직,좌, 2:보행)+진입방위각(3)+진출방위각(3))",null,null,null,"B_ring_5_phas_cd ","VARCHAR(7) ","",",",null,"","",null,null,"B_ring_5_phas_cd ","VARCHAR2(7) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdsgnlctrr.","B_ring_5_phas_cd"," IS ","'B링5현시코드 (구분자(1:직,좌, 2:보행)+진입방위각(3)+진출방위각(3))'",";",null,""]
[17,"B링 6현시 코드","BRING_6PHAS_CD","NUMBER",7,null,null,"B링6현시코드",null,"NULL","B_ring_6_phas_cd","CHAR(7)","VARCHAR(7)","VARCHAR2(7)","B링6현시코드 (구분자(1:직,좌, 2:보행)+진입방위각(3)+진출방위각(3))",null,null,null,"B_ring_6_phas_cd ","VARCHAR(7) ","",",",null,"","",null,null,"B_ring_6_phas_cd ","VARCHAR2(7) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdsgnlctrr.","B_ring_6_phas_cd"," IS ","'B링6현시코드 (구분자(1:직,좌, 2:보행)+진입방위각(3)+진출방위각(3))'",";",null,""]
[18,"B링 7현시 코드","BRING_7PHAS_CD","NUMBER",7,null,null,"B링7현시코드",null,"NULL","B_ring_7_phas_cd","CHAR(7)","VARCHAR(7)","VARCHAR2(7)","B링7현시코드 (구분자(1:직,좌, 2:보행)+진입방위각(3)+진출방위각(3))",null,null,null,"B_ring_7_phas_cd ","VARCHAR(7) ","",",",null,"","",null,null,"B_ring_7_phas_cd ","VARCHAR2(7) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdsgnlctrr.","B_ring_7_phas_cd"," IS ","'B링7현시코드 (구분자(1:직,좌, 2:보행)+진입방위각(3)+진출방위각(3))'",";",null,""]
[19,"B링 8현시 코드","BRING_8PHAS_CD","NUMBER",7,null,null,"B링8현시코드",null,"NULL","B_ring_8_phas_cd","CHAR(7)","VARCHAR(7)","VARCHAR2(7)","B링8현시코드 (구분자(1:직,좌, 2:보행)+진입방위각(3)+진출방위각(3))",null,null,null,"B_ring_8_phas_cd ","VARCHAR(7) ","",",",null,"","",null,null,"B_ring_8_phas_cd ","VARCHAR2(7) ","",{"$f":"\") TABLESPACE \"&AF364&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_D001 NOLOGGING"},null,null,{"$f":"IF(OR(C362=\"PK\", C362=\"PK/FK\"), E362, \"\")","v":""},null,"COMMENT ON COLUMN ","soitdsgnlctrr.","B_ring_8_phas_cd"," IS ","'B링8현시코드 (구분자(1:직,좌, 2:보행)+진입방위각(3)+진출방위각(3))'",";",null,""]
[{"$nulls":18},{"$f":"CONCATENATE(W342:Y362)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AF363:AH363)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (clct_unix_tm) INTERVAL (86400) STORE IN (\"&AF364&\") (PARTITION BFR_\" & H340 & \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AF364&\");\"","v":"PARTITION BY RANGE (clct_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_D001) (PARTITION BFR_soitdsgnlctrr_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_D001);"},{"$f":"\"CREATE INDEX PK_\" & H340& \" ON \" & H340 & CONCATENATE(AG342:AI350) & \" LOCAL (PARTITION BFR_\" & H340 & \"_20221101 TABLESPACE \"&AG364&\") TABLESPACE \"&AG364&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & H340 & \" ADD CONSTRAINT PK_\" & H340 & \" PRIMARY KEY \" & CONCATENATE(AG342:AI355) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$error":"#VALUE!"}]
[{"$nulls":31},"SOIT_D08_D001","SOIT_I08_D001"]
["- 신호 운영 맵3 (SGNL_OPER_MAP3)",{"$nulls":6},"soitdopermap3",{"$nulls":4},{"$f":"LEN(H365)","v":13},{"$nulls":29},{"$f":"IF(LEFT(AB365, 13) = \"CONSTRAINT PK\", AB365, \"\")","v":""}]
["NO","속성명","컬럼명","형태","길이","비고",null,"논리명","PK/FK","NULL","물리명","형태","VOLT","TIBERO","COMMENT",{"$nulls":20},"COMMENT ON TABLE",{"$f":"H365&\" \"","v":"soitdopermap3 "},null," IS ",{"$f":"\"'\"&A365&\"'\"","v":"'- 신호 운영 맵3 (SGNL_OPER_MAP3)'"},";",null,""]
[1,"신호 교차로 번호","SGNL_IXR_NMBR","NUMBER",4,null,null,"현장교차로ID","PK/FK","NOT NULL","spot_ints_id","NUMBER(5)","INTEGER","NUMBER(5)","현장교차로ID",null,"CREATE TABLE ",{"$f":"H365&\" (\"","v":"soitdopermap3 ("},{"$f":"K367&\" \"","v":"spot_ints_id "},{"$f":"M367&\" \"","v":"INTEGER "},{"$f":"IF(J367=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(I367=\"PK\", I367=\"PK/FK\"), K367, \"\")","v":"spot_ints_id"},{"$f":"IF(OR(I367=\"PK\", I367=\"PK/FK\"), \",\", \"\")","v":","},"CREATE TABLE ",{"$f":"H365&\" (\"","v":"soitdopermap3 ("},{"$f":"K367&\" \"","v":"spot_ints_id "},{"$f":"N367&\" \"","v":"NUMBER(5) "},{"$f":"IF(J367=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(I367=\"PK\", I367=\"PK/FK\"), K367, \"\")","v":"spot_ints_id"},{"$f":"IF(OR(I367=\"PK\", I367=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$H$365&\".\"","v":"soitdopermap3."},{"$f":"K367","v":"spot_ints_id"}," IS ",{"$f":"\"'\"&O367&\"'\"","v":"'현장교차로ID'"},";",null,""]
[2,"수집 일시","CLCT_DT","INTEGER","UTC",null,null,"수집유닉스시각","PK","NOT NULL","clct_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)","수집유닉스시각",null,null,null,"clct_unix_tm ","INTEGER ","NOT NULL",",",null,"clct_unix_tm",",",null,null,"clct_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"clct_unix_tm",",","COMMENT ON COLUMN ","soitdopermap3.","clct_unix_tm"," IS ","'수집유닉스시각'",";",null,""]
[2,"수집일","CLCT_DATE","VARHCAR2",8,"YYYYMMDD",null,"수집일시",null,"NOT NULL","clct_dt","VARCHAR2(8)","VARCHAR(8)","VARCHAR2(8)","수집일시(yyyyMMdd)",null,null,null,{"$f":"K369","v":"clct_dt"},"VARCHAR(8) ","NOT NULL",",",null,"",null,null,null,"clct_dt ","VARCHAR2(8) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitdopermap3.","clct_dt"," IS ","'수집일시(yyyyMMdd)'",";"]
[3,"교차로 운영 모드","IXR_OPER_MODE","NUMBER",1,"0:일반 , 1:시차1, 2: 시차2, 3:시차3, 4:시차4, 5:시차5, 6:보행맵","운영구분코드(801)","운영구분코드","PK","NOT NULL","oper_se_cd","CHAR(3)","VARCHAR(3)","VARCHAR2(3)","운영구분코드(801)","운영구분코드 (0:일반 , 1:시차1, 2: 시차2, 3:시차3, 4:시차4, 5:시차5, 6:보행맵)",null,null,{"$f":"K370&\" \"","v":"oper_se_cd "},"VARCHAR(3) ","NOT NULL",",",null,"oper_se_cd",{"$f":"IF(OR(I370=\"PK\", I370=\"PK/FK\"), \",\", \"\")","v":","},null,null,"oper_se_cd ","VARCHAR2(3) ","NOT NULL",",",null,null,"oper_se_cd",{"$f":"IF(OR(I370=\"PK\", I370=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ","soitdopermap3.","oper_se_cd"," IS ","'운영구분코드(801)'",";",null,{"$f":"IF(LEFT(AB370, 13) = \"CONSTRAINT PK\", AB370, \"\")","v":""}]
[4,"링 구분","RING_DVSN","NUMBER",1,"0 :A링\n1 :B링","링구분코드(007)","링구분코드","PK","NOT NULL","ring_se_cd","CHAR(1)","VARCHAR(1)","VARCHAR2(1)","링구분코드(007)","링구분코드 (0:A링, 1:B링)",null,null,"ring_se_cd ","VARCHAR(1) ","NOT NULL",",",null,"ring_se_cd",",",null,null,"ring_se_cd ","VARCHAR2(1) ","NOT NULL",",",null,null,"ring_se_cd",",","COMMENT ON COLUMN ","soitdopermap3.","ring_se_cd"," IS ","'링구분코드(007)'",";",null,""]
[5,"스텝 번호","STEP_NMBR","NUMBER",2,"1~32",null,"스탭번호","PK","NOT NULL","step_no","NUMBER(2)","INTEGER","NUMBER(2)","스탭번호 (1~32)",null,null,null,"step_no ","INTEGER ","NOT NULL",",",null,"step_no","));",null,null,"step_no ","NUMBER(2) ","NOT NULL",",",null,null,"step_no",")","COMMENT ON COLUMN ","soitdopermap3.","step_no"," IS ","'스탭번호 (1~32)'",";",null,""]
[6,"LSU1 코드 값","LSU1_CD_VAL","NUMBER",3,"신호운영맵 코드 값의 16진수를 10진수로 변경하여 저장\n0x01 -> 1\n0x02 -> 2\n0x03 -> 3\n0x04 -> 4\n0x05 -> 5\n0x06 -> 6\n0x07 -> 7\n0x08 -> 8\n0x09 -> 9\n0x10 -> 16\n0x20 -> 32\n0x30 -> 48\n0x40 -> 64\n0x50 -> 80\n0x80 -> 128",null,"LSU1코드값",null,"NULL","lsu_1_cd_valu","NUMBER(3)","INTEGER","NUMBER(3)","LSU1코드값 (신호운영맵 코드 값의 10진수변환값)",null,null,null,"lsu_1_cd_valu ","INTEGER ","",",",null,"",{"$f":"IF(OR(I373=\"PK\", I373=\"PK/FK\"), \",\", \"\")","v":""},null,null,"lsu_1_cd_valu ","NUMBER(3) ","",",",null,null,"",{"$f":"IF(OR(I373=\"PK\", I373=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitdopermap3.","lsu_1_cd_valu"," IS ","'LSU1코드값 (신호운영맵 코드 값의 10진수변환값)'",";",null,""]
[7,"LSU2 코드 값","LSU2_CD_VAL","NUMBER",3,null,null,"LSU2코드값",null,"NULL","lsu_2_cd_valu","NUMBER(3)","INTEGER","NUMBER(3)","LSU2코드값 (신호운영맵 코드 값의 10진수변환값)",null,null,null,"lsu_2_cd_valu ","INTEGER ","",",",null,"","",null,null,"lsu_2_cd_valu ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdopermap3.","lsu_2_cd_valu"," IS ","'LSU2코드값 (신호운영맵 코드 값의 10진수변환값)'",";",null,""]
[8,"LSU3 코드 값","LSU3_CD_VAL","NUMBER",3,null,null,"LSU3코드값",null,"NULL","lsu_3_cd_valu","NUMBER(3)","INTEGER","NUMBER(3)","LSU3코드값 (신호운영맵 코드 값의 10진수변환값)",null,null,null,"lsu_3_cd_valu ","INTEGER ","",",",null,"","",null,null,"lsu_3_cd_valu ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdopermap3.","lsu_3_cd_valu"," IS ","'LSU3코드값 (신호운영맵 코드 값의 10진수변환값)'",";",null,""]
[9,"LSU4 코드 값","LSU4_CD_VAL","NUMBER",3,null,null,"LSU4코드값",null,"NULL","lsu_4_cd_valu","NUMBER(3)","INTEGER","NUMBER(3)","LSU4코드값 (신호운영맵 코드 값의 10진수변환값)",null,null,null,"lsu_4_cd_valu ","INTEGER ","",",",null,"","",null,null,"lsu_4_cd_valu ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdopermap3.","lsu_4_cd_valu"," IS ","'LSU4코드값 (신호운영맵 코드 값의 10진수변환값)'",";",null,""]
[10,"LSU5 코드 값","LSU5_CD_VAL","NUMBER",3,null,null,"LSU5코드값",null,"NULL","lsu_5_cd_valu","NUMBER(3)","INTEGER","NUMBER(3)","LSU5코드값 (신호운영맵 코드 값의 10진수변환값)",null,null,null,"lsu_5_cd_valu ","INTEGER ","",",",null,"","",null,null,"lsu_5_cd_valu ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdopermap3.","lsu_5_cd_valu"," IS ","'LSU5코드값 (신호운영맵 코드 값의 10진수변환값)'",";",null,""]
[11,"LSU6 코드 값","LSU6_CD_VAL","NUMBER",3,null,null,"LSU6코드값",null,"NULL","lsu_6_cd_valu","NUMBER(3)","INTEGER","NUMBER(3)","LSU6코드값 (신호운영맵 코드 값의 10진수변환값)",null,null,null,"lsu_6_cd_valu ","INTEGER ","",",",null,"","",null,null,"lsu_6_cd_valu ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdopermap3.","lsu_6_cd_valu"," IS ","'LSU6코드값 (신호운영맵 코드 값의 10진수변환값)'",";",null,""]
[12,"LSU7 코드 값","LSU7_CD_VAL","NUMBER",3,null,null,"LSU7코드값",null,"NULL","lsu_7_cd_valu","NUMBER(3)","INTEGER","NUMBER(3)","LSU7코드값 (신호운영맵 코드 값의 10진수변환값)",null,null,null,"lsu_7_cd_valu ","INTEGER ","",",",null,"","",null,null,"lsu_7_cd_valu ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdopermap3.","lsu_7_cd_valu"," IS ","'LSU7코드값 (신호운영맵 코드 값의 10진수변환값)'",";",null,""]
[13,"LSU8 코드 값","LSU8_CD_VAL","NUMBER",3,null,null,"LSU8코드값",null,"NULL","lsu_8_cd_valu","NUMBER(3)","INTEGER","NUMBER(3)","LSU8코드값 (신호운영맵 코드 값의 10진수변환값)",null,null,null,"lsu_8_cd_valu ","INTEGER ","",",",null,"","",null,null,"lsu_8_cd_valu ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdopermap3.","lsu_8_cd_valu"," IS ","'LSU8코드값 (신호운영맵 코드 값의 10진수변환값)'",";",null,""]
[14,"LSU9 코드 값","LSU9_CD_VAL","NUMBER",3,null,null,"LSU9코드값",null,"NULL","lsu_9_cd_valu","NUMBER(3)","INTEGER","NUMBER(3)","LSU9코드값 (신호운영맵 코드 값의 10진수변환값)",null,null,null,"lsu_9_cd_valu ","INTEGER ","",",",null,"","",null,null,"lsu_9_cd_valu ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdopermap3.","lsu_9_cd_valu"," IS ","'LSU9코드값 (신호운영맵 코드 값의 10진수변환값)'",";",null,""]
[15,"LSU10 코드 값","LSU10_CD_VAL","NUMBER",3,null,null,"LSU10코드값",null,"NULL","lsu_10_cd_valu","NUMBER(3)","INTEGER","NUMBER(3)","LSU10코드값 (신호운영맵 코드 값의 10진수변환값)",null,null,null,"lsu_10_cd_valu ","INTEGER ","",",",null,"","",null,null,"lsu_10_cd_valu ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdopermap3.","lsu_10_cd_valu"," IS ","'LSU10코드값 (신호운영맵 코드 값의 10진수변환값)'",";",null,""]
[16,"LSU11 코드 값","LSU11_CD_VAL","NUMBER",3,null,null,"LSU11코드값",null,"NULL","lsu_11_cd_valu","NUMBER(3)","INTEGER","NUMBER(3)","LSU11코드값 (신호운영맵 코드 값의 10진수변환값)",null,null,null,"lsu_11_cd_valu ","INTEGER ","",",",null,"","",null,null,"lsu_11_cd_valu ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdopermap3.","lsu_11_cd_valu"," IS ","'LSU11코드값 (신호운영맵 코드 값의 10진수변환값)'",";",null,""]
[17,"LSU12 코드 값","LSU12_CD_VAL","NUMBER",3,null,null,"LSU12코드값",null,"NULL","lsu_12_cd_valu","NUMBER(3)","INTEGER","NUMBER(3)","LSU12코드값 (신호운영맵 코드 값의 10진수변환값)",null,null,null,"lsu_12_cd_valu ","INTEGER ","",",",null,"","",null,null,"lsu_12_cd_valu ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdopermap3.","lsu_12_cd_valu"," IS ","'LSU12코드값 (신호운영맵 코드 값의 10진수변환값)'",";",null,""]
[18,"LSU13 코드 값","LSU13_CD_VAL","NUMBER",3,null,null,"LSU13코드값",null,"NULL","lsu_13_cd_valu","NUMBER(3)","INTEGER","NUMBER(3)","LSU13코드값 (신호운영맵 코드 값의 10진수변환값)",null,null,null,"lsu_13_cd_valu ","INTEGER ","",",",null,"","",null,null,"lsu_13_cd_valu ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdopermap3.","lsu_13_cd_valu"," IS ","'LSU13코드값 (신호운영맵 코드 값의 10진수변환값)'",";",null,""]
[19,"LSU14 코드 값","LSU14_CD_VAL","NUMBER",3,null,null,"LSU14코드값",null,"NULL","lsu_14_cd_valu","NUMBER(3)","INTEGER","NUMBER(3)","LSU14코드값 (신호운영맵 코드 값의 10진수변환값)",null,null,null,"lsu_14_cd_valu ","INTEGER ","",",",null,"","",null,null,"lsu_14_cd_valu ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdopermap3.","lsu_14_cd_valu"," IS ","'LSU14코드값 (신호운영맵 코드 값의 10진수변환값)'",";",null,""]
[20,"LSU15 코드 값","LSU15_CD_VAL","NUMBER",3,null,null,"LSU15코드값",null,"NULL","lsu_15_cd_valu","NUMBER(3)","INTEGER","NUMBER(3)","LSU15코드값 (신호운영맵 코드 값의 10진수변환값)",null,null,null,"lsu_15_cd_valu ","INTEGER ","",",",null,"","",null,null,"lsu_15_cd_valu ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdopermap3.","lsu_15_cd_valu"," IS ","'LSU15코드값 (신호운영맵 코드 값의 10진수변환값)'",";",null,""]
[21,"LSU16 코드 값","LSU16_CD_VAL","NUMBER",3,null,null,"LSU16코드값",null,"NULL","lsu_16_cd_valu","NUMBER(3)","INTEGER","NUMBER(3)","LSU16코드값 (신호운영맵 코드 값의 10진수변환값)",null,null,null,"lsu_16_cd_valu ","INTEGER ","",",",null,"","",null,null,"lsu_16_cd_valu ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdopermap3.","lsu_16_cd_valu"," IS ","'LSU16코드값 (신호운영맵 코드 값의 10진수변환값)'",";",null,""]
[22,"최소 값","MIN_VAL","NUMBER",3,"초",null,"최소값",null,"NOT NULL","min_valu","NUMBER(3)","INTEGER","NUMBER(3)","최소값 (sec)",null,null,null,"min_valu ","INTEGER ","NOT NULL",",",null,"","",null,null,"min_valu ","NUMBER(3) ","NOT NULL",",",null,null,"","","COMMENT ON COLUMN ","soitdopermap3.","min_valu"," IS ","'최소값 (sec)'",";",null,""]
[23,"최대 값","MAX_VAL","NUMBER",3,"초",null,"최대값",null,"NOT NULL","max_valu","NUMBER(3)","INTEGER","NUMBER(3)","최대값 (sec)",null,null,null,"max_valu ","INTEGER ","NOT NULL",",",null,"","",null,null,"max_valu ","NUMBER(3) ","NOT NULL",",",null,null,"","","COMMENT ON COLUMN ","soitdopermap3.","max_valu"," IS ","'최대값 (sec)'",";",null,""]
[24,"현시 종료 여부","PHAS_END_YN","NUMBER",1,"1:현시종료 ->Y/N변경요청필요","종료여부(020) Y:종료, N:진행","현시종료여부",null,"NOT NULL","phas_end_yn","CHAR(1)","VARCHAR(1)","VARCHAR2(1)","현시종료여부(020)","현시종료여부 (Y/N)",null,null,"phas_end_yn ","VARCHAR(1) ","NOT NULL",",",null,"","",null,null,"phas_end_yn ","VARCHAR2(1) ","NOT NULL",{"$f":"\") TABLESPACE \"&AF393&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_D001 NOLOGGING"},null,null,{"$f":"IF(OR(C391=\"PK\", C391=\"PK/FK\"), E391, \"\")","v":""},null,"COMMENT ON COLUMN ","soitdopermap3.","phas_end_yn"," IS ","'현시종료여부(020)'",";",null,""]
[{"$nulls":18},{"$f":"CONCATENATE(W367:Y391)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AF392:AH392)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (clct_unix_tm) INTERVAL (86400) STORE IN (\"&AF393&\") (PARTITION BFR_\" & H365 & \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AF393&\");\"","v":"PARTITION BY RANGE (clct_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_D001) (PARTITION BFR_soitdopermap3_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_D001);"},{"$f":"\"CREATE INDEX PK_\" & H365& \" ON \" & H365 & CONCATENATE(AG367:AI377) & \" LOCAL (PARTITION BFR_\" & H365 & \"_20221101 TABLESPACE \"&AG393&\") TABLESPACE \"&AG393&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & H365 & \" ADD CONSTRAINT PK_\" & H365 & \" PRIMARY KEY \" & CONCATENATE(AG367:AI383) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$error":"#VALUE!"}]
[{"$nulls":31},"SOIT_D08_D001","SOIT_I08_D001",{"$nulls":9},""]
["- 신호 운영 맵4 (SGNL_OPER_MAP4)",{"$nulls":6},"soitdopermap4",{"$nulls":4},{"$f":"LEN(H394)","v":13},{"$nulls":29},""]
["NO","속성명","컬럼명","형태","길이","비고",null,"논리명","PK/FK","NULL","물리명","형태","VOLT","TIBERO","COMMENT",{"$nulls":20},"COMMENT ON TABLE",{"$f":"H394&\" \"","v":"soitdopermap4 "},null," IS ",{"$f":"\"'\"&A394&\"'\"","v":"'- 신호 운영 맵4 (SGNL_OPER_MAP4)'"},";",null,""]
[1,"신호 교차로 번호","SGNL_IXR_NMBR","NUMBER",4,null,null,"현장교차로ID","PK/FK","NOT NULL","spot_ints_id","NUMBER(5)","INTEGER","NUMBER(5)","현장교차로ID",null,"CREATE TABLE ",{"$f":"H394&\" (\"","v":"soitdopermap4 ("},{"$f":"K396&\" \"","v":"spot_ints_id "},{"$f":"M396&\" \"","v":"INTEGER "},{"$f":"IF(J396=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(I396=\"PK\", I396=\"PK/FK\"), K396, \"\")","v":"spot_ints_id"},{"$f":"IF(OR(I396=\"PK\", I396=\"PK/FK\"), \",\", \"\")","v":","},"CREATE TABLE ",{"$f":"H394&\" (\"","v":"soitdopermap4 ("},{"$f":"K396&\" \"","v":"spot_ints_id "},{"$f":"N396&\" \"","v":"NUMBER(5) "},{"$f":"IF(J396=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(I396=\"PK\", I396=\"PK/FK\"), K396, \"\")","v":"spot_ints_id"},{"$f":"IF(OR(I396=\"PK\", I396=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$H$394&\".\"","v":"soitdopermap4."},{"$f":"K396","v":"spot_ints_id"}," IS ",{"$f":"\"'\"&O396&\"'\"","v":"'현장교차로ID'"},";",null,""]
[2,"수집 일시","CLCT_DT","INTEGER","UTC",null,null,"수집유닉스시각","PK","NOT NULL","clct_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)","수집유닉스시각",null,null,null,"clct_unix_tm ","INTEGER ","NOT NULL",",",null,"clct_unix_tm",",",null,null,"clct_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"clct_unix_tm",",","COMMENT ON COLUMN ","soitdopermap4.","clct_unix_tm"," IS ","'수집유닉스시각'",";",null,""]
[2,"수집일","CLCT_DATE","VARHCAR2",8,"YYYYMMDD",null,"수집일시",null,"NOT NULL","clct_dt","VARCHAR2(8)","VARCHAR(8)","VARCHAR2(8)","수집일시(yyyyMMdd)",null,null,null,{"$f":"K398","v":"clct_dt"},"VARCHAR(8) ","NOT NULL",",",null,"",null,null,null,"clct_dt ","VARCHAR2(8) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitdopermap4.","clct_dt"," IS ","'수집일시(yyyyMMdd)'",";"]
[3,"교차로 운영 모드","IXR_OPER_MODE","NUMBER",1,"0 :일반 \n1 :시차","운영구분코드(801)","운영구분코드","PK","NOT NULL","oper_se_cd","CHAR(3)","VARCHAR(3)","VARCHAR2(3)","운영구분코드(801)","운영구분코드 (0:일반 , 1:시차1, 2: 시차2, 3:시차3, 4:시차4, 5:시차5, 6:보행맵)",null,null,{"$f":"K399&\" \"","v":"oper_se_cd "},"VARCHAR(3) ","NOT NULL",",",null,"oper_se_cd",{"$f":"IF(OR(I399=\"PK\", I399=\"PK/FK\"), \",\", \"\")","v":","},null,null,"oper_se_cd ","VARCHAR2(3) ","NOT NULL",",",null,null,"oper_se_cd",{"$f":"IF(OR(I399=\"PK\", I399=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ","soitdopermap4.","oper_se_cd"," IS ","'운영구분코드(801)'",";",null,{"$f":"IF(LEFT(AB399, 13) = \"CONSTRAINT PK\", AB399, \"\")","v":""}]
[4,"링 구분","RING_DVSN","NUMBER",1,"0 :A링\n1 :B링","링구분코드(007)","링구분코드","PK","NOT NULL","ring_se_cd","CHAR(1)","VARCHAR(1)","VARCHAR2(1)","링구분코드(007)","링구분코드 (0:A링, 1:B링)",null,null,"ring_se_cd ","VARCHAR(1) ","NOT NULL",",",null,"ring_se_cd",",",null,null,"ring_se_cd ","VARCHAR2(1) ","NOT NULL",",",null,null,"ring_se_cd",",","COMMENT ON COLUMN ","soitdopermap4.","ring_se_cd"," IS ","'링구분코드(007)'",";",null,""]
[5,"스텝 번호","STEP_NMBR","NUMBER",2,"1~32",null,"스탭번호","PK","NOT NULL","step_no","NUMBER(2)","INTEGER","NUMBER(2)","스탭번호 (1~32)",null,null,null,"step_no ","INTEGER ","NOT NULL",",",null,"step_no","));",null,null,"step_no ","NUMBER(2) ","NOT NULL",",",null,null,"step_no",")","COMMENT ON COLUMN ","soitdopermap4.","step_no"," IS ","'스탭번호 (1~32)'",";",null,""]
[6,"차량등1 코드 값","VHLP1_CD_VAL","NUMBER",3,"신호운영맵 코드 값의 16진수를 10진수로 변경하여 저장\n0x01 -> 1\n0x02 -> 2\n0x03 -> 3\n0x04 -> 4\n0x05 -> 5\n0x06 -> 6\n0x07 -> 7\n0x08 -> 8\n0x09 -> 9\n0x10 -> 16\n0x20 -> 32\n0x30 -> 48\n0x40 -> 64\n0x50 -> 80\n0x80 -> 128",null,"차량등1코드값",null,"NULL","vhcl_lght_1_cd_valu","NUMBER(3)","INTEGER","NUMBER(3)","차량등1코드값 (신호운영맵 코드 값의 10진수변환값)",null,null,null,"vhcl_lght_1_cd_valu ","INTEGER ","",",",null,"",{"$f":"IF(OR(I402=\"PK\", I402=\"PK/FK\"), \",\", \"\")","v":""},null,null,"vhcl_lght_1_cd_valu ","NUMBER(3) ","",",",null,null,"",{"$f":"IF(OR(I402=\"PK\", I402=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitdopermap4.","vhcl_lght_1_cd_valu"," IS ","'차량등1코드값 (신호운영맵 코드 값의 10진수변환값)'",";",null,""]
[7,"차량등2 코드 값","VHLP2_CD_VAL","NUMBER",3,null,null,"차량등2코드값",null,"NULL","vhcl_lght_2_cd_valu","NUMBER(3)","INTEGER","NUMBER(3)","차량등2코드값 (신호운영맵 코드 값의 10진수변환값)",null,null,null,"vhcl_lght_2_cd_valu ","INTEGER ","",",",null,"","",null,null,"vhcl_lght_2_cd_valu ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdopermap4.","vhcl_lght_2_cd_valu"," IS ","'차량등2코드값 (신호운영맵 코드 값의 10진수변환값)'",";",null,""]
[8,"차량등3 코드 값","VHLP3_CD_VAL","NUMBER",3,null,null,"차량등3코드값",null,"NULL","vhcl_lght_3_cd_valu","NUMBER(3)","INTEGER","NUMBER(3)","차량등3코드값 (신호운영맵 코드 값의 10진수변환값)",null,null,null,"vhcl_lght_3_cd_valu ","INTEGER ","",",",null,"","",null,null,"vhcl_lght_3_cd_valu ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdopermap4.","vhcl_lght_3_cd_valu"," IS ","'차량등3코드값 (신호운영맵 코드 값의 10진수변환값)'",";",null,""]
[9,"차량등4 코드 값","VHLP4_CD_VAL","NUMBER",3,null,null,"차량등4코드값",null,"NULL","vhcl_lght_4_cd_valu","NUMBER(3)","INTEGER","NUMBER(3)","차량등4코드값 (신호운영맵 코드 값의 10진수변환값)",null,null,null,"vhcl_lght_4_cd_valu ","INTEGER ","",",",null,"","",null,null,"vhcl_lght_4_cd_valu ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdopermap4.","vhcl_lght_4_cd_valu"," IS ","'차량등4코드값 (신호운영맵 코드 값의 10진수변환값)'",";",null,""]
[10,"차량등5 코드 값","VHLP5_CD_VAL","NUMBER",3,null,null,"차량등5코드값",null,"NULL","vhcl_lght_5_cd_valu","NUMBER(3)","INTEGER","NUMBER(3)","차량등5코드값 (신호운영맵 코드 값의 10진수변환값)",null,null,null,"vhcl_lght_5_cd_valu ","INTEGER ","",",",null,"","",null,null,"vhcl_lght_5_cd_valu ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdopermap4.","vhcl_lght_5_cd_valu"," IS ","'차량등5코드값 (신호운영맵 코드 값의 10진수변환값)'",";",null,""]
[11,"차량등6 코드 값","VHLP6_CD_VAL","NUMBER",3,null,null,"차량등6코드값",null,"NULL","vhcl_lght_6_cd_valu","NUMBER(3)","INTEGER","NUMBER(3)","차량등6코드값 (신호운영맵 코드 값의 10진수변환값)",null,null,null,"vhcl_lght_6_cd_valu ","INTEGER ","",",",null,"","",null,null,"vhcl_lght_6_cd_valu ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdopermap4.","vhcl_lght_6_cd_valu"," IS ","'차량등6코드값 (신호운영맵 코드 값의 10진수변환값)'",";",null,""]
[12,"차량등7 코드 값","VHLP7_CD_VAL","NUMBER",3,null,null,"차량등7코드값",null,"NULL","vhcl_lght_7_cd_valu","NUMBER(3)","INTEGER","NUMBER(3)","차량등7코드값 (신호운영맵 코드 값의 10진수변환값)",null,null,null,"vhcl_lght_7_cd_valu ","INTEGER ","",",",null,"","",null,null,"vhcl_lght_7_cd_valu ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdopermap4.","vhcl_lght_7_cd_valu"," IS ","'차량등7코드값 (신호운영맵 코드 값의 10진수변환값)'",";",null,""]
[13,"차량등8 코드 값","VHLP8_CD_VAL","NUMBER",3,null,null,"차량등8코드값",null,"NULL","vhcl_lght_8_cd_valu","NUMBER(3)","INTEGER","NUMBER(3)","차량등8코드값 (신호운영맵 코드 값의 10진수변환값)",null,null,null,"vhcl_lght_8_cd_valu ","INTEGER ","",",",null,"","",null,null,"vhcl_lght_8_cd_valu ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdopermap4.","vhcl_lght_8_cd_valu"," IS ","'차량등8코드값 (신호운영맵 코드 값의 10진수변환값)'",";",null,""]
[14,"보행등1 코드 값","WKLP1_CD_VAL","NUMBER",3,null,null,"보행등1코드값",null,"NULL","ambl_lght_1_cd_valu","NUMBER(3)","INTEGER","NUMBER(3)","보행등1코드값 (신호운영맵 코드 값의 10진수변환값)",null,null,null,"ambl_lght_1_cd_valu ","INTEGER ","",",",null,"","",null,null,"ambl_lght_1_cd_valu ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdopermap4.","ambl_lght_1_cd_valu"," IS ","'보행등1코드값 (신호운영맵 코드 값의 10진수변환값)'",";",null,""]
[15,"보행등2 코드 값","WKLP2_CD_VAL","NUMBER",3,null,null,"보행등2코드값",null,"NULL","ambl_lght_2_cd_valu","NUMBER(3)","INTEGER","NUMBER(3)","보행등2코드값 (신호운영맵 코드 값의 10진수변환값)",null,null,null,"ambl_lght_2_cd_valu ","INTEGER ","",",",null,"","",null,null,"ambl_lght_2_cd_valu ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdopermap4.","ambl_lght_2_cd_valu"," IS ","'보행등2코드값 (신호운영맵 코드 값의 10진수변환값)'",";",null,""]
[16,"보행등3 코드 값","WKLP3_CD_VAL","NUMBER",3,null,null,"보행등3코드값",null,"NULL","ambl_lght_3_cd_valu","NUMBER(3)","INTEGER","NUMBER(3)","보행등3코드값 (신호운영맵 코드 값의 10진수변환값)",null,null,null,"ambl_lght_3_cd_valu ","INTEGER ","",",",null,"","",null,null,"ambl_lght_3_cd_valu ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdopermap4.","ambl_lght_3_cd_valu"," IS ","'보행등3코드값 (신호운영맵 코드 값의 10진수변환값)'",";",null,""]
[17,"보행등4 코드 값","WKLP4_CD_VAL","NUMBER",3,null,null,"보행등4코드값",null,"NULL","ambl_lght_4_cd_valu","NUMBER(3)","INTEGER","NUMBER(3)","보행등4코드값 (신호운영맵 코드 값의 10진수변환값)",null,null,null,"ambl_lght_4_cd_valu ","INTEGER ","",",",null,"","",null,null,"ambl_lght_4_cd_valu ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdopermap4.","ambl_lght_4_cd_valu"," IS ","'보행등4코드값 (신호운영맵 코드 값의 10진수변환값)'",";",null,""]
[18,"보행등5 코드 값","WKLP5_CD_VAL","NUMBER",3,null,null,"보행등5코드값",null,"NULL","ambl_lght_5_cd_valu","NUMBER(3)","INTEGER","NUMBER(3)","보행등5코드값 (신호운영맵 코드 값의 10진수변환값)",null,null,null,"ambl_lght_5_cd_valu ","INTEGER ","",",",null,"","",null,null,"ambl_lght_5_cd_valu ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdopermap4.","ambl_lght_5_cd_valu"," IS ","'보행등5코드값 (신호운영맵 코드 값의 10진수변환값)'",";",null,""]
[19,"보행등6 코드 값","WKLP6_CD_VAL","NUMBER",3,null,null,"보행등6코드값",null,"NULL","ambl_lght_6_cd_valu","NUMBER(3)","INTEGER","NUMBER(3)","보행등6코드값 (신호운영맵 코드 값의 10진수변환값)",null,null,null,"ambl_lght_6_cd_valu ","INTEGER ","",",",null,"","",null,null,"ambl_lght_6_cd_valu ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdopermap4.","ambl_lght_6_cd_valu"," IS ","'보행등6코드값 (신호운영맵 코드 값의 10진수변환값)'",";",null,""]
[20,"보행등7 코드 값","WKLP7_CD_VAL","NUMBER",3,null,null,"보행등7코드값",null,"NULL","ambl_lght_7_cd_valu","NUMBER(3)","INTEGER","NUMBER(3)","보행등7코드값 (신호운영맵 코드 값의 10진수변환값)",null,null,null,"ambl_lght_7_cd_valu ","INTEGER ","",",",null,"","",null,null,"ambl_lght_7_cd_valu ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdopermap4.","ambl_lght_7_cd_valu"," IS ","'보행등7코드값 (신호운영맵 코드 값의 10진수변환값)'",";",null,""]
[21,"보행등8 코드 값","WKLP8_CD_VAL","NUMBER",3,null,null,"보행등8코드값",null,"NULL","ambl_lght_8_cd_valu","NUMBER(3)","INTEGER","NUMBER(3)","보행등8코드값 (신호운영맵 코드 값의 10진수변환값)",null,null,null,"ambl_lght_8_cd_valu ","INTEGER ","",",",null,"","",null,null,"ambl_lght_8_cd_valu ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdopermap4.","ambl_lght_8_cd_valu"," IS ","'보행등8코드값 (신호운영맵 코드 값의 10진수변환값)'",";",null,""]
[22,"최소 값","MIN_VAL","NUMBER",3,"초",null,"최소값",null,"NOT NULL","min_valu","NUMBER(3)","INTEGER","NUMBER(3)","최소값 (sec)",null,null,null,"min_valu ","INTEGER ","NOT NULL",",",null,"","",null,null,"min_valu ","NUMBER(3) ","NOT NULL",",",null,null,"","","COMMENT ON COLUMN ","soitdopermap4.","min_valu"," IS ","'최소값 (sec)'",";",null,""]
[23,"최대 값","MAX_VAL","NUMBER",3,"초",null,"최대값",null,"NOT NULL","max_valu","NUMBER(3)","INTEGER","NUMBER(3)","최대값 (sec)",null,null,null,"max_valu ","INTEGER ","NOT NULL",",",null,"","",null,null,"max_valu ","NUMBER(3) ","NOT NULL",",",null,null,"","","COMMENT ON COLUMN ","soitdopermap4.","max_valu"," IS ","'최대값 (sec)'",";",null,""]
[24,"현시 종료 여부","PHAS_END_YN","NUMBER",1,"1:현시종료 ->Y/N변경요청필요","종료여부(020) Y:종료, N:진행","현시종료여부",null,"NOT NULL","phas_end_yn","CHAR(1)","VARCHAR(1)","VARCHAR2(1)","현시종료여부(020)","현시종료여부 (Y/N)",null,null,"phas_end_yn ","VARCHAR(1) ","NOT NULL",",",null,"","",null,null,"phas_end_yn ","VARCHAR2(1) ","NOT NULL",{"$f":"\") TABLESPACE \"&AF422&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_D001 NOLOGGING"},null,null,{"$f":"IF(OR(C420=\"PK\", C420=\"PK/FK\"), E420, \"\")","v":""},null,"COMMENT ON COLUMN ","soitdopermap4.","phas_end_yn"," IS ","'현시종료여부(020)'",";",null,""]
[{"$nulls":18},{"$f":"CONCATENATE(W396:Y420)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AF421:AH421)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (clct_unix_tm) INTERVAL (86400) STORE IN (\"&AF422&\") (PARTITION BFR_\" & H394 & \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AF422&\");\"","v":"PARTITION BY RANGE (clct_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_D001) (PARTITION BFR_soitdopermap4_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_D001);"},{"$f":"\"CREATE INDEX PK_\" & H394& \" ON \" & H394 & CONCATENATE(AG396:AI406) & \" LOCAL (PARTITION BFR_\" & H394 & \"_20221101 TABLESPACE \"&AG422&\") TABLESPACE \"&AG422&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & H394 & \" ADD CONSTRAINT PK_\" & H394 & \" PRIMARY KEY \" & CONCATENATE(AG396:AI412) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$error":"#VALUE!"}]
[{"$nulls":31},"SOIT_D08_D001","SOIT_I08_D001"]
["- 신호 출력 (SGNL_PRNT)",{"$nulls":6},"soitdsgnlotptdrct",{"$nulls":4},{"$f":"LEN(H423)","v":17},{"$nulls":29},{"$f":"IF(LEFT(AB423, 13) = \"CONSTRAINT PK\", AB423, \"\")","v":""}]
["NO","속성명","컬럼명","형태","길이","비고",null,"논리명","PK/FK","NULL","물리명","형태","VOLT","TIBERO","COMMENT",{"$nulls":20},"COMMENT ON TABLE",{"$f":"H423&\" \"","v":"soitdsgnlotptdrct "},null," IS ",{"$f":"\"'\"&A423&\"'\"","v":"'- 신호 출력 (SGNL_PRNT)'"},";",null,""]
[1,"신호 교차로 번호","SGNL_IXR_NMBR","NUMBER",4,null,null,"현장교차로ID","PK/FK","NOT NULL","spot_ints_id","NUMBER(5)","INTEGER","NUMBER(5)","현장교차로ID",null,"CREATE TABLE ",{"$f":"H423&\" (\"","v":"soitdsgnlotptdrct ("},{"$f":"K425&\" \"","v":"spot_ints_id "},{"$f":"M425&\" \"","v":"INTEGER "},{"$f":"IF(J425=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(I425=\"PK\", I425=\"PK/FK\"), K425, \"\")","v":"spot_ints_id"},{"$f":"IF(OR(I425=\"PK\", I425=\"PK/FK\"), \",\", \"\")","v":","},"CREATE TABLE ",{"$f":"H423&\" (\"","v":"soitdsgnlotptdrct ("},{"$f":"K425&\" \"","v":"spot_ints_id "},{"$f":"N425&\" \"","v":"NUMBER(5) "},{"$f":"IF(J425=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(I425=\"PK\", I425=\"PK/FK\"), K425, \"\")","v":"spot_ints_id"},{"$f":"IF(OR(I425=\"PK\", I425=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$H$423&\".\"","v":"soitdsgnlotptdrct."},{"$f":"K425","v":"spot_ints_id"}," IS ",{"$f":"\"'\"&O425&\"'\"","v":"'현장교차로ID'"},";",null,""]
[2,"수집 일시","CLCT_DT","INTEGER","UTC",null,null,"수집유닉스시각","PK","NOT NULL","clct_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)","수집유닉스시각",null,null,null,"clct_unix_tm ","INTEGER ","NOT NULL",",",null,"clct_unix_tm",",",null,null,"clct_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"clct_unix_tm",",","COMMENT ON COLUMN ","soitdsgnlotptdrct.","clct_unix_tm"," IS ","'수집유닉스시각'",";",null,""]
[2,"수집일","CLCT_DATE","VARHCAR2",8,"YYYYMMDD",null,"수집일시",null,"NOT NULL","clct_dt","VARCHAR2(8)","VARCHAR(8)","VARCHAR2(8)","수집일시(yyyyMMdd)",null,null,null,{"$f":"K427","v":"clct_dt"},"VARCHAR(8) ","NOT NULL",",",null,"",null,null,null,"clct_dt ","VARCHAR2(8) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitdsgnlotptdrct.","clct_dt"," IS ","'수집일시(yyyyMMdd)'",";"]
[3,"신호 출력 방향","SGNL_PRNT_DRCT","NUMBER",2,"0:북\n 1:동\n 2:남\n 3:서\n 4:북동\n 5:남동\n 6:남서\n 7:북서\n 8:예비1\n 9:예비2","신호출력방향(805)","신호출력방향코드","PK","NOT NULL","sgnl_otpt_drct_cd","CHAR(3)","VARCHAR(3)","VARCHAR2(3)","신호출력방향(805)","신호출력방향코드 (0:북, 1:동, 2:남, 3:서, 4:북동, 5:남동, 6:남서, 7:북서, 8:예비1, 9:예비2)",null,null,{"$f":"K428&\" \"","v":"sgnl_otpt_drct_cd "},"VARCHAR(3) ","NOT NULL",",",null,"sgnl_otpt_drct_cd","));",null,null,"sgnl_otpt_drct_cd ","VARCHAR2(3) ","NOT NULL",",",null,null,"sgnl_otpt_drct_cd",")","COMMENT ON COLUMN ","soitdsgnlotptdrct.","sgnl_otpt_drct_cd"," IS ","'신호출력방향(805)'",";",null,{"$f":"IF(LEFT(AB428, 13) = \"CONSTRAINT PK\", AB428, \"\")","v":""}]
[4,"보행 LSU","WALK_LSU","NUMBER",2,"0:없음 \n 1: LSU1\n 2: LSU2\n 3: LSU3\n 4: LSU4\n 5: LSU5\n 6: LSU6\n 7: LSU7\n 8: LSU8\n 9: LSU9\n10: LSU10\n11: LSU11\n12: LSU12\n13: LSU13\n14: LSU14\n15: LSU15\n16: LSU16","보행 LSU(806)","보행LSU번호",null,"NOT NULL","ambl_lsu_no","NUMBER(2)","INTEGER","NUMBER(2)","보행 LSU코드(806)","보행LSU번호 (0:없음, 1~16:LSU번호)",null,null,"ambl_lsu_no ","INTEGER ","NOT NULL",",",null,"",{"$f":"IF(OR(I429=\"PK\", I429=\"PK/FK\"), \",\", \"\")","v":""},null,null,"ambl_lsu_no ","NUMBER(2) ","NOT NULL",",",null,null,"",{"$f":"IF(OR(I429=\"PK\", I429=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitdsgnlotptdrct.","ambl_lsu_no"," IS ","'보행 LSU코드(806)'",";",null,""]
[5,"보행 출력 신호","WALK_PRNT_SGNL","NUMBER",1,"0 :없음\n1 :G1\n2 :G2\n3 :Y1","보행 출력 신호(807)","보행출력신호코드",null,"NOT NULL","ambl_otpt_sgnl_cd","CHAR(3)","VARCHAR(3)","VARCHAR2(3)","보행 출력 신호코드(807)","보행출력신호코드 (0:없음, 1:G1, 2:G2, 3:Y1)",null,null,"ambl_otpt_sgnl_cd ","VARCHAR(3) ","NOT NULL",",",null,"","",null,null,"ambl_otpt_sgnl_cd ","VARCHAR2(3) ","NOT NULL",{"$f":"\") TABLESPACE \"&AF432&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_D001 NOLOGGING"},null,null,{"$f":"IF(OR(C430=\"PK\", C430=\"PK/FK\"), E430, \"\")","v":""},null,"COMMENT ON COLUMN ","soitdsgnlotptdrct.","ambl_otpt_sgnl_cd"," IS ","'보행 출력 신호코드(807)'",";",null,""]
[{"$nulls":18},{"$f":"CONCATENATE(W425:Y430)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AF431:AH431)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (clct_unix_tm) INTERVAL (86400) STORE IN (\"&AF432&\") (PARTITION BFR_\" & H423& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AF432&\");\"","v":"PARTITION BY RANGE (clct_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_D001) (PARTITION BFR_soitdsgnlotptdrct_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_D001);"},{"$f":"\"CREATE INDEX PK_\" & H423& \" ON \" & H423 & CONCATENATE(AG425:AI429) & \" LOCAL (PARTITION BFR_\" & H423 & \"_20221101 TABLESPACE \"&AG432&\") TABLESPACE \"&AG432&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & H423 & \" ADD CONSTRAINT PK_\" & H423 & \" PRIMARY KEY \" & CONCATENATE(AG425:AI429) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$error":"#VALUE!"}]
[{"$nulls":31},"SOIT_D08_D001","SOIT_I08_D001"]
["- 긴급차량운영이력(EMRG_VHCL_OPER_HS)",{"$nulls":6},"soitdemrgvhcloperhstr",{"$nulls":4},{"$f":"LEN(H433)","v":21},{"$nulls":29},{"$f":"IF(LEFT(AB433, 13) = \"CONSTRAINT PK\", AB433, \"\")","v":""}]
["NO","속성명","컬럼명","형태","길이","비고",null,"논리명","PK/FK","NULL","물리명","형태","VOLT","TIBERO","COMMENT",{"$nulls":20},"COMMENT ON TABLE",{"$f":"H433&\" \"","v":"soitdemrgvhcloperhstr "},null," IS ",{"$f":"\"'\"&A433&\"'\"","v":"'- 긴급차량운영이력(EMRG_VHCL_OPER_HS)'"},";",null,""]
[1,"수집 일시","CLCT_DT","INTEGER","UTC",null,null,"수집유닉스시각","PK","NOT NULL","clct_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)","수집유닉스시각",null,"CREATE TABLE ",{"$f":"H433&\" (\"","v":"soitdemrgvhcloperhstr ("},{"$f":"K435&\" \"","v":"clct_unix_tm "},{"$f":"M435&\" \"","v":"INTEGER "},{"$f":"IF(J435=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(I435=\"PK\", I435=\"PK/FK\"), K435, \"\")","v":"clct_unix_tm"},{"$f":"IF(OR(I435=\"PK\", I435=\"PK/FK\"), \",\", \"\")","v":","},"CREATE TABLE ",{"$f":"H433&\" (\"","v":"soitdemrgvhcloperhstr ("},{"$f":"K435&\" \"","v":"clct_unix_tm "},{"$f":"N435&\" \"","v":"NUMBER(10) "},{"$f":"IF(J435=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(I435=\"PK\", I435=\"PK/FK\"), K435, \"\")","v":"clct_unix_tm"},{"$f":"IF(OR(I435=\"PK\", I435=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$H$433&\".\"","v":"soitdemrgvhcloperhstr."},{"$f":"K435","v":"clct_unix_tm"}," IS ",{"$f":"\"'\"&O435&\"'\"","v":"'수집유닉스시각'"},";",null,""]
[2,"수집일","CLCT_DATE","VARHCAR2",8,"YYYYMMDD",null,"수집일시",null,"NOT NULL","clct_dt","VARCHAR2(8)","VARCHAR(8)","VARCHAR2(8)","수집일시(yyyyMMdd)",null,null,null,{"$f":"K436","v":"clct_dt"},"VARCHAR(8) ","NOT NULL",",",null,"",null,null,null,"clct_dt ","VARCHAR2(8) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitdemrgvhcloperhstr.","clct_dt"," IS ","'수집일시(yyyyMMdd)'",";"]
[2,"수집 번호","CLCT_NMBR","NUMBER",8,null,null,"수집일련번호","PK","NOT NULL","clct_sn","NUMBER(10)","INTEGER","NUMBER(10)","수집일련번호",null,null,null,{"$f":"K437&\" \"","v":"clct_sn "},"INTEGER ","NOT NULL",",",null,"clct_sn",",",null,null,"clct_sn ","NUMBER(10) ","NOT NULL",",",null,null,"clct_sn",",","COMMENT ON COLUMN ","soitdemrgvhcloperhstr.","clct_sn"," IS ","'수집일련번호'",";",null,{"$f":"IF(LEFT(AB437, 13) = \"CONSTRAINT PK\", AB437, \"\")","v":""}]
[3,"긴급차량 ID","EMRG_VHCL_ID","NUMBER",3,null,null,"긴급차량ID","FK","NOT NULL","emrg_vhcl_id","NUMBER(5)","INTEGER","NUMBER(5)","긴급차량ID",null,null,null,"emrg_vhcl_id ","INTEGER ","NOT NULL",",",null,"",{"$f":"IF(OR(I438=\"PK\", I438=\"PK/FK\"), \",\", \"\")","v":""},null,null,"emrg_vhcl_id ","NUMBER(5) ","NOT NULL",",",null,null,"",{"$f":"IF(OR(I438=\"PK\", I438=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitdemrgvhcloperhstr.","emrg_vhcl_id"," IS ","'긴급차량ID'",";",null,""]
[4,"서비스 ID","SRVC_ID","VARCHAR2",12,null,null,"서비스ID","PK","NOT NULL","srvc_id","VARCHAR2(20)","VARCHAR(20)","VARCHAR2(20)","서비스ID",null,null,null,"srvc_id ","VARCHAR(20) ","NOT NULL",",",null,"srvc_id","));",null,null,"srvc_id ","VARCHAR2(20) ","NOT NULL",",",null,null,"srvc_id",")","COMMENT ON COLUMN ","soitdemrgvhcloperhstr.","srvc_id"," IS ","'서비스ID'",";",null,""]
[5,"X 좌표","X_CRDN","NUMBER",10,null,null,"수집위치경도",null,"NULL","clct_locn_lot","NUMBER(13,10)","FLOAT","NUMBER(13,10)","수집위치경도",null,null,null,"clct_locn_lot ","FLOAT ","",",",null,"",{"$f":"IF(OR(I440=\"PK\", I440=\"PK/FK\"), \",\", \"\")","v":""},null,null,"clct_locn_lot ","NUMBER(13,10) ","",",",null,null,"",{"$f":"IF(OR(I440=\"PK\", I440=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitdemrgvhcloperhstr.","clct_locn_lot"," IS ","'수집위치경도'",";",null,""]
[6,"Y 좌표","Y_CRDN","NUMBER",10,null,null,"수집위치위도",null,"NULL","clct_locn_lat","NUMBER(12,10)","FLOAT","NUMBER(12,10)","수집위치위도",null,null,null,"clct_locn_lat ","FLOAT ","",",",null,"","",null,null,"clct_locn_lat ","NUMBER(12,10) ","",{"$f":"\") TABLESPACE \"&AF443&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_D003 NOLOGGING"},null,null,{"$f":"IF(OR(C441=\"PK\", C441=\"PK/FK\"), E441, \"\")","v":""},null,"COMMENT ON COLUMN ","soitdemrgvhcloperhstr.","clct_locn_lat"," IS ","'수집위치위도'",";",null,""]
[{"$nulls":18},{"$f":"CONCATENATE(W435:Y441)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AF442:AH442)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (clct_unix_tm) INTERVAL (3600) STORE IN (\"&AF443&\") (PARTITION BFR_\" & H433& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AF443&\");\"","v":"PARTITION BY RANGE (clct_unix_tm) INTERVAL (3600) STORE IN (SOIT_D08_D003) (PARTITION BFR_soitdemrgvhcloperhstr_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_D003);"},{"$f":"\"CREATE INDEX PK_\" & H433& \" ON \" & H433 & CONCATENATE(AG435:AI440) & \" LOCAL (PARTITION BFR_\" & H433 & \"_20221101 TABLESPACE \"&AG443&\") TABLESPACE \"&AG443&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & H433 & \" ADD CONSTRAINT PK_\" & H433 & \" PRIMARY KEY \" & CONCATENATE(AG435:AI440) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$error":"#VALUE!"}]
[{"$nulls":31},"SOIT_D08_D003","SOIT_I08_D003"]
["- 우선신호요청정보(PRIO_SGNL_REQ_INFR)",{"$nulls":6},"soitdemrgsgnlinfo",{"$nulls":4},{"$f":"LEN(H444)","v":17},"긴급신호요청정보",{"$nulls":28},{"$f":"IF(LEFT(AB444, 13) = \"CONSTRAINT PK\", AB444, \"\")","v":""}]
["NO","속성명","컬럼명","형태","길이","비고",null,"논리명","PK/FK","NULL","물리명","형태","VOLT","TIBERO","COMMENT",{"$nulls":20},"COMMENT ON TABLE",{"$f":"H444&\" \"","v":"soitdemrgsgnlinfo "},null," IS ",{"$f":"\"'\"&A444&\"'\"","v":"'- 우선신호요청정보(PRIO_SGNL_REQ_INFR)'"},";",null,""]
[1,"긴급차량 ID","EMRG_VHCL_ID","NUMBER",3,null,null,"긴급차량ID","PK/FK","NOT NULL","emrg_vhcl_id","NUMBER(5)","INTEGER","NUMBER(5)","긴급차량ID",null,"CREATE TABLE ",{"$f":"H444&\" (\"","v":"soitdemrgsgnlinfo ("},{"$f":"K446&\" \"","v":"emrg_vhcl_id "},{"$f":"M446&\" \"","v":"INTEGER "},{"$f":"IF(J446=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(I446=\"PK\", I446=\"PK/FK\"), K446, \"\")","v":"emrg_vhcl_id"},{"$f":"IF(OR(I446=\"PK\", I446=\"PK/FK\"), \",\", \"\")","v":","},"CREATE TABLE ",{"$f":"H444&\" (\"","v":"soitdemrgsgnlinfo ("},{"$f":"K446&\" \"","v":"emrg_vhcl_id "},{"$f":"N446&\" \"","v":"NUMBER(5) "},{"$f":"IF(J446=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(I446=\"PK\", I446=\"PK/FK\"), K446, \"\")","v":"emrg_vhcl_id"},{"$f":"IF(OR(I446=\"PK\", I446=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$H$444&\".\"","v":"soitdemrgsgnlinfo."},{"$f":"K446","v":"emrg_vhcl_id"}," IS ",{"$f":"\"'\"&O446&\"'\"","v":"'긴급차량ID'"},";",null,""]
[2,"수집 일시","CLCT_DT","INTEGER","UTC",null,null,"수집유닉스시각","PK","NOT NULL","clct_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)","수집유닉스시각",null,null,null,"clct_unix_tm ","INTEGER ","NOT NULL",",",null,"clct_unix_tm",",",null,null,"clct_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"clct_unix_tm",",","COMMENT ON COLUMN ","soitdemrgsgnlinfo.","clct_unix_tm"," IS ","'수집유닉스시각'",";",null,""]
[2,"수집일","CLCT_DATE","VARHCAR2",8,"YYYYMMDD",null,"수집일시",null,"NOT NULL","clct_dt","VARCHAR2(8)","VARCHAR(8)","VARCHAR2(8)","수집일시(yyyyMMdd)",null,null,null,{"$f":"K448","v":"clct_dt"},"VARCHAR(8) ","NOT NULL",",",null,"",null,null,null,"clct_dt ","VARCHAR2(8) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitdemrgsgnlinfo.","clct_dt"," IS ","'수집일시(yyyyMMdd)'",";"]
[2,"서비스 ID","SRVC_ID","VARCHAR2",12,null,null,"서비스ID","PK/FK","NOT NULL","srvc_id","VARCHAR2(20)","VARCHAR(20)","VARCHAR2(20)","서비스ID",null,null,null,{"$f":"K449&\" \"","v":"srvc_id "},"VARCHAR(20) ","NOT NULL",",",null,"srvc_id","));",null,null,"srvc_id ","VARCHAR2(20) ","NOT NULL",",",null,null,"srvc_id",")","COMMENT ON COLUMN ","soitdemrgsgnlinfo.","srvc_id"," IS ","'서비스ID'",";",null,{"$f":"IF(LEFT(AB449, 13) = \"CONSTRAINT PK\", AB449, \"\")","v":""}]
[3,"종료 여부","END_YN","VARCHAR2",1,"Y:종료\nN:진행중","종료여부(020) Y:종료, N:진행","종료여부",null,"NOT NULL","end_yn","CHAR(1)","VARCHAR(1)","VARCHAR2(1)","종료여부(020)","종료여부 (Y/N)",null,null,"end_yn ","VARCHAR(1) ","NOT NULL",",",null,"",{"$f":"IF(OR(I450=\"PK\", I450=\"PK/FK\"), \",\", \"\")","v":""},null,null,"end_yn ","VARCHAR2(1) ","NOT NULL",",",null,null,"",{"$f":"IF(OR(I450=\"PK\", I450=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitdemrgsgnlinfo.","end_yn"," IS ","'종료여부(020)'",";",null,""]
[4,"출발지 X좌표","DPTR_X_CRDN","NUMBER",10,null,null,"출발지경도",null,"NULL","dptre_rgn_lot","NUMBER(13,10)","FLOAT","NUMBER(13,10)","출발지경도",null,null,null,"dptre_rgn_lot ","FLOAT ","",",",null,"","",null,null,"dptre_rgn_lot ","NUMBER(13,10) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdemrgsgnlinfo.","dptre_rgn_lot"," IS ","'출발지경도'",";",null,""]
[5,"출발지 Y좌표","DPTR_Y_CRDN","NUMBER",10,null,null,"출발지위도",null,"NULL","dptre_rgn_lat","NUMBER(12,10)","FLOAT","NUMBER(12,10)","출발지위도",null,null,null,"dptre_rgn_lat ","FLOAT ","",",",null,"","",null,null,"dptre_rgn_lat ","NUMBER(12,10) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdemrgsgnlinfo.","dptre_rgn_lat"," IS ","'출발지위도'",";",null,""]
[6,"목적지 X좌표","DEST_X_CRDN","NUMBER",10,null,null,"도착지경도",null,"NULL","arvl_rgn_lot","NUMBER(13,10)","FLOAT","NUMBER(13,10)","도착지경도",null,null,null,"arvl_rgn_lot ","FLOAT ","",",",null,"","",null,null,"arvl_rgn_lot ","NUMBER(13,10) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdemrgsgnlinfo.","arvl_rgn_lot"," IS ","'도착지경도'",";",null,""]
[7,"목적지 Y좌표","DEST_Y_CRDN","NUMBER",10,null,null,"도착지위도",null,"NULL","arvl_rgn_lat","NUMBER(12,10)","FLOAT","NUMBER(12,10)","도착지위도",null,null,null,"arvl_rgn_lat ","FLOAT ","",",",null,"","",null,null,"arvl_rgn_lat ","NUMBER(12,10) ","",{"$f":"\") TABLESPACE \"&AF456&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_D002 NOLOGGING"},null,null,{"$f":"IF(OR(C454=\"PK\", C454=\"PK/FK\"), E454, \"\")","v":""},null,"COMMENT ON COLUMN ","soitdemrgsgnlinfo.","arvl_rgn_lat"," IS ","'도착지위도'",";",null,""]
[{"$nulls":18},{"$f":"CONCATENATE(W446:Y454)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AF455:AH455)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (clct_unix_tm) INTERVAL (86400) STORE IN (\"&AF456&\") (PARTITION BFR_\" & H444& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AF456&\");\"","v":"PARTITION BY RANGE (clct_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_D002) (PARTITION BFR_soitdemrgsgnlinfo_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_D002);"},{"$f":"\"CREATE INDEX PK_\" & H444& \" ON \" & H444 & CONCATENATE(AG446:AI452) & \" LOCAL (PARTITION BFR_\" & H444 & \"_20221101 TABLESPACE \"&AG456&\") TABLESPACE \"&AG456&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & H444 & \" ADD CONSTRAINT PK_\" & H444 & \" PRIMARY KEY \" & CONCATENATE(AG446:AI452) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$error":"#VALUE!"}]
[{"$nulls":31},"SOIT_D08_D002","SOIT_I08_D002"]
["- 긴급차량(EMRG_VHCL)",{"$nulls":6},"soitdemrgvhclinfo",{"$nulls":4},{"$f":"LEN(H457)","v":17},{"$nulls":29},{"$f":"IF(LEFT(AB457, 13) = \"CONSTRAINT PK\", AB457, \"\")","v":""}]
["NO","속성명","컬럼명","형태","길이","비고",null,"논리명","PK/FK","NULL","물리명","형태","VOLT","TIBERO","COMMENT",{"$nulls":20},"COMMENT ON TABLE",{"$f":"H457&\" \"","v":"soitdemrgvhclinfo "},null," IS ",{"$f":"\"'\"&A457&\"'\"","v":"'- 긴급차량(EMRG_VHCL)'"},";",null,""]
[1,"긴급차량ID","EMRG_VHCL_ID","NUMBER",3,null,null,"긴급차량ID","PK/FK","NOT NULL","emrg_vhcl_id","NUMBER(5)","INTEGER","NUMBER(5)","긴급차량ID",null,"CREATE TABLE ",{"$f":"H457&\" (\"","v":"soitdemrgvhclinfo ("},{"$f":"K459&\" \"","v":"emrg_vhcl_id "},{"$f":"M459&\" \"","v":"INTEGER "},{"$f":"IF(J459=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(I459=\"PK\", I459=\"PK/FK\"), K459, \"\")","v":"emrg_vhcl_id"},{"$f":"IF(OR(I459=\"PK\", I459=\"PK/FK\"), \",\", \"\")","v":","},"CREATE TABLE ",{"$f":"H457&\" (\"","v":"soitdemrgvhclinfo ("},{"$f":"K459&\" \"","v":"emrg_vhcl_id "},{"$f":"N459&\" \"","v":"NUMBER(5) "},{"$f":"IF(J459=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(I459=\"PK\", I459=\"PK/FK\"), K459, \"\")","v":"emrg_vhcl_id"},{"$f":"IF(OR(I459=\"PK\", I459=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$H$457&\".\"","v":"soitdemrgvhclinfo."},{"$f":"K459","v":"emrg_vhcl_id"}," IS ",{"$f":"\"'\"&O459&\"'\"","v":"'긴급차량ID'"},";",null,""]
[2,"수집 일시","CLCT_DT","INTEGER","UTC",null,null,"수집유닉스시각","PK","NOT NULL","clct_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)","수집유닉스시각",null,null,null,"clct_unix_tm ","INTEGER ","NOT NULL",",",null,"clct_unix_tm","));",null,null,"clct_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"clct_unix_tm",")","COMMENT ON COLUMN ","soitdemrgvhclinfo.","clct_unix_tm"," IS ","'수집유닉스시각'",";",null,""]
[2,"수집일","CLCT_DATE","VARHCAR2",8,"YYYYMMDD",null,"수집일시",null,"NOT NULL","clct_dt","VARCHAR2(8)","VARCHAR(8)","VARCHAR2(8)","수집일시(yyyyMMdd)",null,null,null,{"$f":"K461","v":"clct_dt"},"VARCHAR(8) ","NOT NULL",",",null,"",null,null,null,"clct_dt ","VARCHAR2(8) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitdemrgvhclinfo.","clct_dt"," IS ","'수집일시(yyyyMMdd)'",";"]
[3,"인증 IMEI","ATHN_IMEI","VARCHAR2",20,null,null,"인증IMEI명",null,"NULL","cert_imei_nm","VARCHAR2(20)","VARCHAR(20)","VARCHAR2(20)","인증IMEI",null,null,null,{"$f":"K462&\" \"","v":"cert_imei_nm "},"VARCHAR(20) ","",",",null,{"$f":"IF(OR(I463=\"PK\", I463=\"PK/FK\"), K463, \"\")","v":""},{"$f":"IF(OR(I463=\"PK\", I463=\"PK/FK\"), \",\", \"\")","v":""},null,null,"cert_imei_nm ","VARCHAR2(20) ",{"$f":"IF(J463=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",null,null,{"$f":"IF(OR(I463=\"PK\", I463=\"PK/FK\"), K463, \"\")","v":""},{"$f":"IF(OR(I463=\"PK\", I463=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitdemrgvhclinfo.","cert_imei_nm"," IS ","'인증IMEI'",";",null,{"$f":"IF(LEFT(AB462, 13) = \"CONSTRAINT PK\", AB462, \"\")","v":""}]
[4,"차량번호","VHCL_NMBR","VARCHAR2",20,null,null,"차량번호명",null,"NULL","vhno_nm","VARCHAR2(20)","VARCHAR(20)","VARCHAR2(20)","차량번호명",null,null,null,"vhno_nm ","VARCHAR(20) ","",",",null,{"$f":"IF(OR(I466=\"PK\", I466=\"PK/FK\"), K466, \"\")","v":""},{"$f":"IF(OR(I466=\"PK\", I466=\"PK/FK\"), \",\", \"\")","v":""},null,null,"vhno_nm ","VARCHAR2(20) ",{"$f":"IF(J466=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",null,null,{"$f":"IF(OR(I466=\"PK\", I466=\"PK/FK\"), K466, \"\")","v":""},{"$f":"IF(OR(I466=\"PK\", I466=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitdemrgvhclinfo.","vhno_nm"," IS ","'차량번호명'",";",null,""]
[5,"단말기 모델 명","TRMN_MODEL_NM","VARCHAR2",20,null,null,"단말기모델명",null,"NULL","tmnl_modl_nm","VARCHAR2(20)","VARCHAR(20)","VARCHAR2(20)","단말기모델명",null,null,null,"tmnl_modl_nm ","VARCHAR(20) ","",",",null,"","",null,null,"tmnl_modl_nm ","VARCHAR2(20) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdemrgvhclinfo.","tmnl_modl_nm"," IS ","'단말기모델명'",";",null,""]
[6,"차량종류","VHCL_KIND","NUMBER",1,"0:엠블란스\n1:소방차\n2:경찰차","긴급차종코드(018)","긴급차량종류코드",null,"NULL","emrg_vhcl_kind_cd","CHAR(3)","VARCHAR(3)","VARCHAR2(3)","긴급차종코드(018)","긴급차량종류코드 (0:엠블란스, 1:소방차, 2:경찰차)",null,null,"emrg_vhcl_kind_cd ","VARCHAR(3) ","",",",{"$nulls":5},"emrg_vhcl_kind_cd ","VARCHAR2(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdemrgvhclinfo.","emrg_vhcl_kind_cd"," IS ","'긴급차종코드(018)'",";",null,""]
[7,"경로 ID","PATH_ID","NUMBER",3,null,null,"경로ID",null,"NULL","path_id","NUMBER(5)","INTEGER","NUMBER(5)","경로ID",null,null,null,"path_id ",{"$f":"M465&\" \"","v":"VARCHAR(3) "},"",",",{"$nulls":5},"path_id ","NUMBER(5) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdemrgvhclinfo.","path_id"," IS ","'경로ID'",";",null,""]
[8,"사용 여부","USE_YN","VARCHAR2",1,"Y:사용\nN:미사용","사용여부(003)","사용여부",null,"NULL","use_yn","CHAR(1)","VARCHAR(1)","VARCHAR2(1)","사용여부(003)","사용여부 (Y/N)",null,null,"use_yn ",{"$f":"M467&\" \"","v":"VARCHAR(1) "},"",",",{"$nulls":5},"use_yn ","VARCHAR2(1) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdemrgvhclinfo.","use_yn"," IS ","'사용여부(003)'",";",null,""]
[9,"앱 ID","APP_ID","NUMBER",3,null,null,"프로그램ID",null,"NULL","prgr_id","NUMBER(5)","INTEGER","NUMBER(5)","앱ID",null,null,null,"prgr_id ","INTEGER ","",",",{"$nulls":5},"prgr_id ","NUMBER(5) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdemrgvhclinfo.","prgr_id"," IS ","'앱ID'",";",null,""]
[10,"태블릿 ID","TABLET_ID","NUMBER",3,null,null,"장비ID",null,"NULL","eqpm_id","NUMBER(5)","INTEGER","NUMBER(5)","테블릿ID",null,null,null,"eqpm_id ","INTEGER ","",",",{"$nulls":5},"eqpm_id ","NUMBER(5) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitdemrgvhclinfo.","eqpm_id"," IS ","'테블릿ID'",";",null,""]
[11,"관리기관 ID","MNGMINTN_ID","NUMBER",3,null,null,"관리기관ID",null,"NULL","mng_inst_id","NUMBER(5)","INTEGER","NUMBER(5)","관리기관ID",null,null,null,"mng_inst_id ","INTEGER ","",",",{"$nulls":5},"mng_inst_id ","NUMBER(5) ",{"$f":"IF(J474=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",{"$nulls":4},"COMMENT ON COLUMN ","soitdemrgvhclinfo.","mng_inst_id"," IS ","'관리기관ID'",";",null,""]
[12,"적용 상태","APLY_STTS","VARCHAR2"," ",null,null,"적용상태코드",null,"NULL","aplcn_stts_cd","CHAR(1)","VARCHAR(1)","VARCHAR2(1)","적용상태코드",null,null,null,"aplcn_stts_cd ","VARCHAR(1) ","",",",{"$nulls":5},"aplcn_stts_cd ","VARCHAR2(1) ","",{"$f":"\") TABLESPACE \"&AF473&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_D002 NOLOGGING"},null,null,{"$f":"IF(OR(C471=\"PK\", C471=\"PK/FK\"), E471, \"\")","v":""},null,"COMMENT ON COLUMN ","soitdemrgvhclinfo.","aplcn_stts_cd"," IS ","'적용상태코드'",";",null,""]
[{"$nulls":18},{"$f":"CONCATENATE(W459:Y464)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AF472:AH472)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (clct_unix_tm) INTERVAL (86400) STORE IN (\"&AF473&\") (PARTITION BFR_\" & H457& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AF473&\");\"","v":"PARTITION BY RANGE (clct_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_D002) (PARTITION BFR_soitdemrgvhclinfo_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_D002);"},{"$f":"\"CREATE INDEX PK_\" & H457& \" ON \" & H457 & CONCATENATE(AG459:AI468) & \" LOCAL (PARTITION BFR_\" & H457 & \"_20221101 TABLESPACE \"&AG473&\") TABLESPACE \"&AG473&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & H457 & \" ADD CONSTRAINT PK_\" & H457 & \" PRIMARY KEY \" & CONCATENATE(AG459:AI468) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$error":"#VALUE!"}]
[{"$nulls":31},"SOIT_D08_D002","SOIT_I08_D002"]
["- 우선 신호 운영 교차로 (PRIO_SGNL_OPER_IXR)",{"$nulls":6},"soitdemrgsgnlpasghstr",{"$nulls":4},{"$f":"LEN(H474)","v":21},{"$nulls":29},{"$f":"IF(LEFT(AB474, 13) = \"CONSTRAINT PK\", AB474, \"\")","v":""}]
["NO","속성명","컬럼명","형태","길이","비고",null,"논리명","PK/FK","NULL","물리명","형태","VOLT","TIBERO","COMMENT",{"$nulls":20},"COMMENT ON TABLE",{"$f":"H474&\" \"","v":"soitdemrgsgnlpasghstr "},null," IS ",{"$f":"\"'\"&A474&\"'\"","v":"'- 우선 신호 운영 교차로 (PRIO_SGNL_OPER_IXR)'"},";",null,""]
[1,"서비스ID","SRVC_ID","VARCHAR2",12,null,null,"서비스ID","PK/FK","NOT NULL","srvc_id","VARCHAR2(20)","VARCHAR(20)","VARCHAR2(20)","서비스ID",null,"CREATE TABLE ",{"$f":"H474&\" (\"","v":"soitdemrgsgnlpasghstr ("},{"$f":"K476&\" \"","v":"srvc_id "},{"$f":"M476&\" \"","v":"VARCHAR(20) "},{"$f":"IF(J476=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(I476=\"PK\", I476=\"PK/FK\"), K476, \"\")","v":"srvc_id"},{"$f":"IF(OR(I476=\"PK\", I476=\"PK/FK\"), \",\", \"\")","v":","},"CREATE TABLE ",{"$f":"H474&\" (\"","v":"soitdemrgsgnlpasghstr ("},{"$f":"K476&\" \"","v":"srvc_id "},{"$f":"N476&\" \"","v":"VARCHAR2(20) "},{"$f":"IF(J476=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(I476=\"PK\", I476=\"PK/FK\"), K476, \"\")","v":"srvc_id"},{"$f":"IF(OR(I476=\"PK\", I476=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$H$474&\".\"","v":"soitdemrgsgnlpasghstr."},{"$f":"K476","v":"srvc_id"}," IS ",{"$f":"\"'\"&O476&\"'\"","v":"'서비스ID'"},";",null,""]
[2,"수집 일시","CLCT_DT","INTEGER","UTC",null,null,"수집유닉스시각","PK","NOT NULL","clct_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)","수집유닉스시각",null,null,null,"clct_unix_tm ","INTEGER ","NOT NULL",",",null,"clct_unix_tm",",",null,null,"clct_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"clct_unix_tm",",","COMMENT ON COLUMN ","soitdemrgsgnlpasghstr.","clct_unix_tm"," IS ","'수집유닉스시각'",";",null,""]
[2,"수집일","CLCT_DATE","VARHCAR2",8,"YYYYMMDD",null,"수집일시",null,"NOT NULL","clct_dt","VARCHAR2(8)","VARCHAR(8)","VARCHAR2(8)","수집일시(yyyyMMdd)",null,null,null,{"$f":"K478","v":"clct_dt"},"VARCHAR(8) ","NOT NULL",",",null,"",null,null,null,"clct_dt ","VARCHAR2(8) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitdemrgsgnlpasghstr.","clct_dt"," IS ","'수집일시(yyyyMMdd)'",";"]
[3,"교차로번호","IXR_NMBR","NUMBER",5,null,null,"현장교차로ID","PK/FK","NOT NULL","spot_ints_id","NUMBER(5)","INTEGER","NUMBER(5)","현장교차로ID",null,null,null,{"$f":"K479&\" \"","v":"spot_ints_id "},"INTEGER ","NOT NULL",",",null,"spot_ints_id",{"$f":"IF(OR(I479=\"PK\", I479=\"PK/FK\"), \",\", \"\")","v":","},null,null,"spot_ints_id ","NUMBER(5) ","NOT NULL",",",null,null,"spot_ints_id",{"$f":"IF(OR(I479=\"PK\", I479=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ","soitdemrgsgnlpasghstr.","spot_ints_id"," IS ","'현장교차로ID'",";",null,{"$f":"IF(LEFT(AB479, 13) = \"CONSTRAINT PK\", AB479, \"\")","v":""}]
[4,"교차로순서","IXR_ORD","NUMBER",2,null,null,"통과순서번호","PK","NOT NULL","pasg_seq_no","NUMBER(2)","INTEGER","NUMBER(2)","통과순서번호",null,null,null,"pasg_seq_no ","INTEGER ","NOT NULL",",",null,"pasg_seq_no","));",null,null,"pasg_seq_no ","NUMBER(2) ","NOT NULL",{"$f":"\") TABLESPACE \"&AF482&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_D002 NOLOGGING"},null,null,"pasg_seq_no",")","COMMENT ON COLUMN ","soitdemrgsgnlpasghstr.","pasg_seq_no"," IS ","'통과순서번호'",";",null,""]
[{"$nulls":18},{"$f":"CONCATENATE(W476:Y480)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AF481:AH481)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (clct_unix_tm) INTERVAL (86400) STORE IN (\"&AF482&\") (PARTITION BFR_\" & H474& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AF482&\");\"","v":"PARTITION BY RANGE (clct_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_D002) (PARTITION BFR_soitdemrgsgnlpasghstr_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_D002);"},{"$f":"\"CREATE INDEX PK_\" & H474& \" ON \" & H474 & CONCATENATE(AG476:AI480) & \" LOCAL (PARTITION BFR_\" & H474 & \"_20221101 TABLESPACE \"&AG482&\") TABLESPACE \"&AG482&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & H474 & \" ADD CONSTRAINT PK_\" & H474 & \" PRIMARY KEY \" & CONCATENATE(AG476:AI480) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$error":"#VALUE!"}]
[{"$nulls":31},"SOIT_D08_D002","SOIT_I08_D002"]
["- 긴급차량 목적지 마스터 정보 (EMRG_VHCL_DEST_INFR)",{"$nulls":6},"soitdemrgdestinfo",{"$nulls":4},{"$f":"LEN(H483)","v":17},{"$nulls":29},{"$f":"IF(LEFT(AB483, 13) = \"CONSTRAINT PK\", AB483, \"\")","v":""}]
["NO","속성명","컬럼명","형태","길이","비고",null,"논리명","PK/FK","NULL","물리명","형태","VOLT","TIBERO","COMMENT",{"$nulls":20},"COMMENT ON TABLE",{"$f":"H483&\" \"","v":"soitdemrgdestinfo "},null," IS ",{"$f":"\"'\"&A483&\"'\"","v":"'- 긴급차량 목적지 마스터 정보 (EMRG_VHCL_DEST_INFR)'"},";",null,""]
[1,"목적지 ID","DEST_ID","NUMBER",2,null,null,"목적지ID","PK","NOT NULL","dest_id","NUMBER(5)","INTEGER","NUMBER(5)","목적지ID",null,"CREATE TABLE ",{"$f":"H483&\" (\"","v":"soitdemrgdestinfo ("},{"$f":"K485&\" \"","v":"dest_id "},{"$f":"M485&\" \"","v":"INTEGER "},{"$f":"IF(J485=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(I485=\"PK\", I485=\"PK/FK\"), K485, \"\")","v":"dest_id"},{"$f":"IF(OR(I485=\"PK\", I485=\"PK/FK\"), \",\", \"\")","v":","},"CREATE TABLE ",{"$f":"H483&\" (\"","v":"soitdemrgdestinfo ("},{"$f":"K485&\" \"","v":"dest_id "},{"$f":"N485&\" \"","v":"NUMBER(5) "},{"$f":"IF(J485=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(I485=\"PK\", I485=\"PK/FK\"), K485, \"\")","v":"dest_id"},{"$f":"IF(OR(I485=\"PK\", I485=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$H$483&\".\"","v":"soitdemrgdestinfo."},{"$f":"K485","v":"dest_id"}," IS ",{"$f":"\"'\"&O485&\"'\"","v":"'목적지ID'"},";",null,""]
[2,"수집 일시","CLCT_DT","INTEGER","UTC",null,null,"수집유닉스시각","PK","NOT NULL","clct_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)","수집유닉스시각",null,null,null,"clct_unix_tm ","INTEGER ","NOT NULL",",",null,"clct_unix_tm","));",null,null,"clct_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"clct_unix_tm",")","COMMENT ON COLUMN ","soitdemrgdestinfo.","clct_unix_tm"," IS ","'수집유닉스시각'",";",null,""]
[2,"수집일","CLCT_DATE","VARHCAR2",8,"YYYYMMDD",null,"수집일시",null,"NOT NULL","clct_dt","VARCHAR2(8)","VARCHAR(8)","VARCHAR2(8)","수집일시(yyyyMMdd)",null,null,null,{"$f":"K487","v":"clct_dt"},"VARCHAR(8) ","NOT NULL",",",null,"",null,null,null,"clct_dt ","VARCHAR2(8) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitdemrgdestinfo.","clct_dt"," IS ","'수집일시(yyyyMMdd)'",";"]
[3,"목적지 명","DEST_NM","VARCHAR2",32,null,null,"목적지명",null,null,"dest_nm","VARCHAR2(50)","VARCHAR(50)","VARCHAR2(50)","목적지명",null,null,null,{"$f":"K488&\" \"","v":"dest_nm "},"VARCHAR(50) ","",",",null,"",{"$f":"IF(OR(I488=\"PK\", I488=\"PK/FK\"), \",\", \"\")","v":""},null,null,"dest_nm ","VARCHAR2(50) ","",",",null,null,"",{"$f":"IF(OR(I488=\"PK\", I488=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitdemrgdestinfo.","dest_nm"," IS ","'목적지명'",";",null,{"$f":"IF(LEFT(AB488, 13) = \"CONSTRAINT PK\", AB488, \"\")","v":""}]
[4,"X 좌표","X_CRDN","NUMBER",10,null,null,"목적지경도",null,null,"dest_lot","NUMBER(13,10)","FLOAT","NUMBER(13,10)","목적지경도",null,null,null,"dest_lot ","FLOAT ","",",",null,"","",null,null,"dest_lot ","NUMBER(13,10) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdemrgdestinfo.","dest_lot"," IS ","'목적지경도'",";",null,""]
[5,"Y 좌표","Y_CRDN","NUMBER",10,null,null,"목적지위도",null,null,"dest_lat","NUMBER(12,10)","FLOAT","NUMBER(12,10)","목적지위도",null,null,null,"dest_lat ","FLOAT ","",",",null,"","",null,null,"dest_lat ","NUMBER(12,10) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdemrgdestinfo.","dest_lat"," IS ","'목적지위도'",";",null,""]
[6,"목적지 상세 내용","DEST_DETL_CONT","VARCHAR2",255,null,null,"비고",null,null,"rmrk","VARCHAR2(2000)","VARCHAR(2000)","VARCHAR2(2000)","비고",null,null,null,"rmrk ","VARCHAR(2000) ","",",",null,"","",null,null,"rmrk ","VARCHAR2(2000) ","",{"$f":"\") TABLESPACE \"&AF493&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_D002 NOLOGGING"},null,null,"","","COMMENT ON COLUMN ","soitdemrgdestinfo.","rmrk"," IS ","'비고'",";",null,""]
[{"$nulls":18},{"$f":"CONCATENATE(W485:Y491)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AF492:AH492)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (clct_unix_tm) INTERVAL (86400) STORE IN (\"&AF493&\") (PARTITION BFR_\" & H483& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AF493&\");\"","v":"PARTITION BY RANGE (clct_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_D002) (PARTITION BFR_soitdemrgdestinfo_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_D002);"},{"$f":"\"CREATE INDEX PK_\" & H483& \" ON \" & H483 & CONCATENATE(AG485:AI490) & \" LOCAL (PARTITION BFR_\" & H483 & \"_20221101 TABLESPACE \"&AG493&\") TABLESPACE \"&AG493&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & H483 & \" ADD CONSTRAINT PK_\" & H483 & \" PRIMARY KEY \" & CONCATENATE(AG485:AI490) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$error":"#VALUE!"}]
[{"$nulls":31},"SOIT_D08_D002","SOIT_I08_D002"]
["- 우선신호 안내경로 정보 (PRIO_SGNL_PATH)",{"$nulls":6},"soitdemrgvhclpathinfo",{"$nulls":4},{"$f":"LEN(H494)","v":21},{"$nulls":29},{"$f":"IF(LEFT(AB494, 13) = \"CONSTRAINT PK\", AB494, \"\")","v":""}]
["NO","속성명","컬럼명","형태","길이","비고",null,"논리명","PK/FK","NULL","물리명","형태","VOLT","TIBERO","COMMENT",{"$nulls":20},"COMMENT ON TABLE",{"$f":"H494&\" \"","v":"soitdemrgvhclpathinfo "},null," IS ",{"$f":"\"'\"&A494&\"'\"","v":"'- 우선신호 안내경로 정보 (PRIO_SGNL_PATH)'"},";",null,""]
[1,"서비스 ID","SRVC_ID","VARCHAR2",12,null,null,"서비스 ID","PK","NOT NULL","srvc_id","VARCHAR2(20)",null,"VARCHAR2(20)","서비스 ID",{"$nulls":10},"CREATE TABLE ",{"$f":"H494&\" (\"","v":"soitdemrgvhclpathinfo ("},{"$f":"K496&\" \"","v":"srvc_id "},{"$f":"N496&\" \"","v":"VARCHAR2(20) "},{"$f":"IF(J496=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(I496=\"PK\", I496=\"PK/FK\"), K496, \"\")","v":"srvc_id"},{"$f":"IF(OR(I496=\"PK\", I496=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$H$494&\".\"","v":"soitdemrgvhclpathinfo."},{"$f":"K496","v":"srvc_id"}," IS ",{"$f":"\"'\"&O496&\"'\"","v":"'서비스 ID'"},";",null,""]
[2,"수집 일시","CLCT_DT","INTEGER","UTC",null,null,"수집유닉스시각","PK","NOT NULL","clct_unix_tm","NUMBER(10)",null,"NUMBER(10)","수집유닉스시각",{"$nulls":12},"clct_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"clct_unix_tm",")","COMMENT ON COLUMN ","soitdemrgvhclpathinfo.","clct_unix_tm"," IS ","'수집유닉스시각'",";",null,""]
[2,"수집일","CLCT_DATE","VARHCAR2",8,"YYYYMMDD",null,"수집일시",null,"NOT NULL","clct_dt","VARCHAR2(8)","VARCHAR(8)","VARCHAR2(8)","수집일시(yyyyMMdd)",{"$nulls":8},{"$f":"IF(OR(I498=\"PK\", I498=\"PK/FK\"), K498, \"\")","v":""},null,null,null,"clct_dt ","VARCHAR2(8) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitdemrgvhclpathinfo.","clct_dt"," IS ","'수집일시(yyyyMMdd)'",";"]
[3,"경로","PATH","CLOB",null,null,null,"경로정보",null,null,"path_info","CLOB",null,"CLOB","경로정보 (CLOB)",{"$nulls":12},"path_info ","CLOB ","",{"$f":"\") TABLESPACE \"&AF501&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_D002 NOLOGGING"},null,null,"",{"$f":"IF(OR(I499=\"PK\", I499=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitdemrgvhclpathinfo.","path_info"," IS ","'경로정보 (CLOB)'",";",null,{"$f":"IF(LEFT(AB499, 13) = \"CONSTRAINT PK\", AB499, \"\")","v":""}]
[{"$nulls":27},{"$f":"CONCATENATE(AF500:AH500)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (clct_unix_tm) INTERVAL (86400) STORE IN (\"&AF501&\") (PARTITION BFR_\" & H494& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AF501&\");\"","v":"PARTITION BY RANGE (clct_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_D002) (PARTITION BFR_soitdemrgvhclpathinfo_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_D002);"},{"$f":"\"CREATE INDEX PK_\" & H494& \" ON \" & H494 & CONCATENATE(AG496:AI499) & \" LOCAL (PARTITION BFR_\" & H494 & \"_20221101 TABLESPACE \"&AG501&\") TABLESPACE \"&AG501&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & H494 & \" ADD CONSTRAINT PK_\" & H494 & \" PRIMARY KEY \" & CONCATENATE(AG496:AI498) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$error":"#VALUE!"}]
[{"$nulls":31},"SOIT_D08_D002","SOIT_I08_D002"]
["- 긴급차량 기관정보 (EMRG_VHCL_INTN)",{"$nulls":6},"soitdemrgintninfo",{"$nulls":4},{"$f":"LEN(H502)","v":17},{"$nulls":29},{"$f":"IF(LEFT(AB502, 13) = \"CONSTRAINT PK\", AB502, \"\")","v":""}]
["NO","속성명","컬럼명","형태","길이","비고",null,"논리명","PK/FK","NULL","물리명","형태","VOLT","TIBERO","COMMENT",{"$nulls":20},"COMMENT ON TABLE",{"$f":"H502&\" \"","v":"soitdemrgintninfo "},null," IS ",{"$f":"\"'\"&A502&\"'\"","v":"'- 긴급차량 기관정보 (EMRG_VHCL_INTN)'"},";",null,""]
[1,"관리기관 ID","MNGMINTN_ID","NUMBER",3,null,null,"관리기관ID","PK","NOT NULL","mng_inst_id","NUMBER(5)","INTEGER","NUMBER(5)","관리기관ID",null,"CREATE TABLE ",{"$f":"H502&\" (\"","v":"soitdemrgintninfo ("},{"$f":"K504&\" \"","v":"mng_inst_id "},{"$f":"M504&\" \"","v":"INTEGER "},{"$f":"IF(J504=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(I504=\"PK\", I504=\"PK/FK\"), K504, \"\")","v":"mng_inst_id"},{"$f":"IF(OR(I504=\"PK\", I504=\"PK/FK\"), \",\", \"\")","v":","},"CREATE TABLE ",{"$f":"H502&\" (\"","v":"soitdemrgintninfo ("},{"$f":"K504&\" \"","v":"mng_inst_id "},{"$f":"N504&\" \"","v":"NUMBER(5) "},{"$f":"IF(J504=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(I504=\"PK\", I504=\"PK/FK\"), K504, \"\")","v":"mng_inst_id"},{"$f":"IF(OR(I504=\"PK\", I504=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$H$502&\".\"","v":"soitdemrgintninfo."},{"$f":"K504","v":"mng_inst_id"}," IS ",{"$f":"\"'\"&O504&\"'\"","v":"'관리기관ID'"},";",null,""]
[2,"수집 일시","CLCT_DT","INTEGER","UTC",null,null,"수집유닉스시각","PK","NOT NULL","clct_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)","수집유닉스시각",null,null,null,"clct_unix_tm ","INTEGER ","NOT NULL",",",null,"clct_unix_tm","));",null,null,"clct_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"clct_unix_tm",")","COMMENT ON COLUMN ","soitdemrgintninfo.","clct_unix_tm"," IS ","'수집유닉스시각'",";",null,""]
[2,"수집일","CLCT_DATE","VARHCAR2",8,"YYYYMMDD",null,"수집일시",null,"NOT NULL","clct_dt","VARCHAR2(8)","VARCHAR(8)","VARCHAR2(8)","수집일시(yyyyMMdd)",null,null,null,{"$f":"K506","v":"clct_dt"},"VARCHAR(8) ","NOT NULL",",",null,"",null,null,null,"clct_dt ","VARCHAR2(8) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitdemrgintninfo.","clct_dt"," IS ","'수집일시(yyyyMMdd)'",";"]
[3,"관리기관 명","MNGMINTN_NM","VARCHAR2",30,null,null,"관리기관명",null,null,"mng_inst_nm","VARCHAR2(30)","VARCHAR(30)","VARCHAR2(30)","관리기관명",null,null,null,{"$f":"K507&\" \"","v":"mng_inst_nm "},"VARCHAR(30) ","",",",null,"",{"$f":"IF(OR(I507=\"PK\", I507=\"PK/FK\"), \",\", \"\")","v":""},null,null,"mng_inst_nm ","VARCHAR2(30) ","",",",null,null,"",{"$f":"IF(OR(I507=\"PK\", I507=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitdemrgintninfo.","mng_inst_nm"," IS ","'관리기관명'",";",null,{"$f":"IF(LEFT(AB507, 13) = \"CONSTRAINT PK\", AB507, \"\")","v":""}]
[4,"X 좌표","X_CRDN","NUMBER",10,null,null,"기관경도",null,null,"inst_lot","NUMBER(13,10)","FLOAT","NUMBER(13,10)","기관경도",null,null,null,"inst_lot ","FLOAT ","",",",null,"","",null,null,"inst_lot ","NUMBER(13,10) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdemrgintninfo.","inst_lot"," IS ","'기관경도'",";",null,""]
[5,"Y 좌표","Y_CRDN","NUMBER",10,null,null,"기관위도",null,null,"inst_lat","NUMBER(12,10)","FLOAT","NUMBER(12,10)","기관위도",null,null,null,"inst_lat ","FLOAT ","",",",null,"","",null,null,"inst_lat ","NUMBER(12,10) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdemrgintninfo.","inst_lat"," IS ","'기관위도'",";",null,""]
[6,"사용 여부","USE_YN","VARCHAR2",1,null,null,"비고",null,null,"rmrk","VARCHAR2(2000)","VARCHAR(2000)","VARCHAR2(2000)","비고",null,null,null,"rmrk ","VARCHAR(2000) ","",",",null,"","",null,null,"rmrk ","VARCHAR2(2000) ","",",",null,null,"","","COMMENT ON COLUMN ","soitdemrgintninfo.","rmrk"," IS ","'비고'",";",null,""]
[7,"관리기관 설명","MNGMINTN_EXPL","VARCHAR2",255,null,null,"사용여부",null,null,"use_yn","CHAR(1)","VARCHAR(1)","CHAR(1)","사용여부(003)","사용여부 (Y/N)",null,null,"use_yn ","VARCHAR(1) ","",",",null,"","",null,null,"use_yn ","CHAR(1) ","",{"$f":"\") TABLESPACE \"&AF513&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_D002 NOLOGGING"},null,null,"","","COMMENT ON COLUMN ","soitdemrgintninfo.","use_yn"," IS ","'사용여부(003)'",";",null,""]
[{"$nulls":18},{"$f":"CONCATENATE(W504:Y511)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AF512:AH512)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (clct_unix_tm) INTERVAL (86400) STORE IN (\"&AF513&\") (PARTITION BFR_\" & H502& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AF513&\");\"","v":"PARTITION BY RANGE (clct_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_D002) (PARTITION BFR_soitdemrgintninfo_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_D002);"},{"$f":"\"CREATE INDEX PK_\" & H502& \" ON \" & H502 & CONCATENATE(AG504:AI509) & \" LOCAL (PARTITION BFR_\" & H502 & \"_20221101 TABLESPACE \"&AG513&\") TABLESPACE \"&AG513&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & H502 & \" ADD CONSTRAINT PK_\" & H502 & \" PRIMARY KEY \" & CONCATENATE(AG504:AI510) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$error":"#VALUE!"}]
[{"$nulls":31},"SOIT_D08_D002","SOIT_I08_D002"]

{"sheet":"센터(시스템운영)","index":6,"n_rows":143,"n_cols":48,"rows_kept":143,"cut":false,"hidden":false,"merged":[[11,0,11,19],[11,21,11,26],[11,30,11,39],[11,40,11,45],[12,0,12,9],[22,0,22,19],[23,0,23,9],[37,0,37,19],[38,0,38,9],[49,0,49,19],[50,0,50,9],[63,0,63,19],[64,0,64,9],[69,0,69,19],[108,0,108,19],[133,0,133,19],[134,0,134,9],[70,0,70,9],[78,0,78,19],[79,0,79,9],[88,0,88,19],[89,0,89,9],[96,0,96,19],[97,0,97,9],[109,0,109,9],[115,0,115,19],[116,0,116,9],[123,0,123,19],[124,0,124,9]]}
[null,"최적화 반복횟수 코드 테이블"]
[null,"연동그룹 시각화를 위한 기초데이터를 postgregis 에서 가공해서 생성한 정보",{"$nulls":7},"postgregis 설치해서 거기에서 아예 가져올까?"]
[null,"도로에 대한 postgregis 가공테이블"]
[null,"신호등정보테이블(교차로id, 신호등 순번, 신호등 이미지 구분, 신호등방향각도, 신호등방향코드, x, y)  postgregis 가공테이블",{"$nulls":7},"화면에서 어떻게 표현할거?"]
[null,"그 외 postgregis 가공테이블 정의 필요"]
[null,"글로벌브릿지 제공용 뷰"]
[null,"tod상의 이동류코드와  이동류 이미지 코드 매칭 테이블또는 코드 정보 필요",{"$nulls":7},"front 단에서  내부 json 파일로 정의해도 되지않을까?"]
[]
[]
[]
[]
["공해차량 단속지점 정보 ",{"$nulls":29},"TIBERO DDL",{"$nulls":9},"COMMENTS"]
["soitcpltnvhclcrdnints",{"$nulls":10},{"$f":"LEN(A13)","v":21}]
["NO","속성명","컬럼명","PK/FK","NULL","형태","VOLT","TIBERO","길이","비고",null,null,"교차로ID","카메라순번","카메라 ID","여부",{"$nulls":24},"COMMENT ON TABLE",{"$f":"A13","v":"soitcpltnvhclcrdnints"},null," IS ",{"$f":"\"'\"&A12&\"'\"","v":"'공해차량 단속지점 정보 '"},";"]
[1,"현장교차로ID","spot_ints_id","PK/FK","NOT NULL","NUMBER(5)","INTEGER","NUMBER(5)",5,"현장교차로ID",null,null,3039,3,"3039_05_02","Y",{"$nulls":14},"CREATE TABLE ",{"$f":"A13&\" (\"","v":"soitcpltnvhclcrdnints ("},{"$f":"C15&\" \"","v":"spot_ints_id "},{"$f":"H15&\" \"","v":"NUMBER(5) "},{"$f":"IF(E15=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","CONSTRAINT ",{"$f":"\"PK_\"&A13&\" PRIMARY KEY (\"","v":"PK_soitcpltnvhclcrdnints PRIMARY KEY ("},{"$f":"IF(OR(D15=\"PK\", D15=\"PK/FK\"), C15, \"\")","v":"spot_ints_id"},{"$f":"IF(OR(D15=\"PK\", D15=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"A$13&\".\"","v":"soitcpltnvhclcrdnints."},{"$f":"C15","v":"spot_ints_id"}," IS ",{"$f":"\"'\"&J15&\"'\"","v":"'현장교차로ID'"},";"]
[2,"현장카메라위치ID","spot_camr_locn_id","PK/FK","NOT NULL","VARCHAR2(64)","VARCHAR(64)","VARCHAR2(64)",null,"현장카메라위치ID",null,null,4061,1,"4061_07_04","Y",{"$nulls":16},"spot_camr_locn_id ","VARCHAR2(64) ","NOT NULL",",",null,null,"spot_camr_locn_id",",","COMMENT ON COLUMN ","soitcpltnvhclcrdnints.","spot_camr_locn_id"," IS ","'현장카메라위치ID'",";"]
[3,"현장카메라ID","spot_camr_id","PK/FK","NOT NULL","VARCHAR2(10)","VARCHAR(10)","VARCHAR2(10)",10,"현장카메라ID",null,null,5012,2,"5012_03_08","Y",{"$nulls":16},"spot_camr_id ","VARCHAR2(10) ","NOT NULL",",",null,null,"spot_camr_id",{"$f":"\") using index tablespace \" &AL22  & \") TABLESPACE \" & AK22&\";\"","v":") using index tablespace SOIT_I08_M001) TABLESPACE SOIT_D08_M001;"},"COMMENT ON COLUMN ","soitcpltnvhclcrdnints.","spot_camr_id"," IS ","'현장카메라ID'",";"]
[4,"공해차량 단속지점 여부","crdn_pont_yn",null,"NOT NULL","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",1,"공해차량 단속지점 여부(Y/N)","단속지점",null,5034,3,"5034_05_02","Y",{"$nulls":16},"crdn_pont_yn ","VARCHAR2(1) ","NOT NULL",",",null,null,"",{"$f":"IF(OR(D18=\"PK\", D18=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitcpltnvhclcrdnints.","crdn_pont_yn"," IS ","'공해차량 단속지점 여부(Y/N)'",";"]
[5,"등록유닉스시각","reg_unix_tm",null,"NOT NULL","NUMBER(10)","INTEGER","NUMBER(10)",null,"등록유닉스시각",null,null,6047,2,"6047_07_04","Y",{"$nulls":16},"reg_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitcpltnvhclcrdnints.","reg_unix_tm"," IS ","'등록유닉스시각'",";"]
[6,"변경유닉스시각","chg_unix_tm",null,"NOT NULL","NUMBER(10)","INTEGER","NUMBER(10)",null,"변경유닉스시각",null,null,5128,1,"5128_07_04","Y",{"$nulls":16},"chg_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitcpltnvhclcrdnints.","chg_unix_tm"," IS ","'변경유닉스시각'",";"]
[{"$nulls":12},"공해단속지점 - 스마트교차로",{"$nulls":19},{"$f":"CONCATENATE(AK15:AN19)","v":{"$error":"#VALUE!"}}]
[{"$nulls":36},"SOIT_D08_M001","SOIT_I08_M001"]
["스마트교차로연결정보"]
["soitasmrtintscnctinfo",{"$nulls":10},{"$f":"LEN(A24)","v":21}]
["NO","속성명","컬럼명","PK/FK","NULL","형태","VOLT(구현안함)","TIBERO","길이","비고",{"$nulls":30},"COMMENT ON TABLE",{"$f":"A24","v":"soitasmrtintscnctinfo"},null," IS ",{"$f":"\"'\"&A23&\"'\"","v":"'스마트교차로연결정보'"},";"]
[1,"현장교차로ID","spot_ints_id","PK/FK","NOT NULL","NUMBER(5)","INTEGER","NUMBER(5)",null,"현장교차로ID",null,null,"BI용 집계 용도 /그외 용도",{"$nulls":17},"CREATE TABLE ",{"$f":"A24&\" (\"","v":"soitasmrtintscnctinfo ("},{"$f":"C26&\" \"","v":"spot_ints_id "},{"$f":"H26&\" \"","v":"NUMBER(5) "},{"$f":"IF(E26=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","CONSTRAINT ",{"$f":"\"PK_\"&A24&\" PRIMARY KEY (\"","v":"PK_soitasmrtintscnctinfo PRIMARY KEY ("},{"$f":"IF(OR(D26=\"PK\", D26=\"PK/FK\"), C26, \"\")","v":"spot_ints_id"},{"$f":"IF(OR(D26=\"PK\", D26=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"A$24&\".\"","v":"soitasmrtintscnctinfo."},{"$f":"C26","v":"spot_ints_id"}," IS ",{"$f":"\"'\"&J26&\"'\"","v":"'현장교차로ID'"},";"]
[2,"현장카메라위치ID","spot_camr_locn_id","PK/FK","NOT NULL","VARCHAR2(64)","VARCHAR(64)","VARCHAR2(64)",null,"현장카메라위치ID",{"$nulls":22},"spot_camr_locn_id ","VARCHAR2(64) ","NOT NULL",",",null,null,"spot_camr_locn_id",",","COMMENT ON COLUMN ","soitasmrtintscnctinfo.","spot_camr_locn_id"," IS ","'현장카메라위치ID'",";"]
[3,"현장카메라ID","spot_camr_id","PK/FK","NOT NULL","VARCHAR2(10)","VARCHAR(10)","VARCHAR2(10)",null,"현장카메라ID",{"$nulls":22},"spot_camr_id ","VARCHAR2(10) ","NOT NULL",",",null,null,"spot_camr_id",",","COMMENT ON COLUMN ","soitasmrtintscnctinfo.","spot_camr_id"," IS ","'현장카메라ID'",";"]
[4,"진입이동류코드","entr_mvmt_cd","PK","NOT NULL","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",null,"동인 제공 이동류번호","방위(006)",{"$nulls":21},"entr_mvmt_cd ","VARCHAR2(2) ","NOT NULL",",",null,null,"entr_mvmt_cd",",","COMMENT ON COLUMN ","soitasmrtintscnctinfo.","entr_mvmt_cd"," IS ","'동인 제공 이동류번호'",";"]
[5,"진입 현장교차로ID","entr_spot_ints_id",null,"NOT NULL","VARCHAR2(300)","VARCHAR2(300)","VARCHAR2(300)",null,"진입 현장교차로ID",{"$nulls":22},"entr_spot_ints_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"","","COMMENT ON COLUMN ","soitasmrtintscnctinfo.","entr_spot_ints_id"," IS ","'진입 현장교차로ID'",";"]
[6,"진입비고","entr_rmrk",null,"NULL","VARCHAR2(200)","VARCHAR(200)","VARCHAR2(200)",null,"진입기타정보",{"$nulls":22},"entr_rmrk ","VARCHAR2(200) ","",",",null,null,"","","COMMENT ON COLUMN ","soitasmrtintscnctinfo.","entr_rmrk"," IS ","'진입기타정보'",";"]
[7,"회전유형명","turn_type_nm","PK","NOT NULL","VARCHAR2(30)","VARCHAR(30)","VARCHAR2(30)",null,"글로벌 제공 회전유형명","회전유형코드(700)",{"$nulls":21},"turn_type_nm ","VARCHAR2(30) ","NOT NULL",",",null,null,"turn_type_nm",",","COMMENT ON COLUMN ","soitasmrtintscnctinfo.","turn_type_nm"," IS ","'글로벌 제공 회전유형명'",";"]
[8,"진출이동류코드","exit_mvmt_cd","PK","NOT NULL","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",null,"동인 제공 이동류 번호","방위(006)",{"$nulls":21},"exit_mvmt_cd ","VARCHAR2(2) ","NOT NULL",",",null,null,"exit_mvmt_cd",{"$f":"\") using index tablespace \" &AL37  & \") TABLESPACE \" & AK37&\";\"","v":") using index tablespace SOIT_I08_M001) TABLESPACE SOIT_D08_M001;"},"COMMENT ON COLUMN ","soitasmrtintscnctinfo.","exit_mvmt_cd"," IS ","'동인 제공 이동류 번호'",";"]
[9,"진출 현장교차로ID","exit_spot_ints_id",null,"NOT NULL","VARCHAR2(300)","VARCHAR2(300)","VARCHAR2(300)",null,"진출 현장교차로ID",{"$nulls":22},"exit_spot_ints_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"",{"$f":"IF(OR(D34=\"PK\", D34=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitasmrtintscnctinfo.","exit_spot_ints_id"," IS ","'진출 현장교차로ID'",";"]
[10,"진출비고","exit_rmrk",null,"NULL","VARCHAR2(200)","VARCHAR(200)","VARCHAR2(200)",null,"진출기타정보",{"$nulls":22},"exit_rmrk ","VARCHAR2(200) ","",",",null,null,"","","COMMENT ON COLUMN ","soitasmrtintscnctinfo.","exit_rmrk"," IS ","'진출기타정보'",";"]
[{"$nulls":32},{"$f":"CONCATENATE(AK25:AN35)","v":{"$error":"#VALUE!"}}]
[{"$nulls":36},"SOIT_D08_M001","SOIT_I08_M001"]
["교통시간대정보"]
["soitctrfctmslinfo"]
["NO","속성명","컬럼명","PK/FK","NULL","형태","VOLT(구현안함)","TIBERO","길이","비고",{"$nulls":30},"COMMENT ON TABLE",{"$f":"A39","v":"soitctrfctmslinfo"},null," IS ",{"$f":"\"'\"&A38&\"'\"","v":"'교통시간대정보'"},";"]
[1,"시간대코드","tmsl_cd","PK","NOT NULL","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",null,"교통시간대코드(050)",null,null,"첨두/비첨두 관리 마스터",{"$nulls":17},"CREATE TABLE ",{"$f":"A39&\" (\"","v":"soitctrfctmslinfo ("},{"$f":"C41&\" \"","v":"tmsl_cd "},{"$f":"H41&\" \"","v":"VARCHAR2(2) "},{"$f":"IF(E41=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","CONSTRAINT ",{"$f":"\"PK_\"&A39&\" PRIMARY KEY (\"","v":"PK_soitctrfctmslinfo PRIMARY KEY ("},{"$f":"IF(OR(D41=\"PK\", D41=\"PK/FK\"), C41, \"\")","v":"tmsl_cd"},{"$f":"\") using index tablespace \" &AL50& \") TABLESPACE \" &AK50&\";\"","v":") using index tablespace SOIT_I08_M001) TABLESPACE SOIT_D08_M001;"},"COMMENT ON COLUMN ",{"$f":"A$39&\".\"","v":"soitctrfctmslinfo."},{"$f":"C41","v":"tmsl_cd"}," IS ",{"$f":"\"'\"&J41&\"'\"","v":"'교통시간대코드(050)'"},";"]
[2,"첨두여부","peak_yn",null,"NOT NULL","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",null,"첨두비첨두여부(Y/N)","첨두비첨두(002)",{"$nulls":21},"peak_yn ","VARCHAR2(1) ","NOT NULL",",",null,null,"",{"$f":"IF(OR(D42=\"PK\", D42=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitctrfctmslinfo.","peak_yn"," IS ","'첨두비첨두여부(Y/N)'",";"]
[3,"시작시","bgng_hh",null,"NOT NULL","NUMBER(2)","INTEGER","NUMBER(2)",null,"시작 시(HH24)",{"$nulls":22},"bgng_hh ","NUMBER(2) ","NOT NULL",",",null,null,"","","COMMENT ON COLUMN ","soitctrfctmslinfo.","bgng_hh"," IS ","'시작 시(HH24)'",";"]
[4,"시작분","bgng_mi",null,"NOT NULL","NUMBER(2)","INTEGER","NUMBER(2)",null,"시작 분(mm)",{"$nulls":22},"bgng_mi ","NUMBER(2) ","NOT NULL",",",null,null,"","","COMMENT ON COLUMN ","soitctrfctmslinfo.","bgng_mi"," IS ","'시작 분(mm)'",";"]
[5,"종료시","end_hh",null,"NOT NULL","NUMBER(2)","INTEGER","NUMBER(2)",null,"종료 시(HH24)",{"$nulls":22},"end_hh ","NUMBER(2) ","NOT NULL",",",null,null,"","","COMMENT ON COLUMN ","soitctrfctmslinfo.","end_hh"," IS ","'종료 시(HH24)'",";"]
[6,"종료분","end_mi",null,"NOT NULL","NUMBER(2)","INTEGER","NUMBER(2)",null,"종료 분(mm)",{"$nulls":22},"end_mi ","NUMBER(2) ","NOT NULL",",",null,null,"","","COMMENT ON COLUMN ","soitctrfctmslinfo.","end_mi"," IS ","'종료 분(mm)'",";"]
[7,"사용여부","use_yn",null,"NOT NULL","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",null,"사용여부 (Y/N)","사용여부(003)",{"$nulls":21},"use_yn ","VARCHAR2(1) ","NOT NULL",",",null,null,"","","COMMENT ON COLUMN ","soitctrfctmslinfo.","use_yn"," IS ","'사용여부 (Y/N)'",";"]
[8,"비고","rmrk",null,"NULL","VARCHAR2(200)","VARCHAR(200)","VARCHAR2(200)",null,"비고",{"$nulls":22},"rmrk ","VARCHAR2(200) ","",",",null,null,"","","COMMENT ON COLUMN ","soitctrfctmslinfo.","rmrk"," IS ","'비고'",";"]
[{"$nulls":32},{"$f":"CONCATENATE(AK40:AN48)","v":{"$error":"#VALUE!"}},{"$nulls":14},{"$f":"IF(LEFT(AG49, 13) = \"CONSTRAINT PK\", AG49, \"\")","v":{"$error":"#VALUE!"}}]
["교통시간대이력",{"$nulls":35},"SOIT_D08_M001","SOIT_I08_M001",{"$nulls":9},""]
["soitctrfctmslhstr",{"$nulls":46},""]
["NO","속성명","컬럼명","PK/FK","NULL","형태","VOLT(구현안함)","TIBERO","길이","비고",{"$nulls":30},"COMMENT ON TABLE",{"$f":"A51","v":"soitctrfctmslhstr"},null," IS ",{"$f":"\"'\"&A50&\"'\"","v":"'교통시간대이력'"},";",null,""]
[1,"수정유닉스시각","mdfcn_unix_tm","PK","NOT NULL","NUMBER(10)","INTEGER","NUMBER(10)",null,"수정시각 (second)",null,null,"첨두/비첨두 관리 마스터",{"$nulls":17},"CREATE TABLE ",{"$f":"A51&\" (\"","v":"soitctrfctmslhstr ("},{"$f":"C53&\" \"","v":"mdfcn_unix_tm "},{"$f":"H53&\" \"","v":"NUMBER(10) "},{"$f":"IF(E53=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","CONSTRAINT ",{"$f":"\"PK_\"&A51&\" PRIMARY KEY (\"","v":"PK_soitctrfctmslhstr PRIMARY KEY ("},{"$f":"IF(OR(D53=\"PK\", D53=\"PK/FK\"), C53, \"\")","v":"mdfcn_unix_tm"},{"$f":"IF(OR(D53=\"PK\", D53=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"A$51&\".\"","v":"soitctrfctmslhstr."},{"$f":"C53","v":"mdfcn_unix_tm"}," IS ",{"$f":"\"'\"&J53&\"'\"","v":"'수정시각 (second)'"},";",null,""]
[2,"시간대코드","tmsl_cd","PK/FK","NOT NULL","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",null,"교통시간대코드(050)",{"$nulls":22},"tmsl_cd ","VARCHAR2(2) ","NOT NULL",",",null,null,"tmsl_cd",{"$f":"\") using index tablespace \" &AL64& \") TABLESPACE \" &AK64&\";\"","v":") using index tablespace SOIT_I08_M001) TABLESPACE SOIT_D08_M001;"},"COMMENT ON COLUMN ","soitctrfctmslhstr.","tmsl_cd"," IS ","'교통시간대코드(050)'",";",null,""]
[3,"첨두여부","peak_yn",null,"NOT NULL","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",null,"첨두비첨두여부(Y/N) (002)",{"$nulls":22},"peak_yn ","VARCHAR2(1) ","NOT NULL",",",null,null,"",{"$f":"IF(OR(D55=\"PK\", D55=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitctrfctmslhstr.","peak_yn"," IS ","'첨두비첨두여부(Y/N) (002)'",";",null,""]
[4,"시작시","bgng_hh",null,"NOT NULL","NUMBER(2)","INTEGER","NUMBER(2)",null,"시작 시(HH24)",{"$nulls":22},"bgng_hh ","NUMBER(2) ","NOT NULL",",",null,null,"","","COMMENT ON COLUMN ","soitctrfctmslhstr.","bgng_hh"," IS ","'시작 시(HH24)'",";",null,""]
[5,"시작분","bgng_mi",null,"NOT NULL","NUMBER(2)","INTEGER","NUMBER(2)",null,"시작 분(mm)",{"$nulls":22},"bgng_mi ","NUMBER(2) ","NOT NULL",",",null,null,"","","COMMENT ON COLUMN ","soitctrfctmslhstr.","bgng_mi"," IS ","'시작 분(mm)'",";",null,""]
[6,"종료시","end_hh",null,"NOT NULL","NUMBER(2)","INTEGER","NUMBER(2)",null,"종료 시(HH24)",{"$nulls":22},"end_hh ","NUMBER(2) ","NOT NULL",",",null,null,"","","COMMENT ON COLUMN ","soitctrfctmslhstr.","end_hh"," IS ","'종료 시(HH24)'",";",null,""]
[7,"종료분","end_mi",null,"NOT NULL","NUMBER(2)","INTEGER","NUMBER(2)",null,"종료 분(mm)",{"$nulls":22},"end_mi ","NUMBER(2) ","NOT NULL",",",null,null,"","","COMMENT ON COLUMN ","soitctrfctmslhstr.","end_mi"," IS ","'종료 분(mm)'",";",null,""]
[8,"사용여부","use_yn",null,"NOT NULL","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",null,"사용여부 (Y/N) (002)",{"$nulls":22},"use_yn ","VARCHAR2(1) ","NOT NULL",",",null,null,"","","COMMENT ON COLUMN ","soitctrfctmslhstr.","use_yn"," IS ","'사용여부 (Y/N) (002)'",";",null,""]
[9,"비고","rmrk",null,"NULL","VARCHAR2(200)","VARCHAR(200)","VARCHAR2(200)",null,"비고",{"$nulls":22},"rmrk ","VARCHAR2(200) ","",",",null,null,"","","COMMENT ON COLUMN ","soitctrfctmslhstr.","rmrk"," IS ","'비고'",";",null,""]
[10,"수정자ID","mdfr_id","FK","NOT NULL","VARCHAR2(20)","VARCHAR(20)","VARCHAR2(20)",null,"수정처리한 사용자 ID",{"$nulls":22},"mdfr_id ","VARCHAR2(20) ","NOT NULL",",",null,null,"","","COMMENT ON COLUMN ","soitctrfctmslhstr.","mdfr_id"," IS ","'수정처리한 사용자 ID'",";",null,""]
[{"$nulls":32},{"$f":"CONCATENATE(AK53:AN62)","v":{"$error":"#VALUE!"}},{"$nulls":14},{"$error":"#VALUE!"}]
["코드테이블 - 대분류",{"$nulls":35},"SOIT_D08_M001","SOIT_I08_M001",{"$nulls":9},""]
["soitclrgclsfcdinfo",{"$nulls":46},""]
["NO","속성명","컬럼명","PK/FK","NULL","형태","VOLT","TIBERO","길이","비고",{"$nulls":30},"COMMENT ON TABLE",{"$f":"A65","v":"soitclrgclsfcdinfo"},null," IS ",{"$f":"\"'\"&A64&\"'\"","v":"'코드테이블 - 대분류'"},";",null,""]
[1,"대분류코드","lrg_clsf_cd","PK","NOT NULL","CHAR(5)","VARCHAR(5)","VARCHAR2(5)",null,"대분류코드",{"$nulls":20},"CREATE TABLE ",{"$f":"A65&\" (\"","v":"soitclrgclsfcdinfo ("},{"$f":"C67&\" \"","v":"lrg_clsf_cd "},{"$f":"H67&\" \"","v":"VARCHAR2(5) "},{"$f":"IF(E67=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","CONSTRAINT ",{"$f":"\"PK_\"&A65&\" PRIMARY KEY (\"","v":"PK_soitclrgclsfcdinfo PRIMARY KEY ("},{"$f":"IF(OR(D67=\"PK\", D67=\"PK/FK\"), C67, \"\")","v":"lrg_clsf_cd"},{"$f":"\") using index tablespace \" &AL70& \") TABLESPACE \" &AK70&\";\"","v":") using index tablespace SOIT_I08_M001) TABLESPACE SOIT_D08_M001;"},"COMMENT ON COLUMN ",{"$f":"A$65&\".\"","v":"soitclrgclsfcdinfo."},{"$f":"C67","v":"lrg_clsf_cd"}," IS ",{"$f":"\"'\"&J67&\"'\"","v":"'대분류코드'"},";",null,""]
[2,"코드명","cd_nm",null,"NOT NULL","VARCHAR2(50)","VARCHAR(50)","VARCHAR2(50)",null,"대분류코드명",{"$nulls":22},"cd_nm ","VARCHAR2(50) ","NOT NULL",",",null,null,"",{"$f":"IF(OR(D68=\"PK\", D68=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitclrgclsfcdinfo.","cd_nm"," IS ","'대분류코드명'",";",null,""]
[{"$nulls":32},{"$f":"CONCATENATE(AK66:AN68)","v":{"$error":"#VALUE!"}},{"$nulls":14},{"$error":"#VALUE!"}]
["코드테이블 - 소분류",{"$nulls":35},"SOIT_D08_M001","SOIT_I08_M001",{"$nulls":9},""]
["soitcsmlclsfcdinfo",{"$nulls":46},""]
["NO","속성명","컬럼명","PK/FK","NULL","형태","VOLT","TIBERO","길이","비고",{"$nulls":30},"COMMENT ON TABLE",{"$f":"A71","v":"soitcsmlclsfcdinfo"},null," IS ",{"$f":"\"'\"&A70&\"'\"","v":"'코드테이블 - 소분류'"},";",null,""]
[1,"대분류코드","lrg_clsf_cd","PK/FK","NOT NULL","CHAR(5)","VARCHAR(5)","VARCHAR2(5)",null,"대분류코드",{"$nulls":20},"CREATE TABLE ",{"$f":"A71&\" (\"","v":"soitcsmlclsfcdinfo ("},{"$f":"C73&\" \"","v":"lrg_clsf_cd "},{"$f":"H73&\" \"","v":"VARCHAR2(5) "},{"$f":"IF(E73=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","CONSTRAINT ",{"$f":"\"PK_\"&A71&\" PRIMARY KEY (\"","v":"PK_soitcsmlclsfcdinfo PRIMARY KEY ("},{"$f":"IF(OR(D73=\"PK\", D73=\"PK/FK\"), C73, \"\")","v":"lrg_clsf_cd"},{"$f":"IF(OR(D73=\"PK\", D73=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"A$71&\".\"","v":"soitcsmlclsfcdinfo."},{"$f":"C73","v":"lrg_clsf_cd"}," IS ",{"$f":"\"'\"&J73&\"'\"","v":"'대분류코드'"},";",null,""]
[2,"소분류코드","sml_clsf_cd","PK","NOT NULL","CHAR(12)","VARCHAR(12)","VARCHAR2(12)",null,"소분류코드",{"$nulls":22},"sml_clsf_cd ","VARCHAR2(12) ","NOT NULL",",",null,null,"sml_clsf_cd",{"$f":"\") using index tablespace \" &AL79& \") TABLESPACE \" &AK79&\";\"","v":") using index tablespace SOIT_I08_M001) TABLESPACE SOIT_D08_M001;"},"COMMENT ON COLUMN ","soitcsmlclsfcdinfo.","sml_clsf_cd"," IS ","'소분류코드'",";",null,""]
[3,"순서","seq",null,"NOT NULL","NUMBER(3)","INTEGER","NUMBER(3)",null,"순서",{"$nulls":22},"seq ","NUMBER(3) ","NOT NULL",",",null,null,"",{"$f":"IF(OR(D75=\"PK\", D75=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitcsmlclsfcdinfo.","seq"," IS ","'순서'",";",null,""]
[4,"코드명","cd_nm",null,"NOT NULL","VARCHAR2(50)","VARCHAR(50)","VARCHAR2(50)",null,"소분류코드명",{"$nulls":22},"cd_nm ","VARCHAR2(50) ","NOT NULL",",",null,null,"","","COMMENT ON COLUMN ","soitcsmlclsfcdinfo.","cd_nm"," IS ","'소분류코드명'",";",null,""]
[5,"비고","rmrk",null,"NULL","VARCHAR2(200)","VARCHAR(200)","VARCHAR2(200)",null,"비고",{"$nulls":22},"rmrk ","VARCHAR2(200) ","",",",null,null,"","","COMMENT ON COLUMN ","soitcsmlclsfcdinfo.","rmrk"," IS ","'비고'",";",null,""]
[{"$nulls":32},{"$f":"CONCATENATE(AK73:AN77)","v":{"$error":"#VALUE!"}},{"$nulls":14},{"$error":"#VALUE!"}]
["TOD보고서 변경이력 테이블",{"$nulls":35},"SOIT_D08_M001","SOIT_I08_M001",{"$nulls":9},""]
["soitatodrprthstr",{"$nulls":46},""]
["NO","속성명","컬럼명","PK/FK","NULL","형태","VOLT(구현안함)","TIBERO","길이","비고",{"$nulls":30},"COMMENT ON TABLE",{"$f":"A80","v":"soitatodrprthstr"},null," IS ",{"$f":"\"'\"&A79&\"'\"","v":"'TOD보고서 변경이력 테이블'"},";",null,""]
[1,"수정유닉스시각","mdfcn_unix_tm","PK","NOT NULL","NUMBER(10)","INTEGER","NUMBER(10)",null,"최종 등록/수정일자",{"$nulls":20},"CREATE TABLE ",{"$f":"A80&\" (\"","v":"soitatodrprthstr ("},{"$f":"C82&\" \"","v":"mdfcn_unix_tm "},{"$f":"H82&\" \"","v":"NUMBER(10) "},{"$f":"IF(E82=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","CONSTRAINT ",{"$f":"\"PK_\"&A80&\" PRIMARY KEY (\"","v":"PK_soitatodrprthstr PRIMARY KEY ("},{"$f":"IF(OR(D82=\"PK\", D82=\"PK/FK\"), C82, \"\")","v":"mdfcn_unix_tm"},{"$f":"IF(OR(D82=\"PK\", D82=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"A$80&\".\"","v":"soitatodrprthstr."},{"$f":"C82&\" \"","v":"mdfcn_unix_tm "}," IS ",{"$f":"\"'\"&J82&\"'\"","v":"'최종 등록/수정일자'"},";",null,""]
[2,"노드ID","node_id","PK/FK","NOT NULL","VARCHAR2(300)","VARCHAR2(300)","VARCHAR2(300)",null,"교차로 노드ID",{"$nulls":22},"node_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"node_id",{"$f":"\") using index tablespace \" &AL88& \") TABLESPACE \" &AK88&\";\"","v":") using index tablespace SOIT_I08_M001) TABLESPACE SOIT_D08_M001;"},"COMMENT ON COLUMN ","soitatodrprthstr.","node_id "," IS ","'교차로 노드ID'",";",null,""]
[3,"현장교차로ID","spot_ints_id","FK",null,"NUMBER(5)","INTEGER","NUMBER(5)",null,"현장교차로ID",{"$nulls":22},"spot_ints_id ","NUMBER(5) ","",",",null,null,"",{"$f":"IF(OR(D84=\"PK\", D84=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitatodrprthstr.","spot_ints_id "," IS ","'현장교차로ID'",";",null,""]
[4,"보고서파일명","rprt_file_nm",null,"NOT NULL","VARCHAR2(256)","VARCHAR(256)","VARCHAR2(256)",null,"TOD 보고서 파일명",{"$nulls":22},"rprt_file_nm ","VARCHAR2(256) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitatodrprthstr.","rprt_file_nm "," IS ","'TOD 보고서 파일명'",";",null,""]
[5,"수정자ID","mdfr_id",null,"NOT NULL","VARCHAR2(20)","VARCHAR(20)","VARCHAR2(20)",null,"최종 수정자 ID",{"$nulls":22},"mdfr_id ","VARCHAR2(20) ","NOT NULL",",",null,null,"",{"$f":"IF(OR(D86=\"PK\", D86=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitatodrprthstr.","mdfr_id "," IS ","'최종 수정자 ID'",";",null,""]
[{"$nulls":32},{"$f":"CONCATENATE(AK82:AN86)","v":{"$error":"#VALUE!"}},{"$nulls":14},{"$error":"#VALUE!"}]
[{"$nulls":36},"SOIT_D08_M001","SOIT_I08_M001"]
["테이블 데이터 보관주기 테이블",{"$nulls":46},{"$f":"IF(LEFT(AG89, 13) = \"CONSTRAINT PK\", AG89, \"\")","v":""}]
["soitatableagiginfo",{"$nulls":46},""]
["NO","속성명","컬럼명","PK/FK","NULL","형태","VOLT(구현안함)","TIBERO","길이","비고",{"$nulls":30},"COMMENT ON TABLE",{"$f":"A90","v":"soitatableagiginfo"},null," IS ",{"$f":"\"'\"&A89&\"'\"","v":"'테이블 데이터 보관주기 테이블'"},";",null,""]
[1,"테이블명","tb_nm","PK","NOT NULL","VARCHAR2(1000)","INTEGER","VARCHAR2(1000)",null,"테이블명",{"$nulls":20},"CREATE TABLE ",{"$f":"A90&\" (\"","v":"soitatableagiginfo ("},{"$f":"C92&\" \"","v":"tb_nm "},{"$f":"H92&\" \"","v":"VARCHAR2(1000) "},{"$f":"IF(E92=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","CONSTRAINT ",{"$f":"\"PK_\"&A90&\" PRIMARY KEY (\"","v":"PK_soitatableagiginfo PRIMARY KEY ("},{"$f":"IF(OR(D92=\"PK\", D92=\"PK/FK\"), C92, \"\")","v":"tb_nm"},{"$f":"\") using index tablespace \" &AL97& \") TABLESPACE \" &AK97&\";\"","v":") using index tablespace SOIT_I08_M001) TABLESPACE SOIT_D08_M001;"},"COMMENT ON COLUMN ",{"$f":"A$90&\".\"","v":"soitatableagiginfo."},{"$f":"C92&\" \"","v":"tb_nm "}," IS ",{"$f":"\"'\"&J92&\"'\"","v":"'테이블명'"},";",null,""]
[2,"유지일자","mtnm_day_cnt",null,null,"NUMBER(3)",null,"NUMBER(3)",null,"유지기간 일수",{"$nulls":22},"mtnm_day_cnt ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitatableagiginfo.","mtnm_day_cnt "," IS ","'유지기간 일수'",";"]
[3,"최종수정일자","mdfcn_unix_tm",null,null,"NUMBER(10)","INTEGER","NUMBER(10)",null,"최종수정일자",{"$nulls":22},"mdfcn_unix_tm ","NUMBER(10) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitatableagiginfo.","mdfcn_unix_tm "," IS ","'최종수정일자'",";"]
[4,"최종수정자ID","mdfcn_usid",null,null,"VARCHAR2(20)",null,"VARCHAR2(20)",null,"최종수정자ID",{"$nulls":22},"mdfcn_usid ","VARCHAR2(20) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitatableagiginfo.","mdfcn_usid "," IS ","'최종수정자ID'",";"]
[{"$nulls":32},{"$f":"CONCATENATE(AK92:AN96)","v":{"$error":"#VALUE!"}}," ",""]
["데이터 보관주기 관리 로그 테이블",{"$nulls":35},"SOIT_D08_M001","SOIT_I08_M001",{"$nulls":9},{"$f":"IF(LEFT(AG97, 13) = \"CONSTRAINT PK\", AG97, \"\")","v":""}]
["soitatableagighstr",{"$nulls":46},""]
["NO","속성명","컬럼명","PK/FK","NULL","형태","VOLT(구현안함)","TIBERO","길이","비고",{"$nulls":30},"COMMENT ON TABLE",{"$f":"A98","v":"soitatableagighstr"},null," IS ",{"$f":"\"'\"&A97&\"'\"","v":"'데이터 보관주기 관리 로그 테이블'"},";",null,""]
[1,"테이블명","tb_nm","PK","NOT NULL","VARCHAR2(1000)","INTEGER","VARCHAR2(1000)",null,"테이블명",{"$nulls":20},"CREATE TABLE ",{"$f":"A98&\" (\"","v":"soitatableagighstr ("},{"$f":"C100&\" \"","v":"tb_nm "},{"$f":"H100&\" \"","v":"VARCHAR2(1000) "},{"$f":"IF(E100=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","CONSTRAINT ",{"$f":"\"PK_\"&A98&\" PRIMARY KEY (\"","v":"PK_soitatableagighstr PRIMARY KEY ("},{"$f":"IF(OR(D100=\"PK\", D100=\"PK/FK\"), C100, \"\")","v":"tb_nm"},",","COMMENT ON COLUMN ",{"$f":"A$98&\".\"","v":"soitatableagighstr."},{"$f":"C100&\" \"","v":"tb_nm "}," IS ",{"$f":"\"'\"&J100&\"'\"","v":"'테이블명'"},";"]
[2,"유지시간","mtnm_hour",null,null,"NUMBER(3)",null,"NUMBER(3)",null,"유지시간",{"$nulls":22},"mtnm_hour ","NUMBER(3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitatableagighstr.","mtnm_hour "," IS ","'유지시간'",";"]
[3,"삭제건수","mtnm_cnt",null,null,"NUMBER(10)","INTEGER","NUMBER(10)",null,"삭제건수",{"$nulls":22},"mtnm_cnt ","NUMBER(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitatableagighstr.","mtnm_cnt "," IS ","'삭제건수'",";"]
[4,"대상일자","agig_dt",null,null,"VARCHAR2(8)","INTEGER","VARCHAR2(8)",null,"해당 파티션 기준일자",{"$nulls":22},"agig_dt ","VARCHAR2(8) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitatableagighstr.","agig_dt "," IS ","'해당 파티션 기준일자'",";"]
[5,"삭제유닉스시각","prc_unix_tm","PK","NOT NULL","NUMBER(10)","INTEGER","NUMBER(10)",null,"삭제유닉스시각",{"$nulls":22},"prc_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"prc_unix_tm",{"$f":"\") using index tablespace \" &AL109& \") TABLESPACE \" &AK109&\";\"","v":") using index tablespace SOIT_I08_M001) TABLESPACE SOIT_D08_M001;"},"COMMENT ON COLUMN ","soitatableagighstr.","prc_unix_tm "," IS ","'삭제유닉스시각'",";"]
[6,"삭제시각","prc_tm",null,null,"VARCHAR2(20)",null,"VARCHAR2(20)",null,"삭제시각",{"$nulls":22},"prc_tm ","VARCHAR2(20) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitatableagighstr.","prc_tm "," IS ","'삭제시각'",";"]
[7,"파티션명","partition_nm",null,null,"VARCHAR2(1000)","INTEGER","VARCHAR2(1000)",null,"파티션명",{"$nulls":22},"partition_nm ","VARCHAR2(1000) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitatableagighstr.","partition_nm "," IS ","'파티션명'",";"]
[8,"파티션 바운드값","partition_bound",null,null,"NUMBER(10)","INTEGER","NUMBER(10)",null,"파티션 바운드값",{"$nulls":22},"partition_bound ","NUMBER(10) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitatableagighstr.","partition_bound "," IS ","'파티션 바운드값'",";"]
[{"$nulls":32},{"$f":"CONCATENATE(AK100:AN106)","v":{"$error":"#VALUE!"}}]
["시스템 환경변수 테이블",{"$nulls":35},"SOIT_D08_M001","SOIT_I08_M001",{"$nulls":9},{"$f":"IF(LEFT(#REF!, 13) = \"CONSTRAINT PK\",#REF!, \"\")","v":{"$error":"#REF!"}}]
["soitcenvvarinfo",{"$nulls":46},{"$f":"IF(LEFT(AG110, 13) = \"CONSTRAINT PK\", AG110, \"\")","v":""}]
["NO","속성명","컬럼명","PK/FK","NULL","형태","VOLT(구현안함)","TIBERO","길이","비고",{"$nulls":30},"COMMENT ON TABLE",{"$f":"A110","v":"soitcenvvarinfo"},null," IS ",{"$f":"\"'\"&A109&\"'\"","v":"'시스템 환경변수 테이블'"},";",null,""]
[1,"환경변수명","env_var_nm","PK","NOT NULL","VARCHAR(50)","INTEGER","VARCHAR2(50)",null,"환경변수명",{"$nulls":20},"CREATE TABLE ",{"$f":"A110&\" (\"","v":"soitcenvvarinfo ("},{"$f":"C112&\" \"","v":"env_var_nm "},{"$f":"H112&\" \"","v":"VARCHAR2(50) "},{"$f":"IF(E112=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","CONSTRAINT ",{"$f":"\"PK_\"&A110&\" PRIMARY KEY (\"","v":"PK_soitcenvvarinfo PRIMARY KEY ("},{"$f":"IF(OR(D112=\"PK\", D112=\"PK/FK\"), C112, \"\")","v":"env_var_nm"},{"$f":"\") using index tablespace \" &AL116& \") TABLESPACE \" &AK116&\";\"","v":") using index tablespace SOIT_I08_M001) TABLESPACE SOIT_D08_M001;"},"COMMENT ON COLUMN ",{"$f":"A$110&\".\"","v":"soitcenvvarinfo."},{"$f":"C112","v":"env_var_nm"}," IS ",{"$f":"\"'\"&J112&\"'\"","v":"'환경변수명'"},";",null,""]
[null,"환경변수값","env_var",null,"NOT NULL","VARCHAR(200)",null,"VARCHAR2(200)",null,"환경변수값",{"$nulls":22},"env_var ","VARCHAR2(200) ","NOT NULL",",",null,null,"",{"$f":"IF(OR(D113=\"PK\", D113=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitcenvvarinfo.","env_var"," IS ","'환경변수값'",";"]
[null,"반영유닉스시각","aply_unix_tm",null,"NOT NULL","NUMBER(10)","INTEGER","NUMBER(10)",null,"삭제유닉스시각",{"$nulls":22},"aply_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"","","COMMENT ON COLUMN ","soitcenvvarinfo.","aply_unix_tm"," IS ","'삭제유닉스시각'",";"]
[{"$nulls":32},{"$f":"CONCATENATE(AK112:AN115)","v":{"$error":"#VALUE!"}}," ","",null,null,null,"",""]
["서비스수준 등급 관리 테이블",{"$nulls":35},"SOIT_D08_M001","SOIT_I08_M001",{"$nulls":9},{"$f":"IF(LEFT(AG116, 13) = \"CONSTRAINT PK\", AG116, \"\")","v":""}]
["soitclosgradinfo",{"$nulls":46},""]
["NO","속성명","컬럼명","PK/FK","NULL","형태","VOLT(구현안함)","TIBERO","길이","비고",{"$nulls":30},"COMMENT ON TABLE",{"$f":"A117","v":"soitclosgradinfo"},null," IS ",{"$f":"\"'\"&A116&\"'\"","v":"'서비스수준 등급 관리 테이블'"},";",null,""]
[1,"지표구분코드","indc_se_cd","PK","NOT NULL","CHAR(2)",null,"VARCHAR2(2)",1," 지표구분코드2            ","1:제어지체시간, 2:대기행렬길이, 3:비율FF, 4:속도, 6A:5분교통량, 6B:60분교통량",{"$nulls":19},"CREATE TABLE ",{"$f":"A117&\" (\"","v":"soitclosgradinfo ("},{"$f":"C119&\" \"","v":"indc_se_cd "},{"$f":"H119&\" \"","v":"VARCHAR2(2) "},{"$f":"IF(E119=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","CONSTRAINT ",{"$f":"\"PK_\"&A117&\" PRIMARY KEY (\"","v":"PK_soitclosgradinfo PRIMARY KEY ("},{"$f":"IF(OR(D119=\"PK\", D119=\"PK/FK\"), C119, \"\")","v":"indc_se_cd"},",","COMMENT ON COLUMN ",{"$f":"A$117&\".\"","v":"soitclosgradinfo."},{"$f":"C119","v":"indc_se_cd"}," IS ",{"$f":"\"'\"&J119&\"'\"","v":"' 지표구분코드2            '"},";",null,""]
[2,"서비스수준","srvc_levl_cd","PK","NOT NULL","CHAR(2)",null,"VARCHAR2(2)",1,"서비스수준(609)","서비스수준 (A/B/C/D/E/F/FF)",{"$nulls":21},"srvc_levl_cd ","VARCHAR2(2) ","NOT NULL",",",null,null,"srvc_levl_cd",",","COMMENT ON COLUMN ","soitclosgradinfo.","srvc_levl_cd"," IS ","'서비스수준(609)'",";"]
[3,"서비스지표","srvc_valu",null,"NULL","NUMBER(7,2)",null,"NUMBER(7,2)","5,2","서비스지표",{"$nulls":22},"srvc_valu ","NUMBER(7,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitclosgradinfo.","srvc_valu"," IS ","'서비스지표'",";"]
[4,"집계구분코드","tot_se_cd","PK","NOT NULL","CHAR(1)",null,"VARCHAR2(1)",null,"집계시간구분코드 (011)","집계구분코드 (1:신호현시, 2:1분단위, 3:5분단위, 4:15분, 5:60분, 6:일별)",{"$nulls":21},"tot_se_cd ","VARCHAR2(1) ","NOT NULL",",",null,null,"tot_se_cd",{"$f":"\") using index tablespace \" &AL125& \") TABLESPACE \" &AK125&\";\"","v":") using index tablespace ) TABLESPACE ;"},"COMMENT ON COLUMN ","soitclosgradinfo.","tot_se_cd"," IS ","'집계시간구분코드 (011)'",";"]
[{"$nulls":32},{"$f":"CONCATENATE(AK120:AN122)","v":{"$error":"#VALUE!"}}," ",""]
["프로시저 수행 로그 테이블",{"$nulls":31},{"$f":"C124&\" \"","v":" "}," ","",null,"SOIT_D08_M001","SOIT_I08_M001",{"$nulls":9},{"$f":"IF(LEFT(AG124, 13) = \"CONSTRAINT PK\", AG124, \"\")","v":""}]
["SOITCPROCLOG",{"$nulls":46},""]
["NO","속성명","컬럼명","PK/FK","NULL","형태","VOLT(구현안함)","TIBERO","길이","비고",{"$nulls":30},"COMMENT ON TABLE",{"$f":"A125","v":"SOITCPROCLOG"},null," IS ",{"$f":"\"'\"&A124&\"'\"","v":"'프로시저 수행 로그 테이블'"},";",null,""]
[1,"코드","code",null,null,"VARCHAR2(200)",null,"VARCHAR2(200)",1,"코드",{"$nulls":20},"CREATE TABLE ",{"$f":"A125&\" (\"","v":"SOITCPROCLOG ("},{"$f":"C127&\" \"","v":"code "},{"$f":"H127&\" \"","v":"VARCHAR2(200) "},{"$f":"IF(E127=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",{"$nulls":4},"COMMENT ON COLUMN ",{"$f":"A$125&\".\"","v":"SOITCPROCLOG."},{"$f":"C127","v":"code"}," IS ",{"$f":"\"'\"&J127&\"'\"","v":"'코드'"},";",null,""]
[2,"메시지","msg",null,null,"VARCHAR2(200)",null,"VARCHAR2(200)",null,"메시지",{"$nulls":22},"msg ","VARCHAR2(200) ","",",",null,null,{"$f":"IF(OR(D128=\"PK\", D128=\"PK/FK\"), C128, \"\")","v":""},{"$f":"\") TABLESPACE \" &AK133&\";\"","v":") TABLESPACE SOIT_D08_M001;"},"COMMENT ON COLUMN ","SOITCPROCLOG.","msg"," IS ","'메시지'",";"]
[3,"시작시각","bgng_date",null,null,"DATE",null,"DATE",null,"시작시각",{"$nulls":22},"bgng_date ","DATE ","",",",{"$nulls":4},"COMMENT ON COLUMN ","SOITCPROCLOG.","bgng_date"," IS ","'시작시각'",";"]
[4,"종료시각","end_date",null,null,"DATE",null,"DATE",null,"종료시각",{"$nulls":22},"end_date ","DATE ","",",",{"$nulls":4},"COMMENT ON COLUMN ","SOITCPROCLOG.","end_date"," IS ","'종료시각'",";"]
[5,"파라미터","params",null,null,"VARCHAR2(100)",null,"VARCHAR2(100)",null,"파라미터",{"$nulls":22},"params ","VARCHAR2(100) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","SOITCPROCLOG.","params"," IS ","'파라미터'",";"]
[6,"건수","cnt",null,null,"NUMBER(10)",null,"NUMBER(10)",null,"건수",{"$nulls":22},"cnt ","NUMBER(10) ","",{"$nulls":5},"COMMENT ON COLUMN ","SOITCPROCLOG.","cnt"," IS ","'건수'",";"]
[{"$nulls":32},{"$f":"CONCATENATE(AK127:AN131)","v":{"$error":"#VALUE!"}},null,null,null,"SOIT_D08_M001","SOIT_I08_M001"]
["테이블스페이스 관리 로그 테이블",{"$nulls":31},{"$f":"C134&\" \"","v":" "},{"$f":"H134&\" \"","v":" "},{"$f":"IF(E134=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},null,"SOIT_D08_M001","SOIT_I08_M001",{"$nulls":9},{"$f":"IF(LEFT(AG134, 13) = \"CONSTRAINT PK\", AG134, \"\")","v":""}]
["SOITCTABMTNCLOG",{"$nulls":46},""]
["NO","속성명","컬럼명","PK/FK","NULL","형태","VOLT(구현안함)","TIBERO","길이","비고",{"$nulls":30},"COMMENT ON TABLE",{"$f":"A135","v":"SOITCTABMTNCLOG"},null," IS ",{"$f":"\"'\"&A134&\"'\"","v":"'테이블스페이스 관리 로그 테이블'"},";",null,""]
[1,"코드","code",null,null,"VARCHAR2(200)",null,"VARCHAR2(200)",1,"코드",{"$nulls":20},"CREATE TABLE ",{"$f":"A135&\" (\"","v":"SOITCTABMTNCLOG ("},{"$f":"C137&\" \"","v":"code "},{"$f":"H137&\" \"","v":"VARCHAR2(200) "},{"$f":"IF(E137=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",{"$nulls":4},"COMMENT ON COLUMN ",{"$f":"A$135&\".\"","v":"SOITCTABMTNCLOG."},{"$f":"C137","v":"code"}," IS ",{"$f":"\"'\"&J137&\"'\"","v":"'코드'"},";",null,""]
[2,"메시지","msg",null,null,"VARCHAR2(200)",null,"VARCHAR2(200)",null,"메시지",{"$nulls":22},"msg ","VARCHAR2(200) ","",",",null,null,{"$f":"IF(OR(D138=\"PK\", D138=\"PK/FK\"), C138, \"\")","v":""},{"$f":"\") TABLESPACE \" &AK142&\";\"","v":") TABLESPACE SOIT_D08_M001;"},"COMMENT ON COLUMN ","SOITCTABMTNCLOG.","msg"," IS ","'메시지'",";"]
[3,"테이블스페이스명","tablespace_nm",null,null,"VARCHAR2(200)",null,"VARCHAR2(200)",null,"테이블스페이스명",{"$nulls":22},"tablespace_nm ","VARCHAR2(200) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","SOITCTABMTNCLOG.","tablespace_nm"," IS ","'테이블스페이스명'",";"]
[4,"수행일자","proc_date",null,null,"DATE",null,"DATE",null,"수행일자",{"$nulls":22},"proc_date ","DATE ","",",",{"$nulls":4},"COMMENT ON COLUMN ","SOITCTABMTNCLOG.","proc_date"," IS ","'수행일자'",";"]
[5,"파일명","file_nm",null,null,"VARCHAR2(200)",null,"VARCHAR2(200)",null,"파일명",{"$nulls":22},"file_nm ","VARCHAR2(200) ","",{"$nulls":5},"COMMENT ON COLUMN ","SOITCTABMTNCLOG.","file_nm"," IS ","'파일명'",";"]
[{"$nulls":32},{"$f":"CONCATENATE(AK136:AN140)","v":{"$error":"#VALUE!"}}," ","",null,"SOIT_D08_M001","SOIT_I08_M001"]
[{"$nulls":32},{"$f":"C143&\" \"","v":" "}," ",""]

{"sheet":"센터-네트워크가공","index":7,"n_rows":164,"n_cols":48,"rows_kept":164,"cut":false,"hidden":false,"merged":[[30,1,30,10],[30,13,30,17],[109,9,126,10],[128,1,128,10],[128,13,128,15],[94,1,95,1],[97,1,97,10],[97,13,97,17],[98,9,106,10],[108,1,108,10],[108,13,108,17],[99,1,106,1],[32,1,40,1],[42,13,42,17],[32,9,40,10],[42,1,42,10],[14,1,20,1],[22,13,22,15],[14,9,20,10],[22,1,22,10],[24,1,28,1],[24,9,28,10],[1,1,1,10],[1,13,1,15],[3,1,10,1],[3,9,9,10],[12,1,12,10],[12,13,12,15],[44,1,56,1],[44,9,56,10],[59,1,59,10],[59,13,59,17],[61,1,71,1],[73,13,73,17],[61,9,71,10],[73,1,73,10],[75,1,90,1],[75,9,90,10],[92,1,92,10],[92,13,92,17],[93,9,95,10],[158,13,158,15],[141,1,145,1],[150,1,155,1],[148,13,148,15],[130,9,136,10],[139,1,139,10],[139,13,139,15],[110,1,126,1],[130,1,136,1],[160,1,161,1],[141,9,145,10],[150,9,155,10],[158,1,158,10],[148,1,148,10]]}
[]
[null,"도로 정보 테이블",{"$nulls":11},"soitsroadinfo",{"$nulls":33},{"$f":"IF(LEFT(AE2, 13) = \"CONSTRAINT PK\", AE2, \"\")","v":""}]
[21,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment",{"$nulls":4},"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N2&\" \"","v":"soitsroadinfo "},null," IS ",{"$f":"\"'\"&B2&\"'\"","v":"'도로 정보 테이블'"},";",null,null,null,""]
[null,"soitsroadinfo","도로명","road_nm",1,"VARCHAR2(50)","PK","NOT NULL","도로명","ICT사업본부에서 데이터 입력 예정",null,null,{"$f":"IF(F4=P4, \"EQ\", \"NEQ)\")","v":"EQ"},"도로명","road_nm","VARCHAR2(50)",null,"VARCHAR2(50)",{"$nulls":10},"CREATE TABLE ",{"$f":"N2&\" (\"","v":"soitsroadinfo ("},{"$f":"O4&\" \"","v":"road_nm "},{"$f":"R4&\" \"","v":"VARCHAR2(50) "},{"$f":"IF(H4=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","CONSTRAINT ",{"$f":"\"PK_\"&N2&\" PRIMARY KEY (\"","v":"PK_soitsroadinfo PRIMARY KEY ("},{"$f":"IF(OR(G4=\"PK\", G4=\"PK/FK\"), O4, \"\")","v":"road_nm"},",","COMMENT ON COLUMN ",{"$f":"$N$2&\".\"","v":"soitsroadinfo."},{"$f":"O4","v":"road_nm"}," IS ",{"$f":"\"'\"&I4&\"'\"","v":"'도로명'"},";",null,null,null,""]
[null,null,"방향구분코드","drct_se_cd",2,"CHAR(1)","PK","NOT NULL","방향구분코드(004), 0:대표",{"$nulls":4},"방향구분코드","drct_se_cd","CHAR(1)",null,"CHAR(1)",{"$nulls":12},"drct_se_cd ","CHAR(1) ","NOT NULL",",",null,null,"drct_se_cd",{"$f":"\") using index tablespace \" &AJ13& \") TABLESPACE \" &AI13&\";\"","v":") using index tablespace SOIT_I08_M001) TABLESPACE SOIT_D08_M001;"},"COMMENT ON COLUMN ","soitsroadinfo.","drct_se_cd"," IS ","'방향구분코드(004), 0:대표'",";"]
[null,null,"도로공간정보","road_spin",3,"VARCHAR2(2000)",null,"NOT NULL","도로 지리정보(WKT LineString)",{"$nulls":4},"도로공간정보","road_spin","BINARY",null,"GEOMETRY",{"$nulls":12},"road_spin ","GEOMETRY ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsroadinfo.","road_spin"," IS ","'도로 지리정보(WKT LineString)'",";"]
[null,null,"세그먼트길이","road_lngt",4,"NUMBER(19,9)",null,null,"도로명 길이(meter)",{"$nulls":4},"세그먼트길이","road_lngt","NUMBER(19,9)",null,"NUMBER(19,9)",{"$nulls":12},"road_lngt ","NUMBER(19,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsroadinfo.","road_lngt"," IS ","'도로명 길이(meter)'",";"]
[null,null,"대표경도","rprs_lot",5,"NUMBER(13,10)",null,null,"대표경도",{"$nulls":4},"대표경도","rprs_lot","NUMBER(13,10)",null,"NUMBER(13,10)",{"$nulls":12},"rprs_lot ","NUMBER(13,10) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsroadinfo.","rprs_lot"," IS ","'대표경도'",";"]
[null,null,"대표위도","rprs_lat",6,"NUMBER(12,10)",null,null,"대표위도",{"$nulls":4},"대표위도","rprs_lat","NUMBER(12,10)",null,"NUMBER(12,10)",{"$nulls":12},"rprs_lat ","NUMBER(12,10) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsroadinfo.","rprs_lat"," IS ","'대표위도'",";"]
[null,null,"차선수","lane_cnt",7,"NUMBER(7,5)",null,null,"평균차선수",{"$nulls":4},"차선수","lane_cnt","NUMBER(7,5)",null,"NUMBER(7,5)",{"$nulls":12},"lane_cnt ","NUMBER(7,5) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsroadinfo.","lane_cnt"," IS ","'평균차선수'",";"]
[null,null,"합침여부","union_yn",null,"VARCAHR2(1)",null,null,"합침여부",{"$nulls":4},"합침여부","union_yn","VARCAHR2(1)",null,"VARCAHR2(1)",{"$nulls":12},"union_yn ","VARCAHR2(1) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsroadinfo.","union_yn"," IS ","'합침여부'",";"]
[{"$nulls":30},{"$f":"CONCATENATE(AI4:AL7)","v":{"$error":"#VALUE!"}}]
[null,"도로 소속 교차로 정보 테이블",{"$nulls":11},"soitsroadintsinfo",{"$nulls":20},"SOIT_D08_M001","SOIT_I08_M001",{"$nulls":11},{"$f":"IF(LEFT(AE13, 13) = \"CONSTRAINT PK\", AE13, \"\")","v":""}]
["21-1","Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment",{"$nulls":4},"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N13&\" \"","v":"soitsroadintsinfo "},null," IS ",{"$f":"\"'\"&B13&\"'\"","v":"'도로 소속 교차로 정보 테이블'"},";",null,null,null,""]
[null,"soitsroadintsinfo","도로명","road_nm",1,"VARCHAR2(50)","PK","NOT NULL","도로명","ICT사업본부에서 데이터 입력 예정",null,null,{"$f":"IF(F15=P15, \"EQ\", \"NEQ)\")","v":"EQ"},"도로명","road_nm","VARCHAR2(50)",null,"VARCHAR2(50)",{"$nulls":10},"CREATE TABLE ",{"$f":"N13&\" (\"","v":"soitsroadintsinfo ("},{"$f":"O15&\" \"","v":"road_nm "},{"$f":"R15&\" \"","v":"VARCHAR2(50) "},{"$f":"IF(H15=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","CONSTRAINT ",{"$f":"\"PK_\"&N13&\" PRIMARY KEY (\"","v":"PK_soitsroadintsinfo PRIMARY KEY ("},{"$f":"IF(OR(G15=\"PK\", G15=\"PK/FK\"), O15, \"\")","v":"road_nm"},",","COMMENT ON COLUMN ",{"$f":"$N$13&\".\"","v":"soitsroadintsinfo."},{"$f":"O15","v":"road_nm"}," IS ",{"$f":"\"'\"&I15&\"'\"","v":"'도로명'"},";",null,null,null,""]
[null,null,"운영구분코드","oper_se_cd",2,"VARCHAR2(1)","PK","NOT NULL","운영구분코드 (901)",{"$nulls":4},"운영구분코드","oper_se_cd","VARCHAR2(1)",null,"VARCHAR2(1)",{"$nulls":12},"oper_se_cd ","VARCHAR2(1) ","NOT NULL",",",null,null,"oper_se_cd",",","COMMENT ON COLUMN ","soitsroadintsinfo.","oper_se_cd"," IS ","'운영구분코드 (901)'",";"]
[null,null,"방향구분코드","drct_se_cd",3,"CHAR(1)","PK","NOT NULL","방향구분코드(004)",{"$nulls":4},"방향구분코드","drct_se_cd","CHAR(1)",null,"CHAR(1)",{"$nulls":12},"drct_se_cd ","CHAR(1) ","NOT NULL",",",null,null,"drct_se_cd",",","COMMENT ON COLUMN ","soitsroadintsinfo.","drct_se_cd"," IS ","'방향구분코드(004)'",";"]
[null,null,"구성순번","cnfg_seq",4,"NUMBER(3)","PK","NOT NULL","방향별 노드 구성 순번",{"$nulls":4},"구성순번","cnfg_seq","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"cnfg_seq ","NUMBER(3) ","NOT NULL",",",null,null,"cnfg_seq",{"$f":"\") using index tablespace \" &AJ23& \") TABLESPACE \" &AI23&\";\"","v":") using index tablespace SOIT_I08_M001) TABLESPACE SOIT_D08_M001;"},"COMMENT ON COLUMN ","soitsroadintsinfo.","cnfg_seq"," IS ","'방향별 노드 구성 순번'",";"]
[null,null,"노드ID","node_id",5,"VARCHAR2(300)",null,null,"소속 교차로 노드ID",{"$nulls":4},"노드ID","node_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":12},"node_id ","VARCHAR2(300) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsroadintsinfo.","node_id"," IS ","'소속 교차로 노드ID'",";"]
[null,null,"현장교차로ID","spot_ints_id",6,"NUMBER(5)",null,null,"현장교차로ID",{"$nulls":4},"현장교차로ID","spot_ints_id","NUMBER(5)",null,"NUMBER(5)",{"$nulls":12},"spot_ints_id ","NUMBER(5) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsroadintsinfo.","spot_ints_id"," IS ","'현장교차로ID'",";"]
[null,null,"최적화대상여부","anls_ints_yn",7,"CHAR(1)",null,null,"대상여부 (500)",{"$nulls":4},"최적화대상여부","anls_ints_yn","CHAR(1)",null,"CHAR(1)",{"$nulls":12},"anls_ints_yn ","CHAR(1) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsroadintsinfo.","anls_ints_yn"," IS ","'대상여부 (500)'",";"]
[{"$nulls":30},{"$f":"CONCATENATE(AI15:AL21)","v":{"$error":"#VALUE!"}}]
[null,"도로 소속 엣지 정보 테이블",{"$nulls":11},"soitsroadedgegrupinfo",{"$nulls":20},"SOIT_D08_M001","SOIT_I08_M001",{"$nulls":11},{"$f":"IF(LEFT(AE23, 13) = \"CONSTRAINT PK\", AE23, \"\")","v":""}]
["21-2","Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment",{"$nulls":4},"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N23&\" \"","v":"soitsroadedgegrupinfo "},null," IS ",{"$f":"\"'\"&B23&\"'\"","v":"'도로 소속 엣지 정보 테이블'"},";",null,null,null,""]
[null,"soitsroadedgegrupinfo","도로명","road_nm",1,"VARCHAR2(50)","PK","NOT NULL","도로명","ICT사업본부에서 데이터 입력 예정",null,null,null,"도로명","road_nm","VARCHAR2(50)",null,"VARCHAR2(50)",{"$nulls":10},"CREATE TABLE ",{"$f":"N23&\" (\"","v":"soitsroadedgegrupinfo ("},{"$f":"O25&\" \"","v":"road_nm "},{"$f":"R25&\" \"","v":"VARCHAR2(50) "},{"$f":"IF(H25=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","CONSTRAINT ",{"$f":"\"PK_\"&N23&\" PRIMARY KEY (\"","v":"PK_soitsroadedgegrupinfo PRIMARY KEY ("},{"$f":"IF(OR(G25=\"PK\", G25=\"PK/FK\"), O25, \"\")","v":"road_nm"},",","COMMENT ON COLUMN ",{"$f":"$N$23&\".\"","v":"soitsroadedgegrupinfo."},{"$f":"O25","v":"road_nm"}," IS ",{"$f":"\"'\"&I25&\"'\"","v":"'도로명'"},";"]
[null,null,"방향구분코드","drct_se_cd",2,"CHAR(1)","PK","NOT NULL","방향구분코드(004)",{"$nulls":4},"방향구분코드","drct_se_cd","CHAR(1)",null,"CHAR(1)",{"$nulls":12},"drct_se_cd ","CHAR(1) ","NOT NULL",",",null,null,"drct_se_cd",",","COMMENT ON COLUMN ","soitsroadedgegrupinfo.","drct_se_cd"," IS ","'방향구분코드(004)'",";"]
[null,null,"구성순번","cnfg_seq",3,"NUMBER(3)","PK","NOT NULL","방향별 엣지그룹 구성 순번",{"$nulls":4},"구성순번","cnfg_seq","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"cnfg_seq ","NUMBER(3) ","NOT NULL",",",null,null,"cnfg_seq",",","COMMENT ON COLUMN ","soitsroadedgegrupinfo.","cnfg_seq"," IS ","'방향별 엣지그룹 구성 순번'",";"]
[null,null,"병렬구성순번","prll_seq",4,null,"PK",null,"병렬구성순번",{"$nulls":4},"병렬구성순번","prll_seq","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"prll_seq ","NUMBER(3) ","",",",null,null,"prll_seq",{"$f":"\") using index tablespace \" &AJ31& \") TABLESPACE \" &AI31&\";\"","v":") using index tablespace SOIT_I08_M001) TABLESPACE SOIT_D08_M001;"},"COMMENT ON COLUMN ","soitsroadedgegrupinfo.","prll_seq"," IS ","'병렬구성순번'",";"]
[null,null,"엣지그룹ID","edge_grup_id",5,"VARCHAR2(300)","FK","NOT NULL","엣지그룹 ID",{"$nulls":4},"엣지그룹ID","edge_grup_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":12},"edge_grup_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitsroadedgegrupinfo.","edge_grup_id"," IS ","'엣지그룹 ID'",";"]
[{"$nulls":30},{"$f":"CONCATENATE(AI25:AL29)","v":{"$error":"#VALUE!"}}]
[null,"엣지그룹 진출세그먼트 정보 - 안씀 일단 제외",{"$nulls":11},"soitscnctendsgmninfo",{"$nulls":20},"SOIT_D08_M001","SOIT_I08_M001",{"$nulls":11},{"$f":"IF(LEFT(AE31, 13) = \"CONSTRAINT PK\", AE31, \"\")","v":""}]
[null,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment",{"$nulls":4},"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N$809&\" \"","v":" "},null," IS ",{"$f":"\"'\"&B31&\"'\"","v":"'엣지그룹 진출세그먼트 정보 - 안씀 일단 제외'"},";",null,null,null,""]
[null,"soitscnctendsgmninfo","엣지그룹ID","edge_grup_id",1,"VARCHAR2(300)","PK/FK",null,"엣지그룹ID","ICT본부 2차가공 테이블\nICT본부에서 데이터 생성하여 입력\n\nTIBERO 전용 테이블\n\n교차로 정지선 정보 등 산출 시 사용",null,null,null,"엣지그룹ID","edge_grup_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":10},"CREATE TABLE ",{"$f":"N31&\" (\"","v":"soitscnctendsgmninfo ("},{"$f":"O33&\" \"","v":"edge_grup_id "},{"$f":"R33&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(H33=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",","CONSTRAINT ",{"$f":"\"PK_\"&N31&\" PRIMARY KEY (\"","v":"PK_soitscnctendsgmninfo PRIMARY KEY ("},{"$f":"IF(OR(G33=\"PK\", G33=\"PK/FK\"), O33, \"\")","v":"edge_grup_id"},",","COMMENT ON COLUMN ",{"$f":"N$809&\". \"","v":". "},{"$f":"O33","v":"edge_grup_id"}," IS ",{"$f":"\"'\"&I33&\"'\"","v":"'엣지그룹ID'"},";",null,null,null,""]
[null,null,"시작노드ID","bgng_node_id",2,"VARCHAR2(300)","FK",null,"시작노드ID",{"$nulls":4},"시작노드ID","bgng_node_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":12},"bgng_node_id ","VARCHAR2(300) ","",",",{"$nulls":4},"COMMENT ON COLUMN ",". ","bgng_node_id"," IS ","'시작노드ID'",";",null,null,null,""]
[null,null,"종료노드ID","end_node_id",3,"VARCHAR2(300)","FK",null,"종료노드ID",{"$nulls":4},"종료노드ID","end_node_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":12},"end_node_id ","VARCHAR2(300) ","",",",{"$nulls":4},"COMMENT ON COLUMN ",". ","end_node_id"," IS ","'종료노드ID'",";",null,null,null,""]
[null,null,"차로번호","lane_no",4,"NUMBER(2)",null,null,"차로번호",{"$nulls":4},"차로번호","lane_no","NUMBER(2)",null,"NUMBER(2)",{"$nulls":12},"lane_no ","NUMBER(2) ","",",",{"$nulls":4},"COMMENT ON COLUMN ",". ","lane_no"," IS ","'차로번호'",";",null,null,null,""]
[null,null,"차로ID","lane_id",5,"VARCHAR2(300)","PK/FK",null,"통행차로ID",{"$nulls":4},"차로ID","lane_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":12},"lane_id ","VARCHAR2(300) ","",",",null,null,{"$f":"IF(OR(G37=\"PK\", G37=\"PK/FK\"), O37, \"\")","v":"lane_id"},",","COMMENT ON COLUMN ",". ","lane_id"," IS ","'통행차로ID'",";",null,null,null,""]
[null,null,"차로구성순서","lane_cnfg_seq",6,"NUMBER(3)",null,"NOT NULL","진입 방향에서 교차로 방향으로 구성순번",{"$nulls":4},"차로구성순서","lane_cnfg_seq","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"lane_cnfg_seq ","NUMBER(3) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ",". ","lane_cnfg_seq"," IS ","'진입 방향에서 교차로 방향으로 구성순번'",";",null,null,null,""]
[null,null,"세그먼트ID","sgmn_id",7,"VARCHAR2(300)","PK/FK","NOT NULL","세그먼트 ID",{"$nulls":4},"세그먼트ID","sgmn_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":12},"sgmn_id ","VARCHAR2(300) ","NOT NULL",",",null,null,{"$f":"IF(OR(G39=\"PK\", G39=\"PK/FK\"), O39, \"\")","v":"sgmn_id"},") using index tablespace SOIT_I08);","COMMENT ON COLUMN ",". ","sgmn_id"," IS ","'세그먼트 ID'",";",null,null,null,""]
[null,null,"종료_경도","end_lot",8,"NUMBER(13,10)",null,null,"진출점 경도",{"$nulls":4},"종료_경도","end_lot","NUMBER(13,10)",null,"NUMBER(13,10)",{"$nulls":12},"end_lot ","NUMBER(13,10) ","",",",{"$nulls":4},"COMMENT ON COLUMN ",". ","end_lot"," IS ","'진출점 경도'",";",null,null,null,""]
[null,null,"종료_위도","end_lat",9,"NUMBER(12,10)",null,null,"진출점 위도",{"$nulls":4},"종료_위도","end_lat","NUMBER(12,10)",null,"NUMBER(12,10)",{"$nulls":12},"end_lat ","NUMBER(12,10) ","",",",{"$nulls":4},"COMMENT ON COLUMN ",". ","end_lat"," IS ","'진출점 위도'",";",null,null,null,""]
[{"$nulls":47},""]
[null,"엣지그룹 구성세그먼트 정보",{"$nulls":11},"soitsedgegrupsgmninfo",{"$nulls":33},""]
[null,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment",{"$nulls":4},"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N43&\" \"","v":"soitsedgegrupsgmninfo "},null," IS ",{"$f":"\"'\"&B43&\"'\"","v":"'엣지그룹 구성세그먼트 정보'"},";",null,null,null,""]
[null,"soitsedgegrupsgmninfo","엣지그룹ID","edge_grup_id",1,"VARCHAR2(300)","PK/FK","NOT NULL","엣지그룹ID","ICT본부 2차가공 테이블\nICT본부에서 데이터 생성하여 입력\n\nTIBERO 전용 테이블\n대기행렬  등 관계정보 구성 시 사용",null,null,null,"엣지그룹ID","edge_grup_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":10},"CREATE TABLE ",{"$f":"N43&\" (\"","v":"soitsedgegrupsgmninfo ("},{"$f":"O45&\" \"","v":"edge_grup_id "},{"$f":"R45&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(H45=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","CONSTRAINT ",{"$f":"\"PK_\"&N43&\" PRIMARY KEY (\"","v":"PK_soitsedgegrupsgmninfo PRIMARY KEY ("},{"$f":"IF(OR(G45=\"PK\", G45=\"PK/FK\"), O45, \"\")","v":"edge_grup_id"},",","COMMENT ON COLUMN ",{"$f":"N$43&\". \"","v":"soitsedgegrupsgmninfo. "},{"$f":"O45","v":"edge_grup_id"}," IS ",{"$f":"\"'\"&I45&\"'\"","v":"'엣지그룹ID'"},";",null,null,null,""]
[null,null,"엣지ID","edge_id",2,"VARCHAR2(300)","PK/FK","NOT NULL","엣지ID",{"$nulls":4},"엣지ID","edge_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":12},"edge_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"edge_id",",","COMMENT ON COLUMN ","soitsedgegrupsgmninfo. ","edge_id"," IS ","'엣지ID'",";",null,null,null,""]
[null,null,"누적거리","edge_acml_len",3,"NUMBER(19,9)",null,null,"엣지 누적 거리",{"$nulls":4},"누적거리","edge_acml_len","NUMBER(19,9)",null,"NUMBER(19,9)",{"$nulls":12},"edge_acml_len ","NUMBER(19,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsedgegrupsgmninfo. ","edge_acml_len"," IS ","'엣지 누적 거리'",";",null,null,null,""]
[null,null,"엣지구성순번","edge_cnfg_seq",4,"NUMBER(3)",null,null,"엣지 구성 순번",{"$nulls":4},"엣지구성순서","edge_cnfg_seq","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"edge_cnfg_seq ","NUMBER(3) ","",",",null,null,{"$f":"IF(OR(G48=\"PK\", G48=\"PK/FK\"), O48, \"\")","v":""},null,"COMMENT ON COLUMN ","soitsedgegrupsgmninfo. ","edge_cnfg_seq"," IS ","'엣지 구성 순번'",";",null,null,null,""]
[null,null,"엣지병렬순번","edge_prll_seq",5,"NUMBER(3)",null,null,"엣지 병렬 구성 순번",{"$nulls":4},"엣지병렬순번","edge_prll_seq","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"edge_prll_seq ","NUMBER(3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsedgegrupsgmninfo. ","edge_prll_seq"," IS ","'엣지 병렬 구성 순번'",";",null,null,null,""]
[null,null,"차로ID","lane_id",6,"VARCHAR2(300)","PK/FK",null,"차로ID",{"$nulls":4},"차로ID","lane_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":12},"lane_id ","VARCHAR2(300) ","",",",null,null,"lane_id",",","COMMENT ON COLUMN ","soitsedgegrupsgmninfo. ","lane_id"," IS ","'차로ID'",";",null,null,null,""]
[null,null,"차로번호","lane_no",7,"NUMBER(3)",null,null,"차로번호",{"$nulls":4},"차로구성순번","lane_no","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"lane_no ","NUMBER(3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsedgegrupsgmninfo. ","lane_no"," IS ","'차로번호'",";",null,null,null,""]
[null,null,"세그먼트ID","sgmn_id",8,"VARCHAR2(300)","PK/FK","NOT NULL","세그먼트ID",{"$nulls":4},"세그먼트ID","sgmn_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":12},"sgmn_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"sgmn_id",{"$f":"\") using index tablespace \" &AJ59& \") TABLESPACE \" &AI59&\";\"","v":") using index tablespace SOIT_I08_M001) TABLESPACE SOIT_D08_M001;"},"COMMENT ON COLUMN ","soitsedgegrupsgmninfo. ","sgmn_id"," IS ","'세그먼트ID'",";",null,null,null,""]
[null,null,"세그먼트구성순번","sgmn_cnfg_seq",9,"NUMBER(3)",null,null,"세그먼트 구성 순번",{"$nulls":4},"세그먼트구성순서","sgmn_cnfg_seq","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"sgmn_cnfg_seq ","NUMBER(3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsedgegrupsgmninfo. ","sgmn_cnfg_seq"," IS ","'세그먼트 구성 순번'",";",null,null,null,""]
[null,null,"누적거리","sgmn_acml_len",10,"NUMBER(19,9)",null,null,"세그먼트 누적 거리",{"$nulls":4},"누적거리","sgmn_acml_len","NUMBER(19,9)",null,"NUMBER(19,9)",{"$nulls":12},"sgmn_acml_len ","NUMBER(19,9) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsedgegrupsgmninfo. ","sgmn_acml_len"," IS ","'세그먼트 누적 거리'",";",null,null,null,""]
[null,null,"구성순번","cnfg_seq",11,"NUMBER(3)",null,null,"차선별 세그먼트 구성 순번",{"$nulls":4},"구성순번","cnfg_seq","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"cnfg_seq ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsedgegrupsgmninfo. ","cnfg_seq"," IS ","'차선별 세그먼트 구성 순번'",";",null,null,null,""]
[null,null,"구성역순번","cnfg_desc_seq",12,"NUMBER(3)",null,null,"차선별 세그먼트 역순번",{"$nulls":4},"구성역순번","cnfg_desc_seq","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"cnfg_desc_seq ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsedgegrupsgmninfo. ","cnfg_desc_seq"," IS ","'차선별 세그먼트 역순번'",";",null,null,null,""]
[null,null,"순서구분코드","sgmn_seq_cd",13,"VARCHAR2(1)",null,null,"시작/종료세그먼트 구분코드 (B, E, D)",{"$nulls":4},"순서구분코드","sgmn_seq_cd","VARCHAR2(1)",null,"VARCHAR2(1)",{"$nulls":12},"sgmn_seq_cd ","VARCHAR2(1) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsedgegrupsgmninfo. ","sgmn_seq_cd"," IS ","'시작/종료세그먼트 구분코드 (B, E, D)'",";",null,null,null,""]
[{"$nulls":30},{"$f":"CONCATENATE(AI45:AL57)","v":{"$error":"#VALUE!"}},{"$nulls":16},{"$error":"#VALUE!"}]
[{"$nulls":31},{"$f":"R59&\" \"","v":" "},{"$f":"IF(H59=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},null,"SOIT_D08_M001","SOIT_I08_M001",{"$nulls":11},""]
[null,"교차로 연결세그먼트 정보",{"$nulls":11},"SOITSINTSSGMNINFO",{"$nulls":16},{"$f":"O60&\" \"","v":" "}," ","",{"$nulls":14},""]
[null,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment",{"$nulls":4},"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N60&\" \"","v":"SOITSINTSSGMNINFO "},null," IS ",{"$f":"\"'\"&B60&\"'\"","v":"'교차로 연결세그먼트 정보'"},";",null,null,null,""]
[null,"SOITSINTSSGMNINFO","노드ID","node_id",1,"VARCHAR2(300)","PK/FK",null,"교차로 노드ID","ICT본부 2차가공 테이블\nICT본부에서 데이터 생성하여 입력\n\nTIBERO 전용 테이블\n집계용 교차로 내부 네트워크 관계 테이블",null,null,null,"노드ID","node_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":10},"CREATE TABLE ",{"$f":"N60&\" (\"","v":"SOITSINTSSGMNINFO ("},{"$f":"O62&\" \"","v":"node_id "},{"$f":"R62&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(H62=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",","CONSTRAINT ",{"$f":"\"PK_\"&N60&\" PRIMARY KEY (\"","v":"PK_SOITSINTSSGMNINFO PRIMARY KEY ("},{"$f":"IF(OR(G62=\"PK\", G62=\"PK/FK\"), O62, \"\")","v":"node_id"},",","COMMENT ON COLUMN ",{"$f":"N$60&\". \"","v":"SOITSINTSSGMNINFO. "},{"$f":"O62","v":"node_id"}," IS ",{"$f":"\"'\"&I62&\"'\"","v":"'교차로 노드ID'"},";",null,null,null,""]
[null,null,"연결엣지ID","cnct_edge_id",2,"VARCHAR2(300)","PK","NOT NULL","연결 엣지 ID",{"$nulls":4},"연결엣지ID","cnct_edge_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":12},"cnct_edge_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"cnct_edge_id",",","COMMENT ON COLUMN ","SOITSINTSSGMNINFO. ","cnct_edge_id"," IS ","'연결 엣지 ID'",";",null,null,null,""]
[null,null,"진입방위코드","entr_pocm_cd",3,"CHAR(2)",null,"NOT NULL","진입방위코드 (006)",{"$nulls":4},"진입방위코드","entr_pocm_cd","CHAR(2)",null,"VARCHAR2(2)",{"$nulls":12},"entr_pocm_cd ","VARCHAR2(2) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","SOITSINTSSGMNINFO. ","entr_pocm_cd"," IS ","'진입방위코드 (006)'",";",null,null,null,""]
[null,null,"진출방위코드","exit_pocm_cd",4,"CHAR(2)",null,"NOT NULL","진출방위코드 (006)",{"$nulls":4},"진출방위코드","exit_pocm_cd","CHAR(2)",null,"VARCHAR2(2)",{"$nulls":12},"exit_pocm_cd ","VARCHAR2(2) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","SOITSINTSSGMNINFO. ","exit_pocm_cd"," IS ","'진출방위코드 (006)'",";",null,null,null,""]
[null,null,"진입엣지ID","entr_edge_id",5,"VARCHAR2(300)","FK","NOT NULL","진입 엣지 ID",{"$nulls":4},"진입엣지ID","entr_edge_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":12},"entr_edge_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","SOITSINTSSGMNINFO. ","entr_edge_id"," IS ","'진입 엣지 ID'",";",null,null,null,""]
[null,null,"진출엣지ID","exit_edge_id",6,"VARCHAR2(300)","FK","NOT NULL","진출 엣지 ID",{"$nulls":4},"진출엣지ID","exit_edge_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":12},"exit_edge_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","SOITSINTSSGMNINFO. ","exit_edge_id"," IS ","'진출 엣지 ID'",";",null,null,null,""]
[null,null,"회전분류코드","turn_clsf_cd",7,"CHAR(1)",null,"NOT NULL","회전코드(005)",{"$nulls":4},"회전분류코드","turn_clsf_cd","CHAR(1)",null,"VARCHAR2(1)",{"$nulls":12},"turn_clsf_cd ","VARCHAR2(1) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","SOITSINTSSGMNINFO. ","turn_clsf_cd"," IS ","'회전코드(005)'",";",null,null,null,""]
[null,null,"차로번호","lane_no",8,"NUMBER(3)",null,null,"차로번호",{"$nulls":4},"차로번호","lane_no","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"lane_no ","NUMBER(3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","SOITSINTSSGMNINFO. ","lane_no"," IS ","'차로번호'",";",null,null,null,""]
[null,null,"연결차로ID","cnct_lane_id",9,"VARCHAR2(300)","PK","NOT NULL","연결 엣지 ID",{"$nulls":4},"연결차로ID","cnct_lane_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":12},"cnct_lane_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"cnct_lane_id",",","COMMENT ON COLUMN ","SOITSINTSSGMNINFO. ","cnct_lane_id"," IS ","'연결 엣지 ID'",";",null,null,null,""]
[null,null,"세그먼트ID","sgmn_id",10,"VARCHAR2(300)","PK/FK","NOT NULL","세그먼트ID",{"$nulls":4},"세그먼트ID","sgmn_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":12},"sgmn_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"sgmn_id",{"$f":"\") using index tablespace \" &AJ74& \") TABLESPACE \" &AI74&\";\"","v":") using index tablespace SOIT_I08_M001) TABLESPACE SOIT_D08_M001;"},"COMMENT ON COLUMN ","SOITSINTSSGMNINFO. ","sgmn_id"," IS ","'세그먼트ID'",";",null,null,null,""]
[null,null,"세그먼트구성순번","sgmn_cnfg_seq",11,"NUMBER(3)",null,null,"세그먼트 구성 순번",{"$nulls":4},"세그먼트구성순번","sgmn_cnfg_seq","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"sgmn_cnfg_seq ","NUMBER(3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","SOITSINTSSGMNINFO. ","sgmn_cnfg_seq"," IS ","'세그먼트 구성 순번'",";",null,null,null,""]
[{"$nulls":30},{"$f":"CONCATENATE(AI62:AL72)","v":{"$error":"#VALUE!"}},{"$nulls":16},{"$error":"#VALUE!"}]
[null,"교차로 연결정보",{"$nulls":11},"soitsintscnctinfo",{"$nulls":16},{"$f":"O74&\" \"","v":" "},{"$f":"R74&\" \"","v":" "},{"$f":"IF(H74=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},null,"SOIT_D08_M001","SOIT_I08_M001",{"$nulls":11},""]
[null,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment",{"$nulls":4},"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N74&\" \"","v":"soitsintscnctinfo "},null," IS ",{"$f":"\"'\"&B74&\"'\"","v":"'교차로 연결정보'"},";",null,null,null,""]
[null,"SOITSINTSCNCTINFO","노드ID","node_id",1,"VARCHAR2(300)","PK/FK",null,"교차로 노드ID","ICT본부 2차가공 테이블\nICT본부에서 데이터 생성하여 입력\n\nTIBERO 전용 테이블\n집계용 교차로 내부 네트워크 관계 테이블",null,null,null,"노드ID","node_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":10},"CREATE TABLE ",{"$f":"N74&\" (\"","v":"soitsintscnctinfo ("},{"$f":"O76&\" \"","v":"node_id "},{"$f":"R76&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(H76=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",","CONSTRAINT ",{"$f":"\"PK_\"&N74&\" PRIMARY KEY (\"","v":"PK_soitsintscnctinfo PRIMARY KEY ("},{"$f":"IF(OR(G76=\"PK\", G76=\"PK/FK\"), O76, \"\")","v":"node_id"},",","COMMENT ON COLUMN ",{"$f":"N$74&\". \"","v":"soitsintscnctinfo. "},{"$f":"O76","v":"node_id"}," IS ",{"$f":"\"'\"&I76&\"'\"","v":"'교차로 노드ID'"},";",null,null,null,""]
[null,null,"연결엣지ID","cnct_edge_id",2,"VARCHAR2(300)","PK/FK","NOT NULL","연결 엣지 ID",{"$nulls":4},"연결엣지ID","cnct_edge_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":12},"cnct_edge_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"cnct_edge_id",",","COMMENT ON COLUMN ","soitsintscnctinfo. ","cnct_edge_id"," IS ","'연결 엣지 ID'",";",null,null,null,""]
[null,null,"진입엣지ID","entr_edge_id",3,"VARCHAR2(300)","FK","NOT NULL","진입 엣지 ID",{"$nulls":4},"진입엣지ID","entr_edge_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":12},"entr_edge_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitsintscnctinfo. ","entr_edge_id"," IS ","'진입 엣지 ID'",";",null,null,null,""]
[null,null,"진출엣지ID","exit_edge_id",4,"VARCHAR2(300)","FK","NOT NULL","진출 엣지 ID",{"$nulls":4},"진출엣지ID","exit_edge_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":12},"exit_edge_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitsintscnctinfo. ","exit_edge_id"," IS ","'진출 엣지 ID'",";",null,null,null,""]
[null,null,"회전분류코드","turn_clsf_cd",5,"CHAR(1)",null,"NOT NULL","회전코드(005)",{"$nulls":4},"회전분류코드","turn_clsf_cd","CHAR(1)",null,"VARCHAR2(1)",{"$nulls":12},"turn_clsf_cd ","VARCHAR2(1) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitsintscnctinfo. ","turn_clsf_cd"," IS ","'회전코드(005)'",";",null,null,null,""]
[null,null,"연결차로ID","cnct_lane_id",6,"VARCHAR2(300)","PK/FK","NOT NULL","연결 엣지 ID",{"$nulls":4},"연결차로ID","cnct_lane_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":12},"cnct_lane_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"cnct_lane_id",{"$f":"\") using index tablespace \" &AJ93& \") TABLESPACE \" &AI93&\";\"","v":") using index tablespace SOIT_I08_M001) TABLESPACE SOIT_D08_M001;"},"COMMENT ON COLUMN ","soitsintscnctinfo. ","cnct_lane_id"," IS ","'연결 엣지 ID'",";",null,null,null,""]
[null,null,"차로번호","lane_no",7,"NUMBER(3)",null,null,"차로번호",{"$nulls":4},"차로번호","lane_no","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"lane_no ","NUMBER(3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsintscnctinfo. ","lane_no"," IS ","'차로번호'",";",null,null,null,""]
[null,null,"진입차로ID","entr_lane_id",8,"VARCHAR2(300)","FK","NOT NULL","진입 차로 ID",{"$nulls":4},"진입차로ID","entr_lane_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":12},"entr_lane_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitsintscnctinfo. ","entr_lane_id"," IS ","'진입 차로 ID'",";",null,null,null,""]
[null,null,"진입차로번호","entr_lane_no",9,"NUMBER(3)",null,null,"진입차로번호",{"$nulls":4},"진입차로번호","entr_lane_no","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"entr_lane_no ","NUMBER(3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsintscnctinfo. ","entr_lane_no"," IS ","'진입차로번호'",";",null,null,null,""]
[null,null,"진출차로ID","exit_lane_id",10,"VARCHAR2(300)","FK","NOT NULL","진출 차로 ID",{"$nulls":4},"진출차로ID","exit_lane_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":12},"exit_lane_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitsintscnctinfo. ","exit_lane_id"," IS ","'진출 차로 ID'",";",null,null,null,""]
[null,null,"진출차로번호","exit_lane_no",11,"NUMBER(3)",null,null,"진출차로번호",{"$nulls":4},"진출차로번호","exit_lane_no","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"exit_lane_no ","NUMBER(3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsintscnctinfo. ","exit_lane_no"," IS ","'진출차로번호'",";",null,null,null,""]
[null,null,"진입방위각도","entr_pocm_angl",12,"NUMBER(6,3)",null,null,"진북기준 교차로 진입각도",{"$nulls":4},"진입방위각도","entr_pocm_angl","NUMBER(6,3)",null,"NUMBER(6,3)",{"$nulls":12},"entr_pocm_angl ","NUMBER(6,3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsintscnctinfo. ","entr_pocm_angl"," IS ","'진북기준 교차로 진입각도'",";",null,null,null,""]
[null,null,"진출방위각도","exit_pocm_angl",13,"NUMBER(6,3)",null,null,"진북기준 교차로 진출각도",{"$nulls":4},"진출방위각도","exit_pocm_angl","NUMBER(6,3)",null,"NUMBER(6,3)",{"$nulls":12},"exit_pocm_angl ","NUMBER(6,3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsintscnctinfo. ","exit_pocm_angl"," IS ","'진북기준 교차로 진출각도'",";",null,null,null,""]
[null,null,"진입방위코드","entr_pocm_cd",14,"CHAR(2)",null,"NOT NULL","진입방위코드 (006)",{"$nulls":4},"진입방위코드","entr_pocm_cd","CHAR(2)",null,"VARCHAR2(2)",{"$nulls":12},"entr_pocm_cd ","VARCHAR2(2) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitsintscnctinfo. ","entr_pocm_cd"," IS ","'진입방위코드 (006)'",";",null,null,null,""]
[null,null,"진출방위코드","exit_pocm_cd",15,"CHAR(2)",null,"NOT NULL","진출방위코드 (006)",{"$nulls":4},"진출방위코드","exit_pocm_cd","CHAR(2)",null,"VARCHAR2(2)",{"$nulls":12},"exit_pocm_cd ","VARCHAR2(2) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitsintscnctinfo. ","exit_pocm_cd"," IS ","'진출방위코드 (006)'",";",null,null,null,""]
[null,null,"현장카메라ID","spot_camr_id",16,"VARCHAR2(10)",null,null,"현장스마트교차로 카메라 ID",{"$nulls":4},"현장카메라ID","spot_camr_id","CHAR(10)",null,"VARCHAR2(10)",{"$nulls":12},"spot_camr_id ","VARCHAR2(10) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsintscnctinfo. ","spot_camr_id"," IS ","'현장스마트교차로 카메라 ID'",";",null,null,null,""]
[{"$nulls":30},{"$f":"CONCATENATE(AI76:AL90)","v":{"$error":"#VALUE!"}}," ","",{"$nulls":14},{"$error":"#VALUE!"}]
[null,"교차로군 정보",{"$nulls":11},"SOITSINTSGRUPINFO",{"$nulls":20},"SOIT_D08_M001","SOIT_I08_M001",{"$nulls":11},""]
[null,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","ICT본부 수집자료 저장 테이블\nTIBERO 전용 테이블\nTOD보고서에서 수집한 교차로군 명칭 목록",null,null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N93&\" \"","v":"SOITSINTSGRUPINFO "},null," IS ",{"$f":"\"'\"&B93&\"'\"","v":"'교차로군 정보'"},";",null,null,null,""]
[null,"SOITSINTSGRUPINFO","교차로 그룹","ints_grop_id",null,"NUMBER(5)","PK/FK",null,"교차로군ID",{"$nulls":4},"교차로 그룹","ints_grop_id","NUMBER(5)",null,"NUMBER(5)",{"$nulls":10},"CREATE TABLE ",{"$f":"N93&\" (\"","v":"SOITSINTSGRUPINFO ("},{"$f":"O95&\" \"","v":"ints_grop_id "},{"$f":"R95&\" \"","v":"NUMBER(5) "},{"$f":"IF(H95=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",","CONSTRAINT ",{"$f":"\"PK_\"&N93&\" PRIMARY KEY (\"","v":"PK_SOITSINTSGRUPINFO PRIMARY KEY ("},{"$f":"IF(OR(G95=\"PK\", G95=\"PK/FK\"), O95, \"\")","v":"ints_grop_id"},{"$f":"\") using index tablespace \" &AJ98& \") TABLESPACE \" &AI98&\";\"","v":") using index tablespace SOIT_I08_M001) TABLESPACE SOIT_D08_M001;"},"COMMENT ON COLUMN ",{"$f":"N$93&\". \"","v":"SOITSINTSGRUPINFO. "},{"$f":"O95","v":"ints_grop_id"}," IS ",{"$f":"\"'\"&I95&\"'\"","v":"'교차로군ID'"},";",null,null,null,""]
[null,null,"교차로 명","ints_grop_nm",null,"VARCHAR2(50)",null,null,"교차로군명",{"$nulls":4},"교차로 명","ints_grop_nm","VARCHAR2(50)",null,"VARCHAR2(50)",{"$nulls":12},"ints_grop_nm ","VARCHAR2(50) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","SOITSINTSGRUPINFO. ","ints_grop_nm"," IS ","'교차로군명'",";",null,null,null,""]
[{"$nulls":30},{"$f":"CONCATENATE(AI95:AL96)","v":{"$error":"#VALUE!"}},{"$nulls":16},{"$error":"#VALUE!"}]
[null,"현시구간이력 정보",{"$nulls":11},"SOITSPHASSGNLCHGHSTR",{"$nulls":20},"SOIT_D08_M001","SOIT_I08_M001",{"$nulls":11},""]
[null,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","ICT본부 수집자료 저장 테이블\nTIBERO 전용 테이블\n\n현시구간별 신호변경이력 테이블",null,null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N98&\" \"","v":"SOITSPHASSGNLCHGHSTR "},null," IS ",{"$f":"\"'\"&B98&\"'\"","v":"'현시구간이력 정보'"},";",null,null,null,""]
[null,"SOITSPHASSGNLCHGHSTR","노드ID","node_id",1,"VARCHAR2(300)","PK/FK",null,"교차로 노드ID",{"$nulls":4},"노드ID","node_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":10},"CREATE TABLE ",{"$f":"N98&\" (\"","v":"SOITSPHASSGNLCHGHSTR ("},{"$f":"O100&\" \"","v":"node_id "},{"$f":"R100&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(H100=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",null,"(",{"$f":"IF(OR(G100=\"PK\", G100=\"PK/FK\"), O100, \"\")","v":"node_id"},",","COMMENT ON COLUMN ",{"$f":"N$98&\". \"","v":"SOITSPHASSGNLCHGHSTR. "},{"$f":"O100","v":"node_id"}," IS ",{"$f":"\"'\"&I100&\"'\"","v":"'교차로 노드ID'"},";",null,null,null,""]
[null,null,"진입엣지ID","entr_edge_id",2,"VARCHAR2(300)",null,"NOT NULL","진입 엣지 ID",{"$nulls":4},"진입엣지ID","entr_edge_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":12},"entr_edge_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","SOITSPHASSGNLCHGHSTR. ","entr_edge_id"," IS ","'진입 엣지 ID'",";",null,null,null,""]
[null,null,"연결엣지","cnct_edge_id",3,"VARCHAR2(300)","PK/FK","NOT NULL","연결 엣지 ID",{"$nulls":4},"연결엣지","cnct_edge_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":12},"cnct_edge_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"cnct_edge_id",",","COMMENT ON COLUMN ","SOITSPHASSGNLCHGHSTR. ","cnct_edge_id"," IS ","'연결 엣지 ID'",";"]
[null,null,"진출엣지ID","exit_edge_id",4,"VARCHAR2(300)",null,"NOT NULL","진출 엣지 ID",{"$nulls":4},"진출엣지ID","exit_edge_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":12},"exit_edge_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","SOITSPHASSGNLCHGHSTR. ","exit_edge_id"," IS ","'진출 엣지 ID'",";"]
[null,null,"회전분류코드","turn_clsf_cd",5,"CHAR(1)",null,"NOT NULL","회전코드(005)",{"$nulls":4},"회전분류코드","turn_clsf_cd","CHAR(1)",null,"CHAR(1)",{"$nulls":12},"turn_clsf_cd ","CHAR(1) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","SOITSPHASSGNLCHGHSTR. ","turn_clsf_cd"," IS ","'회전코드(005)'",";",null,null,null,{"$f":"IF(LEFT(AE104, 13) = \"CONSTRAINT PK\", AE104, \"\")","v":""}]
[null,null,"시작유닉스시각","bgng_unix_tm",6,"NUMBER(10)","PK",null,"신호 시작시각(현시)",{"$nulls":4},"시작유닉스시각","bgng_unix_tm","NUMBER(10)",null,"NUMBER(10)",{"$nulls":12},"bgng_unix_tm ","NUMBER(10) ","",",",null,null,"bgng_unix_tm",")","COMMENT ON COLUMN ","SOITSPHASSGNLCHGHSTR. ","bgng_unix_tm"," IS ","'신호 시작시각(현시)'",";",null,null,null,""]
[null,null,"종료유닉스시각","end_unix_tm",7,"NUMBER(10)",null,null,"신호 종료시각(현시)",{"$nulls":4},"종료유닉스시각","end_unix_tm","NUMBER(10)",null,"NUMBER(10)",{"$nulls":12},"end_unix_tm ","NUMBER(10) ",null,",",null,null,"",null,"COMMENT ON COLUMN ","SOITSPHASSGNLCHGHSTR. ","end_unix_tm"," IS ","'신호 종료시각(현시)'",";",null,null,null,""]
[null,null,"신호상태코드","sgnl_stts_cd",8,"CHAR(1)",null,null,"신호상태코드 (505)",{"$nulls":4},"신호상태코드","sgnl_stts_cd","CHAR(1)",null,"CHAR(1)",{"$nulls":12},"sgnl_stts_cd ","CHAR(1) ",{"$f":"IF(H107=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},{"$f":"\") TABLESPACE \"&AI109&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_M001 NOLOGGING"},null,null,{"$f":"IF(OR(F107=\"PK\", F107=\"PK/FK\"), H107, \"\")","v":""},null,"COMMENT ON COLUMN ","SOITSPHASSGNLCHGHSTR. ","sgnl_stts_cd"," IS ","'신호상태코드 (505)'",";",null,null,null,""]
[{"$nulls":30},{"$f":"CONCATENATE(AI108:AK108)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (bgng_unix_tm) INTERVAL (3600) STORE IN (\"&AI109&\") (PARTITION BFR_\" & N98& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AI109&\");\"","v":"PARTITION BY RANGE (bgng_unix_tm) INTERVAL (3600) STORE IN (SOIT_D08_M001) (PARTITION BFR_SOITSPHASSGNLCHGHSTR_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_M001);"},{"$f":"\"CREATE INDEX PK_\" & N98& \" ON \" & N98 & CONCATENATE(AJ100:AL106) & \" LOCAL (PARTITION BFR_\" & N98 & \"_20221101 TABLESPACE \"&AJ109&\") TABLESPACE \"&AJ109&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & N98 & \" ADD CONSTRAINT PK_\" & N98 & \" PRIMARY KEY \" & CONCATENATE(AJ100:AL106) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":10},{"$error":"#VALUE!"}]
[null,"교차로 차선별 정지선 정보",{"$nulls":11},"SOITSINTSSTOPLOCINFO",{"$nulls":20},"SOIT_D08_M001","SOIT_I08_M001",{"$nulls":11},""]
[null,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","ICT본부 2차가공 테이블\nICT본부에서 데이터 생성하여 입력\n\nTIBERO 전용 테이블\n교차로 정지선 정보 테이블",null,null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N109&\" \"","v":"SOITSINTSSTOPLOCINFO "},null," IS ",{"$f":"\"'\"&B109&\"'\"","v":"'교차로 차선별 정지선 정보'"},";",null,null,null,""]
[null,"SOITSINTSSTOPLOCINFO","노드ID","node_id",1,"VARCHAR2(300)","PK/FK",null,"교차로 노드ID",{"$nulls":4},"노드ID","node_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":10},"CREATE TABLE ",{"$f":"N109&\" (\"","v":"SOITSINTSSTOPLOCINFO ("},{"$f":"O111&\" \"","v":"node_id "},{"$f":"R111&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(H111=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",","CONSTRAINT ",{"$f":"\"PK_\"&N109&\" PRIMARY KEY (\"","v":"PK_SOITSINTSSTOPLOCINFO PRIMARY KEY ("},{"$f":"IF(OR(G111=\"PK\", G111=\"PK/FK\"), O111, \"\")","v":"node_id"},",","COMMENT ON COLUMN ",{"$f":"N$109&\". \"","v":"SOITSINTSSTOPLOCINFO. "},{"$f":"O111","v":"node_id"}," IS ",{"$f":"\"'\"&I111&\"'\"","v":"'교차로 노드ID'"},";",null,null,null,""]
[null,null,"진입엣지ID","entr_edge_id",2,"VARCHAR2(300)","PK/FK","NOT NULL","진입 엣지 ID",{"$nulls":4},"진입엣지ID","entr_edge_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":12},"entr_edge_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"entr_edge_id",",","COMMENT ON COLUMN ","SOITSINTSSTOPLOCINFO. ","entr_edge_id"," IS ","'진입 엣지 ID'",";",null,null,null,""]
[null,null,"방향구분코드","drct_se_cd",3,"VARCHAR(1)","PK","NOT NULL","집계방향구분(600)",null,null,"방향구분코드 (1:진입차로별, 2:내부회전별)",null,"방향구분코드","drct_se_cd","VARCHAR2(1)",null,"VARCHAR2(1)",{"$nulls":12},"drct_se_cd ","VARCHAR2(1) ","NOT NULL",",",null,null,"drct_se_cd",",","COMMENT ON COLUMN ","SOITSINTSSTOPLOCINFO. ","drct_se_cd"," IS ","'집계방향구분(600)'",";",null,null,null,""]
[null,null,"흐름구분코드","flow_se_cd",4,"VARCHAR(2)","PK","NOT NULL","진입차로별:진입차로번호, 내부회전별:회전(005)",null,null,"진입차로별:진입차로번호, 내부회전별:(s:직진, r:우회전, l:좌회전, u:유턴)",null,"흐름구분코드","flow_se_cd","VARCHAR2(2)",null,"VARCHAR2(2)",{"$nulls":12},"flow_se_cd ","VARCHAR2(2) ","NOT NULL",",",null,null,"flow_se_cd",{"$f":"\") using index tablespace \" &AJ129& \") TABLESPACE \" &AI129&\";\"","v":") using index tablespace SOIT_I08_M001) TABLESPACE SOIT_D08_M001;"},"COMMENT ON COLUMN ","SOITSINTSSTOPLOCINFO. ","flow_se_cd"," IS ","'진입차로별:진입차로번호, 내부회전별:회전(005)'",";",null,null,null,""]
[null,null,"진입방위코드","entr_pocm_cd",5,"CHAR(2)",null,"NOT NULL","진입방위코드 (006)",{"$nulls":4},"진입방위코드","entr_pocm_cd","CHAR(2)",null,"VARCHAR2(2)",{"$nulls":12},"entr_pocm_cd ","VARCHAR2(2) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","SOITSINTSSTOPLOCINFO. ","entr_pocm_cd"," IS ","'진입방위코드 (006)'",";",null,null,null,""]
[null,null,"진입방위각도","entr_pocm_angl",6,"NUMBER(6,3)",null,null,"진북기준 교차로 진입각도",{"$nulls":4},"진입방위각도","entr_pocm_angl","NUMBER(6,3)",null,"NUMBER(6,3)",{"$nulls":12},"entr_pocm_angl ","NUMBER(6,3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","SOITSINTSSTOPLOCINFO. ","entr_pocm_angl"," IS ","'진북기준 교차로 진입각도'",";",null,null,null,""]
[null,null,"차선진입각도","lane_pocm_angl",7,"NUMBER(6,3)",null,null,"진북기준 차선 진입각도",{"$nulls":4},"차선방위각도","lane_pocm_angl","NUMBER(6,3)",null,"NUMBER(6,3)",{"$nulls":12},"lane_pocm_angl ","NUMBER(6,3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","SOITSINTSSTOPLOCINFO. ","lane_pocm_angl"," IS ","'진북기준 차선 진입각도'",";",null,null,null,""]
[null,null,"정지각도","stop_angl",8,"NUMBER(6,3)",null,null,"정지선 각도",{"$nulls":4},"정지각도","stop_angl","NUMBER(6,3)",null,"NUMBER(6,3)",{"$nulls":12},"stop_angl ","NUMBER(6,3) ","",",",null,null,{"$f":"IF(OR(G118=\"PK\", G118=\"PK/FK\"), O118, \"\")","v":""},null,"COMMENT ON COLUMN ","SOITSINTSSTOPLOCINFO. ","stop_angl"," IS ","'정지선 각도'",";",null,null,null,""]
[null,null,"지표 텍스트 각도","valu_angl",9,"NUMBER(6,3)",null,null,"지표 텍스트 라벨 각도",{"$nulls":4},"지표 텍스트 각도","valu_angl","NUMBER(6,3)",null,"NUMBER(6,3)",{"$nulls":12},"valu_angl ","NUMBER(6,3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","SOITSINTSSTOPLOCINFO. ","valu_angl"," IS ","'지표 텍스트 라벨 각도'",";",null,null,null,""]
[null,null,"정지점1경도","STOP_1_LOT",10,"NUMBER(13,10)",null,null,"정지점1경도(실제 정지선)",{"$nulls":4},"정지점1경도","STOP_1_LOT","NUMBER(13,10)",null,"NUMBER(13,10)",{"$nulls":12},"STOP_1_LOT ","NUMBER(13,10) ","",",",null,null,{"$f":"IF(OR(G120=\"PK\", G120=\"PK/FK\"), O120, \"\")","v":""},null,"COMMENT ON COLUMN ","SOITSINTSSTOPLOCINFO. ","STOP_1_LOT"," IS ","'정지점1경도(실제 정지선)'",";",null,null,null,""]
[null,null,"정지점1위도","STOP_1_LAT",11,"NUMBER(12,10)",null,null,"정지점1위도(실제 정지선)",{"$nulls":4},"정지점1위도","STOP_1_LAT","NUMBER(12,10)",null,"NUMBER(12,10)",{"$nulls":12},"STOP_1_LAT ","NUMBER(12,10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","SOITSINTSSTOPLOCINFO. ","STOP_1_LAT"," IS ","'정지점1위도(실제 정지선)'",";",null,null,null,""]
[null,null,"정지점2경도","STOP_2_LOT",12,"NUMBER(13,10)",null,null,"정지점2경도",{"$nulls":4},"정지점2경도","STOP_2_LOT","NUMBER(13,10)",null,"NUMBER(13,10)",{"$nulls":12},"STOP_2_LOT ","NUMBER(13,10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","SOITSINTSSTOPLOCINFO. ","STOP_2_LOT"," IS ","'정지점2경도'",";",null,null,null,""]
[null,null,"정지점2위도","STOP_2_LAT",13,"NUMBER(12,10)",null,null,"정지점2위도",{"$nulls":4},"정지점2위도","STOP_2_LAT","NUMBER(12,10)",null,"NUMBER(12,10)",{"$nulls":12},"STOP_2_LAT ","NUMBER(12,10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","SOITSINTSSTOPLOCINFO. ","STOP_2_LAT"," IS ","'정지점2위도'",";",null,null,null,""]
[null,null,"정지점3경도","STOP_3_LOT",14,"NUMBER(13,10)",null,null,"정지점3경도",{"$nulls":4},"정지점3경도","STOP_3_LOT","NUMBER(13,10)",null,"NUMBER(13,10)",{"$nulls":12},"STOP_3_LOT ","NUMBER(13,10) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","SOITSINTSSTOPLOCINFO. ","STOP_3_LOT"," IS ","'정지점3경도'",";",null,null,null,""]
[null,null,"정지점3위도","STOP_3_LAT",15,"NUMBER(12,10)",null,null,"정지점3위도",{"$nulls":4},"정지점3위도","STOP_3_LAT","NUMBER(12,10)",null,"NUMBER(12,10)",{"$nulls":12},"STOP_3_LAT ","NUMBER(12,10) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","SOITSINTSSTOPLOCINFO. ","STOP_3_LAT"," IS ","'정지점3위도'",";",null,null,null,""]
[null,null,"정지점4경도","STOP_4_LOT",16,"NUMBER(13,10)",null,null,"정지점4경도",{"$nulls":4},"정지점4경도","STOP_4_LOT","NUMBER(13,10)",null,"NUMBER(13,10)",{"$nulls":12},"STOP_4_LOT ","NUMBER(13,10) ","",",",null,null,{"$f":"IF(OR(G126=\"PK\", G126=\"PK/FK\"), O126, \"\")","v":""},null,"COMMENT ON COLUMN ","SOITSINTSSTOPLOCINFO. ","STOP_4_LOT"," IS ","'정지점4경도'",";",null,null,null,""]
[null,null,"정지점4위도","STOP_4_LAT",17,"NUMBER(12,10)",null,null,"정지점4위도",{"$nulls":4},"정지점4위도","STOP_4_LAT","NUMBER(12,10)",null,"NUMBER(12,10)",{"$nulls":12},"STOP_4_LAT ","NUMBER(12,10) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","SOITSINTSSTOPLOCINFO. ","STOP_4_LAT"," IS ","'정지점4위도'",";",null,null,null,""]
[{"$nulls":30},{"$f":"CONCATENATE(AI111:AL127)","v":{"$error":"#VALUE!"}},{"$nulls":16},{"$error":"#VALUE!"}]
[null,"지역 분할정보 공간 테이블",{"$nulls":11},"soitspbadmsprttninfo",{"$nulls":20},"SOIT_D08_M001","SOIT_I08_M001",{"$nulls":11},""]
[8,"Table Name","Attribute Name","Column Name","f","Data type","PK/FK","Column Null Option","Comment",{"$nulls":4},"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N129&\" \"","v":"soitspbadmsprttninfo "},null," IS ",{"$f":"\"'\"&B129&\"'\"","v":"'지역 분할정보 공간 테이블'"},";",null,null,null,""]
[null,"soitspbadmsprttninfo\n(확정)","지역분할코드","rgn_prttn_cd",1,"CHAR(2)","PK","NOT NULL","지역분할코드 (051)","ICT사업본부에서 입력 예정",null,null,{"$f":"IF(F131=P131, \"EQ\", \"NEQ)\")","v":"EQ"},"지역분할코드","rgn_prttn_cd","CHAR(2)",null,"VARCHAR2(2)",{"$nulls":10},"CREATE TABLE ",{"$f":"N129&\" (\"","v":"soitspbadmsprttninfo ("},{"$f":"O131&\" \"","v":"rgn_prttn_cd "},{"$f":"R131&\" \"","v":"VARCHAR2(2) "},{"$f":"IF(H131=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","CONSTRAINT ",{"$f":"\"PK_\"&N129&\" PRIMARY KEY (\"","v":"PK_soitspbadmsprttninfo PRIMARY KEY ("},{"$f":"IF(OR(G131=\"PK\", G131=\"PK/FK\"), O131, \"\")","v":"rgn_prttn_cd"},",","COMMENT ON COLUMN ",{"$f":"$N$129&\".\"","v":"soitspbadmsprttninfo."},{"$f":"O131","v":"rgn_prttn_cd"}," IS ",{"$f":"\"'\"&I131&\"'\"","v":"'지역분할코드 (051)'"},";",null,null,null,""]
[null,null,"행정구역코드","pbadms_dstt_cd",2,"CHAR(5)","FK",null,"소속 행정구역코드 (052)",null,null,null,"EQ","행정구역코드","pbadms_dstt_cd","CHAR(5)",null,"VARCHAR2(5)",{"$nulls":12},"pbadms_dstt_cd ","VARCHAR2(5) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitspbadmsprttninfo.","pbadms_dstt_cd"," IS ","'소속 행정구역코드 (052)'",";",null,null,null,""]
[null,null,"구역구분코드","dstt_se_cd",null,"CHAR(1)","PK",0,"구역구분코드 (053)",{"$nulls":4},"구역구분코드","dstt_se_cd","CHAR(1)",null,"VARCHAR2(1)",{"$nulls":12},"dstt_se_cd ","VARCHAR2(1) ","",",",null,null,"dstt_se_cd",{"$f":"\") using index tablespace \" &AJ139& \") TABLESPACE \" &AI139&\";\"","v":") using index tablespace SOIT_I08_M001) TABLESPACE SOIT_D08_M001;"},"COMMENT ON COLUMN ","soitspbadmsprttninfo.","dstt_se_cd"," IS ","'구역구분코드 (053)'",";",null,null,null,""]
[null,null,"분할공간정보","rgn_prttn_spin",3,"BINARY",null,"NOT NULL","지역분할공간정보",null,null,null,{"$f":"IF(F134=P134, \"EQ\", \"NEQ)\")","v":"EQ"},"지역분할공간정보","rgn_prttn_spin","BINARY",null,"GEOMETRY",{"$nulls":12},"rgn_prttn_spin ","GEOMETRY ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitspbadmsprttninfo.","rgn_prttn_spin"," IS ","'지역분할공간정보'",";",null,null,null,""]
[null,null,"외곽공간정보","outr_spin",null,"BINARY",null,null,"외곽강조공간정보",null,null,null,"EQ","외곽공간정보","outr_spin","BINARY",null,"GEOMETRY",{"$nulls":12},"outr_spin ","GEOMETRY ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitspbadmsprttninfo.","outr_spin"," IS ","'외곽강조공간정보'",";",null,null,null,""]
[null,null,"중심경도","centr_lot",4,"NUMBER(13,10)",null,null,"분할지역 중심좌표 경도",null,null,null,"EQ","중심경도","centr_lot","NUMBER(13,10)",null,"NUMBER(13,10)",{"$nulls":12},"centr_lot ","NUMBER(13,10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitspbadmsprttninfo.","centr_lot"," IS ","'분할지역 중심좌표 경도'",";",null,null,null,""]
[null,null,"중심위도","centr_lat",5,"NUMBER(12,10)",null,null,"분할지역 중심좌표 위도",null,null,null,"EQ","중심위도","centr_lat","NUMBER(12,10)",null,"NUMBER(12,10)",{"$nulls":12},"centr_lat ","NUMBER(12,10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitspbadmsprttninfo.","centr_lat"," IS ","'분할지역 중심좌표 위도'",";",null,null,null,""]
[{"$nulls":30},{"$f":"CONCATENATE(AI131:AL137)","v":{"$error":"#VALUE!"}},{"$nulls":16},{"$error":"#VALUE!"}]
[{"$nulls":34},"SOIT_D08_M001","SOIT_I08_M001"]
[null,"노드 신호등 위치정보 테이블",{"$nulls":11},"soitssglginfo",{"$nulls":33},{"$f":"IF(LEFT(AE140, 13) = \"CONSTRAINT PK\", AE140, \"\")","v":""}]
[16,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment",{"$nulls":4},"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"$N140&\" \"","v":"soitssglginfo "},null," IS ",{"$f":"\"'\"&B140&\"'\"","v":"'노드 신호등 위치정보 테이블'"},";",null,null,null,""]
[null,"soitssglginfo","노드ID","node_id",1,"VARCHAR2(300)","PK","NOT NULL","노드ID","ICT본부 2차가공 테이블\nICT본부에서 데이터 생성하여 입력\n\nTIBERO 전용 테이블",null,null,null,"노드ID","node_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":10},"CREATE TABLE ",{"$f":"N140&\" (\"","v":"soitssglginfo ("},{"$f":"O142&\" \"","v":"node_id "},{"$f":"R142&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(H142=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","CONSTRAINT ",{"$f":"\"PK_\"&N140&\" PRIMARY KEY (\"","v":"PK_soitssglginfo PRIMARY KEY ("},{"$f":"IF(OR(G142=\"PK\", G142=\"PK/FK\"), O142, \"\")","v":"node_id"},",","COMMENT ON COLUMN ",{"$f":"$N$140&\". \"","v":"soitssglginfo. "},{"$f":"O142","v":"node_id"}," IS ",{"$f":"\"'\"&I142&\"'\"","v":"'노드ID'"},";",null,null,null,""]
[null,null,"현장교차로ID","spot_ints_id",2,"NUMBER(5)","FK","NULL","현장교차로ID",{"$nulls":4},"현장교차로ID","spot_ints_id","NUMBER(5)",null,"NUMBER(5)",{"$nulls":12},"spot_ints_id ","NUMBER(5) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitssglginfo. ","spot_ints_id"," IS ","'현장교차로ID'",";",null,null,null,""]
[null,null,"연결엣지ID","cnct_edge_id",3,"VARCHAR2(300)","PK/FK","NOT NULL","진입 연결엣지 ID",{"$nulls":4},"연결엣지ID","cnct_edge_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":12},"cnct_edge_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"cnct_edge_id",{"$f":"\") using index tablespace \" &AJ148& \") TABLESPACE \" &AI148&\";\"","v":") using index tablespace SOIT_I08_M001) TABLESPACE SOIT_D08_M001;"},"COMMENT ON COLUMN ","soitssglginfo. ","cnct_edge_id"," IS ","'진입 연결엣지 ID'",";",null,null,null,""]
[null,null,"신호등 경도","sglg_lot",4,"NUMBER(13,10)",null,"NOT NULL","신호등 경도",{"$nulls":4},"신호등 경도","sglg_lot","NUMBER(13,10)",null,"NUMBER(13,10)",{"$nulls":12},"sglg_lot ","NUMBER(13,10) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitssglginfo. ","sglg_lot"," IS ","'신호등 경도'",";",null,null,null,""]
[null,null,"신호등 위도","sglg_lat",5,"NUMBER(12,10)",null,"NOT NULL","신호등 위도",{"$nulls":4},"신호등 위도","sglg_lat","NUMBER(12,10)",null,"NUMBER(12,10)",{"$nulls":12},"sglg_lat ","NUMBER(12,10) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitssglginfo. ","sglg_lat"," IS ","'신호등 위도'",";",null,null,null,""]
[{"$nulls":30},{"$f":"CONCATENATE(AI142:AL146)","v":{"$error":"#VALUE!"}},{"$nulls":16},{"$error":"#VALUE!"}]
[{"$nulls":34},"SOIT_D08_M001","SOIT_I08_M001"]
[null,"노드 신호등 위치정보 테이블",{"$nulls":11},"soitssignallocinfo",{"$nulls":33},{"$f":"IF(LEFT(AE149, 13) = \"CONSTRAINT PK\", AE149, \"\")","v":""}]
[16,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment",{"$nulls":4},"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"$N149&\" \"","v":"soitssignallocinfo "},null," IS ",{"$f":"\"'\"&B149&\"'\"","v":"'노드 신호등 위치정보 테이블'"},";",null,null,null,""]
[null,"soitssignallocinfo","노드ID","node_id",1,"VARCHAR2(300)","PK","NOT NULL","노드ID","ICT본부 2차가공 테이블\nICT본부에서 데이터 생성하여 입력\n\nTIBERO 전용 테이블",null,null,null,"노드ID","node_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":10},"CREATE TABLE ",{"$f":"N149&\" (\"","v":"soitssignallocinfo ("},{"$f":"O151&\" \"","v":"node_id "},{"$f":"R151&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(H151=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","CONSTRAINT ",{"$f":"\"PK_\"&N149&\" PRIMARY KEY (\"","v":"PK_soitssignallocinfo PRIMARY KEY ("},{"$f":"IF(OR(G151=\"PK\", G151=\"PK/FK\"), O151, \"\")","v":"node_id"},",","COMMENT ON COLUMN ",{"$f":"$N$149&\". \"","v":"soitssignallocinfo. "},{"$f":"O151","v":"node_id"}," IS ",{"$f":"\"'\"&I151&\"'\"","v":"'노드ID'"},";",null,null,null,""]
[null,null,"현장교차로ID","spot_ints_id",2,"NUMBER(5)","FK","NULL","현장교차로ID",{"$nulls":4},"현장교차로ID","spot_ints_id","NUMBER(5)",null,"NUMBER(5)",{"$nulls":12},"spot_ints_id ","NUMBER(5) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitssignallocinfo. ","spot_ints_id"," IS ","'현장교차로ID'",";"]
[null,null,"진입방위코드","entr_pocm_cd",5,"VARCHAR(2)","PK","NOT NULL","진입방위코드 (006)",{"$nulls":4},"진입방위코드","entr_pocm_cd","VARCHAR(2)",null,"VARCHAR(2)",{"$nulls":12},"entr_pocm_cd ","VARCHAR(2) ","NOT NULL",",",null,null,"entr_pocm_cd",",","COMMENT ON COLUMN ","soitssignallocinfo. ","entr_pocm_cd"," IS ","'진입방위코드 (006)'",";"]
[null,null,"진입방위각도","entr_pocm_angl",6,"NUMBER(6,3)","PK",null,"진북기준 교차로 진입각도",{"$nulls":4},"진입방위각도","entr_pocm_angl","NUMBER(6,3)",null,"NUMBER(6,3)",{"$nulls":12},"entr_pocm_angl ","NUMBER(6,3) ","",",",null,null,"entr_pocm_angl",{"$f":"\") using index tablespace \" &AJ158& \") TABLESPACE \" &AI158&\";\"","v":") using index tablespace SOIT_I08_M001) TABLESPACE SOIT_D08_M001;"},"COMMENT ON COLUMN ","soitssignallocinfo. ","entr_pocm_angl"," IS ","'진북기준 교차로 진입각도'",";"]
[null,null,"신호등 경도","sglg_lot",4,"NUMBER(13,10)",null,"NOT NULL","신호등 경도",{"$nulls":4},"신호등 경도","sglg_lot","NUMBER(13,10)",null,"NUMBER(13,10)",{"$nulls":12},"sglg_lot ","NUMBER(13,10) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitssignallocinfo. ","sglg_lot"," IS ","'신호등 경도'",";"]
[null,null,"신호등 위도","sglg_lat",5,"NUMBER(12,10)",null,"NOT NULL","신호등 위도",{"$nulls":4},"신호등 위도","sglg_lat","NUMBER(12,10)",null,"NUMBER(12,10)",{"$nulls":12},"sglg_lat ","NUMBER(12,10) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitssignallocinfo. ","sglg_lat"," IS ","'신호등 위도'",";"]
[{"$nulls":30},{"$f":"CONCATENATE(AI151:AL156)","v":{"$error":"#VALUE!"}}," ",""]
[{"$nulls":30},{"$f":"O158&\" \"","v":" "}," ","",null,"SOIT_D08_M001","SOIT_I08_M001"]
[null,"3D 세그먼트 이관용 임시테이블",{"$nulls":11},"soitssgmn_3D",{"$nulls":33},{"$f":"IF(LEFT(AE159, 13) = \"CONSTRAINT PK\", AE159, \"\")","v":""}]
[16,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment",{"$nulls":4},"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"$N159&\" \"","v":"soitssgmn_3D "},null," IS ",{"$f":"\"'\"&B159&\"'\"","v":"'3D 세그먼트 이관용 임시테이블'"},";",null,null,null,""]
[null,"soitssgmn_3D","세그먼트ID","sgmn_id",1,"VARCHAR2(300)","PK","NOT NULL","세그먼트 ID",{"$nulls":4},"노드ID","sgmn_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":10},"CREATE TABLE ",{"$f":"N159&\" (\"","v":"soitssgmn_3D ("},{"$f":"O161&\" \"","v":"sgmn_id "},{"$f":"R161&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(H161=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","CONSTRAINT ",{"$f":"\"PK_\"&N159&\" PRIMARY KEY (\"","v":"PK_soitssgmn_3D PRIMARY KEY ("},{"$f":"IF(OR(G161=\"PK\", G161=\"PK/FK\"), O161, \"\")","v":"sgmn_id"},{"$f":"\") using index tablespace \" &AJ164& \") TABLESPACE \" &AI164&\";\"","v":") using index tablespace SOIT_I08_M001) TABLESPACE SOIT_D08_M001;"},"COMMENT ON COLUMN ",{"$f":"$N$159&\". \"","v":"soitssgmn_3D. "},{"$f":"O161","v":"sgmn_id"}," IS ",{"$f":"\"'\"&I161&\"'\"","v":"'세그먼트 ID'"},";",null,null,null,""]
[null,null,"세그먼트3D공간정보","sgmn_3d_spin",2,"BINARY",null,null,"3D 세그먼트 지리정보","ICT본부에서 가공/입력",null,null,null,"외곽공간정보","sgmn_3d_spin","BINARY",null,"GEOMETRY",{"$nulls":12},"sgmn_3d_spin ","GEOMETRY ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitssgmn_3D. ","sgmn_3d_spin"," IS ","'3D 세그먼트 지리정보'",";"]
[{"$nulls":30},{"$f":"CONCATENATE(AI161:AL162)","v":{"$error":"#VALUE!"}}]
[{"$nulls":34},"SOIT_D08_M001","SOIT_I08_M001"]

{"sheet":"SUMO-현시,네트워크","index":8,"n_rows":530,"n_cols":55,"rows_kept":530,"cut":false,"hidden":false,"merged":[[1,13,1,15],[1,19,1,24],[1,28,1,33],[1,38,1,43],[2,1,2,10],[2,13,2,15],[4,1,9,1],[11,1,11,10],[11,13,11,15],[202,1,215,1],[82,13,82,15],[104,13,104,15],[126,13,126,15],[13,1,18,1],[20,1,20,10],[20,13,20,15],[32,1,32,10],[32,13,32,15],[44,1,44,10],[44,13,44,15],[56,1,56,10],[56,13,56,15],[104,1,104,10],[126,1,126,10],[68,1,68,10],[68,13,68,15],[75,13,75,15],[106,1,124,1],[128,1,148,1],[152,1,172,1],[180,1,184,1],[22,1,30,1],[34,1,42,1],[46,1,54,1],[58,1,66,1],[70,1,73,1],[77,1,80,1],[84,1,102,1],[75,1,75,10],[82,1,82,10],[392,13,392,15],[394,9,399,9],[256,13,256,15],[258,1,276,1],[279,1,279,10],[279,13,279,15],[281,1,293,1],[295,1,295,10],[295,13,295,15],[297,1,314,1],[317,1,317,10],[317,13,317,15],[319,1,330,1],[325,9,328,9],[333,1,333,10],[333,13,333,15],[335,1,345,1],[218,1,218,10],[218,13,218,15],[226,1,226,10],[226,13,226,15],[244,1,253,1],[256,1,256,10],[242,1,242,10],[242,13,242,15],[381,1,381,10],[381,13,381,15],[220,1,223,1],[228,1,239,1],[377,1,378,1],[377,9,378,9],[150,1,150,10],[150,13,150,15],[174,1,174,10],[178,1,178,10],[178,13,178,15],[186,1,186,10],[186,13,186,15],[188,9,197,9],[200,1,200,10],[200,13,200,15],[188,1,197,1],[446,1,484,1],[488,1,497,1],[341,9,344,9],[348,1,348,10],[348,13,348,15],[350,1,359,1],[362,1,362,10],[362,13,362,15],[364,1,372,1],[375,1,375,10],[375,13,375,15],[402,13,402,15],[394,1,400,1],[402,1,402,10],[404,1,442,1],[444,1,444,10],[444,13,444,15],[486,1,486,10],[486,13,486,15],[383,1,389,1],[383,9,388,9],[392,1,392,10]]}
[{"$nulls":10},"INTS_SE_CD"]
[{"$nulls":13},"변경후(센터 도메인 및 용어기준)",{"$nulls":5},"VOLT DDL",{"$nulls":8},"TIBERO DDL",{"$nulls":9},"COMMENTS"]
[null,"시차제 교차로 정보 테이블",{"$nulls":11},"soitsspotintstmdiff"]
[1,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO"]
[null,"soitsspotintstmdiff\n(확정)","현장교차로ID","spot_ints_id",1,"NUMBER(5)","PK",null,"현장교차로ID",null,null,null,{"$f":"IF(F5=P5, \"EQ\", \"NEQ)\")","v":"EQ"},"현장교차로ID","spot_ints_id","NUMBER(5)","INTEGER",null,null,"CREATE TABLE ",{"$f":"N3&\" (\"","v":"soitsspotintstmdiff ("},{"$f":"O5&\" \"","v":"spot_ints_id "},{"$f":"Q5&\" \"","v":"INTEGER "},{"$f":"IF(H5=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",","PRIMARY KEY (",{"$f":"IF(OR(G5=\"PK\", G5=\"PK/FK\"), O5, \"\")","v":"spot_ints_id"},","]
[null,null,"노드ID","node_id",2,"VARCHAR2(300)","PK",null,"노드ID",null,null,null,"EQ","노드ID","node_id","VARCHAR2(300)","VARCHAR(300)",{"$nulls":4},"node_id ","VARCHAR(300) ","",",",null,"node_id",","]
[null,null,"시간순번","tm_seq",3,"NUMBER(5)","PK",null,"시간순번",null,null,null,"EQ","순번","seq","NUMBER(5)","INTEGER",{"$nulls":4},"seq ","INTEGER ","",",",null,"seq","));"]
[null,null,"시차시작시각","bgng_unix_tm",4,"NUMBER(2)",null,null,"시작시각",null,null,null,"NEQ)","시차시작시각","bgng_unix_tm","NUMBER(10)","INTEGER",{"$nulls":4},"bgng_unix_tm ","INTEGER ","",",",null,""]
[null,null,"종료시작시각","end_unix_tm",5,"CHAR(100)",null,null,"종료시각",null,null,null,"NEQ)","종료시작시각","end_unix_tm","NUMBER(10)","INTEGER",{"$nulls":4},"end_unix_tm ","INTEGER ","",",",null,""]
[null,null,"요일구분코드","dotw_se_cd",6,"CHAR(2)",null,null,"요일구분코드2 (027)",null,null,"1:평일, 2: 일주일","EQ","요일구분코드","dotw_se_cd","CHAR(2)","VARCHAR(2)",{"$nulls":4},"dotw_se_cd ","VARCHAR(2) ","",",",null,""]
[{"$nulls":21},{"$f":"CONCATENATE(Z5:AB11)","v":{"$error":"#VALUE!"}},{"$nulls":25},{"$f":"IF(LEFT(AE11, 13) = \"CONSTRAINT PK\", AE11, \"\")","v":""}]
[null,"(메타버스) 시차제 교차로 정보 테이블",{"$nulls":11},"mtvsspotintstmdiff"]
["2023-01-01","Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO"]
[null,"mtvsspotintstmdiff","현장교차로ID","spot_ints_id",1,"NUMBER(5)","PK",null,"현장교차로ID",null,null,null,{"$f":"IF(F14=P14, \"EQ\", \"NEQ)\")","v":"EQ"},"현장교차로ID","spot_ints_id","NUMBER(5)","INTEGER",null,null,"CREATE TABLE ",{"$f":"N12&\" (\"","v":"mtvsspotintstmdiff ("},{"$f":"O14&\" \"","v":"spot_ints_id "},{"$f":"Q14&\" \"","v":"INTEGER "},{"$f":"IF(H14=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",","PRIMARY KEY (",{"$f":"IF(OR(G14=\"PK\", G14=\"PK/FK\"), O14, \"\")","v":"spot_ints_id"},","]
[null,null,"노드ID","node_id",2,"VARCHAR2(300)","PK",null,"노드ID",null,null,null,"EQ","노드ID","node_id","VARCHAR2(300)","VARCHAR(300)",{"$nulls":4},"node_id ","VARCHAR(300) ","",",",null,"node_id",","]
[null,null,"시간순번","tm_seq",3,"NUMBER(5)","PK",null,"시간순번",null,null,null,"EQ","순번","seq","NUMBER(5)","INTEGER",{"$nulls":4},"seq ","INTEGER ","",",",null,"seq","));"]
[null,null,"시차시작시각","bgng_unix_tm",4,"NUMBER(2)",null,null,"시작시각",null,null,null,"NEQ)","시차시작시각","bgng_unix_tm","NUMBER(10)","INTEGER",{"$nulls":4},"bgng_unix_tm ","INTEGER ","",",",null,""]
[null,null,"종료시작시각","end_unix_tm",5,"CHAR(100)",null,null,"종료시각",null,null,null,"NEQ)","종료시작시각","end_unix_tm","NUMBER(10)","INTEGER",{"$nulls":4},"end_unix_tm ","INTEGER ","",",",null,""]
[null,null,"요일구분코드","dotw_se_cd",6,"CHAR(2)",null,null,"요일구분코드2 (027)",null,null,"1:평일, 2: 일주일","EQ","요일구분코드","dotw_se_cd","CHAR(2)","VARCHAR(2)",{"$nulls":4},"dotw_se_cd ","VARCHAR(2) ","",",",null,""]
[{"$nulls":21},{"$f":"CONCATENATE(Z14:AB20)","v":{"$error":"#VALUE!"}},{"$nulls":25},{"$f":"IF(LEFT(AE20, 13) = \"CONSTRAINT PK\", AE20, \"\")","v":""}]
[null,"현시정보 테이블",{"$nulls":11},"soitsphasinfo"]
["2022-02-01","Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N21&\" \"","v":"soitsphasinfo "},null," IS ",{"$f":"\"'\"&B21&\"'\"","v":"'현시정보 테이블'"},";"]
[null,"soitsphasinfo\n(확정)","현장교차로ID","spot_ints_id",1,"NUMBER(5)","PK",null,"현장교차로ID",null,null,null,{"$f":"IF(F23=P23, \"EQ\", \"NEQ)\")","v":"EQ"},"현장교차로ID","spot_ints_id","NUMBER(5)","INTEGER","NUMBER(5)",null,"CREATE TABLE ",{"$f":"N21&\" (\"","v":"soitsphasinfo ("},{"$f":"O23&\" \"","v":"spot_ints_id "},{"$f":"Q23&\" \"","v":"INTEGER "},{"$f":"IF(H23=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",","PRIMARY KEY (",{"$f":"IF(OR(G23=\"PK\", G23=\"PK/FK\"), O23, \"\")","v":"spot_ints_id"},",","CREATE TABLE ",{"$f":"N21&\" (\"","v":"soitsphasinfo ("},{"$f":"O23&\" \"","v":"spot_ints_id "},{"$f":"R23&\" \"","v":"NUMBER(5) "},{"$f":"IF(H23=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",","CONSTRAINT ",{"$f":"\"PK_\"&N21&\" PRIMARY KEY (\"","v":"PK_soitsphasinfo PRIMARY KEY ("},{"$f":"IF(OR(G23=\"PK\", G23=\"PK/FK\"), O23, \"\")","v":"spot_ints_id"},",","COMMENT ON COLUMN ",{"$f":"$N$21&\".\"","v":"soitsphasinfo."},{"$f":"O23","v":"spot_ints_id"}," IS ",{"$f":"\"'\"&I23&\"'\"","v":"'현장교차로ID'"},";"]
[null,null,"노드ID","node_id",2,"VARCHAR2(300)","PK",null,"노드ID",null,null,null,"EQ","노드ID","node_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,null,null,"node_id ","VARCHAR(300) ","",",",null,"node_id",",",null,null,"node_id ","VARCHAR2(300) ","",",",null,null,"node_id",",","COMMENT ON COLUMN ","soitsphasinfo.","node_id"," IS ","'노드ID'",";"]
[null,null,"주교차로구분코드","majr_ints_se_cd",3,"CHAR(2)","PK",null,"주교차로구분코드 (062)",null,null,"주교차로구분 (1:주교차로, 2:연등교차로)","EQ","주교차로구분코드","majr_ints_se_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",null,null,null,"majr_ints_se_cd ","VARCHAR(2) ","",",",null,"majr_ints_se_cd",",",null,null,"majr_ints_se_cd ","VARCHAR2(2) ","",",",null,null,"majr_ints_se_cd",",","COMMENT ON COLUMN ","soitsphasinfo.","majr_ints_se_cd"," IS ","'주교차로구분코드 (062)'",";"]
[null,null,"현시번호","phas_no",4,"NUMBER(2)","PK",null,"현시번호",null,null,null,"EQ","현시번호","phas_no","NUMBER(2)","INTEGER","NUMBER(2)",null,null,null,"phas_no ","INTEGER ","",",",null,"phas_no","));",null,null,"phas_no ","NUMBER(2) ","",",",null,null,"phas_no",{"$f":"\") using index tablespace \" &AJ33& \") TABLESPACE \" &AI33&\";\"","v":") using index tablespace SOIT_I08_M001) TABLESPACE SOIT_D08_M001;"},"COMMENT ON COLUMN ","soitsphasinfo.","phas_no"," IS ","'현시번호'",";"]
[null,null,"신호상태","sgnl_stts",5,"CHAR(100)",null,null,"신호상태 결합 (rrrgggGGGrr)",null,null,null,"EQ","신호상태","sgnl_stts","CHAR(100)","VARCHAR(100)","VARCHAR2(100)",null,null,null,"sgnl_stts ","VARCHAR(100) ","",",",null,"",null,null,null,"sgnl_stts ","VARCHAR2(100) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsphasinfo.","sgnl_stts"," IS ","'신호상태 결합 (rrrgggGGGrr)'",";"]
[null,null,"최소녹색시간","min_gren_hr",6,"NUMBER(3)",null,null,"최소녹색시간",null,null,null,"EQ","최소녹색시간","min_gren_hr","NUMBER(3)","INTEGER","NUMBER(3)",null,null,null,"min_gren_hr ","INTEGER ","",",",null,"",null,null,null,"min_gren_hr ","NUMBER(3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsphasinfo.","min_gren_hr"," IS ","'최소녹색시간'",";"]
[null,null,"황색시간","yelw_hr",7,"NUMBER(3)",null,null,"황색시간",null,null,null,"EQ","황색시간","yelw_hr","NUMBER(3)","INTEGER","NUMBER(3)",null,null,null,"yelw_hr ","INTEGER ",null,",",null,"",null,null,null,"yelw_hr ","NUMBER(3) ",null,",",null,null,"",null,"COMMENT ON COLUMN ","soitsphasinfo.","yelw_hr"," IS ","'황색시간'",";"]
[null,null,"적색시간","red_hr",8,"NUMBER(3)",null,null,"적색시간",null,null,null,"EQ","적색시간","red_hr","NUMBER(3)","INTEGER","NUMBER(3)",null,null,null,"red_hr ","INTEGER ",null,",",null,"",null,null,null,"red_hr ","NUMBER(3) ",null,",",null,null,"",null,"COMMENT ON COLUMN ","soitsphasinfo.","red_hr"," IS ","'적색시간'",";"]
[null,null,"주도로구분코드","majr_road_se_cd",9,"CHAR(2)",null,null,"주도로구분코드 (063)",null,null,"주도로구분 (10:부도로, 20:주도로)","EQ","주도로구분코드","majr_road_se_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",null,null,null,"majr_road_se_cd ","VARCHAR(2) ",{"$f":"IF(H31=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",null,"",null,null,null,"majr_road_se_cd ","VARCHAR2(2) ",{"$f":"IF(H31=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",null,null,"",null,"COMMENT ON COLUMN ","soitsphasinfo.","majr_road_se_cd"," IS ","'주도로구분코드 (063)'",";"]
[{"$nulls":21},{"$f":"CONCATENATE(Z23:AB32)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AI23:AL31)","v":{"$error":"#VALUE!"}},{"$nulls":16},{"$f":"IF(LEFT(AE32, 13) = \"CONSTRAINT PK\", AE32, \"\")","v":{"$error":"#VALUE!"}}]
[null,"(메타버스) 현시정보 테이블",{"$nulls":11},"mtvsphasinfo",{"$nulls":20},"SOIT_D08_M001","SOIT_I08_M001"]
["2023-02-11","Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N33&\" \"","v":"mtvsphasinfo "},null," IS ",{"$f":"\"'\"&B33&\"'\"","v":"'(메타버스) 현시정보 테이블'"},";"]
[null,"mtvsphasinfo","현장교차로ID","spot_ints_id",1,"NUMBER(5)","PK",null,"현장교차로ID",null,null,null,{"$f":"IF(F35=P35, \"EQ\", \"NEQ)\")","v":"EQ"},"현장교차로ID","spot_ints_id","NUMBER(5)","INTEGER","NUMBER(5)",null,"CREATE TABLE ",{"$f":"N33&\" (\"","v":"mtvsphasinfo ("},{"$f":"O35&\" \"","v":"spot_ints_id "},{"$f":"Q35&\" \"","v":"INTEGER "},{"$f":"IF(H35=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",","PRIMARY KEY (",{"$f":"IF(OR(G35=\"PK\", G35=\"PK/FK\"), O35, \"\")","v":"spot_ints_id"},",","CREATE TABLE ",{"$f":"N33&\" (\"","v":"mtvsphasinfo ("},{"$f":"O35&\" \"","v":"spot_ints_id "},{"$f":"R35&\" \"","v":"NUMBER(5) "},{"$f":"IF(H35=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",","CONSTRAINT ",{"$f":"\"PK_\"&N33&\" PRIMARY KEY (\"","v":"PK_mtvsphasinfo PRIMARY KEY ("},{"$f":"IF(OR(G35=\"PK\", G35=\"PK/FK\"), O35, \"\")","v":"spot_ints_id"},",","COMMENT ON COLUMN ",{"$f":"$N$33&\".\"","v":"mtvsphasinfo."},{"$f":"O35","v":"spot_ints_id"}," IS ",{"$f":"\"'\"&I35&\"'\"","v":"'현장교차로ID'"},";"]
[null,null,"노드ID","node_id",2,"VARCHAR2(300)","PK",null,"노드ID",null,null,null,"EQ","노드ID","node_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,null,null,"node_id ","VARCHAR(300) ","",",",null,"node_id",",",null,null,"node_id ","VARCHAR2(300) ","",",",null,null,"node_id",",","COMMENT ON COLUMN ","mtvsphasinfo.","node_id"," IS ","'노드ID'",";"]
[null,null,"주교차로구분코드","majr_ints_se_cd",3,"CHAR(2)","PK",null,"주교차로구분코드 (062)",null,null,"주교차로구분 (1:주교차로, 2:연등교차로)","EQ","주교차로구분코드","majr_ints_se_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",null,null,null,"majr_ints_se_cd ","VARCHAR(2) ","",",",null,"majr_ints_se_cd",",",null,null,"majr_ints_se_cd ","VARCHAR2(2) ","",",",null,null,"majr_ints_se_cd",",","COMMENT ON COLUMN ","mtvsphasinfo.","majr_ints_se_cd"," IS ","'주교차로구분코드 (062)'",";"]
[null,null,"현시번호","phas_no",4,"NUMBER(2)","PK",null,"현시번호",null,null,null,"EQ","현시번호","phas_no","NUMBER(2)","INTEGER","NUMBER(2)",null,null,null,"phas_no ","INTEGER ","",",",null,"phas_no","));",null,null,"phas_no ","NUMBER(2) ","",",",null,null,"phas_no",") using index tablespace SOIT_I08);","COMMENT ON COLUMN ","mtvsphasinfo.","phas_no"," IS ","'현시번호'",";"]
[null,null,"신호상태","sgnl_stts",5,"CHAR(100)",null,null,"신호상태 결합 (rrrgggGGGrr)",null,null,null,"EQ","신호상태","sgnl_stts","CHAR(100)","VARCHAR(100)","VARCHAR2(100)",null,null,null,"sgnl_stts ","VARCHAR(100) ","",",",null,"",null,null,null,"sgnl_stts ","VARCHAR2(100) ","",",",null,null,"",null,"COMMENT ON COLUMN ","mtvsphasinfo.","sgnl_stts"," IS ","'신호상태 결합 (rrrgggGGGrr)'",";"]
[null,null,"최소녹색시간","min_gren_hr",6,"NUMBER(3)",null,null,"최소녹색시간",null,null,null,"EQ","최소녹색시간","min_gren_hr","NUMBER(3)","INTEGER","NUMBER(3)",null,null,null,"min_gren_hr ","INTEGER ","",",",null,"",null,null,null,"min_gren_hr ","NUMBER(3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","mtvsphasinfo.","min_gren_hr"," IS ","'최소녹색시간'",";"]
[null,null,"황색시간","yelw_hr",7,"NUMBER(3)",null,null,"황색시간",null,null,null,"EQ","황색시간","yelw_hr","NUMBER(3)","INTEGER","NUMBER(3)",null,null,null,"yelw_hr ","INTEGER ",null,",",null,"",null,null,null,"yelw_hr ","NUMBER(3) ",null,",",null,null,"",null,"COMMENT ON COLUMN ","mtvsphasinfo.","yelw_hr"," IS ","'황색시간'",";"]
[null,null,"적색시간","red_hr",7,"NUMBER(3)",null,null,"적색시간",null,null,null,"EQ","적색시간","red_hr","NUMBER(3)","INTEGER","NUMBER(3)",null,null,null,"red_hr ","INTEGER ",null,",",null,"",null,null,null,"red_hr ","NUMBER(3) ",null,",",null,null,"",null,"COMMENT ON COLUMN ","mtvsphasinfo.","red_hr"," IS ","'적색시간'",";"]
[null,null,"주도로구분코드","majr_road_se_cd",8,"CHAR(2)",null,null,"주도로구분코드 (063)",null,null,"주도로구분 (10:부도로, 20:주도로)","EQ","주도로구분코드","majr_road_se_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",null,null,null,"majr_road_se_cd ","VARCHAR(2) ",{"$f":"IF(H43=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",null,"",null,null,null,"majr_road_se_cd ","VARCHAR2(2) ",{"$f":"IF(H43=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",null,null,"",null,"COMMENT ON COLUMN ","mtvsphasinfo.","majr_road_se_cd"," IS ","'주도로구분코드 (063)'",";"]
[{"$nulls":21},{"$f":"CONCATENATE(Z35:AB44)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AI35:AL43)","v":{"$error":"#VALUE!"}},{"$nulls":16},{"$f":"IF(LEFT(AE44, 13) = \"CONSTRAINT PK\", AE44, \"\")","v":{"$error":"#VALUE!"}}]
[null,"현시정보(시차제) 테이블",{"$nulls":11},"soitsphasinfotmdiff"]
["2022-02-02","Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N45&\" \"","v":"soitsphasinfotmdiff "},null," IS ",{"$f":"\"'\"&B45&\"'\"","v":"'현시정보(시차제) 테이블'"},";"]
[null,"soitsphasinfotmdiff\n(확정)\n시차제 추가","현장교차로ID","spot_ints_id",1,"NUMBER(5)","PK",null,"현장교차로ID",null,null,null,{"$f":"IF(F47=P47, \"EQ\", \"NEQ)\")","v":"EQ"},"현장교차로ID","spot_ints_id","NUMBER(5)","INTEGER","NUMBER(5)",null,"CREATE TABLE ",{"$f":"N45&\" (\"","v":"soitsphasinfotmdiff ("},{"$f":"O47&\" \"","v":"spot_ints_id "},{"$f":"Q47&\" \"","v":"INTEGER "},{"$f":"IF(H47=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",","PRIMARY KEY (",{"$f":"IF(OR(G47=\"PK\", G47=\"PK/FK\"), O47, \"\")","v":"spot_ints_id"},",","CREATE TABLE ",{"$f":"N45&\" (\"","v":"soitsphasinfotmdiff ("},{"$f":"O47&\" \"","v":"spot_ints_id "},{"$f":"R47&\" \"","v":"NUMBER(5) "},{"$f":"IF(H47=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",","CONSTRAINT ",{"$f":"\"PK_\"&N45&\" PRIMARY KEY (\"","v":"PK_soitsphasinfotmdiff PRIMARY KEY ("},{"$f":"IF(OR(G47=\"PK\", G47=\"PK/FK\"), O47, \"\")","v":"spot_ints_id"},",","COMMENT ON COLUMN ",{"$f":"$N$45&\".\"","v":"soitsphasinfotmdiff."},{"$f":"O47","v":"spot_ints_id"}," IS ",{"$f":"\"'\"&I47&\"'\"","v":"'현장교차로ID'"},";"]
[null,null,"노드ID","node_id",2,"VARCHAR2(300)","PK",null,"노드ID",null,null,null,"EQ","노드ID","node_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,null,null,"node_id ","VARCHAR(300) ","",",",null,"node_id",",",null,null,"node_id ","VARCHAR2(300) ","",",",null,null,"node_id",",","COMMENT ON COLUMN ","soitsphasinfotmdiff.","node_id"," IS ","'노드ID'",";"]
[null,null,"주교차로구분코드","majr_ints_se_cd",3,"CHAR(2)","PK",null,"주교차로구분코드 (062)",null,null,"주교차로구분 (1:주교차로, 2:연등교차로)","EQ","주교차로구분코드","majr_ints_se_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",null,null,null,"majr_ints_se_cd ","VARCHAR(2) ","",",",null,"majr_ints_se_cd",",",null,null,"majr_ints_se_cd ","VARCHAR2(2) ","",",",null,null,"majr_ints_se_cd",",","COMMENT ON COLUMN ","soitsphasinfotmdiff.","majr_ints_se_cd"," IS ","'주교차로구분코드 (062)'",";"]
[null,null,"현시번호","phas_no",4,"NUMBER(2)","PK",null,"현시번호",null,null,null,"EQ","현시번호","phas_no","NUMBER(2)","INTEGER","NUMBER(2)",null,null,null,"phas_no ","INTEGER ","",",",null,"phas_no","));",null,null,"phas_no ","NUMBER(2) ","",",",null,null,"phas_no",{"$f":"\") using index tablespace \" &AJ57& \") TABLESPACE \" &AI57&\";\"","v":") using index tablespace SOIT_I08_M001) TABLESPACE SOIT_D08_M001;"},"COMMENT ON COLUMN ","soitsphasinfotmdiff.","phas_no"," IS ","'현시번호'",";"]
[null,null,"신호상태","sgnl_stts",5,"CHAR(100)",null,null,"신호상태 결합 (rrrgggGGGrr)",null,null,null,"EQ","신호상태","sgnl_stts","CHAR(100)","VARCHAR(100)","VARCHAR2(100)",null,null,null,"sgnl_stts ","VARCHAR(100) ","",",",null,"",null,null,null,"sgnl_stts ","VARCHAR2(100) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsphasinfotmdiff.","sgnl_stts"," IS ","'신호상태 결합 (rrrgggGGGrr)'",";"]
[null,null,"최소녹색시간","min_gren_hr",6,"NUMBER(3)",null,null,"최소녹색시간",null,null,null,"EQ","최소녹색시간","min_gren_hr","NUMBER(3)","INTEGER","NUMBER(3)",null,null,null,"min_gren_hr ","INTEGER ","",",",null,"",null,null,null,"min_gren_hr ","NUMBER(3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsphasinfotmdiff.","min_gren_hr"," IS ","'최소녹색시간'",";"]
[null,null,"황색시간","yelw_hr",7,"NUMBER(3)",null,null,"황색시간",null,null,null,"EQ","황색시간","yelw_hr","NUMBER(3)","INTEGER","NUMBER(3)",null,null,null,"yelw_hr ","INTEGER ",null,",",null,"",null,null,null,"yelw_hr ","NUMBER(3) ",null,",",null,null,"",null,"COMMENT ON COLUMN ","soitsphasinfotmdiff.","yelw_hr"," IS ","'황색시간'",";"]
[null,null,"적색시간","red_hr",8,"NUMBER(3)",null,null,"적색시간",{"$nulls":4},"적색시간","red_hr","NUMBER(3)","INTEGER","NUMBER(3)",null,null,null,"red_hr ","INTEGER ",null,",",null,"",null,null,null,"red_hr ","NUMBER(3) ",null,",",null,null,"",null,"COMMENT ON COLUMN ",{"$f":"$N$21&\".\"","v":"soitsphasinfo."},"red_hr"," IS ","'적색시간'",";"]
[null,null,"주도로구분코드","majr_road_se_cd",9,"CHAR(2)",null,null,"주도로구분코드 (063)",null,null,"주도로구분 (10:부도로, 20:주도로)",{"$f":"IF(F55=P55, \"EQ\", \"NEQ)\")","v":"EQ"},"주도로구분코드","majr_road_se_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",null,null,null,"majr_road_se_cd ","VARCHAR(2) ",{"$f":"IF(H55=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",null,"",null,null,null,"majr_road_se_cd ","VARCHAR2(2) ",{"$f":"IF(H55=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",null,null,"",null,"COMMENT ON COLUMN ",{"$f":"$N$45&\".\"","v":"soitsphasinfotmdiff."},"majr_road_se_cd"," IS ","'주도로구분코드 (063)'",";"]
[{"$nulls":21},{"$f":"CONCATENATE(Z47:AB56)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AI47:AL55)","v":{"$error":"#VALUE!"}},{"$nulls":16},{"$f":"IF(LEFT(AE56, 13) = \"CONSTRAINT PK\", AE56, \"\")","v":{"$error":"#VALUE!"}}]
[null,"(메타버스) 현시정보(시차제) 테이블",{"$nulls":11},"mtvsphasinfotmdiff",{"$nulls":20},"SOIT_D08_M001","SOIT_I08_M001"]
["2023-02-22","Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N57&\" \"","v":"mtvsphasinfotmdiff "},null," IS ",{"$f":"\"'\"&B57&\"'\"","v":"'(메타버스) 현시정보(시차제) 테이블'"},";"]
[null,"mtvsphasinfotmdiff","현장교차로ID","spot_ints_id",1,"NUMBER(5)","PK",null,"현장교차로ID",null,null,null,{"$f":"IF(F59=P59, \"EQ\", \"NEQ)\")","v":"EQ"},"현장교차로ID","spot_ints_id","NUMBER(5)","INTEGER","NUMBER(5)",null,"CREATE TABLE ",{"$f":"N57&\" (\"","v":"mtvsphasinfotmdiff ("},{"$f":"O59&\" \"","v":"spot_ints_id "},{"$f":"Q59&\" \"","v":"INTEGER "},{"$f":"IF(H59=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",","PRIMARY KEY (",{"$f":"IF(OR(G59=\"PK\", G59=\"PK/FK\"), O59, \"\")","v":"spot_ints_id"},",","CREATE TABLE ",{"$f":"N57&\" (\"","v":"mtvsphasinfotmdiff ("},{"$f":"O59&\" \"","v":"spot_ints_id "},{"$f":"R59&\" \"","v":"NUMBER(5) "},{"$f":"IF(H59=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",","CONSTRAINT ",{"$f":"\"PK_\"&N57&\" PRIMARY KEY (\"","v":"PK_mtvsphasinfotmdiff PRIMARY KEY ("},{"$f":"IF(OR(G59=\"PK\", G59=\"PK/FK\"), O59, \"\")","v":"spot_ints_id"},",","COMMENT ON COLUMN ",{"$f":"$N$57&\".\"","v":"mtvsphasinfotmdiff."},{"$f":"O59","v":"spot_ints_id"}," IS ",{"$f":"\"'\"&I59&\"'\"","v":"'현장교차로ID'"},";"]
[null,null,"노드ID","node_id",2,"VARCHAR2(300)","PK",null,"노드ID",null,null,null,"EQ","노드ID","node_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,null,null,"node_id ","VARCHAR(300) ","",",",null,"node_id",",",null,null,"node_id ","VARCHAR2(300) ","",",",null,null,"node_id",",","COMMENT ON COLUMN ","mtvsphasinfotmdiff.","node_id"," IS ","'노드ID'",";"]
[null,null,"주교차로구분코드","majr_ints_se_cd",3,"CHAR(2)","PK",null,"주교차로구분코드 (062)",null,null,"주교차로구분 (1:주교차로, 2:연등교차로)","EQ","주교차로구분코드","majr_ints_se_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",null,null,null,"majr_ints_se_cd ","VARCHAR(2) ","",",",null,"majr_ints_se_cd",",",null,null,"majr_ints_se_cd ","VARCHAR2(2) ","",",",null,null,"majr_ints_se_cd",",","COMMENT ON COLUMN ","mtvsphasinfotmdiff.","majr_ints_se_cd"," IS ","'주교차로구분코드 (062)'",";"]
[null,null,"현시번호","phas_no",4,"NUMBER(2)","PK",null,"현시번호",null,null,null,"EQ","현시번호","phas_no","NUMBER(2)","INTEGER","NUMBER(2)",null,null,null,"phas_no ","INTEGER ","",",",null,"phas_no","));",null,null,"phas_no ","NUMBER(2) ","",",",null,null,"phas_no",") using index tablespace SOIT_I08);","COMMENT ON COLUMN ","mtvsphasinfotmdiff.","phas_no"," IS ","'현시번호'",";"]
[null,null,"신호상태","SOITGKNCRSTATS",5,"CHAR(100)",null,null,"신호상태 결합 (rrrgggGGGrr)",null,null,null,"EQ","신호상태","sgnl_stts","CHAR(100)","VARCHAR(100)","VARCHAR2(100)",null,null,null,"sgnl_stts ","VARCHAR(100) ","",",",null,"",null,null,null,"sgnl_stts ","VARCHAR2(100) ","",",",null,null,"",null,"COMMENT ON COLUMN ","mtvsphasinfotmdiff.","sgnl_stts"," IS ","'신호상태 결합 (rrrgggGGGrr)'",";"]
[null,null,"최소녹색시간","min_gren_hr",6,"NUMBER(3)",null,null,"최소녹색시간",null,null,null,"EQ","최소녹색시간","min_gren_hr","NUMBER(3)","INTEGER","NUMBER(3)",null,null,null,"min_gren_hr ","INTEGER ","",",",null,"",null,null,null,"min_gren_hr ","NUMBER(3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","mtvsphasinfotmdiff.","min_gren_hr"," IS ","'최소녹색시간'",";"]
[null,null,"황색시간","yelw_hr",7,"NUMBER(3)",null,null,"황색시간",null,null,null,"EQ","황색시간","yelw_hr","NUMBER(3)","INTEGER","NUMBER(3)",null,null,null,"yelw_hr ","INTEGER ",null,",",null,"",null,null,null,"yelw_hr ","NUMBER(3) ",null,",",null,null,"",null,"COMMENT ON COLUMN ","mtvsphasinfotmdiff.","yelw_hr"," IS ","'황색시간'",";"]
[null,null,"적색시간","red_hr",7,"NUMBER(3)",null,null,"적색시간",{"$nulls":4},"적색시간","red_hr","NUMBER(3)","INTEGER","NUMBER(3)",null,null,null,"red_hr ","INTEGER ",null,",",null,"",null,null,null,"red_hr ","NUMBER(3) ",null,",",null,null,"",null,"COMMENT ON COLUMN ","mtvsphasinfotmdiff.","red_hr"," IS ","'적색시간'",";"]
[null,null,"주도로구분코드","majr_road_se_cd",8,"CHAR(2)",null,null,"주도로구분코드 (063)",null,null,"주도로구분 (10:부도로, 20:주도로)",{"$f":"IF(F67=P67, \"EQ\", \"NEQ)\")","v":"EQ"},"주도로구분코드","majr_road_se_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",null,null,null,"majr_road_se_cd ","VARCHAR(2) ",{"$f":"IF(H67=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",null,"",null,null,null,"majr_road_se_cd ","VARCHAR2(2) ",{"$f":"IF(H67=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",null,null,"",null,"COMMENT ON COLUMN ","mtvsphasinfotmdiff.","majr_road_se_cd"," IS ","'주도로구분코드 (063)'",";"]
[{"$nulls":21},{"$f":"CONCATENATE(Z59:AB68)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AI59:AL67)","v":{"$error":"#VALUE!"}},{"$nulls":16},{"$f":"IF(LEFT(AE68, 13) = \"CONSTRAINT PK\", AE68, \"\")","v":{"$error":"#VALUE!"}}]
[null,"연결차로 신호상태순서 테이블",{"$nulls":11},"soitsintscnctlaneinfo"]
[3,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N69&\" \"","v":"soitsintscnctlaneinfo "},null," IS ",{"$f":"\"'\"&B69&\"'\"","v":"'연결차로 신호상태순서 테이블'"},";",null,null,null,{"$f":"IF(LEFT(AE70, 13) = \"CONSTRAINT PK\", AE70, \"\")","v":""}]
[null,"soitsintscnctlaneinfo\n(확정)","현장교차로ID","spot_ints_id",1,"NUMBER(5)","PK",null,"현장교차로ID",null,null,null,{"$f":"IF(F71=P71, \"EQ\", \"NEQ)\")","v":"EQ"},"현장교차로ID","spot_ints_id","NUMBER(5)","INTEGER","NUMBER(5)",null,"CREATE TABLE ",{"$f":"N69&\" (\"","v":"soitsintscnctlaneinfo ("},{"$f":"O71&\" \"","v":"spot_ints_id "},{"$f":"Q71&\" \"","v":"INTEGER "},{"$f":"IF(H71=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",","PRIMARY KEY (",{"$f":"IF(OR(G71=\"PK\", G71=\"PK/FK\"), O71, \"\")","v":"spot_ints_id"},",","CREATE TABLE ",{"$f":"N69&\" (\"","v":"soitsintscnctlaneinfo ("},{"$f":"O71&\" \"","v":"spot_ints_id "},{"$f":"R71&\" \"","v":"NUMBER(5) "},{"$f":"IF(H71=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",","CONSTRAINT ",{"$f":"\"PK_\"&N69&\" PRIMARY KEY (\"","v":"PK_soitsintscnctlaneinfo PRIMARY KEY ("},{"$f":"IF(OR(G71=\"PK\", G71=\"PK/FK\"), O71, \"\")","v":"spot_ints_id"},",","COMMENT ON COLUMN ",{"$f":"$N$69&\".\"","v":"soitsintscnctlaneinfo."},{"$f":"O71","v":"spot_ints_id"}," IS ",{"$f":"\"'\"&I71&\"'\"","v":"'현장교차로ID'"},";",null,null,null,""]
[null,null,"노드ID","node_id",2,"VARCHAR2(300)","PK",null,"노드ID",null,null,null,"EQ","노드ID","node_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,null,null,"node_id ","VARCHAR(300) ","",",",null,"node_id",",",null,null,"node_id ","VARCHAR2(300) ","",",",null,null,"node_id",",","COMMENT ON COLUMN ","soitsintscnctlaneinfo.","node_id"," IS ","'노드ID'",";",null,null,null,""]
[null,null,"신호상태순서","sgnl_stts_seq",3,"NUMBER(5)","PK",null,"신호상태순서",null,null,null,"EQ","신호상태순서","sgnl_stts_seq","NUMBER(5)","INTEGER","INTEGER",null,null,null,"sgnl_stts_seq ","INTEGER ","",",",null,"sgnl_stts_seq","));",null,null,"sgnl_stts_seq ","INTEGER ","",",",null,null,"sgnl_stts_seq",{"$f":"\") using index tablespace \" &AJ76& \") TABLESPACE \" &AI76&\";\"","v":") using index tablespace SOIT_I08_M001) TABLESPACE SOIT_D08_M001;"},"COMMENT ON COLUMN ","soitsintscnctlaneinfo.","sgnl_stts_seq"," IS ","'신호상태순서'",";",null,null,null,""]
[null,null,"연결차로ID","cnct_lane_id",4,"VARCHAR2(300)",null,null,"연결차로 ID",null,null,null,"EQ","연결차로ID","cnct_lane_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,null,null,"cnct_lane_id ","VARCHAR(300) ","",",",{"$nulls":5},"cnct_lane_id ","VARCHAR2(300) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsintscnctlaneinfo.","cnct_lane_id"," IS ","'연결차로 ID'",";",null,null,null,""]
[{"$nulls":21},{"$f":"CONCATENATE(Z71:AB75)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AI71:AL74)","v":{"$error":"#VALUE!"}},{"$nulls":16},{"$error":"#VALUE!"}]
[null,"(메타버스) 연결차로 신호상태순서 테이블",{"$nulls":11},"mtvsintscnctlaneinfo",{"$nulls":20},"SOIT_D08_M001","SOIT_I08_M001"]
["2023-03-01","Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N76&\" \"","v":"mtvsintscnctlaneinfo "},null," IS ",{"$f":"\"'\"&B76&\"'\"","v":"'(메타버스) 연결차로 신호상태순서 테이블'"},";",null,null,null,{"$f":"IF(LEFT(AE77, 13) = \"CONSTRAINT PK\", AE77, \"\")","v":""}]
[null,"mtvsintscnctlaneinfo","현장교차로ID","spot_ints_id",1,"NUMBER(5)","PK",null,"현장교차로ID",null,null,null,{"$f":"IF(F78=P78, \"EQ\", \"NEQ)\")","v":"EQ"},"현장교차로ID","spot_ints_id","NUMBER(5)","INTEGER","NUMBER(5)",null,"CREATE TABLE ",{"$f":"N76&\" (\"","v":"mtvsintscnctlaneinfo ("},{"$f":"O78&\" \"","v":"spot_ints_id "},{"$f":"Q78&\" \"","v":"INTEGER "},{"$f":"IF(H78=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",","PRIMARY KEY (",{"$f":"IF(OR(G78=\"PK\", G78=\"PK/FK\"), O78, \"\")","v":"spot_ints_id"},",","CREATE TABLE ",{"$f":"N76&\" (\"","v":"mtvsintscnctlaneinfo ("},{"$f":"O78&\" \"","v":"spot_ints_id "},{"$f":"R78&\" \"","v":"NUMBER(5) "},{"$f":"IF(H78=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",","CONSTRAINT ",{"$f":"\"PK_\"&N76&\" PRIMARY KEY (\"","v":"PK_mtvsintscnctlaneinfo PRIMARY KEY ("},{"$f":"IF(OR(G78=\"PK\", G78=\"PK/FK\"), O78, \"\")","v":"spot_ints_id"},",","COMMENT ON COLUMN ",{"$f":"$N$76&\".\"","v":"mtvsintscnctlaneinfo."},{"$f":"O78","v":"spot_ints_id"}," IS ",{"$f":"\"'\"&I78&\"'\"","v":"'현장교차로ID'"},";",null,null,null,""]
[null,null,"노드ID","node_id",2,"VARCHAR2(300)","PK",null,"노드ID",null,null,null,"EQ","노드ID","node_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,null,null,"node_id ","VARCHAR(300) ","",",",null,"node_id",",",null,null,"node_id ","VARCHAR2(300) ","",",",null,null,"node_id",",","COMMENT ON COLUMN ","mtvsintscnctlaneinfo.","node_id"," IS ","'노드ID'",";",null,null,null,""]
[null,null,"신호상태순서","sgnl_stts_seq",3,"NUMBER(5)","PK",null,"신호상태순서",null,null,null,"EQ","신호상태순서","sgnl_stts_seq","NUMBER(5)","INTEGER","INTEGER",null,null,null,"sgnl_stts_seq ","INTEGER ","",",",null,"sgnl_stts_seq","));",null,null,"sgnl_stts_seq ","INTEGER ","",",",null,null,"sgnl_stts_seq",") using index tablespace SOIT_I08);","COMMENT ON COLUMN ","mtvsintscnctlaneinfo.","sgnl_stts_seq"," IS ","'신호상태순서'",";",null,null,null,""]
[null,null,"연결차로ID","cnct_lane_id",4,"VARCHAR2(300)",null,null,"연결차로 ID",null,null,null,"EQ","연결차로ID","cnct_lane_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,null,null,"cnct_lane_id ","VARCHAR(300) ","",",",{"$nulls":5},"cnct_lane_id ","VARCHAR2(300) ","",",",null,null,"",null,"COMMENT ON COLUMN ","mtvsintscnctlaneinfo.","cnct_lane_id"," IS ","'연결차로 ID'",";",null,null,null,""]
[{"$nulls":21},{"$f":"CONCATENATE(Z78:AB82)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AI78:AL81)","v":{"$error":"#VALUE!"}},{"$nulls":16},{"$error":"#VALUE!"}]
[null,"현시신호정보 테이블 (1분 단위로 동인 신호이력으로 생성되는 테이블) - 참조 테이블 : soitsphasinfo / soitsphasinfotmdiff",{"$nulls":11},"soitsphassgnlinfo",{"$nulls":33},""]
[4,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N83&\" \"","v":"soitsphassgnlinfo "},null," IS ",{"$f":"\"'\"&B83&\"'\"","v":"'현시신호정보 테이블 (1분 단위로 동인 신호이력으로 생성되는 테이블) - 참조 테이블 : soitsphasinfo / soitsphasinfotmdiff'"},";",null,null,null,""]
[null,"soitsphassgnlinfo\n(확정)","수집유닉스시각","clct_unix_tm",1,"NUMBER(10)","PK",null,"동인 신호이력수집시각",null,null,null,{"$f":"IF(F85=P85, \"EQ\", \"NEQ)\")","v":"EQ"},"수집유닉스시각","clct_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",null,"CREATE TABLE ",{"$f":"N83&\" (\"","v":"soitsphassgnlinfo ("},{"$f":"O85&\" \"","v":"clct_unix_tm "},{"$f":"Q85&\" \"","v":"INTEGER "},{"$f":"IF(H85=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",","PRIMARY KEY (",{"$f":"IF(OR(G85=\"PK\", G85=\"PK/FK\"), O85, \"\")","v":"clct_unix_tm"},",","CREATE TABLE ",{"$f":"N83&\" (\"","v":"soitsphassgnlinfo ("},{"$f":"O85&\" \"","v":"clct_unix_tm "},{"$f":"R85&\" \"","v":"NUMBER(10) "},{"$f":"IF(H85=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",null,"(",{"$f":"IF(OR(G85=\"PK\", G85=\"PK/FK\"), O85, \"\")","v":"clct_unix_tm"},",","COMMENT ON COLUMN ",{"$f":"$N$83&\".\"","v":"soitsphassgnlinfo."},{"$f":"O85","v":"clct_unix_tm"}," IS ",{"$f":"\"'\"&I85&\"'\"","v":"'동인 신호이력수집시각'"},";",null,null,null,""]
[null,null,"시작유닉스시각","bgng_unix_tm",2,"NUMBER(10)","PK",null,"신호 시작시각(주기)",null,null,null,"EQ","시작유닉스시각","bgng_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",null,null,null,"bgng_unix_tm ","INTEGER ","",",",null,"bgng_unix_tm",",",null,null,"bgng_unix_tm ","NUMBER(10) ","",",",null,null,"bgng_unix_tm",",","COMMENT ON COLUMN ","soitsphassgnlinfo.","bgng_unix_tm"," IS ","'신호 시작시각(주기)'",";",null,null,null,""]
[null,null,"실측여부","acsr_yn",3,"CHAR(1)","PK",null,"실측여부 (500)",null,null,"실측여부 (Y/N)","EQ","실측여부","acsr_yn","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",null,null,null,"acsr_yn ","VARCHAR(1) ","",",",null,"acsr_yn",",",null,null,"acsr_yn ","VARCHAR2(1) ","",",",null,null,"acsr_yn",",","COMMENT ON COLUMN ","soitsphassgnlinfo.","acsr_yn"," IS ","'실측여부 (500)'",";",null,null,null,""]
[null,null,"참조정보구분코드","ref_info_se_cd",4,"CHAR(1)",null,null,"참조정보구분코드(504)",null,null,"참조정보구분코드 (1:이력정보, 2:LC_카운트, 3:TOD)","EQ","참조정보구분코드","ref_info_se_cd","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",null,null,null,"ref_info_se_cd ","VARCHAR(1) ","",",",null,"",null,null,null,"ref_info_se_cd ","VARCHAR2(1) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsphassgnlinfo.","ref_info_se_cd"," IS ","'참조정보구분코드(504)'",";",null,null,null,""]
[null,null,"현장교차로ID","spot_ints_id",5,"NUMBER(5)","PK/FK",null,"현장교차로ID",null,null,null,"EQ","현장교차로ID","spot_ints_id","NUMBER(5)","INTEGER","NUMBER(5)",null,null,null,"spot_ints_id ","INTEGER ","",",",null,"spot_ints_id",",",null,null,"spot_ints_id ","NUMBER(5) ","",",",null,null,"spot_ints_id",",","COMMENT ON COLUMN ","soitsphassgnlinfo.","spot_ints_id"," IS ","'현장교차로ID'",";",null,null,null,""]
[null,null,"노드ID","node_id",6,"VARCHAR2(300)","PK/FK",null,"해당 교차로 노드ID",null,null,null,"EQ","노드ID","node_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,null,null,"node_id ","VARCHAR(300) ","",",",null,"node_id",",",null,null,"node_id ","VARCHAR2(300) ","",",",null,null,"node_id",",","COMMENT ON COLUMN ","soitsphassgnlinfo.","node_id"," IS ","'해당 교차로 노드ID'",";",null,null,null,""]
[null,null,"주교차로구분코드","majr_ints_se_cd",7,"CHAR(2)",null,null,"주교차로구분코드 (062)",null,null,"주교차로구분 (1:주교차로, 2:연등교차로)","EQ","주교차로구분코드","majr_ints_se_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",null,null,null,"majr_ints_se_cd ","VARCHAR(2) ","",",",null,"",null,null,null,"majr_ints_se_cd ","VARCHAR2(2) ","",",",null,null,"",{"$f":"IF(OR(H91=\"PK\", H91=\"PK/FK\"), P91, \"\")","v":""},"COMMENT ON COLUMN ","soitsphassgnlinfo.","majr_ints_se_cd"," IS ","'주교차로구분코드 (062)'",";",null,null,null,""]
[null,null,"신호상태","sgnl_stts",8,"CHAR(100)",null,null,"신호상태 결합 (rrrgggGGGrr)",null,null,null,"EQ","신호상태","sgnl_stts","CHAR(100)","VARCHAR(100)","VARCHAR2(100)",null,null,null,"sgnl_stts ","VARCHAR(100) ","",",",null,"",null,null,null,"sgnl_stts ","VARCHAR2(100) ","",",",null,null,"","","COMMENT ON COLUMN ","soitsphassgnlinfo.","sgnl_stts"," IS ","'신호상태 결합 (rrrgggGGGrr)'",";",null,null,null,""]
[null,null,"제어구분코드","ctrl_se_cd",9,"NUMBER(3)",null,null,"제어구분코드",null,null,"제어구분코드(009)","EQ","제어구분코드","ctrl_se_cd","NUMBER(3)","INTEGER","NUMBER(3)",null,null,null,"ctrl_se_cd ","INTEGER ","",",",null,"",null,null,null,"ctrl_se_cd ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitsphassgnlinfo.","ctrl_se_cd"," IS ","'제어구분코드'",";",null,null,null,""]
[null,null,"제어상태코드","ctrl_stts_cd",10,"NUMBER(3)",null,null,"제어상태코드",null,null,"제어상태코드(010)","EQ","제어상태코드","ctrl_stts_cd","NUMBER(3)","INTEGER","NUMBER(3)",null,null,null,"ctrl_stts_cd ","INTEGER ","",",",null,"",null,null,null,"ctrl_stts_cd ","NUMBER(3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsphassgnlinfo.","ctrl_stts_cd"," IS ","'제어상태코드'",";",null,null,null,""]
[null,null,"주기시간","cycl_hr",11,"NUMBER(3)",null,null,"주기시간",null,null,null,"EQ","주기시간","cycl_hr","NUMBER(3)","INTEGER","NUMBER(3)",null,null,null,"cycl_hr ","INTEGER ","",",",null,"",null,null,null,"cycl_hr ","NUMBER(3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsphassgnlinfo.","cycl_hr"," IS ","'주기시간'",";",null,null,null,""]
[null,null,"옵셋시간","ofst_hr",12,"NUMBER(3)",null,null,"옵셋시간",null,null,null,"EQ","옵셋시간","ofst_hr","NUMBER(3)","INTEGER","NUMBER(3)",null,null,null,"ofst_hr ","INTEGER ","",",",null,"",null,null,null,"ofst_hr ","NUMBER(3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsphassgnlinfo.","ofst_hr"," IS ","'옵셋시간'",";",null,null,null,""]
[null,null,"현시번호","phas_no",13,"NUMBER(2)","PK",null,"현시번호 (1~8)",null,null,null,"EQ","현시번호","phas_no","NUMBER(2)","INTEGER","NUMBER(2)",null,null,null,"phas_no ","INTEGER ","",",",null,"phas_no",",",null,null,"phas_no ","NUMBER(2) ","",",",null,null,"phas_no",",","COMMENT ON COLUMN ","soitsphassgnlinfo.","phas_no"," IS ","'현시번호 (1~8)'",";",null,null,null,""]
[null,null,"황색시간","yelw_hr",14,"NUMBER(3)",null,null,"황색시간",null,null,null,"EQ","황색시간","yelw_hr","NUMBER(3)","INTEGER","NUMBER(3)",null,null,null,"yelw_hr ","INTEGER ","",",",null,"",null,null,null,"yelw_hr ","NUMBER(3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsphassgnlinfo.","yelw_hr"," IS ","'황색시간'",";",null,null,null,""]
[null,null,"주도로구분코드","majr_road_se_cd",15,"CHAR(2)",null,null,"주도로구분코드 (063)",null,null,"주도로구분 (10:부도로, 20:주도로)","EQ","주도로구분코드","majr_road_se_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",null,null,null,"majr_road_se_cd ","VARCHAR(2) ","",",",null,"",null,null,null,"majr_road_se_cd ","VARCHAR2(2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsphassgnlinfo.","majr_road_se_cd"," IS ","'주도로구분코드 (063)'",";",null,null,null,""]
[null,null,"진행상태코드","prgrs_stts_cd",16,"CHAR(2)",null,null,"진행상태코드(506)",null,null,"0:초기셋팅, 1:신호이력insert, 2:종료시각update, 3:황색시간insert\n데이터 처리 종료 후 - 11:신호이력insert, 12:종료시각update, 13:황색시간insert","EQ","진행상태코드","prgrs_stts_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",null,null,null,"prgrs_stts_cd ","VARCHAR(2) ","",",",null,"",null,null,null,"prgrs_stts_cd ","VARCHAR2(2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsphassgnlinfo.","prgrs_stts_cd"," IS ","'진행상태코드(506)'",";",null,null,null,""]
[null,null,"현시시간","phas_hr",17,"NUMBER(3)",null,null,"현시소요시간",null,null,null,"EQ","현시시간","phas_hr","NUMBER(3)","INTEGER","NUMBER(3)",null,null,null,"phas_hr ","INTEGER ","",",",null,"",null,null,null,"phas_hr ","NUMBER(3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsphassgnlinfo.","phas_hr"," IS ","'현시소요시간'",";",null,null,null,""]
[null,null,"현시시작시간","phas_bgng_unix_tm",18,"NUMBER(10)","PK",null,"신호 시작시각(현시)",null,null,null,"EQ","현시시작시간","phas_bgng_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",null,null,null,"phas_bgng_unix_tm ","INTEGER ","",",",null,"phas_bgng_unix_tm","));",null,null,"phas_bgng_unix_tm ","NUMBER(10) ","",",",null,null,"phas_bgng_unix_tm",")","COMMENT ON COLUMN ","soitsphassgnlinfo.","phas_bgng_unix_tm"," IS ","'신호 시작시각(현시)'",";",null,null,null,""]
[null,null,"입력일시","inpt_dt",19,"TIMESTAMP",null,"NOT NULL","데이터입력일시",null,null,null,"EQ","입력일시","inpt_dt","TIMESTAMP","TIMESTAMP","TIMESTAMP",null,null,null,"inpt_dt ",{"$f":"IF(Q103=\"TIMESTAMP\", Q103&\" DEFAULT NOW \", Q103&\" \")","v":"TIMESTAMP DEFAULT NOW "},"NOT NULL",",",null,"",null,null,null,"inpt_dt ","TIMESTAMP ","NOT NULL",{"$f":"\") TABLESPACE \"&AI105&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_S001 NOLOGGING"},null,null,{"$f":"IF(OR(F103=\"PK\", F103=\"PK/FK\"), H103, \"\")","v":""},null,"COMMENT ON COLUMN ","soitsphassgnlinfo.","inpt_dt"," IS ","'데이터입력일시'",";",null,null,null,""]
[{"$nulls":21},{"$f":"CONCATENATE(Z85:AB100)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AI104:AK104)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (clct_unix_tm) INTERVAL (3600) STORE IN (\"&AI105&\") (PARTITION BFR_\" & N83& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AI105&\");\"","v":"PARTITION BY RANGE (clct_unix_tm) INTERVAL (3600) STORE IN (SOIT_D08_S001) (PARTITION BFR_soitsphassgnlinfo_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_S001);"},{"$f":"\"CREATE INDEX PK_\" & N83& \" ON \" & N83 & CONCATENATE(AJ85:AL102) & \" LOCAL (PARTITION BFR_\" & N83 & \"_20221101 TABLESPACE \"&AJ105&\") TABLESPACE \"&AJ105&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & N83 & \" ADD CONSTRAINT PK_\" & N83 & \" PRIMARY KEY \" & CONCATENATE(AJ85:AL102) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":10},{"$error":"#VALUE!"}]
[null,"(메타버스) 현시신호정보 테이블 (1분 단위로 동인 신호이력으로 생성되는 테이블) - 참조 테이블 : soitsphasinfo / soitsphasinfotmdiff",{"$nulls":11},"mtvsphassgnlinfo",{"$nulls":20},"SOIT_D08_S001","SOIT_I08_S001",{"$nulls":11},""]
["2023-04-01","Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N105&\" \"","v":"mtvsphassgnlinfo "},null," IS ",{"$f":"\"'\"&B105&\"'\"","v":"'(메타버스) 현시신호정보 테이블 (1분 단위로 동인 신호이력으로 생성되는 테이블) - 참조 테이블 : soitsphasinfo / soitsphasinfotmdiff'"},";",null,null,null,""]
[null,"mtvsphassgnlinfo","수집유닉스시각","clct_unix_tm",1,"NUMBER(10)","PK",null,"동인 신호이력수집시각",null,null,null,{"$f":"IF(F107=P107, \"EQ\", \"NEQ)\")","v":"EQ"},"수집유닉스시각","clct_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",null,"CREATE TABLE ",{"$f":"N105&\" (\"","v":"mtvsphassgnlinfo ("},{"$f":"O107&\" \"","v":"clct_unix_tm "},{"$f":"Q107&\" \"","v":"INTEGER "},{"$f":"IF(H107=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",","PRIMARY KEY (",{"$f":"IF(OR(G107=\"PK\", G107=\"PK/FK\"), O107, \"\")","v":"clct_unix_tm"},",","CREATE TABLE ",{"$f":"N105&\" (\"","v":"mtvsphassgnlinfo ("},{"$f":"O107&\" \"","v":"clct_unix_tm "},{"$f":"R107&\" \"","v":"NUMBER(10) "},{"$f":"IF(H107=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",null,"(",{"$f":"IF(OR(G107=\"PK\", G107=\"PK/FK\"), O107, \"\")","v":"clct_unix_tm"},",","COMMENT ON COLUMN ",{"$f":"$N$105&\".\"","v":"mtvsphassgnlinfo."},{"$f":"O107","v":"clct_unix_tm"}," IS ",{"$f":"\"'\"&I107&\"'\"","v":"'동인 신호이력수집시각'"},";",null,null,null,""]
[null,null,"시작유닉스시각","bgng_unix_tm",2,"NUMBER(10)","PK",null,"신호 시작시각(주기)",null,null,null,"EQ","시작유닉스시각","bgng_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",null,null,null,"bgng_unix_tm ","INTEGER ","",",",null,"bgng_unix_tm",",",null,null,"bgng_unix_tm ","NUMBER(10) ","",",",null,null,"bgng_unix_tm",",","COMMENT ON COLUMN ","mtvsphassgnlinfo.","bgng_unix_tm"," IS ","'신호 시작시각(주기)'",";",null,null,null,""]
[null,null,"실측여부","acsr_yn",3,"CHAR(1)","PK",null,"실측여부 (500)",null,null,"실측여부 (Y/N)","EQ","실측여부","acsr_yn","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",null,null,null,"acsr_yn ","VARCHAR(1) ","",",",null,"acsr_yn",",",null,null,"acsr_yn ","VARCHAR2(1) ","",",",null,null,"acsr_yn",",","COMMENT ON COLUMN ","mtvsphassgnlinfo.","acsr_yn"," IS ","'실측여부 (500)'",";",null,null,null,""]
[null,null,"참조정보구분코드","ref_info_se_cd",4,"CHAR(1)",null,null,"참조정보구분코드(504)",null,null,"참조정보구분코드 (1:이력정보, 2:LC_카운트, 3:TOD)","EQ","참조정보구분코드","ref_info_se_cd","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",null,null,null,"ref_info_se_cd ","VARCHAR(1) ","",",",null,"",null,null,null,"ref_info_se_cd ","VARCHAR2(1) ","",",",null,null,"",null,"COMMENT ON COLUMN ","mtvsphassgnlinfo.","ref_info_se_cd"," IS ","'참조정보구분코드(504)'",";",null,null,null,""]
[null,null,"현장교차로ID","spot_ints_id",5,"NUMBER(5)","PK/FK",null,"현장교차로ID",null,null,null,"EQ","현장교차로ID","spot_ints_id","NUMBER(5)","INTEGER","NUMBER(5)",null,null,null,"spot_ints_id ","INTEGER ","",",",null,"spot_ints_id",",",null,null,"spot_ints_id ","NUMBER(5) ","",",",null,null,"spot_ints_id",",","COMMENT ON COLUMN ","mtvsphassgnlinfo.","spot_ints_id"," IS ","'현장교차로ID'",";",null,null,null,""]
[null,null,"노드ID","node_id",6,"VARCHAR2(300)","PK/FK",null,"해당 교차로 노드ID",null,null,null,"EQ","노드ID","node_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,null,null,"node_id ","VARCHAR(300) ","",",",null,"node_id",",",null,null,"node_id ","VARCHAR2(300) ","",",",null,null,"node_id",",","COMMENT ON COLUMN ","mtvsphassgnlinfo.","node_id"," IS ","'해당 교차로 노드ID'",";",null,null,null,""]
[null,null,"주교차로구분코드","majr_ints_se_cd",7,"CHAR(2)",null,null,"주교차로구분코드 (062)",null,null,"주교차로구분 (1:주교차로, 2:연등교차로)","EQ","주교차로구분코드","majr_ints_se_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",null,null,null,"majr_ints_se_cd ","VARCHAR(2) ","",",",null,"",null,null,null,"majr_ints_se_cd ","VARCHAR2(2) ","",",",null,null,"",{"$f":"IF(OR(H113=\"PK\", H113=\"PK/FK\"), P113, \"\")","v":""},"COMMENT ON COLUMN ","mtvsphassgnlinfo.","majr_ints_se_cd"," IS ","'주교차로구분코드 (062)'",";",null,null,null,""]
[null,null,"신호상태","sgnl_stts",8,"CHAR(100)",null,null,"신호상태 결합 (rrrgggGGGrr)",null,null,null,"EQ","신호상태","sgnl_stts","CHAR(100)","VARCHAR(100)","VARCHAR2(100)",null,null,null,"sgnl_stts ","VARCHAR(100) ","",",",null,"",null,null,null,"sgnl_stts ","VARCHAR2(100) ","",",",null,null,"","","COMMENT ON COLUMN ","mtvsphassgnlinfo.","sgnl_stts"," IS ","'신호상태 결합 (rrrgggGGGrr)'",";",null,null,null,""]
[null,null,"제어구분코드","ctrl_se_cd",9,"NUMBER(3)",null,null,"제어구분코드",null,null,"제어구분코드(009)","EQ","제어구분코드","ctrl_se_cd","NUMBER(3)","INTEGER","NUMBER(3)",null,null,null,"ctrl_se_cd ","INTEGER ","",",",null,"",null,null,null,"ctrl_se_cd ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","mtvsphassgnlinfo.","ctrl_se_cd"," IS ","'제어구분코드'",";",null,null,null,""]
[null,null,"제어상태코드","ctrl_stts_cd",10,"NUMBER(3)",null,null,"제어상태코드",null,null,"제어상태코드(010)","EQ","제어상태코드","ctrl_stts_cd","NUMBER(3)","INTEGER","NUMBER(3)",null,null,null,"ctrl_stts_cd ","INTEGER ","",",",null,"",null,null,null,"ctrl_stts_cd ","NUMBER(3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","mtvsphassgnlinfo.","ctrl_stts_cd"," IS ","'제어상태코드'",";",null,null,null,""]
[null,null,"주기시간","cycl_hr",11,"NUMBER(3)",null,null,"주기시간",null,null,null,"EQ","주기시간","cycl_hr","NUMBER(3)","INTEGER","NUMBER(3)",null,null,null,"cycl_hr ","INTEGER ","",",",null,"",null,null,null,"cycl_hr ","NUMBER(3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","mtvsphassgnlinfo.","cycl_hr"," IS ","'주기시간'",";",null,null,null,""]
[null,null,"옵셋시간","ofst_hr",12,"NUMBER(3)",null,null,"옵셋시간",null,null,null,"EQ","옵셋시간","ofst_hr","NUMBER(3)","INTEGER","NUMBER(3)",null,null,null,"ofst_hr ","INTEGER ","",",",null,"",null,null,null,"ofst_hr ","NUMBER(3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","mtvsphassgnlinfo.","ofst_hr"," IS ","'옵셋시간'",";",null,null,null,""]
[null,null,"현시번호","phas_no",13,"NUMBER(2)","PK",null,"현시번호 (1~8)",null,null,null,"EQ","현시번호","phas_no","NUMBER(2)","INTEGER","NUMBER(2)",null,null,null,"phas_no ","INTEGER ","",",",null,"phas_no",",",null,null,"phas_no ","NUMBER(2) ","",",",null,null,"phas_no",",","COMMENT ON COLUMN ","mtvsphassgnlinfo.","phas_no"," IS ","'현시번호 (1~8)'",";",null,null,null,""]
[null,null,"황색시간","yelw_hr",14,"NUMBER(3)",null,null,"황색시간",null,null,null,"EQ","황색시간","yelw_hr","NUMBER(3)","INTEGER","NUMBER(3)",null,null,null,"yelw_hr ","INTEGER ","",",",null,"",null,null,null,"yelw_hr ","NUMBER(3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","mtvsphassgnlinfo.","yelw_hr"," IS ","'황색시간'",";",null,null,null,""]
[null,null,"주도로구분코드","majr_road_se_cd",15,"CHAR(2)",null,null,"주도로구분코드 (063)",null,null,"주도로구분 (10:부도로, 20:주도로)","EQ","주도로구분코드","majr_road_se_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",null,null,null,"majr_road_se_cd ","VARCHAR(2) ","",",",null,"",null,null,null,"majr_road_se_cd ","VARCHAR2(2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","mtvsphassgnlinfo.","majr_road_se_cd"," IS ","'주도로구분코드 (063)'",";",null,null,null,""]
[null,null,"진행상태코드","prgrs_stts_cd",16,"CHAR(2)",null,null,"진행상태코드(506)",null,null,"0:초기셋팅, 1:신호이력insert, 2:종료시각update, 3:황색시간insert\n데이터 처리 종료 후 - 11:신호이력insert, 12:종료시각update, 13:황색시간insert","EQ","진행상태코드","prgrs_stts_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",null,null,null,"prgrs_stts_cd ","VARCHAR(2) ","",",",null,"",null,null,null,"prgrs_stts_cd ","VARCHAR2(2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","mtvsphassgnlinfo.","prgrs_stts_cd"," IS ","'진행상태코드(506)'",";",null,null,null,""]
[null,null,"현시시간","phas_hr",17,"NUMBER(3)",null,null,"현시소요시간",null,null,null,"EQ","현시시간","phas_hr","NUMBER(3)","INTEGER","NUMBER(3)",null,null,null,"phas_hr ","INTEGER ","",",",null,"",null,null,null,"phas_hr ","NUMBER(3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","mtvsphassgnlinfo.","phas_hr"," IS ","'현시소요시간'",";",null,null,null,""]
[null,null,"현시시작시간","phas_bgng_unix_tm",18,"NUMBER(10)","PK",null,"신호 시작시각(현시)",null,null,null,"EQ","현시시작시간","phas_bgng_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",null,null,null,"phas_bgng_unix_tm ","INTEGER ","",",",null,"phas_bgng_unix_tm","));",null,null,"phas_bgng_unix_tm ","NUMBER(10) ","",",",null,null,"phas_bgng_unix_tm",")","COMMENT ON COLUMN ","mtvsphassgnlinfo.","phas_bgng_unix_tm"," IS ","'신호 시작시각(현시)'",";",null,null,null,""]
[null,null,"입력일시","inpt_dt",20,"TIMESTAMP",null,"NOT NULL","데이터입력일시",null,null,null,"EQ","입력일시","inpt_dt","TIMESTAMP","TIMESTAMP","TIMESTAMP",null,null,null,"inpt_dt ",{"$f":"IF(Q125=\"TIMESTAMP\", Q125&\" DEFAULT NOW \", Q125&\" \")","v":"TIMESTAMP DEFAULT NOW "},"NOT NULL",",",null,"",null,null,null,"inpt_dt ","TIMESTAMP ","NOT NULL",")",null,null,"",null,"COMMENT ON COLUMN ","mtvsphassgnlinfo.","inpt_dt"," IS ","'데이터입력일시'",";",null,null,null,""]
[{"$nulls":21},{"$f":"CONCATENATE(Z107:AB122)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AI126:AK126)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (CLCT_UNIX_TM) INTERVAL (86400) (PARTITION BFR_\" & N105 & \"_20221101 VALUES LESS THAN (1667228400));\"","v":"PARTITION BY RANGE (CLCT_UNIX_TM) INTERVAL (86400) (PARTITION BFR_mtvsphassgnlinfo_20221101 VALUES LESS THAN (1667228400));"},{"$f":"\"CREATE INDEX PK_\" & N105 & \" ON \" & N105 & CONCATENATE(AJ107:AL124) & \" LOCAL (PARTITION BFR_\" & N105 & \"_20221101 TABLESPACE SOIT_I08);\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & N105 & \" ADD CONSTRAINT PK_\" & N105 & \" PRIMARY KEY \" & CONCATENATE(AJ107:AL125) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":10},{"$error":"#VALUE!"}]
[null,"현시TOD정보 테이블",{"$nulls":11},"soitsphastodinfo",{"$nulls":33},""]
[5,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N127&\" \"","v":"soitsphastodinfo "},null," IS ",{"$f":"\"'\"&B127&\"'\"","v":"'현시TOD정보 테이블'"},";",null,null,null,""]
[null,"soitsphastodinfo\n(확정)","시나리오 id","scen_id",1,"CHAR(50)","PK",null,"시나리오ID",null,null,"이거 어디다 쓰나요?",null,"시나리오 id","scen_id","CHAR(50)","VARCHAR(50)","VARCHAR2(50)",null,"CREATE TABLE ",{"$f":"N127&\" (\"","v":"soitsphastodinfo ("},{"$f":"O129&\" \"","v":"scen_id "},{"$f":"Q129&\" \"","v":"VARCHAR(50) "},{"$f":"IF(H129=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",","PRIMARY KEY (",{"$f":"IF(OR(G129=\"PK\", G129=\"PK/FK\"), O129, \"\")","v":"scen_id"},",","CREATE TABLE ",{"$f":"N127&\" (\"","v":"soitsphastodinfo ("},{"$f":"O129&\" \"","v":"scen_id "},{"$f":"R129&\" \"","v":"VARCHAR2(50) "},{"$f":"IF(H129=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",null,"(",{"$f":"IF(OR(G129=\"PK\", G129=\"PK/FK\"), O129, \"\")","v":"scen_id"},",","COMMENT ON COLUMN ",{"$f":"$N$127&\".\"","v":"soitsphastodinfo."},{"$f":"O129","v":"scen_id"}," IS ",{"$f":"\"'\"&I129&\"'\"","v":"'시나리오ID'"},";",null,null,null,""]
[null,null,"수집유닉스시각","clct_unix_tm",2,null,"PK",null,"동인 신호이력수집시각",null,null,null,{"$f":"IF(F130=P130, \"EQ\", \"NEQ)\")","v":"NEQ)"},"수집유닉스시각","clct_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",null,null,null,"clct_unix_tm ","INTEGER ","",",",null,"clct_unix_tm",",",null,null,"clct_unix_tm ","NUMBER(10) ","",",",null,null,"clct_unix_tm",",","COMMENT ON COLUMN ","soitsphastodinfo.","clct_unix_tm"," IS ","'동인 신호이력수집시각'",";",null,null,null,""]
[null,null,"시작유닉스시각","bgng_unix_tm",3,"NUMBER(10)","PK",null,"신호 시작시각(주기)",null,null,null,"EQ","시작유닉스시각","bgng_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",null,null,null,"bgng_unix_tm ","INTEGER ","",",",null,"bgng_unix_tm",",",null,null,"bgng_unix_tm ","NUMBER(10) ","",",",null,null,"bgng_unix_tm",",","COMMENT ON COLUMN ","soitsphastodinfo.","bgng_unix_tm"," IS ","'신호 시작시각(주기)'",";",null,null,null,""]
[null,null,"현장교차로ID","spot_ints_id",4,"NUMBER(5)","PK/FK",null,"현장교차로ID",null,null,null,"EQ","현장교차로ID","spot_ints_id","NUMBER(5)","INTEGER","NUMBER(5)",null,null,null,"spot_ints_id ","INTEGER ","",",",null,"spot_ints_id",",",null,null,"spot_ints_id ","NUMBER(5) ","",",",null,null,"spot_ints_id",",","COMMENT ON COLUMN ","soitsphastodinfo.","spot_ints_id"," IS ","'현장교차로ID'",";",null,null,null,""]
[null,null,"노드ID","node_id",5,"VARCHAR2(300)","PK/FK",null,"해당 교차로 노드ID",null,null,null,"EQ","노드ID","node_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,null,null,"node_id ","VARCHAR(300) ","",",",null,"node_id",",",null,null,"node_id ","VARCHAR2(300) ","",",",null,null,"node_id",",","COMMENT ON COLUMN ","soitsphastodinfo.","node_id"," IS ","'해당 교차로 노드ID'",";",null,null,null,""]
[null,null,"시각계획번호","tm_plan_no",6,"NUMBER(2)",null,null,"시각계획번호 (tod plan구분, 1~10)",null,null,null,"EQ","시각계획번호","tm_plan_no","NUMBER(2)","INTEGER","NUMBER(2)",null,null,null,"tm_plan_no ","INTEGER ","",",",null,"",null,null,null,"tm_plan_no ","NUMBER(2) ","",",",null,null,"",{"$f":"IF(OR(H134=\"PK\", H134=\"PK/FK\"), P134, \"\")","v":""},"COMMENT ON COLUMN ","soitsphastodinfo.","tm_plan_no"," IS ","'시각계획번호 (tod plan구분, 1~10)'",";",null,null,null,""]
[null,null,"현시운영계획번호","phas_oper_plan_no",7,"NUMBER(2)",null,null,"현시운영계획번호 (time plan ID, 1~16)",null,null,null,"EQ","현시운영계획번호","phas_oper_plan_no","NUMBER(2)","INTEGER","NUMBER(2)",null,null,null,"phas_oper_plan_no ","INTEGER ","",",",null,"",null,null,null,"phas_oper_plan_no ","NUMBER(2) ","",",",null,null,"","","COMMENT ON COLUMN ","soitsphastodinfo.","phas_oper_plan_no"," IS ","'현시운영계획번호 (time plan ID, 1~16)'",";",null,null,null,""]
[null,null,"시작시","bgng_hh",8,"NUMBER(2)",null,null,"시작시 (HH)",null,null,null,"EQ","시작시","bgng_hh","NUMBER(2)","INTEGER","NUMBER(2)",null,null,null,"bgng_hh ","INTEGER ","",",",null,"",null,null,null,"bgng_hh ","NUMBER(2) ","",",",null,null,"","","COMMENT ON COLUMN ","soitsphastodinfo.","bgng_hh"," IS ","'시작시 (HH)'",";",null,null,null,""]
[null,null,"시작분","bgng_mi",9,"NUMBER(2)",null,null,"시작분 (mm)",null,null,null,"EQ","시작분","bgng_mi","NUMBER(2)","INTEGER","NUMBER(2)",null,null,null,"bgng_mi ","INTEGER ","",",",null,"",null,null,null,"bgng_mi ","NUMBER(2) ","",",",null,null,"","","COMMENT ON COLUMN ","soitsphastodinfo.","bgng_mi"," IS ","'시작분 (mm)'",";",null,null,null,""]
[null,null,"주교차로구분코드","majr_ints_se_cd",10,"CHAR(2)",null,null,"주교차로구분코드 (062)",null,null,"주교차로구분 (1:주교차로, 2:연등교차로)","EQ","주교차로구분코드","majr_ints_se_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",null,null,null,"majr_ints_se_cd ","VARCHAR(2) ","",",",null,"",null,null,null,"majr_ints_se_cd ","VARCHAR2(2) ","",",",null,null,"","","COMMENT ON COLUMN ","soitsphastodinfo.","majr_ints_se_cd"," IS ","'주교차로구분코드 (062)'",";",null,null,null,""]
[null,null,"신호상태","sgnl_stts",11,"CHAR(100)",null,null,"신호상태 결합 (rrrgggGGGrr)",null,null,null,"EQ","신호상태","sgnl_stts","CHAR(100)","VARCHAR(100)","VARCHAR2(100)",null,null,null,"sgnl_stts ","VARCHAR(100) ","",",",null,"",null,null,null,"sgnl_stts ","VARCHAR2(100) ","",",",null,null,"","","COMMENT ON COLUMN ","soitsphastodinfo.","sgnl_stts"," IS ","'신호상태 결합 (rrrgggGGGrr)'",";",null,null,null,""]
[null,null,"주기시간","cycl_hr",12,"NUMBER(3)",null,null,"주기시간",null,null,null,"EQ","주기시간","cycl_hr","NUMBER(3)","INTEGER","NUMBER(3)",null,null,null,"cycl_hr ","INTEGER ","",",",null,"",null,null,null,"cycl_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitsphastodinfo.","cycl_hr"," IS ","'주기시간'",";",null,null,null,""]
[null,null,"옵셋시간","ofst_hr",13,"NUMBER(3)",null,null,"옵셋시간",null,null,null,"EQ","옵셋시간","ofst_hr","NUMBER(3)","INTEGER","NUMBER(3)",null,null,null,"ofst_hr ","INTEGER ","",",",null,"",null,null,null,"ofst_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitsphastodinfo.","ofst_hr"," IS ","'옵셋시간'",";",null,null,null,""]
[null,null,"현시번호","phas_no",14,"NUMBER(2)","PK",null,"현시번호 (1~8)",null,null,null,"EQ","현시번호","phas_no","NUMBER(2)","INTEGER","NUMBER(2)",null,null,null,"phas_no ","INTEGER ","",",",null,"phas_no",",",null,null,"phas_no ","NUMBER(2) ","",",",null,null,"phas_no",",","COMMENT ON COLUMN ","soitsphastodinfo.","phas_no"," IS ","'현시번호 (1~8)'",";",null,null,null,""]
[null,null,"황색시간","yelw_hr",15,"NUMBER(3)",null,null,"황색시간",null,null,null,"EQ","황색시간","yelw_hr","NUMBER(3)","INTEGER","NUMBER(3)",null,null,null,"yelw_hr ","INTEGER ","",",",null,"",null,null,null,"yelw_hr ","NUMBER(3) ","",",",null,null,"",{"$f":"IF(OR(H143=\"PK\", H143=\"PK/FK\"), P143, \"\")","v":""},"COMMENT ON COLUMN ","soitsphastodinfo.","yelw_hr"," IS ","'황색시간'",";",null,null,null,""]
[null,null,"최소녹색시간","min_gren_hr",16,"NUMBER(3)",null,null,"최소녹색시간",null,null,null,"EQ","최소녹색시간","min_gren_hr","NUMBER(3)","INTEGER","NUMBER(3)",null,null,null,"min_gren_hr ","INTEGER ",{"$f":"IF(H144=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",null,"",null,null,null,"min_gren_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitsphastodinfo.","min_gren_hr"," IS ","'최소녹색시간'",";",null,null,null,""]
[null,null,"주도로구분코드","majr_road_se_cd",17,"CHAR(2)",null,null,"주도로구분코드 (063)",null,null,"주도로구분 (10:부도로, 20:주도로)","EQ","주도로구분코드","majr_road_se_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",null,null,null,"majr_road_se_cd ","VARCHAR(2) ","",",",null,"",null,null,null,"majr_road_se_cd ","VARCHAR2(2) ","",",",null,null,"","","COMMENT ON COLUMN ","soitsphastodinfo.","majr_road_se_cd"," IS ","'주도로구분코드 (063)'",";",null,null,null,""]
[null,null,"진행상태코드","prgrs_stts_cd",18,"CHAR(2)",null,null,"진행상태코드(506)",null,null,"0:초기셋팅, 1:신호이력insert, 2:종료시각update, 3:황색시간insert\n데이터 처리 종료 후 - 11:신호이력insert, 12:종료시각update, 13:황색시간insert","EQ","진행상태코드","prgrs_stts_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",null,null,null,"prgrs_stts_cd ","VARCHAR(2) ","",",",null,"",null,null,null,"prgrs_stts_cd ","VARCHAR2(2) ","",",",null,null,"","","COMMENT ON COLUMN ","soitsphastodinfo.","prgrs_stts_cd"," IS ","'진행상태코드(506)'",";",null,null,null,""]
[null,null,"현시시간","phas_hr",19,"NUMBER(3)",null,null,"현시소요시간",null,null,null,"EQ","현시시간","phas_hr","NUMBER(3)","INTEGER","NUMBER(3)",null,null,null,"phas_hr ","INTEGER ","",",",null,"",null,null,null,"phas_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","soitsphastodinfo.","phas_hr"," IS ","'현시소요시간'",";",null,null,null,""]
[null,null,"현시시작시간","phas_bgng_unix_tm",20,"NUMBER(10)","PK",null,"신호 시작시각(현시)",null,null,null,"EQ","현시시작시간","phas_bgng_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",null,null,null,"phas_bgng_unix_tm ","INTEGER ","",",",null,"phas_bgng_unix_tm","));",null,null,"phas_bgng_unix_tm ","NUMBER(10) ","",",",null,null,"phas_bgng_unix_tm",")","COMMENT ON COLUMN ","soitsphastodinfo.","phas_bgng_unix_tm"," IS ","'신호 시작시각(현시)'",";",null,null,null,""]
[null,null,"입력일시","inpt_dt",21,"TIMESTAMP",null,"NOT NULL","데이터입력일시",null,null,null,"EQ","입력일시","inpt_dt","TIMESTAMP","TIMESTAMP","TIMESTAMP",null,null,null,"inpt_dt ",{"$f":"IF(Q149=\"TIMESTAMP\", Q149&\" DEFAULT NOW \", Q149&\" \")","v":"TIMESTAMP DEFAULT NOW "},"NOT NULL",",",null,"",null,null,null,"inpt_dt ","TIMESTAMP ","NOT NULL",{"$f":"\") TABLESPACE \"&AI151&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_S002 NOLOGGING"},null,null,{"$f":"IF(OR(F149=\"PK\", F149=\"PK/FK\"), H149, \"\")","v":""},null,"COMMENT ON COLUMN ","soitsphastodinfo.","inpt_dt"," IS ","'데이터입력일시'",";",null,null,null,""]
[{"$nulls":21},{"$f":"CONCATENATE(Z129:AB150)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AI150:AK150)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (clct_unix_tm) INTERVAL (3600) STORE IN (\"&AI151&\") (PARTITION BFR_\" & N127& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AI151&\");\"","v":"PARTITION BY RANGE (clct_unix_tm) INTERVAL (3600) STORE IN (SOIT_D08_S002) (PARTITION BFR_soitsphastodinfo_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_S002);"},{"$f":"\"CREATE INDEX PK_\" & N127& \" ON \" & N127 & CONCATENATE(AJ129:AL148) & \" LOCAL (PARTITION BFR_\" & N127 & \"_20221101 TABLESPACE \"&AJ151&\") TABLESPACE \"&AJ151&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & N127 & \" ADD CONSTRAINT PK_\" & N127 & \" PRIMARY KEY \" & CONCATENATE(AJ129:AL148) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":10},{"$error":"#VALUE!"}]
[null,"(메타버스) 현시TOD정보 테이블",{"$nulls":11},"mtvsphastodinfo",{"$nulls":20},"SOIT_D08_S002","SOIT_I08_S002",{"$nulls":11},""]
["2023-05-01","Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N151&\" \"","v":"mtvsphastodinfo "},null," IS ",{"$f":"\"'\"&B151&\"'\"","v":"'(메타버스) 현시TOD정보 테이블'"},";",null,null,null,""]
[null,"mtvsphastodinfo","시나리오 id","scen_id",1,"CHAR(50)","PK",null,"시나리오ID",null,null,"이거 어디다 쓰나요?",null,"시나리오 id","scen_id","CHAR(50)","VARCHAR(50)","VARCHAR2(50)",null,"CREATE TABLE ",{"$f":"N151&\" (\"","v":"mtvsphastodinfo ("},{"$f":"O153&\" \"","v":"scen_id "},{"$f":"Q153&\" \"","v":"VARCHAR(50) "},{"$f":"IF(H153=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",","PRIMARY KEY (",{"$f":"IF(OR(G153=\"PK\", G153=\"PK/FK\"), O153, \"\")","v":"scen_id"},",","CREATE TABLE ",{"$f":"N151&\" (\"","v":"mtvsphastodinfo ("},{"$f":"O153&\" \"","v":"scen_id "},{"$f":"R153&\" \"","v":"VARCHAR2(50) "},{"$f":"IF(H153=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",null,"(",{"$f":"IF(OR(G153=\"PK\", G153=\"PK/FK\"), O153, \"\")","v":"scen_id"},",","COMMENT ON COLUMN ",{"$f":"$N$151&\".\"","v":"mtvsphastodinfo."},{"$f":"O153","v":"scen_id"}," IS ",{"$f":"\"'\"&I153&\"'\"","v":"'시나리오ID'"},";",null,null,null,""]
[null,null,"수집유닉스시각","clct_unix_tm",2,null,"PK",null,"동인 신호이력수집시각",null,null,null,{"$f":"IF(F154=P154, \"EQ\", \"NEQ)\")","v":"NEQ)"},"수집유닉스시각","clct_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",null,null,null,"clct_unix_tm ","INTEGER ","",",",null,"clct_unix_tm",",",null,null,"clct_unix_tm ","NUMBER(10) ","",",",null,null,"clct_unix_tm",",","COMMENT ON COLUMN ","mtvsphastodinfo.","clct_unix_tm"," IS ","'동인 신호이력수집시각'",";",null,null,null,""]
[null,null,"시작유닉스시각","bgng_unix_tm",3,"NUMBER(10)","PK",null,"신호 시작시각(주기)",null,null,null,"EQ","시작유닉스시각","bgng_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",null,null,null,"bgng_unix_tm ","INTEGER ","",",",null,"bgng_unix_tm",",",null,null,"bgng_unix_tm ","NUMBER(10) ","",",",null,null,"bgng_unix_tm",",","COMMENT ON COLUMN ","mtvsphastodinfo.","bgng_unix_tm"," IS ","'신호 시작시각(주기)'",";",null,null,null,""]
[null,null,"현장교차로ID","spot_ints_id",4,"NUMBER(5)","PK/FK",null,"현장교차로ID",null,null,null,"EQ","현장교차로ID","spot_ints_id","NUMBER(5)","INTEGER","NUMBER(5)",null,null,null,"spot_ints_id ","INTEGER ","",",",null,"spot_ints_id",",",null,null,"spot_ints_id ","NUMBER(5) ","",",",null,null,"spot_ints_id",",","COMMENT ON COLUMN ","mtvsphastodinfo.","spot_ints_id"," IS ","'현장교차로ID'",";",null,null,null,""]
[null,null,"노드ID","node_id",5,"VARCHAR2(300)","PK/FK",null,"해당 교차로 노드ID",null,null,null,"EQ","노드ID","node_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,null,null,"node_id ","VARCHAR(300) ","",",",null,"node_id",",",null,null,"node_id ","VARCHAR2(300) ","",",",null,null,"node_id",",","COMMENT ON COLUMN ","mtvsphastodinfo.","node_id"," IS ","'해당 교차로 노드ID'",";",null,null,null,""]
[null,null,"시각계획번호","tm_plan_no",6,"NUMBER(2)",null,null,"시각계획번호 (tod plan구분, 1~10)",null,null,null,"EQ","시각계획번호","tm_plan_no","NUMBER(2)","INTEGER","NUMBER(2)",null,null,null,"tm_plan_no ","INTEGER ","",",",null,"",null,null,null,"tm_plan_no ","NUMBER(2) ","",",",null,null,"",{"$f":"IF(OR(H158=\"PK\", H158=\"PK/FK\"), P158, \"\")","v":""},"COMMENT ON COLUMN ","mtvsphastodinfo.","tm_plan_no"," IS ","'시각계획번호 (tod plan구분, 1~10)'",";",null,null,null,""]
[null,null,"현시운영계획번호","phas_oper_plan_no",7,"NUMBER(2)",null,null,"현시운영계획번호 (time plan ID, 1~16)",null,null,null,"EQ","현시운영계획번호","phas_oper_plan_no","NUMBER(2)","INTEGER","NUMBER(2)",null,null,null,"phas_oper_plan_no ","INTEGER ","",",",null,"",null,null,null,"phas_oper_plan_no ","NUMBER(2) ","",",",null,null,"","","COMMENT ON COLUMN ","mtvsphastodinfo.","phas_oper_plan_no"," IS ","'현시운영계획번호 (time plan ID, 1~16)'",";",null,null,null,""]
[null,null,"시작시","bgng_hh",8,"NUMBER(2)",null,null,"시작시 (HH)",null,null,null,"EQ","시작시","bgng_hh","NUMBER(2)","INTEGER","NUMBER(2)",null,null,null,"bgng_hh ","INTEGER ","",",",null,"",null,null,null,"bgng_hh ","NUMBER(2) ","",",",null,null,"","","COMMENT ON COLUMN ","mtvsphastodinfo.","bgng_hh"," IS ","'시작시 (HH)'",";",null,null,null,""]
[null,null,"시작분","bgng_mi",9,"NUMBER(2)",null,null,"시작분 (mm)",null,null,null,"EQ","시작분","bgng_mi","NUMBER(2)","INTEGER","NUMBER(2)",null,null,null,"bgng_mi ","INTEGER ","",",",null,"",null,null,null,"bgng_mi ","NUMBER(2) ","",",",null,null,"","","COMMENT ON COLUMN ","mtvsphastodinfo.","bgng_mi"," IS ","'시작분 (mm)'",";",null,null,null,""]
[null,null,"주교차로구분코드","majr_ints_se_cd",10,"CHAR(2)",null,null,"주교차로구분코드 (062)",null,null,"주교차로구분 (1:주교차로, 2:연등교차로)","EQ","주교차로구분코드","majr_ints_se_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",null,null,null,"majr_ints_se_cd ","VARCHAR(2) ","",",",null,"",null,null,null,"majr_ints_se_cd ","VARCHAR2(2) ","",",",null,null,"","","COMMENT ON COLUMN ","mtvsphastodinfo.","majr_ints_se_cd"," IS ","'주교차로구분코드 (062)'",";",null,null,null,""]
[null,null,"신호상태","sgnl_stts",11,"CHAR(100)",null,null,"신호상태 결합 (rrrgggGGGrr)",null,null,null,"EQ","신호상태","sgnl_stts","CHAR(100)","VARCHAR(100)","VARCHAR2(100)",null,null,null,"sgnl_stts ","VARCHAR(100) ","",",",null,"",null,null,null,"sgnl_stts ","VARCHAR2(100) ","",",",null,null,"","","COMMENT ON COLUMN ","mtvsphastodinfo.","sgnl_stts"," IS ","'신호상태 결합 (rrrgggGGGrr)'",";",null,null,null,""]
[null,null,"주기시간","cycl_hr",12,"NUMBER(3)",null,null,"주기시간",null,null,null,"EQ","주기시간","cycl_hr","NUMBER(3)","INTEGER","NUMBER(3)",null,null,null,"cycl_hr ","INTEGER ","",",",null,"",null,null,null,"cycl_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","mtvsphastodinfo.","cycl_hr"," IS ","'주기시간'",";",null,null,null,""]
[null,null,"옵셋시간","ofst_hr",13,"NUMBER(3)",null,null,"옵셋시간",null,null,null,"EQ","옵셋시간","ofst_hr","NUMBER(3)","INTEGER","NUMBER(3)",null,null,null,"ofst_hr ","INTEGER ","",",",null,"",null,null,null,"ofst_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","mtvsphastodinfo.","ofst_hr"," IS ","'옵셋시간'",";",null,null,null,""]
[null,null,"현시번호","phas_no",14,"NUMBER(2)","PK",null,"현시번호 (1~8)",null,null,null,"EQ","현시번호","phas_no","NUMBER(2)","INTEGER","NUMBER(2)",null,null,null,"phas_no ","INTEGER ","",",",null,"phas_no",",",null,null,"phas_no ","NUMBER(2) ","",",",null,null,"phas_no",",","COMMENT ON COLUMN ","mtvsphastodinfo.","phas_no"," IS ","'현시번호 (1~8)'",";",null,null,null,""]
[null,null,"황색시간","yelw_hr",15,"NUMBER(3)",null,null,"황색시간",null,null,null,"EQ","황색시간","yelw_hr","NUMBER(3)","INTEGER","NUMBER(3)",null,null,null,"yelw_hr ","INTEGER ","",",",null,"",null,null,null,"yelw_hr ","NUMBER(3) ","",",",null,null,"",{"$f":"IF(OR(H167=\"PK\", H167=\"PK/FK\"), P167, \"\")","v":""},"COMMENT ON COLUMN ","mtvsphastodinfo.","yelw_hr"," IS ","'황색시간'",";",null,null,null,""]
[null,null,"최소녹색시간","min_gren_hr",16,"NUMBER(3)",null,null,"최소녹색시간",null,null,null,"EQ","최소녹색시간","min_gren_hr","NUMBER(3)","INTEGER","NUMBER(3)",null,null,null,"min_gren_hr ","INTEGER ",{"$f":"IF(H168=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",null,"",null,null,null,"min_gren_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","mtvsphastodinfo.","min_gren_hr"," IS ","'최소녹색시간'",";",null,null,null,""]
[null,null,"주도로구분코드","majr_road_se_cd",17,"CHAR(2)",null,null,"주도로구분코드 (063)",null,null,"주도로구분 (10:부도로, 20:주도로)","EQ","주도로구분코드","majr_road_se_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",null,null,null,"majr_road_se_cd ","VARCHAR(2) ","",",",null,"",null,null,null,"majr_road_se_cd ","VARCHAR2(2) ","",",",null,null,"","","COMMENT ON COLUMN ","mtvsphastodinfo.","majr_road_se_cd"," IS ","'주도로구분코드 (063)'",";",null,null,null,""]
[null,null,"진행상태코드","prgrs_stts_cd",18,"CHAR(2)",null,null,"진행상태코드(506)",null,null,"0:초기셋팅, 1:신호이력insert, 2:종료시각update, 3:황색시간insert\n데이터 처리 종료 후 - 11:신호이력insert, 12:종료시각update, 13:황색시간insert","EQ","진행상태코드","prgrs_stts_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",null,null,null,"prgrs_stts_cd ","VARCHAR(2) ","",",",null,"",null,null,null,"prgrs_stts_cd ","VARCHAR2(2) ","",",",null,null,"","","COMMENT ON COLUMN ","mtvsphastodinfo.","prgrs_stts_cd"," IS ","'진행상태코드(506)'",";",null,null,null,""]
[null,null,"현시시간","phas_hr",19,"NUMBER(3)",null,null,"현시소요시간",null,null,null,"EQ","현시시간","phas_hr","NUMBER(3)","INTEGER","NUMBER(3)",null,null,null,"phas_hr ","INTEGER ","",",",null,"",null,null,null,"phas_hr ","NUMBER(3) ","",",",null,null,"","","COMMENT ON COLUMN ","mtvsphastodinfo.","phas_hr"," IS ","'현시소요시간'",";",null,null,null,""]
[null,null,"현시시작시간","phas_bgng_unix_tm",20,"NUMBER(10)","PK",null,"신호 시작시각(현시)",null,null,null,"EQ","현시시작시간","phas_bgng_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",null,null,null,"phas_bgng_unix_tm ","INTEGER ","",",",null,"phas_bgng_unix_tm","));",null,null,"phas_bgng_unix_tm ","NUMBER(10) ","",",",null,null,"phas_bgng_unix_tm",")","COMMENT ON COLUMN ","mtvsphastodinfo.","phas_bgng_unix_tm"," IS ","'신호 시작시각(현시)'",";",null,null,null,""]
[null,null,"입력일시","inpt_dt",21,"TIMESTAMP",null,"NOT NULL","데이터입력일시",null,null,null,"EQ","입력일시","inpt_dt","TIMESTAMP","TIMESTAMP","TIMESTAMP",null,null,null,"inpt_dt ",{"$f":"IF(Q173=\"TIMESTAMP\", Q173&\" DEFAULT NOW \", Q173&\" \")","v":"TIMESTAMP DEFAULT NOW "},"NOT NULL",",",null,"",null,null,null,"inpt_dt ","TIMESTAMP ","NOT NULL",")",null,null,"",{"$f":"IF(OR(H173=\"PK\", H173=\"PK/FK\"), P173, \"\")","v":""},"COMMENT ON COLUMN ","mtvsphastodinfo.","inpt_dt"," IS ","'데이터입력일시'",";",null,null,null,""]
[{"$nulls":21},{"$f":"CONCATENATE(Z153:AB174)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AI174:AK174)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (CLCT_UNIX_TM) INTERVAL (86400) (PARTITION BFR_\" & N151 & \"_20221101 VALUES LESS THAN (1667228400));\"","v":"PARTITION BY RANGE (CLCT_UNIX_TM) INTERVAL (86400) (PARTITION BFR_mtvsphastodinfo_20221101 VALUES LESS THAN (1667228400));"},{"$f":"\"CREATE INDEX PK_\" & N151 & \" ON \" & N151 & CONCATENATE(AJ153:AL173) & \" LOCAL (PARTITION BFR_\" & N151 & \"_20221101 TABLESPACE SOIT_I08);\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & N151 & \" ADD CONSTRAINT PK_\" & N151 & \" PRIMARY KEY \" & CONCATENATE(AJ153:AL173) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":10},{"$error":"#VALUE!"}]
[null,"더미테이블",{"$nulls":9},"코드 id 정리",{"$nulls":35},""]
[6,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",{"$nulls":36},""]
[null,"soitsdummy\n(확정)","더미컬럼","dummy",1,"VARCHAR2(1)",null,null,"데이터 1건 들어가 있으며, dual 대신 활용할 테이블",{"$nulls":38},""]
[{"$nulls":47},""]
[null,"지역 분할정보 테이블",{"$nulls":11},"soitsrgnprttninfo",{"$nulls":33},""]
[7,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N179&\" \"","v":"soitsrgnprttninfo "},null," IS ",{"$f":"\"'\"&B179&\"'\"","v":"'지역 분할정보 테이블'"},";",null,null,null,""]
[null,"soitsrgnprttninfo\n(확정)","지역분할코드","rgn_prttn_cd",1,"CHAR(2)","PK/FK","NOT NULL","지역분할코드 (051)",null,null,"0 : 메타버스 POC,1 : 계양구,2 : 남동구_상단,3 : 남동구_하단,4 : 미추홀구,5 : 부평구_상단,6 : 부평구_하단,7 : 서구+동구,8 : 연수구,9 : 중구",{"$f":"IF(F181=P181, \"EQ\", \"NEQ)\")","v":"EQ"},"지역분할코드","rgn_prttn_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",null,"CREATE TABLE ",{"$f":"N179&\" (\"","v":"soitsrgnprttninfo ("},{"$f":"O181&\" \"","v":"rgn_prttn_cd "},{"$f":"Q181&\" \"","v":"VARCHAR(2) "},{"$f":"IF(H181=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(G181=\"PK\", G181=\"PK/FK\"), O181, \"\")","v":"rgn_prttn_cd"},",","CREATE TABLE ",{"$f":"N179&\" (\"","v":"soitsrgnprttninfo ("},{"$f":"O181&\" \"","v":"rgn_prttn_cd "},{"$f":"R181&\" \"","v":"VARCHAR2(2) "},{"$f":"IF(H181=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","CONSTRAINT ",{"$f":"\"PK_\"&N179&\" PRIMARY KEY (\"","v":"PK_soitsrgnprttninfo PRIMARY KEY ("},{"$f":"IF(OR(G181=\"PK\", G181=\"PK/FK\"), O181, \"\")","v":"rgn_prttn_cd"},",","COMMENT ON COLUMN ",{"$f":"$N$179&\".\"","v":"soitsrgnprttninfo."},{"$f":"O181","v":"rgn_prttn_cd"}," IS ",{"$f":"\"'\"&I181&\"'\"","v":"'지역분할코드 (051)'"},";",null,null,null,""]
[null,null,"노드ID","node_id",2,"VARCHAR2(300)","PK/FK","NOT NULL","구역내 소속교차로 노드ID",null,null,null,"EQ","노드ID","node_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,null,null,"node_id ","VARCHAR(300) ","NOT NULL",",",null,"node_id","));",null,null,"node_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"node_id",{"$f":"\") using index tablespace \" &AJ187& \") TABLESPACE \" &AI187&\";\"","v":") using index tablespace SOIT_I08_M001) TABLESPACE SOIT_D08_M001;"},"COMMENT ON COLUMN ","soitsrgnprttninfo.","node_id"," IS ","'구역내 소속교차로 노드ID'",";",null,null,null,""]
[null,null,"현장교차로ID","spot_ints_id",3,"NUMBER(5)","FK","NOT NULL","구역내 소속 현장교차로ID",null,null,null,"EQ","현장교차로ID","spot_ints_id","NUMBER(5)","INTEGER","NUMBER(5)",null,null,null,"spot_ints_id ","INTEGER ","NOT NULL",",",null,"",null,null,null,"spot_ints_id ","NUMBER(5) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrgnprttninfo.","spot_ints_id"," IS ","'구역내 소속 현장교차로ID'",";",null,null,null,""]
[null,null,"지역분할명","rgn_prttn_nm",4,"VARCHAR2(50)",null,"NOT NULL","지역분할명",null,null,null,"EQ","지역분할명","rgn_prttn_nm","VARCHAR2(50)","VARCHAR(50)","VARCHAR2(50)",null,null,null,"rgn_prttn_nm ","VARCHAR(50) ","NOT NULL",",",null,"",null,null,null,"rgn_prttn_nm ","VARCHAR2(50) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrgnprttninfo.","rgn_prttn_nm"," IS ","'지역분할명'",";",null,null,null,""]
[null,null,"소속구분코드","ogdp_se_cd",5,"CHAR(1)",null,"NOT NULL","소속구분코드 (056)",null,null,"소속구분 (대상지역 : 1 / 주변지역 : 2)","EQ","소속구분코드","ogdp_se_cd","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",null,null,null,"ogdp_se_cd ","VARCHAR(1) ","NOT NULL",",",null,"",null,null,null,"ogdp_se_cd ","VARCHAR2(1) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrgnprttninfo.","ogdp_se_cd"," IS ","'소속구분코드 (056)'",";",null,null,null,""]
[{"$nulls":21},{"$f":"CONCATENATE(Z181:AB185)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AI181:AL185)","v":{"$error":"#VALUE!"}},{"$nulls":16},{"$error":"#VALUE!"}]
[null,"시뮬레이션수행이력 테이블",{"$nulls":11},"soitssmlnflfmthstr",{"$nulls":20},"SOIT_D08_M001","SOIT_I08_M001",{"$nulls":11},""]
[9,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","전략본부의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N187&\" \"","v":"soitssmlnflfmthstr "},null," IS ",{"$f":"\"'\"&B187&\"'\"","v":"'시뮬레이션수행이력 테이블'"},";",null,null,null,""]
[null,"soitssmlnflfmthstr\n(확정)","지역분할코드","rgn_prttn_cd",1,"CHAR(2)","PK/FK","NOT NULL","지역분할코드","안양의 TB_DATA_HISTORY 대응하는 테이블\n시뮬레이선 종료 후 이동궤적과 신호변경이력 INSERT 후\n1 ROW INSERT",null,null,{"$f":"IF(F189=P189, \"EQ\", \"NEQ)\")","v":"EQ"},"지역분할코드","rgn_prttn_cd","CHAR(2)",null,"VARCHAR2(2)",{"$nulls":10},"CREATE TABLE ",{"$f":"N187&\" (\"","v":"soitssmlnflfmthstr ("},{"$f":"O189&\" \"","v":"rgn_prttn_cd "},{"$f":"R189&\" \"","v":"VARCHAR2(2) "},{"$f":"IF(H189=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(G189=\"PK\", G189=\"PK/FK\"), O189, \"\")","v":"rgn_prttn_cd"},",","COMMENT ON COLUMN ",{"$f":"$N$187&\".\"","v":"soitssmlnflfmthstr."},{"$f":"O189","v":"rgn_prttn_cd"}," IS ",{"$f":"\"'\"&I189&\"'\"","v":"'지역분할코드'"},";",null,null,null,""]
[null,null,"시뮬레이션구분코드","smln_se_cd",2,"CHAR(1)","PK","NOT NULL","시뮬레이션 구분 코드 (057)",null,null,"작업 구분 코드 (1:실시간(5분), 2:메타버스(5분), 3:배치(1시간), 4:모델학습(1주일))","EQ","시뮬레이션구분코드","smln_se_cd","CHAR(1)",null,"VARCHAR2(1)",{"$nulls":12},"smln_se_cd ","VARCHAR2(1) ","NOT NULL",",",null,null,"smln_se_cd",",","COMMENT ON COLUMN ","soitssmlnflfmthstr.","smln_se_cd"," IS ","'시뮬레이션 구분 코드 (057)'",";",null,null,null,""]
[null,null,"실측여부","acsr_yn",3,"CHAR(1)","PK","NOT NULL","실측여부(500)",null,null,"실측여부 (Y:실측, N:예측)","EQ","실측여부","acsr_yn","CHAR(1)",null,"VARCHAR2(1)",{"$nulls":12},"acsr_yn ","VARCHAR2(1) ","NOT NULL",",",null,null,"acsr_yn",",","COMMENT ON COLUMN ","soitssmlnflfmthstr.","acsr_yn"," IS ","'실측여부(500)'",";",null,null,null,""]
[null,null,"시작유닉스시각","bgng_unix_tm",4,"NUMBER(10)","PK","NOT NULL","시뮬레이션 대상 시작 시각",null,null,null,"EQ","시작유닉스시각","bgng_unix_tm","NUMBER(10)",null,"NUMBER(10)",{"$nulls":12},"bgng_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"bgng_unix_tm",")","COMMENT ON COLUMN ","soitssmlnflfmthstr.","bgng_unix_tm"," IS ","'시뮬레이션 대상 시작 시각'",";",null,null,null,""]
[null,null,"종료유닉스시각","end_unix_tm",5,"NUMBER(10)",null,"NOT NULL","시뮬레이션 대상 종료 시각",null,null,null,"EQ","종료유닉스시각","end_unix_tm","NUMBER(10)",null,"NUMBER(10)",{"$nulls":12},"end_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitssmlnflfmthstr.","end_unix_tm"," IS ","'시뮬레이션 대상 종료 시각'",";",null,null,null,""]
[null,null,"수행시작유닉스시각","flfmt_bgng_unix_tm",6,"NUMBER(10)",null,"NOT NULL","요청이 들어온 시각",null,null,null,"EQ","수행시작유닉스시각","flfmt_bgng_unix_tm","NUMBER(10)",null,"NUMBER(10)",{"$nulls":12},"flfmt_bgng_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitssmlnflfmthstr.","flfmt_bgng_unix_tm"," IS ","'요청이 들어온 시각'",";",null,null,null,""]
[null,null,"수행종료유닉스시각","flfmt_end_unix_tm",7,"NUMBER(10)",null,"NULL","시뮬레이션을 실제 수행종료한 시각",{"$nulls":4},"수행종료유닉스시각","flfmt_end_unix_tm","NUMBER(10)",null,"NUMBER(10)",{"$nulls":12},"flfmt_end_unix_tm ","NUMBER(10) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitssmlnflfmthstr.","flfmt_end_unix_tm"," IS ","'시뮬레이션을 실제 수행종료한 시각'",";",null,null,null,""]
[null,null,"파일명","file_nm",8,"VARCHAR2(50)",null,"NOT NULL","파일경로",null,null,null,{"$f":"IF(F196=P196, \"EQ\", \"NEQ)\")","v":"EQ"},"파일명","file_nm","VARCHAR2(50)",null,"VARCHAR2(50)",{"$nulls":12},"file_nm ","VARCHAR2(50) ","NOT NULL",",",null,null,{"$f":"IF(OR(G196=\"PK\", G196=\"PK/FK\"), O196, \"\")","v":""},null,"COMMENT ON COLUMN ","soitssmlnflfmthstr.","file_nm"," IS ","'파일경로'",";",null,null,null,""]
[null,null,"이동궤적수","mvmn_cnt",9,"NUMBER(10)",null,"NOT NULL","총 이동궤적수",{"$nulls":4},"이동궤적수","mvmn_cnt","NUMBER(10)",null,"NUMBER(10)",{"$nulls":12},"mvmn_cnt ","NUMBER(10) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitssmlnflfmthstr.","mvmn_cnt"," IS ","'총 이동궤적수'",";"]
[null,null,"진행상태코드","prgrs_stts_cd",10,"CHAR(1)",null,"NOT NULL","진행상태코드 (501)",null,null,null,{"$f":"IF(F198=P198, \"EQ\", \"NEQ)\")","v":"EQ"},"진행상태코드","prgrs_stts_cd","CHAR(1)",null,"VARCHAR2(1)",{"$nulls":12},"prgrs_stts_cd ","VARCHAR2(1) ","NOT NULL",{"$f":"\") TABLESPACE \"&AI200&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_M001 NOLOGGING"},null,null,{"$f":"IF(OR(G198=\"PK\", G198=\"PK/FK\"), O198, \"\")","v":""},null,"COMMENT ON COLUMN ","soitssmlnflfmthstr.","prgrs_stts_cd"," IS ","'진행상태코드 (501)'",";",null,null,null,{"$f":"IF(LEFT(AE198, 13) = \"CONSTRAINT PK\", AE198, \"\")","v":""}]
[{"$nulls":30},{"$f":"CONCATENATE(AI199:AK199)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (bgng_unix_tm) INTERVAL (86400) STORE IN (\"&AI200&\") (PARTITION BFR_\" & N187& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AI200&\");\"","v":"PARTITION BY RANGE (bgng_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_M001) (PARTITION BFR_soitssmlnflfmthstr_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_M001);"},{"$f":"\"CREATE INDEX PK_\" & N187& \" ON \" & N187 & CONCATENATE(AJ189:AL196) & \" LOCAL (PARTITION BFR_\" & N187 & \"_20221101 TABLESPACE \"&AJ200&\") TABLESPACE \"&AJ200&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & N187 & \" ADD CONSTRAINT PK_\" & N187 & \" PRIMARY KEY \" & CONCATENATE(AJ189:AL196) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":10},{"$error":"#VALUE!"}]
[{"$nulls":34},"SOIT_D08_M001","SOIT_I08_M001"]
[null,"엣지그룹 테이블",{"$nulls":11},"soitsedgegrup",{"$nulls":33},{"$f":"IF(LEFT(AE201, 13) = \"CONSTRAINT PK\", AE201, \"\")","v":""}]
[11,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N201&\" \"","v":"soitsedgegrup "},null," IS ",{"$f":"\"'\"&B201&\"'\"","v":"'엣지그룹 테이블'"},";",null,null,null,""]
[null,"soitsedgegrup\n(tb_edge_group)\n(확정)","엣지그룹ID","edge_grup_id",1,"VARCHAR2(300)","PK/FK","NOT NULL","엣지그룹ID","엣지그룹은 교차로 지점(골목길 포함)을 노드로 구분, 자동 혹은 수작업 예정",null,null,{"$f":"IF(F203=P203, \"EQ\", \"NEQ)\")","v":"EQ"},"엣지그룹ID","edge_grup_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":10},"CREATE TABLE ",{"$f":"N201&\" (\"","v":"soitsedgegrup ("},{"$f":"O203&\" \"","v":"edge_grup_id "},{"$f":"R203&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(H203=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","CONSTRAINT ",{"$f":"\"PK_\"&N201&\" PRIMARY KEY (\"","v":"PK_soitsedgegrup PRIMARY KEY ("},{"$f":"IF(OR(G203=\"PK\", G203=\"PK/FK\"), O203, \"\")","v":"edge_grup_id"},{"$f":"\") using index tablespace \" &AJ218& \") TABLESPACE \" &AI218&\";\"","v":") using index tablespace SOIT_I08_M001) TABLESPACE SOIT_D08_M001;"},"COMMENT ON COLUMN ",{"$f":"$N$201&\".\"","v":"soitsedgegrup."},{"$f":"O203","v":"edge_grup_id"}," IS ",{"$f":"\"'\"&I203&\"'\"","v":"'엣지그룹ID'"},";",null,null,null,""]
[null,null,"시작노드ID","bgng_node_id",2,"VARCHAR2(300)","FK","NOT NULL","출발 교차로 노드 ID","자동 혹은 수작업 예정",null,null,"EQ","시작교차로ID","bgng_node_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":12},"bgng_node_id ","VARCHAR2(300) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsedgegrup.","bgng_node_id"," IS ","'출발 교차로 노드 ID'",";",null,null,null,""]
[null,null,"종료노드ID","end_node_id",3,"VARCHAR2(300)","FK","NOT NULL","도착 교차로 노드 ID","자동 혹은 수작업 예정",null,null,"EQ","종료교차로ID","end_node_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":12},"end_node_id ","VARCHAR2(300) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsedgegrup.","end_node_id"," IS ","'도착 교차로 노드 ID'",";",null,null,null,""]
[null,null,"시작엣지ID","bgng_edge_id",4,"VARCHAR2(300)","FK","NOT NULL","내부 시작엣지ID","ICT사업본부에서 생성/입력 예정",null,null,null,"진입엣지ID","entr_edge_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":12},"entr_edge_id ","VARCHAR2(300) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsedgegrup.","entr_edge_id"," IS ","'내부 시작엣지ID'",";",null,null,null,""]
[null,null,"종료엣지ID","end_edge_id",5,"VARCHAR2(300)","FK","NOT NULL","내부 종료엣지ID","ICT사업본부에서 생성/입력 예정",null,null,null,"진출엣지ID","exit_edge_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":12},"exit_edge_id ","VARCHAR2(300) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsedgegrup.","exit_edge_id"," IS ","'내부 종료엣지ID'",";",null,null,null,""]
[null,null,"공간구분코드","bgng_rgn_prttn_cd",{"$f":"E207+1","v":6},"CHAR(2)","FK","NOT NULL","출발교차로 지역분할코드 (051)","ICT사업본부에서 생성/입력 예정",null,null,null,"지역분할코드","bgng_rgn_prttn_cd","CHAR(2)",null,"VARCHAR2(2)",{"$nulls":12},"bgng_rgn_prttn_cd ","VARCHAR2(2) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsedgegrup.","bgng_rgn_prttn_cd"," IS ","'출발교차로 지역분할코드 (051)'",";"]
[null,null,"공간구분코드","end_rgn_prttn_cd",7,"CHAR(2)","FK","NOT NULL","도착교차로 지역분할코드 (051)","ICT사업본부에서 생성/입력 예정",null,null,null,"지역분할코드","end_rgn_prttn_cd","CHAR(2)",null,"VARCHAR2(2)",{"$nulls":12},"end_rgn_prttn_cd ","VARCHAR2(2) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsedgegrup.","end_rgn_prttn_cd"," IS ","'도착교차로 지역분할코드 (051)'",";"]
[null,null,"평균 차로수","avg_lane_cnt",8,"NUMBER(5,2)",null,"NOT NULL","평균 차로수","4차로>5차로 변경 시, 좀 더 길게 구성되어 잇는 차로수로 계산하는 게 맞을 듯",null,null,{"$f":"IF(F210=P210, \"EQ\", \"NEQ)\")","v":"EQ"},"차로수","avg_lane_cnt","NUMBER(5,2)",null,"NUMBER(5,2)",{"$nulls":12},"avg_lane_cnt ","NUMBER(5,2) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsedgegrup.","avg_lane_cnt"," IS ","'평균 차로수'",";",null,null,null,{"$f":"IF(LEFT(AE210, 13) = \"CONSTRAINT PK\", AE210, \"\")","v":""}]
[null,null,"방향구분코드","drct_se_cd",9,"CHAR(1)",null,"NOT NULL","방향구분코드(004)","위의 연동그룹과 같게 방향구성해야 될 듯",null,"상/하 혹은 좌/우 기준으로 1/2","EQ","방향구분코드","drct_se_cd","CHAR(1)",null,"VARCHAR2(1)",{"$nulls":12},"drct_se_cd ","VARCHAR2(1) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsedgegrup.","drct_se_cd"," IS ","'방향구분코드(004)'",";",null,null,null,""]
[null,null,"엣지그룹공간정보","edge_grup_spin",10,"BINARY",null,null,"엣지그룹공간정보 (WKT LineString) ","ICT사업본부에서 생성/입력 예정",null,null,"EQ","엣지그룹공간정보","edge_grup_spin","BINARY",null,"GEOMETRY",{"$nulls":12},"edge_grup_spin ","GEOMETRY ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsedgegrup.","edge_grup_spin"," IS ","'엣지그룹공간정보 (WKT LineString) '",";",null,null,null,""]
[null,null,"대표경도","rprs_lot",11,"NUMBER(13,10)",null,null,"대표경도","ICT사업본부에서 생성/입력 예정",null,null,"EQ","대표경도","rprs_lot","NUMBER(13,10)",null,"NUMBER(13,10)",{"$nulls":12},"rprs_lot ","NUMBER(13,10) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsedgegrup.","rprs_lot"," IS ","'대표경도'",";",null,null,null,""]
[null,null,"대표위도","rprs_lat",12,"NUMBER(12,10)",null,null,"대표위도","ICT사업본부에서 생성/입력 예정",null,null,"EQ","대표위도","rprs_lat","NUMBER(12,10)",null,"NUMBER(12,10)",{"$nulls":12},"rprs_lat ","NUMBER(12,10) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsedgegrup.","rprs_lat"," IS ","'대표위도'",";",null,null,null,""]
[null,null,"소속엣지수","edge_cnt",13,"NUMBER(2)",null,null,"소속엣지수","ICT사업본부에서 생성/입력 예정",null,null,null,"소속엣지수","edge_cnt","NUMBER(2)",null,"NUMBER(2)",{"$nulls":12},"edge_cnt ","NUMBER(2) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsedgegrup.","edge_cnt"," IS ","'소속엣지수'",";",null,null,null,""]
[null,null,"엣지그룹길이","edge_grup_lngt",14,"NUMBER(19,9)",null,null,"엣지그룹길이","ICT사업본부에서 생성/입력 예정",null,null,null,"엣지그룹길이","edge_grup_lngt","NUMBER(19,9)",null,"NUMBER(19,9)",{"$nulls":12},"edge_grup_lngt ","NUMBER(19,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsedgegrup.","edge_grup_lngt"," IS ","'엣지그룹길이'",";",null,null,null,""]
[{"$nulls":30},{"$f":"CONCATENATE(AI203:AL215)","v":{"$error":"#VALUE!"}},{"$nulls":16},{"$error":"#VALUE!"}]
[{"$nulls":34},"SOIT_D08_M001","SOIT_I08_M001"]
[null,"엣지그룹구성 테이블",{"$nulls":11},"soitsedgegrupcnfg",{"$nulls":33},{"$f":"IF(LEFT(AE219, 13) = \"CONSTRAINT PK\", AE219, \"\")","v":""}]
[12,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N219&\" \"","v":"soitsedgegrupcnfg "},null," IS ",{"$f":"\"'\"&B219&\"'\"","v":"'엣지그룹구성 테이블'"},";",null,null,null,""]
[null,"soitsedgegrupcnfg","엣지그룹ID","edge_grup_id",1,"VARCHAR2(300)","PK/FK","NOT NULL","엣지그룹 ID",{"$nulls":4},"엣지그룹ID","edge_grup_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,"CREATE TABLE ",{"$f":"N219&\" (\"","v":"soitsedgegrupcnfg ("},{"$f":"O221&\" \"","v":"edge_grup_id "},{"$f":"Q221&\" \"","v":"VARCHAR(300) "},{"$f":"IF(H221=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(G221=\"PK\", G221=\"PK/FK\"), O221, \"\")","v":"edge_grup_id"},",","CREATE TABLE ",{"$f":"N219&\" (\"","v":"soitsedgegrupcnfg ("},{"$f":"O221&\" \"","v":"edge_grup_id "},{"$f":"R221&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(H221=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","CONSTRAINT ",{"$f":"\"PK_\"&N219&\" PRIMARY KEY (\"","v":"PK_soitsedgegrupcnfg PRIMARY KEY ("},{"$f":"IF(OR(G221=\"PK\", G221=\"PK/FK\"), O221, \"\")","v":"edge_grup_id"},",","COMMENT ON COLUMN ",{"$f":"$N$219&\".\"","v":"soitsedgegrupcnfg."},{"$f":"O221","v":"edge_grup_id"}," IS ",{"$f":"\"'\"&I221&\"'\"","v":"'엣지그룹 ID'"},";",null,null,null,""]
[null,null,"구성순번","cnfg_seq",2,"NUMBER(3)","PK","NOT NULL","그룹구성순서",{"$nulls":4},"구성순번","cnfg_seq","NUMBER(3)","INTEGER","NUMBER(3)",null,null,null,"cnfg_seq ","INTEGER ","NOT NULL",",",null,"cnfg_seq",",",null,null,"cnfg_seq ","NUMBER(3) ","NOT NULL",",",null,null,"cnfg_seq",",","COMMENT ON COLUMN ","soitsedgegrupcnfg.","cnfg_seq"," IS ","'그룹구성순서'",";",null,null,null,""]
[null,null,"병렬순번","prll_seq",3,"NUMBER(3)","PK",null,"병렬엣지구성순서",{"$nulls":4},"병렬순번","prll_seq","NUMBER(3)","INTEGER","NUMBER(3)",null,null,null,"prll_seq ","INTEGER ","",",",null,"prll_seq","));",null,null,"prll_seq ","NUMBER(3) ","",",",null,null,"prll_seq",{"$f":"\") using index tablespace \" &AJ226& \") TABLESPACE \" &AI226&\";\"","v":") using index tablespace SOIT_I08_M001) TABLESPACE SOIT_D08_M001;"},"COMMENT ON COLUMN ","soitsedgegrupcnfg.","prll_seq"," IS ","'병렬엣지구성순서'",";",null,null,null,""]
[null,null,"엣지ID","edge_id",4,"VARCHAR2(300)","FK","NOT NULL","소속 엣지ID",{"$nulls":4},"엣지ID","edge_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,null,null,"edge_id ","VARCHAR(300) ","NOT NULL",",",null,"",null,null,null,"edge_id ","VARCHAR2(300) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsedgegrupcnfg.","edge_id"," IS ","'소속 엣지ID'",";",null,null,null,""]
[{"$nulls":21},{"$f":"CONCATENATE(Z221:AB224)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AI221:AL224)","v":{"$error":"#VALUE!"}},{"$nulls":16},{"$error":"#VALUE!"}]
[{"$nulls":34},"SOIT_D08_M001","SOIT_I08_M001"]
[null,"연결엣지 테이블",{"$nulls":11},"soitscnctedge",{"$nulls":33},{"$f":"IF(LEFT(AE227, 13) = \"CONSTRAINT PK\", AE227, \"\")","v":""}]
[13,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N227&\" \"","v":"soitscnctedge "},null," IS ",{"$f":"\"'\"&B227&\"'\"","v":"'연결엣지 테이블'"},";",null,null,null,""]
[null,"soitscnctedge\n(tb_connect_edge)\n(확정)","연결엣지ID","cnct_edge_id",1,"VARCHAR2(300)","PK","NOT NULL","연결 엣지 ID","SUMO 자동생성",null,null,{"$f":"IF(F229=P229, \"EQ\", \"NEQ)\")","v":"EQ"},"연결엣지ID","cnct_edge_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,"CREATE TABLE ",{"$f":"N227&\" (\"","v":"soitscnctedge ("},{"$f":"O229&\" \"","v":"cnct_edge_id "},{"$f":"Q229&\" \"","v":"VARCHAR(300) "},{"$f":"IF(H229=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(G229=\"PK\", G229=\"PK/FK\"), O229, \"\")","v":"cnct_edge_id"},"));","CREATE TABLE ",{"$f":"N227&\" (\"","v":"soitscnctedge ("},{"$f":"O229&\" \"","v":"cnct_edge_id "},{"$f":"R229&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(H229=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","CONSTRAINT ",{"$f":"\"PK_\"&N227&\" PRIMARY KEY (\"","v":"PK_soitscnctedge PRIMARY KEY ("},{"$f":"IF(OR(G229=\"PK\", G229=\"PK/FK\"), O229, \"\")","v":"cnct_edge_id"},{"$f":"\") using index tablespace \" &AJ242& \") TABLESPACE \" &AI242&\";\"","v":") using index tablespace SOIT_I08_M001) TABLESPACE SOIT_D08_M001;"},"COMMENT ON COLUMN ",{"$f":"$N$227&\".\"","v":"soitscnctedge."},{"$f":"O229","v":"cnct_edge_id"}," IS ",{"$f":"\"'\"&I229&\"'\"","v":"'연결 엣지 ID'"},";",null,null,null,""]
[null,null,"노드ID","node_id",2,"VARCHAR2(300)","FK","NOT NULL","소속 교차로 노드 ID","교차로 아닌경우(차선변경), 변경지점의 노드ID",null,null,"EQ","노드ID","node_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,null,null,"node_id ","VARCHAR(300) ","NOT NULL",",",null,"",null,null,null,"node_id ","VARCHAR2(300) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitscnctedge.","node_id"," IS ","'소속 교차로 노드 ID'",";",null,null,null,""]
[null,null,"진입엣지ID","entr_edge_id",3,"VARCHAR2(300)","FK","NOT NULL","진입 엣지 ID","SUMO 자동생성",null,null,"EQ","진입엣지ID","entr_edge_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,null,null,"entr_edge_id ","VARCHAR(300) ","NOT NULL",",",null,"",null,null,null,"entr_edge_id ","VARCHAR2(300) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitscnctedge.","entr_edge_id"," IS ","'진입 엣지 ID'",";",null,null,null,""]
[null,null,"진출엣지ID","exit_edge_id",4,"VARCHAR2(300)","FK","NOT NULL","진출 엣지 ID","SUMO 자동생성",null,null,"EQ","진출엣지ID","exit_edge_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,null,null,"exit_edge_id ","VARCHAR(300) ","NOT NULL",",",null,"",null,null,null,"exit_edge_id ","VARCHAR2(300) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitscnctedge.","exit_edge_id"," IS ","'진출 엣지 ID'",";",null,null,null,""]
[null,null,"회전분류코드","turn_clsf_cd",7,"CHAR(1)",null,"NOT NULL","회전코드(005)","알바(기반정보)와 JOIN, 골목길 등은 수작업",null,"회전정보 (s:직진, r:우회전, l:좌회전, u:유턴)","EQ","회전분류코드","turn_clsf_cd","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",null,null,null,"turn_clsf_cd ","VARCHAR(1) ","NOT NULL",",",null,"",null,null,null,"turn_clsf_cd ","VARCHAR2(1) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitscnctedge.","turn_clsf_cd"," IS ","'회전코드(005)'",";",null,null,null,""]
[null,null,"진입방위코드","entr_pocm_cd",8,"CHAR(2)",null,"NOT NULL","진입방위코드 (006)","동인 제공 이동류 번호 이용",null,"(2:동,6:서,8:남,4:북,12:북서,10:남서,16:남동,14:북동) ","EQ","진입방위코드","entr_pocm_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",null,null,null,"entr_pocm_cd ","VARCHAR(2) ","NOT NULL",",",null,"",null,null,null,"entr_pocm_cd ","VARCHAR2(2) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitscnctedge.","entr_pocm_cd"," IS ","'진입방위코드 (006)'",";",null,null,null,""]
[null,null,"진출방위코드","exit_pocm_cd",9,"CHAR(2)",null,"NOT NULL","진출방위코드 (006)","모양은 다르지만 편의성 위해 이동류 번호 그대로 차용",null,"(2:동,6:서,8:남,4:북,12:북서,10:남서,16:남동,14:북동) ","EQ","진출방위코드","exit_pocm_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",null,null,null,"exit_pocm_cd ","VARCHAR(2) ","NOT NULL",",",null,"",null,null,null,"exit_pocm_cd ","VARCHAR2(2) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitscnctedge.","exit_pocm_cd"," IS ","'진출방위코드 (006)'",";",null,null,null,""]
[null,null,"연결엣지공간정보","cnct_edge_spin",10,"VARHCAR2(2000)",null,"NOT NULL","연결엣지공간정보 (WKT LineString) ","SUMO 자동생성",null,null,"NEQ)","연결엣지공간정보","cnct_edge_spin","BINARY","VARCHAR(2000)","GEOMETRY",null,null,null,"cnct_edge_spin ","VARCHAR(2000) ","NOT NULL",",",null,"",null,null,null,"cnct_edge_spin ","GEOMETRY ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitscnctedge.","cnct_edge_spin"," IS ","'연결엣지공간정보 (WKT LineString) '",";",null,null,null,""]
[null,null,"포화교통류율","strtn_trst_rt",11,"NUMBER(13,9)",null,null,"포화교통류율 (직진 : 2200, 좌회전 : 1800) * 녹색시간 / 주기","수작업 입력",null,null,"EQ","포화교통류율","strtn_trst_rt","NUMBER(13,9)","FLOAT","NUMBER(13,9)",null,null,null,"strtn_trst_rt ","FLOAT ","",",",null,"",null,null,null,"strtn_trst_rt ","NUMBER(13,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitscnctedge.","strtn_trst_rt"," IS ","'포화교통류율 (직진 : 2200, 좌회전 : 1800) * 녹색시간 / 주기'",";",null,null,null,""]
[null,null,"연결엣지길이","cnct_edge_lngt",12,"NUMBER(19,9)",null,null,"연결엣지길이","ICT사업본부에서 생성/입력 예정",null,null,null,"연결엣지길이","cnct_edge_lngt","NUMBER(19,9)","FLOAT","NUMBER(19,9)",null,null,null,"cnct_edge_lngt ","FLOAT ","",",",{"$nulls":5},"cnct_edge_lngt ","NUMBER(19,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitscnctedge.","cnct_edge_lngt"," IS ","'연결엣지길이'",";",null,null,null,""]
[null,null,"진입방위각도","entr_pocm_angl",12,"NUMBER(6,3)",null,null,"진북기준 교차로 진입각도","SUMO 자동생성",null,null,{"$f":"IF(F239=P239, \"EQ\", \"NEQ)\")","v":"EQ"},"진입방위각도","entr_pocm_angl","NUMBER(6,3)","FLOAT","NUMBER(6,3)",null,null,null,"entr_pocm_angl ","FLOAT ","",",",null,{"$f":"IF(OR(G239=\"PK\", G239=\"PK/FK\"), O239, \"\")","v":""},null,null,null,"entr_pocm_angl ","NUMBER(6,3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitscnctedge.","entr_pocm_angl"," IS ","'진북기준 교차로 진입각도'",";",null,null,null,""]
[null,null,"진출방위각도","exit_pocm_angl",13,"NUMBER(6,3)",null,null,"진북기준 교차로 진출각도","SUMO 자동생성",null,null,"EQ","진출방위각도","exit_pocm_angl","NUMBER(6,3)","FLOAT","NUMBER(6,3)",null,null,null,"exit_pocm_angl ","FLOAT ","",",",null,"",null,null,null,"exit_pocm_angl ","NUMBER(6,3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitscnctedge.","exit_pocm_angl"," IS ","'진북기준 교차로 진출각도'",";",null,null,null,""]
[{"$nulls":21},{"$f":"CONCATENATE(Z229:AB240)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AI229:AL240)","v":{"$error":"#VALUE!"}},{"$nulls":16},{"$error":"#VALUE!"}]
[{"$nulls":34},"SOIT_D08_M001","SOIT_I08_M001"]
[null,"연결차로 테이블",{"$nulls":11},"soitscnctlane",{"$nulls":33},{"$f":"IF(LEFT(AE243, 13) = \"CONSTRAINT PK\", AE243, \"\")","v":""}]
[14,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N243&\" \"","v":"soitscnctlane "},null," IS ",{"$f":"\"'\"&B243&\"'\"","v":"'연결차로 테이블'"},";",null,null,null,""]
[null,"soitscnctlane\n(tb_connect_lane)\n(확정)","연결차로ID","cnct_lane_id",1,"VARCHAR2(300)","PK","NOT NULL","연결차로 ID","SUMO 자동생성",null,null,{"$f":"IF(F245=P245, \"EQ\", \"NEQ)\")","v":"EQ"},"연결차로ID","cnct_lane_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,"CREATE TABLE ",{"$f":"N243&\" (\"","v":"soitscnctlane ("},{"$f":"O245&\" \"","v":"cnct_lane_id "},{"$f":"Q245&\" \"","v":"VARCHAR(300) "},{"$f":"IF(H245=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(G245=\"PK\", G245=\"PK/FK\"), O245, \"\")","v":"cnct_lane_id"},"));","CREATE TABLE ",{"$f":"N243&\" (\"","v":"soitscnctlane ("},{"$f":"O245&\" \"","v":"cnct_lane_id "},{"$f":"R245&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(H245=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","CONSTRAINT ",{"$f":"\"PK_\"&N243&\" PRIMARY KEY (\"","v":"PK_soitscnctlane PRIMARY KEY ("},{"$f":"IF(OR(G245=\"PK\", G245=\"PK/FK\"), O245, \"\")","v":"cnct_lane_id"},{"$f":"\") using index tablespace \" &AJ256& \") TABLESPACE \" &AI256&\";\"","v":") using index tablespace SOIT_I08_M001) TABLESPACE SOIT_D08_M001;"},"COMMENT ON COLUMN ",{"$f":"$N$243&\".\"","v":"soitscnctlane."},{"$f":"O245","v":"cnct_lane_id"}," IS ",{"$f":"\"'\"&I245&\"'\"","v":"'연결차로 ID'"},";",null,null,null,""]
[null,null,"연결엣지ID","cnct_edge_id",{"$f":"E245+1","v":2},"VARCHAR2(300)","FK","NOT NULL","연결엣지 ID","SUMO 자동생성",null,null,"EQ","연결엣지ID","cnct_edge_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,null,null,"cnct_edge_id ","VARCHAR(300) ","NOT NULL",",",null,"",null,null,null,"cnct_edge_id ","VARCHAR2(300) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitscnctlane.","cnct_edge_id"," IS ","'연결엣지 ID'",";",null,null,null,""]
[null,null,"진입차로ID","entr_lane_id",3,"VARCHAR2(300)","FK","NOT NULL","진입차로 ID","SUMO 자동생성",null,null,"EQ","진입차로ID","entr_lane_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,null,null,"entr_lane_id ","VARCHAR(300) ","NOT NULL",",",null,"",null,null,null,"entr_lane_id ","VARCHAR2(300) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitscnctlane.","entr_lane_id"," IS ","'진입차로 ID'",";",null,null,null,""]
[null,null,"진출차로ID","exit_lane_id",2,"VARCHAR2(300)","FK","NOT NULL","진출차로 ID","SUMO 자동생성",null,null,"EQ","진출차로ID","exit_lane_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,null,null,"exit_lane_id ","VARCHAR(300) ","NOT NULL",",",null,"",null,null,null,"exit_lane_id ","VARCHAR2(300) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitscnctlane.","exit_lane_id"," IS ","'진출차로 ID'",";",null,null,null,""]
[null,null,"노드ID","node_id",{"$f":"E248+1","v":3},"VARCHAR2(300)","FK","NOT NULL","해당 교차로 노드ID","SUMO 자동생성",null,null,"EQ","소속노드ID","node_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,null,null,"node_id ","VARCHAR(300) ","NOT NULL",",",null,"",null,null,null,"node_id ","VARCHAR2(300) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitscnctlane.","node_id"," IS ","'해당 교차로 노드ID'",";",null,null,null,""]
[null,null,"진입엣지그룹ID","entr_edge_id",4,"VARCHAR2(300)","FK",null,"진입 엣지그룹ID",null,null,null,"EQ","진입엣지그룹ID","entr_edge_grup_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,null,null,"entr_edge_grup_id ","VARCHAR(300) ","",",",null,"",null,null,null,"entr_edge_grup_id ","VARCHAR2(300) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitscnctlane.","entr_edge_grup_id"," IS ","'진입 엣지그룹ID'",";",null,null,null,""]
[null,null,"진출엣지그룹ID","exit_edge_id",3,"VARCHAR2(300)","FK",null,"진출 엣지그룹ID",null,null,null,"EQ","진출엣지그룹ID","exit_edge_grup_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,null,null,"exit_edge_grup_id ","VARCHAR(300) ","",",",null,"",null,null,null,"exit_edge_grup_id ","VARCHAR2(300) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitscnctlane.","exit_edge_grup_id"," IS ","'진출 엣지그룹ID'",";",null,null,null,""]
[null,null,"차로번호","lane_no",{"$f":"E251+1","v":4},"NUMBER(2)",null,"NOT NULL","차로번호","SUMO 자동생성",null,null,"EQ","차로번호","lane_no","NUMBER(2)","INTEGER","NUMBER(2)",null,null,null,"lane_no ","INTEGER ","NOT NULL",",",null,"",null,null,null,"lane_no ","NUMBER(2) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitscnctlane.","lane_no"," IS ","'차로번호'",";",null,null,null,""]
[null,null,"회전연결순서","turn_cnct_seq",5,"NUMBER(3)",null,"NOT NULL","회전연결순서","차로순번과 동일한 항목 같은데, 필요한가?",null,null,"EQ","회전연결순서","turn_cnct_seq","NUMBER(3)","INTEGER","NUMBER(3)",null,null,null,"turn_cnct_seq ","INTEGER ","NOT NULL",",",null,"",null,null,null,"turn_cnct_seq ","NUMBER(3) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitscnctlane.","turn_cnct_seq"," IS ","'회전연결순서'",";",null,null,null,""]
[null,null,"연결차로공간정보","cnct_lane_spin",4,"VARCHAR2(2000)",null,"NOT NULL","연결차로 지리정보(WKT LineString)","SUMO 자동생성",null,null,"NEQ)","연결차로공간정보","cnct_lane_spin","BINARY","VARCHAR(2000)","GEOMETRY",{"$nulls":8},"",null,null,null,"cnct_lane_spin ","GEOMETRY ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitscnctlane.","cnct_lane_spin"," IS ","'연결차로 지리정보(WKT LineString)'",";",null,null,null,""]
[{"$nulls":21},{"$f":"CONCATENATE(Z245:AB254)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AI245:AL254)","v":{"$error":"#VALUE!"}},{"$nulls":16},{"$error":"#VALUE!"}]
[{"$nulls":34},"SOIT_D08_M001","SOIT_I08_M001"]
[null,"노드 테이블",{"$nulls":11},"soitsnode",{"$nulls":33},{"$f":"IF(LEFT(AE257, 13) = \"CONSTRAINT PK\", AE257, \"\")","v":""}]
[15,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N257&\" \"","v":"soitsnode "},null," IS ",{"$f":"\"'\"&B257&\"'\"","v":"'노드 테이블'"},";",null,null,null,""]
[null,"soitsnode\n(tb_node)\n(확정)","노드ID","node_id",1,"VARCHAR2(300)","PK","NOT NULL","노드ID","SUMO 자동생성",null,null,{"$f":"IF(F259=P259, \"EQ\", \"NEQ)\")","v":"EQ"},"노드ID","node_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,"CREATE TABLE ",{"$f":"N257&\" (\"","v":"soitsnode ("},{"$f":"O259&\" \"","v":"node_id "},{"$f":"Q259&\" \"","v":"VARCHAR(300) "},{"$f":"IF(H259=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(G259=\"PK\", G259=\"PK/FK\"), O259, \"\")","v":"node_id"},"));","CREATE TABLE ",{"$f":"N257&\" (\"","v":"soitsnode ("},{"$f":"O259&\" \"","v":"node_id "},{"$f":"R259&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(H259=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","CONSTRAINT ",{"$f":"\"PK_\"&N257&\" PRIMARY KEY (\"","v":"PK_soitsnode PRIMARY KEY ("},{"$f":"IF(OR(G259=\"PK\", G259=\"PK/FK\"), O259, \"\")","v":"node_id"},{"$f":"\") using index tablespace \" &AJ279& \") TABLESPACE \" &AI279&\";\"","v":") using index tablespace SOIT_I08_M001) TABLESPACE SOIT_D08_M001;"},"COMMENT ON COLUMN ",{"$f":"$N$257&\".\"","v":"soitsnode."},{"$f":"O259","v":"node_id"}," IS ",{"$f":"\"'\"&I259&\"'\"","v":"'노드ID'"},";",null,null,null,""]
[null,null,"현장교차로ID","spot_ints_id",{"$f":"E259+1","v":2},"NUMBER(5)","FK","NULL","현장교차로ID","매핑 테이블이 아닌, 마스터에 같이 관리",null,null,"EQ","현장교차로ID","spot_ints_id","NUMBER(5)","INTEGER","NUMBER(5)",null,null,null,"spot_ints_id ","INTEGER ","",",",{"$nulls":5},"spot_ints_id ","NUMBER(5) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsnode.","spot_ints_id"," IS ","'현장교차로ID'",";",null,null,null,""]
[null,null,"연동그룹ID","lnkg_grup_id",3,"VARCHAR2(20)","FK","NULL","소속연동그룹ID","알바(기반정보)와 JOIN, 골목길 등은 수작업",null,null,"EQ","소속연동그룹ID","lnkg_grup_id","VARCHAR2(20)","VARCHAR(20)","VARCHAR2(20)",null,null,null,"lnkg_grup_id ","VARCHAR(20) ","",",",{"$nulls":5},"lnkg_grup_id ","VARCHAR2(20) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsnode.","lnkg_grup_id"," IS ","'소속연동그룹ID'",";",null,null,null,""]
[null,null,"행정구역코드","pbadms_dstt_cd",4,"CHAR(5)","FK","NOT NULL","행정구역코드 (052)","QGIS에서 한 번에 작업",null,null,"EQ","행정구역코드","pbadms_dstt_cd","CHAR(5)","VARCHAR(5)","VARCHAR2(5)",null,null,null,"pbadms_dstt_cd ","VARCHAR(5) ","NOT NULL",",",{"$nulls":5},"pbadms_dstt_cd ","VARCHAR2(5) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsnode.","pbadms_dstt_cd"," IS ","'행정구역코드 (052)'",";",null,null,null,""]
[null,null,"지역분할코드","rgn_prttn_cd",5,"CHAR(2)","FK","NOT NULL","지역분할코드 (051)","99:외부교차로",null,null,"EQ","지역분할코드","rgn_prttn_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",null,null,null,"rgn_prttn_cd ","VARCHAR(2) ","NOT NULL",",",{"$nulls":5},"rgn_prttn_cd ","VARCHAR2(2) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsnode.","rgn_prttn_cd"," IS ","'지역분할코드 (051)'",";",null,null,null,""]
[null,null,"현장교차로일련번호","spot_ints_sn",6,"NUMBER(4)",null,null,"현장교차로일련번호","매핑 테이블이 아닌, 마스터에 같이 관리",null,null,"EQ","현장교차로일련번호","spot_ints_sn","NUMBER(4)","INTEGER","NUMBER(4)",null,null,null,"spot_ints_sn ","INTEGER ","",",",{"$nulls":5},"spot_ints_sn ","NUMBER(4) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsnode.","spot_ints_sn"," IS ","'현장교차로일련번호'",";",null,null,null,""]
[null,null,"주교차로구분코드","majr_ints_se_cd",7,"CHAR(2)",null,null,"주교차로구분코드 (062)"," (1:주교차로, 2:연등교차로)",null,"김종성 추가 요청",null,"주교차로구분코드","majr_ints_se_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",{"$nulls":12},"majr_ints_se_cd ","VARCHAR2(2) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsnode.","majr_ints_se_cd"," IS ","'주교차로구분코드 (062)'",";",null,null,null,""]
[null,null,"교차로명","ints_nm",8,"VARCHAR2(50)",null,null,"교차로명","매핑 테이블이 아닌, 마스터에 같이 관리",null,null,{"$f":"IF(F266=P266, \"EQ\", \"NEQ)\")","v":"EQ"},"교차로명","ints_nm","VARCHAR2(50)","VARCHAR(50)","VARCHAR2(50)",null,null,null,{"$f":"O266&\" \"","v":"ints_nm "},{"$f":"Q266&\" \"","v":"VARCHAR(50) "},{"$f":"IF(H266=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",{"$nulls":5},"ints_nm ","VARCHAR2(50) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsnode.","ints_nm"," IS ","'교차로명'",";",null,null,null,""]
[null,null,"교차로구분코드","ints_se_cd",9,"CHAR(1)",null,null,"교차로구분코드 (054)","1 : 일반노드,2 : 신호교차로,3 : 스마트교차로,4 : 차선변경노드,5 : 골목길노드","엣지그룹 구성 시 일반노드간 구성이 될수도 있나요?\n-> 연동그룹 표현 시 일반노드까지 분리됨",null,"EQ","교차로구분코드","ints_se_cd","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",null,null,null,"ints_se_cd ","VARCHAR(1) ","",",",{"$nulls":5},"ints_se_cd ","VARCHAR2(1) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsnode.","ints_se_cd"," IS ","'교차로구분코드 (054)'",";",null,null,null,""]
[null,null,"연동그룹구성구분코드","lnkg_grup_cnfg_se_cd",10,"CHAR(1)",null,null,"연동그룹구성구분코드 (055)","알바(기반정보)와 JOIN, 골목길 등은 수작업\n1 : 일반교차로(중간노드), 2 : CI, 3 : SCI, 4 : MI",null,null,"EQ","연동그룹구성구분코드","lnkg_grup_cnfg_se_cd","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",null,null,null,"lnkg_grup_cnfg_se_cd ","VARCHAR(1) ","",",",{"$nulls":5},"lnkg_grup_cnfg_se_cd ","VARCHAR2(1) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsnode.","lnkg_grup_cnfg_se_cd"," IS ","'연동그룹구성구분코드 (055)'",";",null,null,null,""]
[null,null,"노드경도","node_lot",11,"NUMBER(13,10)",null,"NOT NULL","경도 좌표(x축)","SUMO 자동생성",null,null,"EQ","노드경도","node_lot","NUMBER(13,10)","FLOAT","NUMBER(13,10)",null,null,null,"node_lot ","FLOAT ","NOT NULL",",",{"$nulls":5},"node_lot ","NUMBER(13,10) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsnode.","node_lot"," IS ","'경도 좌표(x축)'",";",null,null,null,""]
[null,null,"노드위도","node_lat",12,"NUMBER(12,10)",null,"NOT NULL","위도 좌표(y축)","SUMO 자동생성",null,null,"EQ","노드위도","node_lat","NUMBER(12,10)","FLOAT","NUMBER(12,10)",null,null,null,"node_lat ","FLOAT ","NOT NULL",",",{"$nulls":5},"node_lat ","NUMBER(12,10) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsnode.","node_lat"," IS ","'위도 좌표(y축)'",";",null,null,null,""]
[null,null,"노드고도","node_lntd",13,"NUMBER(10,2)",null,null,"고도 높이(z축, meter)","SUMO 자동생성",null,null,"EQ","노드고도","node_lntd","NUMBER(10,2)","FLOAT","NUMBER(10,2)",null,null,null,"node_lntd ","FLOAT ","",",",{"$nulls":5},"node_lntd ","NUMBER(10,2) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsnode.","node_lntd"," IS ","'고도 높이(z축, meter)'",";",null,null,null,""]
[null,null,"CI 경도","ci_lot",14,"NUMBER(13,10)",null,null,"CI 경도 좌표(x축)","ICT본부에서 데이터 생성하여 입력",null,null,null,"CI 경도","ci_lot","NUMBER(13,10)","FLOAT","NUMBER(13,10)",null,null,null,"ci_lot ","FLOAT ","",",",{"$nulls":5},"ci_lot ","NUMBER(13,10) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsnode.","ci_lot"," IS ","'CI 경도 좌표(x축)'",";",null,null,null,""]
[null,null,"CI 위도","ci_lat",15,"NUMBER(12,10)",null,null,"CI 위도 좌표(y축)","ICT본부에서 데이터 생성하여 입력",null,null,null,"CI 위도","ci_lat","NUMBER(12,10)","FLOAT","NUMBER(12,10)",null,null,null,"ci_lat ","FLOAT ","",",",{"$nulls":5},"ci_lat ","NUMBER(12,10) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsnode.","ci_lat"," IS ","'CI 위도 좌표(y축)'",";",null,null,null,""]
[null,null,"LOS 경도","los_lot",16,"NUMBER(13,10)",null,null,"LOS 경도 좌표(x축)","ICT본부에서 데이터 생성하여 입력",null,null,null,"LOS 경도","los_lot","NUMBER(13,10)","FLOAT","NUMBER(13,10)",null,null,null,"los_lot ","FLOAT ","",",",{"$nulls":5},"los_lot ","NUMBER(13,10) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsnode.","los_lot"," IS ","'LOS 경도 좌표(x축)'",";",null,null,null,""]
[null,null,"LOS 위도","los_lat",17,"NUMBER(12,10)",null,null,"LOS 위도 좌표(y축)","ICT본부에서 데이터 생성하여 입력",null,null,null,"LOS 위도","los_lat","NUMBER(12,10)","FLOAT","NUMBER(12,10)",null,null,null,"los_lat ","FLOAT ","",",",{"$nulls":5},"los_lat ","NUMBER(12,10) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsnode.","los_lat"," IS ","'LOS 위도 좌표(y축)'",";",null,null,null,""]
[null,null,"횡단보도지점여부","across_ints_yn",18,"CHAR(1)",null,null,"횡단보도지점여부","ICT본부에서 데이터 생성하여 입력 (예측값)",null,null,null,"횡단보도지점여부","across_ints_yn","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",null,null,null,"across_ints_yn ","VARCHAR(1) ","",",",{"$nulls":5},"across_ints_yn ","VARCHAR2(1) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsnode.","across_ints_yn"," IS ","'횡단보도지점여부'",";",null,null,null,""]
[null,null,"진입엣지수","entr_edge_cnt",19,"NUMBER(2)",null,null,"교차로 진입엣지수","ICT본부에서 데이터 생성하여 입력",null,null,null,"진입엣지수","entr_edge_cnt","NUMBER(2)","INTEGER","NUMBER(2)",null,null,null,"entr_edge_cnt ","INTEGER ","",",",{"$nulls":5},"entr_edge_cnt ","NUMBER(2) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsnode.","entr_edge_cnt"," IS ","'교차로 진입엣지수'",";",null,null,null,""]
[{"$nulls":21},{"$f":"CONCATENATE(Z259:AB271)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AI259:AL271)","v":{"$error":"#VALUE!"}},{"$nulls":16},{"$error":"#VALUE!"}]
[{"$nulls":34},"SOIT_D08_M001","SOIT_I08_M001"]
[null,"노드 테이블",{"$nulls":11},"mtvsnode",{"$nulls":33},{"$f":"IF(LEFT(AE280, 13) = \"CONSTRAINT PK\", AE280, \"\")","v":""}]
["15-1","Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N280&\" \"","v":"mtvsnode "},null," IS ",{"$f":"\"'\"&B280&\"'\"","v":"'노드 테이블'"},";",null,null,null,""]
[null,"mtvsnode","노드ID","node_id",1,"VARCHAR2(300)","PK","NOT NULL","노드ID","SUMO 자동생성",null,null,{"$f":"IF(F282=P282, \"EQ\", \"NEQ)\")","v":"EQ"},"노드ID","node_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,"CREATE TABLE ",{"$f":"N280&\" (\"","v":"mtvsnode ("},{"$f":"O282&\" \"","v":"node_id "},{"$f":"Q282&\" \"","v":"VARCHAR(300) "},{"$f":"IF(H282=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(G282=\"PK\", G282=\"PK/FK\"), O282, \"\")","v":"node_id"},"));","CREATE TABLE ",{"$f":"N280&\" (\"","v":"mtvsnode ("},{"$f":"O282&\" \"","v":"node_id "},{"$f":"R282&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(H282=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","CONSTRAINT ",{"$f":"\"PK_\"&N280&\" PRIMARY KEY (\"","v":"PK_mtvsnode PRIMARY KEY ("},{"$f":"IF(OR(G282=\"PK\", G282=\"PK/FK\"), O282, \"\")","v":"node_id"},") using index tablespace SOIT_I08);","COMMENT ON COLUMN ",{"$f":"$N$280&\".\"","v":"mtvsnode."},{"$f":"O282","v":"node_id"}," IS ",{"$f":"\"'\"&I282&\"'\"","v":"'노드ID'"},";",null,null,null,""]
[null,null,"현장교차로ID","spot_ints_id",{"$f":"E282+1","v":2},"NUMBER(5)","FK","NULL","현장교차로ID","매핑 테이블이 아닌, 마스터에 같이 관리",null,null,"EQ","현장교차로ID","spot_ints_id","NUMBER(5)","INTEGER","NUMBER(5)",null,null,null,"spot_ints_id ","INTEGER ","",",",{"$nulls":5},"spot_ints_id ","NUMBER(5) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","mtvsnode.","spot_ints_id"," IS ","'현장교차로ID'",";",null,null,null,""]
[null,null,"연동그룹ID","lnkg_grup_id",3,"VARCHAR2(20)","FK","NULL","소속연동그룹ID","알바(기반정보)와 JOIN, 골목길 등은 수작업",null,null,"EQ","소속연동그룹ID","lnkg_grup_id","VARCHAR2(20)","VARCHAR(20)","VARCHAR2(20)",null,null,null,"lnkg_grup_id ","VARCHAR(20) ","",",",{"$nulls":5},"lnkg_grup_id ","VARCHAR2(20) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","mtvsnode.","lnkg_grup_id"," IS ","'소속연동그룹ID'",";",null,null,null,""]
[null,null,"행정구역코드","pbadms_dstt_cd",4,"CHAR(5)","FK","NOT NULL","행정구역코드 (052)","QGIS에서 한 번에 작업",null,null,"EQ","행정구역코드","pbadms_dstt_cd","CHAR(5)","VARCHAR(5)","VARCHAR2(5)",null,null,null,"pbadms_dstt_cd ","VARCHAR(5) ","NOT NULL",",",{"$nulls":5},"pbadms_dstt_cd ","VARCHAR2(5) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","mtvsnode.","pbadms_dstt_cd"," IS ","'행정구역코드 (052)'",";",null,null,null,""]
[null,null,"지역분할코드","rgn_prttn_cd",5,"CHAR(2)","FK","NOT NULL","지역분할코드 (051)","99:외부교차로",null,null,"EQ","지역분할코드","rgn_prttn_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",null,null,null,"rgn_prttn_cd ","VARCHAR(2) ","NOT NULL",",",{"$nulls":5},"rgn_prttn_cd ","VARCHAR2(2) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","mtvsnode.","rgn_prttn_cd"," IS ","'지역분할코드 (051)'",";",null,null,null,""]
[null,null,"현장교차로일련번호","spot_ints_sn",6,"NUMBER(4)",null,null,"현장교차로일련번호","매핑 테이블이 아닌, 마스터에 같이 관리",null,null,"EQ","현장교차로일련번호","spot_ints_sn","NUMBER(4)","INTEGER","NUMBER(4)",null,null,null,"spot_ints_sn ","INTEGER ","",",",{"$nulls":5},"spot_ints_sn ","NUMBER(4) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","mtvsnode.","spot_ints_sn"," IS ","'현장교차로일련번호'",";",null,null,null,""]
[null,null,"주교차로구분코드","majr_ints_se_cd",7,"CHAR(2)",null,null,"주교차로구분코드 (062)"," (1:주교차로, 2:연등교차로)",null,"김종성 추가 요청",null,"주교차로구분코드","majr_ints_se_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",null,null,null,"majr_ints_se_cd ","VARCHAR(2) ","",",",{"$nulls":5},"majr_ints_se_cd ","VARCHAR2(2) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","mtvsnode.","majr_ints_se_cd"," IS ","'주교차로구분코드 (062)'",";",null,null,null,""]
[null,null,"교차로명","ints_nm",8,"VARCHAR2(50)",null,null,"교차로명","매핑 테이블이 아닌, 마스터에 같이 관리",null,null,{"$f":"IF(F289=P289, \"EQ\", \"NEQ)\")","v":"EQ"},"교차로명","ints_nm","VARCHAR2(50)","VARCHAR(50)","VARCHAR2(50)",null,null,null,"ints_nm ","VARCHAR(50) ","",",",{"$nulls":5},"ints_nm ","VARCHAR2(50) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","mtvsnode.","ints_nm"," IS ","'교차로명'",";",null,null,null,""]
[null,null,"교차로구분코드","ints_se_cd",9,"CHAR(1)",null,null,"교차로구분코드 (054)","1 : 일반노드,2 : 신호교차로,3 : 스마트교차로,4 : 차선변경노드,5 : 골목길노드","엣지그룹 구성 시 일반노드간 구성이 될수도 있나요?\n-> 연동그룹 표현 시 일반노드까지 분리됨",null,"EQ","교차로구분코드","ints_se_cd","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",null,null,null,"ints_se_cd ","VARCHAR(1) ","",",",{"$nulls":5},"ints_se_cd ","VARCHAR2(1) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","mtvsnode.","ints_se_cd"," IS ","'교차로구분코드 (054)'",";",null,null,null,""]
[null,null,"연동그룹구성구분코드","lnkg_grup_cnfg_se_cd",10,"CHAR(1)",null,null,"연동그룹구성구분코드 (055)","알바(기반정보)와 JOIN, 골목길 등은 수작업\n1 : 일반교차로(중간노드), 2 : CI, 3 : SCI, 4 : MI",null,null,"EQ","연동그룹구성구분코드","lnkg_grup_cnfg_se_cd","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",null,null,null,"lnkg_grup_cnfg_se_cd ","VARCHAR(1) ","",",",{"$nulls":5},"lnkg_grup_cnfg_se_cd ","VARCHAR2(1) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","mtvsnode.","lnkg_grup_cnfg_se_cd"," IS ","'연동그룹구성구분코드 (055)'",";",null,null,null,""]
[null,null,"노드경도","node_lot",11,"NUMBER(13,10)",null,"NOT NULL","경도 좌표(x축)","SUMO 자동생성",null,null,"EQ","노드경도","node_lot","NUMBER(13,10)","FLOAT","NUMBER(13,10)",null,null,null,"node_lot ","FLOAT ","NOT NULL",",",{"$nulls":5},"node_lot ","NUMBER(13,10) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","mtvsnode.","node_lot"," IS ","'경도 좌표(x축)'",";",null,null,null,""]
[null,null,"노드위도","node_lat",12,"NUMBER(12,10)",null,"NOT NULL","위도 좌표(y축)","SUMO 자동생성",null,null,"EQ","노드위도","node_lat","NUMBER(12,10)","FLOAT","NUMBER(12,10)",null,null,null,"node_lat ","FLOAT ","NOT NULL",",",{"$nulls":5},"node_lat ","NUMBER(12,10) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","mtvsnode.","node_lat"," IS ","'위도 좌표(y축)'",";",null,null,null,""]
[null,null,"노드고도","node_lntd",13,"NUMBER(10,2)",null,null,"고도 높이(z축, meter)","SUMO 자동생성",null,null,"EQ","노드고도","node_lntd","NUMBER(10,2)","FLOAT","NUMBER(10,2)",null,null,null,"node_lntd ","FLOAT ","",",",{"$nulls":5},"node_lntd ","NUMBER(10,2) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","mtvsnode.","node_lntd"," IS ","'고도 높이(z축, meter)'",";",null,null,null,""]
[{"$nulls":21},{"$f":"CONCATENATE(Z282:AB294)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AI282:AL294)","v":{"$error":"#VALUE!"}},{"$nulls":16},{"$error":"#VALUE!"}]
[null,"엣지 테이블",{"$nulls":11},"soitsedge",{"$nulls":33},""]
[17,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N296&\" \"","v":"soitsedge "},null," IS ",{"$f":"\"'\"&B296&\"'\"","v":"'엣지 테이블'"},";",null,null,null,""]
[null,"soitsedge\n(tb_edge)\n(확정)","엣지ID","edge_id",1,"VARCHAR2(300)","PK","NOT NULL","엣지ID","SUMO 자동생성",null,null,{"$f":"IF(F298=P298, \"EQ\", \"NEQ)\")","v":"EQ"},"엣지ID","edge_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",{"$nulls":10},"CREATE TABLE ",{"$f":"N296&\" (\"","v":"soitsedge ("},{"$f":"O298&\" \"","v":"edge_id "},{"$f":"R298&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(H298=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","CONSTRAINT ",{"$f":"\"PK_\"&N296&\" PRIMARY KEY (\"","v":"PK_soitsedge PRIMARY KEY ("},{"$f":"IF(OR(G298=\"PK\", G298=\"PK/FK\"), O298, \"\")","v":"edge_id"},{"$f":"\") using index tablespace \" &AJ317& \") TABLESPACE \" &AI317&\";\"","v":") using index tablespace SOIT_I08_M001) TABLESPACE SOIT_D08_M001;"},"COMMENT ON COLUMN ",{"$f":"$N$296&\".\"","v":"soitsedge."},{"$f":"O298","v":"edge_id"}," IS ",{"$f":"\"'\"&I298&\"'\"","v":"'엣지ID'"},";",null,null,null,""]
[null,null,"진입엣지ID","entr_edge_id",2,"VARCHAR2(300)","FK",null,"진입엣지ID","SUMO 자동생성",null,null,"EQ","도로인접진입엣지ID","entr_edge_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",{"$nulls":12},"entr_edge_id ","VARCHAR2(300) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsedge.","entr_edge_id"," IS ","'진입엣지ID'",";",null,null,null,""]
[null,null,"진출엣지ID","exit_edge_id",3,"VARCHAR2(300)","FK",null,"진출엣지ID","SUMO 자동생성",null,null,"EQ","도로인접진출엣지ID","exit_edge_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",{"$nulls":12},"exit_edge_id ","VARCHAR2(300) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsedge.","exit_edge_id"," IS ","'진출엣지ID'",";",null,null,null,""]
[null,null,"시작노드ID","bgng_node_id",4,"VARCHAR2(300)","FK",null,"시작노드ID","SUMO 자동생성",null,null,"EQ","시작노드ID","bgng_node_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",{"$nulls":12},"bgng_node_id ","VARCHAR2(300) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsedge.","bgng_node_id"," IS ","'시작노드ID'",";",null,null,null,""]
[null,null,"종료노드ID","end_node_id",5,"VARCHAR2(300)","FK",null,"종료노드ID","SUMO 자동생성",null,null,"EQ","종료노드ID","end_node_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",{"$nulls":12},"end_node_id ","VARCHAR2(300) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsedge.","end_node_id"," IS ","'종료노드ID'",";",null,null,null,""]
[null,null,"엣지길이","edge_lngt",7,"NUMBER(19,9)",null,"NOT NULL","엣지 길이(meter)","SUMO 자동생성",null,null,"EQ","엣지길이","edge_lngt","NUMBER(19,9)","FLOAT","NUMBER(19,9)",{"$nulls":12},"edge_lngt ","NUMBER(19,9) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsedge.","edge_lngt"," IS ","'엣지 길이(meter)'",";",null,null,null,""]
[null,null,"방향구분코드","drct_se_cd",8,"CHAR(1)",null,"NOT NULL","방향구분코드(004)","상/하행으로 구분, 위의 엣지그룹 테이블 등과 JOIN 후 자동생성",null,"상/하 혹은 좌/우 기준으로 1/2","EQ","방향구분코드","drct_se_cd","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",{"$nulls":12},"drct_se_cd ","VARCHAR2(1) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsedge.","drct_se_cd"," IS ","'방향구분코드(004)'",";",null,null,null,""]
[null,null,"차로수","lane_cnt",9,"NUMBER(2)",null,"NOT NULL","차로 수","SUMO 자동생성",null,null,"EQ","차로수","lane_cnt","NUMBER(2)","INTEGER","NUMBER(2)",{"$nulls":12},"lane_cnt ","NUMBER(2) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsedge.","lane_cnt"," IS ","'차로 수'",";",null,null,null,""]
[null,null,"도로설계속도","road_design_sped",10,"NUMBER(5)",null,null,"도로설계속도","SUMO 자동생성",null,null,"EQ","도로설계속도","road_design_sped","NUMBER(5)","INTEGER","NUMBER(5)",{"$nulls":12},"road_design_sped ","NUMBER(5) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsedge.","road_design_sped"," IS ","'도로설계속도'",";",null,null,null,"",{"$nulls":6},"FLOAT"]
[null,null,"도로등급코드","road_grad_cd",11,"CHAR(7)",null,null,"도로등급코드(060)","SUMO 자동생성",null,"101:고속국도, 102:도시고속화도로, 103:일반국도, 104:특별/광역시도, 105:국가지원지방도, 106:지방도, 107:시/군도, 108:고속도로 연결램프","EQ","도로등급코드","road_grad_cd","CHAR(7)","VARCHAR(7)","VARCHAR2(7)",{"$nulls":12},"road_grad_cd ","VARCHAR2(7) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsedge.","road_grad_cd"," IS ","'도로등급코드(060)'",";",null,null,null,""]
[null,null,"행정구역코드","pbadms_dstt_cd",12,"CHAR(5)","FK",null,"행정구역코드 (052)","SUMO 자동생성",null,null,"EQ","행정구역코드","pbadms_dstt_cd","CHAR(5)","VARCHAR(5)","VARCHAR2(5)",{"$nulls":12},"pbadms_dstt_cd ","VARCHAR2(5) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsedge.","pbadms_dstt_cd"," IS ","'행정구역코드 (052)'",";",null,null,null,""]
[null,null,"지역분할코드","rgn_prttn_cd",13,"CHAR(2)","FK",null,"지역분할코드 (051)",{"$nulls":4},"지역분할코드","rgn_prttn_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",{"$nulls":12},"rgn_prttn_cd ","VARCHAR2(2) ",null,",",{"$nulls":4},"COMMENT ON COLUMN ","soitsedge.","rgn_prttn_cd"," IS ","'지역분할코드 (051)'",";",null,null,null,""]
[null,null,"도로형태구분코드","road_form_se_cd",14,"CHAR(2)",null,null,"도로형태구분코드(061)","SUMO 자동생성",null,"01:일반도로, 02:교량, 03:터널, 04:고가도로, 05:지하차도",{"$f":"IF(F310=P310, \"EQ\", \"NEQ)\")","v":"EQ"},"도로형태구분코드","road_form_se_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",{"$nulls":12},"road_form_se_cd ","VARCHAR2(2) ",{"$f":"IF(H310=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",{"$nulls":4},"COMMENT ON COLUMN ","soitsedge.","road_form_se_cd"," IS ","'도로형태구분코드(061)'",";",null,null,null,""]
[null,null,"엣지공간정보","edge_spin",15,"VARCHAR2(2000)",null,"NOT NULL","엣지 지리정보(WKT LineString)","SUMO 자동생성",null,null,"NEQ)","엣지공간정보","edge_spin","BINARY","VARCHAR(2000)","GEOMETRY",{"$nulls":12},"edge_spin ","GEOMETRY ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsedge.","edge_spin"," IS ","'엣지 지리정보(WKT LineString)'",";",null,null,null,""]
[null,null,"대표경도","rprs_lot",16,"NUMBER(13,10)",null,null,"대표경도","ICT사업본부에서 생성/입력 예정",null,null,null,"대표경도","rprs_lot","NUMBER(13,10)",null,"NUMBER(13,10)",{"$nulls":12},"rprs_lot ","NUMBER(13,10) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsedge.","rprs_lot"," IS ","'대표경도'",";",null,null,null,""]
[null,null,"대표위도","rprs_lat",17,"NUMBER(12,10)",null,null,"대표위도","ICT사업본부에서 생성/입력 예정",null,null,null,"대표위도","rprs_lat","NUMBER(12,10)",null,"NUMBER(12,10)",{"$nulls":12},"rprs_lat ","NUMBER(12,10) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsedge.","rprs_lat"," IS ","'대표위도'",";",null,null,null,""]
[null,null,"종료세그먼트 순번","end_sgmn_no",18,"NUMBER(3)",null,null,"종료세그먼트순번","ICT사업본부에서 생성/입력 예정",null,null,null,"종료세그먼트 순번","end_sgmn_no","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"end_sgmn_no ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsedge.","end_sgmn_no"," IS ","'종료세그먼트순번'",";",null,null,null,""]
[null,null,"일방통행여부","oneway_yn",19,"CHAR(1)",null,"NOT NULL","일방통행여부","ICT본부에서 데이터 입력, 인식되는 구간만 입력됨.",null,null,null,"일방통행여부","oneway_yn","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",{"$nulls":12},"oneway_yn ","VARCHAR2(1) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsedge.","oneway_yn"," IS ","'일방통행여부'",";",null,null,null,""]
[{"$nulls":30},{"$f":"CONCATENATE(AI298:AL311)","v":{"$error":"#VALUE!"}},{"$nulls":16},{"$error":"#VALUE!"}]
[{"$nulls":34},"SOIT_D08_M001","SOIT_I08_M001"]
[null,"차로 테이블",{"$nulls":11},"soitslane",{"$nulls":33},{"$f":"IF(LEFT(AE318, 13) = \"CONSTRAINT PK\", AE318, \"\")","v":""}]
[18,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N318&\" \"","v":"soitslane "},null," IS ",{"$f":"\"'\"&B318&\"'\"","v":"'차로 테이블'"},";",null,null,null,""]
[null,"soitslane\n(tb_lane)\n(확정)","차로ID","lane_id",1,"VARCHAR2(300)","PK","NOT NULL","차로ID",null,null,null,{"$f":"IF(F320=P320, \"EQ\", \"NEQ)\")","v":"EQ"},"차로ID","lane_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,"CREATE TABLE ",{"$f":"N318&\" (\"","v":"soitslane ("},{"$f":"O320&\" \"","v":"lane_id "},{"$f":"Q320&\" \"","v":"VARCHAR(300) "},{"$f":"IF(H320=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(G320=\"PK\", G320=\"PK/FK\"), O320, \"\")","v":"lane_id"},"));","CREATE TABLE ",{"$f":"N318&\" (\"","v":"soitslane ("},{"$f":"O320&\" \"","v":"lane_id "},{"$f":"R320&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(H320=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","CONSTRAINT ",{"$f":"\"PK_\"&N318&\" PRIMARY KEY (\"","v":"PK_soitslane PRIMARY KEY ("},{"$f":"IF(OR(G320=\"PK\", G320=\"PK/FK\"), O320, \"\")","v":"lane_id"},{"$f":"\") using index tablespace \" &AJ333& \") TABLESPACE \" &AI333&\";\"","v":") using index tablespace SOIT_I08_M001) TABLESPACE SOIT_D08_M001;"},"COMMENT ON COLUMN ",{"$f":"$N$318&\".\"","v":"soitslane."},{"$f":"O320","v":"lane_id"}," IS ",{"$f":"\"'\"&I320&\"'\"","v":"'차로ID'"},";",null,null,null,""]
[null,null,"엣지ID","edge_id",2,"VARCHAR2(300)","FK","NOT NULL","소속 엣지ID",null,null,null,"EQ","소속엣지ID","edge_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,null,null,"edge_id ","VARCHAR(300) ","NOT NULL",",",{"$nulls":5},"edge_id ","VARCHAR2(300) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitslane.","edge_id"," IS ","'소속 엣지ID'",";",null,null,null,""]
[null,null,"차로번호","lane_no",3,"NUMBER(2)",null,"NOT NULL","차로번호",null,null,null,"EQ","차로번호","lane_no","NUMBER(2)","INTEGER","NUMBER(2)",null,null,null,"lane_no ","INTEGER ","NOT NULL",",",{"$nulls":5},"lane_no ","NUMBER(2) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitslane.","lane_no"," IS ","'차로번호'",";",null,null,null,""]
[null,null,"방향구분코드","drct_se_cd",4,"CHAR(1)",null,"NOT NULL","방향구분코드(004)",null,null,"상/하 혹은 좌/우 기준으로 1/2","EQ","방향구분코드","drct_se_cd","CHAR(1)","VARCHAR(1)","CHAR(1)",null,null,null,"drct_se_cd ","VARCHAR(1) ","NOT NULL",",",{"$nulls":5},"drct_se_cd ","CHAR(1) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitslane.","drct_se_cd"," IS ","'방향구분코드(004)'",";",null,null,null,""]
[null,null,"차로길이","lane_lngt",5,"NUMBER(19,9)",null,null,"차로 길이(meter)",null,null,null,"EQ","차로길이","lane_lngt","NUMBER(19,9)","FLOAT","NUMBER(19,9)",null,null,null,"lane_lngt ","FLOAT ","",",",{"$nulls":5},"lane_lngt ","NUMBER(19,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitslane.","lane_lngt"," IS ","'차로 길이(meter)'",";",null,null,null,""]
[null,null,"전용차로구분코드","exus_lane_se_cd",6,"CHAR(2)",null,"NOT NULL","전용차로구분코드(059)","서울소통광장의 버스전용차로구분 참조\n",null,"전용차로구분코드 (AA : 모든차량허용,\nBA : 버스전용차로 - 전일제,\nBB : 버스전용차로 - 시간제,\nBC : 버스전용차로 - 중앙차로(24시간),\nFF : 모든 차량 이동불가)","EQ","전용차로구분코드","exus_lane_se_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",null,null,null,"exus_lane_se_cd ","VARCHAR(2) ","NOT NULL",",",{"$nulls":5},"exus_lane_se_cd ","VARCHAR2(2) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitslane.","exus_lane_se_cd"," IS ","'전용차로구분코드(059)'",";",null,null,null,""]
[null,null,"전용차로A시작시분","exus_lane_A_bgng_hm",7,"CHAR(4)",null,null,"A시작시각(HHmm)","전일제일 경우 A만 이용 (평일 낮주간)\n시간제일 경우 A/B 모두 이용 (평일 오전오후)\n중앙차로는 사용X (24시간제)",null,null,"EQ","전용차로A시작시분","exus_lane_A_bgng_hm","CHAR(4)","VARCHAR(4)","VARCHAR2(4)",null,null,null,"exus_lane_A_bgng_hm ","VARCHAR(4) ","",",",{"$nulls":5},"exus_lane_A_bgng_hm ","VARCHAR2(4) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitslane.","exus_lane_A_bgng_hm"," IS ","'A시작시각(HHmm)'",";",null,null,null,""]
[null,null,"전용차로A종료시분","exus_lane_A_end_hm",8,"CHAR(4)",null,null,"A종료시각(HHmm)",null,null,null,"EQ","전용차로A종료시분","exus_lane_A_end_hm","CHAR(4)","VARCHAR(4)","VARCHAR2(4)",null,null,null,"exus_lane_A_end_hm ","VARCHAR(4) ","",",",{"$nulls":5},"exus_lane_A_end_hm ","VARCHAR2(4) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitslane.","exus_lane_A_end_hm"," IS ","'A종료시각(HHmm)'",";",null,null,null,""]
[null,null,"전용차로B시작시분","exus_lane_B_bgng_hm",9,"CHAR(4)",null,null,"B시작시각(HHmm)",null,null,null,"EQ","전용차로B시작시분","exus_lane_B_bgng_hm","CHAR(4)","VARCHAR(4)","VARCHAR2(4)",null,null,null,"exus_lane_B_bgng_hm ","VARCHAR(4) ","",",",{"$nulls":5},"exus_lane_B_bgng_hm ","VARCHAR2(4) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitslane.","exus_lane_B_bgng_hm"," IS ","'B시작시각(HHmm)'",";",null,null,null,""]
[null,null,"전용차로B종료시분","exus_lane_B_end_hm",10,"CHAR(4)",null,null,"B종료시각(HHmm)",null,null,null,"EQ","전용차로B종료시분","exus_lane_B_end_hm","CHAR(4)","VARCHAR(4)","VARCHAR2(4)",null,null,null,"exus_lane_B_end_hm ","VARCHAR(4) ","",",",{"$nulls":5},"exus_lane_B_end_hm ","VARCHAR2(4) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitslane.","exus_lane_B_end_hm"," IS ","'B종료시각(HHmm)'",";",null,null,null,""]
[null,null,"차로공간정보","lane_spin",11,"VARCHAR2(10000)",null,"NOT NULL","차로공간정보(WKT LineString)",null,null,null,"NEQ)","차로공간정보","lane_spin","BINARY","VARCHAR(2000)","GEOMETRY",{"$nulls":12},"lane_spin ","GEOMETRY ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitslane.","lane_spin"," IS ","'차로공간정보(WKT LineString)'",";",null,null,null,""]
[null,null,"소속세그먼트수","sgmn_cnt",12,"NUMBER(4)",null,null,"소속세그먼트 수","ICT사업본부에서 생성/입력 예정",null,null,null,"소속세그먼트수","sgmn_cnt","NUMBER(4)",null,"NUMBER(4)",{"$nulls":12},"sgmn_cnt ","NUMBER(4) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitslane.","sgmn_cnt"," IS ","'소속세그먼트 수'",";",null,null,null,""]
[{"$nulls":21},{"$f":"CONCATENATE(Z320:AB330)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AI320:AL330)","v":{"$error":"#VALUE!"}},{"$nulls":16},{"$error":"#VALUE!"}]
[{"$nulls":34},"SOIT_D08_M001","SOIT_I08_M001"]
[null,"(메타버스) 차로 테이블",{"$nulls":11},"mtvslane",{"$nulls":33},{"$f":"IF(LEFT(AE334, 13) = \"CONSTRAINT PK\", AE334, \"\")","v":""}]
["18-1","Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N334&\" \"","v":"mtvslane "},null," IS ",{"$f":"\"'\"&B334&\"'\"","v":"'(메타버스) 차로 테이블'"},";",null,null,null,""]
[null,"mtvslane","차로ID","lane_id",1,"VARCHAR2(300)","PK","NOT NULL","차로ID",null,null,null,{"$f":"IF(F336=P336, \"EQ\", \"NEQ)\")","v":"EQ"},"차로ID","lane_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,"CREATE TABLE ",{"$f":"N334&\" (\"","v":"mtvslane ("},{"$f":"O336&\" \"","v":"lane_id "},{"$f":"Q336&\" \"","v":"VARCHAR(300) "},{"$f":"IF(H336=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(G336=\"PK\", G336=\"PK/FK\"), O336, \"\")","v":"lane_id"},"));","CREATE TABLE ",{"$f":"N334&\" (\"","v":"mtvslane ("},{"$f":"O336&\" \"","v":"lane_id "},{"$f":"R336&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(H336=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","CONSTRAINT ",{"$f":"\"PK_\"&N334&\" PRIMARY KEY (\"","v":"PK_mtvslane PRIMARY KEY ("},{"$f":"IF(OR(G336=\"PK\", G336=\"PK/FK\"), O336, \"\")","v":"lane_id"},") using index tablespace SOIT_I08);","COMMENT ON COLUMN ",{"$f":"$N$334&\".\"","v":"mtvslane."},{"$f":"O336","v":"lane_id"}," IS ",{"$f":"\"'\"&I336&\"'\"","v":"'차로ID'"},";",null,null,null,""]
[null,null,"엣지ID","edge_id",2,"VARCHAR2(300)","FK","NOT NULL","소속 엣지ID",null,null,null,"EQ","소속엣지ID","edge_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,null,null,"edge_id ","VARCHAR(300) ","NOT NULL",",",{"$nulls":5},"edge_id ","VARCHAR2(300) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","mtvslane.","edge_id"," IS ","'소속 엣지ID'",";",null,null,null,""]
[null,null,"차로번호","lane_no",3,"NUMBER(2)",null,"NOT NULL","차로번호",null,null,null,"EQ","차로번호","lane_no","NUMBER(2)","INTEGER","NUMBER(2)",null,null,null,"lane_no ","INTEGER ","NOT NULL",",",{"$nulls":5},"lane_no ","NUMBER(2) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","mtvslane.","lane_no"," IS ","'차로번호'",";",null,null,null,""]
[null,null,"방향구분코드","drct_se_cd",4,"CHAR(1)",null,"NOT NULL","방향구분코드(004)",null,null,"상/하 혹은 좌/우 기준으로 1/2","EQ","방향구분코드","drct_se_cd","CHAR(1)","VARCHAR(1)","CHAR(1)",null,null,null,"drct_se_cd ","VARCHAR(1) ","NOT NULL",",",{"$nulls":5},"drct_se_cd ","CHAR(1) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","mtvslane.","drct_se_cd"," IS ","'방향구분코드(004)'",";",null,null,null,""]
[null,null,"차로길이","lane_lngt",5,"NUMBER(19,9)",null,null,"차로 길이(meter)",null,null,null,"EQ","차로길이","lane_lngt","NUMBER(19,9)","FLOAT","NUMBER(19,9)",null,null,null,"lane_lngt ","FLOAT ","",",",{"$nulls":5},"lane_lngt ","NUMBER(19,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","mtvslane.","lane_lngt"," IS ","'차로 길이(meter)'",";",null,null,null,""]
[null,null,"전용차로구분코드","exus_lane_se_cd",6,"CHAR(2)",null,"NOT NULL","전용차로구분코드(059)","서울소통광장의 버스전용차로구분 참조\n",null,"전용차로구분코드 (AA : 모든차량허용,\nBA : 버스전용차로 - 전일제,\nBB : 버스전용차로 - 시간제,\nBC : 버스전용차로 - 중앙차로(24시간),\nFF : 모든 차량 이동불가)","EQ","전용차로구분코드","exus_lane_se_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",null,null,null,"exus_lane_se_cd ","VARCHAR(2) ","NOT NULL",",",{"$nulls":5},"exus_lane_se_cd ","VARCHAR2(2) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","mtvslane.","exus_lane_se_cd"," IS ","'전용차로구분코드(059)'",";",null,null,null,""]
[null,null,"전용차로A시작시분","exus_lane_A_bgng_hm",7,"CHAR(4)",null,null,"A시작시각(HHmm)","전일제일 경우 A만 이용 (평일 낮주간)\n시간제일 경우 A/B 모두 이용 (평일 오전오후)\n중앙차로는 사용X (24시간제)",null,null,"EQ","전용차로A시작시분","exus_lane_A_bgng_hm","CHAR(4)","VARCHAR(4)","VARCHAR2(4)",null,null,null,"exus_lane_A_bgng_hm ","VARCHAR(4) ","",",",{"$nulls":5},"exus_lane_A_bgng_hm ","VARCHAR2(4) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","mtvslane.","exus_lane_A_bgng_hm"," IS ","'A시작시각(HHmm)'",";",null,null,null,""]
[null,null,"전용차로A종료시분","exus_lane_A_end_hm",8,"CHAR(4)",null,null,"A종료시각(HHmm)",null,null,null,"EQ","전용차로A종료시분","exus_lane_A_end_hm","CHAR(4)","VARCHAR(4)","VARCHAR2(4)",null,null,null,"exus_lane_A_end_hm ","VARCHAR(4) ","",",",{"$nulls":5},"exus_lane_A_end_hm ","VARCHAR2(4) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","mtvslane.","exus_lane_A_end_hm"," IS ","'A종료시각(HHmm)'",";",null,null,null,""]
[null,null,"전용차로B시작시분","exus_lane_B_bgng_hm",9,"CHAR(4)",null,null,"B시작시각(HHmm)",null,null,null,"EQ","전용차로B시작시분","exus_lane_B_bgng_hm","CHAR(4)","VARCHAR(4)","VARCHAR2(4)",null,null,null,"exus_lane_B_bgng_hm ","VARCHAR(4) ","",",",{"$nulls":5},"exus_lane_B_bgng_hm ","VARCHAR2(4) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","mtvslane.","exus_lane_B_bgng_hm"," IS ","'B시작시각(HHmm)'",";",null,null,null,""]
[null,null,"전용차로B종료시분","exus_lane_B_end_hm",10,"CHAR(4)",null,null,"B종료시각(HHmm)",null,null,null,"EQ","전용차로B종료시분","exus_lane_B_end_hm","CHAR(4)","VARCHAR(4)","VARCHAR2(4)",null,null,null,"exus_lane_B_end_hm ","VARCHAR(4) ","",",",{"$nulls":5},"exus_lane_B_end_hm ","VARCHAR2(4) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","mtvslane.","exus_lane_B_end_hm"," IS ","'B종료시각(HHmm)'",";",null,null,null,""]
[null,null,"차로공간정보","lane_spin",11,"VARCHAR2(30000)",null,"NOT NULL","차로공간정보(WKT LineString)",null,null,null,"NEQ)","차로공간정보","lane_spin","BINARY","VARCHAR(2000)","GEOMETRY",{"$nulls":12},"lane_spin ","GEOMETRY ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","mtvslane.","lane_spin"," IS ","'차로공간정보(WKT LineString)'",";",null,null,null,""]
[{"$nulls":21},{"$f":"CONCATENATE(Z336:AB346)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AI336:AL346)","v":{"$error":"#VALUE!"}},{"$nulls":16},{"$error":"#VALUE!"}]
[]
[null,"세그먼트 테이블",{"$nulls":11},"soitssgmn",{"$nulls":33},{"$f":"IF(LEFT(AE349, 13) = \"CONSTRAINT PK\", AE349, \"\")","v":""}]
[19,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N349&\" \"","v":"soitssgmn "},null," IS ",{"$f":"\"'\"&B349&\"'\"","v":"'세그먼트 테이블'"},";",null,null,null,""]
[null,"soitssgmn\n(tb_segment)\n(확정)","세그먼트ID","sgmn_id",1,"VARCHAR2(300)","PK","NOT NULL","세그먼트 ID",null,null,null,{"$f":"IF(F351=P351, \"EQ\", \"NEQ)\")","v":"EQ"},"세그먼트ID","sgmn_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,"CREATE TABLE ",{"$f":"N349&\" (\"","v":"soitssgmn ("},{"$f":"O351&\" \"","v":"sgmn_id "},{"$f":"Q351&\" \"","v":"VARCHAR(300) "},{"$f":"IF(H351=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(G351=\"PK\", G351=\"PK/FK\"), O351, \"\")","v":"sgmn_id"},"));","CREATE TABLE ",{"$f":"N349&\" (\"","v":"soitssgmn ("},{"$f":"O351&\" \"","v":"sgmn_id "},{"$f":"R351&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(H351=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","CONSTRAINT ",{"$f":"\"PK_\"&N349&\" PRIMARY KEY (\"","v":"PK_soitssgmn PRIMARY KEY ("},{"$f":"IF(OR(G351=\"PK\", G351=\"PK/FK\"), O351, \"\")","v":"sgmn_id"},{"$f":"\") using index tablespace \" &AJ362& \") TABLESPACE \" &AI362&\";\"","v":") using index tablespace SOIT_I08_M001) TABLESPACE SOIT_D08_M001;"},"COMMENT ON COLUMN ",{"$f":"$N$349&\".\"","v":"soitssgmn."},{"$f":"O351","v":"sgmn_id"}," IS ",{"$f":"\"'\"&I351&\"'\"","v":"'세그먼트 ID'"},";",null,null,null,""]
[null,null,"차로ID","lane_id",2,"VARCHAR2(300)","FK","NOT NULL","소속 차로ID",null,null,null,"EQ","소속차로ID","lane_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,null,null,"lane_id ","VARCHAR(300) ","NOT NULL",",",{"$nulls":5},"lane_id ","VARCHAR2(300) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitssgmn.","lane_id"," IS ","'소속 차로ID'",";",null,null,null,""]
[null,null,"행정구역코드","pbadms_dstt_cd",3,"CHAR(5)","FK",null,"행정구역코드(052)","시작점 기준",null,"\n행정구역코드 (중구:23010, 동구:23020, 연수구:23040, 남동구:23050, \n부평구:23060, 계양구:23070, 서구:23080, 미추홀구:23090)","EQ","행정구역코드","pbadms_dstt_cd","CHAR(5)","VARCHAR(5)","VARCHAR2(5)",null,null,null,"pbadms_dstt_cd ","VARCHAR(5) ","",",",{"$nulls":5},"pbadms_dstt_cd ","VARCHAR2(5) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitssgmn.","pbadms_dstt_cd"," IS ","'행정구역코드(052)'",";",null,null,null,""]
[null,null,"지역분할코드","rgn_prttn_cd",1,"CHAR(2)","FK",null,"지역분할코드(051)",null,null,"지역분할코드 (0 : 메타버스 POC,\n1 : 계양구,\n2 : 남동구_상단,\n3 : 남동구_하단,\n4 : 미추홀구,\n5 : 부평구_상단,\n6 : 부평구_하단,\n7 : 서구+동구,\n8 : 연수구,\n9 : 중구)","EQ","지역분할코드","rgn_prttn_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",null,null,null,"rgn_prttn_cd ","VARCHAR(2) ","",",",{"$nulls":5},"rgn_prttn_cd ","VARCHAR2(2) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitssgmn.","rgn_prttn_cd"," IS ","'지역분할코드(051)'",";",null,null,null,""]
[null,null,"차로구성순서","lane_cnfg_seq",5,"NUMBER(3)",null,"NOT NULL","진입 방향에서 교차로 방향으로 구성순번",null,"진입에서 진출 방향으로 1, 2, 3, ...",null,"EQ","차로구성순서","lane_cnfg_seq","NUMBER(3)","INTEGER","NUMBER(3)",null,null,null,"lane_cnfg_seq ","INTEGER ","NOT NULL",",",{"$nulls":5},"lane_cnfg_seq ","NUMBER(3) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitssgmn.","lane_cnfg_seq"," IS ","'진입 방향에서 교차로 방향으로 구성순번'",";",null,null,null,""]
[null,null,"세그먼트길이","sgmn_lngt",6,"NUMBER(19,9)",null,"NOT NULL","세그먼트 길이(meter)","짜투리는 그대로. / 짜투리 세그먼트 지표는 집계안될수도","세그먼트 기준길이 : 20m\nlane진입 부분은 자투리가 있어서\n길이가 짧을 수 있음",null,"EQ","세그먼트길이","sgmn_lngt","NUMBER(19,9)","FLOAT","NUMBER(19,9)",null,null,null,"sgmn_lngt ","FLOAT ","NOT NULL",",",{"$nulls":5},"sgmn_lngt ","NUMBER(19,9) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitssgmn.","sgmn_lngt"," IS ","'세그먼트 길이(meter)'",";",null,null,null,""]
[null,null,"세그먼트시작거리","sgmn_bgng_dstn",7,"NUMBER(19,9)",null,"NOT NULL","세그먼트 시작지점(m 단위)",null,"lane의 진입 위치 0을 기준으로\n기준에서 몇 미터 떨어져 있는 길이",null,"EQ","세그먼트시작거리","sgmn_bgng_dstn","NUMBER(19,9)","FLOAT","NUMBER(19,9)",null,null,null,"sgmn_bgng_dstn ","FLOAT ","NOT NULL",",",{"$nulls":5},"sgmn_bgng_dstn ","NUMBER(19,9) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitssgmn.","sgmn_bgng_dstn"," IS ","'세그먼트 시작지점(m 단위)'",";",null,null,null,""]
[null,null,"세그먼트종료거리","sgmn_end_dstn",8,"NUMBER(19,9)",null,"NOT NULL","세그먼트 종료지점(m 단위)",null,"위와 동일",null,"EQ","세그먼트종료거리","sgmn_end_dstn","NUMBER(19,9)","FLOAT","NUMBER(19,9)",null,null,null,"sgmn_end_dstn ","FLOAT ","NOT NULL",",",{"$nulls":5},"sgmn_end_dstn ","NUMBER(19,9) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitssgmn.","sgmn_end_dstn"," IS ","'세그먼트 종료지점(m 단위)'",";",null,null,null,""]
[null,null,"세그먼트공간정보","sgmn_spin",9,"VARCHAR2(2000)",null,"NOT NULL","세그먼트 지리정보(WKT LineString)",null,null,null,"NEQ)","세그먼트공간정보","sgmn_spin","BINARY","VARCHAR(2000)","GEOMETRY",{"$nulls":12},"sgmn_spin ","GEOMETRY ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitssgmn.","sgmn_spin"," IS ","'세그먼트 지리정보(WKT LineString)'",";",null,null,null,""]
[null,null,"세그먼트3D공간정보","sgmn_3d_spin",10,"BINARY",null,null,"3D 세그먼트 지리정보","ICT본부에서 가공/입력",null,null,"EQ","세그먼트3D공간정보","sgmn_3d_spin","BINARY","GEOGRAPHY","GEOMETRY",{"$nulls":12},"sgmn_3d_spin ","GEOMETRY ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitssgmn.","sgmn_3d_spin"," IS ","'3D 세그먼트 지리정보'",";",null,null,null,""]
[{"$nulls":21},{"$f":"CONCATENATE(Z351:AB360)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AI351:AL360)","v":{"$error":"#VALUE!"}},{"$nulls":16},{"$error":"#VALUE!"}]
[{"$nulls":34},"SOIT_D08_M001","SOIT_I08_M001"]
[null,"(메타버스) 세그먼트 테이블",{"$nulls":11},"mtvssgmn",{"$nulls":33},{"$f":"IF(LEFT(AE363, 13) = \"CONSTRAINT PK\", AE363, \"\")","v":""}]
["19-1","Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N363&\" \"","v":"mtvssgmn "},null," IS ",{"$f":"\"'\"&B363&\"'\"","v":"'(메타버스) 세그먼트 테이블'"},";",null,null,null,""]
[null,"mtvssgmn","세그먼트ID","sgmn_id",1,"VARCHAR2(300)","PK","NOT NULL","세그먼트 ID",null,null,null,{"$f":"IF(F365=P365, \"EQ\", \"NEQ)\")","v":"EQ"},"세그먼트ID","sgmn_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,"CREATE TABLE ",{"$f":"N363&\" (\"","v":"mtvssgmn ("},{"$f":"O365&\" \"","v":"sgmn_id "},{"$f":"Q365&\" \"","v":"VARCHAR(300) "},{"$f":"IF(H365=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(G365=\"PK\", G365=\"PK/FK\"), O365, \"\")","v":"sgmn_id"},"));","CREATE TABLE ",{"$f":"N363&\" (\"","v":"mtvssgmn ("},{"$f":"O365&\" \"","v":"sgmn_id "},{"$f":"R365&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(H365=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","CONSTRAINT ",{"$f":"\"PK_\"&N363&\" PRIMARY KEY (\"","v":"PK_mtvssgmn PRIMARY KEY ("},{"$f":"IF(OR(G365=\"PK\", G365=\"PK/FK\"), O365, \"\")","v":"sgmn_id"},") using index tablespace SOIT_I08);","COMMENT ON COLUMN ",{"$f":"$N$363&\".\"","v":"mtvssgmn."},{"$f":"O365","v":"sgmn_id"}," IS ",{"$f":"\"'\"&I365&\"'\"","v":"'세그먼트 ID'"},";",null,null,null,""]
[null,null,"차로ID","lane_id",2,"VARCHAR2(300)","FK","NOT NULL","소속 차로ID",null,null,null,"EQ","소속차로ID","lane_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,null,null,"lane_id ","VARCHAR(300) ","NOT NULL",",",{"$nulls":5},"lane_id ","VARCHAR2(300) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","mtvssgmn.","lane_id"," IS ","'소속 차로ID'",";",null,null,null,""]
[null,null,"행정구역코드","pbadms_dstt_cd",3,"CHAR(5)","FK",null,"행정구역코드(052)","시작점 기준",null,"\n행정구역코드 (중구:23010, 동구:23020, 연수구:23040, 남동구:23050, \n부평구:23060, 계양구:23070, 서구:23080, 미추홀구:23090)","EQ","행정구역코드","pbadms_dstt_cd","CHAR(5)","VARCHAR(5)","VARCHAR2(5)",null,null,null,"pbadms_dstt_cd ","VARCHAR(5) ","",",",{"$nulls":5},"pbadms_dstt_cd ","VARCHAR2(5) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","mtvssgmn.","pbadms_dstt_cd"," IS ","'행정구역코드(052)'",";",null,null,null,""]
[null,null,"지역분할코드","rgn_prttn_cd",1,"CHAR(2)","FK",null,"지역분할코드(051)",null,null,"지역분할코드 (0 : 메타버스 POC,\n1 : 계양구,\n2 : 남동구_상단,\n3 : 남동구_하단,\n4 : 미추홀구,\n5 : 부평구_상단,\n6 : 부평구_하단,\n7 : 서구+동구,\n8 : 연수구,\n9 : 중구)","EQ","지역분할코드","rgn_prttn_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",null,null,null,"rgn_prttn_cd ","VARCHAR(2) ","",",",{"$nulls":5},"rgn_prttn_cd ","VARCHAR2(2) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","mtvssgmn.","rgn_prttn_cd"," IS ","'지역분할코드(051)'",";",null,null,null,""]
[null,null,"차로구성순서","lane_cnfg_seq",5,"NUMBER(3)",null,"NOT NULL","진입 방향에서 교차로 방향으로 구성순번",null,"진입에서 진출 방향으로 1, 2, 3, ...",null,"EQ","차로구성순서","lane_cnfg_seq","NUMBER(3)","INTEGER","NUMBER(3)",null,null,null,"lane_cnfg_seq ","INTEGER ","NOT NULL",",",{"$nulls":5},"lane_cnfg_seq ","NUMBER(3) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","mtvssgmn.","lane_cnfg_seq"," IS ","'진입 방향에서 교차로 방향으로 구성순번'",";",null,null,null,""]
[null,null,"세그먼트길이","sgmn_lngt",6,"NUMBER(19,9)",null,"NOT NULL","세그먼트 길이(meter)","짜투리는 그대로. / 짜투리 세그먼트 지표는 집계안될수도","세그먼트 기준길이 : 20m\nlane진입 부분은 자투리가 있어서\n길이가 짧을 수 있음",null,"EQ","세그먼트길이","sgmn_lngt","NUMBER(19,9)","FLOAT","NUMBER(19,9)",null,null,null,"sgmn_lngt ","FLOAT ","NOT NULL",",",{"$nulls":5},"sgmn_lngt ","NUMBER(19,9) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","mtvssgmn.","sgmn_lngt"," IS ","'세그먼트 길이(meter)'",";",null,null,null,""]
[null,null,"세그먼트시작거리","sgmn_bgng_dstn",7,"NUMBER(19,9)",null,"NOT NULL","세그먼트 시작지점(m 단위)",null,"lane의 진입 위치 0을 기준으로\n기준에서 몇 미터 떨어져 있는 길이",null,"EQ","세그먼트시작거리","sgmn_bgng_dstn","NUMBER(19,9)","FLOAT","NUMBER(19,9)",null,null,null,"sgmn_bgng_dstn ","FLOAT ","NOT NULL",",",{"$nulls":5},"sgmn_bgng_dstn ","NUMBER(19,9) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","mtvssgmn.","sgmn_bgng_dstn"," IS ","'세그먼트 시작지점(m 단위)'",";",null,null,null,""]
[null,null,"세그먼트종료거리","sgmn_end_dstn",8,"NUMBER(19,9)",null,"NOT NULL","세그먼트 종료지점(m 단위)",null,"위와 동일",null,"EQ","세그먼트종료거리","sgmn_end_dstn","NUMBER(19,9)","FLOAT","NUMBER(19,9)",null,null,null,"sgmn_end_dstn ","FLOAT ","NOT NULL",",",{"$nulls":5},"sgmn_end_dstn ","NUMBER(19,9) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","mtvssgmn.","sgmn_end_dstn"," IS ","'세그먼트 종료지점(m 단위)'",";",null,null,null,""]
[null,null,"세그먼트공간정보","sgmn_spin",9,"VARCHAR2(2000)",null,"NOT NULL","세그먼트 지리정보(WKT LineString)",null,null,null,"NEQ)","세그먼트공간정보","sgmn_spin","BINARY","VARCHAR(2000)","GEOMETRY",{"$nulls":12},"sgmn_spin ","GEOMETRY ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","mtvssgmn.","sgmn_spin"," IS ","'세그먼트 지리정보(WKT LineString)'",";",null,null,null,""]
[{"$nulls":21},{"$f":"CONCATENATE(Z365:AB373)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AI365:AL373)","v":{"$error":"#VALUE!"}},{"$nulls":16},{"$error":"#VALUE!"}]
[]
[null,"표준노드링크 구성 테이블",{"$nulls":11},"soitsstdlinkcnfg",{"$nulls":33},{"$f":"IF(LEFT(AE376, 13) = \"CONSTRAINT PK\", AE376, \"\")","v":""}]
[20,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N376&\" \"","v":"soitsstdlinkcnfg "},null," IS ",{"$f":"\"'\"&B376&\"'\"","v":"'표준노드링크 구성 테이블'"},";",null,null,null,""]
[null,"soitsstdlinkcnfg\n(tb_link)\n(확정)","표준링크ID","std_link_id",1,"VARCHAR2(10)","PK",null,"표준노드링크ID","노드링크-세그먼트 관계테이블\n세그먼트가 두 링크에 걸치면 둘 다 넣어주세요",null,null,{"$f":"IF(F378=P378, \"EQ\", \"NEQ)\")","v":"EQ"},"표준링크ID","std_link_id","VARCHAR2(10)","VARCHAR(10)","VARCHAR2(10)",null,"CREATE TABLE ",{"$f":"N376&\" (\"","v":"soitsstdlinkcnfg ("},{"$f":"O378&\" \"","v":"std_link_id "},{"$f":"Q378&\" \"","v":"VARCHAR(10) "},{"$f":"IF(H378=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",","PRIMARY KEY (",{"$f":"IF(OR(G378=\"PK\", G378=\"PK/FK\"), O378, \"\")","v":"std_link_id"},",","CREATE TABLE ",{"$f":"N376&\" (\"","v":"soitsstdlinkcnfg ("},{"$f":"O378&\" \"","v":"std_link_id "},{"$f":"R378&\" \"","v":"VARCHAR2(10) "},{"$f":"IF(H378=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",","CONSTRAINT ",{"$f":"\"PK_\"&N376&\" PRIMARY KEY (\"","v":"PK_soitsstdlinkcnfg PRIMARY KEY ("},{"$f":"IF(OR(G378=\"PK\", G378=\"PK/FK\"), O378, \"\")","v":"std_link_id"},",","COMMENT ON COLUMN ",{"$f":"$N$376&\".\"","v":"soitsstdlinkcnfg."},{"$f":"O378","v":"std_link_id"}," IS ",{"$f":"\"'\"&I378&\"'\"","v":"'표준노드링크ID'"},";",null,null,null,""]
[null,null,"세그먼트ID","sgmn_id",2,"VARCHAR2(300)","PK/FK",null,"소속 세그먼트ID",null,null,null,"EQ","소속세그먼트ID","sgmn_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,null,null,"sgmn_id ","VARCHAR(300) ","",",",null,"sgmn_id","));",null,null,"sgmn_id ","VARCHAR2(300) ","",",",null,null,"sgmn_id",{"$f":"\") using index tablespace \" &AJ381& \") TABLESPACE \" &AI381&\";\"","v":") using index tablespace SOIT_I08_M001) TABLESPACE SOIT_D08_M001;"},"COMMENT ON COLUMN ","soitsstdlinkcnfg.","sgmn_id"," IS ","'소속 세그먼트ID'",";",null,null,null,""]
[{"$nulls":21},{"$f":"CONCATENATE(Z378:AB379)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AI378:AL379)","v":{"$error":"#VALUE!"}},{"$nulls":16},{"$error":"#VALUE!"}]
[{"$nulls":34},"SOIT_D08_M001","SOIT_I08_M001"]
[null,"연결차로 스마트카메라정보 테이블",{"$nulls":11},"soitscnctlanesgnlinfo",{"$nulls":33},{"$f":"IF(LEFT(AE382, 13) = \"CONSTRAINT PK\", AE382, \"\")","v":""}]
[22,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N382&\" \"","v":"soitscnctlanesgnlinfo "},null," IS ",{"$f":"\"'\"&B382&\"'\"","v":"'연결차로 스마트카메라정보 테이블'"},";",null,null,null,""]
[null,"soitscnctlanesgnlinfo","노드ID","node_id",1,"VARCHAR2(300)","PK","NOT NULL","소속 교차로 노드ID",null,null,null,{"$f":"IF(F384=P384, \"EQ\", \"NEQ)\")","v":"EQ"},"노드ID","node_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,"CREATE TABLE ",{"$f":"N382&\" (\"","v":"soitscnctlanesgnlinfo ("},{"$f":"O384&\" \"","v":"node_id "},{"$f":"Q384&\" \"","v":"VARCHAR(300) "},{"$f":"IF(H384=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(G384=\"PK\", G384=\"PK/FK\"), O384, \"\")","v":"node_id"},",","CREATE TABLE ",{"$f":"N382&\" (\"","v":"soitscnctlanesgnlinfo ("},{"$f":"O384&\" \"","v":"node_id "},{"$f":"R384&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(H384=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","CONSTRAINT ",{"$f":"\"PK_\"&N382&\" PRIMARY KEY (\"","v":"PK_soitscnctlanesgnlinfo PRIMARY KEY ("},{"$f":"IF(OR(G384=\"PK\", G384=\"PK/FK\"), O384, \"\")","v":"node_id"},",","COMMENT ON COLUMN ",{"$f":"$N$382&\".\"","v":"soitscnctlanesgnlinfo."},{"$f":"O384","v":"node_id"}," IS ",{"$f":"\"'\"&I384&\"'\"","v":"'소속 교차로 노드ID'"},";",null,null,null,""]
[null,null,"현장교차로ID","spot_ints_id",2,"NUMBER(5)",null,null,"현장교차로ID",null,null,null,"EQ","현장교차로ID","spot_ints_id","NUMBER(5)","INTEGER","NUMBER(5)",null,null,null,"spot_ints_id ","INTEGER ","",",",null,"",null,null,null,"spot_ints_id ","NUMBER(5) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitscnctlanesgnlinfo.","spot_ints_id"," IS ","'현장교차로ID'",";",null,null,null,""]
[null,null,"헤드엣지ID","head_edge_id",3,"VARCHAR2(300)",null,null,"헤드엣지ID",{"$nulls":4},"헤드엣지ID","head_edge_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,null,null,"head_edge_id ","VARCHAR(300) ",null,",",{"$nulls":5},"head_edge_id ","VARCHAR2(300) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitscnctlanesgnlinfo.","head_edge_id"," IS ","'헤드엣지ID'",";"]
[null,null,"진입엣지ID","entr_edge_id",4,"VARCHAR2(300)","PK",null,"진입엣지ID",null,null,null,{"$f":"IF(F387=P387, \"EQ\", \"NEQ)\")","v":"EQ"},"진입엣지ID","entr_edge_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,null,null,"entr_edge_id ","VARCHAR(300) ",{"$f":"IF(H387=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",null,{"$f":"IF(OR(G387=\"PK\", G387=\"PK/FK\"), O387, \"\")","v":"entr_edge_id"},",",null,null,"entr_edge_id ","VARCHAR2(300) ","",",",null,null,{"$f":"IF(OR(G387=\"PK\", G387=\"PK/FK\"), O387, \"\")","v":"entr_edge_id"},",","COMMENT ON COLUMN ","soitscnctlanesgnlinfo.","entr_edge_id"," IS ","'진입엣지ID'",";",null,null,null,{"$f":"IF(LEFT(AE387, 13) = \"CONSTRAINT PK\", AE387, \"\")","v":""}]
[null,null,"진출엣지ID","exit_edge_id",5,"VARCHAR2(300)","PK",null,"진출엣지ID",null,null,null,"EQ","진출엣지ID","exit_edge_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,null,null,"exit_edge_id ","VARCHAR(300) ","",",",null,"exit_edge_id",",",null,null,"exit_edge_id ","VARCHAR2(300) ","",",",null,null,"exit_edge_id",",","COMMENT ON COLUMN ","soitscnctlanesgnlinfo.","exit_edge_id"," IS ","'진출엣지ID'",";",null,null,null,""]
[null,null,"회전분류코드","turn_clsf_cd",6,"CHAR(3)","PK",null,"회전코드(700)",null,null,"11:직진,21:작은좌회전,22:큰좌회전,31:작은우회전,32:큰우회전,41:유턴","EQ","회전분류코드","turn_clsf_cd","CHAR(3)","VARCHAR(3)","VARCHAR2(3)",null,null,null,"turn_clsf_cd ","VARCHAR(3) ","",",",null,"turn_clsf_cd","));",null,null,"turn_clsf_cd ","VARCHAR2(3) ","",",",null,null,"turn_clsf_cd",{"$f":"\") using index tablespace \" &AJ392& \") TABLESPACE \" &AI392&\";\"","v":") using index tablespace SOIT_I08_M001) TABLESPACE SOIT_D08_M001;"},"COMMENT ON COLUMN ","soitscnctlanesgnlinfo.","turn_clsf_cd"," IS ","'회전코드(700)'",";",null,null,null,""]
[null,null,"현장카메라ID","spot_camr_id",7,"VARCHAR2(10)",null,null,"글로벌브릿지 스마트교차로 카메라ID",null,null,null,"EQ","현장카메라ID","spot_camr_id","VARCHAR2(10)","VARCHAR(10)","VARCHAR2(10)",null,null,null,"spot_camr_id ","VARCHAR(10) ","",",",null,"",null,null,null,"spot_camr_id ","VARCHAR2(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitscnctlanesgnlinfo.","spot_camr_id"," IS ","'글로벌브릿지 스마트교차로 카메라ID'",";",null,null,null,""]
[{"$nulls":21},{"$f":"CONCATENATE(Z384:AB390)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AI384:AL390)","v":{"$error":"#VALUE!"}},{"$nulls":16},{"$error":"#VALUE!"}]
[{"$nulls":34},"SOIT_D08_M001","SOIT_I08_M001"]
[null,"(메타버스) 연결차로 스마트카메라정보 테이블",{"$nulls":11},"mtvscnctlanesgnlinfo",{"$nulls":33},{"$f":"IF(LEFT(AE393, 13) = \"CONSTRAINT PK\", AE393, \"\")","v":""}]
["22-1","Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N393&\" \"","v":"mtvscnctlanesgnlinfo "},null," IS ",{"$f":"\"'\"&B393&\"'\"","v":"'(메타버스) 연결차로 스마트카메라정보 테이블'"},";",null,null,null,""]
[null,"mtvscnctlanesgnlinfo","노드ID","node_id",1,"VARCHAR2(300)","PK","NOT NULL","소속 교차로 노드ID",null,null,null,{"$f":"IF(F395=P395, \"EQ\", \"NEQ)\")","v":"EQ"},"노드ID","node_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,"CREATE TABLE ",{"$f":"N393&\" (\"","v":"mtvscnctlanesgnlinfo ("},{"$f":"O395&\" \"","v":"node_id "},{"$f":"Q395&\" \"","v":"VARCHAR(300) "},{"$f":"IF(H395=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","PRIMARY KEY (",{"$f":"IF(OR(G395=\"PK\", G395=\"PK/FK\"), O395, \"\")","v":"node_id"},",","CREATE TABLE ",{"$f":"N393&\" (\"","v":"mtvscnctlanesgnlinfo ("},{"$f":"O395&\" \"","v":"node_id "},{"$f":"R395&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(H395=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",","CONSTRAINT ",{"$f":"\"PK_\"&N393&\" PRIMARY KEY (\"","v":"PK_mtvscnctlanesgnlinfo PRIMARY KEY ("},{"$f":"IF(OR(G395=\"PK\", G395=\"PK/FK\"), O395, \"\")","v":"node_id"},",","COMMENT ON COLUMN ",{"$f":"$N$393&\".\"","v":"mtvscnctlanesgnlinfo."},{"$f":"O395","v":"node_id"}," IS ",{"$f":"\"'\"&I395&\"'\"","v":"'소속 교차로 노드ID'"},";",null,null,null,""]
[null,null,"현장교차로ID","spot_ints_id",2,"NUMBER(5)",null,null,"현장교차로ID",null,null,null,"EQ","현장교차로ID","spot_ints_id","NUMBER(5)","INTEGER","NUMBER(5)",null,null,null,"spot_ints_id ","INTEGER ","",",",null,"",null,null,null,"spot_ints_id ","NUMBER(5) ","",",",null,null,"",null,"COMMENT ON COLUMN ","mtvscnctlanesgnlinfo.","spot_ints_id"," IS ","'현장교차로ID'",";",null,null,null,""]
[null,null,"헤드엣지ID","head_edge_id",3,"VARCHAR2(300)",null,null,"헤드엣지ID",{"$nulls":4},"헤드엣지ID","head_edge_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,null,null,"head_edge_id ","VARCHAR(300) ",null,",",{"$nulls":5},"head_edge_id ","VARCHAR2(300) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","mtvscnctlanesgnlinfo.","head_edge_id"," IS ","'헤드엣지ID'",";"]
[null,null,"진입엣지ID","entr_edge_id",4,"VARCHAR2(300)","PK",null,"진입엣지ID",null,null,null,{"$f":"IF(F398=P398, \"EQ\", \"NEQ)\")","v":"EQ"},"진입엣지ID","entr_edge_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,null,null,"entr_edge_id ","VARCHAR(300) ",{"$f":"IF(H398=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",null,{"$f":"IF(OR(G398=\"PK\", G398=\"PK/FK\"), O398, \"\")","v":"entr_edge_id"},",",null,null,"entr_edge_id ","VARCHAR2(300) ","",",",null,null,{"$f":"IF(OR(G398=\"PK\", G398=\"PK/FK\"), O398, \"\")","v":"entr_edge_id"},",","COMMENT ON COLUMN ","mtvscnctlanesgnlinfo.","entr_edge_id"," IS ","'진입엣지ID'",";",null,null,null,{"$f":"IF(LEFT(AE398, 13) = \"CONSTRAINT PK\", AE398, \"\")","v":""}]
[null,null,"진출엣지ID","exit_edge_id",5,"VARCHAR2(300)","PK",null,"진출엣지ID",null,null,null,"EQ","진출엣지ID","exit_edge_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,null,null,"exit_edge_id ","VARCHAR(300) ","",",",null,"exit_edge_id",",",null,null,"exit_edge_id ","VARCHAR2(300) ","",",",null,null,"exit_edge_id",",","COMMENT ON COLUMN ","mtvscnctlanesgnlinfo.","exit_edge_id"," IS ","'진출엣지ID'",";",null,null,null,""]
[null,null,"회전분류코드","turn_clsf_cd",6,"CHAR(2)","PK",null,"회전코드(700)",null,null,"11:직진,21:작은좌회전,22:큰좌회전,31:작은우회전,32:큰우회전,41:유턴","EQ","회전분류코드","turn_clsf_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",null,null,null,"turn_clsf_cd ","VARCHAR(2) ","",",",null,"turn_clsf_cd","));",null,null,"turn_clsf_cd ","VARCHAR2(2) ","",",",null,null,"turn_clsf_cd",") using index tablespace SOIT_I08);","COMMENT ON COLUMN ","mtvscnctlanesgnlinfo.","turn_clsf_cd"," IS ","'회전코드(700)'",";",null,null,null,""]
[null,null,"현장카메라ID","spot_camr_id",7,"VARCHAR2(10)",null,null,"글로벌브릿지 스마트교차로 카메라ID",null,null,null,"EQ","현장카메라ID","spot_camr_id","VARCHAR2(10)","VARCHAR(10)","VARCHAR2(10)",null,null,null,"spot_camr_id ","VARCHAR(10) ","",",",null,"",null,null,null,"spot_camr_id ","VARCHAR2(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","mtvscnctlanesgnlinfo.","spot_camr_id"," IS ","'글로벌브릿지 스마트교차로 카메라ID'",";",null,null,null,""]
[{"$nulls":21},{"$f":"CONCATENATE(Z395:AB401)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AI395:AL401)","v":{"$error":"#VALUE!"}},{"$nulls":16},{"$error":"#VALUE!"}]
[null,"교차로 신호구성정보 테이블",{"$nulls":11},"soitsintssgnlcnfginfo",{"$nulls":33},""]
["25-1","Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","전략본부",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N403&\" \"","v":"soitsintssgnlcnfginfo "},null," IS ",{"$f":"\"'\"&B403&\"'\"","v":"'교차로 신호구성정보 테이블'"},";",null,null,null,""]
[null,"soitsintssgnlcnfginfo\n(tb_spot_ints)\n(확정)","교차로구분코드","ints_se_cd",1,"CHAR(1)",null,null,"교차로구분코드(054)",null,null,"교차로구분코드 (1 : 일반노드\n2 : 신호교차로\n3 : 스마트교차로\n4 : 차선변경노드\n5 : 골목길노드)",{"$f":"IF(F405=P405, \"EQ\", \"NEQ)\")","v":"EQ"},"교차로구분코드","ints_se_cd","CHAR(1)","VARCHAR(1)",null,null,"CREATE TABLE ",{"$f":"N403&\" (\"","v":"soitsintssgnlcnfginfo ("},{"$f":"O405&\" \"","v":"ints_se_cd "},{"$f":"Q405&\" \"","v":"VARCHAR(1) "},{"$f":"IF(H405=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",{"$nulls":13},"COMMENT ON COLUMN ",{"$f":"$N$403&\".\"","v":"soitsintssgnlcnfginfo."},{"$f":"O405","v":"ints_se_cd"}," IS ",{"$f":"\"'\"&I405&\"'\"","v":"'교차로구분코드(054)'"},";",null,null,null,""]
[null,null,"행정구역코드","pbadms_dstt_cd",2,"CHAR(5)",null,null,"행정구역코드(052)",null,null,"행정구역코드 (중구:23010, 동구:23020, 연수구:23040, 남동구:23050, \n부평구:23060, 계양구:23070, 서구:23080, 미추홀구:23090)","EQ","행정구역코드","pbadms_dstt_cd","CHAR(5)","VARCHAR(5)",{"$nulls":4},"pbadms_dstt_cd ","VARCHAR(5) ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfo.","pbadms_dstt_cd"," IS ","'행정구역코드(052)'",";",null,null,null,""]
[null,null,"현장교차로일련번호","spot_ints_sn",3,"NUMBER(4)",null,null,"현장교차로일련번호",null,null,null,"EQ","현장교차로일련번호","spot_ints_sn","NUMBER(4)","INTEGER",{"$nulls":4},"spot_ints_sn ","INTEGER ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfo.","spot_ints_sn"," IS ","'현장교차로일련번호'",";",null,null,null,""]
[null,null,"현장교차로ID","spot_ints_id",4,"NUMBER(5)",null,null,"현장교차로ID",null,null,null,"EQ","현장교차로ID","spot_ints_id","NUMBER(5)","INTEGER",{"$nulls":4},"spot_ints_id ","INTEGER ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfo.","spot_ints_id"," IS ","'현장교차로ID'",";",null,null,null,""]
[null,null,"교차로군ID","ints_grop_id",5,"NUMBER(4)",null,null,"교차로군ID",null,"데이터 형식 변경 - 2022.07.13",null,"NEQ)","교차로군ID","ints_grop_id","NUMBER(5)","INTEGER",{"$nulls":4},"ints_grop_id ","INTEGER ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfo.","ints_grop_id"," IS ","'교차로군ID'",";",null,null,null,""]
[null,null,"교차로명","ints_nm",6,"VARCHAR2(50)",null,null,"교차로명",null,null,null,"EQ","교차로명","ints_nm","VARCHAR2(50)","VARCHAR(50)",{"$nulls":4},"ints_nm ","VARCHAR(50) ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfo.","ints_nm"," IS ","'교차로명'",";",null,null,null,""]
[null,null,"현장교차로유형코드","spot_ints_type_cd",7,"CHAR(1)",null,null,"현장교차로유형코드 (055)",null,"(SUMO 연동그룹구성코드 차용)"," (2 : CI, 3 : SCI, 4 : MI)","EQ","현장교차로유형코드","spot_ints_type_cd","CHAR(1)","VARCHAR(1)",{"$nulls":4},"spot_ints_type_cd ","VARCHAR(1) ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfo.","spot_ints_type_cd"," IS ","'현장교차로유형코드 (055)'",";",null,null,null,""]
[null,null,"주교차로구분코드","majr_ints_se_cd",8,"CHAR(2)",null,null,"주교차로구분코드 (062)",null,null,"주교차로구분 (1:주교차로, 2:연등교차로)","EQ","주교차로구분코드","majr_ints_se_cd","CHAR(2)","VARCHAR(2)",{"$nulls":4},"majr_ints_se_cd ","VARCHAR(2) ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfo.","majr_ints_se_cd"," IS ","'주교차로구분코드 (062)'",";",null,null,null,""]
[null,null,"교차로경도","ints_lot",9,"NUMBER(13,10)",null,null,"교차로경도",null,null,null,"EQ","교차로경도","ints_lot","NUMBER(13,10)","FLOAT",{"$nulls":4},"ints_lot ","FLOAT ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfo.","ints_lot"," IS ","'교차로경도'",";",null,null,null,""]
[null,null,"교차로위도","ints_lat",10,"NUMBER(12,10)",null,null,"교차로위도",null,null,null,"EQ","교차로위도","ints_lat","NUMBER(12,10)","FLOAT",{"$nulls":4},"ints_lat ","FLOAT ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfo.","ints_lat"," IS ","'교차로위도'",";",null,null,null,""]
[null,null,"노드ID","node_id",11,"VARCHAR2(300)",null,null,"교차로 노드ID",null,null,null,"EQ","노드ID","node_id","VARCHAR2(300)","VARCHAR(300)",{"$nulls":4},"node_id ","VARCHAR(300) ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfo.","node_id"," IS ","'교차로 노드ID'",";",null,null,null,""]
[null,null,"진입이동류코드","entr_mvmt_cd",12,"CHAR(2)",null,null,"진입이동류코드 (006)",null,"동인 제공 이동류코드 차용"," (2:동,6:서,8:남,4:북,12:북서,10:남서,16:남동,14:북동)\n1~18","EQ","진입이동류코드","entr_mvmt_cd","CHAR(2)","VARCHAR(2)",{"$nulls":4},"entr_mvmt_cd ","VARCHAR(2) ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfo.","entr_mvmt_cd"," IS ","'진입이동류코드 (006)'",";",null,null,null,""]
[null,null,"진입엣지ID","entr_edge_id",13,"VARCHAR2(300)",null,null,"진입엣지ID",null,null,null,"EQ","진입엣지ID","entr_edge_id","VARCHAR2(300)","VARCHAR(300)",{"$nulls":4},"entr_edge_id ","VARCHAR(300) ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfo.","entr_edge_id"," IS ","'진입엣지ID'",";",null,null,null,""]
[null,null,"진출이동류코드","exit_mvmt_cd",14,"CHAR(2)",null,null,"진출이동류코드 (006)",null,"동인 제공 이동류코드 차용","(2:동,6:서,8:남,4:북,12:북서,10:남서,16:남동,14:북동)","EQ","진출이동류코드","exit_mvmt_cd","CHAR(2)","VARCHAR(2)",{"$nulls":4},"exit_mvmt_cd ","VARCHAR(2) ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfo.","exit_mvmt_cd"," IS ","'진출이동류코드 (006)'",";",null,null,null,""]
[null,null,"진출엣지ID","exit_edge_id",15,"VARCHAR2(300)",null,null,"진출엣지ID",null,null,null,"EQ","진출엣지ID","exit_edge_id","VARCHAR2(300)","VARCHAR(300)",{"$nulls":4},"exit_edge_id ","VARCHAR(300) ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfo.","exit_edge_id"," IS ","'진출엣지ID'",";",null,null,null,""]
[null,null,"회전분류코드","turn_clsf_cd",16,"CHAR(1)",null,null,"회전정보 (005)",null,null,"(s:직진, r:우회전, l:좌회전, u:유턴)","EQ","회전분류코드","turn_clsf_cd","CHAR(1)","VARCHAR(1)",{"$nulls":4},"turn_clsf_cd ","VARCHAR(1) ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfo.","turn_clsf_cd"," IS ","'회전정보 (005)'",";",null,null,null,""]
[null,null,"유턴진입이동류코드","utrn_entr_mvmt_cd",17,"CHAR(2)",null,null,"유턴진입이동류코드 방위 (006)",null,"동인 제공 이동류코드 차용"," (2:동,6:서,8:남,4:북,12:북서,10:남서,16:남동,14:북동)","EQ","유턴진입이동류코드","utrn_entr_mvmt_cd","CHAR(2)","VARCHAR(2)",{"$nulls":4},"utrn_entr_mvmt_cd ","VARCHAR(2) ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfo.","utrn_entr_mvmt_cd"," IS ","'유턴진입이동류코드 방위 (006)'",";",null,null,null,""]
[null,null,"유턴진입엣지ID","utrn_entr_edge_id",18,"VARCHAR2(300)",null,null,"유턴진입엣지ID",null,null,null,"EQ","유턴진입엣지ID","utrn_entr_edge_id","VARCHAR2(300)","VARCHAR(300)",{"$nulls":4},"utrn_entr_edge_id ","VARCHAR(300) ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfo.","utrn_entr_edge_id"," IS ","'유턴진입엣지ID'",";",null,null,null,""]
[null,null,"링구분코드","ring_se_cd",19,"CHAR(1)",null,null,"링구분코드(007)",null,null,"링구분코드 (A/B)","EQ","링구분코드","ring_se_cd","CHAR(1)","VARCHAR(1)",{"$nulls":4},"ring_se_cd ","VARCHAR(1) ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfo.","ring_se_cd"," IS ","'링구분코드(007)'",";",null,null,null,""]
[null,null,"현시번호","phas_no",20,"NUMBER(2)",null,null,"현시번호 (1~8)",null,null,null,"EQ","현시번호","phas_no","NUMBER(2)","INTEGER",{"$nulls":4},"phas_no ","INTEGER ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfo.","phas_no"," IS ","'현시번호 (1~8)'",";",null,null,null,""]
[null,null,"현시제어코드","phas_ctrl_cd",21,"CHAR(1)",null,null,"현시제어코드 (502)","2022.07.12 황인규주임 추가",null," (1:일반, 2:시차)","EQ","현시제어코드","phas_ctrl_cd","CHAR(1)","VARCHAR(1)",{"$nulls":4},"phas_ctrl_cd ","VARCHAR(1) ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfo.","phas_ctrl_cd"," IS ","'현시제어코드 (502)'",";",null,null,null,""]
[null,null,"주도로구분코드","majr_road_se_cd",22,"CHAR(2)",null,null,"주도로구분코드 (063)",null,null,"주도로구분  (10:부도로, 20:주도로)","EQ","주도로구분코드","majr_road_se_cd","CHAR(2)","VARCHAR(2)",{"$nulls":4},"majr_road_se_cd ","VARCHAR(2) ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfo.","majr_road_se_cd"," IS ","'주도로구분코드 (063)'",";",null,null,null,""]
[null,null,"최소녹색시간","min_gren_hr",23,"NUMBER(3)",null,null,"최소녹색시간",null,null,null,"EQ","최소녹색시간","min_gren_hr","NUMBER(3)","INTEGER",{"$nulls":4},"min_gren_hr ","INTEGER ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfo.","min_gren_hr"," IS ","'최소녹색시간'",";",null,null,null,""]
[null,null,"황색시간","yelw_hr",24,"NUMBER(3)",null,null,"황색시간",null,null,null,"EQ","황색시간","yelw_hr","NUMBER(3)","INTEGER",{"$nulls":4},"yelw_hr ","INTEGER ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfo.","yelw_hr"," IS ","'황색시간'",";",null,null,null,""]
[null,null,"적색시간","red_hr",25,"NUMBER(3)",null,null,"적색시간",null,null,null,"EQ","적색시간","red_hr","NUMBER(3)","INTEGER",{"$nulls":4},"red_hr ","INTEGER ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfo.","red_hr"," IS ","'적색시간'",";",null,null,null,""]
[null,null,"횡단보도1엣지ID","crsw_1_edge_id",26,"VARCHAR2(300)",null,null,"횡단보도1엣지ID","횡단보도1소속엣지ID",null,null,"EQ","횡단보도1엣지ID","crsw_1_edge_id","VARCHAR2(300)","VARCHAR(300)",{"$nulls":4},"crsw_1_edge_id ","VARCHAR(300) ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfo.","crsw_1_edge_id"," IS ","'횡단보도1엣지ID'",";",null,null,null,""]
[null,null,"횡단보도1녹색시간","crsw_1_gren_hr",27,"NUMBER(3)",null,null,"횡단보도1녹색시간","횡단보도1녹색시간",null,null,"EQ","횡단보도1녹색시간","crsw_1_gren_hr","NUMBER(3)","INTEGER",{"$nulls":4},"crsw_1_gren_hr ","INTEGER ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfo.","crsw_1_gren_hr"," IS ","'횡단보도1녹색시간'",";",null,null,null,""]
[null,null,"횡단보도2엣지ID","crsw_2_edge_id",28,"VARCHAR2(300)",null,null,"횡단보도2엣지ID","횡단보도2소속엣지ID",null,null,"EQ","횡단보도2엣지ID","crsw_2_edge_id","VARCHAR2(300)","VARCHAR(300)",{"$nulls":4},"crsw_2_edge_id ","VARCHAR(300) ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfo.","crsw_2_edge_id"," IS ","'횡단보도2엣지ID'",";",null,null,null,""]
[null,null,"횡단보도2녹색시간","crsw_2_gren_hr",29,"NUMBER(3)",null,null,"횡단보도2녹색시간","횡단보도2녹색시간",null,null,"EQ","횡단보도2녹색시간","crsw_2_gren_hr","NUMBER(3)","INTEGER",{"$nulls":4},"crsw_2_gren_hr ","INTEGER ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfo.","crsw_2_gren_hr"," IS ","'횡단보도2녹색시간'",";",null,null,null,""]
[null,null,"횡단보도3엣지ID","crsw_3_edge_id",30,"VARCHAR2(300)",null,null,"횡단보도3엣지ID","횡단보도3소속엣지ID",null,null,"EQ","횡단보도3엣지ID","crsw_3_edge_id","VARCHAR2(300)","VARCHAR(300)",{"$nulls":4},"crsw_3_edge_id ","VARCHAR(300) ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfo.","crsw_3_edge_id"," IS ","'횡단보도3엣지ID'",";",null,null,null,""]
[null,null,"횡단보도3녹색시간","crsw_3_gren_hr",31,"NUMBER(3)",null,null,"횡단보도3녹색시간","횡단보도3녹색시간",null,null,"EQ","횡단보도3녹색시간","crsw_3_gren_hr","NUMBER(3)","INTEGER",{"$nulls":4},"crsw_3_gren_hr ","INTEGER ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfo.","crsw_3_gren_hr"," IS ","'횡단보도3녹색시간'",";",null,null,null,""]
[null,null,"횡단보도4엣지ID","crsw_4_edge_id",32,"VARCHAR2(300)",null,null,"횡단보도4엣지ID","횡단보도4소속엣지ID",null,null,"EQ","횡단보도4엣지ID","crsw_4_edge_id","VARCHAR2(300)","VARCHAR(300)",{"$nulls":4},"crsw_4_edge_id ","VARCHAR(300) ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfo.","crsw_4_edge_id"," IS ","'횡단보도4엣지ID'",";",null,null,null,""]
[null,null,"횡단보도4녹색시간","crsw_4_gren_hr",33,"NUMBER(3)",null,null,"횡단보도4녹색시간","횡단보도4녹색시간",null,null,"EQ","횡단보도4녹색시간","crsw_4_gren_hr","NUMBER(3)","INTEGER",{"$nulls":4},"crsw_4_gren_hr ","INTEGER ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfo.","crsw_4_gren_hr"," IS ","'횡단보도4녹색시간'",";",null,null,null,""]
[null,null,"횡단보도5엣지ID","crsw_5_edge_id",34,"VARCHAR2(300)",null,null,"횡단보도5엣지ID","횡단보도5소속엣지ID",null,null,"EQ","횡단보도5엣지ID","crsw_5_edge_id","VARCHAR2(300)","VARCHAR(300)",{"$nulls":4},"crsw_5_edge_id ","VARCHAR(300) ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfo.","crsw_5_edge_id"," IS ","'횡단보도5엣지ID'",";",null,null,null,""]
[null,null,"횡단보도5녹색시간","crsw_5_gren_hr",35,"NUMBER(3)",null,null,"횡단보도5녹색시간","횡단보도5녹색시간",null,null,"EQ","횡단보도5녹색시간","crsw_5_gren_hr","NUMBER(3)","INTEGER",{"$nulls":4},"crsw_5_gren_hr ","INTEGER ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfo.","crsw_5_gren_hr"," IS ","'횡단보도5녹색시간'",";",null,null,null,""]
[null,null,"신호등경도","sglg_lot",36,"NUMBER(13,10)",null,null,"신호등경도",null,null,null,"EQ","신호등경도","sglg_lot","NUMBER(13,10)","FLOAT",{"$nulls":4},"sglg_lot ","FLOAT ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfo.","sglg_lot"," IS ","'신호등경도'",";",null,null,null,""]
[null,null,"신호등위도","sglg_lat",37,"NUMBER(12,10)",null,null,"신호등위도",null,null,null,"EQ","신호등위도","sglg_lat","NUMBER(12,10)","FLOAT",{"$nulls":4},"sglg_lat ","FLOAT ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfo.","sglg_lat"," IS ","'신호등위도'",";",null,null,null,""]
[null,null,"현장카메라ID","spot_camr_id",38,"VARCHAR2(10)",null,null,"글로벌브릿지 스마트교차로 카메라ID",{"$nulls":4},"현장카메라ID","spot_camr_id","VARCHAR2(10)","VARCHAR(10)",{"$nulls":4},"spot_camr_id ","VARCHAR(10) ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfo.","spot_camr_id"," IS ","'글로벌브릿지 스마트교차로 카메라ID'",";"]
[null,null,"비고","rmrk",39,"VARCHAR2(200)",null,null,"시차제정보 비고",null,null,null,{"$f":"IF(F443=P443, \"EQ\", \"NEQ)\")","v":"EQ"},"비고","rmrk","VARCHAR2(200)","VARCHAR(200)",{"$nulls":4},"rmrk ","VARCHAR(200) ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfo.","rmrk"," IS ","'시차제정보 비고'",";",null,null,null,{"$f":"IF(LEFT(AE443, 13) = \"CONSTRAINT PK\", AE443, \"\")","v":""}]
[{"$nulls":21},{"$f":"CONCATENATE(Z405:AB443)","v":{"$error":"#VALUE!"}},{"$nulls":25},""]
[null,"교차로 신호구성정보(시차제) 테이블",{"$nulls":11},"soitsintssgnlcnfginfotmdiff",{"$nulls":33},""]
["25-2","Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","전략본부",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N445&\" \"","v":"soitsintssgnlcnfginfotmdiff "},null," IS ",{"$f":"\"'\"&B445&\"'\"","v":"'교차로 신호구성정보(시차제) 테이블'"},";",null,null,null,""]
[null,"soitsintssgnlcnfginfotmdiff\n(tb_spot_ints)\n(확정)\n(시차제)","교차로구분코드","ints_se_cd",1,"CHAR(1)",null,null,"교차로구분코드(054)",null,null,"교차로구분코드 (1 : 일반노드\n2 : 신호교차로\n3 : 스마트교차로\n4 : 차선변경노드\n5 : 골목길노드)",{"$f":"IF(F447=P447, \"EQ\", \"NEQ)\")","v":"EQ"},"교차로구분코드","ints_se_cd","CHAR(1)","VARCHAR(1)",null,null,"CREATE TABLE ",{"$f":"N445&\" (\"","v":"soitsintssgnlcnfginfotmdiff ("},{"$f":"O447&\" \"","v":"ints_se_cd "},{"$f":"Q447&\" \"","v":"VARCHAR(1) "},{"$f":"IF(H447=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",","PRIMARY KEY (",{"$f":"IF(OR(G447=\"PK\", G447=\"PK/FK\"), O447, \"\")","v":""},{"$nulls":11},"COMMENT ON COLUMN ",{"$f":"$N$445&\".\"","v":"soitsintssgnlcnfginfotmdiff."},{"$f":"O447","v":"ints_se_cd"}," IS ",{"$f":"\"'\"&I447&\"'\"","v":"'교차로구분코드(054)'"},";",null,null,null,""]
[null,null,"행정구역코드","pbadms_dstt_cd",2,"CHAR(5)",null,null,"행정구역코드(052)",null,null,"행정구역코드 (중구:23010, 동구:23020, 연수구:23040, 남동구:23050, \n부평구:23060, 계양구:23070, 서구:23080, 미추홀구:23090)","EQ","행정구역코드","pbadms_dstt_cd","CHAR(5)","VARCHAR(5)",{"$nulls":4},"pbadms_dstt_cd ","VARCHAR(5) ","",",",null,"",{"$nulls":11},"COMMENT ON COLUMN ","soitsintssgnlcnfginfotmdiff.","pbadms_dstt_cd"," IS ","'행정구역코드(052)'",";",null,null,null,""]
[null,null,"현장교차로일련번호","spot_ints_sn",3,"NUMBER(4)",null,null,"현장교차로일련번호",null,null,null,"EQ","현장교차로일련번호","spot_ints_sn","NUMBER(4)","INTEGER",{"$nulls":4},"spot_ints_sn ","INTEGER ","",",",null,"",{"$nulls":11},"COMMENT ON COLUMN ","soitsintssgnlcnfginfotmdiff.","spot_ints_sn"," IS ","'현장교차로일련번호'",";",null,null,null,""]
[null,null,"현장교차로ID","spot_ints_id",4,"NUMBER(5)",null,null,"현장교차로ID",null,null,null,"EQ","현장교차로ID","spot_ints_id","NUMBER(5)","INTEGER",{"$nulls":4},"spot_ints_id ","INTEGER ","",",",null,"",",",{"$nulls":10},"COMMENT ON COLUMN ","soitsintssgnlcnfginfotmdiff.","spot_ints_id"," IS ","'현장교차로ID'",";",null,null,null,""]
[null,null,"교차로군ID","ints_grop_id",5,"NUMBER(4)",null,null,"교차로군ID",null,"데이터 형식 변경 - 2022.07.13",null,"NEQ)","교차로군ID","ints_grop_id","NUMBER(5)","INTEGER",{"$nulls":4},"ints_grop_id ","INTEGER ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfotmdiff.","ints_grop_id"," IS ","'교차로군ID'",";",null,null,null,""]
[null,null,"교차로명","ints_nm",6,"VARCHAR2(50)",null,null,"교차로명",null,null,null,"EQ","교차로명","ints_nm","VARCHAR2(50)","VARCHAR(50)",{"$nulls":4},"ints_nm ","VARCHAR(50) ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfotmdiff.","ints_nm"," IS ","'교차로명'",";",null,null,null,""]
[null,null,"현장교차로유형코드","spot_ints_type_cd",7,"CHAR(1)",null,null,"현장교차로유형코드 (055)",null,"(SUMO 연동그룹구성코드 차용)"," (2 : CI, 3 : SCI, 4 : MI)","EQ","현장교차로유형코드","spot_ints_type_cd","CHAR(1)","VARCHAR(1)",{"$nulls":4},"spot_ints_type_cd ","VARCHAR(1) ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfotmdiff.","spot_ints_type_cd"," IS ","'현장교차로유형코드 (055)'",";",null,null,null,""]
[null,null,"주교차로구분코드","majr_ints_se_cd",8,"CHAR(2)",null,null,"주교차로구분코드 (062)",null,null,"주교차로구분 (1:주교차로, 2:연등교차로)","EQ","주교차로구분코드","majr_ints_se_cd","CHAR(2)","VARCHAR(2)",{"$nulls":4},"majr_ints_se_cd ","VARCHAR(2) ","",",",null,{"$f":"IF(OR(G454=\"PK\", G454=\"PK/FK\"), O454, \"\")","v":""},",",{"$nulls":10},"COMMENT ON COLUMN ","soitsintssgnlcnfginfotmdiff.","majr_ints_se_cd"," IS ","'주교차로구분코드 (062)'",";",null,null,null,""]
[null,null,"교차로경도","ints_lot",9,"NUMBER(13,10)",null,null,"교차로경도",null,null,null,"EQ","교차로경도","ints_lot","NUMBER(13,10)","FLOAT",{"$nulls":4},"ints_lot ","FLOAT ","",",",null,"",{"$nulls":11},"COMMENT ON COLUMN ","soitsintssgnlcnfginfotmdiff.","ints_lot"," IS ","'교차로경도'",";",null,null,null,""]
[null,null,"교차로위도","ints_lat",10,"NUMBER(12,10)",null,null,"교차로위도",null,null,null,"EQ","교차로위도","ints_lat","NUMBER(12,10)","FLOAT",{"$nulls":4},"ints_lat ","FLOAT ","",",",null,"",{"$nulls":11},"COMMENT ON COLUMN ","soitsintssgnlcnfginfotmdiff.","ints_lat"," IS ","'교차로위도'",";",null,null,null,""]
[null,null,"노드ID","node_id",11,"VARCHAR2(300)",null,null,"교차로 노드ID",null,null,null,"EQ","노드ID","node_id","VARCHAR2(300)","VARCHAR(300)",{"$nulls":4},"node_id ","VARCHAR(300) ","",",",null,"",",",{"$nulls":10},"COMMENT ON COLUMN ","soitsintssgnlcnfginfotmdiff.","node_id"," IS ","'교차로 노드ID'",";",null,null,null,""]
[null,null,"진입이동류코드","entr_mvmt_cd",12,"CHAR(2)",null,null,"진입이동류코드 (006)",null,"동인 제공 이동류코드 차용"," (2:동,6:서,8:남,4:북,12:북서,10:남서,16:남동,14:북동)\n1~18","EQ","진입이동류코드","entr_mvmt_cd","CHAR(2)","VARCHAR(2)",{"$nulls":4},"entr_mvmt_cd ","VARCHAR(2) ","",",",null,"",{"$nulls":11},"COMMENT ON COLUMN ","soitsintssgnlcnfginfotmdiff.","entr_mvmt_cd"," IS ","'진입이동류코드 (006)'",";",null,null,null,""]
[null,null,"진입엣지ID","entr_edge_id",13,"VARCHAR2(300)",null,null,"진입엣지ID",null,null,null,"EQ","진입엣지ID","entr_edge_id","VARCHAR2(300)","VARCHAR(300)",{"$nulls":4},"entr_edge_id ","VARCHAR(300) ","",",",null,"",{"$nulls":11},"COMMENT ON COLUMN ","soitsintssgnlcnfginfotmdiff.","entr_edge_id"," IS ","'진입엣지ID'",";",null,null,null,""]
[null,null,"진출이동류코드","exit_mvmt_cd",14,"CHAR(2)",null,null,"진출이동류코드 (006)",null,"동인 제공 이동류코드 차용","(2:동,6:서,8:남,4:북,12:북서,10:남서,16:남동,14:북동)","EQ","진출이동류코드","exit_mvmt_cd","CHAR(2)","VARCHAR(2)",{"$nulls":4},"exit_mvmt_cd ","VARCHAR(2) ","",",",null,"",{"$nulls":11},"COMMENT ON COLUMN ","soitsintssgnlcnfginfotmdiff.","exit_mvmt_cd"," IS ","'진출이동류코드 (006)'",";",null,null,null,""]
[null,null,"진출엣지ID","exit_edge_id",15,"VARCHAR2(300)",null,null,"진출엣지ID",null,null,null,"EQ","진출엣지ID","exit_edge_id","VARCHAR2(300)","VARCHAR(300)",{"$nulls":4},"exit_edge_id ","VARCHAR(300) ","",",",null,"",{"$nulls":11},"COMMENT ON COLUMN ","soitsintssgnlcnfginfotmdiff.","exit_edge_id"," IS ","'진출엣지ID'",";",null,null,null,""]
[null,null,"회전분류코드","turn_clsf_cd",16,"CHAR(1)",null,null,"회전정보 (005)",null,null,"(s:직진, r:우회전, l:좌회전, u:유턴)","EQ","회전분류코드","turn_clsf_cd","CHAR(1)","VARCHAR(1)",{"$nulls":4},"turn_clsf_cd ","VARCHAR(1) ","",",",null,"",{"$nulls":11},"COMMENT ON COLUMN ","soitsintssgnlcnfginfotmdiff.","turn_clsf_cd"," IS ","'회전정보 (005)'",";",null,null,null,""]
[null,null,"유턴진입이동류코드","utrn_entr_mvmt_cd",17,"CHAR(2)",null,null,"유턴진입이동류코드 방위 (006)",null,"동인 제공 이동류코드 차용"," (2:동,6:서,8:남,4:북,12:북서,10:남서,16:남동,14:북동)","EQ","유턴진입이동류코드","utrn_entr_mvmt_cd","CHAR(2)","VARCHAR(2)",{"$nulls":4},"utrn_entr_mvmt_cd ","VARCHAR(2) ","",",",null,"",{"$nulls":11},"COMMENT ON COLUMN ","soitsintssgnlcnfginfotmdiff.","utrn_entr_mvmt_cd"," IS ","'유턴진입이동류코드 방위 (006)'",";",null,null,null,""]
[null,null,"유턴진입엣지ID","utrn_entr_edge_id",18,"VARCHAR2(300)",null,null,"유턴진입엣지ID",null,null,null,"EQ","유턴진입엣지ID","utrn_entr_edge_id","VARCHAR2(300)","VARCHAR(300)",{"$nulls":4},"utrn_entr_edge_id ","VARCHAR(300) ","",",",null,"",{"$nulls":11},"COMMENT ON COLUMN ","soitsintssgnlcnfginfotmdiff.","utrn_entr_edge_id"," IS ","'유턴진입엣지ID'",";",null,null,null,""]
[null,null,"링구분코드","ring_se_cd",19,"CHAR(1)",null,null,"링구분코드(007)",null,null,"링구분코드 (A/B)","EQ","링구분코드","ring_se_cd","CHAR(1)","VARCHAR(1)",{"$nulls":4},"ring_se_cd ","VARCHAR(1) ","",",",null,"",",",{"$nulls":10},"COMMENT ON COLUMN ","soitsintssgnlcnfginfotmdiff.","ring_se_cd"," IS ","'링구분코드(007)'",";",null,null,null,""]
[null,null,"현시번호","phas_no",20,"NUMBER(2)",null,null,"현시번호 (1~8)",null,null,null,"EQ","현시번호","phas_no","NUMBER(2)","INTEGER",{"$nulls":4},"phas_no ","INTEGER ","",",",null,"",",",{"$nulls":10},"COMMENT ON COLUMN ","soitsintssgnlcnfginfotmdiff.","phas_no"," IS ","'현시번호 (1~8)'",";",null,null,null,""]
[null,null,"현시제어코드","phas_ctrl_cd",21,"CHAR(1)",null,null,"현시제어코드 (502)","2022.07.12 황인규주임 추가",null," (1:일반, 2:시차)","EQ","현시제어코드","phas_ctrl_cd","CHAR(1)","VARCHAR(1)",{"$nulls":4},"phas_ctrl_cd ","VARCHAR(1) ","",",",null,"","));",{"$nulls":10},"COMMENT ON COLUMN ","soitsintssgnlcnfginfotmdiff.","phas_ctrl_cd"," IS ","'현시제어코드 (502)'",";",null,null,null,""]
[null,null,"주도로구분코드","majr_road_se_cd",22,"CHAR(2)",null,null,"주도로구분코드 (063)",null,null,"주도로구분  (10:부도로, 20:주도로)","EQ","주도로구분코드","majr_road_se_cd","CHAR(2)","VARCHAR(2)",{"$nulls":4},"majr_road_se_cd ","VARCHAR(2) ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfotmdiff.","majr_road_se_cd"," IS ","'주도로구분코드 (063)'",";",null,null,null,""]
[null,null,"최소녹색시간","min_gren_hr",23,"NUMBER(3)",null,null,"최소녹색시간",null,null,null,"EQ","최소녹색시간","min_gren_hr","NUMBER(3)","INTEGER",{"$nulls":4},"min_gren_hr ","INTEGER ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfotmdiff.","min_gren_hr"," IS ","'최소녹색시간'",";",null,null,null,""]
[null,null,"황색시간","yelw_hr",24,"NUMBER(3)",null,null,"황색시간",null,null,null,"EQ","황색시간","yelw_hr","NUMBER(3)","INTEGER",{"$nulls":4},"yelw_hr ","INTEGER ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfotmdiff.","yelw_hr"," IS ","'황색시간'",";",null,null,null,""]
[null,null,"적색시간","red_hr",25,"NUMBER(3)",null,null,"적색시간",null,null,null,"EQ","적색시간","red_hr","NUMBER(3)","INTEGER",{"$nulls":4},"red_hr ","INTEGER ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfotmdiff.","red_hr"," IS ","'적색시간'",";",null,null,null,""]
[null,null,"횡단보도1엣지ID","crsw_1_edge_id",26,"VARCHAR2(300)",null,null,"횡단보도1엣지ID","횡단보도1소속엣지ID",null,null,"EQ","횡단보도1엣지ID","crsw_1_edge_id","VARCHAR2(300)","VARCHAR(300)",{"$nulls":4},"crsw_1_edge_id ","VARCHAR(300) ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfotmdiff.","crsw_1_edge_id"," IS ","'횡단보도1엣지ID'",";",null,null,null,""]
[null,null,"횡단보도1녹색시간","crsw_1_gren_hr",27,"NUMBER(3)",null,null,"횡단보도1녹색시간","횡단보도1녹색시간",null,null,"EQ","횡단보도1녹색시간","crsw_1_gren_hr","NUMBER(3)","INTEGER",{"$nulls":4},"crsw_1_gren_hr ","INTEGER ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfotmdiff.","crsw_1_gren_hr"," IS ","'횡단보도1녹색시간'",";",null,null,null,""]
[null,null,"횡단보도2엣지ID","crsw_2_edge_id",28,"VARCHAR2(300)",null,null,"횡단보도2엣지ID","횡단보도2소속엣지ID",null,null,"EQ","횡단보도2엣지ID","crsw_2_edge_id","VARCHAR2(300)","VARCHAR(300)",{"$nulls":4},"crsw_2_edge_id ","VARCHAR(300) ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfotmdiff.","crsw_2_edge_id"," IS ","'횡단보도2엣지ID'",";",null,null,null,""]
[null,null,"횡단보도2녹색시간","crsw_2_gren_hr",29,"NUMBER(3)",null,null,"횡단보도2녹색시간","횡단보도2녹색시간",null,null,"EQ","횡단보도2녹색시간","crsw_2_gren_hr","NUMBER(3)","INTEGER",{"$nulls":4},"crsw_2_gren_hr ","INTEGER ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfotmdiff.","crsw_2_gren_hr"," IS ","'횡단보도2녹색시간'",";",null,null,null,""]
[null,null,"횡단보도3엣지ID","crsw_3_edge_id",30,"VARCHAR2(300)",null,null,"횡단보도3엣지ID","횡단보도3소속엣지ID",null,null,"EQ","횡단보도3엣지ID","crsw_3_edge_id","VARCHAR2(300)","VARCHAR(300)",{"$nulls":4},"crsw_3_edge_id ","VARCHAR(300) ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfotmdiff.","crsw_3_edge_id"," IS ","'횡단보도3엣지ID'",";",null,null,null,""]
[null,null,"횡단보도3녹색시간","crsw_3_gren_hr",31,"NUMBER(3)",null,null,"횡단보도3녹색시간","횡단보도3녹색시간",null,null,"EQ","횡단보도3녹색시간","crsw_3_gren_hr","NUMBER(3)","INTEGER",{"$nulls":4},"crsw_3_gren_hr ","INTEGER ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfotmdiff.","crsw_3_gren_hr"," IS ","'횡단보도3녹색시간'",";",null,null,null,""]
[null,null,"횡단보도4엣지ID","crsw_4_edge_id",32,"VARCHAR2(300)",null,null,"횡단보도4엣지ID","횡단보도4소속엣지ID",null,null,"EQ","횡단보도4엣지ID","crsw_4_edge_id","VARCHAR2(300)","VARCHAR(300)",{"$nulls":4},"crsw_4_edge_id ","VARCHAR(300) ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfotmdiff.","crsw_4_edge_id"," IS ","'횡단보도4엣지ID'",";",null,null,null,""]
[null,null,"횡단보도4녹색시간","crsw_4_gren_hr",33,"NUMBER(3)",null,null,"횡단보도4녹색시간","횡단보도4녹색시간",null,null,"EQ","횡단보도4녹색시간","crsw_4_gren_hr","NUMBER(3)","INTEGER",{"$nulls":4},"crsw_4_gren_hr ","INTEGER ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfotmdiff.","crsw_4_gren_hr"," IS ","'횡단보도4녹색시간'",";",null,null,null,""]
[null,null,"횡단보도5엣지ID","crsw_5_edge_id",34,"VARCHAR2(300)",null,null,"횡단보도5엣지ID","횡단보도5소속엣지ID",null,null,"EQ","횡단보도5엣지ID","crsw_5_edge_id","VARCHAR2(300)","VARCHAR(300)",{"$nulls":4},"crsw_5_edge_id ","VARCHAR(300) ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfotmdiff.","crsw_5_edge_id"," IS ","'횡단보도5엣지ID'",";",null,null,null,""]
[null,null,"횡단보도5녹색시간","crsw_5_gren_hr",35,"NUMBER(3)",null,null,"횡단보도5녹색시간","횡단보도5녹색시간",null,null,"EQ","횡단보도5녹색시간","crsw_5_gren_hr","NUMBER(3)","INTEGER",{"$nulls":4},"crsw_5_gren_hr ","INTEGER ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfotmdiff.","crsw_5_gren_hr"," IS ","'횡단보도5녹색시간'",";",null,null,null,""]
[null,null,"신호등경도","sglg_lot",36,"NUMBER(13,10)",null,null,"신호등경도",null,null,null,"EQ","신호등경도","sglg_lot","NUMBER(13,10)","FLOAT",{"$nulls":4},"sglg_lot ","FLOAT ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfotmdiff.","sglg_lot"," IS ","'신호등경도'",";",null,null,null,""]
[null,null,"신호등위도","sglg_lat",37,"NUMBER(12,10)",null,null,"신호등위도",null,null,null,"EQ","신호등위도","sglg_lat","NUMBER(12,10)","FLOAT",{"$nulls":4},"sglg_lat ","FLOAT ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfotmdiff.","sglg_lat"," IS ","'신호등위도'",";",null,null,null,""]
[null,null,"현장카메라ID","spot_camr_id",38,"VARCHAR2(10)",null,null,"글로벌브릿지 스마트교차로 카메라ID",{"$nulls":4},"현장카메라ID","spot_camr_id","VARCHAR2(10)","VARCHAR(10)",{"$nulls":4},"spot_camr_id ","VARCHAR(10) ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfotmdiff.","spot_camr_id"," IS ","'글로벌브릿지 스마트교차로 카메라ID'",";"]
[null,null,"비고","rmrk",39,"VARCHAR2(200)",null,null,"시차제정보 비고",null,null,null,{"$f":"IF(F485=P485, \"EQ\", \"NEQ)\")","v":"EQ"},"비고","rmrk","VARCHAR2(200)","VARCHAR(200)",{"$nulls":4},"rmrk ","VARCHAR(200) ","",",",{"$nulls":13},"COMMENT ON COLUMN ","soitsintssgnlcnfginfotmdiff.","rmrk"," IS ","'시차제정보 비고'",";",null,null,null,{"$f":"IF(LEFT(AE485, 13) = \"CONSTRAINT PK\", AE485, \"\")","v":""}]
[{"$nulls":21},{"$f":"CONCATENATE(Z447:AB485)","v":{"$error":"#VALUE!"}},{"$nulls":25},""]
[null,"(메타버스) 실시간 신호변경이력 테이블",{"$nulls":11},"mtvsrltmsgnlchghstr",{"$nulls":33},""]
["26-1","Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N487&\" \"","v":"mtvsrltmsgnlchghstr "},null," IS ",{"$f":"\"'\"&B487&\"'\"","v":"'(메타버스) 실시간 신호변경이력 테이블'"},";",null,null,null,""]
["TIBERO","mtvsrltmsgnlchghstr","수집유닉스시각","clct_unix_tm",1,"NUMBER(10)","PK",null,"동인 신호이력수집시각",null,null,null,{"$f":"IF(F489=P489, \"EQ\", \"NEQ)\")","v":"EQ"},"수집유닉스시각","clct_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",null,"CREATE TABLE ",{"$f":"N487&\" (\"","v":"mtvsrltmsgnlchghstr ("},{"$f":"O489&\" \"","v":"clct_unix_tm "},{"$f":"Q489&\" \"","v":"INTEGER "},{"$f":"IF(H489=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",","PRIMARY KEY (",{"$f":"IF(OR(G489=\"PK\", G489=\"PK/FK\"), O489, \"\")","v":"clct_unix_tm"},",","CREATE TABLE ",{"$f":"N487&\" (\"","v":"mtvsrltmsgnlchghstr ("},{"$f":"O489&\" \"","v":"clct_unix_tm "},{"$f":"R489&\" \"","v":"NUMBER(10) "},{"$f":"IF(H489=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",null,"(",{"$f":"IF(OR(G489=\"PK\", G489=\"PK/FK\"), O489, \"\")","v":"clct_unix_tm"},",","COMMENT ON COLUMN ",{"$f":"$N$487&\".\"","v":"mtvsrltmsgnlchghstr."},{"$f":"O489","v":"clct_unix_tm"}," IS ",{"$f":"\"'\"&I489&\"'\"","v":"'동인 신호이력수집시각'"},";",null,null,null,""]
[null,null,"시작유닉스시각","bgng_unix_tm",2,"NUMBER(10)","PK",null,"신호 시작시각(현시)",null,null,null,"EQ","시작유닉스시각","bgng_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",null,null,null,"bgng_unix_tm ","INTEGER ","",",",null,"bgng_unix_tm",",",null,null,"bgng_unix_tm ","NUMBER(10) ","",",",null,null,"bgng_unix_tm",",","COMMENT ON COLUMN ","mtvsrltmsgnlchghstr.","bgng_unix_tm"," IS ","'신호 시작시각(현시)'",";",null,null,null,""]
[null,null,"현시시작시간","phas_bgng_unix_tm",3,"NUMBER(10)","PK",null,"신호 시작시각(현시)",null,null,null,"EQ","현시시작시간","phas_bgng_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",null,null,null,"phas_bgng_unix_tm ","INTEGER ","",",",null,"phas_bgng_unix_tm",",",null,null,"phas_bgng_unix_tm ","NUMBER(10) ","",",",null,null,"phas_bgng_unix_tm",",","COMMENT ON COLUMN ","mtvsrltmsgnlchghstr.","phas_bgng_unix_tm"," IS ","'신호 시작시각(현시)'",";",null,null,null,""]
[null,null,"실측여부","acsr_yn",4,"CHAR(1)","PK",null,"실측여부 (500)",null,null,"실측여부 (Y/N)","EQ","실측여부","acsr_yn","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",null,null,null,"acsr_yn ","VARCHAR(1) ","",",",null,"acsr_yn",",",null,null,"acsr_yn ","VARCHAR2(1) ","",",",null,null,"acsr_yn",",","COMMENT ON COLUMN ","mtvsrltmsgnlchghstr.","acsr_yn"," IS ","'실측여부 (500)'",";",null,null,null,""]
[null,null,"현장교차로ID","spot_ints_id",5,"NUMBER(5)","PK",null,"현장교차로ID",null,null,null,"EQ","현장교차로ID","spot_ints_id","NUMBER(5)","INTEGER","NUMBER(5)",null,null,null,"spot_ints_id ","INTEGER ","",",",null,"spot_ints_id",",",null,null,"spot_ints_id ","NUMBER(5) ","",",",null,null,"spot_ints_id",",","COMMENT ON COLUMN ","mtvsrltmsgnlchghstr.","spot_ints_id"," IS ","'현장교차로ID'",";",null,null,null,""]
[null,null,"노드ID","node_id",6,"VARCHAR2(300)","PK",null,"해당 교차로 노드ID",null,null,null,"EQ","노드ID","node_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,null,null,"node_id ","VARCHAR(300) ","",",",null,"node_id",",",null,null,"node_id ","VARCHAR2(300) ","",",",null,null,"node_id",",","COMMENT ON COLUMN ","mtvsrltmsgnlchghstr.","node_id"," IS ","'해당 교차로 노드ID'",";",null,null,null,""]
[null,null,"신호상태코드","sgnl_stts_cd",7,"CHAR(1)",null,null,"신호상태코드 (505)",null,null,"신호상태코드 (G, g, r, y)","EQ","신호상태코드","sgnl_stts_cd","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",null,null,null,"sgnl_stts_cd ","VARCHAR(1) ","",",",null,"",null,null,null,"sgnl_stts_cd ","VARCHAR2(1) ","",",",null,null,"",null,"COMMENT ON COLUMN ","mtvsrltmsgnlchghstr.","sgnl_stts_cd"," IS ","'신호상태코드 (505)'",";",null,null,null,""]
[null,null,"연결차로ID","cnct_lane_id",8,"VARCHAR2(300)","PK",null,"연결차로ID",null,null,null,"EQ","연결차로ID","cnct_lane_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",null,null,null,"cnct_lane_id ","VARCHAR(300) ","",",",null,"cnct_lane_id",",",null,null,"cnct_lane_id ","VARCHAR2(300) ","",",",null,null,"cnct_lane_id",",","COMMENT ON COLUMN ","mtvsrltmsgnlchghstr.","cnct_lane_id"," IS ","'연결차로ID'",";",null,null,null,""]
[null,null,"현시번호","phas_no",9,"NUMBER(2)","PK",null,"현시번호 (1~8)",null,null,null,"EQ","현시번호","phas_no","NUMBER(2)","INTEGER","NUMBER(2)",null,null,null,"phas_no ","INTEGER ","",",",null,"phas_no","));",null,null,"phas_no ","NUMBER(2) ","",",",null,null,"phas_no",")","COMMENT ON COLUMN ","mtvsrltmsgnlchghstr.","phas_no"," IS ","'현시번호 (1~8)'",";",null,null,null,""]
[null,null,"입력일시","inpt_dt",10,"TIMESTAMP",null,"NOT NULL","데이터입력일시",null,null,null,"EQ","입력일시","inpt_dt","TIMESTAMP","TIMESTAMP","TIMESTAMP",null,null,null,"inpt_dt ",{"$f":"IF(Q498=\"TIMESTAMP\", Q498&\" DEFAULT NOW \", Q498&\" \")","v":"TIMESTAMP DEFAULT NOW "},"NOT NULL",",",null,"",null,null,null,"inpt_dt ","TIMESTAMP ","NOT NULL",")",{"$nulls":4},"COMMENT ON COLUMN ","mtvsrltmsgnlchghstr.","inpt_dt"," IS ","'데이터입력일시'",";",null,null,null,""]
[{"$nulls":21},{"$f":"CONCATENATE(Z489:AB497)","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"CONCATENATE(AI499:AK499)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (CLCT_UNIX_TM) INTERVAL (86400) (PARTITION BFR_\" & N487 & \"_20221101 VALUES LESS THAN (1667228400));\"","v":"PARTITION BY RANGE (CLCT_UNIX_TM) INTERVAL (86400) (PARTITION BFR_mtvsrltmsgnlchghstr_20221101 VALUES LESS THAN (1667228400));"},{"$f":"\"CREATE INDEX PK_\" & N487 & \" ON \" & N487 & CONCATENATE(AJ489:AL498) & \" LOCAL (PARTITION BFR_\" & N487 & \"_20221101 TABLESPACE SOIT_I08);\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & N487 & \" ADD CONSTRAINT PK_\" & N487 & \" PRIMARY KEY \" & CONCATENATE(AJ489:AL498) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":10},{"$error":"#VALUE!"}]
[{"$nulls":47},""]
[{"$nulls":47},""]
[{"$nulls":47},""]
[{"$nulls":47},""]
[{"$nulls":47},""]
[{"$nulls":47},""]
[{"$nulls":47},""]
[{"$nulls":47},""]
[{"$nulls":47},""]
[{"$nulls":47},""]
[{"$nulls":30},{"$f":"O510&\" \"","v":" "},{"$f":"R510&\" \"","v":" "},{"$nulls":15},""]
[{"$nulls":47},""]
[{"$nulls":47},""]
[{"$nulls":30},{"$f":"O513&\" \"","v":" "},{"$f":"R513&\" \"","v":" "},{"$nulls":15},""]
[{"$nulls":30}," "," ",{"$nulls":15},""]
[{"$nulls":30}," "," ",{"$nulls":15},""]
[{"$nulls":47},""]
[{"$nulls":47},""]
[{"$nulls":47},""]
[{"$nulls":47},""]
[{"$nulls":47},""]
[{"$nulls":47},""]
[{"$nulls":47},""]
[{"$nulls":47},""]
[{"$nulls":47},""]
[{"$nulls":47},""]
[{"$nulls":47},""]
[{"$nulls":47},""]
[{"$nulls":47},""]
[{"$nulls":47},""]
[{"$nulls":47},""]

{"sheet":"SUMO-출력","index":9,"n_rows":397,"n_cols":55,"rows_kept":397,"cut":false,"hidden":false,"merged":[[223,1,238,1],[241,1,241,10],[243,1,258,1],[243,9,257,9],[261,1,261,10],[283,9,297,9],[301,1,301,10],[301,13,301,15],[303,9,317,9],[261,13,261,15],[263,9,277,9],[281,13,281,15],[263,1,278,1],[281,1,281,10],[1,1,1,10],[1,13,1,15],[3,1,18,1],[3,9,17,9],[21,1,21,10],[21,13,21,15],[23,9,37,9],[41,13,41,15],[23,1,38,1],[41,1,41,10],[43,1,58,1],[43,9,57,9],[61,1,61,10],[61,13,61,15],[63,9,77,9],[81,13,81,15],[63,1,78,1],[81,1,81,10],[83,1,98,1],[83,9,97,9],[101,1,101,10],[101,13,101,15],[103,9,117,9],[121,13,121,15],[103,1,118,1],[121,1,121,10],[123,1,138,1],[123,9,137,9],[141,1,141,10],[141,13,141,15],[143,9,157,9],[161,13,161,15],[143,1,158,1],[161,1,161,10],[163,1,178,1],[163,9,177,9],[181,1,181,10],[181,13,181,15],[183,9,197,9],[201,13,201,15],[183,1,198,1],[201,1,201,10],[203,1,218,1],[203,9,217,9],[221,1,221,10],[221,13,221,15],[223,9,237,9],[241,13,241,15],[384,1,384,10],[384,13,384,15],[323,9,337,9],[343,9,357,9],[303,1,318,1],[321,1,321,10],[321,13,321,15],[323,1,338,1],[341,1,341,10],[341,13,341,15],[343,1,358,1],[283,1,298,1],[386,1,394,1],[361,1,361,10],[361,13,361,15],[363,1,367,1],[363,9,367,10],[371,1,371,10],[371,13,371,15],[373,1,381,1]]}
[]
[null,"[5분] 실시간 차량이동궤적 테이블(실측) - 1지역",{"$nulls":11},"soitsrltmacsrvhclmvmntowh_1",null,null,"SOIT_D08_01","SOIT_I08",{"$nulls":29},{"$f":"IF(LEFT(AE2, 13) = \"CONSTRAINT PK\", AE2, \"\")","v":""}]
[27,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N2&\" \"","v":"soitsrltmacsrvhclmvmntowh_1 "},null," IS ",{"$f":"\"'\"&B2&\"'\"","v":"'[5분] 실시간 차량이동궤적 테이블(실측) - 1지역'"},";",null,null,null,""]
["TIBERO","soitsrltmacsrvhclmvmntowh_1\n(vehicle_history)","분석유닉스시각","anls_unix_tm",1,"NUMBER(10)","PK",null,"분석 대상기간 시작시각",{"$nulls":4},"분석유닉스시각","anls_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":10},"CREATE TABLE ",{"$f":"N2&\" (\"","v":"soitsrltmacsrvhclmvmntowh_1 ("},{"$f":"O4&\" \"","v":"anls_unix_tm "},{"$f":"R4&\" \"","v":"NUMBER(10) "},{"$f":"IF(H4=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",null,"(",{"$f":"IF(OR(G4=\"PK\", G4=\"PK/FK\"), O4, \"\")","v":"anls_unix_tm"},",","COMMENT ON COLUMN ",{"$f":"$N$2&\".\"","v":"soitsrltmacsrvhclmvmntowh_1."},{"$f":"O4","v":"anls_unix_tm"}," IS ",{"$f":"\"'\"&I4&\"'\"","v":"'분석 대상기간 시작시각'"},";",null,null,null,""]
[null,null,"위치수집유닉스시각","locn_clct_unix_tm",2,"NUMBER(10)","PK",null,"위치수집유닉스시각",{"$nulls":4},"위치수집유닉스시각","locn_clct_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":12},"locn_clct_unix_tm ","NUMBER(10) ","",",",null,null,"locn_clct_unix_tm",",","COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_1.","locn_clct_unix_tm"," IS ","'위치수집유닉스시각'",";",null,null,null,""]
[null,null,"차량ID","vhcl_id",3,"VARCHAR2(150)","PK",null,"차량ID",{"$nulls":4},"차량ID","vhcl_id","VARCHAR2(150)","VARCHAR(150)","VARCHAR2(150)",{"$nulls":12},"vhcl_id ","VARCHAR2(150) ","",",",null,null,"vhcl_id",")","COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_1.","vhcl_id"," IS ","'차량ID'",";",null,null,null,""]
[null,null,"차로ID","lane_id",4,"VARCHAR2(300)","FK",null,"통행차로ID",{"$nulls":4},"차로ID","lane_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",{"$nulls":12},"lane_id ","VARCHAR2(300) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_1.","lane_id"," IS ","'통행차로ID'",";",null,null,null,""]
[null,null,"세그먼트ID","sgmn_id",5,"VARCHAR2(300)","FK","NOT NULL","통행세그먼트ID",{"$nulls":4},"세그먼트ID","sgmn_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",{"$nulls":12},"sgmn_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_1.","sgmn_id"," IS ","'통행세그먼트ID'",";",null,null,null,""]
[null,null,"차종코드","kncr_cd",6,"CHAR(10)",null,null,"차종 (008)",{"$nulls":4},"차종코드","kncr_cd","CHAR(10)","VARCHAR(10)","VARCHAR2(10)",{"$nulls":12},"kncr_cd ","VARCHAR2(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_1.","kncr_cd"," IS ","'차종 (008)'",";",null,null,null,""]
[null,null,"순간속도","mmnt_sped",7,"NUMBER(5,2)",null,null,"순간속도 (m/s)",{"$nulls":4},"순간속도","mmnt_sped","NUMBER(5,2)","FLOAT","NUMBER(5,2)",{"$nulls":12},"mmnt_sped ","NUMBER(5,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_1.","mmnt_sped"," IS ","'순간속도 (m/s)'",";",null,null,null,"",{"$nulls":6},"FLOAT"]
[null,null,"비혼잡속도","non_cngt_sped",8,"NUMBER(5,2)",null,null,"비혼잡속도 (m/s)",{"$nulls":4},"비혼잡속도","non_cngt_sped","NUMBER(5,2)","FLOAT","NUMBER(5,2)",{"$nulls":12},"non_cngt_sped ","NUMBER(5,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_1.","non_cngt_sped"," IS ","'비혼잡속도 (m/s)'",";",null,null,null,"",{"$nulls":6},"FLOAT"]
[null,null,"차량경도","vhcl_lot",9,"NUMBER(13,10)",null,null,"차량경도",{"$nulls":4},"차량경도","vhcl_lot","NUMBER(13,10)","FLOAT","NUMBER(13,10)",{"$nulls":12},"vhcl_lot ","NUMBER(13,10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_1.","vhcl_lot"," IS ","'차량경도'",";",null,null,null,""]
[null,null,"차량위도","vhcl_lat",10,"NUMBER(12,10)",null,null,"차량위도",{"$nulls":4},"차량위도","vhcl_lat","NUMBER(12,10)","FLOAT","NUMBER(12,10)",{"$nulls":12},"vhcl_lat ","NUMBER(12,10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_1.","vhcl_lat"," IS ","'차량위도'",";",null,null,null,""]
[null,null,"차량고도","vhcl_lntd",11,"NUMBER(10)",null,null,"차량고도",{"$nulls":4},"차량고도","vhcl_lntd","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":12},"vhcl_lntd ","NUMBER(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_1.","vhcl_lntd"," IS ","'차량고도'",";",null,null,null,"",{"$nulls":6},"FLOAT"]
[null,null,"이동방위각도","mvmn_pocm_angl",12,"NUMBER(6,3)",null,null,"이동방위각도",{"$nulls":4},"이동방위각도","mvmn_pocm_angl","NUMBER(6,3)","FLOAT","NUMBER(6,3)",{"$nulls":12},"mvmn_pocm_angl ","NUMBER(6,3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_1.","mvmn_pocm_angl"," IS ","'이동방위각도'",";",null,null,null,""]
[null,null,"이동경사각도","mvmn_slop_angl",13,"NUMBER(6,3)",null,null,"이동경사각도",{"$nulls":4},"이동경사각도","mvmn_slop_angl","NUMBER(6,3)","FLOAT","NUMBER(6,3)",{"$nulls":12},"mvmn_slop_angl ","NUMBER(6,3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_1.","mvmn_slop_angl"," IS ","'이동경사각도'",";",null,null,null,""]
[null,null,"차로진행거리","lane_prgrs_dstn",14,"NUMBER(7,2)",null,null,"통행차로진행거리",{"$nulls":4},"차로진행거리","lane_prgrs_dstn","NUMBER(19,9)","FLOAT","NUMBER(19,9)",{"$nulls":12},"lane_prgrs_dstn ","NUMBER(19,9) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_1.","lane_prgrs_dstn"," IS ","'통행차로진행거리'",";",null,null,null,""]
[null,null,"대기행렬관측여부","queu_obsrvn_yn",15,"CHAR(1)",null,null,"대기행렬관측여부 (503)",{"$nulls":4},"대기행렬관측여부","queu_obsrvn_yn","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",{"$nulls":12},"queu_obsrvn_yn ","VARCHAR2(1) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_1.","queu_obsrvn_yn"," IS ","'대기행렬관측여부 (503)'",";",null,null,null,""]
[null,null,"지역구분코드","rgn_prttn_cd",16,"CHAR(2)","FK","NOT NULL","지역분할코드(051)",{"$nulls":4},"지역분할코드","rgn_prttn_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",{"$nulls":12},"rgn_prttn_cd ","VARCHAR2(2) ","NOT NULL",{"$f":"\") TABLESPACE \"&AI21&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_C001 NOLOGGING"},null,null,{"$f":"IF(OR(F19=\"PK\", F19=\"PK/FK\"), H19, \"\")","v":""},null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_1.","rgn_prttn_cd"," IS ","'지역분할코드(051)'",";"]
[{"$nulls":30},{"$f":"CONCATENATE(AI20:AK20)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (locn_clct_unix_tm) INTERVAL (3600) STORE IN (\"&AI21&\") (PARTITION BFR_\" & N2& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AI21&\");\"","v":"PARTITION BY RANGE (locn_clct_unix_tm) INTERVAL (3600) STORE IN (SOIT_D08_C001) (PARTITION BFR_soitsrltmacsrvhclmvmntowh_1_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_C001);"},{"$f":"\"CREATE INDEX PK_\" & N2& \" ON \" & N2 & CONCATENATE(AJ4:AL18) & \" LOCAL (PARTITION BFR_\" & N2 & \"_20221101 TABLESPACE \"&AJ21&\") TABLESPACE \"&AJ21&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & N2 & \" ADD CONSTRAINT PK_\" & N2 & \" PRIMARY KEY \" & CONCATENATE(AJ4:AL18) & \";\"","v":{"$error":"#VALUE!"}}]
[{"$nulls":34},"SOIT_D08_C001","SOIT_I08_C001"]
[null,"[5분] 실시간 차량이동궤적 테이블(실측) - 2지역",{"$nulls":11},"soitsrltmacsrvhclmvmntowh_2",null,null,"SOIT_D08_01","SOIT_I08",{"$nulls":29},{"$f":"IF(LEFT(AE22, 13) = \"CONSTRAINT PK\", AE22, \"\")","v":""}]
[27,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N22&\" \"","v":"soitsrltmacsrvhclmvmntowh_2 "},null," IS ",{"$f":"\"'\"&B22&\"'\"","v":"'[5분] 실시간 차량이동궤적 테이블(실측) - 2지역'"},";",null,null,null,""]
["TIBERO","soitsrltmacsrvhclmvmntowh_2\n(vehicle_history)","분석유닉스시각","anls_unix_tm",1,"NUMBER(10)","PK",null,"분석 대상기간 시작시각",{"$nulls":4},"분석유닉스시각","anls_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":10},"CREATE TABLE ",{"$f":"N22&\" (\"","v":"soitsrltmacsrvhclmvmntowh_2 ("},{"$f":"O24&\" \"","v":"anls_unix_tm "},{"$f":"R24&\" \"","v":"NUMBER(10) "},{"$f":"IF(H24=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",null,"(",{"$f":"IF(OR(G24=\"PK\", G24=\"PK/FK\"), O24, \"\")","v":"anls_unix_tm"},",","COMMENT ON COLUMN ",{"$f":"$N$22&\".\"","v":"soitsrltmacsrvhclmvmntowh_2."},{"$f":"O24","v":"anls_unix_tm"}," IS ",{"$f":"\"'\"&I24&\"'\"","v":"'분석 대상기간 시작시각'"},";",null,null,null,""]
[null,null,"위치수집유닉스시각","locn_clct_unix_tm",2,"NUMBER(10)","PK",null,"위치수집유닉스시각",{"$nulls":4},"위치수집유닉스시각","locn_clct_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":12},"locn_clct_unix_tm ","NUMBER(10) ","",",",null,null,"locn_clct_unix_tm",",","COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_2.","locn_clct_unix_tm"," IS ","'위치수집유닉스시각'",";",null,null,null,""]
[null,null,"차량ID","vhcl_id",3,"VARCHAR2(150)","PK",null,"차량ID",{"$nulls":4},"차량ID","vhcl_id","VARCHAR2(150)","VARCHAR(150)","VARCHAR2(150)",{"$nulls":12},"vhcl_id ","VARCHAR2(150) ","",",",null,null,"vhcl_id",")","COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_2.","vhcl_id"," IS ","'차량ID'",";",null,null,null,""]
[null,null,"차로ID","lane_id",4,"VARCHAR2(300)","FK",null,"통행차로ID",{"$nulls":4},"차로ID","lane_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",{"$nulls":12},"lane_id ","VARCHAR2(300) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_2.","lane_id"," IS ","'통행차로ID'",";",null,null,null,""]
[null,null,"세그먼트ID","sgmn_id",5,"VARCHAR2(300)","FK","NOT NULL","통행세그먼트ID",{"$nulls":4},"세그먼트ID","sgmn_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",{"$nulls":12},"sgmn_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_2.","sgmn_id"," IS ","'통행세그먼트ID'",";",null,null,null,""]
[null,null,"차종코드","kncr_cd",6,"CHAR(10)",null,null,"차종 (008)",{"$nulls":4},"차종코드","kncr_cd","CHAR(10)","VARCHAR(10)","VARCHAR2(10)",{"$nulls":12},"kncr_cd ","VARCHAR2(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_2.","kncr_cd"," IS ","'차종 (008)'",";",null,null,null,""]
[null,null,"순간속도","mmnt_sped",7,"NUMBER(5,2)",null,null,"순간속도 (m/s)",{"$nulls":4},"순간속도","mmnt_sped","NUMBER(5,2)","FLOAT","NUMBER(5,2)",{"$nulls":12},"mmnt_sped ","NUMBER(5,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_2.","mmnt_sped"," IS ","'순간속도 (m/s)'",";",null,null,null,"",{"$nulls":6},"FLOAT"]
[null,null,"비혼잡속도","non_cngt_sped",8,"NUMBER(5,2)",null,null,"비혼잡속도 (m/s)",{"$nulls":4},"비혼잡속도","non_cngt_sped","NUMBER(5,2)","FLOAT","NUMBER(5,2)",{"$nulls":12},"non_cngt_sped ","NUMBER(5,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_2.","non_cngt_sped"," IS ","'비혼잡속도 (m/s)'",";",null,null,null,"",{"$nulls":6},"FLOAT"]
[null,null,"차량경도","vhcl_lot",9,"NUMBER(13,10)",null,null,"차량경도",{"$nulls":4},"차량경도","vhcl_lot","NUMBER(13,10)","FLOAT","NUMBER(13,10)",{"$nulls":12},"vhcl_lot ","NUMBER(13,10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_2.","vhcl_lot"," IS ","'차량경도'",";",null,null,null,""]
[null,null,"차량위도","vhcl_lat",10,"NUMBER(12,10)",null,null,"차량위도",{"$nulls":4},"차량위도","vhcl_lat","NUMBER(12,10)","FLOAT","NUMBER(12,10)",{"$nulls":12},"vhcl_lat ","NUMBER(12,10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_2.","vhcl_lat"," IS ","'차량위도'",";",null,null,null,""]
[null,null,"차량고도","vhcl_lntd",11,"NUMBER(10)",null,null,"차량고도",{"$nulls":4},"차량고도","vhcl_lntd","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":12},"vhcl_lntd ","NUMBER(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_2.","vhcl_lntd"," IS ","'차량고도'",";",null,null,null,"",{"$nulls":6},"FLOAT"]
[null,null,"이동방위각도","mvmn_pocm_angl",12,"NUMBER(6,3)",null,null,"이동방위각도",{"$nulls":4},"이동방위각도","mvmn_pocm_angl","NUMBER(6,3)","FLOAT","NUMBER(6,3)",{"$nulls":12},"mvmn_pocm_angl ","NUMBER(6,3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_2.","mvmn_pocm_angl"," IS ","'이동방위각도'",";",null,null,null,""]
[null,null,"이동경사각도","mvmn_slop_angl",13,"NUMBER(6,3)",null,null,"이동경사각도",{"$nulls":4},"이동경사각도","mvmn_slop_angl","NUMBER(6,3)","FLOAT","NUMBER(6,3)",{"$nulls":12},"mvmn_slop_angl ","NUMBER(6,3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_2.","mvmn_slop_angl"," IS ","'이동경사각도'",";",null,null,null,""]
[null,null,"차로진행거리","lane_prgrs_dstn",14,"NUMBER(7,2)",null,null,"통행차로진행거리",{"$nulls":4},"차로진행거리","lane_prgrs_dstn","NUMBER(19,9)","FLOAT","NUMBER(19,9)",{"$nulls":12},"lane_prgrs_dstn ","NUMBER(19,9) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_2.","lane_prgrs_dstn"," IS ","'통행차로진행거리'",";",null,null,null,""]
[null,null,"대기행렬관측여부","queu_obsrvn_yn",15,"CHAR(1)",null,null,"대기행렬관측여부 (503)",{"$nulls":4},"대기행렬관측여부","queu_obsrvn_yn","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",{"$nulls":12},"queu_obsrvn_yn ","VARCHAR2(1) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_2.","queu_obsrvn_yn"," IS ","'대기행렬관측여부 (503)'",";",null,null,null,""]
[null,null,"지역구분코드","rgn_prttn_cd",16,"CHAR(2)","FK","NOT NULL","지역분할코드(051)",{"$nulls":4},"지역분할코드","rgn_prttn_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",{"$nulls":12},"rgn_prttn_cd ","VARCHAR2(2) ","NOT NULL",{"$f":"\") TABLESPACE \"&AI41&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_C002 NOLOGGING"},null,null,{"$f":"IF(OR(F39=\"PK\", F39=\"PK/FK\"), H39, \"\")","v":""},null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_2.","rgn_prttn_cd"," IS ","'지역분할코드(051)'",";"]
[{"$nulls":30},{"$f":"CONCATENATE(AI40:AK40)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (locn_clct_unix_tm) INTERVAL (3600) STORE IN (\"&AI41&\") (PARTITION BFR_\" & N22& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AI41&\");\"","v":"PARTITION BY RANGE (locn_clct_unix_tm) INTERVAL (3600) STORE IN (SOIT_D08_C002) (PARTITION BFR_soitsrltmacsrvhclmvmntowh_2_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_C002);"},{"$f":"\"CREATE INDEX PK_\" & N22& \" ON \" & N22 & CONCATENATE(AJ24:AL38) & \" LOCAL (PARTITION BFR_\" & N22 & \"_20221101 TABLESPACE \"&AJ41&\") TABLESPACE \"&AJ41&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & N22 & \" ADD CONSTRAINT PK_\" & N22 & \" PRIMARY KEY \" & CONCATENATE(AJ24:AL38) & \";\"","v":{"$error":"#VALUE!"}}]
[{"$nulls":34},"SOIT_D08_C002","SOIT_I08_C002"]
[null,"[5분] 실시간 차량이동궤적 테이블(실측) - 3지역",{"$nulls":11},"soitsrltmacsrvhclmvmntowh_3",null,null,"SOIT_D08_01","SOIT_I08",{"$nulls":29},{"$f":"IF(LEFT(AE42, 13) = \"CONSTRAINT PK\", AE42, \"\")","v":""}]
[27,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N42&\" \"","v":"soitsrltmacsrvhclmvmntowh_3 "},null," IS ",{"$f":"\"'\"&B42&\"'\"","v":"'[5분] 실시간 차량이동궤적 테이블(실측) - 3지역'"},";",null,null,null,""]
["TIBERO","soitsrltmacsrvhclmvmntowh_3\n(vehicle_history)","분석유닉스시각","anls_unix_tm",1,"NUMBER(10)","PK",null,"분석 대상기간 시작시각",{"$nulls":4},"분석유닉스시각","anls_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":10},"CREATE TABLE ",{"$f":"N42&\" (\"","v":"soitsrltmacsrvhclmvmntowh_3 ("},{"$f":"O44&\" \"","v":"anls_unix_tm "},{"$f":"R44&\" \"","v":"NUMBER(10) "},{"$f":"IF(H44=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",null,"(",{"$f":"IF(OR(G44=\"PK\", G44=\"PK/FK\"), O44, \"\")","v":"anls_unix_tm"},",","COMMENT ON COLUMN ",{"$f":"$N$42&\".\"","v":"soitsrltmacsrvhclmvmntowh_3."},{"$f":"O44","v":"anls_unix_tm"}," IS ",{"$f":"\"'\"&I44&\"'\"","v":"'분석 대상기간 시작시각'"},";",null,null,null,""]
[null,null,"위치수집유닉스시각","locn_clct_unix_tm",2,"NUMBER(10)","PK",null,"위치수집유닉스시각",{"$nulls":4},"위치수집유닉스시각","locn_clct_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":12},"locn_clct_unix_tm ","NUMBER(10) ","",",",null,null,"locn_clct_unix_tm",",","COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_3.","locn_clct_unix_tm"," IS ","'위치수집유닉스시각'",";",null,null,null,""]
[null,null,"차량ID","vhcl_id",3,"VARCHAR2(150)","PK",null,"차량ID",{"$nulls":4},"차량ID","vhcl_id","VARCHAR2(150)","VARCHAR(150)","VARCHAR2(150)",{"$nulls":12},"vhcl_id ","VARCHAR2(150) ","",",",null,null,"vhcl_id",")","COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_3.","vhcl_id"," IS ","'차량ID'",";",null,null,null,""]
[null,null,"차로ID","lane_id",4,"VARCHAR2(300)","FK",null,"통행차로ID",{"$nulls":4},"차로ID","lane_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",{"$nulls":12},"lane_id ","VARCHAR2(300) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_3.","lane_id"," IS ","'통행차로ID'",";",null,null,null,""]
[null,null,"세그먼트ID","sgmn_id",5,"VARCHAR2(300)","FK","NOT NULL","통행세그먼트ID",{"$nulls":4},"세그먼트ID","sgmn_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",{"$nulls":12},"sgmn_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_3.","sgmn_id"," IS ","'통행세그먼트ID'",";",null,null,null,""]
[null,null,"차종코드","kncr_cd",6,"CHAR(10)",null,null,"차종 (008)",{"$nulls":4},"차종코드","kncr_cd","CHAR(10)","VARCHAR(10)","VARCHAR2(10)",{"$nulls":12},"kncr_cd ","VARCHAR2(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_3.","kncr_cd"," IS ","'차종 (008)'",";",null,null,null,""]
[null,null,"순간속도","mmnt_sped",7,"NUMBER(5,2)",null,null,"순간속도 (m/s)",{"$nulls":4},"순간속도","mmnt_sped","NUMBER(5,2)","FLOAT","NUMBER(5,2)",{"$nulls":12},"mmnt_sped ","NUMBER(5,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_3.","mmnt_sped"," IS ","'순간속도 (m/s)'",";",null,null,null,"",{"$nulls":6},"FLOAT"]
[null,null,"비혼잡속도","non_cngt_sped",8,"NUMBER(5,2)",null,null,"비혼잡속도 (m/s)",{"$nulls":4},"비혼잡속도","non_cngt_sped","NUMBER(5,2)","FLOAT","NUMBER(5,2)",{"$nulls":12},"non_cngt_sped ","NUMBER(5,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_3.","non_cngt_sped"," IS ","'비혼잡속도 (m/s)'",";",null,null,null,"",{"$nulls":6},"FLOAT"]
[null,null,"차량경도","vhcl_lot",9,"NUMBER(13,10)",null,null,"차량경도",{"$nulls":4},"차량경도","vhcl_lot","NUMBER(13,10)","FLOAT","NUMBER(13,10)",{"$nulls":12},"vhcl_lot ","NUMBER(13,10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_3.","vhcl_lot"," IS ","'차량경도'",";",null,null,null,""]
[null,null,"차량위도","vhcl_lat",10,"NUMBER(12,10)",null,null,"차량위도",{"$nulls":4},"차량위도","vhcl_lat","NUMBER(12,10)","FLOAT","NUMBER(12,10)",{"$nulls":12},"vhcl_lat ","NUMBER(12,10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_3.","vhcl_lat"," IS ","'차량위도'",";",null,null,null,""]
[null,null,"차량고도","vhcl_lntd",11,"NUMBER(10)",null,null,"차량고도",{"$nulls":4},"차량고도","vhcl_lntd","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":12},"vhcl_lntd ","NUMBER(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_3.","vhcl_lntd"," IS ","'차량고도'",";",null,null,null,"",{"$nulls":6},"FLOAT"]
[null,null,"이동방위각도","mvmn_pocm_angl",12,"NUMBER(6,3)",null,null,"이동방위각도",{"$nulls":4},"이동방위각도","mvmn_pocm_angl","NUMBER(6,3)","FLOAT","NUMBER(6,3)",{"$nulls":12},"mvmn_pocm_angl ","NUMBER(6,3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_3.","mvmn_pocm_angl"," IS ","'이동방위각도'",";",null,null,null,""]
[null,null,"이동경사각도","mvmn_slop_angl",13,"NUMBER(6,3)",null,null,"이동경사각도",{"$nulls":4},"이동경사각도","mvmn_slop_angl","NUMBER(6,3)","FLOAT","NUMBER(6,3)",{"$nulls":12},"mvmn_slop_angl ","NUMBER(6,3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_3.","mvmn_slop_angl"," IS ","'이동경사각도'",";",null,null,null,""]
[null,null,"차로진행거리","lane_prgrs_dstn",14,"NUMBER(7,2)",null,null,"통행차로진행거리",{"$nulls":4},"차로진행거리","lane_prgrs_dstn","NUMBER(19,9)","FLOAT","NUMBER(19,9)",{"$nulls":12},"lane_prgrs_dstn ","NUMBER(19,9) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_3.","lane_prgrs_dstn"," IS ","'통행차로진행거리'",";",null,null,null,""]
[null,null,"대기행렬관측여부","queu_obsrvn_yn",15,"CHAR(1)",null,null,"대기행렬관측여부 (503)",{"$nulls":4},"대기행렬관측여부","queu_obsrvn_yn","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",{"$nulls":12},"queu_obsrvn_yn ","VARCHAR2(1) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_3.","queu_obsrvn_yn"," IS ","'대기행렬관측여부 (503)'",";",null,null,null,""]
[null,null,"지역구분코드","rgn_prttn_cd",16,"CHAR(2)","FK","NOT NULL","지역분할코드(051)",{"$nulls":4},"지역분할코드","rgn_prttn_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",{"$nulls":12},"rgn_prttn_cd ","VARCHAR2(2) ","NOT NULL",{"$f":"\") TABLESPACE \"&AI61&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_C003 NOLOGGING"},null,null,{"$f":"IF(OR(F59=\"PK\", F59=\"PK/FK\"), H59, \"\")","v":""},null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_3.","rgn_prttn_cd"," IS ","'지역분할코드(051)'",";"]
[{"$nulls":30},{"$f":"CONCATENATE(AI60:AK60)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (locn_clct_unix_tm) INTERVAL (3600) STORE IN (\"&AI61&\") (PARTITION BFR_\" & N42& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AI61&\");\"","v":"PARTITION BY RANGE (locn_clct_unix_tm) INTERVAL (3600) STORE IN (SOIT_D08_C003) (PARTITION BFR_soitsrltmacsrvhclmvmntowh_3_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_C003);"},{"$f":"\"CREATE INDEX PK_\" & N42& \" ON \" & N42 & CONCATENATE(AJ44:AL58) & \" LOCAL (PARTITION BFR_\" & N42 & \"_20221101 TABLESPACE \"&AJ61&\") TABLESPACE \"&AJ61&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & N42 & \" ADD CONSTRAINT PK_\" & N42 & \" PRIMARY KEY \" & CONCATENATE(AJ44:AL58) & \";\"","v":{"$error":"#VALUE!"}}]
[{"$nulls":34},"SOIT_D08_C003","SOIT_I08_C003"]
[null,"[5분] 실시간 차량이동궤적 테이블(실측) - 4지역",{"$nulls":11},"soitsrltmacsrvhclmvmntowh_4",null,null,"SOIT_D08_01","SOIT_I08",{"$nulls":29},{"$f":"IF(LEFT(AE62, 13) = \"CONSTRAINT PK\", AE62, \"\")","v":""}]
[27,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N62&\" \"","v":"soitsrltmacsrvhclmvmntowh_4 "},null," IS ",{"$f":"\"'\"&B62&\"'\"","v":"'[5분] 실시간 차량이동궤적 테이블(실측) - 4지역'"},";",null,null,null,""]
["TIBERO","soitsrltmacsrvhclmvmntowh_4\n(vehicle_history)","분석유닉스시각","anls_unix_tm",1,"NUMBER(10)","PK",null,"분석 대상기간 시작시각",{"$nulls":4},"분석유닉스시각","anls_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":10},"CREATE TABLE ",{"$f":"N62&\" (\"","v":"soitsrltmacsrvhclmvmntowh_4 ("},{"$f":"O64&\" \"","v":"anls_unix_tm "},{"$f":"R64&\" \"","v":"NUMBER(10) "},{"$f":"IF(H64=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",null,"(",{"$f":"IF(OR(G64=\"PK\", G64=\"PK/FK\"), O64, \"\")","v":"anls_unix_tm"},",","COMMENT ON COLUMN ",{"$f":"$N$62&\".\"","v":"soitsrltmacsrvhclmvmntowh_4."},{"$f":"O64","v":"anls_unix_tm"}," IS ",{"$f":"\"'\"&I64&\"'\"","v":"'분석 대상기간 시작시각'"},";",null,null,null,""]
[null,null,"위치수집유닉스시각","locn_clct_unix_tm",2,"NUMBER(10)","PK",null,"위치수집유닉스시각",{"$nulls":4},"위치수집유닉스시각","locn_clct_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":12},"locn_clct_unix_tm ","NUMBER(10) ","",",",null,null,"locn_clct_unix_tm",",","COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_4.","locn_clct_unix_tm"," IS ","'위치수집유닉스시각'",";",null,null,null,""]
[null,null,"차량ID","vhcl_id",3,"VARCHAR2(150)","PK",null,"차량ID",{"$nulls":4},"차량ID","vhcl_id","VARCHAR2(150)","VARCHAR(150)","VARCHAR2(150)",{"$nulls":12},"vhcl_id ","VARCHAR2(150) ","",",",null,null,"vhcl_id",")","COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_4.","vhcl_id"," IS ","'차량ID'",";",null,null,null,""]
[null,null,"차로ID","lane_id",4,"VARCHAR2(300)","FK",null,"통행차로ID",{"$nulls":4},"차로ID","lane_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",{"$nulls":12},"lane_id ","VARCHAR2(300) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_4.","lane_id"," IS ","'통행차로ID'",";",null,null,null,""]
[null,null,"세그먼트ID","sgmn_id",5,"VARCHAR2(300)","FK","NOT NULL","통행세그먼트ID",{"$nulls":4},"세그먼트ID","sgmn_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",{"$nulls":12},"sgmn_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_4.","sgmn_id"," IS ","'통행세그먼트ID'",";",null,null,null,""]
[null,null,"차종코드","kncr_cd",6,"CHAR(10)",null,null,"차종 (008)",{"$nulls":4},"차종코드","kncr_cd","CHAR(10)","VARCHAR(10)","VARCHAR2(10)",{"$nulls":12},"kncr_cd ","VARCHAR2(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_4.","kncr_cd"," IS ","'차종 (008)'",";",null,null,null,""]
[null,null,"순간속도","mmnt_sped",7,"NUMBER(5,2)",null,null,"순간속도 (m/s)",{"$nulls":4},"순간속도","mmnt_sped","NUMBER(5,2)","FLOAT","NUMBER(5,2)",{"$nulls":12},"mmnt_sped ","NUMBER(5,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_4.","mmnt_sped"," IS ","'순간속도 (m/s)'",";",null,null,null,"",{"$nulls":6},"FLOAT"]
[null,null,"비혼잡속도","non_cngt_sped",8,"NUMBER(5,2)",null,null,"비혼잡속도 (m/s)",{"$nulls":4},"비혼잡속도","non_cngt_sped","NUMBER(5,2)","FLOAT","NUMBER(5,2)",{"$nulls":12},"non_cngt_sped ","NUMBER(5,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_4.","non_cngt_sped"," IS ","'비혼잡속도 (m/s)'",";",null,null,null,"",{"$nulls":6},"FLOAT"]
[null,null,"차량경도","vhcl_lot",9,"NUMBER(13,10)",null,null,"차량경도",{"$nulls":4},"차량경도","vhcl_lot","NUMBER(13,10)","FLOAT","NUMBER(13,10)",{"$nulls":12},"vhcl_lot ","NUMBER(13,10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_4.","vhcl_lot"," IS ","'차량경도'",";",null,null,null,""]
[null,null,"차량위도","vhcl_lat",10,"NUMBER(12,10)",null,null,"차량위도",{"$nulls":4},"차량위도","vhcl_lat","NUMBER(12,10)","FLOAT","NUMBER(12,10)",{"$nulls":12},"vhcl_lat ","NUMBER(12,10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_4.","vhcl_lat"," IS ","'차량위도'",";",null,null,null,""]
[null,null,"차량고도","vhcl_lntd",11,"NUMBER(10)",null,null,"차량고도",{"$nulls":4},"차량고도","vhcl_lntd","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":12},"vhcl_lntd ","NUMBER(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_4.","vhcl_lntd"," IS ","'차량고도'",";",null,null,null,"",{"$nulls":6},"FLOAT"]
[null,null,"이동방위각도","mvmn_pocm_angl",12,"NUMBER(6,3)",null,null,"이동방위각도",{"$nulls":4},"이동방위각도","mvmn_pocm_angl","NUMBER(6,3)","FLOAT","NUMBER(6,3)",{"$nulls":12},"mvmn_pocm_angl ","NUMBER(6,3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_4.","mvmn_pocm_angl"," IS ","'이동방위각도'",";",null,null,null,""]
[null,null,"이동경사각도","mvmn_slop_angl",13,"NUMBER(6,3)",null,null,"이동경사각도",{"$nulls":4},"이동경사각도","mvmn_slop_angl","NUMBER(6,3)","FLOAT","NUMBER(6,3)",{"$nulls":12},"mvmn_slop_angl ","NUMBER(6,3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_4.","mvmn_slop_angl"," IS ","'이동경사각도'",";",null,null,null,""]
[null,null,"차로진행거리","lane_prgrs_dstn",14,"NUMBER(7,2)",null,null,"통행차로진행거리",{"$nulls":4},"차로진행거리","lane_prgrs_dstn","NUMBER(19,9)","FLOAT","NUMBER(19,9)",{"$nulls":12},"lane_prgrs_dstn ","NUMBER(19,9) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_4.","lane_prgrs_dstn"," IS ","'통행차로진행거리'",";",null,null,null,""]
[null,null,"대기행렬관측여부","queu_obsrvn_yn",15,"CHAR(1)",null,null,"대기행렬관측여부 (503)",{"$nulls":4},"대기행렬관측여부","queu_obsrvn_yn","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",{"$nulls":12},"queu_obsrvn_yn ","VARCHAR2(1) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_4.","queu_obsrvn_yn"," IS ","'대기행렬관측여부 (503)'",";",null,null,null,""]
[null,null,"지역구분코드","rgn_prttn_cd",16,"CHAR(2)","FK","NOT NULL","지역분할코드(051)",{"$nulls":4},"지역분할코드","rgn_prttn_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",{"$nulls":12},"rgn_prttn_cd ","VARCHAR2(2) ","NOT NULL",{"$f":"\") TABLESPACE \"&AI81&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_C004 NOLOGGING"},null,null,{"$f":"IF(OR(F79=\"PK\", F79=\"PK/FK\"), H79, \"\")","v":""},null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_4.","rgn_prttn_cd"," IS ","'지역분할코드(051)'",";"]
[{"$nulls":30},{"$f":"CONCATENATE(AI80:AK80)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (locn_clct_unix_tm) INTERVAL (3600) STORE IN (\"&AI81&\") (PARTITION BFR_\" & N62& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AI81&\");\"","v":"PARTITION BY RANGE (locn_clct_unix_tm) INTERVAL (3600) STORE IN (SOIT_D08_C004) (PARTITION BFR_soitsrltmacsrvhclmvmntowh_4_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_C004);"},{"$f":"\"CREATE INDEX PK_\" & N62& \" ON \" & N62 & CONCATENATE(AJ64:AL78) & \" LOCAL (PARTITION BFR_\" & N62 & \"_20221101 TABLESPACE \"&AJ81&\") TABLESPACE \"&AJ81&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & N62 & \" ADD CONSTRAINT PK_\" & N62 & \" PRIMARY KEY \" & CONCATENATE(AJ64:AL78) & \";\"","v":{"$error":"#VALUE!"}}]
[{"$nulls":34},"SOIT_D08_C004","SOIT_I08_C004"]
[null,"[5분] 실시간 차량이동궤적 테이블(실측) - 5지역",{"$nulls":11},"soitsrltmacsrvhclmvmntowh_5",null,null,"SOIT_D08_01","SOIT_I08",{"$nulls":29},{"$f":"IF(LEFT(AE82, 13) = \"CONSTRAINT PK\", AE82, \"\")","v":""}]
[27,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N82&\" \"","v":"soitsrltmacsrvhclmvmntowh_5 "},null," IS ",{"$f":"\"'\"&B82&\"'\"","v":"'[5분] 실시간 차량이동궤적 테이블(실측) - 5지역'"},";",null,null,null,""]
["TIBERO","soitsrltmacsrvhclmvmntowh_5\n(vehicle_history)","분석유닉스시각","anls_unix_tm",1,"NUMBER(10)","PK",null,"분석 대상기간 시작시각",{"$nulls":4},"분석유닉스시각","anls_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":10},"CREATE TABLE ",{"$f":"N82&\" (\"","v":"soitsrltmacsrvhclmvmntowh_5 ("},{"$f":"O84&\" \"","v":"anls_unix_tm "},{"$f":"R84&\" \"","v":"NUMBER(10) "},{"$f":"IF(H84=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",null,"(",{"$f":"IF(OR(G84=\"PK\", G84=\"PK/FK\"), O84, \"\")","v":"anls_unix_tm"},",","COMMENT ON COLUMN ",{"$f":"$N$82&\".\"","v":"soitsrltmacsrvhclmvmntowh_5."},{"$f":"O84","v":"anls_unix_tm"}," IS ",{"$f":"\"'\"&I84&\"'\"","v":"'분석 대상기간 시작시각'"},";",null,null,null,""]
[null,null,"위치수집유닉스시각","locn_clct_unix_tm",2,"NUMBER(10)","PK",null,"위치수집유닉스시각",{"$nulls":4},"위치수집유닉스시각","locn_clct_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":12},"locn_clct_unix_tm ","NUMBER(10) ","",",",null,null,"locn_clct_unix_tm",",","COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_5.","locn_clct_unix_tm"," IS ","'위치수집유닉스시각'",";",null,null,null,""]
[null,null,"차량ID","vhcl_id",3,"VARCHAR2(150)","PK",null,"차량ID",{"$nulls":4},"차량ID","vhcl_id","VARCHAR2(150)","VARCHAR(150)","VARCHAR2(150)",{"$nulls":12},"vhcl_id ","VARCHAR2(150) ","",",",null,null,"vhcl_id",")","COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_5.","vhcl_id"," IS ","'차량ID'",";",null,null,null,""]
[null,null,"차로ID","lane_id",4,"VARCHAR2(300)","FK",null,"통행차로ID",{"$nulls":4},"차로ID","lane_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",{"$nulls":12},"lane_id ","VARCHAR2(300) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_5.","lane_id"," IS ","'통행차로ID'",";",null,null,null,""]
[null,null,"세그먼트ID","sgmn_id",5,"VARCHAR2(300)","FK","NOT NULL","통행세그먼트ID",{"$nulls":4},"세그먼트ID","sgmn_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",{"$nulls":12},"sgmn_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_5.","sgmn_id"," IS ","'통행세그먼트ID'",";",null,null,null,""]
[null,null,"차종코드","kncr_cd",6,"CHAR(10)",null,null,"차종 (008)",{"$nulls":4},"차종코드","kncr_cd","CHAR(10)","VARCHAR(10)","VARCHAR2(10)",{"$nulls":12},"kncr_cd ","VARCHAR2(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_5.","kncr_cd"," IS ","'차종 (008)'",";",null,null,null,""]
[null,null,"순간속도","mmnt_sped",7,"NUMBER(5,2)",null,null,"순간속도 (m/s)",{"$nulls":4},"순간속도","mmnt_sped","NUMBER(5,2)","FLOAT","NUMBER(5,2)",{"$nulls":12},"mmnt_sped ","NUMBER(5,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_5.","mmnt_sped"," IS ","'순간속도 (m/s)'",";",null,null,null,"",{"$nulls":6},"FLOAT"]
[null,null,"비혼잡속도","non_cngt_sped",8,"NUMBER(5,2)",null,null,"비혼잡속도 (m/s)",{"$nulls":4},"비혼잡속도","non_cngt_sped","NUMBER(5,2)","FLOAT","NUMBER(5,2)",{"$nulls":12},"non_cngt_sped ","NUMBER(5,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_5.","non_cngt_sped"," IS ","'비혼잡속도 (m/s)'",";",null,null,null,"",{"$nulls":6},"FLOAT"]
[null,null,"차량경도","vhcl_lot",9,"NUMBER(13,10)",null,null,"차량경도",{"$nulls":4},"차량경도","vhcl_lot","NUMBER(13,10)","FLOAT","NUMBER(13,10)",{"$nulls":12},"vhcl_lot ","NUMBER(13,10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_5.","vhcl_lot"," IS ","'차량경도'",";",null,null,null,""]
[null,null,"차량위도","vhcl_lat",10,"NUMBER(12,10)",null,null,"차량위도",{"$nulls":4},"차량위도","vhcl_lat","NUMBER(12,10)","FLOAT","NUMBER(12,10)",{"$nulls":12},"vhcl_lat ","NUMBER(12,10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_5.","vhcl_lat"," IS ","'차량위도'",";",null,null,null,""]
[null,null,"차량고도","vhcl_lntd",11,"NUMBER(10)",null,null,"차량고도",{"$nulls":4},"차량고도","vhcl_lntd","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":12},"vhcl_lntd ","NUMBER(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_5.","vhcl_lntd"," IS ","'차량고도'",";",null,null,null,"",{"$nulls":6},"FLOAT"]
[null,null,"이동방위각도","mvmn_pocm_angl",12,"NUMBER(6,3)",null,null,"이동방위각도",{"$nulls":4},"이동방위각도","mvmn_pocm_angl","NUMBER(6,3)","FLOAT","NUMBER(6,3)",{"$nulls":12},"mvmn_pocm_angl ","NUMBER(6,3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_5.","mvmn_pocm_angl"," IS ","'이동방위각도'",";",null,null,null,""]
[null,null,"이동경사각도","mvmn_slop_angl",13,"NUMBER(6,3)",null,null,"이동경사각도",{"$nulls":4},"이동경사각도","mvmn_slop_angl","NUMBER(6,3)","FLOAT","NUMBER(6,3)",{"$nulls":12},"mvmn_slop_angl ","NUMBER(6,3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_5.","mvmn_slop_angl"," IS ","'이동경사각도'",";",null,null,null,""]
[null,null,"차로진행거리","lane_prgrs_dstn",14,"NUMBER(7,2)",null,null,"통행차로진행거리",{"$nulls":4},"차로진행거리","lane_prgrs_dstn","NUMBER(19,9)","FLOAT","NUMBER(19,9)",{"$nulls":12},"lane_prgrs_dstn ","NUMBER(19,9) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_5.","lane_prgrs_dstn"," IS ","'통행차로진행거리'",";",null,null,null,""]
[null,null,"대기행렬관측여부","queu_obsrvn_yn",15,"CHAR(1)",null,null,"대기행렬관측여부 (503)",{"$nulls":4},"대기행렬관측여부","queu_obsrvn_yn","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",{"$nulls":12},"queu_obsrvn_yn ","VARCHAR2(1) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_5.","queu_obsrvn_yn"," IS ","'대기행렬관측여부 (503)'",";",null,null,null,""]
[null,null,"지역구분코드","rgn_prttn_cd",16,"CHAR(2)","FK","NOT NULL","지역분할코드(051)",{"$nulls":4},"지역분할코드","rgn_prttn_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",{"$nulls":12},"rgn_prttn_cd ","VARCHAR2(2) ","NOT NULL",{"$f":"\") TABLESPACE \"&AI101&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_C005 NOLOGGING"},null,null,{"$f":"IF(OR(F99=\"PK\", F99=\"PK/FK\"), H99, \"\")","v":""},null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_5.","rgn_prttn_cd"," IS ","'지역분할코드(051)'",";"]
[{"$nulls":30},{"$f":"CONCATENATE(AI100:AK100)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (locn_clct_unix_tm) INTERVAL (3600) STORE IN (\"&AI101&\") (PARTITION BFR_\" & N82& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AI101&\");\"","v":"PARTITION BY RANGE (locn_clct_unix_tm) INTERVAL (3600) STORE IN (SOIT_D08_C005) (PARTITION BFR_soitsrltmacsrvhclmvmntowh_5_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_C005);"},{"$f":"\"CREATE INDEX PK_\" & N82& \" ON \" & N82 & CONCATENATE(AJ84:AL98) & \" LOCAL (PARTITION BFR_\" & N82 & \"_20221101 TABLESPACE \"&AJ101&\") TABLESPACE \"&AJ101&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & N82 & \" ADD CONSTRAINT PK_\" & N82 & \" PRIMARY KEY \" & CONCATENATE(AJ84:AL98) & \";\"","v":{"$error":"#VALUE!"}}]
[{"$nulls":34},"SOIT_D08_C005","SOIT_I08_C005"]
[null,"[5분] 실시간 차량이동궤적 테이블(실측) - 6지역",{"$nulls":11},"soitsrltmacsrvhclmvmntowh_6",null,null,"SOIT_D08_01","SOIT_I08",{"$nulls":29},{"$f":"IF(LEFT(AE102, 13) = \"CONSTRAINT PK\", AE102, \"\")","v":""}]
[27,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N102&\" \"","v":"soitsrltmacsrvhclmvmntowh_6 "},null," IS ",{"$f":"\"'\"&B102&\"'\"","v":"'[5분] 실시간 차량이동궤적 테이블(실측) - 6지역'"},";",null,null,null,""]
["TIBERO","soitsrltmacsrvhclmvmntowh_6\n(vehicle_history)","분석유닉스시각","anls_unix_tm",1,"NUMBER(10)","PK",null,"분석 대상기간 시작시각",{"$nulls":4},"분석유닉스시각","anls_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":10},"CREATE TABLE ",{"$f":"N102&\" (\"","v":"soitsrltmacsrvhclmvmntowh_6 ("},{"$f":"O104&\" \"","v":"anls_unix_tm "},{"$f":"R104&\" \"","v":"NUMBER(10) "},{"$f":"IF(H104=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",null,"(",{"$f":"IF(OR(G104=\"PK\", G104=\"PK/FK\"), O104, \"\")","v":"anls_unix_tm"},",","COMMENT ON COLUMN ",{"$f":"$N$102&\".\"","v":"soitsrltmacsrvhclmvmntowh_6."},{"$f":"O104","v":"anls_unix_tm"}," IS ",{"$f":"\"'\"&I104&\"'\"","v":"'분석 대상기간 시작시각'"},";",null,null,null,""]
[null,null,"위치수집유닉스시각","locn_clct_unix_tm",2,"NUMBER(10)","PK",null,"위치수집유닉스시각",{"$nulls":4},"위치수집유닉스시각","locn_clct_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":12},"locn_clct_unix_tm ","NUMBER(10) ","",",",null,null,"locn_clct_unix_tm",",","COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_6.","locn_clct_unix_tm"," IS ","'위치수집유닉스시각'",";",null,null,null,""]
[null,null,"차량ID","vhcl_id",3,"VARCHAR2(150)","PK",null,"차량ID",{"$nulls":4},"차량ID","vhcl_id","VARCHAR2(150)","VARCHAR(150)","VARCHAR2(150)",{"$nulls":12},"vhcl_id ","VARCHAR2(150) ","",",",null,null,"vhcl_id",")","COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_6.","vhcl_id"," IS ","'차량ID'",";",null,null,null,""]
[null,null,"차로ID","lane_id",4,"VARCHAR2(300)","FK",null,"통행차로ID",{"$nulls":4},"차로ID","lane_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",{"$nulls":12},"lane_id ","VARCHAR2(300) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_6.","lane_id"," IS ","'통행차로ID'",";",null,null,null,""]
[null,null,"세그먼트ID","sgmn_id",5,"VARCHAR2(300)","FK","NOT NULL","통행세그먼트ID",{"$nulls":4},"세그먼트ID","sgmn_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",{"$nulls":12},"sgmn_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_6.","sgmn_id"," IS ","'통행세그먼트ID'",";",null,null,null,""]
[null,null,"차종코드","kncr_cd",6,"CHAR(10)",null,null,"차종 (008)",{"$nulls":4},"차종코드","kncr_cd","CHAR(10)","VARCHAR(10)","VARCHAR2(10)",{"$nulls":12},"kncr_cd ","VARCHAR2(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_6.","kncr_cd"," IS ","'차종 (008)'",";",null,null,null,""]
[null,null,"순간속도","mmnt_sped",7,"NUMBER(5,2)",null,null,"순간속도 (m/s)",{"$nulls":4},"순간속도","mmnt_sped","NUMBER(5,2)","FLOAT","NUMBER(5,2)",{"$nulls":12},"mmnt_sped ","NUMBER(5,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_6.","mmnt_sped"," IS ","'순간속도 (m/s)'",";",null,null,null,"",{"$nulls":6},"FLOAT"]
[null,null,"비혼잡속도","non_cngt_sped",8,"NUMBER(5,2)",null,null,"비혼잡속도 (m/s)",{"$nulls":4},"비혼잡속도","non_cngt_sped","NUMBER(5,2)","FLOAT","NUMBER(5,2)",{"$nulls":12},"non_cngt_sped ","NUMBER(5,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_6.","non_cngt_sped"," IS ","'비혼잡속도 (m/s)'",";",null,null,null,"",{"$nulls":6},"FLOAT"]
[null,null,"차량경도","vhcl_lot",9,"NUMBER(13,10)",null,null,"차량경도",{"$nulls":4},"차량경도","vhcl_lot","NUMBER(13,10)","FLOAT","NUMBER(13,10)",{"$nulls":12},"vhcl_lot ","NUMBER(13,10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_6.","vhcl_lot"," IS ","'차량경도'",";",null,null,null,""]
[null,null,"차량위도","vhcl_lat",10,"NUMBER(12,10)",null,null,"차량위도",{"$nulls":4},"차량위도","vhcl_lat","NUMBER(12,10)","FLOAT","NUMBER(12,10)",{"$nulls":12},"vhcl_lat ","NUMBER(12,10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_6.","vhcl_lat"," IS ","'차량위도'",";",null,null,null,""]
[null,null,"차량고도","vhcl_lntd",11,"NUMBER(10)",null,null,"차량고도",{"$nulls":4},"차량고도","vhcl_lntd","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":12},"vhcl_lntd ","NUMBER(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_6.","vhcl_lntd"," IS ","'차량고도'",";",null,null,null,"",{"$nulls":6},"FLOAT"]
[null,null,"이동방위각도","mvmn_pocm_angl",12,"NUMBER(6,3)",null,null,"이동방위각도",{"$nulls":4},"이동방위각도","mvmn_pocm_angl","NUMBER(6,3)","FLOAT","NUMBER(6,3)",{"$nulls":12},"mvmn_pocm_angl ","NUMBER(6,3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_6.","mvmn_pocm_angl"," IS ","'이동방위각도'",";",null,null,null,""]
[null,null,"이동경사각도","mvmn_slop_angl",13,"NUMBER(6,3)",null,null,"이동경사각도",{"$nulls":4},"이동경사각도","mvmn_slop_angl","NUMBER(6,3)","FLOAT","NUMBER(6,3)",{"$nulls":12},"mvmn_slop_angl ","NUMBER(6,3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_6.","mvmn_slop_angl"," IS ","'이동경사각도'",";",null,null,null,""]
[null,null,"차로진행거리","lane_prgrs_dstn",14,"NUMBER(7,2)",null,null,"통행차로진행거리",{"$nulls":4},"차로진행거리","lane_prgrs_dstn","NUMBER(19,9)","FLOAT","NUMBER(19,9)",{"$nulls":12},"lane_prgrs_dstn ","NUMBER(19,9) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_6.","lane_prgrs_dstn"," IS ","'통행차로진행거리'",";",null,null,null,""]
[null,null,"대기행렬관측여부","queu_obsrvn_yn",15,"CHAR(1)",null,null,"대기행렬관측여부 (503)",{"$nulls":4},"대기행렬관측여부","queu_obsrvn_yn","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",{"$nulls":12},"queu_obsrvn_yn ","VARCHAR2(1) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_6.","queu_obsrvn_yn"," IS ","'대기행렬관측여부 (503)'",";",null,null,null,""]
[null,null,"지역구분코드","rgn_prttn_cd",16,"CHAR(2)","FK","NOT NULL","지역분할코드(051)",{"$nulls":4},"지역분할코드","rgn_prttn_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",{"$nulls":12},"rgn_prttn_cd ","VARCHAR2(2) ","NOT NULL",{"$f":"\") TABLESPACE \"&AI121&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_C006 NOLOGGING"},null,null,{"$f":"IF(OR(F119=\"PK\", F119=\"PK/FK\"), H119, \"\")","v":""},null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_6.","rgn_prttn_cd"," IS ","'지역분할코드(051)'",";"]
[{"$nulls":30},{"$f":"CONCATENATE(AI120:AK120)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (locn_clct_unix_tm) INTERVAL (3600) STORE IN (\"&AI121&\") (PARTITION BFR_\" & N102& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AI121&\");\"","v":"PARTITION BY RANGE (locn_clct_unix_tm) INTERVAL (3600) STORE IN (SOIT_D08_C006) (PARTITION BFR_soitsrltmacsrvhclmvmntowh_6_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_C006);"},{"$f":"\"CREATE INDEX PK_\" & N102& \" ON \" & N102 & CONCATENATE(AJ104:AL118) & \" LOCAL (PARTITION BFR_\" & N102 & \"_20221101 TABLESPACE \"&AJ121&\") TABLESPACE \"&AJ121&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & N102 & \" ADD CONSTRAINT PK_\" & N102 & \" PRIMARY KEY \" & CONCATENATE(AJ104:AL118) & \";\"","v":{"$error":"#VALUE!"}}]
[{"$nulls":34},"SOIT_D08_C006","SOIT_I08_C006"]
[null,"[5분] 실시간 차량이동궤적 테이블(실측) - 7지역",{"$nulls":11},"soitsrltmacsrvhclmvmntowh_7",null,null,"SOIT_D08_01","SOIT_I08",{"$nulls":29},{"$f":"IF(LEFT(AE122, 13) = \"CONSTRAINT PK\", AE122, \"\")","v":""}]
[27,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N122&\" \"","v":"soitsrltmacsrvhclmvmntowh_7 "},null," IS ",{"$f":"\"'\"&B122&\"'\"","v":"'[5분] 실시간 차량이동궤적 테이블(실측) - 7지역'"},";",null,null,null,""]
["TIBERO","soitsrltmacsrvhclmvmntowh_7\n(vehicle_history)","분석유닉스시각","anls_unix_tm",1,"NUMBER(10)","PK",null,"분석 대상기간 시작시각",{"$nulls":4},"분석유닉스시각","anls_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":10},"CREATE TABLE ",{"$f":"N122&\" (\"","v":"soitsrltmacsrvhclmvmntowh_7 ("},{"$f":"O124&\" \"","v":"anls_unix_tm "},{"$f":"R124&\" \"","v":"NUMBER(10) "},{"$f":"IF(H124=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",null,"(",{"$f":"IF(OR(G124=\"PK\", G124=\"PK/FK\"), O124, \"\")","v":"anls_unix_tm"},",","COMMENT ON COLUMN ",{"$f":"$N$122&\".\"","v":"soitsrltmacsrvhclmvmntowh_7."},{"$f":"O124","v":"anls_unix_tm"}," IS ",{"$f":"\"'\"&I124&\"'\"","v":"'분석 대상기간 시작시각'"},";",null,null,null,""]
[null,null,"위치수집유닉스시각","locn_clct_unix_tm",2,"NUMBER(10)","PK",null,"위치수집유닉스시각",{"$nulls":4},"위치수집유닉스시각","locn_clct_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":12},"locn_clct_unix_tm ","NUMBER(10) ","",",",null,null,"locn_clct_unix_tm",",","COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_7.","locn_clct_unix_tm"," IS ","'위치수집유닉스시각'",";",null,null,null,""]
[null,null,"차량ID","vhcl_id",3,"VARCHAR2(150)","PK",null,"차량ID",{"$nulls":4},"차량ID","vhcl_id","VARCHAR2(150)","VARCHAR(150)","VARCHAR2(150)",{"$nulls":12},"vhcl_id ","VARCHAR2(150) ","",",",null,null,"vhcl_id",")","COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_7.","vhcl_id"," IS ","'차량ID'",";",null,null,null,""]
[null,null,"차로ID","lane_id",4,"VARCHAR2(300)","FK",null,"통행차로ID",{"$nulls":4},"차로ID","lane_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",{"$nulls":12},"lane_id ","VARCHAR2(300) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_7.","lane_id"," IS ","'통행차로ID'",";",null,null,null,""]
[null,null,"세그먼트ID","sgmn_id",5,"VARCHAR2(300)","FK","NOT NULL","통행세그먼트ID",{"$nulls":4},"세그먼트ID","sgmn_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",{"$nulls":12},"sgmn_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_7.","sgmn_id"," IS ","'통행세그먼트ID'",";",null,null,null,""]
[null,null,"차종코드","kncr_cd",6,"CHAR(10)",null,null,"차종 (008)",{"$nulls":4},"차종코드","kncr_cd","CHAR(10)","VARCHAR(10)","VARCHAR2(10)",{"$nulls":12},"kncr_cd ","VARCHAR2(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_7.","kncr_cd"," IS ","'차종 (008)'",";",null,null,null,""]
[null,null,"순간속도","mmnt_sped",7,"NUMBER(5,2)",null,null,"순간속도 (m/s)",{"$nulls":4},"순간속도","mmnt_sped","NUMBER(5,2)","FLOAT","NUMBER(5,2)",{"$nulls":12},"mmnt_sped ","NUMBER(5,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_7.","mmnt_sped"," IS ","'순간속도 (m/s)'",";",null,null,null,"",{"$nulls":6},"FLOAT"]
[null,null,"비혼잡속도","non_cngt_sped",8,"NUMBER(5,2)",null,null,"비혼잡속도 (m/s)",{"$nulls":4},"비혼잡속도","non_cngt_sped","NUMBER(5,2)","FLOAT","NUMBER(5,2)",{"$nulls":12},"non_cngt_sped ","NUMBER(5,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_7.","non_cngt_sped"," IS ","'비혼잡속도 (m/s)'",";",null,null,null,"",{"$nulls":6},"FLOAT"]
[null,null,"차량경도","vhcl_lot",9,"NUMBER(13,10)",null,null,"차량경도",{"$nulls":4},"차량경도","vhcl_lot","NUMBER(13,10)","FLOAT","NUMBER(13,10)",{"$nulls":12},"vhcl_lot ","NUMBER(13,10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_7.","vhcl_lot"," IS ","'차량경도'",";",null,null,null,""]
[null,null,"차량위도","vhcl_lat",10,"NUMBER(12,10)",null,null,"차량위도",{"$nulls":4},"차량위도","vhcl_lat","NUMBER(12,10)","FLOAT","NUMBER(12,10)",{"$nulls":12},"vhcl_lat ","NUMBER(12,10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_7.","vhcl_lat"," IS ","'차량위도'",";",null,null,null,""]
[null,null,"차량고도","vhcl_lntd",11,"NUMBER(10)",null,null,"차량고도",{"$nulls":4},"차량고도","vhcl_lntd","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":12},"vhcl_lntd ","NUMBER(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_7.","vhcl_lntd"," IS ","'차량고도'",";",null,null,null,"",{"$nulls":6},"FLOAT"]
[null,null,"이동방위각도","mvmn_pocm_angl",12,"NUMBER(6,3)",null,null,"이동방위각도",{"$nulls":4},"이동방위각도","mvmn_pocm_angl","NUMBER(6,3)","FLOAT","NUMBER(6,3)",{"$nulls":12},"mvmn_pocm_angl ","NUMBER(6,3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_7.","mvmn_pocm_angl"," IS ","'이동방위각도'",";",null,null,null,""]
[null,null,"이동경사각도","mvmn_slop_angl",13,"NUMBER(6,3)",null,null,"이동경사각도",{"$nulls":4},"이동경사각도","mvmn_slop_angl","NUMBER(6,3)","FLOAT","NUMBER(6,3)",{"$nulls":12},"mvmn_slop_angl ","NUMBER(6,3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_7.","mvmn_slop_angl"," IS ","'이동경사각도'",";",null,null,null,""]
[null,null,"차로진행거리","lane_prgrs_dstn",14,"NUMBER(7,2)",null,null,"통행차로진행거리",{"$nulls":4},"차로진행거리","lane_prgrs_dstn","NUMBER(19,9)","FLOAT","NUMBER(19,9)",{"$nulls":12},"lane_prgrs_dstn ","NUMBER(19,9) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_7.","lane_prgrs_dstn"," IS ","'통행차로진행거리'",";",null,null,null,""]
[null,null,"대기행렬관측여부","queu_obsrvn_yn",15,"CHAR(1)",null,null,"대기행렬관측여부 (503)",{"$nulls":4},"대기행렬관측여부","queu_obsrvn_yn","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",{"$nulls":12},"queu_obsrvn_yn ","VARCHAR2(1) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_7.","queu_obsrvn_yn"," IS ","'대기행렬관측여부 (503)'",";",null,null,null,""]
[null,null,"지역구분코드","rgn_prttn_cd",16,"CHAR(2)","FK","NOT NULL","지역분할코드(051)",{"$nulls":4},"지역분할코드","rgn_prttn_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",{"$nulls":12},"rgn_prttn_cd ","VARCHAR2(2) ","NOT NULL",{"$f":"\") TABLESPACE \"&AI141&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_C007 NOLOGGING"},null,null,{"$f":"IF(OR(F139=\"PK\", F139=\"PK/FK\"), H139, \"\")","v":""},null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_7.","rgn_prttn_cd"," IS ","'지역분할코드(051)'",";"]
[{"$nulls":30},{"$f":"CONCATENATE(AI140:AK140)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (locn_clct_unix_tm) INTERVAL (3600) STORE IN (\"&AI141&\") (PARTITION BFR_\" & N122& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AI141&\");\"","v":"PARTITION BY RANGE (locn_clct_unix_tm) INTERVAL (3600) STORE IN (SOIT_D08_C007) (PARTITION BFR_soitsrltmacsrvhclmvmntowh_7_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_C007);"},{"$f":"\"CREATE INDEX PK_\" & N122& \" ON \" & N122 & CONCATENATE(AJ124:AL138) & \" LOCAL (PARTITION BFR_\" & N122 & \"_20221101 TABLESPACE \"&AJ141&\") TABLESPACE \"&AJ141&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & N122 & \" ADD CONSTRAINT PK_\" & N122 & \" PRIMARY KEY \" & CONCATENATE(AJ124:AL138) & \";\"","v":{"$error":"#VALUE!"}}]
[{"$nulls":34},"SOIT_D08_C007","SOIT_I08_C007"]
[null,"[5분] 실시간 차량이동궤적 테이블(실측) - 8지역",{"$nulls":11},"soitsrltmacsrvhclmvmntowh_8",null,null,"SOIT_D08_01","SOIT_I08",{"$nulls":29},{"$f":"IF(LEFT(AE142, 13) = \"CONSTRAINT PK\", AE142, \"\")","v":""}]
[27,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N142&\" \"","v":"soitsrltmacsrvhclmvmntowh_8 "},null," IS ",{"$f":"\"'\"&B142&\"'\"","v":"'[5분] 실시간 차량이동궤적 테이블(실측) - 8지역'"},";",null,null,null,""]
["TIBERO","soitsrltmacsrvhclmvmntowh_8\n(vehicle_history)","분석유닉스시각","anls_unix_tm",1,"NUMBER(10)","PK",null,"분석 대상기간 시작시각",{"$nulls":4},"분석유닉스시각","anls_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":10},"CREATE TABLE ",{"$f":"N142&\" (\"","v":"soitsrltmacsrvhclmvmntowh_8 ("},{"$f":"O144&\" \"","v":"anls_unix_tm "},{"$f":"R144&\" \"","v":"NUMBER(10) "},{"$f":"IF(H144=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",null,"(",{"$f":"IF(OR(G144=\"PK\", G144=\"PK/FK\"), O144, \"\")","v":"anls_unix_tm"},",","COMMENT ON COLUMN ",{"$f":"$N$142&\".\"","v":"soitsrltmacsrvhclmvmntowh_8."},{"$f":"O144","v":"anls_unix_tm"}," IS ",{"$f":"\"'\"&I144&\"'\"","v":"'분석 대상기간 시작시각'"},";",null,null,null,""]
[null,null,"위치수집유닉스시각","locn_clct_unix_tm",2,"NUMBER(10)","PK",null,"위치수집유닉스시각",{"$nulls":4},"위치수집유닉스시각","locn_clct_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":12},"locn_clct_unix_tm ","NUMBER(10) ","",",",null,null,"locn_clct_unix_tm",",","COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_8.","locn_clct_unix_tm"," IS ","'위치수집유닉스시각'",";",null,null,null,""]
[null,null,"차량ID","vhcl_id",3,"VARCHAR2(150)","PK",null,"차량ID",{"$nulls":4},"차량ID","vhcl_id","VARCHAR2(150)","VARCHAR(150)","VARCHAR2(150)",{"$nulls":12},"vhcl_id ","VARCHAR2(150) ","",",",null,null,"vhcl_id",")","COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_8.","vhcl_id"," IS ","'차량ID'",";",null,null,null,""]
[null,null,"차로ID","lane_id",4,"VARCHAR2(300)","FK",null,"통행차로ID",{"$nulls":4},"차로ID","lane_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",{"$nulls":12},"lane_id ","VARCHAR2(300) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_8.","lane_id"," IS ","'통행차로ID'",";",null,null,null,""]
[null,null,"세그먼트ID","sgmn_id",5,"VARCHAR2(300)","FK","NOT NULL","통행세그먼트ID",{"$nulls":4},"세그먼트ID","sgmn_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",{"$nulls":12},"sgmn_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_8.","sgmn_id"," IS ","'통행세그먼트ID'",";",null,null,null,""]
[null,null,"차종코드","kncr_cd",6,"CHAR(10)",null,null,"차종 (008)",{"$nulls":4},"차종코드","kncr_cd","CHAR(10)","VARCHAR(10)","VARCHAR2(10)",{"$nulls":12},"kncr_cd ","VARCHAR2(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_8.","kncr_cd"," IS ","'차종 (008)'",";",null,null,null,""]
[null,null,"순간속도","mmnt_sped",7,"NUMBER(5,2)",null,null,"순간속도 (m/s)",{"$nulls":4},"순간속도","mmnt_sped","NUMBER(5,2)","FLOAT","NUMBER(5,2)",{"$nulls":12},"mmnt_sped ","NUMBER(5,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_8.","mmnt_sped"," IS ","'순간속도 (m/s)'",";",null,null,null,"",{"$nulls":6},"FLOAT"]
[null,null,"비혼잡속도","non_cngt_sped",8,"NUMBER(5,2)",null,null,"비혼잡속도 (m/s)",{"$nulls":4},"비혼잡속도","non_cngt_sped","NUMBER(5,2)","FLOAT","NUMBER(5,2)",{"$nulls":12},"non_cngt_sped ","NUMBER(5,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_8.","non_cngt_sped"," IS ","'비혼잡속도 (m/s)'",";",null,null,null,"",{"$nulls":6},"FLOAT"]
[null,null,"차량경도","vhcl_lot",9,"NUMBER(13,10)",null,null,"차량경도",{"$nulls":4},"차량경도","vhcl_lot","NUMBER(13,10)","FLOAT","NUMBER(13,10)",{"$nulls":12},"vhcl_lot ","NUMBER(13,10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_8.","vhcl_lot"," IS ","'차량경도'",";",null,null,null,""]
[null,null,"차량위도","vhcl_lat",10,"NUMBER(12,10)",null,null,"차량위도",{"$nulls":4},"차량위도","vhcl_lat","NUMBER(12,10)","FLOAT","NUMBER(12,10)",{"$nulls":12},"vhcl_lat ","NUMBER(12,10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_8.","vhcl_lat"," IS ","'차량위도'",";",null,null,null,""]
[null,null,"차량고도","vhcl_lntd",11,"NUMBER(10)",null,null,"차량고도",{"$nulls":4},"차량고도","vhcl_lntd","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":12},"vhcl_lntd ","NUMBER(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_8.","vhcl_lntd"," IS ","'차량고도'",";",null,null,null,"",{"$nulls":6},"FLOAT"]
[null,null,"이동방위각도","mvmn_pocm_angl",12,"NUMBER(6,3)",null,null,"이동방위각도",{"$nulls":4},"이동방위각도","mvmn_pocm_angl","NUMBER(6,3)","FLOAT","NUMBER(6,3)",{"$nulls":12},"mvmn_pocm_angl ","NUMBER(6,3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_8.","mvmn_pocm_angl"," IS ","'이동방위각도'",";",null,null,null,""]
[null,null,"이동경사각도","mvmn_slop_angl",13,"NUMBER(6,3)",null,null,"이동경사각도",{"$nulls":4},"이동경사각도","mvmn_slop_angl","NUMBER(6,3)","FLOAT","NUMBER(6,3)",{"$nulls":12},"mvmn_slop_angl ","NUMBER(6,3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_8.","mvmn_slop_angl"," IS ","'이동경사각도'",";",null,null,null,""]
[null,null,"차로진행거리","lane_prgrs_dstn",14,"NUMBER(7,2)",null,null,"통행차로진행거리",{"$nulls":4},"차로진행거리","lane_prgrs_dstn","NUMBER(19,9)","FLOAT","NUMBER(19,9)",{"$nulls":12},"lane_prgrs_dstn ","NUMBER(19,9) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_8.","lane_prgrs_dstn"," IS ","'통행차로진행거리'",";",null,null,null,""]
[null,null,"대기행렬관측여부","queu_obsrvn_yn",15,"CHAR(1)",null,null,"대기행렬관측여부 (503)",{"$nulls":4},"대기행렬관측여부","queu_obsrvn_yn","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",{"$nulls":12},"queu_obsrvn_yn ","VARCHAR2(1) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_8.","queu_obsrvn_yn"," IS ","'대기행렬관측여부 (503)'",";",null,null,null,""]
[null,null,"지역구분코드","rgn_prttn_cd",16,"CHAR(2)","FK","NOT NULL","지역분할코드(051)",{"$nulls":4},"지역분할코드","rgn_prttn_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",{"$nulls":12},"rgn_prttn_cd ","VARCHAR2(2) ","NOT NULL",{"$f":"\") TABLESPACE \"&AI161&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_C008 NOLOGGING"},null,null,{"$f":"IF(OR(F159=\"PK\", F159=\"PK/FK\"), H159, \"\")","v":""},null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_8.","rgn_prttn_cd"," IS ","'지역분할코드(051)'",";"]
[{"$nulls":30},{"$f":"CONCATENATE(AI160:AK160)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (locn_clct_unix_tm) INTERVAL (3600) STORE IN (\"&AI161&\") (PARTITION BFR_\" & N142& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AI161&\");\"","v":"PARTITION BY RANGE (locn_clct_unix_tm) INTERVAL (3600) STORE IN (SOIT_D08_C008) (PARTITION BFR_soitsrltmacsrvhclmvmntowh_8_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_C008);"},{"$f":"\"CREATE INDEX PK_\" & N142& \" ON \" & N142 & CONCATENATE(AJ144:AL158) & \" LOCAL (PARTITION BFR_\" & N142 & \"_20221101 TABLESPACE \"&AJ161&\") TABLESPACE \"&AJ161&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & N142 & \" ADD CONSTRAINT PK_\" & N142 & \" PRIMARY KEY \" & CONCATENATE(AJ144:AL158) & \";\"","v":{"$error":"#VALUE!"}}]
[{"$nulls":34},"SOIT_D08_C008","SOIT_I08_C008"]
[null,"[5분] 실시간 차량이동궤적 테이블(실측) - 9지역",{"$nulls":11},"soitsrltmacsrvhclmvmntowh_9",null,null,"SOIT_D08_01","SOIT_I08",{"$nulls":29},{"$f":"IF(LEFT(AE162, 13) = \"CONSTRAINT PK\", AE162, \"\")","v":""}]
[27,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N162&\" \"","v":"soitsrltmacsrvhclmvmntowh_9 "},null," IS ",{"$f":"\"'\"&B162&\"'\"","v":"'[5분] 실시간 차량이동궤적 테이블(실측) - 9지역'"},";",null,null,null,""]
["TIBERO","soitsrltmacsrvhclmvmntowh_9\n(vehicle_history)","분석유닉스시각","anls_unix_tm",1,"NUMBER(10)","PK",null,"분석 대상기간 시작시각",{"$nulls":4},"분석유닉스시각","anls_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":10},"CREATE TABLE ",{"$f":"N162&\" (\"","v":"soitsrltmacsrvhclmvmntowh_9 ("},{"$f":"O164&\" \"","v":"anls_unix_tm "},{"$f":"R164&\" \"","v":"NUMBER(10) "},{"$f":"IF(H164=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",null,"(",{"$f":"IF(OR(G164=\"PK\", G164=\"PK/FK\"), O164, \"\")","v":"anls_unix_tm"},",","COMMENT ON COLUMN ",{"$f":"$N$162&\".\"","v":"soitsrltmacsrvhclmvmntowh_9."},{"$f":"O164","v":"anls_unix_tm"}," IS ",{"$f":"\"'\"&I164&\"'\"","v":"'분석 대상기간 시작시각'"},";",null,null,null,""]
[null,null,"위치수집유닉스시각","locn_clct_unix_tm",2,"NUMBER(10)","PK",null,"위치수집유닉스시각",{"$nulls":4},"위치수집유닉스시각","locn_clct_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":12},"locn_clct_unix_tm ","NUMBER(10) ","",",",null,null,"locn_clct_unix_tm",",","COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_9.","locn_clct_unix_tm"," IS ","'위치수집유닉스시각'",";",null,null,null,""]
[null,null,"차량ID","vhcl_id",3,"VARCHAR2(150)","PK",null,"차량ID",{"$nulls":4},"차량ID","vhcl_id","VARCHAR2(150)","VARCHAR(150)","VARCHAR2(150)",{"$nulls":12},"vhcl_id ","VARCHAR2(150) ","",",",null,null,"vhcl_id",")","COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_9.","vhcl_id"," IS ","'차량ID'",";",null,null,null,""]
[null,null,"차로ID","lane_id",4,"VARCHAR2(300)","FK",null,"통행차로ID",{"$nulls":4},"차로ID","lane_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",{"$nulls":12},"lane_id ","VARCHAR2(300) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_9.","lane_id"," IS ","'통행차로ID'",";",null,null,null,""]
[null,null,"세그먼트ID","sgmn_id",5,"VARCHAR2(300)","FK","NOT NULL","통행세그먼트ID",{"$nulls":4},"세그먼트ID","sgmn_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",{"$nulls":12},"sgmn_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_9.","sgmn_id"," IS ","'통행세그먼트ID'",";",null,null,null,""]
[null,null,"차종코드","kncr_cd",6,"CHAR(10)",null,null,"차종 (008)",{"$nulls":4},"차종코드","kncr_cd","CHAR(10)","VARCHAR(10)","VARCHAR2(10)",{"$nulls":12},"kncr_cd ","VARCHAR2(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_9.","kncr_cd"," IS ","'차종 (008)'",";",null,null,null,""]
[null,null,"순간속도","mmnt_sped",7,"NUMBER(5,2)",null,null,"순간속도 (m/s)",{"$nulls":4},"순간속도","mmnt_sped","NUMBER(5,2)","FLOAT","NUMBER(5,2)",{"$nulls":12},"mmnt_sped ","NUMBER(5,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_9.","mmnt_sped"," IS ","'순간속도 (m/s)'",";",null,null,null,"",{"$nulls":6},"FLOAT"]
[null,null,"비혼잡속도","non_cngt_sped",8,"NUMBER(5,2)",null,null,"비혼잡속도 (m/s)",{"$nulls":4},"비혼잡속도","non_cngt_sped","NUMBER(5,2)","FLOAT","NUMBER(5,2)",{"$nulls":12},"non_cngt_sped ","NUMBER(5,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_9.","non_cngt_sped"," IS ","'비혼잡속도 (m/s)'",";",null,null,null,"",{"$nulls":6},"FLOAT"]
[null,null,"차량경도","vhcl_lot",9,"NUMBER(13,10)",null,null,"차량경도",{"$nulls":4},"차량경도","vhcl_lot","NUMBER(13,10)","FLOAT","NUMBER(13,10)",{"$nulls":12},"vhcl_lot ","NUMBER(13,10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_9.","vhcl_lot"," IS ","'차량경도'",";",null,null,null,""]
[null,null,"차량위도","vhcl_lat",10,"NUMBER(12,10)",null,null,"차량위도",{"$nulls":4},"차량위도","vhcl_lat","NUMBER(12,10)","FLOAT","NUMBER(12,10)",{"$nulls":12},"vhcl_lat ","NUMBER(12,10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_9.","vhcl_lat"," IS ","'차량위도'",";",null,null,null,""]
[null,null,"차량고도","vhcl_lntd",11,"NUMBER(10)",null,null,"차량고도",{"$nulls":4},"차량고도","vhcl_lntd","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":12},"vhcl_lntd ","NUMBER(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_9.","vhcl_lntd"," IS ","'차량고도'",";",null,null,null,"",{"$nulls":6},"FLOAT"]
[null,null,"이동방위각도","mvmn_pocm_angl",12,"NUMBER(6,3)",null,null,"이동방위각도",{"$nulls":4},"이동방위각도","mvmn_pocm_angl","NUMBER(6,3)","FLOAT","NUMBER(6,3)",{"$nulls":12},"mvmn_pocm_angl ","NUMBER(6,3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_9.","mvmn_pocm_angl"," IS ","'이동방위각도'",";",null,null,null,""]
[null,null,"이동경사각도","mvmn_slop_angl",13,"NUMBER(6,3)",null,null,"이동경사각도",{"$nulls":4},"이동경사각도","mvmn_slop_angl","NUMBER(6,3)","FLOAT","NUMBER(6,3)",{"$nulls":12},"mvmn_slop_angl ","NUMBER(6,3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_9.","mvmn_slop_angl"," IS ","'이동경사각도'",";",null,null,null,""]
[null,null,"차로진행거리","lane_prgrs_dstn",14,"NUMBER(7,2)",null,null,"통행차로진행거리",{"$nulls":4},"차로진행거리","lane_prgrs_dstn","NUMBER(19,9)","FLOAT","NUMBER(19,9)",{"$nulls":12},"lane_prgrs_dstn ","NUMBER(19,9) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_9.","lane_prgrs_dstn"," IS ","'통행차로진행거리'",";",null,null,null,""]
[null,null,"대기행렬관측여부","queu_obsrvn_yn",15,"CHAR(1)",null,null,"대기행렬관측여부 (503)",{"$nulls":4},"대기행렬관측여부","queu_obsrvn_yn","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",{"$nulls":12},"queu_obsrvn_yn ","VARCHAR2(1) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_9.","queu_obsrvn_yn"," IS ","'대기행렬관측여부 (503)'",";",null,null,null,""]
[null,null,"지역구분코드","rgn_prttn_cd",16,"CHAR(2)","FK","NOT NULL","지역분할코드(051)",{"$nulls":4},"지역분할코드","rgn_prttn_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",{"$nulls":12},"rgn_prttn_cd ","VARCHAR2(2) ","NOT NULL",{"$f":"\") TABLESPACE \"&AI181&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_C009 NOLOGGING"},null,null,{"$f":"IF(OR(F179=\"PK\", F179=\"PK/FK\"), H179, \"\")","v":""},null,"COMMENT ON COLUMN ","soitsrltmacsrvhclmvmntowh_9.","rgn_prttn_cd"," IS ","'지역분할코드(051)'",";"]
[{"$nulls":30},{"$f":"CONCATENATE(AI180:AK180)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (locn_clct_unix_tm) INTERVAL (3600) STORE IN (\"&AI181&\") (PARTITION BFR_\" & N162& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AI181&\");\"","v":"PARTITION BY RANGE (locn_clct_unix_tm) INTERVAL (3600) STORE IN (SOIT_D08_C009) (PARTITION BFR_soitsrltmacsrvhclmvmntowh_9_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_C009);"},{"$f":"\"CREATE INDEX PK_\" & N162& \" ON \" & N162 & CONCATENATE(AJ164:AL178) & \" LOCAL (PARTITION BFR_\" & N162 & \"_20221101 TABLESPACE \"&AJ181&\") TABLESPACE \"&AJ181&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & N162 & \" ADD CONSTRAINT PK_\" & N162 & \" PRIMARY KEY \" & CONCATENATE(AJ164:AL178) & \";\"","v":{"$error":"#VALUE!"}}]
[{"$nulls":34},"SOIT_D08_C009","SOIT_I08_C009"]
[null,"[5분] 실시간 차량이동궤적 테이블(예측) - 1지역",{"$nulls":11},"soitsrltmprdtvhclmvmntowh_1",{"$nulls":33},{"$f":"IF(LEFT(AE182, 13) = \"CONSTRAINT PK\", AE182, \"\")","v":""}]
[27,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N182&\" \"","v":"soitsrltmprdtvhclmvmntowh_1 "},null," IS ",{"$f":"\"'\"&B182&\"'\"","v":"'[5분] 실시간 차량이동궤적 테이블(예측) - 1지역'"},";",null,null,null,""]
["TIBERO","soitsrltmprdtvhclmvmntowh_1\n(vehicle_history)","분석유닉스시각","anls_unix_tm",1,"NUMBER(10)","PK",null,"분석 대상기간 시작시각",{"$nulls":4},"분석유닉스시각","anls_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":10},"CREATE TABLE ",{"$f":"N182&\" (\"","v":"soitsrltmprdtvhclmvmntowh_1 ("},{"$f":"O184&\" \"","v":"anls_unix_tm "},{"$f":"R184&\" \"","v":"NUMBER(10) "},{"$f":"IF(H184=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",null,"(",{"$f":"IF(OR(G184=\"PK\", G184=\"PK/FK\"), O184, \"\")","v":"anls_unix_tm"},",","COMMENT ON COLUMN ",{"$f":"$N$182&\".\"","v":"soitsrltmprdtvhclmvmntowh_1."},{"$f":"O184","v":"anls_unix_tm"}," IS ",{"$f":"\"'\"&I184&\"'\"","v":"'분석 대상기간 시작시각'"},";",null,null,null,""]
[null,null,"위치수집유닉스시각","locn_clct_unix_tm",2,"NUMBER(10)","PK",null,"위치수집유닉스시각",{"$nulls":4},"위치수집유닉스시각","locn_clct_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":12},"locn_clct_unix_tm ","NUMBER(10) ","",",",null,null,"locn_clct_unix_tm",",","COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_1.","locn_clct_unix_tm"," IS ","'위치수집유닉스시각'",";"]
[null,null,"차량ID","vhcl_id",4,"VARCHAR2(150)","PK",null,"차량ID",{"$nulls":4},"차량ID","vhcl_id","VARCHAR2(150)","VARCHAR(150)","VARCHAR2(150)",{"$nulls":12},"vhcl_id ","VARCHAR2(150) ","",",",null,null,"vhcl_id",")","COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_1.","vhcl_id"," IS ","'차량ID'",";"]
[null,null,"차로ID","lane_id",5,"VARCHAR2(300)","FK",null,"통행차로ID",{"$nulls":4},"차로ID","lane_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",{"$nulls":12},"lane_id ","VARCHAR2(300) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_1.","lane_id"," IS ","'통행차로ID'",";",null,null,null,{"$f":"IF(LEFT(AE187, 13) = \"CONSTRAINT PK\", AE187, \"\")","v":""}]
[null,null,"세그먼트ID","sgmn_id",6,"VARCHAR2(300)","FK","NOT NULL","통행세그먼트ID",{"$nulls":4},"세그먼트ID","sgmn_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",{"$nulls":12},"sgmn_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_1.","sgmn_id"," IS ","'통행세그먼트ID'",";"]
[null,null,"차종코드","kncr_cd",7,"CHAR(10)",null,null,"차종 (008)",{"$nulls":4},"차종코드","kncr_cd","CHAR(10)","VARCHAR(10)","VARCHAR2(10)",{"$nulls":12},"kncr_cd ","VARCHAR2(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_1.","kncr_cd"," IS ","'차종 (008)'",";"]
[null,null,"순간속도","mmnt_sped",8,"NUMBER(5,2)",null,null,"순간속도 (m/s)",{"$nulls":4},"순간속도","mmnt_sped","NUMBER(5,2)","FLOAT","NUMBER(5,2)",{"$nulls":12},"mmnt_sped ","NUMBER(5,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_1.","mmnt_sped"," IS ","'순간속도 (m/s)'",";"]
[null,null,"비혼잡속도","non_cngt_sped",9,"NUMBER(5,2)",null,null,"비혼잡속도 (m/s)",{"$nulls":4},"비혼잡속도","non_cngt_sped","NUMBER(5,2)","FLOAT","NUMBER(5,2)",{"$nulls":12},"non_cngt_sped ","NUMBER(5,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_1.","non_cngt_sped"," IS ","'비혼잡속도 (m/s)'",";"]
[null,null,"차량경도","vhcl_lot",10,"NUMBER(13,10)",null,null,"차량경도",{"$nulls":4},"차량경도","vhcl_lot","NUMBER(13,10)","FLOAT","NUMBER(13,10)",{"$nulls":12},"vhcl_lot ","NUMBER(13,10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_1.","vhcl_lot"," IS ","'차량경도'",";"]
[null,null,"차량위도","vhcl_lat",11,"NUMBER(12,10)",null,null,"차량위도",{"$nulls":4},"차량위도","vhcl_lat","NUMBER(12,10)","FLOAT","NUMBER(12,10)",{"$nulls":12},"vhcl_lat ","NUMBER(12,10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_1.","vhcl_lat"," IS ","'차량위도'",";"]
[null,null,"차량고도","vhcl_lntd",12,"NUMBER(10)",null,null,"차량고도",{"$nulls":4},"차량고도","vhcl_lntd","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":12},"vhcl_lntd ","NUMBER(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_1.","vhcl_lntd"," IS ","'차량고도'",";"]
[null,null,"이동방위각도","mvmn_pocm_angl",13,"NUMBER(6,3)",null,null,"이동방위각도",{"$nulls":4},"이동방위각도","mvmn_pocm_angl","NUMBER(6,3)","FLOAT","NUMBER(6,3)",{"$nulls":12},"mvmn_pocm_angl ","NUMBER(6,3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_1.","mvmn_pocm_angl"," IS ","'이동방위각도'",";"]
[null,null,"이동경사각도","mvmn_slop_angl",14,"NUMBER(6,3)",null,null,"이동경사각도",{"$nulls":4},"이동경사각도","mvmn_slop_angl","NUMBER(6,3)","FLOAT","NUMBER(6,3)",{"$nulls":12},"mvmn_slop_angl ","NUMBER(6,3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_1.","mvmn_slop_angl"," IS ","'이동경사각도'",";"]
[null,null,"차로진행거리","lane_prgrs_dstn",15,"NUMBER(7,2)",null,null,"통행차로진행거리",{"$nulls":4},"차로진행거리","lane_prgrs_dstn","NUMBER(19,9)","FLOAT","NUMBER(19,9)",{"$nulls":12},"lane_prgrs_dstn ","NUMBER(19,9) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_1.","lane_prgrs_dstn"," IS ","'통행차로진행거리'",";"]
[null,null,"대기행렬관측여부","queu_obsrvn_yn",16,"CHAR(1)",null,null,"대기행렬관측여부 (503)",{"$nulls":4},"대기행렬관측여부","queu_obsrvn_yn","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",{"$nulls":12},"queu_obsrvn_yn ","VARCHAR2(1) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_1.","queu_obsrvn_yn"," IS ","'대기행렬관측여부 (503)'",";"]
[null,null,"지역구분코드","rgn_prttn_cd",17,"CHAR(2)","FK","NOT NULL","지역분할코드(051)",{"$nulls":4},"지역분할코드","rgn_prttn_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",{"$nulls":12},"rgn_prttn_cd ","VARCHAR2(2) ","NOT NULL",{"$f":"\") TABLESPACE \"&AI201&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_C001 NOLOGGING"},null,null,{"$f":"IF(OR(F199=\"PK\", F199=\"PK/FK\"), H199, \"\")","v":""},null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_1.","rgn_prttn_cd"," IS ","'지역분할코드(051)'",";"]
[{"$nulls":30},{"$f":"CONCATENATE(AI200:AK200)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (locn_clct_unix_tm) INTERVAL (3600) STORE IN (\"&AI201&\") (PARTITION BFR_\" & N182& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AI201&\");\"","v":"PARTITION BY RANGE (locn_clct_unix_tm) INTERVAL (3600) STORE IN (SOIT_D08_C001) (PARTITION BFR_soitsrltmprdtvhclmvmntowh_1_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_C001);"},{"$f":"\"CREATE INDEX PK_\" & N182& \" ON \" & N182 & CONCATENATE(AJ184:AL198) & \" LOCAL (PARTITION BFR_\" & N182 & \"_20221101 TABLESPACE \"&AJ201&\") TABLESPACE \"&AJ201&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & N182 & \" ADD CONSTRAINT PK_\" & N182 & \" PRIMARY KEY \" & CONCATENATE(AJ184:AL198) & \";\"","v":{"$error":"#VALUE!"}}]
[{"$nulls":34},"SOIT_D08_C001","SOIT_I08_C001"]
[null,"[5분] 실시간 차량이동궤적 테이블(예측) - 2지역",{"$nulls":11},"soitsrltmprdtvhclmvmntowh_2",{"$nulls":33},{"$f":"IF(LEFT(AE202, 13) = \"CONSTRAINT PK\", AE202, \"\")","v":""}]
[27,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N202&\" \"","v":"soitsrltmprdtvhclmvmntowh_2 "},null," IS ",{"$f":"\"'\"&B202&\"'\"","v":"'[5분] 실시간 차량이동궤적 테이블(예측) - 2지역'"},";",null,null,null,""]
["TIBERO","soitsrltmprdtvhclmvmntowh_2\n(vehicle_history","분석유닉스시각","anls_unix_tm",1,"NUMBER(10)","PK",null,"분석 대상기간 시작시각",{"$nulls":4},"분석유닉스시각","anls_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":10},"CREATE TABLE ",{"$f":"N202&\" (\"","v":"soitsrltmprdtvhclmvmntowh_2 ("},{"$f":"O204&\" \"","v":"anls_unix_tm "},{"$f":"R204&\" \"","v":"NUMBER(10) "},{"$f":"IF(H204=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",null,"(",{"$f":"IF(OR(G204=\"PK\", G204=\"PK/FK\"), O204, \"\")","v":"anls_unix_tm"},",","COMMENT ON COLUMN ",{"$f":"$N$202&\".\"","v":"soitsrltmprdtvhclmvmntowh_2."},{"$f":"O204","v":"anls_unix_tm"}," IS ",{"$f":"\"'\"&I204&\"'\"","v":"'분석 대상기간 시작시각'"},";",null,null,null,""]
[null,null,"위치수집유닉스시각","locn_clct_unix_tm",2,"NUMBER(10)","PK",null,"위치수집유닉스시각",{"$nulls":4},"위치수집유닉스시각","locn_clct_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":12},"locn_clct_unix_tm ","NUMBER(10) ","",",",null,null,"locn_clct_unix_tm",",","COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_2.","locn_clct_unix_tm"," IS ","'위치수집유닉스시각'",";"]
[null,null,"차량ID","vhcl_id",4,"VARCHAR2(150)","PK",null,"차량ID",{"$nulls":4},"차량ID","vhcl_id","VARCHAR2(150)","VARCHAR(150)","VARCHAR2(150)",{"$nulls":12},"vhcl_id ","VARCHAR2(150) ","",",",null,null,"vhcl_id",")","COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_2.","vhcl_id"," IS ","'차량ID'",";"]
[null,null,"차로ID","lane_id",5,"VARCHAR2(300)","FK",null,"통행차로ID",{"$nulls":4},"차로ID","lane_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",{"$nulls":12},"lane_id ","VARCHAR2(300) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_2.","lane_id"," IS ","'통행차로ID'",";",null,null,null,{"$f":"IF(LEFT(AE207, 13) = \"CONSTRAINT PK\", AE207, \"\")","v":""}]
[null,null,"세그먼트ID","sgmn_id",6,"VARCHAR2(300)","FK","NOT NULL","통행세그먼트ID",{"$nulls":4},"세그먼트ID","sgmn_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",{"$nulls":12},"sgmn_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_2.","sgmn_id"," IS ","'통행세그먼트ID'",";"]
[null,null,"차종코드","kncr_cd",7,"CHAR(10)",null,null,"차종 (008)",{"$nulls":4},"차종코드","kncr_cd","CHAR(10)","VARCHAR(10)","VARCHAR2(10)",{"$nulls":12},"kncr_cd ","VARCHAR2(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_2.","kncr_cd"," IS ","'차종 (008)'",";"]
[null,null,"순간속도","mmnt_sped",8,"NUMBER(5,2)",null,null,"순간속도 (m/s)",{"$nulls":4},"순간속도","mmnt_sped","NUMBER(5,2)","FLOAT","NUMBER(5,2)",{"$nulls":12},"mmnt_sped ","NUMBER(5,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_2.","mmnt_sped"," IS ","'순간속도 (m/s)'",";"]
[null,null,"비혼잡속도","non_cngt_sped",9,"NUMBER(5,2)",null,null,"비혼잡속도 (m/s)",{"$nulls":4},"비혼잡속도","non_cngt_sped","NUMBER(5,2)","FLOAT","NUMBER(5,2)",{"$nulls":12},"non_cngt_sped ","NUMBER(5,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_2.","non_cngt_sped"," IS ","'비혼잡속도 (m/s)'",";"]
[null,null,"차량경도","vhcl_lot",10,"NUMBER(13,10)",null,null,"차량경도",{"$nulls":4},"차량경도","vhcl_lot","NUMBER(13,10)","FLOAT","NUMBER(13,10)",{"$nulls":12},"vhcl_lot ","NUMBER(13,10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_2.","vhcl_lot"," IS ","'차량경도'",";"]
[null,null,"차량위도","vhcl_lat",11,"NUMBER(12,10)",null,null,"차량위도",{"$nulls":4},"차량위도","vhcl_lat","NUMBER(12,10)","FLOAT","NUMBER(12,10)",{"$nulls":12},"vhcl_lat ","NUMBER(12,10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_2.","vhcl_lat"," IS ","'차량위도'",";"]
[null,null,"차량고도","vhcl_lntd",12,"NUMBER(10)",null,null,"차량고도",{"$nulls":4},"차량고도","vhcl_lntd","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":12},"vhcl_lntd ","NUMBER(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_2.","vhcl_lntd"," IS ","'차량고도'",";"]
[null,null,"이동방위각도","mvmn_pocm_angl",13,"NUMBER(6,3)",null,null,"이동방위각도",{"$nulls":4},"이동방위각도","mvmn_pocm_angl","NUMBER(6,3)","FLOAT","NUMBER(6,3)",{"$nulls":12},"mvmn_pocm_angl ","NUMBER(6,3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_2.","mvmn_pocm_angl"," IS ","'이동방위각도'",";"]
[null,null,"이동경사각도","mvmn_slop_angl",14,"NUMBER(6,3)",null,null,"이동경사각도",{"$nulls":4},"이동경사각도","mvmn_slop_angl","NUMBER(6,3)","FLOAT","NUMBER(6,3)",{"$nulls":12},"mvmn_slop_angl ","NUMBER(6,3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_2.","mvmn_slop_angl"," IS ","'이동경사각도'",";"]
[null,null,"차로진행거리","lane_prgrs_dstn",15,"NUMBER(7,2)",null,null,"통행차로진행거리",{"$nulls":4},"차로진행거리","lane_prgrs_dstn","NUMBER(19,9)","FLOAT","NUMBER(19,9)",{"$nulls":12},"lane_prgrs_dstn ","NUMBER(19,9) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_2.","lane_prgrs_dstn"," IS ","'통행차로진행거리'",";"]
[null,null,"대기행렬관측여부","queu_obsrvn_yn",16,"CHAR(1)",null,null,"대기행렬관측여부 (503)",{"$nulls":4},"대기행렬관측여부","queu_obsrvn_yn","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",{"$nulls":12},"queu_obsrvn_yn ","VARCHAR2(1) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_2.","queu_obsrvn_yn"," IS ","'대기행렬관측여부 (503)'",";"]
[null,null,"지역구분코드","rgn_prttn_cd",17,"CHAR(2)","FK","NOT NULL","지역분할코드(051)",{"$nulls":4},"지역분할코드","rgn_prttn_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",{"$nulls":12},"rgn_prttn_cd ","VARCHAR2(2) ","NOT NULL",{"$f":"\") TABLESPACE \"&AI221&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_C002 NOLOGGING"},null,null,{"$f":"IF(OR(F219=\"PK\", F219=\"PK/FK\"), H219, \"\")","v":""},null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_2.","rgn_prttn_cd"," IS ","'지역분할코드(051)'",";"]
[{"$nulls":30},{"$f":"CONCATENATE(AI220:AK220)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (locn_clct_unix_tm) INTERVAL (3600) STORE IN (\"&AI221&\") (PARTITION BFR_\" & N202& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AI221&\");\"","v":"PARTITION BY RANGE (locn_clct_unix_tm) INTERVAL (3600) STORE IN (SOIT_D08_C002) (PARTITION BFR_soitsrltmprdtvhclmvmntowh_2_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_C002);"},{"$f":"\"CREATE INDEX PK_\" & N202& \" ON \" & N202 & CONCATENATE(AJ204:AL218) & \" LOCAL (PARTITION BFR_\" & N202 & \"_20221101 TABLESPACE \"&AJ221&\") TABLESPACE \"&AJ221&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & N202 & \" ADD CONSTRAINT PK_\" & N202 & \" PRIMARY KEY \" & CONCATENATE(AJ204:AL218) & \";\"","v":{"$error":"#VALUE!"}}]
[{"$nulls":34},"SOIT_D08_C002","SOIT_I08_C002"]
[null,"[5분] 실시간 차량이동궤적 테이블(예측) - 3지역",{"$nulls":11},"soitsrltmprdtvhclmvmntowh_3",{"$nulls":33},{"$f":"IF(LEFT(AE222, 13) = \"CONSTRAINT PK\", AE222, \"\")","v":""}]
[27,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N222&\" \"","v":"soitsrltmprdtvhclmvmntowh_3 "},null," IS ",{"$f":"\"'\"&B222&\"'\"","v":"'[5분] 실시간 차량이동궤적 테이블(예측) - 3지역'"},";",null,null,null,""]
["TIBERO","soitsrltmprdtvhclmvmntowh_3\n(vehicle_history","분석유닉스시각","anls_unix_tm",1,"NUMBER(10)","PK",null,"분석 대상기간 시작시각",{"$nulls":4},"분석유닉스시각","anls_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":10},"CREATE TABLE ",{"$f":"N222&\" (\"","v":"soitsrltmprdtvhclmvmntowh_3 ("},{"$f":"O224&\" \"","v":"anls_unix_tm "},{"$f":"R224&\" \"","v":"NUMBER(10) "},{"$f":"IF(H224=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",null,"(",{"$f":"IF(OR(G224=\"PK\", G224=\"PK/FK\"), O224, \"\")","v":"anls_unix_tm"},",","COMMENT ON COLUMN ",{"$f":"$N$222&\".\"","v":"soitsrltmprdtvhclmvmntowh_3."},{"$f":"O224","v":"anls_unix_tm"}," IS ",{"$f":"\"'\"&I224&\"'\"","v":"'분석 대상기간 시작시각'"},";",null,null,null,""]
[null,null,"위치수집유닉스시각","locn_clct_unix_tm",2,"NUMBER(10)","PK",null,"위치수집유닉스시각",{"$nulls":4},"위치수집유닉스시각","locn_clct_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":12},"locn_clct_unix_tm ","NUMBER(10) ","",",",null,null,"locn_clct_unix_tm",",","COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_3.","locn_clct_unix_tm"," IS ","'위치수집유닉스시각'",";"]
[null,null,"차량ID","vhcl_id",4,"VARCHAR2(150)","PK",null,"차량ID",{"$nulls":4},"차량ID","vhcl_id","VARCHAR2(150)","VARCHAR(150)","VARCHAR2(150)",{"$nulls":12},"vhcl_id ","VARCHAR2(150) ","",",",null,null,"vhcl_id",")","COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_3.","vhcl_id"," IS ","'차량ID'",";"]
[null,null,"차로ID","lane_id",5,"VARCHAR2(300)","FK",null,"통행차로ID",{"$nulls":4},"차로ID","lane_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",{"$nulls":12},"lane_id ","VARCHAR2(300) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_3.","lane_id"," IS ","'통행차로ID'",";",null,null,null,{"$f":"IF(LEFT(AE227, 13) = \"CONSTRAINT PK\", AE227, \"\")","v":""}]
[null,null,"세그먼트ID","sgmn_id",6,"VARCHAR2(300)","FK","NOT NULL","통행세그먼트ID",{"$nulls":4},"세그먼트ID","sgmn_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",{"$nulls":12},"sgmn_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_3.","sgmn_id"," IS ","'통행세그먼트ID'",";"]
[null,null,"차종코드","kncr_cd",7,"CHAR(10)",null,null,"차종 (008)",{"$nulls":4},"차종코드","kncr_cd","CHAR(10)","VARCHAR(10)","VARCHAR2(10)",{"$nulls":12},"kncr_cd ","VARCHAR2(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_3.","kncr_cd"," IS ","'차종 (008)'",";"]
[null,null,"순간속도","mmnt_sped",8,"NUMBER(5,2)",null,null,"순간속도 (m/s)",{"$nulls":4},"순간속도","mmnt_sped","NUMBER(5,2)","FLOAT","NUMBER(5,2)",{"$nulls":12},"mmnt_sped ","NUMBER(5,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_3.","mmnt_sped"," IS ","'순간속도 (m/s)'",";"]
[null,null,"비혼잡속도","non_cngt_sped",9,"NUMBER(5,2)",null,null,"비혼잡속도 (m/s)",{"$nulls":4},"비혼잡속도","non_cngt_sped","NUMBER(5,2)","FLOAT","NUMBER(5,2)",{"$nulls":12},"non_cngt_sped ","NUMBER(5,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_3.","non_cngt_sped"," IS ","'비혼잡속도 (m/s)'",";"]
[null,null,"차량경도","vhcl_lot",10,"NUMBER(13,10)",null,null,"차량경도",{"$nulls":4},"차량경도","vhcl_lot","NUMBER(13,10)","FLOAT","NUMBER(13,10)",{"$nulls":12},"vhcl_lot ","NUMBER(13,10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_3.","vhcl_lot"," IS ","'차량경도'",";"]
[null,null,"차량위도","vhcl_lat",11,"NUMBER(12,10)",null,null,"차량위도",{"$nulls":4},"차량위도","vhcl_lat","NUMBER(12,10)","FLOAT","NUMBER(12,10)",{"$nulls":12},"vhcl_lat ","NUMBER(12,10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_3.","vhcl_lat"," IS ","'차량위도'",";"]
[null,null,"차량고도","vhcl_lntd",12,"NUMBER(10)",null,null,"차량고도",{"$nulls":4},"차량고도","vhcl_lntd","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":12},"vhcl_lntd ","NUMBER(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_3.","vhcl_lntd"," IS ","'차량고도'",";"]
[null,null,"이동방위각도","mvmn_pocm_angl",13,"NUMBER(6,3)",null,null,"이동방위각도",{"$nulls":4},"이동방위각도","mvmn_pocm_angl","NUMBER(6,3)","FLOAT","NUMBER(6,3)",{"$nulls":12},"mvmn_pocm_angl ","NUMBER(6,3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_3.","mvmn_pocm_angl"," IS ","'이동방위각도'",";"]
[null,null,"이동경사각도","mvmn_slop_angl",14,"NUMBER(6,3)",null,null,"이동경사각도",{"$nulls":4},"이동경사각도","mvmn_slop_angl","NUMBER(6,3)","FLOAT","NUMBER(6,3)",{"$nulls":12},"mvmn_slop_angl ","NUMBER(6,3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_3.","mvmn_slop_angl"," IS ","'이동경사각도'",";"]
[null,null,"차로진행거리","lane_prgrs_dstn",15,"NUMBER(7,2)",null,null,"통행차로진행거리",{"$nulls":4},"차로진행거리","lane_prgrs_dstn","NUMBER(19,9)","FLOAT","NUMBER(19,9)",{"$nulls":12},"lane_prgrs_dstn ","NUMBER(19,9) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_3.","lane_prgrs_dstn"," IS ","'통행차로진행거리'",";"]
[null,null,"대기행렬관측여부","queu_obsrvn_yn",16,"CHAR(1)",null,null,"대기행렬관측여부 (503)",{"$nulls":4},"대기행렬관측여부","queu_obsrvn_yn","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",{"$nulls":12},"queu_obsrvn_yn ","VARCHAR2(1) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_3.","queu_obsrvn_yn"," IS ","'대기행렬관측여부 (503)'",";"]
[null,null,"지역구분코드","rgn_prttn_cd",17,"CHAR(2)","FK","NOT NULL","지역분할코드(051)",{"$nulls":4},"지역분할코드","rgn_prttn_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",{"$nulls":12},"rgn_prttn_cd ","VARCHAR2(2) ","NOT NULL",{"$f":"\") TABLESPACE \"&AI241&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_C003 NOLOGGING"},null,null,{"$f":"IF(OR(F239=\"PK\", F239=\"PK/FK\"), H239, \"\")","v":""},null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_3.","rgn_prttn_cd"," IS ","'지역분할코드(051)'",";"]
[{"$nulls":30},{"$f":"CONCATENATE(AI240:AK240)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (locn_clct_unix_tm) INTERVAL (3600) STORE IN (\"&AI241&\") (PARTITION BFR_\" & N222& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AI241&\");\"","v":"PARTITION BY RANGE (locn_clct_unix_tm) INTERVAL (3600) STORE IN (SOIT_D08_C003) (PARTITION BFR_soitsrltmprdtvhclmvmntowh_3_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_C003);"},{"$f":"\"CREATE INDEX PK_\" & N222& \" ON \" & N222 & CONCATENATE(AJ224:AL238) & \" LOCAL (PARTITION BFR_\" & N222 & \"_20221101 TABLESPACE \"&AJ241&\") TABLESPACE \"&AJ241&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & N222 & \" ADD CONSTRAINT PK_\" & N222 & \" PRIMARY KEY \" & CONCATENATE(AJ224:AL238) & \";\"","v":{"$error":"#VALUE!"}}]
[{"$nulls":34},"SOIT_D08_C003","SOIT_I08_C003"]
[null,"[5분] 실시간 차량이동궤적 테이블(예측) - 4지역",{"$nulls":11},"soitsrltmprdtvhclmvmntowh_4",{"$nulls":33},{"$f":"IF(LEFT(AE242, 13) = \"CONSTRAINT PK\", AE242, \"\")","v":""}]
[27,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N242&\" \"","v":"soitsrltmprdtvhclmvmntowh_4 "},null," IS ",{"$f":"\"'\"&B242&\"'\"","v":"'[5분] 실시간 차량이동궤적 테이블(예측) - 4지역'"},";",null,null,null,""]
["TIBERO","soitsrltmprdtvhclmvmntowh_4\n(vehicle_history","분석유닉스시각","anls_unix_tm",1,"NUMBER(10)","PK",null,"분석 대상기간 시작시각",{"$nulls":4},"분석유닉스시각","anls_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":10},"CREATE TABLE ",{"$f":"N242&\" (\"","v":"soitsrltmprdtvhclmvmntowh_4 ("},{"$f":"O244&\" \"","v":"anls_unix_tm "},{"$f":"R244&\" \"","v":"NUMBER(10) "},{"$f":"IF(H244=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",null,"(",{"$f":"IF(OR(G244=\"PK\", G244=\"PK/FK\"), O244, \"\")","v":"anls_unix_tm"},",","COMMENT ON COLUMN ",{"$f":"$N$242&\".\"","v":"soitsrltmprdtvhclmvmntowh_4."},{"$f":"O244","v":"anls_unix_tm"}," IS ",{"$f":"\"'\"&I244&\"'\"","v":"'분석 대상기간 시작시각'"},";",null,null,null,""]
[null,null,"위치수집유닉스시각","locn_clct_unix_tm",2,"NUMBER(10)","PK",null,"위치수집유닉스시각",{"$nulls":4},"위치수집유닉스시각","locn_clct_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":12},"locn_clct_unix_tm ","NUMBER(10) ","",",",null,null,"locn_clct_unix_tm",",","COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_4.","locn_clct_unix_tm"," IS ","'위치수집유닉스시각'",";"]
[null,null,"차량ID","vhcl_id",4,"VARCHAR2(150)","PK",null,"차량ID",{"$nulls":4},"차량ID","vhcl_id","VARCHAR2(150)","VARCHAR(150)","VARCHAR2(150)",{"$nulls":12},"vhcl_id ","VARCHAR2(150) ","",",",null,null,"vhcl_id",")","COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_4.","vhcl_id"," IS ","'차량ID'",";"]
[null,null,"차로ID","lane_id",5,"VARCHAR2(300)","FK",null,"통행차로ID",{"$nulls":4},"차로ID","lane_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",{"$nulls":12},"lane_id ","VARCHAR2(300) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_4.","lane_id"," IS ","'통행차로ID'",";",null,null,null,{"$f":"IF(LEFT(AE247, 13) = \"CONSTRAINT PK\", AE247, \"\")","v":""}]
[null,null,"세그먼트ID","sgmn_id",6,"VARCHAR2(300)","FK","NOT NULL","통행세그먼트ID",{"$nulls":4},"세그먼트ID","sgmn_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",{"$nulls":12},"sgmn_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_4.","sgmn_id"," IS ","'통행세그먼트ID'",";"]
[null,null,"차종코드","kncr_cd",7,"CHAR(10)",null,null,"차종 (008)",{"$nulls":4},"차종코드","kncr_cd","CHAR(10)","VARCHAR(10)","VARCHAR2(10)",{"$nulls":12},"kncr_cd ","VARCHAR2(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_4.","kncr_cd"," IS ","'차종 (008)'",";"]
[null,null,"순간속도","mmnt_sped",8,"NUMBER(5,2)",null,null,"순간속도 (m/s)",{"$nulls":4},"순간속도","mmnt_sped","NUMBER(5,2)","FLOAT","NUMBER(5,2)",{"$nulls":12},"mmnt_sped ","NUMBER(5,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_4.","mmnt_sped"," IS ","'순간속도 (m/s)'",";"]
[null,null,"비혼잡속도","non_cngt_sped",9,"NUMBER(5,2)",null,null,"비혼잡속도 (m/s)",{"$nulls":4},"비혼잡속도","non_cngt_sped","NUMBER(5,2)","FLOAT","NUMBER(5,2)",{"$nulls":12},"non_cngt_sped ","NUMBER(5,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_4.","non_cngt_sped"," IS ","'비혼잡속도 (m/s)'",";"]
[null,null,"차량경도","vhcl_lot",10,"NUMBER(13,10)",null,null,"차량경도",{"$nulls":4},"차량경도","vhcl_lot","NUMBER(13,10)","FLOAT","NUMBER(13,10)",{"$nulls":12},"vhcl_lot ","NUMBER(13,10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_4.","vhcl_lot"," IS ","'차량경도'",";"]
[null,null,"차량위도","vhcl_lat",11,"NUMBER(12,10)",null,null,"차량위도",{"$nulls":4},"차량위도","vhcl_lat","NUMBER(12,10)","FLOAT","NUMBER(12,10)",{"$nulls":12},"vhcl_lat ","NUMBER(12,10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_4.","vhcl_lat"," IS ","'차량위도'",";"]
[null,null,"차량고도","vhcl_lntd",12,"NUMBER(10)",null,null,"차량고도",{"$nulls":4},"차량고도","vhcl_lntd","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":12},"vhcl_lntd ","NUMBER(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_4.","vhcl_lntd"," IS ","'차량고도'",";"]
[null,null,"이동방위각도","mvmn_pocm_angl",13,"NUMBER(6,3)",null,null,"이동방위각도",{"$nulls":4},"이동방위각도","mvmn_pocm_angl","NUMBER(6,3)","FLOAT","NUMBER(6,3)",{"$nulls":12},"mvmn_pocm_angl ","NUMBER(6,3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_4.","mvmn_pocm_angl"," IS ","'이동방위각도'",";"]
[null,null,"이동경사각도","mvmn_slop_angl",14,"NUMBER(6,3)",null,null,"이동경사각도",{"$nulls":4},"이동경사각도","mvmn_slop_angl","NUMBER(6,3)","FLOAT","NUMBER(6,3)",{"$nulls":12},"mvmn_slop_angl ","NUMBER(6,3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_4.","mvmn_slop_angl"," IS ","'이동경사각도'",";"]
[null,null,"차로진행거리","lane_prgrs_dstn",15,"NUMBER(7,2)",null,null,"통행차로진행거리",{"$nulls":4},"차로진행거리","lane_prgrs_dstn","NUMBER(19,9)","FLOAT","NUMBER(19,9)",{"$nulls":12},"lane_prgrs_dstn ","NUMBER(19,9) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_4.","lane_prgrs_dstn"," IS ","'통행차로진행거리'",";"]
[null,null,"대기행렬관측여부","queu_obsrvn_yn",16,"CHAR(1)",null,null,"대기행렬관측여부 (503)",{"$nulls":4},"대기행렬관측여부","queu_obsrvn_yn","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",{"$nulls":12},"queu_obsrvn_yn ","VARCHAR2(1) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_4.","queu_obsrvn_yn"," IS ","'대기행렬관측여부 (503)'",";"]
[null,null,"지역구분코드","rgn_prttn_cd",17,"CHAR(2)","FK","NOT NULL","지역분할코드(051)",{"$nulls":4},"지역분할코드","rgn_prttn_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",{"$nulls":12},"rgn_prttn_cd ","VARCHAR2(2) ","NOT NULL",{"$f":"\") TABLESPACE \"&AI261&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_C004 NOLOGGING"},null,null,{"$f":"IF(OR(F259=\"PK\", F259=\"PK/FK\"), H259, \"\")","v":""},null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_4.","rgn_prttn_cd"," IS ","'지역분할코드(051)'",";"]
[{"$nulls":30},{"$f":"CONCATENATE(AI260:AK260)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (locn_clct_unix_tm) INTERVAL (3600) STORE IN (\"&AI261&\") (PARTITION BFR_\" & N242& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AI261&\");\"","v":"PARTITION BY RANGE (locn_clct_unix_tm) INTERVAL (3600) STORE IN (SOIT_D08_C004) (PARTITION BFR_soitsrltmprdtvhclmvmntowh_4_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_C004);"},{"$f":"\"CREATE INDEX PK_\" & N242& \" ON \" & N242 & CONCATENATE(AJ244:AL258) & \" LOCAL (PARTITION BFR_\" & N242 & \"_20221101 TABLESPACE \"&AJ261&\") TABLESPACE \"&AJ261&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & N242 & \" ADD CONSTRAINT PK_\" & N242 & \" PRIMARY KEY \" & CONCATENATE(AJ244:AL258) & \";\"","v":{"$error":"#VALUE!"}}]
[{"$nulls":34},"SOIT_D08_C004","SOIT_I08_C004"]
[null,"[5분] 실시간 차량이동궤적 테이블(예측) - 5지역",{"$nulls":11},"soitsrltmprdtvhclmvmntowh_5",{"$nulls":33},{"$f":"IF(LEFT(AE262, 13) = \"CONSTRAINT PK\", AE262, \"\")","v":""}]
[27,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N262&\" \"","v":"soitsrltmprdtvhclmvmntowh_5 "},null," IS ",{"$f":"\"'\"&B262&\"'\"","v":"'[5분] 실시간 차량이동궤적 테이블(예측) - 5지역'"},";",null,null,null,""]
["TIBERO","soitsrltmprdtvhclmvmntowh_5\n(vehicle_history","분석유닉스시각","anls_unix_tm",1,"NUMBER(10)","PK",null,"분석 대상기간 시작시각",{"$nulls":4},"분석유닉스시각","anls_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":10},"CREATE TABLE ",{"$f":"N262&\" (\"","v":"soitsrltmprdtvhclmvmntowh_5 ("},{"$f":"O264&\" \"","v":"anls_unix_tm "},{"$f":"R264&\" \"","v":"NUMBER(10) "},{"$f":"IF(H264=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",null,"(",{"$f":"IF(OR(G264=\"PK\", G264=\"PK/FK\"), O264, \"\")","v":"anls_unix_tm"},",","COMMENT ON COLUMN ",{"$f":"$N$262&\".\"","v":"soitsrltmprdtvhclmvmntowh_5."},{"$f":"O264","v":"anls_unix_tm"}," IS ",{"$f":"\"'\"&I264&\"'\"","v":"'분석 대상기간 시작시각'"},";",null,null,null,""]
[null,null,"위치수집유닉스시각","locn_clct_unix_tm",2,"NUMBER(10)","PK",null,"위치수집유닉스시각",{"$nulls":4},"위치수집유닉스시각","locn_clct_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":12},"locn_clct_unix_tm ","NUMBER(10) ","",",",null,null,"locn_clct_unix_tm",",","COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_5.","locn_clct_unix_tm"," IS ","'위치수집유닉스시각'",";"]
[null,null,"차량ID","vhcl_id",4,"VARCHAR2(150)","PK",null,"차량ID",{"$nulls":4},"차량ID","vhcl_id","VARCHAR2(150)","VARCHAR(150)","VARCHAR2(150)",{"$nulls":12},"vhcl_id ","VARCHAR2(150) ","",",",null,null,"vhcl_id",")","COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_5.","vhcl_id"," IS ","'차량ID'",";"]
[null,null,"차로ID","lane_id",5,"VARCHAR2(300)","FK",null,"통행차로ID",{"$nulls":4},"차로ID","lane_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",{"$nulls":12},"lane_id ","VARCHAR2(300) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_5.","lane_id"," IS ","'통행차로ID'",";",null,null,null,{"$f":"IF(LEFT(AE267, 13) = \"CONSTRAINT PK\", AE267, \"\")","v":""}]
[null,null,"세그먼트ID","sgmn_id",6,"VARCHAR2(300)","FK","NOT NULL","통행세그먼트ID",{"$nulls":4},"세그먼트ID","sgmn_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",{"$nulls":12},"sgmn_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_5.","sgmn_id"," IS ","'통행세그먼트ID'",";"]
[null,null,"차종코드","kncr_cd",7,"CHAR(10)",null,null,"차종 (008)",{"$nulls":4},"차종코드","kncr_cd","CHAR(10)","VARCHAR(10)","VARCHAR2(10)",{"$nulls":12},"kncr_cd ","VARCHAR2(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_5.","kncr_cd"," IS ","'차종 (008)'",";"]
[null,null,"순간속도","mmnt_sped",8,"NUMBER(5,2)",null,null,"순간속도 (m/s)",{"$nulls":4},"순간속도","mmnt_sped","NUMBER(5,2)","FLOAT","NUMBER(5,2)",{"$nulls":12},"mmnt_sped ","NUMBER(5,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_5.","mmnt_sped"," IS ","'순간속도 (m/s)'",";"]
[null,null,"비혼잡속도","non_cngt_sped",9,"NUMBER(5,2)",null,null,"비혼잡속도 (m/s)",{"$nulls":4},"비혼잡속도","non_cngt_sped","NUMBER(5,2)","FLOAT","NUMBER(5,2)",{"$nulls":12},"non_cngt_sped ","NUMBER(5,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_5.","non_cngt_sped"," IS ","'비혼잡속도 (m/s)'",";"]
[null,null,"차량경도","vhcl_lot",10,"NUMBER(13,10)",null,null,"차량경도",{"$nulls":4},"차량경도","vhcl_lot","NUMBER(13,10)","FLOAT","NUMBER(13,10)",{"$nulls":12},"vhcl_lot ","NUMBER(13,10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_5.","vhcl_lot"," IS ","'차량경도'",";"]
[null,null,"차량위도","vhcl_lat",11,"NUMBER(12,10)",null,null,"차량위도",{"$nulls":4},"차량위도","vhcl_lat","NUMBER(12,10)","FLOAT","NUMBER(12,10)",{"$nulls":12},"vhcl_lat ","NUMBER(12,10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_5.","vhcl_lat"," IS ","'차량위도'",";"]
[null,null,"차량고도","vhcl_lntd",12,"NUMBER(10)",null,null,"차량고도",{"$nulls":4},"차량고도","vhcl_lntd","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":12},"vhcl_lntd ","NUMBER(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_5.","vhcl_lntd"," IS ","'차량고도'",";"]
[null,null,"이동방위각도","mvmn_pocm_angl",13,"NUMBER(6,3)",null,null,"이동방위각도",{"$nulls":4},"이동방위각도","mvmn_pocm_angl","NUMBER(6,3)","FLOAT","NUMBER(6,3)",{"$nulls":12},"mvmn_pocm_angl ","NUMBER(6,3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_5.","mvmn_pocm_angl"," IS ","'이동방위각도'",";"]
[null,null,"이동경사각도","mvmn_slop_angl",14,"NUMBER(6,3)",null,null,"이동경사각도",{"$nulls":4},"이동경사각도","mvmn_slop_angl","NUMBER(6,3)","FLOAT","NUMBER(6,3)",{"$nulls":12},"mvmn_slop_angl ","NUMBER(6,3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_5.","mvmn_slop_angl"," IS ","'이동경사각도'",";"]
[null,null,"차로진행거리","lane_prgrs_dstn",15,"NUMBER(7,2)",null,null,"통행차로진행거리",{"$nulls":4},"차로진행거리","lane_prgrs_dstn","NUMBER(19,9)","FLOAT","NUMBER(19,9)",{"$nulls":12},"lane_prgrs_dstn ","NUMBER(19,9) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_5.","lane_prgrs_dstn"," IS ","'통행차로진행거리'",";"]
[null,null,"대기행렬관측여부","queu_obsrvn_yn",16,"CHAR(1)",null,null,"대기행렬관측여부 (503)",{"$nulls":4},"대기행렬관측여부","queu_obsrvn_yn","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",{"$nulls":12},"queu_obsrvn_yn ","VARCHAR2(1) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_5.","queu_obsrvn_yn"," IS ","'대기행렬관측여부 (503)'",";"]
[null,null,"지역구분코드","rgn_prttn_cd",17,"CHAR(2)","FK","NOT NULL","지역분할코드(051)",{"$nulls":4},"지역분할코드","rgn_prttn_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",{"$nulls":12},"rgn_prttn_cd ","VARCHAR2(2) ","NOT NULL",{"$f":"\") TABLESPACE \"&AI281&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_C005 NOLOGGING"},null,null,{"$f":"IF(OR(F279=\"PK\", F279=\"PK/FK\"), H279, \"\")","v":""},null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_5.","rgn_prttn_cd"," IS ","'지역분할코드(051)'",";"]
[{"$nulls":30},{"$f":"CONCATENATE(AI280:AK280)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (locn_clct_unix_tm) INTERVAL (3600) STORE IN (\"&AI281&\") (PARTITION BFR_\" & N262& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AI281&\");\"","v":"PARTITION BY RANGE (locn_clct_unix_tm) INTERVAL (3600) STORE IN (SOIT_D08_C005) (PARTITION BFR_soitsrltmprdtvhclmvmntowh_5_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_C005);"},{"$f":"\"CREATE INDEX PK_\" & N262& \" ON \" & N262 & CONCATENATE(AJ264:AL278) & \" LOCAL (PARTITION BFR_\" & N262 & \"_20221101 TABLESPACE \"&AJ281&\") TABLESPACE \"&AJ281&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & N262 & \" ADD CONSTRAINT PK_\" & N262 & \" PRIMARY KEY \" & CONCATENATE(AJ264:AL278) & \";\"","v":{"$error":"#VALUE!"}}]
[{"$nulls":34},"SOIT_D08_C005","SOIT_I08_C005"]
[null,"[5분] 실시간 차량이동궤적 테이블(예측) - 6지역",{"$nulls":11},"soitsrltmprdtvhclmvmntowh_6",{"$nulls":33},{"$f":"IF(LEFT(AE282, 13) = \"CONSTRAINT PK\", AE282, \"\")","v":""}]
[27,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N282&\" \"","v":"soitsrltmprdtvhclmvmntowh_6 "},null," IS ",{"$f":"\"'\"&B282&\"'\"","v":"'[5분] 실시간 차량이동궤적 테이블(예측) - 6지역'"},";",null,null,null,""]
["TIBERO","soitsrltmprdtvhclmvmntowh_6\n(vehicle_history","분석유닉스시각","anls_unix_tm",1,"NUMBER(10)","PK",null,"분석 대상기간 시작시각",{"$nulls":4},"분석유닉스시각","anls_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":10},"CREATE TABLE ",{"$f":"N282&\" (\"","v":"soitsrltmprdtvhclmvmntowh_6 ("},{"$f":"O284&\" \"","v":"anls_unix_tm "},{"$f":"R284&\" \"","v":"NUMBER(10) "},{"$f":"IF(H284=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",null,"(",{"$f":"IF(OR(G284=\"PK\", G284=\"PK/FK\"), O284, \"\")","v":"anls_unix_tm"},",","COMMENT ON COLUMN ",{"$f":"$N$282&\".\"","v":"soitsrltmprdtvhclmvmntowh_6."},{"$f":"O284","v":"anls_unix_tm"}," IS ",{"$f":"\"'\"&I284&\"'\"","v":"'분석 대상기간 시작시각'"},";",null,null,null,""]
[null,null,"위치수집유닉스시각","locn_clct_unix_tm",2,"NUMBER(10)","PK",null,"위치수집유닉스시각",{"$nulls":4},"위치수집유닉스시각","locn_clct_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":12},"locn_clct_unix_tm ","NUMBER(10) ","",",",null,null,"locn_clct_unix_tm",",","COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_6.","locn_clct_unix_tm"," IS ","'위치수집유닉스시각'",";"]
[null,null,"차량ID","vhcl_id",4,"VARCHAR2(150)","PK",null,"차량ID",{"$nulls":4},"차량ID","vhcl_id","VARCHAR2(150)","VARCHAR(150)","VARCHAR2(150)",{"$nulls":12},"vhcl_id ","VARCHAR2(150) ","",",",null,null,"vhcl_id",")","COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_6.","vhcl_id"," IS ","'차량ID'",";"]
[null,null,"차로ID","lane_id",5,"VARCHAR2(300)","FK",null,"통행차로ID",{"$nulls":4},"차로ID","lane_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",{"$nulls":12},"lane_id ","VARCHAR2(300) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_6.","lane_id"," IS ","'통행차로ID'",";",null,null,null,{"$f":"IF(LEFT(AE287, 13) = \"CONSTRAINT PK\", AE287, \"\")","v":""}]
[null,null,"세그먼트ID","sgmn_id",6,"VARCHAR2(300)","FK","NOT NULL","통행세그먼트ID",{"$nulls":4},"세그먼트ID","sgmn_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",{"$nulls":12},"sgmn_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_6.","sgmn_id"," IS ","'통행세그먼트ID'",";"]
[null,null,"차종코드","kncr_cd",7,"CHAR(10)",null,null,"차종 (008)",{"$nulls":4},"차종코드","kncr_cd","CHAR(10)","VARCHAR(10)","VARCHAR2(10)",{"$nulls":12},"kncr_cd ","VARCHAR2(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_6.","kncr_cd"," IS ","'차종 (008)'",";"]
[null,null,"순간속도","mmnt_sped",8,"NUMBER(5,2)",null,null,"순간속도 (m/s)",{"$nulls":4},"순간속도","mmnt_sped","NUMBER(5,2)","FLOAT","NUMBER(5,2)",{"$nulls":12},"mmnt_sped ","NUMBER(5,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_6.","mmnt_sped"," IS ","'순간속도 (m/s)'",";"]
[null,null,"비혼잡속도","non_cngt_sped",9,"NUMBER(5,2)",null,null,"비혼잡속도 (m/s)",{"$nulls":4},"비혼잡속도","non_cngt_sped","NUMBER(5,2)","FLOAT","NUMBER(5,2)",{"$nulls":12},"non_cngt_sped ","NUMBER(5,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_6.","non_cngt_sped"," IS ","'비혼잡속도 (m/s)'",";"]
[null,null,"차량경도","vhcl_lot",10,"NUMBER(13,10)",null,null,"차량경도",{"$nulls":4},"차량경도","vhcl_lot","NUMBER(13,10)","FLOAT","NUMBER(13,10)",{"$nulls":12},"vhcl_lot ","NUMBER(13,10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_6.","vhcl_lot"," IS ","'차량경도'",";"]
[null,null,"차량위도","vhcl_lat",11,"NUMBER(12,10)",null,null,"차량위도",{"$nulls":4},"차량위도","vhcl_lat","NUMBER(12,10)","FLOAT","NUMBER(12,10)",{"$nulls":12},"vhcl_lat ","NUMBER(12,10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_6.","vhcl_lat"," IS ","'차량위도'",";"]
[null,null,"차량고도","vhcl_lntd",12,"NUMBER(10)",null,null,"차량고도",{"$nulls":4},"차량고도","vhcl_lntd","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":12},"vhcl_lntd ","NUMBER(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_6.","vhcl_lntd"," IS ","'차량고도'",";"]
[null,null,"이동방위각도","mvmn_pocm_angl",13,"NUMBER(6,3)",null,null,"이동방위각도",{"$nulls":4},"이동방위각도","mvmn_pocm_angl","NUMBER(6,3)","FLOAT","NUMBER(6,3)",{"$nulls":12},"mvmn_pocm_angl ","NUMBER(6,3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_6.","mvmn_pocm_angl"," IS ","'이동방위각도'",";"]
[null,null,"이동경사각도","mvmn_slop_angl",14,"NUMBER(6,3)",null,null,"이동경사각도",{"$nulls":4},"이동경사각도","mvmn_slop_angl","NUMBER(6,3)","FLOAT","NUMBER(6,3)",{"$nulls":12},"mvmn_slop_angl ","NUMBER(6,3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_6.","mvmn_slop_angl"," IS ","'이동경사각도'",";"]
[null,null,"차로진행거리","lane_prgrs_dstn",15,"NUMBER(7,2)",null,null,"통행차로진행거리",{"$nulls":4},"차로진행거리","lane_prgrs_dstn","NUMBER(19,9)","FLOAT","NUMBER(19,9)",{"$nulls":12},"lane_prgrs_dstn ","NUMBER(19,9) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_6.","lane_prgrs_dstn"," IS ","'통행차로진행거리'",";"]
[null,null,"대기행렬관측여부","queu_obsrvn_yn",16,"CHAR(1)",null,null,"대기행렬관측여부 (503)",{"$nulls":4},"대기행렬관측여부","queu_obsrvn_yn","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",{"$nulls":12},"queu_obsrvn_yn ","VARCHAR2(1) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_6.","queu_obsrvn_yn"," IS ","'대기행렬관측여부 (503)'",";"]
[null,null,"지역구분코드","rgn_prttn_cd",17,"CHAR(2)","FK","NOT NULL","지역분할코드(051)",{"$nulls":4},"지역분할코드","rgn_prttn_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",{"$nulls":12},"rgn_prttn_cd ","VARCHAR2(2) ","NOT NULL",{"$f":"\") TABLESPACE \"&AI301&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_C006 NOLOGGING"},null,null,{"$f":"IF(OR(F299=\"PK\", F299=\"PK/FK\"), H299, \"\")","v":""},null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_6.","rgn_prttn_cd"," IS ","'지역분할코드(051)'",";"]
[{"$nulls":30},{"$f":"CONCATENATE(AI300:AK300)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (locn_clct_unix_tm) INTERVAL (3600) STORE IN (\"&AI301&\") (PARTITION BFR_\" & N282& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AI301&\");\"","v":"PARTITION BY RANGE (locn_clct_unix_tm) INTERVAL (3600) STORE IN (SOIT_D08_C006) (PARTITION BFR_soitsrltmprdtvhclmvmntowh_6_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_C006);"},{"$f":"\"CREATE INDEX PK_\" & N282& \" ON \" & N282 & CONCATENATE(AJ284:AL298) & \" LOCAL (PARTITION BFR_\" & N282 & \"_20221101 TABLESPACE \"&AJ301&\") TABLESPACE \"&AJ301&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & N282 & \" ADD CONSTRAINT PK_\" & N282 & \" PRIMARY KEY \" & CONCATENATE(AJ284:AL298) & \";\"","v":{"$error":"#VALUE!"}}]
[{"$nulls":34},"SOIT_D08_C006","SOIT_I08_C006"]
[null,"[5분] 실시간 차량이동궤적 테이블(예측) - 7지역",{"$nulls":11},"soitsrltmprdtvhclmvmntowh_7",{"$nulls":33},{"$f":"IF(LEFT(AE302, 13) = \"CONSTRAINT PK\", AE302, \"\")","v":""}]
[27,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N302&\" \"","v":"soitsrltmprdtvhclmvmntowh_7 "},null," IS ",{"$f":"\"'\"&B302&\"'\"","v":"'[5분] 실시간 차량이동궤적 테이블(예측) - 7지역'"},";",null,null,null,""]
["TIBERO","soitsrltmprdtvhclmvmntowh_7\n(vehicle_history","분석유닉스시각","anls_unix_tm",1,"NUMBER(10)","PK",null,"분석 대상기간 시작시각",{"$nulls":4},"분석유닉스시각","anls_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":10},"CREATE TABLE ",{"$f":"N302&\" (\"","v":"soitsrltmprdtvhclmvmntowh_7 ("},{"$f":"O304&\" \"","v":"anls_unix_tm "},{"$f":"R304&\" \"","v":"NUMBER(10) "},{"$f":"IF(H304=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",null,"(",{"$f":"IF(OR(G304=\"PK\", G304=\"PK/FK\"), O304, \"\")","v":"anls_unix_tm"},",","COMMENT ON COLUMN ",{"$f":"$N$302&\".\"","v":"soitsrltmprdtvhclmvmntowh_7."},{"$f":"O304","v":"anls_unix_tm"}," IS ",{"$f":"\"'\"&I304&\"'\"","v":"'분석 대상기간 시작시각'"},";",null,null,null,""]
[null,null,"위치수집유닉스시각","locn_clct_unix_tm",2,"NUMBER(10)","PK",null,"위치수집유닉스시각",{"$nulls":4},"위치수집유닉스시각","locn_clct_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":12},"locn_clct_unix_tm ","NUMBER(10) ","",",",null,null,"locn_clct_unix_tm",",","COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_7.","locn_clct_unix_tm"," IS ","'위치수집유닉스시각'",";"]
[null,null,"차량ID","vhcl_id",4,"VARCHAR2(150)","PK",null,"차량ID",{"$nulls":4},"차량ID","vhcl_id","VARCHAR2(150)","VARCHAR(150)","VARCHAR2(150)",{"$nulls":12},"vhcl_id ","VARCHAR2(150) ","",",",null,null,"vhcl_id",")","COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_7.","vhcl_id"," IS ","'차량ID'",";"]
[null,null,"차로ID","lane_id",5,"VARCHAR2(300)","FK",null,"통행차로ID",{"$nulls":4},"차로ID","lane_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",{"$nulls":12},"lane_id ","VARCHAR2(300) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_7.","lane_id"," IS ","'통행차로ID'",";",null,null,null,{"$f":"IF(LEFT(AE307, 13) = \"CONSTRAINT PK\", AE307, \"\")","v":""}]
[null,null,"세그먼트ID","sgmn_id",6,"VARCHAR2(300)","FK","NOT NULL","통행세그먼트ID",{"$nulls":4},"세그먼트ID","sgmn_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",{"$nulls":12},"sgmn_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_7.","sgmn_id"," IS ","'통행세그먼트ID'",";"]
[null,null,"차종코드","kncr_cd",7,"CHAR(10)",null,null,"차종 (008)",{"$nulls":4},"차종코드","kncr_cd","CHAR(10)","VARCHAR(10)","VARCHAR2(10)",{"$nulls":12},"kncr_cd ","VARCHAR2(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_7.","kncr_cd"," IS ","'차종 (008)'",";"]
[null,null,"순간속도","mmnt_sped",8,"NUMBER(5,2)",null,null,"순간속도 (m/s)",{"$nulls":4},"순간속도","mmnt_sped","NUMBER(5,2)","FLOAT","NUMBER(5,2)",{"$nulls":12},"mmnt_sped ","NUMBER(5,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_7.","mmnt_sped"," IS ","'순간속도 (m/s)'",";"]
[null,null,"비혼잡속도","non_cngt_sped",9,"NUMBER(5,2)",null,null,"비혼잡속도 (m/s)",{"$nulls":4},"비혼잡속도","non_cngt_sped","NUMBER(5,2)","FLOAT","NUMBER(5,2)",{"$nulls":12},"non_cngt_sped ","NUMBER(5,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_7.","non_cngt_sped"," IS ","'비혼잡속도 (m/s)'",";"]
[null,null,"차량경도","vhcl_lot",10,"NUMBER(13,10)",null,null,"차량경도",{"$nulls":4},"차량경도","vhcl_lot","NUMBER(13,10)","FLOAT","NUMBER(13,10)",{"$nulls":12},"vhcl_lot ","NUMBER(13,10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_7.","vhcl_lot"," IS ","'차량경도'",";"]
[null,null,"차량위도","vhcl_lat",11,"NUMBER(12,10)",null,null,"차량위도",{"$nulls":4},"차량위도","vhcl_lat","NUMBER(12,10)","FLOAT","NUMBER(12,10)",{"$nulls":12},"vhcl_lat ","NUMBER(12,10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_7.","vhcl_lat"," IS ","'차량위도'",";"]
[null,null,"차량고도","vhcl_lntd",12,"NUMBER(10)",null,null,"차량고도",{"$nulls":4},"차량고도","vhcl_lntd","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":12},"vhcl_lntd ","NUMBER(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_7.","vhcl_lntd"," IS ","'차량고도'",";"]
[null,null,"이동방위각도","mvmn_pocm_angl",13,"NUMBER(6,3)",null,null,"이동방위각도",{"$nulls":4},"이동방위각도","mvmn_pocm_angl","NUMBER(6,3)","FLOAT","NUMBER(6,3)",{"$nulls":12},"mvmn_pocm_angl ","NUMBER(6,3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_7.","mvmn_pocm_angl"," IS ","'이동방위각도'",";"]
[null,null,"이동경사각도","mvmn_slop_angl",14,"NUMBER(6,3)",null,null,"이동경사각도",{"$nulls":4},"이동경사각도","mvmn_slop_angl","NUMBER(6,3)","FLOAT","NUMBER(6,3)",{"$nulls":12},"mvmn_slop_angl ","NUMBER(6,3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_7.","mvmn_slop_angl"," IS ","'이동경사각도'",";"]
[null,null,"차로진행거리","lane_prgrs_dstn",15,"NUMBER(7,2)",null,null,"통행차로진행거리",{"$nulls":4},"차로진행거리","lane_prgrs_dstn","NUMBER(19,9)","FLOAT","NUMBER(19,9)",{"$nulls":12},"lane_prgrs_dstn ","NUMBER(19,9) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_7.","lane_prgrs_dstn"," IS ","'통행차로진행거리'",";"]
[null,null,"대기행렬관측여부","queu_obsrvn_yn",16,"CHAR(1)",null,null,"대기행렬관측여부 (503)",{"$nulls":4},"대기행렬관측여부","queu_obsrvn_yn","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",{"$nulls":12},"queu_obsrvn_yn ","VARCHAR2(1) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_7.","queu_obsrvn_yn"," IS ","'대기행렬관측여부 (503)'",";"]
[null,null,"지역구분코드","rgn_prttn_cd",17,"CHAR(2)","FK","NOT NULL","지역분할코드(051)",{"$nulls":4},"지역분할코드","rgn_prttn_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",{"$nulls":12},"rgn_prttn_cd ","VARCHAR2(2) ","NOT NULL",{"$f":"\") TABLESPACE \"&AI321&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_C007 NOLOGGING"},null,null,{"$f":"IF(OR(F319=\"PK\", F319=\"PK/FK\"), H319, \"\")","v":""},null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_7.","rgn_prttn_cd"," IS ","'지역분할코드(051)'",";"]
[{"$nulls":30},{"$f":"CONCATENATE(AI320:AK320)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (locn_clct_unix_tm) INTERVAL (3600) STORE IN (\"&AI321&\") (PARTITION BFR_\" & N302& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AI321&\");\"","v":"PARTITION BY RANGE (locn_clct_unix_tm) INTERVAL (3600) STORE IN (SOIT_D08_C007) (PARTITION BFR_soitsrltmprdtvhclmvmntowh_7_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_C007);"},{"$f":"\"CREATE INDEX PK_\" & N302& \" ON \" & N302 & CONCATENATE(AJ304:AL318) & \" LOCAL (PARTITION BFR_\" & N302 & \"_20221101 TABLESPACE \"&AJ321&\") TABLESPACE \"&AJ321&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & N302 & \" ADD CONSTRAINT PK_\" & N302 & \" PRIMARY KEY \" & CONCATENATE(AJ304:AL318) & \";\"","v":{"$error":"#VALUE!"}}]
[{"$nulls":34},"SOIT_D08_C007","SOIT_I08_C007"]
[null,"[5분] 실시간 차량이동궤적 테이블(예측) - 8지역",{"$nulls":11},"soitsrltmprdtvhclmvmntowh_8",{"$nulls":33},{"$f":"IF(LEFT(AE322, 13) = \"CONSTRAINT PK\", AE322, \"\")","v":""}]
[27,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N322&\" \"","v":"soitsrltmprdtvhclmvmntowh_8 "},null," IS ",{"$f":"\"'\"&B322&\"'\"","v":"'[5분] 실시간 차량이동궤적 테이블(예측) - 8지역'"},";",null,null,null,""]
["TIBERO","soitsrltmprdtvhclmvmntowh_8\n(vehicle_history","분석유닉스시각","anls_unix_tm",1,"NUMBER(10)","PK",null,"분석 대상기간 시작시각",{"$nulls":4},"분석유닉스시각","anls_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":10},"CREATE TABLE ",{"$f":"N322&\" (\"","v":"soitsrltmprdtvhclmvmntowh_8 ("},{"$f":"O324&\" \"","v":"anls_unix_tm "},{"$f":"R324&\" \"","v":"NUMBER(10) "},{"$f":"IF(H324=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",null,"(",{"$f":"IF(OR(G324=\"PK\", G324=\"PK/FK\"), O324, \"\")","v":"anls_unix_tm"},",","COMMENT ON COLUMN ",{"$f":"$N$322&\".\"","v":"soitsrltmprdtvhclmvmntowh_8."},{"$f":"O324","v":"anls_unix_tm"}," IS ",{"$f":"\"'\"&I324&\"'\"","v":"'분석 대상기간 시작시각'"},";",null,null,null,""]
[null,null,"위치수집유닉스시각","locn_clct_unix_tm",2,"NUMBER(10)","PK",null,"위치수집유닉스시각",{"$nulls":4},"위치수집유닉스시각","locn_clct_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":12},"locn_clct_unix_tm ","NUMBER(10) ","",",",null,null,"locn_clct_unix_tm",",","COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_8.","locn_clct_unix_tm"," IS ","'위치수집유닉스시각'",";"]
[null,null,"차량ID","vhcl_id",4,"VARCHAR2(150)","PK",null,"차량ID",{"$nulls":4},"차량ID","vhcl_id","VARCHAR2(150)","VARCHAR(150)","VARCHAR2(150)",{"$nulls":12},"vhcl_id ","VARCHAR2(150) ","",",",null,null,"vhcl_id",")","COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_8.","vhcl_id"," IS ","'차량ID'",";"]
[null,null,"차로ID","lane_id",5,"VARCHAR2(300)","FK",null,"통행차로ID",{"$nulls":4},"차로ID","lane_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",{"$nulls":12},"lane_id ","VARCHAR2(300) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_8.","lane_id"," IS ","'통행차로ID'",";",null,null,null,{"$f":"IF(LEFT(AE327, 13) = \"CONSTRAINT PK\", AE327, \"\")","v":""}]
[null,null,"세그먼트ID","sgmn_id",6,"VARCHAR2(300)","FK","NOT NULL","통행세그먼트ID",{"$nulls":4},"세그먼트ID","sgmn_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",{"$nulls":12},"sgmn_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_8.","sgmn_id"," IS ","'통행세그먼트ID'",";"]
[null,null,"차종코드","kncr_cd",7,"CHAR(10)",null,null,"차종 (008)",{"$nulls":4},"차종코드","kncr_cd","CHAR(10)","VARCHAR(10)","VARCHAR2(10)",{"$nulls":12},"kncr_cd ","VARCHAR2(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_8.","kncr_cd"," IS ","'차종 (008)'",";"]
[null,null,"순간속도","mmnt_sped",8,"NUMBER(5,2)",null,null,"순간속도 (m/s)",{"$nulls":4},"순간속도","mmnt_sped","NUMBER(5,2)","FLOAT","NUMBER(5,2)",{"$nulls":12},"mmnt_sped ","NUMBER(5,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_8.","mmnt_sped"," IS ","'순간속도 (m/s)'",";"]
[null,null,"비혼잡속도","non_cngt_sped",9,"NUMBER(5,2)",null,null,"비혼잡속도 (m/s)",{"$nulls":4},"비혼잡속도","non_cngt_sped","NUMBER(5,2)","FLOAT","NUMBER(5,2)",{"$nulls":12},"non_cngt_sped ","NUMBER(5,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_8.","non_cngt_sped"," IS ","'비혼잡속도 (m/s)'",";"]
[null,null,"차량경도","vhcl_lot",10,"NUMBER(13,10)",null,null,"차량경도",{"$nulls":4},"차량경도","vhcl_lot","NUMBER(13,10)","FLOAT","NUMBER(13,10)",{"$nulls":12},"vhcl_lot ","NUMBER(13,10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_8.","vhcl_lot"," IS ","'차량경도'",";"]
[null,null,"차량위도","vhcl_lat",11,"NUMBER(12,10)",null,null,"차량위도",{"$nulls":4},"차량위도","vhcl_lat","NUMBER(12,10)","FLOAT","NUMBER(12,10)",{"$nulls":12},"vhcl_lat ","NUMBER(12,10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_8.","vhcl_lat"," IS ","'차량위도'",";"]
[null,null,"차량고도","vhcl_lntd",12,"NUMBER(10)",null,null,"차량고도",{"$nulls":4},"차량고도","vhcl_lntd","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":12},"vhcl_lntd ","NUMBER(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_8.","vhcl_lntd"," IS ","'차량고도'",";"]
[null,null,"이동방위각도","mvmn_pocm_angl",13,"NUMBER(6,3)",null,null,"이동방위각도",{"$nulls":4},"이동방위각도","mvmn_pocm_angl","NUMBER(6,3)","FLOAT","NUMBER(6,3)",{"$nulls":12},"mvmn_pocm_angl ","NUMBER(6,3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_8.","mvmn_pocm_angl"," IS ","'이동방위각도'",";"]
[null,null,"이동경사각도","mvmn_slop_angl",14,"NUMBER(6,3)",null,null,"이동경사각도",{"$nulls":4},"이동경사각도","mvmn_slop_angl","NUMBER(6,3)","FLOAT","NUMBER(6,3)",{"$nulls":12},"mvmn_slop_angl ","NUMBER(6,3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_8.","mvmn_slop_angl"," IS ","'이동경사각도'",";"]
[null,null,"차로진행거리","lane_prgrs_dstn",15,"NUMBER(7,2)",null,null,"통행차로진행거리",{"$nulls":4},"차로진행거리","lane_prgrs_dstn","NUMBER(19,9)","FLOAT","NUMBER(19,9)",{"$nulls":12},"lane_prgrs_dstn ","NUMBER(19,9) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_8.","lane_prgrs_dstn"," IS ","'통행차로진행거리'",";"]
[null,null,"대기행렬관측여부","queu_obsrvn_yn",16,"CHAR(1)",null,null,"대기행렬관측여부 (503)",{"$nulls":4},"대기행렬관측여부","queu_obsrvn_yn","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",{"$nulls":12},"queu_obsrvn_yn ","VARCHAR2(1) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_8.","queu_obsrvn_yn"," IS ","'대기행렬관측여부 (503)'",";"]
[null,null,"지역구분코드","rgn_prttn_cd",17,"CHAR(2)","FK","NOT NULL","지역분할코드(051)",{"$nulls":4},"지역분할코드","rgn_prttn_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",{"$nulls":12},"rgn_prttn_cd ","VARCHAR2(2) ","NOT NULL",{"$f":"\") TABLESPACE \"&AI341&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_C008 NOLOGGING"},null,null,{"$f":"IF(OR(F339=\"PK\", F339=\"PK/FK\"), H339, \"\")","v":""},null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_8.","rgn_prttn_cd"," IS ","'지역분할코드(051)'",";"]
[{"$nulls":30},{"$f":"CONCATENATE(AI340:AK340)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (locn_clct_unix_tm) INTERVAL (3600) STORE IN (\"&AI341&\") (PARTITION BFR_\" & N322& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AI341&\");\"","v":"PARTITION BY RANGE (locn_clct_unix_tm) INTERVAL (3600) STORE IN (SOIT_D08_C008) (PARTITION BFR_soitsrltmprdtvhclmvmntowh_8_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_C008);"},{"$f":"\"CREATE INDEX PK_\" & N322& \" ON \" & N322 & CONCATENATE(AJ324:AL338) & \" LOCAL (PARTITION BFR_\" & N322 & \"_20221101 TABLESPACE \"&AJ341&\") TABLESPACE \"&AJ341&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & N322 & \" ADD CONSTRAINT PK_\" & N322 & \" PRIMARY KEY \" & CONCATENATE(AJ324:AL338) & \";\"","v":{"$error":"#VALUE!"}}]
[{"$nulls":34},"SOIT_D08_C008","SOIT_I08_C008"]
[null,"[5분] 실시간 차량이동궤적 테이블(예측) - 9지역",{"$nulls":11},"soitsrltmprdtvhclmvmntowh_9",{"$nulls":33},{"$f":"IF(LEFT(AE342, 13) = \"CONSTRAINT PK\", AE342, \"\")","v":""}]
[27,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N342&\" \"","v":"soitsrltmprdtvhclmvmntowh_9 "},null," IS ",{"$f":"\"'\"&B342&\"'\"","v":"'[5분] 실시간 차량이동궤적 테이블(예측) - 9지역'"},";",null,null,null,""]
["TIBERO","soitsrltmprdtvhclmvmntowh_9\n(vehicle_history","분석유닉스시각","anls_unix_tm",1,"NUMBER(10)","PK",null,"분석 대상기간 시작시각",{"$nulls":4},"분석유닉스시각","anls_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":10},"CREATE TABLE ",{"$f":"N342&\" (\"","v":"soitsrltmprdtvhclmvmntowh_9 ("},{"$f":"O344&\" \"","v":"anls_unix_tm "},{"$f":"R344&\" \"","v":"NUMBER(10) "},{"$f":"IF(H344=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",null,"(",{"$f":"IF(OR(G344=\"PK\", G344=\"PK/FK\"), O344, \"\")","v":"anls_unix_tm"},",","COMMENT ON COLUMN ",{"$f":"$N$342&\".\"","v":"soitsrltmprdtvhclmvmntowh_9."},{"$f":"O344","v":"anls_unix_tm"}," IS ",{"$f":"\"'\"&I344&\"'\"","v":"'분석 대상기간 시작시각'"},";",null,null,null,""]
[null,null,"위치수집유닉스시각","locn_clct_unix_tm",2,"NUMBER(10)","PK",null,"위치수집유닉스시각",{"$nulls":4},"위치수집유닉스시각","locn_clct_unix_tm","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":12},"locn_clct_unix_tm ","NUMBER(10) ","",",",null,null,"locn_clct_unix_tm",",","COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_9.","locn_clct_unix_tm"," IS ","'위치수집유닉스시각'",";"]
[null,null,"차량ID","vhcl_id",4,"VARCHAR2(150)","PK",null,"차량ID",{"$nulls":4},"차량ID","vhcl_id","VARCHAR2(150)","VARCHAR(150)","VARCHAR2(150)",{"$nulls":12},"vhcl_id ","VARCHAR2(150) ","",",",null,null,"vhcl_id",")","COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_9.","vhcl_id"," IS ","'차량ID'",";"]
[null,null,"차로ID","lane_id",5,"VARCHAR2(300)","FK",null,"통행차로ID",{"$nulls":4},"차로ID","lane_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",{"$nulls":12},"lane_id ","VARCHAR2(300) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_9.","lane_id"," IS ","'통행차로ID'",";",null,null,null,{"$f":"IF(LEFT(AE347, 13) = \"CONSTRAINT PK\", AE347, \"\")","v":""}]
[null,null,"세그먼트ID","sgmn_id",6,"VARCHAR2(300)","FK","NOT NULL","통행세그먼트ID",{"$nulls":4},"세그먼트ID","sgmn_id","VARCHAR2(300)","VARCHAR(300)","VARCHAR2(300)",{"$nulls":12},"sgmn_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_9.","sgmn_id"," IS ","'통행세그먼트ID'",";"]
[null,null,"차종코드","kncr_cd",7,"CHAR(10)",null,null,"차종 (008)",{"$nulls":4},"차종코드","kncr_cd","CHAR(10)","VARCHAR(10)","VARCHAR2(10)",{"$nulls":12},"kncr_cd ","VARCHAR2(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_9.","kncr_cd"," IS ","'차종 (008)'",";"]
[null,null,"순간속도","mmnt_sped",8,"NUMBER(5,2)",null,null,"순간속도 (m/s)",{"$nulls":4},"순간속도","mmnt_sped","NUMBER(5,2)","FLOAT","NUMBER(5,2)",{"$nulls":12},"mmnt_sped ","NUMBER(5,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_9.","mmnt_sped"," IS ","'순간속도 (m/s)'",";"]
[null,null,"비혼잡속도","non_cngt_sped",9,"NUMBER(5,2)",null,null,"비혼잡속도 (m/s)",{"$nulls":4},"비혼잡속도","non_cngt_sped","NUMBER(5,2)","FLOAT","NUMBER(5,2)",{"$nulls":12},"non_cngt_sped ","NUMBER(5,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_9.","non_cngt_sped"," IS ","'비혼잡속도 (m/s)'",";"]
[null,null,"차량경도","vhcl_lot",10,"NUMBER(13,10)",null,null,"차량경도",{"$nulls":4},"차량경도","vhcl_lot","NUMBER(13,10)","FLOAT","NUMBER(13,10)",{"$nulls":12},"vhcl_lot ","NUMBER(13,10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_9.","vhcl_lot"," IS ","'차량경도'",";"]
[null,null,"차량위도","vhcl_lat",11,"NUMBER(12,10)",null,null,"차량위도",{"$nulls":4},"차량위도","vhcl_lat","NUMBER(12,10)","FLOAT","NUMBER(12,10)",{"$nulls":12},"vhcl_lat ","NUMBER(12,10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_9.","vhcl_lat"," IS ","'차량위도'",";"]
[null,null,"차량고도","vhcl_lntd",12,"NUMBER(10)",null,null,"차량고도",{"$nulls":4},"차량고도","vhcl_lntd","NUMBER(10)","INTEGER","NUMBER(10)",{"$nulls":12},"vhcl_lntd ","NUMBER(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_9.","vhcl_lntd"," IS ","'차량고도'",";"]
[null,null,"이동방위각도","mvmn_pocm_angl",13,"NUMBER(6,3)",null,null,"이동방위각도",{"$nulls":4},"이동방위각도","mvmn_pocm_angl","NUMBER(6,3)","FLOAT","NUMBER(6,3)",{"$nulls":12},"mvmn_pocm_angl ","NUMBER(6,3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_9.","mvmn_pocm_angl"," IS ","'이동방위각도'",";"]
[null,null,"이동경사각도","mvmn_slop_angl",14,"NUMBER(6,3)",null,null,"이동경사각도",{"$nulls":4},"이동경사각도","mvmn_slop_angl","NUMBER(6,3)","FLOAT","NUMBER(6,3)",{"$nulls":12},"mvmn_slop_angl ","NUMBER(6,3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_9.","mvmn_slop_angl"," IS ","'이동경사각도'",";"]
[null,null,"차로진행거리","lane_prgrs_dstn",15,"NUMBER(7,2)",null,null,"통행차로진행거리",{"$nulls":4},"차로진행거리","lane_prgrs_dstn","NUMBER(19,9)","FLOAT","NUMBER(19,9)",{"$nulls":12},"lane_prgrs_dstn ","NUMBER(19,9) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_9.","lane_prgrs_dstn"," IS ","'통행차로진행거리'",";"]
[null,null,"대기행렬관측여부","queu_obsrvn_yn",16,"CHAR(1)",null,null,"대기행렬관측여부 (503)",{"$nulls":4},"대기행렬관측여부","queu_obsrvn_yn","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",{"$nulls":12},"queu_obsrvn_yn ","VARCHAR2(1) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_9.","queu_obsrvn_yn"," IS ","'대기행렬관측여부 (503)'",";"]
[null,null,"지역구분코드","rgn_prttn_cd",17,"CHAR(2)","FK","NOT NULL","지역분할코드(051)",{"$nulls":4},"지역분할코드","rgn_prttn_cd","CHAR(2)","VARCHAR(2)","VARCHAR2(2)",{"$nulls":12},"rgn_prttn_cd ","VARCHAR2(2) ","NOT NULL",{"$f":"\") TABLESPACE \"&AI361&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_C009 NOLOGGING"},null,null,{"$f":"IF(OR(F359=\"PK\", F359=\"PK/FK\"), H359, \"\")","v":""},null,"COMMENT ON COLUMN ","soitsrltmprdtvhclmvmntowh_9.","rgn_prttn_cd"," IS ","'지역분할코드(051)'",";"]
[{"$nulls":30},{"$f":"CONCATENATE(AI360:AK360)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (locn_clct_unix_tm) INTERVAL (3600) STORE IN (\"&AI361&\") (PARTITION BFR_\" & N342& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AI361&\");\"","v":"PARTITION BY RANGE (locn_clct_unix_tm) INTERVAL (3600) STORE IN (SOIT_D08_C009) (PARTITION BFR_soitsrltmprdtvhclmvmntowh_9_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_C009);"},{"$f":"\"CREATE INDEX PK_\" & N342& \" ON \" & N342 & CONCATENATE(AJ344:AL358) & \" LOCAL (PARTITION BFR_\" & N342 & \"_20221101 TABLESPACE \"&AJ361&\") TABLESPACE \"&AJ361&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & N342 & \" ADD CONSTRAINT PK_\" & N342 & \" PRIMARY KEY \" & CONCATENATE(AJ344:AL358) & \";\"","v":{"$error":"#VALUE!"}}]
[{"$nulls":34},"SOIT_D08_C009","SOIT_I08_C009"]
[null,"[5분] 실시간 차량번호정보 테이블",{"$nulls":11},"soitsrltmvhclnoinfo",{"$nulls":33},{"$f":"IF(LEFT(AE362, 13) = \"CONSTRAINT PK\", AE362, \"\")","v":""}]
[28,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N362&\" \"","v":"soitsrltmvhclnoinfo "},null," IS ",{"$f":"\"'\"&B362&\"'\"","v":"'[5분] 실시간 차량번호정보 테이블'"},";",null,null,null,""]
["TIBERO","soitsrltmvhclnoinfo\n(tibero)","분석유닉스시각","anls_unix_tm",1,"NUMBER(10)","PK",null,"분석 대상기간 시작시각",{"$nulls":4},"분석유닉스시각","anls_unix_tm","NUMBER(10)",null,"NUMBER(10)",{"$nulls":10},"CREATE TABLE ",{"$f":"N362&\" (\"","v":"soitsrltmvhclnoinfo ("},{"$f":"O364&\" \"","v":"anls_unix_tm "},{"$f":"R364&\" \"","v":"NUMBER(10) "},{"$f":"IF(H364=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",null,"(",{"$f":"IF(OR(G364=\"PK\", G364=\"PK/FK\"), O364, \"\")","v":"anls_unix_tm"},",","COMMENT ON COLUMN ",{"$f":"$N$362&\".\"","v":"soitsrltmvhclnoinfo."},{"$f":"O364","v":"anls_unix_tm"}," IS ",{"$f":"\"'\"&I364&\"'\"","v":"'분석 대상기간 시작시각'"},";",null,null,null,""]
[null,null,"지역분할코드","rgn_prttn_cd",1,"CHAR(2)","PK/FK","NOT NULL","지역분할코드 (051)",{"$nulls":4},"지역분할코드","rgn_prttn_cd","CHAR(2)",null,"VARCHAR2(2)",{"$nulls":12},"rgn_prttn_cd ","VARCHAR2(2) ","NOT NULL",",",null,null,"rgn_prttn_cd",",","COMMENT ON COLUMN ","soitsrltmvhclnoinfo.","rgn_prttn_cd"," IS ","'지역분할코드 (051)'",";"]
[null,null,"차량ID","vhcl_id",3,"VARCHAR2(150)","PK",null,"차량ID",{"$nulls":4},"차량ID","vhcl_id","VARCHAR2(150)","VARCHAR(150)","VARCHAR2(150)",{"$nulls":12},"vhcl_id ","VARCHAR2(150) ","",",",null,null,"vhcl_id",",","COMMENT ON COLUMN ","soitsrltmvhclnoinfo.","vhcl_id"," IS ","'차량ID'",";",null,null,null,{"$f":"IF(LEFT(AE366, 13) = \"CONSTRAINT PK\", AE366, \"\")","v":""}]
[null,null,"실측여부","acsr_yn",null,"CHAR(1)","PK",null,"실측여부(500)",{"$nulls":4},"실측여부","acsr_yn","CHAR(1)","VARCHAR(1)","VARCHAR2(1)",{"$nulls":12},"acsr_yn ","VARCHAR2(1) ","",",",null,null,"acsr_yn",")","COMMENT ON COLUMN ","soitsrltmvhclnoinfo.","acsr_yn"," IS ","'실측여부(500)'",";"]
[null,null,"차량번호","vhcl_no",4,"VARCHAR2(200)",null,null,"차량번호",{"$nulls":4},"차량번호","vhcl_no","VARCHAR2(200)",null,"VARCHAR2(200)",{"$nulls":12},"vhcl_no ","VARCHAR2(200) ","",{"$f":"\") TABLESPACE \"&AI370&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_C009 NOLOGGING"},null,null,{"$f":"IF(OR(F368=\"PK\", F368=\"PK/FK\"), H368, \"\")","v":""},null,"COMMENT ON COLUMN ","soitsrltmvhclnoinfo.","vhcl_no"," IS ","'차량번호'",";",null,null,null,{"$f":"IF(LEFT(AE368, 13) = \"CONSTRAINT PK\", AE368, \"\")","v":""}]
[{"$nulls":30},{"$f":"CONCATENATE(AI369:AK369)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (anls_unix_tm) INTERVAL (3600) STORE IN (\"&AI370&\") (PARTITION BFR_\" & N362& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AI370&\");\"","v":"PARTITION BY RANGE (anls_unix_tm) INTERVAL (3600) STORE IN (SOIT_D08_C009) (PARTITION BFR_soitsrltmvhclnoinfo_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_C009);"},{"$f":"\"CREATE INDEX PK_\" & N362& \" ON \" & N362 & CONCATENATE(AJ364:AL367) & \" LOCAL (PARTITION BFR_\" & N362 & \"_20221101 TABLESPACE \"&AJ370&\") TABLESPACE \"&AJ370&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & N362 & \" ADD CONSTRAINT PK_\" & N362 & \" PRIMARY KEY \" & CONCATENATE(AJ364:AL367) & \";\"","v":{"$error":"#VALUE!"}}]
[{"$nulls":34},"SOIT_D08_C009","SOIT_I08_C009"]
[]
[null,"실시간 신호변경이력 (실측) 테이블",{"$nulls":11},"soitsrltmacsrsgnlchghstr",{"$nulls":33},{"$f":"IF(LEFT(AE372, 13) = \"CONSTRAINT PK\", AE372, \"\")","v":""}]
["26-1","Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N372&\" \"","v":"soitsrltmacsrsgnlchghstr "},null," IS ",{"$f":"\"'\"&B372&\"'\"","v":"'실시간 신호변경이력 (실측) 테이블'"},";",null,null,null,""]
["TIBERO","soitsrltmacsrsgnlchghstr\n(signal_history)\n(확정)","수집유닉스시각","clct_unix_tm",1,"NUMBER(10)","PK",null,"동인 신호이력수집시각",null,null,null,{"$f":"IF(F374=P374, \"EQ\", \"NEQ)\")","v":"EQ"},"수집유닉스시각","clct_unix_tm","NUMBER(10)",null,"NUMBER(10)",{"$nulls":10},"CREATE TABLE ",{"$f":"N372&\" (\"","v":"soitsrltmacsrsgnlchghstr ("},{"$f":"O374&\" \"","v":"clct_unix_tm "},{"$f":"R374&\" \"","v":"NUMBER(10) "},{"$f":"IF(H374=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",null,"(",{"$f":"IF(OR(G374=\"PK\", G374=\"PK/FK\"), O374, \"\")","v":"clct_unix_tm"},",","COMMENT ON COLUMN ",{"$f":"$N$372&\".\"","v":"soitsrltmacsrsgnlchghstr."},{"$f":"O374","v":"clct_unix_tm"}," IS ",{"$f":"\"'\"&I374&\"'\"","v":"'동인 신호이력수집시각'"},";",null,null,null,""]
[null,null,"시작유닉스시각","bgng_unix_tm",2,"NUMBER(10)","PK",null,"신호 시작시각(현시)",{"$nulls":4},"시작유닉스시각","bgng_unix_tm","NUMBER(10)",null,"NUMBER(10)",{"$nulls":12},"bgng_unix_tm ","NUMBER(10) ","",",",null,null,"bgng_unix_tm",",","COMMENT ON COLUMN ","soitsrltmacsrsgnlchghstr.","bgng_unix_tm"," IS ","'신호 시작시각(현시)'",";"]
[null,null,"현시시작시간","phas_bgng_unix_tm",3,"NUMBER(10)","PK",null,"신호 시작시각(현시)",{"$nulls":4},"현시시작시간","phas_bgng_unix_tm","NUMBER(10)",null,"NUMBER(10)",{"$nulls":12},"phas_bgng_unix_tm ","NUMBER(10) ","",",",null,null,"phas_bgng_unix_tm",",","COMMENT ON COLUMN ","soitsrltmacsrsgnlchghstr.","phas_bgng_unix_tm"," IS ","'신호 시작시각(현시)'",";"]
[null,null,"현장교차로ID","spot_ints_id",5,"NUMBER(5)","PK",null,"현장교차로ID",{"$nulls":4},"현장교차로ID","spot_ints_id","NUMBER(5)",null,"NUMBER(5)",{"$nulls":12},"spot_ints_id ","NUMBER(5) ","",",",null,null,"spot_ints_id",",","COMMENT ON COLUMN ","soitsrltmacsrsgnlchghstr.","spot_ints_id"," IS ","'현장교차로ID'",";"]
[null,null,"노드ID","node_id",6,"VARCHAR2(300)","PK",null,"해당 교차로 노드ID",{"$nulls":4},"노드ID","node_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":12},"node_id ","VARCHAR2(300) ","",",",null,null,"node_id",",","COMMENT ON COLUMN ","soitsrltmacsrsgnlchghstr.","node_id"," IS ","'해당 교차로 노드ID'",";"]
[null,null,"신호상태코드","sgnl_stts_cd",7,"CHAR(1)",null,null,"신호상태코드 (505)",{"$nulls":4},"신호상태코드","sgnl_stts_cd","CHAR(1)",null,"CHAR(1)",{"$nulls":12},"sgnl_stts_cd ","CHAR(1) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmacsrsgnlchghstr.","sgnl_stts_cd"," IS ","'신호상태코드 (505)'",";"]
[null,null,"연결차로ID","cnct_lane_id",8,"VARCHAR2(300)","PK",null,"연결차로ID",{"$nulls":4},"연결차로ID","cnct_lane_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":12},"cnct_lane_id ","VARCHAR2(300) ","",",",null,null,"cnct_lane_id",",","COMMENT ON COLUMN ","soitsrltmacsrsgnlchghstr.","cnct_lane_id"," IS ","'연결차로ID'",";"]
[null,null,"현시번호","phas_no",9,"NUMBER(2)","PK",null,"현시번호 (1~8)",{"$nulls":4},"현시번호","phas_no","NUMBER(2)",null,"NUMBER(2)",{"$nulls":12},"phas_no ","NUMBER(2) ","",",",null,null,"phas_no",")","COMMENT ON COLUMN ","soitsrltmacsrsgnlchghstr.","phas_no"," IS ","'현시번호 (1~8)'",";"]
[null,null,"입력일시","inpt_dt",10,"TIMESTAMP",null,"NOT NULL","데이터입력일시",{"$nulls":4},"입력일시","inpt_dt","TIMESTAMP",null,"TIMESTAMP",{"$nulls":12},"inpt_dt ","TIMESTAMP ","NOT NULL",{"$f":"\") TABLESPACE \"&AI384&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_S001 NOLOGGING"},null,null,{"$f":"IF(OR(F382=\"PK\", F382=\"PK/FK\"), H382, \"\")","v":""},null,"COMMENT ON COLUMN ","soitsrltmacsrsgnlchghstr.","inpt_dt"," IS ","'데이터입력일시'",";"]
[{"$nulls":30},{"$f":"CONCATENATE(AI383:AK383)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (clct_unix_tm) INTERVAL (3600) STORE IN (\"&AI384&\") (PARTITION BFR_\" & N372& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AI384&\");\"","v":"PARTITION BY RANGE (clct_unix_tm) INTERVAL (3600) STORE IN (SOIT_D08_S001) (PARTITION BFR_soitsrltmacsrsgnlchghstr_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_S001);"},{"$f":"\"CREATE INDEX PK_\" & N372& \" ON \" & N372 & CONCATENATE(AJ374:AL381) & \" LOCAL (PARTITION BFR_\" & N372 & \"_20221101 TABLESPACE \"&AJ384&\") TABLESPACE \"&AJ384&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & N372 & \" ADD CONSTRAINT PK_\" & N372 & \" PRIMARY KEY \" & CONCATENATE(AJ374:AL381) & \";\"","v":{"$error":"#VALUE!"}}]
[{"$nulls":34},"SOIT_D08_S001","SOIT_I08_S001"]
[null,"실시간 신호변경이력 (예측) 테이블",{"$nulls":11},"soitsrltmprdtsgnlchghstr",{"$nulls":33},{"$f":"IF(LEFT(AE385, 13) = \"CONSTRAINT PK\", AE385, \"\")","v":""}]
["26-1","Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment","최명훈 의견","박산하 의견",null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N385&\" \"","v":"soitsrltmprdtsgnlchghstr "},null," IS ",{"$f":"\"'\"&B385&\"'\"","v":"'실시간 신호변경이력 (예측) 테이블'"},";",null,null,null,""]
["TIBERO","soitsrltmprdtsgnlchghstr\n(signal_history)\n(확정)","수집유닉스시각","clct_unix_tm",1,"NUMBER(10)","PK",null,"동인 신호이력수집시각",null,null,null,{"$f":"IF(F387=P387, \"EQ\", \"NEQ)\")","v":"EQ"},"수집유닉스시각","clct_unix_tm","NUMBER(10)",null,"NUMBER(10)",{"$nulls":10},"CREATE TABLE ",{"$f":"N385&\" (\"","v":"soitsrltmprdtsgnlchghstr ("},{"$f":"O387&\" \"","v":"clct_unix_tm "},{"$f":"R387&\" \"","v":"NUMBER(10) "},{"$f":"IF(H387=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",",null,"(",{"$f":"IF(OR(G387=\"PK\", G387=\"PK/FK\"), O387, \"\")","v":"clct_unix_tm"},",","COMMENT ON COLUMN ",{"$f":"$N$385&\".\"","v":"soitsrltmprdtsgnlchghstr."},{"$f":"O387","v":"clct_unix_tm"}," IS ",{"$f":"\"'\"&I387&\"'\"","v":"'동인 신호이력수집시각'"},";",null,null,null,""]
[null,null,"시작유닉스시각","bgng_unix_tm",2,"NUMBER(10)","PK",null,"신호 시작시각(현시)",{"$nulls":4},"시작유닉스시각","bgng_unix_tm","NUMBER(10)",null,"NUMBER(10)",{"$nulls":12},"bgng_unix_tm ","NUMBER(10) ","",",",null,null,"bgng_unix_tm",",","COMMENT ON COLUMN ","soitsrltmprdtsgnlchghstr.","bgng_unix_tm"," IS ","'신호 시작시각(현시)'",";"]
[null,null,"현시시작시간","phas_bgng_unix_tm",3,"NUMBER(10)","PK",null,"신호 시작시각(현시)",{"$nulls":4},"현시시작시간","phas_bgng_unix_tm","NUMBER(10)",null,"NUMBER(10)",{"$nulls":12},"phas_bgng_unix_tm ","NUMBER(10) ","",",",null,null,"phas_bgng_unix_tm",",","COMMENT ON COLUMN ","soitsrltmprdtsgnlchghstr.","phas_bgng_unix_tm"," IS ","'신호 시작시각(현시)'",";"]
[null,null,"현장교차로ID","spot_ints_id",5,"NUMBER(5)","PK",null,"현장교차로ID",{"$nulls":4},"현장교차로ID","spot_ints_id","NUMBER(5)",null,"NUMBER(5)",{"$nulls":12},"spot_ints_id ","NUMBER(5) ","",",",null,null,"spot_ints_id",",","COMMENT ON COLUMN ","soitsrltmprdtsgnlchghstr.","spot_ints_id"," IS ","'현장교차로ID'",";"]
[null,null,"노드ID","node_id",6,"VARCHAR2(300)","PK",null,"해당 교차로 노드ID",{"$nulls":4},"노드ID","node_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":12},"node_id ","VARCHAR2(300) ","",",",null,null,"node_id",",","COMMENT ON COLUMN ","soitsrltmprdtsgnlchghstr.","node_id"," IS ","'해당 교차로 노드ID'",";"]
[null,null,"신호상태코드","sgnl_stts_cd",7,"CHAR(1)",null,null,"신호상태코드 (505)",{"$nulls":4},"신호상태코드","sgnl_stts_cd","CHAR(1)",null,"CHAR(1)",{"$nulls":12},"sgnl_stts_cd ","CHAR(1) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsrltmprdtsgnlchghstr.","sgnl_stts_cd"," IS ","'신호상태코드 (505)'",";"]
[null,null,"연결차로ID","cnct_lane_id",8,"VARCHAR2(300)","PK",null,"연결차로ID",{"$nulls":4},"연결차로ID","cnct_lane_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":12},"cnct_lane_id ","VARCHAR2(300) ","",",",null,null,"cnct_lane_id",",","COMMENT ON COLUMN ","soitsrltmprdtsgnlchghstr.","cnct_lane_id"," IS ","'연결차로ID'",";"]
[null,null,"현시번호","phas_no",9,"NUMBER(2)","PK",null,"현시번호 (1~8)",{"$nulls":4},"현시번호","phas_no","NUMBER(2)",null,"NUMBER(2)",{"$nulls":12},"phas_no ","NUMBER(2) ","",",",null,null,"phas_no",")","COMMENT ON COLUMN ","soitsrltmprdtsgnlchghstr.","phas_no"," IS ","'현시번호 (1~8)'",";"]
[null,null,"입력일시","inpt_dt",10,"TIMESTAMP",null,"NOT NULL","데이터입력일시",{"$nulls":4},"입력일시","inpt_dt","TIMESTAMP",null,"TIMESTAMP",{"$nulls":12},"inpt_dt ","TIMESTAMP ","NOT NULL",{"$f":"\") TABLESPACE \"&AI397&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_S002 NOLOGGING"},null,null,{"$f":"IF(OR(F395=\"PK\", F395=\"PK/FK\"), H395, \"\")","v":""},null,"COMMENT ON COLUMN ","soitsrltmprdtsgnlchghstr.","inpt_dt"," IS ","'데이터입력일시'",";"]
[{"$nulls":30},{"$f":"CONCATENATE(AI396:AK396)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (clct_unix_tm) INTERVAL (3600) STORE IN (\"&AI397&\") (PARTITION BFR_\" & N385& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AI397&\");\"","v":"PARTITION BY RANGE (clct_unix_tm) INTERVAL (3600) STORE IN (SOIT_D08_S002) (PARTITION BFR_soitsrltmprdtsgnlchghstr_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_S002);"},{"$f":"\"CREATE INDEX PK_\" & N385& \" ON \" & N385 & CONCATENATE(AJ387:AL394) & \" LOCAL (PARTITION BFR_\" & N385 & \"_20221101 TABLESPACE \"&AJ397&\") TABLESPACE \"&AJ397&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & N385 & \" ADD CONSTRAINT PK_\" & N385 & \" PRIMARY KEY \" & CONCATENATE(AJ387:AL394) & \";\"","v":{"$error":"#VALUE!"}}]
[{"$nulls":34},"SOIT_D08_S002","SOIT_I08_S002"]

{"sheet":"SUMO-최적화","index":10,"n_rows":192,"n_cols":48,"rows_kept":192,"cut":false,"hidden":false,"merged":[[3,1,3,10],[3,13,3,15],[5,1,26,1],[29,1,29,10],[29,13,29,17],[38,1,38,10],[38,13,38,17],[31,1,35,1],[40,1,61,1],[46,9,61,9],[64,1,64,10],[64,13,64,17],[106,1,106,10],[106,13,106,17],[155,1,155,10],[114,1,114,10],[114,13,114,17],[127,1,127,10],[127,13,127,17],[140,1,140,10],[140,13,140,17],[155,13,155,17],[171,13,171,17],[178,1,178,10],[178,13,178,17],[185,1,185,10],[185,13,185,17],[180,1,182,1],[187,1,189,1],[66,1,100,1],[108,1,110,1],[116,1,124,1],[129,1,136,1],[142,1,151,1],[157,1,168,1],[173,1,175,1],[171,1,171,10]]}
[]
[null,"신호최적화 결과 집계 테이블은 모니터링 테이블에 '시나리오번호' / '분석일자' 등 조회조건에 해당되는 컬럼 추가하여 테이블 관리",{"$nulls":45},{"$f":"IF(LEFT(AE2, 13) = \"CONSTRAINT PK\", AE2, \"\")","v":""}]
[{"$nulls":47},""]
[null,"분석처리상태 테이블",{"$nulls":11},"soitsanlsprcsinfo",{"$nulls":33},""]
[31,"Table Name","Attribute Name","Column Name","#","Data type","PK/FK","Column Null Option","Comment",{"$nulls":4},"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N4&\" \"","v":"soitsanlsprcsinfo "},null," IS ",{"$f":"\"'\"&B4&\"'\"","v":"'분석처리상태 테이블'"},";",null,null,null,""]
["TIBERO","soitsanlsprcsinfo","시나리오ID","scnr_id",null,"VARCHAR2(40)","PK",null,"시나리오ID","시나리오 고유 id (백단에서 seq)",null,null,null,"시나리오ID","scnr_id","VARCHAR2(40)",null,"VARCHAR2(40)",{"$nulls":10},"CREATE TABLE ",{"$f":"N4&\" (\"","v":"soitsanlsprcsinfo ("},{"$f":"O6&\" \"","v":"scnr_id "},{"$f":"R6&\" \"","v":"VARCHAR2(40) "},{"$f":"IF(H6=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",","CONSTRAINT ",{"$f":"\"PK_\"&N4&\" PRIMARY KEY (\"","v":"PK_soitsanlsprcsinfo PRIMARY KEY ("},{"$f":"IF(OR(G6=\"PK\", G6=\"PK/FK\"), O6, \"\")","v":"scnr_id"},",","COMMENT ON COLUMN ",{"$f":"$N$4&\".\"","v":"soitsanlsprcsinfo."},{"$f":"O6","v":"scnr_id"}," IS ",{"$f":"\"'\"&I6&\"'\"","v":"'시나리오ID'"},";",null,null,null,""]
[null,null,"운영구분코드","oper_se_cd",null,"VARCHAR2(1)",null,null,"운영구분코드 (901)","(1:실운영, 2:시범운영)",null,null,null,"운영구분코드","oper_se_cd","VARCHAR2(1)",null,"VARCHAR2(1)",{"$nulls":12},"oper_se_cd ","VARCHAR2(1) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsanlsprcsinfo.","oper_se_cd"," IS ","'운영구분코드 (901)'",";"]
[null,null,"분석구분코드","anls_div_cd",null,"VARCHAR2(1)","PK",null,"분석구분코드 (902)","(1:현황. 2:최적화)",null,null,null,"분석구분코드","anls_div_cd","VARCHAR2(1)",null,"VARCHAR2(1)",{"$nulls":12},"anls_div_cd ","VARCHAR2(1) ","",",",null,null,"anls_div_cd",{"$f":"\") using index tablespace \" &AJ29& \") TABLESPACE \" &AI29&\";\"","v":") using index tablespace SOIT_I08_A001) TABLESPACE SOIT_D08_A001;"},"COMMENT ON COLUMN ","soitsanlsprcsinfo.","anls_div_cd"," IS ","'분석구분코드 (902)'",";",null,null,null,{"$f":"IF(LEFT(AE8, 13) = \"CONSTRAINT PK\", AE8, \"\")","v":""}]
[null,null,"시나리오명","scnr_nm",null,"VARCHAR2(80)",null,null,"시나리오명",{"$nulls":4},"시나리오명","scnr_nm","VARCHAR2(80)",null,"VARCHAR2(80)",{"$nulls":12},"scnr_nm ","VARCHAR2(80) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsanlsprcsinfo.","scnr_nm"," IS ","'시나리오명'",";",null,null,null,""]
[null,null,"분석유닉스시각","anls_unix_tm",null,"NUMBER(10)",null,null,"분석유닉스시각","선택된 분석일의 유닉스타임 (00시 00분 00초)\n - 검색편의용, 요청 시 API에서 입력하겠습니다",null,null,null,"분석유닉스시각","anls_unix_tm","NUMBER(10)",null,"NUMBER(10)",{"$nulls":12},"anls_unix_tm ","NUMBER(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsanlsprcsinfo.","anls_unix_tm"," IS ","'분석유닉스시각'",";",null,null,null,""]
[null,null,"분석_년","anls_yy",null,"CHAR(4)",null,null,"분석_년 (yyyy)","선택된 년도 (백단에서 자동 계산) ",null,null,null,"분석_년","anls_yy","NUMBER(4)",null,"NUMBER(4)",{"$nulls":12},"anls_yy ","NUMBER(4) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsanlsprcsinfo.","anls_yy"," IS ","'분석_년 (yyyy)'",";",null,null,null,""]
[null,null,"분석_월","anls_mm",null,"NUMBER(2)",null,null,"분석_월 (MM)","선택된 월 (백단에서 자동 계산)",null,null,null,"분석_월","anls_mm","NUMBER(2)",null,"NUMBER(2)",{"$nulls":12},"anls_mm ","NUMBER(2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsanlsprcsinfo.","anls_mm"," IS ","'분석_월 (MM)'",";",null,null,null,""]
[null,null,"분석_일","anls_day",null,"NUMBER(2)",null,null,"분석_일 (dd)","선택된 일 (백단에서 자동 계산)",null,null,null,"분석_일","anls_day","NUMBER(2)",null,"NUMBER(2)",{"$nulls":12},"anls_day ","NUMBER(2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsanlsprcsinfo.","anls_day"," IS ","'분석_일 (dd)'",";",null,null,null,""]
[null,null,"분석요일구분코드","anls_dotw_se_cd",null,"CHAR(2)",null,null,"분석요일구분코드 (025)","선택된 요일 (화면에서 요일 선택)\n1:일요일, 6:금요일,7:토요일,8:월요일~목요일",null,null,null,"분석요일구분코드","anls_dotw_se_cd","VARCHAR(2)",null,"VARCHAR(2)",{"$nulls":12},"anls_dotw_se_cd ","VARCHAR(2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsanlsprcsinfo.","anls_dotw_se_cd"," IS ","'분석요일구분코드 (025)'",";",null,null,null,""]
[null,null,"공간구분코드","spae_se_cd",null,"CHAR(2)",null,null,"공간구분코드 (601)","공간분석단위 (1:교차로, 2:도로,5:행정구역(네트워크))",null,null,null,"공간구분코드","spae_se_cd","VARCHAR(2)",null,"VARCHAR(2)",{"$nulls":12},"spae_se_cd ","VARCHAR(2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsanlsprcsinfo.","spae_se_cd"," IS ","'공간구분코드 (601)'",";",null,null,null,""]
[null,null,"공간구분ID","spae_se_id",null,"VARCHAR2(20)",null,null,"공간구분ID","교차로ID(리스트), 행정구ID, 도로명",null,null,null,"공간구분ID","spae_se_id","VARCHAR2(20)",null,"VARCHAR2(20)",{"$nulls":12},"spae_se_id ","VARCHAR2(20) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsanlsprcsinfo.","spae_se_id"," IS ","'공간구분ID'",";",null,null,null,""]
[null,null,"시간계획분석여부","hr_plan_anls_yn",null,"CHAR(1)",null,null,"시간계획분석여부 (019)","time_plan (N:미분석/Y:분석)\n인천시에서는 자동으로 분석 대상으로 선정됨\n향후를 위해 컬럼 뚫어놓음",null,null,null,"시간계획분석여부","hr_plan_anls_yn","VARCHAR2(1)",null,"VARCHAR2(1)",{"$nulls":12},"hr_plan_anls_yn ","VARCHAR2(1) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsanlsprcsinfo.","hr_plan_anls_yn"," IS ","'시간계획분석여부 (019)'",";",null,null,null,""]
[null,null,"현시분석여부","phas_anls_yn",null,"CHAR(1)",null,null,"현시분석여부 (019)","현시 (N:미분석/Y:분석)\n인천시에서는 자동으로 분석 대상으로 선정됨\n향후를 위해 컬럼 뚫어놓음",null,null,null,"현시분석여부","phas_anls_yn","VARCHAR2(1)",null,"VARCHAR2(1)",{"$nulls":12},"phas_anls_yn ","VARCHAR2(1) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsanlsprcsinfo.","phas_anls_yn"," IS ","'현시분석여부 (019)'",";",null,null,null,""]
[null,null,"옵셋분석여부","ofst_anls_yn",null,"CHAR(1)",null,null,"옵셋분석여부 (019)","옵셋 (N:미분석/Y:분석)\n인천시에서는 자동으로 분석 대상으로 선정됨\n향후를 위해 컬럼 뚫어놓음",null,null,null,"옵셋분석여부","ofst_anls_yn","VARCHAR2(1)",null,"VARCHAR2(1)",{"$nulls":12},"ofst_anls_yn ","VARCHAR2(1) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsanlsprcsinfo.","ofst_anls_yn"," IS ","'옵셋분석여부 (019)'",";",null,null,null,""]
[null,null,"분석진행상태코드","anls_prgrs_stts_cd",null,"CHAR(2)",null,null,"분석진행상태코드 (903, 904)",{"$nulls":4},"분석진행상태코드","anls_prgrs_stts_cd","VARCHAR2(2)",null,"VARCHAR2(2)",{"$nulls":12},"anls_prgrs_stts_cd ","VARCHAR2(2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsanlsprcsinfo.","anls_prgrs_stts_cd"," IS ","'분석진행상태코드 (903, 904)'",";",null,null,null,""]
[null,null,"취소처리여부","rtncl_yn",null,"CHAR(1)",null,null,"취소처리여부 (026)",{"$nulls":4},"취소처리여부","rtncl_yn","VARCHAR2(1)",null,"VARCHAR2(1)",{"$nulls":12},"rtncl_yn ","VARCHAR2(1) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlsprcsinfo.","rtncl_yn"," IS ","'취소처리여부 (026)'",";",null,null,null,""]
[null,null,"요청유닉스시각","dmnd_unix_tm",null,"NUMBER(10)",null,null,"분석요청유닉스시각","API 가 INSERT",null,null,null,"요청유닉스시각","dmnd_unix_tm","NUMBER(10)",null,"NUMBER(10)",{"$nulls":12},"dmnd_unix_tm ","NUMBER(10) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlsprcsinfo.","dmnd_unix_tm"," IS ","'분석요청유닉스시각'",";",null,null,null,""]
[null,null,"취소유닉스시각","rtncl_unix_tm",null,"NUMBER(10)",null,null,"취소요청유닉스시각","API 가 UPDATE",null,null,null,"취소유닉스시각","rtncl_unix_tm","NUMBER(10)",null,"NUMBER(10)",{"$nulls":12},"rtncl_unix_tm ","NUMBER(10) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlsprcsinfo.","rtncl_unix_tm"," IS ","'취소요청유닉스시각'",";",null,null,null,""]
[null,null,"완료유닉스시각","cmptn_unix_tm",null,"NUMBER(10)",null,null,"완료유닉스시각","오효섭차장 UPDATE",null,null,null,"완료유닉스시각","cmptn_unix_tm","NUMBER(10)",null,"NUMBER(10)",{"$nulls":12},"cmptn_unix_tm ","NUMBER(10) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlsprcsinfo.","cmptn_unix_tm"," IS ","'완료유닉스시각'",";",null,null,null,""]
[null,null,"PID","pid",null,"VARCHAR2(50)",null,null,"분석프로세스ID","미들웨어 체크 -> API UPDATE",null,null,null,"분석프로세스ID","pid","VARCHAR2(50)",null,"VARCHAR2(50)",{"$nulls":12},"pid ","VARCHAR2(50) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlsprcsinfo.","pid"," IS ","'분석프로세스ID'",";",null,null,null,""]
[null,null,"분석반복회차","rcrn_cnt",null,"NUMBER(10)",null,null,"분석반복회차","API 가 INSERT",null,null,null,"분석반복회차","rcrn_cnt","NUMBER(10)",null,"NUMBER(10)",{"$nulls":12},"rcrn_cnt ","NUMBER(10) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlsprcsinfo.","rcrn_cnt"," IS ","'분석반복회차'",";"]
[null,null,"에러코드","err_cd",null,"CHAR(3)",null,null,"에러코드","200 : 정상, 여타 에러코드는 메모 참조 >>",null,null,null,"에러코드","err_cd","VARCHAR2(3)",null,"VARCHAR2(3)",{"$nulls":12},"err_cd ","VARCHAR2(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlsprcsinfo.","err_cd"," IS ","'에러코드'",";",null,null,null,{"$f":"IF(LEFT(AE27, 13) = \"CONSTRAINT PK\", AE27, \"\")","v":""}]
[{"$nulls":30},{"$f":"CONCATENATE(AI5:AL27)","v":{"$error":"#VALUE!"}},{"$nulls":16},{"$error":"#VALUE!"}]
[{"$nulls":34},"SOIT_D08_A001","SOIT_I08_A001"]
[null,"시간계획분석구성 테이블",{"$nulls":11},"soitsanlshrplancnfg",{"$nulls":33},{"$f":"IF(LEFT(AE30, 13) = \"CONSTRAINT PK\", AE30, \"\")","v":""}]
[32,"Table Name","Attribute Name","Column Name","#","Data type",null,"Column Null Option","Comment",{"$nulls":4},"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N30&\" \"","v":"soitsanlshrplancnfg "},null," IS ",{"$f":"\"'\"&B30&\"'\"","v":"'시간계획분석구성 테이블'"},";",null,null,null,""]
["TIBERO","soitsanlshrplancnfg","시간계획ID","hr_plan_id",null,"VARCHAR2(10)","PK/FK",null,"시간계획ID",{"$nulls":4},"시간계획ID","hr_plan_id","VARCHAR2(20)",null,"VARCHAR2(20)",{"$nulls":10},"CREATE TABLE ",{"$f":"N30&\" (\"","v":"soitsanlshrplancnfg ("},{"$f":"O32&\" \"","v":"hr_plan_id "},{"$f":"R32&\" \"","v":"VARCHAR2(20) "},{"$f":"IF(H32=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",","CONSTRAINT ",{"$f":"\"PK_\"&N30&\" PRIMARY KEY (\"","v":"PK_soitsanlshrplancnfg PRIMARY KEY ("},{"$f":"IF(OR(G32=\"PK\", G32=\"PK/FK\"), O32, \"\")","v":"hr_plan_id"},",","COMMENT ON COLUMN ",{"$f":"N$30&\". \"","v":"soitsanlshrplancnfg. "},{"$f":"O32","v":"hr_plan_id"}," IS ",{"$f":"\"'\"&I32&\"'\"","v":"'시간계획ID'"},";",null,null,null,""]
[null,null,"연동그룹ID","lnkg_grup_id",null,"VARCHAR2(20)","PK/FK",null,"연동그룹ID",{"$nulls":4},"연동그룹ID","lnkg_grup_id","VARCHAR2(20)",null,"VARCHAR2(20)",{"$nulls":12},"lnkg_grup_id ","VARCHAR2(20) ","",",",null,null,"lnkg_grup_id",",","COMMENT ON COLUMN ","soitsanlshrplancnfg. ","lnkg_grup_id"," IS ","'연동그룹ID'",";",null,null,null,""]
[null,null,"시나리오ID","scnr_id",null,"VARCHAR2(40)","PK/FK",null,"시나리오ID",{"$nulls":4},"시나리오ID","scnr_id","VARCHAR2(40)",null,"VARCHAR2(40)",{"$nulls":12},"scnr_id ","VARCHAR2(40) ","",",",null,null,"scnr_id",{"$f":"\") using index tablespace \" &AJ38& \") TABLESPACE \" &AI38&\";\"","v":") using index tablespace SOIT_I08_A001) TABLESPACE SOIT_D08_A001;"},"COMMENT ON COLUMN ","soitsanlshrplancnfg. ","scnr_id"," IS ","'시나리오ID'",";",null,null,null,""]
[null,null,"시작유닉스시각","bgng_unix_tm",null,"NUMBER(10)",null,null,"계획시작유닉스시각","초, sec",null,null,null,"시작유닉스시각","bgng_unix_tm","NUMBER(10)",null,"NUMBER(10)",{"$nulls":12},"bgng_unix_tm ","NUMBER(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsanlshrplancnfg. ","bgng_unix_tm"," IS ","'계획시작유닉스시각'",";",null,null,null,""]
[null,null,"종료유닉스시각","end_unix_tm",null,"NUMBER(10)",null,null,"계획종료유닉스시각","초, sec",null,null,null,"종료유닉스시각","end_unix_tm","NUMBER(10)",null,"NUMBER(10)",{"$nulls":12},"end_unix_tm ","NUMBER(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsanlshrplancnfg. ","end_unix_tm"," IS ","'계획종료유닉스시각'",";",null,null,null,""]
[{"$nulls":30},{"$f":"CONCATENATE(AI32:AL36)","v":{"$error":"#VALUE!"}},{"$nulls":16},{"$error":"#VALUE!"}]
[{"$nulls":34},"SOIT_D08_A001","SOIT_I08_A001"]
[null,"최적시간계획결과 테이블",{"$nulls":11},"soitsanlshrplanrslt",{"$nulls":33},{"$f":"IF(LEFT(AE39, 13) = \"CONSTRAINT PK\", AE39, \"\")","v":""}]
[33,"Table Name","Attribute Name","Column Name","#","Data type",null,"Column Null Option","Comment",{"$nulls":4},"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N$39&\" \"","v":"soitsanlshrplanrslt "},null," IS ",{"$f":"\"'\"&B39&\"'\"","v":"'최적시간계획결과 테이블'"},";",null,null,null,""]
["TIBERO","soitsanlshrplanrslt","노드ID","node_id",null,"VARCHAR2(300)","PK",null,"교차로 노드ID",{"$nulls":4},"노드ID","node_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":10},"CREATE TABLE ",{"$f":"N39&\" (\"","v":"soitsanlshrplanrslt ("},{"$f":"O41&\" \"","v":"node_id "},{"$f":"R41&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(H41=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",","CONSTRAINT ",{"$f":"\"PK_\"&N39&\" PRIMARY KEY (\"","v":"PK_soitsanlshrplanrslt PRIMARY KEY ("},{"$f":"IF(OR(G41=\"PK\", G41=\"PK/FK\"), O41, \"\")","v":"node_id"},",","COMMENT ON COLUMN ",{"$f":"N$39&\". \"","v":"soitsanlshrplanrslt. "},{"$f":"O41","v":"node_id"}," IS ",{"$f":"\"'\"&I41&\"'\"","v":"'교차로 노드ID'"},";",null,null,null,""]
[null,null,"시간계획ID","hr_plan_id",null,"VARCHAR2(10)","PK/FK",null,"시간계획ID",{"$nulls":4},"시간계획ID","hr_plan_id","VARCHAR2(10)",null,"VARCHAR2(10)",{"$nulls":12},"hr_plan_id ","VARCHAR2(10) ","",",",null,null,"hr_plan_id",",","COMMENT ON COLUMN ","soitsanlshrplanrslt. ","hr_plan_id"," IS ","'시간계획ID'",";",null,null,null,""]
[null,null,"연동그룹ID","lnkg_grup_id",null,"VARCHAR2(20)","PK/FK",null,"연동그룹ID",{"$nulls":4},"연동그룹ID","lnkg_grup_id","VARCHAR2(20)",null,"VARCHAR2(20)",{"$nulls":12},"lnkg_grup_id ","VARCHAR2(20) ","",",",null,null,"lnkg_grup_id",",","COMMENT ON COLUMN ","soitsanlshrplanrslt. ","lnkg_grup_id"," IS ","'연동그룹ID'",";",null,null,null,""]
[null,null,"시나리오ID","scnr_id",null,"VARCHAR2(40)","PK/FK",null,"시나리오ID",{"$nulls":4},"시나리오ID","scnr_id","VARCHAR2(40)",null,"VARCHAR2(40)",{"$nulls":12},"scnr_id ","VARCHAR2(40) ","",",",null,null,"scnr_id",{"$f":"\") using index tablespace \" &AJ64& \") TABLESPACE \" &AI64&\";\"","v":") using index tablespace SOIT_I08_A001) TABLESPACE SOIT_D08_A001;"},"COMMENT ON COLUMN ","soitsanlshrplanrslt. ","scnr_id"," IS ","'시나리오ID'",";",null,null,null,""]
[null,null,"옵셋시간","ofst_hr",null,"NUMBER(3)",null,null,"옵셋시간",{"$nulls":4},"옵셋시간","ofst_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"ofst_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlshrplanrslt. ","ofst_hr"," IS ","'옵셋시간'",";",null,null,null,""]
[null,null,"주기시간","cycl_hr",null,"NUMBER(3)",null,null,"주기시간",{"$nulls":4},"주기시간","cycl_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"cycl_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlshrplanrslt. ","cycl_hr"," IS ","'주기시간'",";",null,null,null,""]
[null,null,"A링1현시녹색시간","A_ring_1_phas_gren_hr",null,"NUMBER(3)",null,null,"A링1현시녹색시간","중요!!!\n\n실제 디비에 들어오는 정보는 순수녹색시간+황색시간+전적색시간\n\n-> 현시시간이 들어온다!",null,null,null,"A링1현시녹색시간","A_ring_1_phas_gren_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"A_ring_1_phas_gren_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlshrplanrslt. ","A_ring_1_phas_gren_hr"," IS ","'A링1현시녹색시간'",";",null,null,null,""]
[null,null,"A링2현시녹색시간","A_ring_2_phas_gren_hr",null,"NUMBER(3)",null,null,"A링2현시녹색시간",{"$nulls":4},"A링2현시녹색시간","A_ring_2_phas_gren_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"A_ring_2_phas_gren_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlshrplanrslt. ","A_ring_2_phas_gren_hr"," IS ","'A링2현시녹색시간'",";",null,null,null,""]
[null,null,"A링3현시녹색시간","A_ring_3_phas_gren_hr",null,"NUMBER(3)",null,null,"A링3현시녹색시간",{"$nulls":4},"A링3현시녹색시간","A_ring_3_phas_gren_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"A_ring_3_phas_gren_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlshrplanrslt. ","A_ring_3_phas_gren_hr"," IS ","'A링3현시녹색시간'",";",null,null,null,""]
[null,null,"A링4현시녹색시간","A_ring_4_phas_gren_hr",null,"NUMBER(3)",null,null,"A링4현시녹색시간",{"$nulls":4},"A링4현시녹색시간","A_ring_4_phas_gren_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"A_ring_4_phas_gren_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlshrplanrslt. ","A_ring_4_phas_gren_hr"," IS ","'A링4현시녹색시간'",";",null,null,null,""]
[null,null,"A링5현시녹색시간","A_ring_5_phas_gren_hr",null,"NUMBER(3)",null,null,"A링5현시녹색시간",{"$nulls":4},"A링5현시녹색시간","A_ring_5_phas_gren_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"A_ring_5_phas_gren_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlshrplanrslt. ","A_ring_5_phas_gren_hr"," IS ","'A링5현시녹색시간'",";",null,null,null,""]
[null,null,"A링6현시녹색시간","A_ring_6_phas_gren_hr",null,"NUMBER(3)",null,null,"A링6현시녹색시간",{"$nulls":4},"A링6현시녹색시간","A_ring_6_phas_gren_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"A_ring_6_phas_gren_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlshrplanrslt. ","A_ring_6_phas_gren_hr"," IS ","'A링6현시녹색시간'",";",null,null,null,""]
[null,null,"A링7현시녹색시간","A_ring_7_phas_gren_hr",null,"NUMBER(3)",null,null,"A링7현시녹색시간",{"$nulls":4},"A링7현시녹색시간","A_ring_7_phas_gren_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"A_ring_7_phas_gren_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlshrplanrslt. ","A_ring_7_phas_gren_hr"," IS ","'A링7현시녹색시간'",";",null,null,null,""]
[null,null,"A링8현시녹색시간","A_ring_8_phas_gren_hr",null,"NUMBER(3)",null,null,"A링8현시녹색시간",{"$nulls":4},"A링8현시녹색시간","A_ring_8_phas_gren_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"A_ring_8_phas_gren_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlshrplanrslt. ","A_ring_8_phas_gren_hr"," IS ","'A링8현시녹색시간'",";",null,null,null,""]
[null,null,"B링1현시녹색시간","B_ring_1_phas_gren_hr",null,"NUMBER(3)",null,null,"B링1현시녹색시간",{"$nulls":4},"B링1현시녹색시간","B_ring_1_phas_gren_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"B_ring_1_phas_gren_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlshrplanrslt. ","B_ring_1_phas_gren_hr"," IS ","'B링1현시녹색시간'",";",null,null,null,""]
[null,null,"B링2현시녹색시간","B_ring_2_phas_gren_hr",null,"NUMBER(3)",null,null,"B링2현시녹색시간",{"$nulls":4},"B링2현시녹색시간","B_ring_2_phas_gren_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"B_ring_2_phas_gren_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlshrplanrslt. ","B_ring_2_phas_gren_hr"," IS ","'B링2현시녹색시간'",";",null,null,null,""]
[null,null,"B링3현시녹색시간","B_ring_3_phas_gren_hr",null,"NUMBER(3)",null,null,"B링3현시녹색시간",{"$nulls":4},"B링3현시녹색시간","B_ring_3_phas_gren_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"B_ring_3_phas_gren_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlshrplanrslt. ","B_ring_3_phas_gren_hr"," IS ","'B링3현시녹색시간'",";",null,null,null,""]
[null,null,"B링4현시녹색시간","B_ring_4_phas_gren_hr",null,"NUMBER(3)",null,null,"B링4현시녹색시간",{"$nulls":4},"B링4현시녹색시간","B_ring_4_phas_gren_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"B_ring_4_phas_gren_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlshrplanrslt. ","B_ring_4_phas_gren_hr"," IS ","'B링4현시녹색시간'",";",null,null,null,""]
[null,null,"B링5현시녹색시간","B_ring_5_phas_gren_hr",null,"NUMBER(3)",null,null,"B링5현시녹색시간",{"$nulls":4},"B링5현시녹색시간","B_ring_5_phas_gren_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"B_ring_5_phas_gren_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlshrplanrslt. ","B_ring_5_phas_gren_hr"," IS ","'B링5현시녹색시간'",";",null,null,null,""]
[null,null,"B링6현시녹색시간","B_ring_6_phas_gren_hr",null,"NUMBER(3)",null,null,"B링6현시녹색시간",{"$nulls":4},"B링6현시녹색시간","B_ring_6_phas_gren_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"B_ring_6_phas_gren_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlshrplanrslt. ","B_ring_6_phas_gren_hr"," IS ","'B링6현시녹색시간'",";",null,null,null,""]
[null,null,"B링7현시녹색시간","B_ring_7_phas_gren_hr",null,"NUMBER(3)",null,null,"B링7현시녹색시간",{"$nulls":4},"B링7현시녹색시간","B_ring_7_phas_gren_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"B_ring_7_phas_gren_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlshrplanrslt. ","B_ring_7_phas_gren_hr"," IS ","'B링7현시녹색시간'",";",null,null,null,""]
[null,null,"B링8현시녹색시간","B_ring_8_phas_gren_hr",null,"NUMBER(3)",null,null,"B링8현시녹색시간",{"$nulls":4},"B링8현시녹색시간","B_ring_8_phas_gren_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"B_ring_8_phas_gren_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlshrplanrslt. ","B_ring_8_phas_gren_hr"," IS ","'B링8현시녹색시간'",";",null,null,null,""]
[{"$nulls":30},{"$f":"CONCATENATE(AI41:AL62)","v":{"$error":"#VALUE!"}}]
[{"$nulls":34},"SOIT_D08_A001","SOIT_I08_A001"]
[null,"최적현시결과 테이블",{"$nulls":11},"soitsanlsphasrslt",{"$nulls":33},{"$f":"IF(LEFT(AE65, 13) = \"CONSTRAINT PK\", AE65, \"\")","v":""}]
[34,"Table Name","Attribute Name","Column Name","#","Data type",null,"Column Null Option","Comment",{"$nulls":4},"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":18},{"$f":"IF(OR(G66=\"PK\", G66=\"PK/FK\"), O66, \"\")","v":""},{"$nulls":10},""]
["TIBERO","soitsanlsphasrslt","노드ID","node_id",null,"VARCHAR2(300)","PK",null,"교차로 노드ID",{"$nulls":4},"노드ID","node_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":10},"CREATE TABLE ",{"$f":"N65&\" (\"","v":"soitsanlsphasrslt ("},{"$f":"O67&\" \"","v":"node_id "},{"$f":"R67&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(H67=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",","CONSTRAINT ",{"$f":"\"PK_\"&N65&\" PRIMARY KEY (\"","v":"PK_soitsanlsphasrslt PRIMARY KEY ("},"node_id",",","COMMENT ON TABLE",{"$f":"N$65&\" \"","v":"soitsanlsphasrslt "},null," IS ",{"$f":"\"'\"&B65&\"'\"","v":"'최적현시결과 테이블'"},";"]
[null,null,"시나리오ID","scnr_id",null,"VARCHAR2(40)","PK/FK",null,"시나리오ID",{"$nulls":4},"시나리오ID","scnr_id","VARCHAR2(40)",null,"VARCHAR2(40)",{"$nulls":12},"scnr_id ","VARCHAR2(40) ","",",",null,null,"scnr_id",{"$f":"\") using index tablespace \" &AJ103& \") TABLESPACE \" &AI103&\";\"","v":") using index tablespace SOIT_I08_A001) TABLESPACE SOIT_D08_A001;"},"COMMENT ON COLUMN ",{"$f":"N$65&\". \"","v":"soitsanlsphasrslt. "},{"$f":"O68","v":"scnr_id"}," IS ",{"$f":"\"'\"&I68&\"'\"","v":"'시나리오ID'"},";"]
[null,null,"주현시번호","majr_phas_no",null,"NUMBER(1)",null,null,"주 현시번호(OPTION 20)",{"$nulls":4},"주현시번호","majr_phas_no","NUMBER(1)",null,"NUMBER(1)",{"$nulls":12},"majr_phas_no ","NUMBER(1) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsanlsphasrslt. ","majr_phas_no"," IS ","'주 현시번호(OPTION 20)'",";"]
[null,null,"A링1현시황색시간","A_ring_1_phas_yelw_hr",null,"NUMBER(3)",null,null,"A링1현시황색시간","default : 4sec",null,null,null,"A링1현시황색시간","A_ring_1_phas_yelw_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"A_ring_1_phas_yelw_hr ","NUMBER(3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsanlsphasrslt. ","A_ring_1_phas_yelw_hr"," IS ","'A링1현시황색시간'",";",null,null,null,{"$f":"IF(LEFT(AE70, 13) = \"CONSTRAINT PK\", AE70, \"\")","v":""}]
[null,null,"A링2현시황색시간","A_ring_2_phas_yelw_hr",null,"NUMBER(3)",null,null,"A링2현시황색시간","default : 4sec",null,null,null,"A링2현시황색시간","A_ring_2_phas_yelw_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"A_ring_2_phas_yelw_hr ","NUMBER(3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsanlsphasrslt. ","A_ring_2_phas_yelw_hr"," IS ","'A링2현시황색시간'",";",null,null,null,""]
[null,null,"A링3현시황색시간","A_ring_3_phas_yelw_hr",null,"NUMBER(3)",null,null,"A링3현시황색시간","default : 4sec",null,null,null,"A링3현시황색시간","A_ring_3_phas_yelw_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"A_ring_3_phas_yelw_hr ","NUMBER(3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsanlsphasrslt. ","A_ring_3_phas_yelw_hr"," IS ","'A링3현시황색시간'",";",null,null,null,""]
[null,null,"A링4현시황색시간","A_ring_4_phas_yelw_hr",null,"NUMBER(3)",null,null,"A링4현시황색시간","default : 4sec",null,null,null,"A링4현시황색시간","A_ring_4_phas_yelw_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"A_ring_4_phas_yelw_hr ","NUMBER(3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsanlsphasrslt. ","A_ring_4_phas_yelw_hr"," IS ","'A링4현시황색시간'",";",null,null,null,""]
[null,null,"A링5현시황색시간","A_ring_5_phas_yelw_hr",null,"NUMBER(3)",null,null,"A링5현시황색시간","default : 4sec",null,null,null,"A링5현시황색시간","A_ring_5_phas_yelw_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"A_ring_5_phas_yelw_hr ","NUMBER(3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsanlsphasrslt. ","A_ring_5_phas_yelw_hr"," IS ","'A링5현시황색시간'",";",null,null,null,""]
[null,null,"A링6현시황색시간","A_ring_6_phas_yelw_hr",null,"NUMBER(3)",null,null,"A링6현시황색시간","default : 4sec",null,null,null,"A링6현시황색시간","A_ring_6_phas_yelw_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"A_ring_6_phas_yelw_hr ","NUMBER(3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsanlsphasrslt. ","A_ring_6_phas_yelw_hr"," IS ","'A링6현시황색시간'",";",null,null,null,""]
[null,null,"A링7현시황색시간","A_ring_7_phas_yelw_hr",null,"NUMBER(3)",null,null,"A링7현시황색시간","default : 4sec",null,null,null,"A링7현시황색시간","A_ring_7_phas_yelw_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"A_ring_7_phas_yelw_hr ","NUMBER(3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsanlsphasrslt. ","A_ring_7_phas_yelw_hr"," IS ","'A링7현시황색시간'",";",null,null,null,""]
[null,null,"A링8현시황색시간","A_ring_8_phas_yelw_hr",null,"NUMBER(3)",null,null,"A링8현시황색시간","default : 4sec",null,null,null,"A링8현시황색시간","A_ring_8_phas_yelw_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"A_ring_8_phas_yelw_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlsphasrslt. ","A_ring_8_phas_yelw_hr"," IS ","'A링8현시황색시간'",";",null,null,null,""]
[null,null,"B링1현시황색시간","B_ring_1_phas_yelw_hr",null,"NUMBER(3)",null,null,"B링1현시황색시간","default : 4sec",null,null,null,"B링1현시황색시간","B_ring_1_phas_yelw_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"B_ring_1_phas_yelw_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlsphasrslt. ","B_ring_1_phas_yelw_hr"," IS ","'B링1현시황색시간'",";",null,null,null,""]
[null,null,"B링2현시황색시간","B_ring_2_phas_yelw_hr",null,"NUMBER(3)",null,null,"B링2현시황색시간","default : 4sec",null,null,null,"B링2현시황색시간","B_ring_2_phas_yelw_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"B_ring_2_phas_yelw_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlsphasrslt. ","B_ring_2_phas_yelw_hr"," IS ","'B링2현시황색시간'",";",null,null,null,""]
[null,null,"B링3현시황색시간","B_ring_3_phas_yelw_hr",null,"NUMBER(3)",null,null,"B링3현시황색시간","default : 4sec",null,null,null,"B링3현시황색시간","B_ring_3_phas_yelw_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"B_ring_3_phas_yelw_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlsphasrslt. ","B_ring_3_phas_yelw_hr"," IS ","'B링3현시황색시간'",";",null,null,null,""]
[null,null,"B링4현시황색시간","B_ring_4_phas_yelw_hr",null,"NUMBER(3)",null,null,"B링4현시황색시간","default : 4sec",null,null,null,"B링4현시황색시간","B_ring_4_phas_yelw_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"B_ring_4_phas_yelw_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlsphasrslt. ","B_ring_4_phas_yelw_hr"," IS ","'B링4현시황색시간'",";",null,null,null,""]
[null,null,"B링5현시황색시간","B_ring_5_phas_yelw_hr",null,"NUMBER(3)",null,null,"B링5현시황색시간","default : 4sec",null,null,null,"B링5현시황색시간","B_ring_5_phas_yelw_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"B_ring_5_phas_yelw_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlsphasrslt. ","B_ring_5_phas_yelw_hr"," IS ","'B링5현시황색시간'",";",null,null,null,""]
[null,null,"B링6현시황색시간","B_ring_6_phas_yelw_hr",null,"NUMBER(3)",null,null,"B링6현시황색시간","default : 4sec",null,null,null,"B링6현시황색시간","B_ring_6_phas_yelw_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"B_ring_6_phas_yelw_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlsphasrslt. ","B_ring_6_phas_yelw_hr"," IS ","'B링6현시황색시간'",";",null,null,null,""]
[null,null,"B링7현시황색시간","B_ring_7_phas_yelw_hr",null,"NUMBER(3)",null,null,"B링7현시황색시간","default : 4sec",null,null,null,"B링7현시황색시간","B_ring_7_phas_yelw_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"B_ring_7_phas_yelw_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlsphasrslt. ","B_ring_7_phas_yelw_hr"," IS ","'B링7현시황색시간'",";",null,null,null,""]
[null,null,"B링8현시황색시간","B_ring_8_phas_yelw_hr",null,"NUMBER(3)",null,null,"B링8현시황색시간","default : 4sec",null,null,null,"B링8현시황색시간","B_ring_8_phas_yelw_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"B_ring_8_phas_yelw_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlsphasrslt. ","B_ring_8_phas_yelw_hr"," IS ","'B링8현시황색시간'",";",null,null,null,""]
[null,null,"A링1현시전적색시간","A_ring_1_phas_all_red_hr",null,"NUMBER(3)",null,null,"A링1현시전적색시간",{"$nulls":4},"A링1현시전적색시간","A_ring_1_phas_all_red_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"A_ring_1_phas_all_red_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlsphasrslt. ","A_ring_1_phas_all_red_hr"," IS ","'A링1현시전적색시간'",";"]
[null,null,"A링2현시전적색시간","A_ring_2_phas_all_red_hr",null,"NUMBER(3)",null,null,"A링2현시전적색시간",{"$nulls":4},"A링2현시전적색시간","A_ring_2_phas_all_red_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"A_ring_2_phas_all_red_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlsphasrslt. ","A_ring_2_phas_all_red_hr"," IS ","'A링2현시전적색시간'",";"]
[null,null,"A링3현시전적색시간","A_ring_3_phas_all_red_hr",null,"NUMBER(3)",null,null,"A링3현시전적색시간",{"$nulls":4},"A링3현시전적색시간","A_ring_3_phas_all_red_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"A_ring_3_phas_all_red_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlsphasrslt. ","A_ring_3_phas_all_red_hr"," IS ","'A링3현시전적색시간'",";"]
[null,null,"A링4현시전적색시간","A_ring_4_phas_all_red_hr",null,"NUMBER(3)",null,null,"A링4현시전적색시간",{"$nulls":4},"A링4현시전적색시간","A_ring_4_phas_all_red_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"A_ring_4_phas_all_red_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlsphasrslt. ","A_ring_4_phas_all_red_hr"," IS ","'A링4현시전적색시간'",";"]
[null,null,"A링5현시전적색시간","A_ring_5_phas_all_red_hr",null,"NUMBER(3)",null,null,"A링5현시전적색시간",{"$nulls":4},"A링5현시전적색시간","A_ring_5_phas_all_red_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"A_ring_5_phas_all_red_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlsphasrslt. ","A_ring_5_phas_all_red_hr"," IS ","'A링5현시전적색시간'",";"]
[null,null,"A링6현시전적색시간","A_ring_6_phas_all_red_hr",null,"NUMBER(3)",null,null,"A링6현시전적색시간",{"$nulls":4},"A링6현시전적색시간","A_ring_6_phas_all_red_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"A_ring_6_phas_all_red_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlsphasrslt. ","A_ring_6_phas_all_red_hr"," IS ","'A링6현시전적색시간'",";"]
[null,null,"A링7현시전적색시간","A_ring_7_phas_all_red_hr",null,"NUMBER(3)",null,null,"A링7현시전적색시간",{"$nulls":4},"A링7현시전적색시간","A_ring_7_phas_all_red_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"A_ring_7_phas_all_red_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlsphasrslt. ","A_ring_7_phas_all_red_hr"," IS ","'A링7현시전적색시간'",";"]
[null,null,"A링8현시전적색시간","A_ring_8_phas_all_red_hr",null,"NUMBER(3)",null,null,"A링8현시전적색시간",{"$nulls":4},"A링8현시전적색시간","A_ring_8_phas_all_red_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"A_ring_8_phas_all_red_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlsphasrslt. ","A_ring_8_phas_all_red_hr"," IS ","'A링8현시전적색시간'",";"]
[null,null,"B링1현시전적색시간","B_ring_1_phas_all_red_hr",null,"NUMBER(3)",null,null,"B링1현시전적색시간",{"$nulls":4},"B링1현시전적색시간","B_ring_1_phas_all_red_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"B_ring_1_phas_all_red_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlsphasrslt. ","B_ring_1_phas_all_red_hr"," IS ","'B링1현시전적색시간'",";"]
[null,null,"B링2현시전적색시간","B_ring_2_phas_all_red_hr",null,"NUMBER(3)",null,null,"B링2현시전적색시간",{"$nulls":4},"B링2현시전적색시간","B_ring_2_phas_all_red_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"B_ring_2_phas_all_red_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlsphasrslt. ","B_ring_2_phas_all_red_hr"," IS ","'B링2현시전적색시간'",";"]
[null,null,"B링3현시전적색시간","B_ring_3_phas_all_red_hr",null,"NUMBER(3)",null,null,"B링3현시전적색시간",{"$nulls":4},"B링3현시전적색시간","B_ring_3_phas_all_red_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"B_ring_3_phas_all_red_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlsphasrslt. ","B_ring_3_phas_all_red_hr"," IS ","'B링3현시전적색시간'",";"]
[null,null,"B링4현시전적색시간","B_ring_4_phas_all_red_hr",null,"NUMBER(3)",null,null,"B링4현시전적색시간",{"$nulls":4},"B링4현시전적색시간","B_ring_4_phas_all_red_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"B_ring_4_phas_all_red_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlsphasrslt. ","B_ring_4_phas_all_red_hr"," IS ","'B링4현시전적색시간'",";"]
[null,null,"B링5현시전적색시간","B_ring_5_phas_all_red_hr",null,"NUMBER(3)",null,null,"B링5현시전적색시간",{"$nulls":4},"B링5현시전적색시간","B_ring_5_phas_all_red_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"B_ring_5_phas_all_red_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlsphasrslt. ","B_ring_5_phas_all_red_hr"," IS ","'B링5현시전적색시간'",";"]
[null,null,"B링6현시전적색시간","B_ring_6_phas_all_red_hr",null,"NUMBER(3)",null,null,"B링6현시전적색시간",{"$nulls":4},"B링6현시전적색시간","B_ring_6_phas_all_red_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"B_ring_6_phas_all_red_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlsphasrslt. ","B_ring_6_phas_all_red_hr"," IS ","'B링6현시전적색시간'",";"]
[null,null,"B링7현시전적색시간","B_ring_7_phas_all_red_hr",null,"NUMBER(3)",null,null,"B링7현시전적색시간",{"$nulls":4},"B링7현시전적색시간","B_ring_7_phas_all_red_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"B_ring_7_phas_all_red_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlsphasrslt. ","B_ring_7_phas_all_red_hr"," IS ","'B링7현시전적색시간'",";"]
[null,null,"B링8현시전적색시간","B_ring_8_phas_all_red_hr",null,"NUMBER(3)",null,null,"B링8현시전적색시간",{"$nulls":4},"B링8현시전적색시간","B_ring_8_phas_all_red_hr","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"B_ring_8_phas_all_red_hr ","NUMBER(3) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlsphasrslt. ","B_ring_8_phas_all_red_hr"," IS ","'B링8현시전적색시간'",";"]
[{"$nulls":30},{"$f":"CONCATENATE(AI67:AL101)","v":{"$error":"#VALUE!"}}," ",""]
[{"$nulls":34},"SOIT_D08_A001","SOIT_I08_A001"]
[]
[]
[]
[null,"반복분석이력 테이블",{"$nulls":11},"soitsanlsrcrnhstr",{"$nulls":33},{"$f":"IF(LEFT(AE107, 13) = \"CONSTRAINT PK\", AE107, \"\")","v":""}]
[35,"Table Name","Attribute Name","Column Name","#","Data type",null,"Column Null Option","Comment",{"$nulls":4},"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N$107&\" \"","v":"soitsanlsrcrnhstr "},null," IS ",{"$f":"\"'\"&B107&\"'\"","v":"'반복분석이력 테이블'"},";",null,null,null,""]
["TIBERO","soitsanlsrcrnhstr\n(파이썬)","시나리오ID","scnr_id",null,"VARCHAR2(40)","PK",null,"시나리오ID","반복 1회차마다 데이터 쌓임",null,null,null,"시나리오ID","scnr_id","VARCHAR2(40)",null,"VARCHAR2(40)",{"$nulls":10},"CREATE TABLE ",{"$f":"N107&\" (\"","v":"soitsanlsrcrnhstr ("},{"$f":"O109&\" \"","v":"scnr_id "},{"$f":"R109&\" \"","v":"VARCHAR2(40) "},{"$f":"IF(H109=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",","CONSTRAINT ",{"$f":"\"PK_\"&N107&\" PRIMARY KEY (\"","v":"PK_soitsanlsrcrnhstr PRIMARY KEY ("},{"$f":"IF(OR(G109=\"PK\", G109=\"PK/FK\"), O109, \"\")","v":"scnr_id"},",","COMMENT ON COLUMN ",{"$f":"N$107&\". \"","v":"soitsanlsrcrnhstr. "},{"$f":"O109","v":"scnr_id"}," IS ",{"$f":"\"'\"&I109&\"'\"","v":"'시나리오ID'"},";",null,null,null,""]
[null,null,"반복횟수","rcrn_notm",null,"NUMBER(4)","PK",null,"반복횟수",{"$nulls":4},"반복횟수","rcrn_notm","NUMBER(4)",null,"NUMBER(4)",{"$nulls":12},"rcrn_notm ","NUMBER(4) ","",",",null,null,"rcrn_notm",{"$f":"\") using index tablespace \" &AJ113& \") TABLESPACE \" &AI113&\";\"","v":") using index tablespace SOIT_I08_A001) TABLESPACE SOIT_D08_A001;"},"COMMENT ON COLUMN ","soitsanlsrcrnhstr. ","rcrn_notm"," IS ","'반복횟수'",";",null,null,null,""]
[null,null,"최적화값","otmz_valu",null,"NUMBER(19,9)",null,null,"최적화 비교수치","단위가 애매함 (초일지 대기행렬일지)",null,null,null,"최적화값","otmz_valu","NUMBER(19,9)",null,"NUMBER(19,9)",{"$nulls":12},"otmz_valu ","NUMBER(19,9) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsanlsrcrnhstr. ","otmz_valu"," IS ","'최적화 비교수치'",";",null,null,null,""]
[{"$nulls":30},{"$f":"CONCATENATE(AI109:AL111)","v":{"$error":"#VALUE!"}},{"$nulls":16},{"$error":"#VALUE!"}]
[null,null,"before/after",{"$nulls":31},"SOIT_D08_A001","SOIT_I08_A001",{"$nulls":11},""]
[{"$nulls":47},""]
[null,"5분 대상지역 종합지표 테이블",{"$nulls":11},"soitsanls5minvalue",{"$nulls":33},""]
[36,"Table Name","Attribute Name","Column Name","#","Data type",null,"Column Null Option","Comment",{"$nulls":4},"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N115&\" \"","v":"soitsanls5minvalue "},null," IS ",{"$f":"\"'\"&B115&\"'\"","v":"'5분 대상지역 종합지표 테이블'"},";",null,null,null,""]
["TIBERO","soitsanls5minvalue","시나리오ID","scnr_id",null,"VARCHAR2(40)","PK",null,"시나리오ID","시나리오 고유 id (백단에서 seq)",null,null,null,"시나리오ID","scnr_id",null,null,"VARCHAR2(40)",{"$nulls":10},"CREATE TABLE ",{"$f":"N115&\" (\"","v":"soitsanls5minvalue ("},{"$f":"O117&\" \"","v":"scnr_id "},{"$f":"R117&\" \"","v":"VARCHAR2(40) "},{"$f":"IF(H117=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",","CONSTRAINT ",{"$f":"\"PK_\"&N115&\" PRIMARY KEY (\"","v":"PK_soitsanls5minvalue PRIMARY KEY ("},{"$f":"IF(OR(G117=\"PK\", G117=\"PK/FK\"), O117, \"\")","v":"scnr_id"},",","COMMENT ON COLUMN ",{"$f":"N$115&\". \"","v":"soitsanls5minvalue. "},{"$f":"O117","v":"scnr_id"}," IS ",{"$f":"\"'\"&I117&\"'\"","v":"'시나리오ID'"},";",null,null,null,""]
[null,null,"분석구분코드","anls_div_cd",null,"VARCHAR2(1)","PK",null,"분석구분코드(1:현황. 2:최적화)",{"$nulls":4},"분석구분코드","anls_div_cd",null,null,"VARCHAR2(1)",{"$nulls":12},"anls_div_cd ","VARCHAR2(1) ","",",",null,null,"anls_div_cd",",","COMMENT ON COLUMN ","soitsanls5minvalue. ","anls_div_cd"," IS ","'분석구분코드(1:현황. 2:최적화)'",";",null,null,null,""]
[null,null,"시간계획ID","hr_plan_id",null,"VARCHAR2(10)","PK",null,"타임플랜번호","HH24MI_HH24MI",null,null,null,"시간계획ID","hr_plan_id","VARCHAR2(10)",null,"VARCHAR2(10)",{"$nulls":12},"hr_plan_id ","VARCHAR2(10) ","",",",null,null,"hr_plan_id",",","COMMENT ON COLUMN ","soitsanls5minvalue. ","hr_plan_id"," IS ","'타임플랜번호'",";",null,null,null,""]
[null,null,"시간그룹번호","TM_GRUP_NO",null,"NUMBER(10)","PK",null,"시간그룹번호(초단위 시작시간)","5분(300) 단위로 누적값",null,null,null,"시간그룹번호","TM_GRUP_NO",null,null,"NUMBER(10)",{"$nulls":12},"TM_GRUP_NO ","NUMBER(10) ","",",",null,null,"TM_GRUP_NO",{"$f":"\") using index tablespace \" &AJ127& \") TABLESPACE \" &AI127&\";\"","v":") using index tablespace SOIT_I08_A001) TABLESPACE SOIT_D08_A001;"},"COMMENT ON COLUMN ","soitsanls5minvalue. ","TM_GRUP_NO"," IS ","'시간그룹번호(초단위 시작시간)'",";",null,null,null,""]
[null,null,"교통량","trvl",null,"NUMBER(10)",null,null,"총교통량",{"$nulls":4},"교통량","trvl",null,null,"NUMBER(10)",{"$nulls":12},"trvl ","NUMBER(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsanls5minvalue. ","trvl"," IS ","'총교통량'",";",null,null,null,""]
[null,null,"평균속도","avg_sped",null,"NUMBER(5,2)",null,null,"평균속도",{"$nulls":4},"평균속도","avg_sped",null,null,"NUMBER(5,2)",{"$nulls":12},"avg_sped ","NUMBER(5,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsanls5minvalue. ","avg_sped"," IS ","'평균속도'",";",null,null,null,""]
[null,null,"평균지체시간","avg_dely_tm",null,"NUMBER(7,2)",null,null,"평균지체시간",{"$nulls":4},"평균지체시간","avg_dely_tm",null,null,"NUMBER(7,2)",{"$nulls":12},"avg_dely_tm ","NUMBER(7,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsanls5minvalue. ","avg_dely_tm"," IS ","'평균지체시간'",";",null,null,null,""]
[null,null,"평균대기행렬","avg_queu_lngt",null,"NUMBER(19,9)",null,null,"평균대기행렬 길이(m)","초당",null,null,null,"평균대기행렬","avg_queu_lngt",null,null,"NUMBER(19,9)",{"$nulls":12},"avg_queu_lngt ","NUMBER(19,9) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsanls5minvalue. ","avg_queu_lngt"," IS ","'평균대기행렬 길이(m)'",";",null,null,null,""]
[null,null,"차선별평균대기행렬","lane_avg_queu_lngt",null,"NUMBER(19,9)",null,null,"차선별 평균대기행렬 길이(m)","초당",null,null,null,"차선별평균대기행렬","lane_avg_queu_lngt",null,null,"NUMBER(19,9)",{"$nulls":12},"lane_avg_queu_lngt ","NUMBER(19,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanls5minvalue. ","lane_avg_queu_lngt"," IS ","'차선별 평균대기행렬 길이(m)'",";"]
[{"$nulls":30},{"$f":"CONCATENATE(AI117:AL124)","v":{"$error":"#VALUE!"}}," ","",{"$nulls":14},{"$f":"IF(LEFT(AE126, 13) = \"CONSTRAINT PK\", AE126, \"\")","v":{"$error":"#VALUE!"}}]
[{"$nulls":34},"SOIT_D08_A001","SOIT_I08_A001"]
[null,"전체지역 종합지표 테이블",{"$nulls":11},"soitsanlsallvalue",{"$nulls":33},{"$f":"IF(LEFT(AE128, 13) = \"CONSTRAINT PK\", AE128, \"\")","v":""}]
[37,"Table Name","Attribute Name","Column Name","#","Data type",null,"Column Null Option","Comment","시간계획 마스터테이블로 활용",null,null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N128&\" \"","v":"soitsanlsallvalue "},null," IS ",{"$f":"\"'\"&B128&\"'\"","v":"'전체지역 종합지표 테이블'"},";",null,null,null,""]
["TIBERO","soitsanlsallvalue","시나리오ID","scnr_id",null,"VARCHAR2(40)","PK",null,"시나리오ID","시나리오 고유 id (백단에서 seq)",null,null,null,"시나리오ID","scnr_id",null,null,"VARCHAR2(40)",{"$nulls":10},"CREATE TABLE ",{"$f":"N128&\" (\"","v":"soitsanlsallvalue ("},{"$f":"O130&\" \"","v":"scnr_id "},{"$f":"R130&\" \"","v":"VARCHAR2(40) "},{"$f":"IF(H130=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",","CONSTRAINT ",{"$f":"\"PK_\"&N128&\" PRIMARY KEY (\"","v":"PK_soitsanlsallvalue PRIMARY KEY ("},{"$f":"IF(OR(G130=\"PK\", G130=\"PK/FK\"), O130, \"\")","v":"scnr_id"},",","COMMENT ON COLUMN ",{"$f":"N$128&\". \"","v":"soitsanlsallvalue. "},{"$f":"O130","v":"scnr_id"}," IS ",{"$f":"\"'\"&I130&\"'\"","v":"'시나리오ID'"},";",null,null,null,""]
[null,null,"분석구분코드","anls_div_cd",null,"VARCHAR2(1)","PK",null,"분석구분코드(1:현황. 2:최적화)",{"$nulls":4},"분석구분코드","anls_div_cd",null,null,"VARCHAR2(1)",{"$nulls":12},"anls_div_cd ","VARCHAR2(1) ","",",",null,null,"anls_div_cd",",","COMMENT ON COLUMN ","soitsanlsallvalue. ","anls_div_cd"," IS ","'분석구분코드(1:현황. 2:최적화)'",";",null,null,null,""]
[null,null,"시간계획ID","hr_plan_id",null,"VARCHAR2(10)","PK",null,"타임플랜번호","HH24MI_HH24MI","0612_1200",null,null,"시간계획ID","hr_plan_id","VARCHAR2(10)",null,"VARCHAR2(10)",{"$nulls":12},"hr_plan_id ","VARCHAR2(10) ","",",",null,null,"hr_plan_id",{"$f":"\") using index tablespace \" &AJ140& \") TABLESPACE \" &AI140&\";\"","v":") using index tablespace SOIT_I08_A001) TABLESPACE SOIT_D08_A001;"},"COMMENT ON COLUMN ","soitsanlsallvalue. ","hr_plan_id"," IS ","'타임플랜번호'",";",null,null,null,""]
[null,null,"교통량","trvl",null,"NUMBER(10)",null,null,"총교통량",{"$nulls":4},"교통량","trvl",null,null,"NUMBER(10)",{"$nulls":12},"trvl ","NUMBER(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsanlsallvalue. ","trvl"," IS ","'총교통량'",";",null,null,null,""]
[null,null,"평균속도","avg_sped",null,"NUMBER(5,2)",null,null,"평균속도",{"$nulls":4},"평균속도","avg_sped",null,null,"NUMBER(5,2)",{"$nulls":12},"avg_sped ","NUMBER(5,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsanlsallvalue. ","avg_sped"," IS ","'평균속도'",";",null,null,null,""]
[null,null,"평균지체시간","avg_dely_tm",null,"NUMBER(7,2)",null,null,"평균지체시간",{"$nulls":4},"평균지체시간","avg_dely_tm",null,null,"NUMBER(7,2)",{"$nulls":12},"avg_dely_tm ","NUMBER(7,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsanlsallvalue. ","avg_dely_tm"," IS ","'평균지체시간'",";",null,null,null,""]
[null,null,"평균대기행렬","avg_queu_lngt",null,"NUMBER(19,9)",null,null,"평균대기행렬 길이(m)",{"$nulls":4},"평균대기행렬","avg_queu_lngt",null,null,"NUMBER(19,9)",{"$nulls":12},"avg_queu_lngt ","NUMBER(19,9) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsanlsallvalue. ","avg_queu_lngt"," IS ","'평균대기행렬 길이(m)'",";",null,null,null,""]
[null,null,"차선별평균대기행렬","lane_avg_queu_lngt",null,"NUMBER(19,9)",null,null,"차선별 평균대기행렬 길이(m)",{"$nulls":4},"차선별평균대기행렬","lane_avg_queu_lngt","NUMBER(19,9)",null,"NUMBER(19,9)",{"$nulls":12},"lane_avg_queu_lngt ","NUMBER(19,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlsallvalue. ","lane_avg_queu_lngt"," IS ","'차선별 평균대기행렬 길이(m)'",";"]
[null,null,"교차로별평균대기행렬","ints_avg_queu_lngt",null,"NUMBER(19,9)",null,null,"교차로별 평균대기행렬 길이(m)",{"$nulls":4},"교차로별 평균대기행렬","ints_avg_queu_lngt","NUMBER(19,9)",null,"NUMBER(19,9)",{"$nulls":12},"ints_avg_queu_lngt ","NUMBER(19,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlsallvalue. ","ints_avg_queu_lngt"," IS ","'교차로별 평균대기행렬 길이(m)'",";"]
[{"$nulls":30},{"$f":"CONCATENATE(AI130:AL136)","v":{"$error":"#VALUE!"}}," ","",{"$nulls":14},{"$f":"IF(LEFT(AE139, 13) = \"CONSTRAINT PK\", AE139, \"\")","v":{"$error":"#VALUE!"}}]
[{"$nulls":34},"SOIT_D08_A001","SOIT_I08_A001"]
[null,"교차로별 평균지표 테이블",{"$nulls":11},"soitsanlsintsvalue",{"$nulls":33},{"$f":"IF(LEFT(AE141, 13) = \"CONSTRAINT PK\", AE141, \"\")","v":""}]
[38,"Table Name","Attribute Name","Column Name","#","Data type",null,"Column Null Option","Comment",{"$nulls":4},"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N141&\" \"","v":"soitsanlsintsvalue "},null," IS ",{"$f":"\"'\"&B141&\"'\"","v":"'교차로별 평균지표 테이블'"},";",null,null,null,""]
["TIBERO","soitsanlsintsvalue","시나리오ID","scnr_id",null,"VARCHAR2(40)","PK",null,"시나리오ID","시나리오 고유 id (백단에서 seq)",null,null,null,"시나리오ID","scnr_id",null,null,"VARCHAR2(40)",{"$nulls":10},"CREATE TABLE ",{"$f":"N141&\" (\"","v":"soitsanlsintsvalue ("},{"$f":"O143&\" \"","v":"scnr_id "},{"$f":"R143&\" \"","v":"VARCHAR2(40) "},{"$f":"IF(H143=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",","CONSTRAINT ",{"$f":"\"PK_\"&N141&\" PRIMARY KEY (\"","v":"PK_soitsanlsintsvalue PRIMARY KEY ("},{"$f":"IF(OR(G143=\"PK\", G143=\"PK/FK\"), O143, \"\")","v":"scnr_id"},",","COMMENT ON COLUMN ",{"$f":"N$141&\". \"","v":"soitsanlsintsvalue. "},{"$f":"O143","v":"scnr_id"}," IS ",{"$f":"\"'\"&I143&\"'\"","v":"'시나리오ID'"},";",null,null,null,""]
[null,null,"시간계획ID","hr_plan_id",null,"VARCHAR2(10)","PK",null,"타임플랜번호","HH24MI_HH24MI",null,null,null,"시간계획ID","hr_plan_id","VARCHAR2(10)",null,"VARCHAR2(10)",{"$nulls":12},"hr_plan_id ","VARCHAR2(10) ","",",",null,null,"hr_plan_id",",","COMMENT ON COLUMN ","soitsanlsintsvalue. ","hr_plan_id"," IS ","'타임플랜번호'",";",null,null,null,""]
[null,null,"분석구분코드","anls_div_cd",null,"VARCHAR2(1)","PK",null,"분석구분코드(1:현황. 2:최적화)",{"$nulls":4},"분석구분코드","anls_div_cd",null,null,"VARCHAR2(1)",{"$nulls":12},"anls_div_cd ","VARCHAR2(1) ","",",",null,null,"anls_div_cd",",","COMMENT ON COLUMN ","soitsanlsintsvalue. ","anls_div_cd"," IS ","'분석구분코드(1:현황. 2:최적화)'",";",null,null,null,""]
[null,null,"노드 ID","node_id",11,"VARCHAR2(300)","PK/FK",null,"교차로 노드ID",{"$nulls":4},"노드 ID","node_id",null,null,"VARCHAR2(300)",{"$nulls":12},"node_id ","VARCHAR2(300) ","",",",null,null,"node_id",{"$f":"\") using index tablespace \" &AJ155& \") TABLESPACE \" &AI155&\";\"","v":") using index tablespace SOIT_I08_A001) TABLESPACE SOIT_D08_A001;"},"COMMENT ON COLUMN ","soitsanlsintsvalue. ","node_id"," IS ","'교차로 노드ID'",";",null,null,null,""]
[null,null,"총지체시간","tot_dely_tm",null,"NUMBER(9,2)",null,null,"총지체시간",{"$nulls":4},"총지체시간","tot_dely_tm",null,null,"NUMBER(7,2)",{"$nulls":12},"tot_dely_tm ","NUMBER(7,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsanlsintsvalue. ","tot_dely_tm"," IS ","'총지체시간'",";",null,null,null,""]
[null,null,"평균지체시간","avg_dely_tm",null,"NUMBER(7,2)",null,null,"평균지체시간",{"$nulls":4},"평균지체시간","avg_dely_tm",null,null,"NUMBER(7,2)",{"$nulls":12},"avg_dely_tm ","NUMBER(7,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsanlsintsvalue. ","avg_dely_tm"," IS ","'평균지체시간'",";",null,null,null,""]
[null,null,"교통량","trvl",null,"NUMBER(10)",null,null,"관측교통량",{"$nulls":4},"교통량","trvl",null,null,"NUMBER(10)",{"$nulls":12},"trvl ","NUMBER(10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsanlsintsvalue. ","trvl"," IS ","'관측교통량'",";",null,null,null,""]
[null,null,"평균속도","avg_sped",null,"NUMBER(5,2)",null,null,"평균속도",{"$nulls":4},"평균속도","avg_sped","NUMBER(5,2)",null,"NUMBER(5,2)",{"$nulls":12},"avg_sped ","NUMBER(5,2) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlsintsvalue. ","avg_sped"," IS ","'평균속도'",";"]
[null,null,"평균대기행렬","avg_queu_lngt",null,"NUMBER(19,9)",null,null,"평균대기행렬 길이(m)",{"$nulls":4},"평균대기행렬","avg_queu_lngt","NUMBER(19,9)",null,"NUMBER(19,9)",{"$nulls":12},"avg_queu_lngt ","NUMBER(19,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlsintsvalue. ","avg_queu_lngt"," IS ","'평균대기행렬 길이(m)'",";"]
[null,null,"차선별평균대기행렬","lane_avg_queu_lngt",null,"NUMBER(19,9)",null,null,"차선별 평균대기행렬 길이(m)",{"$nulls":4},"차선별평균대기행렬","lane_avg_queu_lngt","NUMBER(19,9)",null,"NUMBER(19,9)",{"$nulls":12},"lane_avg_queu_lngt ","NUMBER(19,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlsintsvalue. ","lane_avg_queu_lngt"," IS ","'차선별 평균대기행렬 길이(m)'",";"]
[null,null,"진입로최대대기행렬","entr_max_queu_lngt",null,"NUMBER(19,9)",null,null,"진입로별 최대대기행렬 길이(m)",{"$nulls":4},"진입로별 최대대기행렬","entr_max_queu_lngt","NUMBER(19,9)",null,"NUMBER(19,9)",{"$nulls":12},"entr_max_queu_lngt ","NUMBER(19,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitsanlsintsvalue. ","entr_max_queu_lngt"," IS ","'진입로별 최대대기행렬 길이(m)'",";"]
[{"$nulls":30},{"$f":"CONCATENATE(AI143:AL149)","v":{"$error":"#VALUE!"}}," ",{"$nulls":15},{"$f":"IF(LEFT(AE154, 13) = \"CONSTRAINT PK\", AE154, \"\")","v":{"$error":"#VALUE!"}}]
[{"$nulls":34},"SOIT_D08_A001","SOIT_I08_A001"]
[null,"차량 이동궤적 테이블",{"$nulls":11},"soitsanlsvhclmvmntowh",{"$nulls":33},{"$f":"IF(LEFT(AE156, 13) = \"CONSTRAINT PK\", AE156, \"\")","v":""}]
[39,"Table Name","Attribute Name","Column Name","#","Data type",null,"Column Null Option","Comment","1초단위로 하지 않고 주기를 여유있게 잡아서 데이터화",null,null,null,"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N156&\" \"","v":"soitsanlsvhclmvmntowh "},null," IS ",{"$f":"\"'\"&B156&\"'\"","v":"'차량 이동궤적 테이블'"},";",null,null,null,""]
["TIBERO","soitsanlsvhclmvmntowh","시나리오ID","scnr_id",null,"VARCHAR2(40)","PK",null,"시나리오ID","시나리오 고유 id (백단에서 seq)",null,null,null,"시나리오ID","scnr_id",null,null,"VARCHAR2(40)",{"$nulls":10},"CREATE TABLE ",{"$f":"N156&\" (\"","v":"soitsanlsvhclmvmntowh ("},{"$f":"O158&\" \"","v":"scnr_id "},{"$f":"R158&\" \"","v":"VARCHAR2(40) "},{"$f":"IF(H158=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",","CONSTRAINT ",{"$f":"\"PK_\"&N156&\" PRIMARY KEY (\"","v":"PK_soitsanlsvhclmvmntowh PRIMARY KEY ("},{"$f":"IF(OR(G158=\"PK\", G158=\"PK/FK\"), O158, \"\")","v":"scnr_id"},",","COMMENT ON COLUMN ",{"$f":"N$156&\". \"","v":"soitsanlsvhclmvmntowh. "},{"$f":"O158","v":"scnr_id"}," IS ",{"$f":"\"'\"&I158&\"'\"","v":"'시나리오ID'"},";",null,null,null,""]
[null,null,"분석구분코드","anls_div_cd",null,"VARCHAR2(1)","PK",null,"분석구분코드(1:현황. 2:최적화)",{"$nulls":4},"분석구분코드","anls_div_cd",null,null,"VARCHAR2(1)",{"$nulls":12},"anls_div_cd ","VARCHAR2(1) ","",",",null,null,"anls_div_cd",",","COMMENT ON COLUMN ","soitsanlsvhclmvmntowh. ","anls_div_cd"," IS ","'분석구분코드(1:현황. 2:최적화)'",";",null,null,null,""]
[null,null,"시간계획ID","hr_plan_id",null,"VARCHAR2(10)","PK",null,"타임플랜번호","HH24MI_HH24MI",null,null,null,"시간계획ID","hr_plan_id","VARCHAR2(10)",null,"VARCHAR2(10)",{"$nulls":12},"hr_plan_id ","VARCHAR2(10) ","",",",null,null,"hr_plan_id",",","COMMENT ON COLUMN ","soitsanlsvhclmvmntowh. ","hr_plan_id"," IS ","'타임플랜번호'",";",null,null,null,""]
[null,null,"시간그룹번호","TM_GRUP_NO",null,"NUMBER(10)","PK",null,"시간그룹번호(초단위 시작시간)","5분(300) 단위로 누적값",null,null,null,"시간그룹번호","TM_GRUP_NO",null,null,"NUMBER(10)",{"$nulls":12},"TM_GRUP_NO ","NUMBER(10) ","",",",null,null,"TM_GRUP_NO",",","COMMENT ON COLUMN ","soitsanlsvhclmvmntowh. ","TM_GRUP_NO"," IS ","'시간그룹번호(초단위 시작시간)'",";",null,null,null,""]
[null,null,"위치수집유닉스시각","locn_clct_unix_tm",null,"NUMBER(10)","PK",null,"위치수집유닉스시각",{"$nulls":4},"위치수집유닉스시각","locn_clct_unix_tm",null,null,"NUMBER(10)",{"$nulls":12},"locn_clct_unix_tm ","NUMBER(10) ","",",",null,null,"locn_clct_unix_tm",",","COMMENT ON COLUMN ","soitsanlsvhclmvmntowh. ","locn_clct_unix_tm"," IS ","'위치수집유닉스시각'",";",null,null,null,""]
[null,null,"차량ID","vhcl_id",null,"VARCHAR2(20)","PK",null,"차량ID",{"$nulls":4},"차량ID","vhcl_id",null,null,"VARCHAR2(20)",{"$nulls":12},"vhcl_id ","VARCHAR2(20) ","",",",null,null,"vhcl_id",{"$f":"\") using index tablespace \" &AJ171& \") TABLESPACE \" &AI171&\";\"","v":") using index tablespace SOIT_I08_A001) TABLESPACE SOIT_D08_A001;"},"COMMENT ON COLUMN ","soitsanlsvhclmvmntowh. ","vhcl_id"," IS ","'차량ID'",";",null,null,null,""]
[null,null,"순간속도","mmnt_sped",null,"NUMBER(5,2)",null,null,"순간속도 (m/s)",{"$nulls":4},"순간속도","mmnt_sped",null,null,"NUMBER(5,2)",{"$nulls":12},"mmnt_sped ","NUMBER(5,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsanlsvhclmvmntowh. ","mmnt_sped"," IS ","'순간속도 (m/s)'",";",null,null,null,""]
[null,null,"비혼잡속도","non_cngt_sped",null,"NUMBER(5,2)",null,null,"비혼잡속도 (m/s)",{"$nulls":4},"비혼잡속도","non_cngt_sped",null,null,"NUMBER(5,2)",{"$nulls":12},"non_cngt_sped ","NUMBER(5,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsanlsvhclmvmntowh. ","non_cngt_sped"," IS ","'비혼잡속도 (m/s)'",";",null,null,null,""]
[null,null,"차량경도","vhcl_lot",null,"NUMBER(13,10)",null,null,"차량경도",{"$nulls":4},"차량경도","vhcl_lot",null,null,"NUMBER(13,10)",{"$nulls":12},"vhcl_lot ","NUMBER(13,10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsanlsvhclmvmntowh. ","vhcl_lot"," IS ","'차량경도'",";",null,null,null,""]
[null,null,"차량위도","vhcl_lat",null,"NUMBER(12,10)",null,null,"차량위도",{"$nulls":4},"차량위도","vhcl_lat",null,null,"NUMBER(12,10)",{"$nulls":12},"vhcl_lat ","NUMBER(12,10) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsanlsvhclmvmntowh. ","vhcl_lat"," IS ","'차량위도'",";",null,null,null,""]
[null,null,"지체시간","dely_tm",null,"NUMBER(5,2)",null,null,"평균지체시간",{"$nulls":4},"지체시간","dely_tm",null,null,"NUMBER(5,2)",{"$nulls":12},"dely_tm ","NUMBER(5,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsanlsvhclmvmntowh. ","dely_tm"," IS ","'평균지체시간'",";",null,null,null,""]
[null,null,"차량길이","vhcl_lngt",null,"NUMBER(5,2)",null,null,"차량길이(m)",{"$nulls":4},"차량길이","vhcl_lngt",null,null,"NUMBER(5,2)",{"$nulls":12},"vhcl_lngt ","NUMBER(5,2) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsanlsvhclmvmntowh. ","vhcl_lngt"," IS ","'차량길이(m)'",";",null,null,null,""]
[{"$nulls":30},{"$f":"CONCATENATE(AI158:AL169)","v":{"$error":"#VALUE!"}}," ",{"$nulls":15},{"$error":"#VALUE!"}]
[{"$nulls":34},"SOIT_D08_A001","SOIT_I08_A001"]
[null,"최적 연동그룹 테이블",{"$nulls":11},"soitsanlslnkggrupinfo",{"$nulls":33},{"$f":"IF(LEFT(AE172, 13) = \"CONSTRAINT PK\", AE172, \"\")","v":""}]
[40,"Table Name","Attribute Name","Column Name","#","Data type",null,"Column Null Option","Comment",{"$nulls":4},"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N172&\" \"","v":"soitsanlslnkggrupinfo "},null," IS ",{"$f":"\"'\"&B172&\"'\"","v":"'최적 연동그룹 테이블'"},";",null,null,null,""]
["TIBERO","soitsanlslnkggrupinfo","연동그룹ID","lnkg_grup_id",null,"VARCHAR2(20)","PK/FK",null,"연동그룹ID",{"$nulls":4},"연동그룹ID","lnkg_grup_id","VARCHAR2(20)",null,"VARCHAR2(20)",{"$nulls":10},"CREATE TABLE ",{"$f":"N172&\" (\"","v":"soitsanlslnkggrupinfo ("},{"$f":"O174&\" \"","v":"lnkg_grup_id "},{"$f":"R174&\" \"","v":"VARCHAR2(20) "},{"$f":"IF(H174=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",","CONSTRAINT ",{"$f":"\"PK_\"&N172&\" PRIMARY KEY (\"","v":"PK_soitsanlslnkggrupinfo PRIMARY KEY ("},{"$f":"IF(OR(G174=\"PK\", G174=\"PK/FK\"), O174, \"\")","v":"lnkg_grup_id"},",","COMMENT ON COLUMN ",{"$f":"N$172&\". \"","v":"soitsanlslnkggrupinfo. "},{"$f":"O174","v":"lnkg_grup_id"}," IS ",{"$f":"\"'\"&I174&\"'\"","v":"'연동그룹ID'"},";",null,null,null,""]
[null,null,"노드 ID","node_id",null,"VARCHAR2(300)","PK/FK",null,"교차로 노드ID",{"$nulls":4},"노드 ID","node_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":12},"node_id ","VARCHAR2(300) ","",",",null,null,"node_id",{"$f":"\") using index tablespace \" &AJ178& \") TABLESPACE \" &AI178&\";\"","v":") using index tablespace SOIT_I08_A001) TABLESPACE SOIT_D08_A001;"},"COMMENT ON COLUMN ","soitsanlslnkggrupinfo. ","node_id"," IS ","'교차로 노드ID'",";",null,null,null,""]
[null,null,"연동그룹구성순서","lnkg_grup_cnfg_seq",null,"NUMBER(3)",null,null,"연동그룹구성순서",{"$nulls":4},"연동그룹구성순서","lnkg_grup_cnfg_seq","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"lnkg_grup_cnfg_seq ","NUMBER(3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsanlslnkggrupinfo. ","lnkg_grup_cnfg_seq"," IS ","'연동그룹구성순서'",";",null,null,null,""]
[{"$nulls":30},{"$f":"CONCATENATE(AI174:AL176)","v":{"$error":"#VALUE!"}}," ","",null,null,null,"",{"$nulls":10},{"$error":"#VALUE!"}]
[{"$nulls":34},"SOIT_D08_A001","SOIT_I08_A001"]
[null,"최적연동그룹 구성 엣지그룹 테이블",{"$nulls":11},"soitsanlsedgegrupinfo",{"$nulls":16},{"$f":"O179&\" \"","v":" "},{"$f":"R179&\" \"","v":" "},{"$f":"IF(H179=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},null,null,null,{"$f":"IF(OR(G179=\"PK\", G179=\"PK/FK\"), O179, \"\")","v":""},{"$nulls":10},{"$f":"IF(LEFT(AE179, 13) = \"CONSTRAINT PK\", AE179, \"\")","v":""}]
[41,"Table Name","Attribute Name","Column Name","#","Data type",null,"Column Null Option","Comment",{"$nulls":4},"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N179&\" \"","v":"soitsanlsedgegrupinfo "},null," IS ",{"$f":"\"'\"&B179&\"'\"","v":"'최적연동그룹 구성 엣지그룹 테이블'"},";",null,null,null,""]
["TIBERO","soitsanlsedgegrupinfo","엣지그룹ID","edge_grup_id",null,"VARCHAR2(300)","PK/FK",null,"엣지그룹ID",{"$nulls":4},"엣지그룹ID","edge_grup_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":10},"CREATE TABLE ",{"$f":"N179&\" (\"","v":"soitsanlsedgegrupinfo ("},{"$f":"O181&\" \"","v":"edge_grup_id "},{"$f":"R181&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(H181=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",","CONSTRAINT ",{"$f":"\"PK_\"&N179&\" PRIMARY KEY (\"","v":"PK_soitsanlsedgegrupinfo PRIMARY KEY ("},{"$f":"IF(OR(G181=\"PK\", G181=\"PK/FK\"), O181, \"\")","v":"edge_grup_id"},",","COMMENT ON COLUMN ",{"$f":"N$179&\". \"","v":"soitsanlsedgegrupinfo. "},{"$f":"O181","v":"edge_grup_id"}," IS ",{"$f":"\"'\"&I181&\"'\"","v":"'엣지그룹ID'"},";",null,null,null,""]
[null,null,"시작노드 ID","bgng_node_id",null,"VARCHAR2(300)","PK/FK",null,"시작 교차로 노드ID",{"$nulls":4},"시작노드 ID","bgng_node_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":12},"bgng_node_id ","VARCHAR2(300) ","",",",null,null,"bgng_node_id",",","COMMENT ON COLUMN ","soitsanlsedgegrupinfo. ","bgng_node_id"," IS ","'시작 교차로 노드ID'",";",null,null,null,""]
[null,null,"종료노드 ID","end_node_id",null,"VARCHAR2(300)","PK/FK",null,"종료 교차로 노드ID",{"$nulls":4},"종료노드 ID","end_node_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":12},"end_node_id ","VARCHAR2(300) ","",",",null,null,"end_node_id",{"$f":"\") using index tablespace \" &AJ185& \") TABLESPACE \" &AI185&\";\"","v":") using index tablespace SOIT_I08_A001) TABLESPACE SOIT_D08_A001;"},"COMMENT ON COLUMN ","soitsanlsedgegrupinfo. ","end_node_id"," IS ","'종료 교차로 노드ID'",";",null,null,null,""]
[{"$nulls":30},{"$f":"CONCATENATE(AI181:AL183)","v":{"$error":"#VALUE!"}}," ","",{"$nulls":14},{"$error":"#VALUE!"}]
[{"$nulls":34},"SOIT_D08_A001","SOIT_I08_A001"]
[null,"최적연동그룹 구성 엣지 테이블",{"$nulls":11},"soitsanlsedgeinfo",{"$nulls":16},{"$f":"O186&\" \"","v":" "},{"$f":"R186&\" \"","v":" "},{"$f":"IF(H186=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},{"$nulls":14},{"$f":"IF(LEFT(AE186, 13) = \"CONSTRAINT PK\", AE186, \"\")","v":""}]
[42,"Table Name","Attribute Name","Column Name","#","Data type",null,"Column Null Option","Comment",{"$nulls":4},"논리명","물리명","형태","VOLT","TIBERO",{"$nulls":20},"COMMENT ON TABLE",{"$f":"N186&\" \"","v":"soitsanlsedgeinfo "},null," IS ",{"$f":"\"'\"&B186&\"'\"","v":"'최적연동그룹 구성 엣지 테이블'"},";",null,null,null,""]
["TIBERO","soitsanlsedgeinfo","엣지그룹ID","edge_grup_id",null,"VARCHAR2(300)","PK/FK",null,"엣지그룹ID",{"$nulls":4},"엣지그룹ID","edge_grup_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":10},"CREATE TABLE ",{"$f":"N186&\" (\"","v":"soitsanlsedgeinfo ("},{"$f":"O188&\" \"","v":"edge_grup_id "},{"$f":"R188&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(H188=\"NOT NULL\", \"NOT NULL\", \"\")","v":""},",","CONSTRAINT ",{"$f":"\"PK_\"&N186&\" PRIMARY KEY (\"","v":"PK_soitsanlsedgeinfo PRIMARY KEY ("},{"$f":"IF(OR(G188=\"PK\", G188=\"PK/FK\"), O188, \"\")","v":"edge_grup_id"},",","COMMENT ON COLUMN ",{"$f":"N$186&\". \"","v":"soitsanlsedgeinfo. "},{"$f":"O188","v":"edge_grup_id"}," IS ",{"$f":"\"'\"&I188&\"'\"","v":"'엣지그룹ID'"},";",null,null,null,""]
[null,null,"엣지그룹구성순서","edge_grup_cnfg_seq",null,"NUMBER(3)",null,null,"엣지그룹구성순서",{"$nulls":4},"엣지그룹구성순서","edge_grup_cnfg_seq","NUMBER(3)",null,"NUMBER(3)",{"$nulls":12},"edge_grup_cnfg_seq ","NUMBER(3) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitsanlsedgeinfo. ","edge_grup_cnfg_seq"," IS ","'엣지그룹구성순서'",";",null,null,null,""]
[null,null,"엣지ID","edge_id",null,"VARCHAR2(300)","PK/FK",null,"소속 엣지ID",{"$nulls":4},"엣지ID","edge_id","VARCHAR2(300)",null,"VARCHAR2(300)",{"$nulls":12},"edge_id ","VARCHAR2(300) ","",",",null,null,"edge_id",{"$f":"\") using index tablespace \" &AJ192& \") TABLESPACE \" &AI192&\";\"","v":") using index tablespace SOIT_I08_A001) TABLESPACE SOIT_D08_A001;"},"COMMENT ON COLUMN ","soitsanlsedgeinfo. ","edge_id"," IS ","'소속 엣지ID'",";",null,null,null,""]
[{"$nulls":30},{"$f":"CONCATENATE(AI188:AL190)","v":{"$error":"#VALUE!"}},null,"",{"$nulls":14},{"$error":"#VALUE!"}]
[{"$nulls":34},"SOIT_D08_A001","SOIT_I08_A001"]

{"sheet":"센터(집계,통계,화면표출용 등)","index":11,"n_rows":532,"n_cols":64,"rows_kept":532,"cut":false,"hidden":false,"merged":[[302,0,302,9],[303,0,303,9],[320,0,320,9],[321,0,321,9],[331,0,331,9],[332,0,332,9],[342,0,342,9],[343,0,343,9],[352,0,352,9],[353,0,353,9],[364,0,364,9],[365,0,365,9],[374,0,374,9],[375,0,375,9],[385,0,385,9],[386,0,386,9],[396,0,396,9],[397,0,397,9],[407,0,407,9],[408,0,408,9],[418,0,418,9],[419,0,419,9],[429,0,429,9],[430,0,430,9],[440,0,440,9],[441,0,441,9],[451,0,451,9],[452,0,452,9],[498,0,498,9],[509,0,509,9],[510,0,510,9],[520,0,520,9],[521,0,521,9],[462,0,462,9],[463,0,463,9],[473,0,473,9],[474,0,474,9],[484,0,484,9],[485,0,485,9],[497,0,497,9],[0,0,0,9],[0,12,0,17],[0,21,0,30],[0,31,0,36],[1,0,1,9],[19,12,19,17],[19,31,19,36],[19,0,19,9],[20,0,20,9],[36,0,36,9],[37,0,37,9],[49,0,49,9],[50,0,50,9],[74,0,74,9],[75,0,75,9],[98,0,98,9],[99,0,99,9],[113,0,113,9],[114,0,114,9],[127,0,127,9],[128,0,128,9],[223,0,223,9],[239,0,239,9],[240,0,240,9],[256,0,256,9],[148,0,148,9],[149,0,149,9],[167,0,167,9],[168,0,168,9],[195,0,195,9],[196,0,196,9],[222,0,222,9],[257,0,257,9],[259,45,259,47],[260,45,260,47],[274,45,274,47],[276,45,276,47],[263,45,263,47],[264,45,264,47],[266,45,266,47],[267,45,267,47],[270,0,270,9],[271,0,271,9],[273,45,273,47],[277,45,277,47],[279,45,279,47],[280,45,280,47],[283,0,283,9],[284,0,284,9]]}
["세그먼트별 집계 테이블 - 실시간",{"$nulls":11},"VOLT DDL",{"$nulls":8},"TIBERO DDL",{"$nulls":9},"COMMENTS"]
["soitcsgmnrltmtot"]
["NO","속성명","컬럼명","PK/FK","NULL","형태",null,"TIBERO","길이","비고",{"$nulls":21},"COMMENT ON TABLE",{"$f":"A2&\" \"","v":"soitcsgmnrltmtot "},null," IS ",{"$f":"\"'\"&SUBSTITUTE(A1,\"테이블\",\"\")&\"'\"","v":"'세그먼트별 집계  - 실시간'"},";"]
[1,"세그먼트ID","sgmn_id","PK/FK","NOT NULL","VARCHAR2(300)",null,"VARCHAR2(300)",20,"세그먼트ID",{"$nulls":11},"CREATE TABLE ",{"$f":"A2&\" (\"","v":"soitcsgmnrltmtot ("},{"$f":"C4&\" \"","v":"sgmn_id "},{"$f":"H4&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(E4=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(D4=\"PK\", D4=\"PK/FK\"), C4, \"\")","v":"sgmn_id"},{"$f":"IF(OR(D4=\"PK\", D4=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$A$2&\".\"","v":"soitcsgmnrltmtot."},{"$f":"C4","v":"sgmn_id"}," IS ",{"$f":"\"'\"&J4&\"'\"","v":"'세그먼트ID'"},";"]
[2,"지역구분코드","rgn_prttn_cd","PK/FK","NOT NULL","CHAR(2)",null,"VARCHAR2(2)",null,"지역분할코드(051)",{"$nulls":13},"rgn_prttn_cd ","VARCHAR2(2) ","NOT NULL",",",null,null,"rgn_prttn_cd",",","COMMENT ON COLUMN ","soitcsgmnrltmtot.","rgn_prttn_cd"," IS ","'지역분할코드(051)'",";"]
[3,"실측여부","acsr_yn","PK","NOT NULL","CHAR(1)",null,"VARCHAR2(1)",1,"실측여부 (500)",{"$nulls":13},"acsr_yn ","VARCHAR2(1) ","NOT NULL",",",null,null,"acsr_yn",",","COMMENT ON COLUMN ","soitcsgmnrltmtot.","acsr_yn"," IS ","'실측여부 (500)'",";"]
[4,"집계시작유닉스시각","tot_bgng_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"집계시작유닉스시각",{"$nulls":13},"tot_bgng_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"tot_bgng_unix_tm",",","COMMENT ON COLUMN ","soitcsgmnrltmtot.","tot_bgng_unix_tm"," IS ","'집계시작유닉스시각'",";"]
[5,"집계종료유닉스시각","tot_end_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"집계종료유닉스시각",{"$nulls":13},"tot_end_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"tot_end_unix_tm",",","COMMENT ON COLUMN ","soitcsgmnrltmtot.","tot_end_unix_tm"," IS ","'집계종료유닉스시각'",";"]
[6,"차종코드","kncr_cd","PK","NOT NULL","CHAR(10)",null,"VARCHAR2(10)",3,"차종구분코드 (008)","차종\n( LBUS:대형버스, LTRUCK:대형트럭(4.5T이상), MBUS:미니버스,\nMOTOR:오토바이, MTRUCK:트럭(4.5T미만), PCAR:승용차 )",{"$nulls":12},"kncr_cd ","VARCHAR2(10) ","NOT NULL",",",null,null,"kncr_cd",")","COMMENT ON COLUMN ","soitcsgmnrltmtot.","kncr_cd"," IS ","'차종구분코드 (008)'",";"]
[7,"교통량","trvl",null,"NULL","NUMBER(10)",null,"NUMBER(10)",10,"기간내 총통행량",{"$nulls":13},"trvl ","NUMBER(10) ","",",",null,null,"",{"$f":"IF(OR(D10=\"PK\", D10=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitcsgmnrltmtot.","trvl"," IS ","'기간내 총통행량'",";"]
[8,"궤적건수","cnt",null,"NULL","NUMBER(10)",null,"NUMBER(10)",10,"기간내 궤적건수",{"$nulls":13},"cnt ","NUMBER(10) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcsgmnrltmtot.","cnt"," IS ","'기간내 궤적건수'",";"]
[9,"속도","sped",null,"NULL","NUMBER(5,2)",null,"NUMBER(5,2)","5,2","기간내 평균속도",{"$nulls":13},"sped ","NUMBER(5,2) ","",",",null,null,{"$f":"IF(OR(D12=\"PK\", D12=\"PK/FK\"), C12, \"\")","v":""},{"$f":"IF(OR(D12=\"PK\", D12=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitcsgmnrltmtot.","sped"," IS ","'기간내 평균속도'",";"]
[10,"시간점유율","hr_ocpn_rt",null,"NULL","NUMBER(13,9)",null,"NUMBER(13,9)","12,9","시간점유율 (SUM(세그먼트길이/기간내 속도))",{"$nulls":13},"hr_ocpn_rt ","NUMBER(13,9) ","",",",null,null,"","","COMMENT ON COLUMN ","soitcsgmnrltmtot.","hr_ocpn_rt"," IS ","'시간점유율 (SUM(세그먼트길이/기간내 속도))'",";"]
[11,"공간점유율","spae_ocpn_rt",null,"NULL","NUMBER(13,9)",null,"NUMBER(13,9)","12,9","공간점유율 (기간내 총통행량/세그먼트길이)",{"$nulls":13},"spae_ocpn_rt ","NUMBER(13,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcsgmnrltmtot.","spae_ocpn_rt"," IS ","'공간점유율 (기간내 총통행량/세그먼트길이)'",";"]
[12,"지체시간","dely_tm",null,"NULL","NUMBER(7,2)",null,"NUMBER(7,2)","5,2","차량당 평균지체시간 (SUM(1 - 속도/자유속도))",{"$nulls":13},"dely_tm ","NUMBER(7,2) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcsgmnrltmtot.","dely_tm"," IS ","'차량당 평균지체시간 (SUM(1 - 속도/자유속도))'",";"]
[13,"포화도","strtn_trst_rt",null,"NULL","NUMBER(12,9)",null,"NUMBER(13,9)","12,9","포화도 (교통량/2200)","집계안함.",{"$nulls":12},"strtn_trst_rt ","NUMBER(13,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcsgmnrltmtot.","strtn_trst_rt"," IS ","'포화도 (교통량/2200)'",";"]
[14,"정지율","stop_notm_rt",null,"NULL","NUMBER(7,2)",null,"NUMBER(7,2)","5,2","정지율 (속도가 0인 이동궤적 비율)",{"$nulls":13},"stop_notm_rt ","NUMBER(7,2) ","",{"$f":"\") TABLESPACE \"&AB19&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_T001 NOLOGGING"},{"$nulls":4},"COMMENT ON COLUMN ","soitcsgmnrltmtot.","stop_notm_rt"," IS ","'정지율 (속도가 0인 이동궤적 비율)'",";"]
[{"$nulls":23},{"$f":"CONCATENATE(AB18:AD18)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (tot_bgng_unix_tm) INTERVAL (86400) STORE IN (\"&AB19&\") (PARTITION BFR_\" & A2& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AB19&\");\"","v":"PARTITION BY RANGE (tot_bgng_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_T001) (PARTITION BFR_soitcsgmnrltmtot_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_T001);"},{"$f":"\"CREATE INDEX PK_\" & A2& \" ON \" & A2 & CONCATENATE(AC4:AE15) & \" LOCAL (PARTITION BFR_\" & A2 & \"_20221101 TABLESPACE \"&AC19&\") TABLESPACE \"&AC19&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & A2 & \" ADD CONSTRAINT PK_\" & A2 & \" PRIMARY KEY \" & CONCATENATE(AC4:AE15) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"IF(LEFT(X18, 13) = \"CONSTRAINT PK\", X18, \"\")","v":{"$error":"#VALUE!"}}]
[{"$nulls":27},"SOIT_D08_T001","SOIT_I08_T001"]
["세그먼트별 집계 테이블 - 배치",{"$nulls":37},{"$f":"IF(LEFT(X20, 13) = \"CONSTRAINT PK\", X20, \"\")","v":""}]
["soitcsgmnarngtot",{"$nulls":37},""]
["NO","속성명","컬럼명","PK/FK","NULL","형태",null,"TIBERO","길이","비고",{"$nulls":21},"COMMENT ON TABLE",{"$f":"A21&\" \"","v":"soitcsgmnarngtot "},null," IS ",{"$f":"\"'\"&SUBSTITUTE(A20,\"테이블\",\"\")&\"'\"","v":"'세그먼트별 집계  - 배치'"},";",null,""]
[1,"세그먼트ID","sgmn_id","PK/FK","NOT NULL","VARCHAR2(300)",null,"VARCHAR2(300)",20,"세그먼트ID",{"$nulls":11},"CREATE TABLE ",{"$f":"A21&\" (\"","v":"soitcsgmnarngtot ("},{"$f":"C23&\" \"","v":"sgmn_id "},{"$f":"H23&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(E23=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(D23=\"PK\", D23=\"PK/FK\"), C23, \"\")","v":"sgmn_id"},{"$f":"IF(OR(D23=\"PK\", D23=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$A$21&\".\"","v":"soitcsgmnarngtot."},{"$f":"C23","v":"sgmn_id"}," IS ",{"$f":"\"'\"&J23&\"'\"","v":"'세그먼트ID'"},";",null,""]
[2,"집계구분코드","tot_se_cd","PK","NOT NULL","CHAR(1)",null,"VARCHAR2(1)",1,"시간유형 (011)","집계구분코드 (1:신호현시, 2:1분단위, 3:5분단위, 4:15분, 5:60분, 6:일별)",{"$nulls":12},"tot_se_cd ","VARCHAR2(1) ","NOT NULL",",",null,null,"tot_se_cd",",","COMMENT ON COLUMN ","soitcsgmnarngtot.","tot_se_cd"," IS ","'시간유형 (011)'",";",null,"",null,null,"시간구분  첨두시간별?"]
[3,"집계시작유닉스시각","tot_bgng_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"집계시작유닉스시각",{"$nulls":13},"tot_bgng_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"tot_bgng_unix_tm",",","COMMENT ON COLUMN ","soitcsgmnarngtot.","tot_bgng_unix_tm"," IS ","'집계시작유닉스시각'",";",null,""]
[4,"집계종료유닉스시각","tot_end_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"집계종료유닉스시각",{"$nulls":13},"tot_end_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"tot_end_unix_tm",",","COMMENT ON COLUMN ","soitcsgmnarngtot.","tot_end_unix_tm"," IS ","'집계종료유닉스시각'",";",null,""]
[5,"차종코드","kncr_cd","PK","NOT NULL","CHAR(10)",null,"VARCHAR2(10)",3,"차종구분코드 (008)","차종\n( LBUS:대형버스, LTRUCK:대형트럭(4.5T이상), MBUS:미니버스,\nMOTOR:오토바이, MTRUCK:트럭(4.5T미만), PCAR:승용차 )",{"$nulls":12},"kncr_cd ","VARCHAR2(10) ","NOT NULL",",",null,null,"kncr_cd",")","COMMENT ON COLUMN ","soitcsgmnarngtot.","kncr_cd"," IS ","'차종구분코드 (008)'",";",null,""]
[6,"교통량","trvl",null,"NULL","NUMBER(10)",null,"NUMBER(10)",10,"기간내 총통행량",{"$nulls":13},"trvl ","NUMBER(10) ","",",",null,null,"",{"$f":"IF(OR(D28=\"PK\", D28=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitcsgmnarngtot.","trvl"," IS ","'기간내 총통행량'",";",null,""]
[7,"속도","sped",null,"NULL","NUMBER(5,2)",null,"NUMBER(5,2)","5,2","기간내 평균속도",{"$nulls":13},"sped ","NUMBER(5,2) ","",",",null,null,"","","COMMENT ON COLUMN ","soitcsgmnarngtot.","sped"," IS ","'기간내 평균속도'",";",null,""]
[8,"시간점유율","hr_ocpn_rt",null,"NULL","NUMBER(13,9)",null,"NUMBER(13,9)","12,9","시간점유율 (SUM(세그먼트길이/기간내 속도))",{"$nulls":13},"hr_ocpn_rt ","NUMBER(13,9) ","",",",null,null,"","","COMMENT ON COLUMN ","soitcsgmnarngtot.","hr_ocpn_rt"," IS ","'시간점유율 (SUM(세그먼트길이/기간내 속도))'",";",null,""]
[9,"공간점유율","spae_ocpn_rt",null,"NULL","NUMBER(13,9)",null,"NUMBER(13,9)","12,9","공간점유율 (기간내 총통행량/세그먼트길이)",{"$nulls":13},"spae_ocpn_rt ","NUMBER(13,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcsgmnarngtot.","spae_ocpn_rt"," IS ","'공간점유율 (기간내 총통행량/세그먼트길이)'",";",null,""]
[11,"지체시간","dely_tm",null,"NULL","NUMBER(7,2)",null,"NUMBER(7,2)","5,2","차량당 평균지체시간 (SUM(1 - 속도/자유속도))",{"$nulls":13},"dely_tm ","NUMBER(7,2) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcsgmnarngtot.","dely_tm"," IS ","'차량당 평균지체시간 (SUM(1 - 속도/자유속도))'",";"]
[12,"포화도","strtn_trst_rt",null,"NULL","NUMBER(12,9)",null,"NUMBER(13,9)","12,9","포화도 (교통량/2200)","집계안함.",{"$nulls":12},"strtn_trst_rt ","NUMBER(13,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcsgmnarngtot.","strtn_trst_rt"," IS ","'포화도 (교통량/2200)'",";"]
[13,"정지율","stop_notm_rt",null,"NULL","NUMBER(7,2)",null,"NUMBER(7,2)","5,2","정지율 (속도가 0인 이동궤적 비율)",{"$nulls":13},"stop_notm_rt ","NUMBER(7,2) ","",{"$f":"\") TABLESPACE \"&AB36&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_T002 NOLOGGING"},{"$nulls":4},"COMMENT ON COLUMN ","soitcsgmnarngtot.","stop_notm_rt"," IS ","'정지율 (속도가 0인 이동궤적 비율)'",";"]
[{"$nulls":23},{"$f":"CONCATENATE(AB35:AD35)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (tot_bgng_unix_tm) INTERVAL (86400) STORE IN (\"&AB36&\") (PARTITION BFR_\" & A21& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AB36&\");\"","v":"PARTITION BY RANGE (tot_bgng_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_T002) (PARTITION BFR_soitcsgmnarngtot_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_T002);"},{"$f":"\"CREATE INDEX PK_\" & A21& \" ON \" & A21 & CONCATENATE(AC22:AE32) & \" LOCAL (PARTITION BFR_\" & A21 & \"_20221101 TABLESPACE \"&AC36&\") TABLESPACE \"&AC36&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & A21 & \" ADD CONSTRAINT PK_\" & A21 & \" PRIMARY KEY \" & CONCATENATE(AC22:AE32) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"IF(LEFT(X35, 13) = \"CONSTRAINT PK\", X35, \"\")","v":{"$error":"#VALUE!"}}]
[{"$nulls":27},"SOIT_D08_T002","SOIT_I08_T002"]
["엣지그룹별 실시간 대기행렬/공간점유율 테이블 - 실시간",{"$nulls":37},{"$f":"IF(LEFT(X37, 13) = \"CONSTRAINT PK\", X37, \"\")","v":""}]
["soitcedgegruprltmqueu",{"$nulls":10},{"$f":"LEN(A38)","v":21},{"$nulls":26},""]
["NO","속성명","컬럼명","PK/FK","NULL","형태",null,"TIBERO","길이","비고",{"$nulls":21},"COMMENT ON TABLE",{"$f":"A38&\" \"","v":"soitcedgegruprltmqueu "},null," IS ",{"$f":"\"'\"&SUBSTITUTE(A37,\"테이블\",\"\")&\"'\"","v":"'엣지그룹별 실시간 대기행렬/공간점유율  - 실시간'"},";",null,""]
[1,"엣지그룹ID","edge_grup_id","PK/FK","NOT NULL","VARCHAR2(300)",null,"VARCHAR2(300)",20,"엣지그룹ID",{"$nulls":11},"CREATE TABLE ",{"$f":"A38&\" (\"","v":"soitcedgegruprltmqueu ("},{"$f":"C40&\" \"","v":"edge_grup_id "},{"$f":"H40&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(E40=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(D40=\"PK\", D40=\"PK/FK\"), C40, \"\")","v":"edge_grup_id"},{"$f":"IF(OR(D40=\"PK\", D40=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$A$38&\".\"","v":"soitcedgegruprltmqueu."},{"$f":"C40","v":"edge_grup_id"}," IS ",{"$f":"\"'\"&J40&\"'\"","v":"'엣지그룹ID'"},";",null,""]
[2,"지역구분코드","rgn_prttn_cd","PK/FK","NOT NULL","CHAR(2)",null,"VARCHAR2(2)",null,"지역분할코드(051)",{"$nulls":13},"rgn_prttn_cd ","VARCHAR2(2) ","NOT NULL",",",null,null,"rgn_prttn_cd",",","COMMENT ON COLUMN ","soitcedgegruprltmqueu.","rgn_prttn_cd"," IS ","'지역분할코드(051)'",";"]
[3,"차로번호","lane_no","PK","NOT NULL","NUMBER(2)",null,"NUMBER(2)",2,"차로번호",{"$nulls":13},"lane_no ","NUMBER(2) ","NOT NULL",",",null,null,"lane_no",",","COMMENT ON COLUMN ","soitcedgegruprltmqueu.","lane_no"," IS ","'차로번호'",";",null,{"$f":"IF(LEFT(X42, 13) = \"CONSTRAINT PK\", X42, \"\")","v":""}]
[4,"실측여부","acsr_yn","PK","NOT NULL","CHAR(1)",null,"VARCHAR2(1)",1,"실측여부 (500) (실시간만 예측있음)",{"$nulls":13},"acsr_yn ","VARCHAR2(1) ","NOT NULL",",",null,null,"acsr_yn",",","COMMENT ON COLUMN ","soitcedgegruprltmqueu.","acsr_yn"," IS ","'실측여부 (500) (실시간만 예측있음)'",";",null,""]
[5,"수집유닉스시각","clct_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"수집유닉스시각",{"$nulls":13},"clct_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"clct_unix_tm",")","COMMENT ON COLUMN ","soitcedgegruprltmqueu.","clct_unix_tm"," IS ","'수집유닉스시각'",";",null,""]
[6,"대기행렬길이","queu_lngt",null,"NULL","NUMBER(19,9)",null,"NUMBER(19,9)","19,9","대기행렬길이 (meter)",{"$nulls":13},"queu_lngt ","NUMBER(19,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruprltmqueu.","queu_lngt"," IS ","'대기행렬길이 (meter)'",";",null,""]
[7,"대기행렬대수","queu_trcn",null,"NULL","NUMBER(5)",null,"NUMBER(5)",5,"대기행렬대수",{"$nulls":13},"queu_trcn ","NUMBER(5) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruprltmqueu.","queu_trcn"," IS ","'대기행렬대수'",";",null,""]
[8,"공간점유율","spae_ocpn_rt",null,"NULL","NUMBER(13,9)",null,"NUMBER(13,9)","12,9","공간점유율 (차량길이/세그먼트길이)",{"$nulls":13},"spae_ocpn_rt ","NUMBER(13,9) ","",{"$f":"\") TABLESPACE \"&AB49&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_T001 NOLOGGING"},{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruprltmqueu.","spae_ocpn_rt"," IS ","'공간점유율 (차량길이/세그먼트길이)'",";",null,""]
[{"$nulls":23},{"$f":"CONCATENATE(AB48:AD48)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (clct_unix_tm) INTERVAL (86400) STORE IN (\"&AB49&\") (PARTITION BFR_\" & A38& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AB49&\");\"","v":"PARTITION BY RANGE (clct_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_T001) (PARTITION BFR_soitcedgegruprltmqueu_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_T001);"},{"$f":"\"CREATE INDEX PK_\" & A38& \" ON \" & A38 & CONCATENATE(AC40:AE45) & \" LOCAL (PARTITION BFR_\" & A38 & \"_20221101 TABLESPACE \"&AC49&\") TABLESPACE \"&AC49&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & A38 & \" ADD CONSTRAINT PK_\" & A38 & \" PRIMARY KEY \" & CONCATENATE(AC40:AE46) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$error":"#VALUE!"}]
[{"$nulls":27},"SOIT_D08_T001","SOIT_I08_T001"]
["엣지그룹 내부차선별 집계 테이블 - 실시간 -> 종료단계 산출물 후 추가",{"$nulls":37},{"$f":"IF(LEFT(X50, 13) = \"CONSTRAINT PK\", X50, \"\")","v":""},null,null,null,"첨두시간별 집계?"]
["soitcedgegruplanerltmtot",{"$nulls":10},{"$f":"LEN(A51)","v":24},{"$nulls":26},""]
["NO","속성명","컬럼명","PK/FK","NULL","형태",null,"TIBERO","길이","비고",{"$nulls":21},"COMMENT ON TABLE",{"$f":"A51&\" \"","v":"soitcedgegruplanerltmtot "},null," IS ",{"$f":"\"'\"&SUBSTITUTE(A50,\"테이블\",\"\")&\"'\"","v":"'엣지그룹 내부차선별 집계  - 실시간 -> 종료단계 산출물 후 추가'"},";",null,""]
[1,"엣지그룹ID","edge_grup_id","PK/FK","NOT NULL","VARCHAR2(300)",null,"VARCHAR2(300)",20,"엣지그룹ID",{"$nulls":11},"CREATE TABLE ",{"$f":"A51&\" (\"","v":"soitcedgegruplanerltmtot ("},{"$f":"C53&\" \"","v":"edge_grup_id "},{"$f":"H53&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(E53=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(D53=\"PK\", D53=\"PK/FK\"), C53, \"\")","v":"edge_grup_id"},{"$f":"IF(OR(D53=\"PK\", D53=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$A$51&\".\"","v":"soitcedgegruplanerltmtot."},{"$f":"C53","v":"edge_grup_id"}," IS ",{"$f":"\"'\"&J53&\"'\"","v":"'엣지그룹ID'"},";",null,""]
[2,"지역구분코드","rgn_prttn_cd","PK/FK","NOT NULL","CHAR(2)",null,"VARCHAR2(2)",null,"지역분할코드(051)",{"$nulls":13},"rgn_prttn_cd ","VARCHAR2(2) ","NOT NULL",",",null,null,"rgn_prttn_cd",",","COMMENT ON COLUMN ","soitcedgegruplanerltmtot.","rgn_prttn_cd"," IS ","'지역분할코드(051)'",";"]
[3,"실측여부","acsr_yn","PK","NOT NULL","CHAR(1)",null,"VARCHAR2(1)",1,"실측여부 (500) (실시간만 예측있음)",{"$nulls":13},"acsr_yn ","VARCHAR2(1) ","NOT NULL",",",null,null,"acsr_yn",",","COMMENT ON COLUMN ","soitcedgegruplanerltmtot.","acsr_yn"," IS ","'실측여부 (500) (실시간만 예측있음)'",";",null,{"$f":"IF(LEFT(X55, 13) = \"CONSTRAINT PK\", X55, \"\")","v":""}]
[4,"차로번호","lane_no","PK","NOT NULL","NUMBER(2)",null,"NUMBER(2)",2,"차로번호",{"$nulls":13},"lane_no ","NUMBER(2) ","NOT NULL",",",null,null,"lane_no",",","COMMENT ON COLUMN ","soitcedgegruplanerltmtot.","lane_no"," IS ","'차로번호'",";",null,""]
[5,"차종코드","kncr_cd","PK","NOT NULL","CHAR(10)",null,"VARCHAR2(10)",3,"차종(008)",{"$nulls":13},"kncr_cd ","VARCHAR2(10) ","NOT NULL",",",null,null,"kncr_cd",",","COMMENT ON COLUMN ","soitcedgegruplanerltmtot.","kncr_cd"," IS ","'차종(008)'",";",null,""]
[6,"집계시작유닉스시각","tot_bgng_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"집계시작유닉스시각",{"$nulls":13},"tot_bgng_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"tot_bgng_unix_tm",",","COMMENT ON COLUMN ","soitcedgegruplanerltmtot.","tot_bgng_unix_tm"," IS ","'집계시작유닉스시각'",";",null,""]
[7,"집계종료유닉스시각","tot_end_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"집계종료유닉스시각",{"$nulls":13},"tot_end_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"tot_end_unix_tm",")","COMMENT ON COLUMN ","soitcedgegruplanerltmtot.","tot_end_unix_tm"," IS ","'집계종료유닉스시각'",";",null,""]
[8,"교통량","trvl",null,"NULL","NUMBER(10)",null,"NUMBER(10)",10,"기간내 내부교통량",{"$nulls":13},"trvl ","NUMBER(10) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruplanerltmtot.","trvl"," IS ","'기간내 내부교통량'",";",null,""]
[9,"구간평균속도","sect_avg_sped",null,"NULL","NUMBER(5,2)",null,"NUMBER(5,2)","5,2","구간평균속도 (기간내 차량당 평균속도)",{"$nulls":13},"sect_avg_sped ","NUMBER(5,2) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruplanerltmtot.","sect_avg_sped"," IS ","'구간평균속도 (기간내 차량당 평균속도)'",";",null,""]
[10,"밀도","trfc_dnst",null,"NULL","NUMBER(7,2)",null,"NUMBER(7,2)",5,"교통밀도(단위:대/m)",{"$nulls":13},"trfc_dnst ","NUMBER(7,2) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruplanerltmtot.","trfc_dnst"," IS ","'교통밀도(단위:대/m)'",";",null,""]
[11,"포화도","strtn_trst_rt",null,"NULL","NUMBER(12,9)",null,"NUMBER(13,9)","12,9","포화도 (교통량/2200)",{"$nulls":13},"strtn_trst_rt ","NUMBER(13,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruplanerltmtot.","strtn_trst_rt"," IS ","'포화도 (교통량/2200)'",";",null,""]
[12,"공간점유율","spae_ocpn_rt",null,"NULL","NUMBER(13,9)",null,"NUMBER(13,9)","12,9","공간점유율 (AVG(차량길이/세그먼트길이))",{"$nulls":13},"spae_ocpn_rt ","NUMBER(13,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruplanerltmtot.","spae_ocpn_rt"," IS ","'공간점유율 (AVG(차량길이/세그먼트길이))'",";",null,""]
[13,"최소대기행렬길이","min_queu_lngt",null,"NULL","NUMBER(19,9)",null,"NUMBER(19,9)","19,9","최소대기행렬길이 (meter)",{"$nulls":13},"min_queu_lngt ","NUMBER(19,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruplanerltmtot.","min_queu_lngt"," IS ","'최소대기행렬길이 (meter)'",";",null,""]
[14,"최대대기행렬길이","max_queu_lngt",null,"NULL","NUMBER(19,9)",null,"NUMBER(19,9)","19,9","최대대기행렬길이 (meter)",{"$nulls":13},"max_queu_lngt ","NUMBER(19,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruplanerltmtot.","max_queu_lngt"," IS ","'최대대기행렬길이 (meter)'",";",null,""]
[15,"구간거리대비 최소대기행렬","min_queu_rt",null,"NULL","NUMBER(19,9)",null,"NUMBER(19,9)","19,9","거리대비 최소대기행렬",{"$nulls":13},"min_queu_rt ","NUMBER(19,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruplanerltmtot.","min_queu_rt"," IS ","'거리대비 최소대기행렬'",";"]
[16,"구간거리대비 최대대기행렬","max_queu_rt",null,"NULL","NUMBER(19,9)",null,"NUMBER(19,9)","19,9","거리대비 최대대기행렬",{"$nulls":13},"max_queu_rt ","NUMBER(19,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruplanerltmtot.","max_queu_rt"," IS ","'거리대비 최대대기행렬'",";"]
[17,"최소대기행렬대수","min_queu_trcn",null,"NULL","NUMBER(5)",null,"NUMBER(5)",5,"최소대기행렬대수",{"$nulls":13},"min_queu_trcn ","NUMBER(5) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruplanerltmtot.","min_queu_trcn"," IS ","'최소대기행렬대수'",";",null,{"$f":"IF(LEFT(X69, 13) = \"CONSTRAINT PK\", X69, \"\")","v":""}]
[18,"최대대기행렬대수","max_queu_trcn",null,"NULL","NUMBER(5)",null,"NUMBER(5)",5,"최대대기행렬대수",{"$nulls":13},"max_queu_trcn ","NUMBER(5) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruplanerltmtot.","max_queu_trcn"," IS ","'최대대기행렬대수'",";",null,""]
[19,"정지율","stop_notm_rt",null,"NULL","NUMBER(7,2)",null,"NUMBER(7,2)","5,2","정지율 (소속세그먼트 평균정지율)",{"$nulls":13},"stop_notm_rt ","NUMBER(7,2) ","",",",{"$nulls":4},"COMMENT ON COLUMN ",{"$f":"$A$100&\".\"","v":"soitcedgegrupioutrltmtot."},"stop_notm_rt"," IS ","'정지율 (소속세그먼트 평균정지율)'",";",null,""]
[20,"지체시간","dely_tm",null,"NULL","NUMBER(7,2)",null,"NUMBER(7,2)","5,2","지체시간 (소속세그먼트 평균지체시간)",{"$nulls":13},"dely_tm ","NUMBER(7,2) ","",{"$f":"\") TABLESPACE \"&AB74&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_T001 NOLOGGING"},{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegrupioutrltmtot.","dely_tm"," IS ","'지체시간 (소속세그먼트 평균지체시간)'",";",null,""]
[{"$nulls":23},{"$f":"CONCATENATE(AB73:AD73)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (tot_bgng_unix_tm) INTERVAL (86400) STORE IN (\"&AB74&\") (PARTITION BFR_\" & A51& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AB74&\");\"","v":"PARTITION BY RANGE (tot_bgng_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_T001) (PARTITION BFR_soitcedgegruplanerltmtot_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_T001);"},{"$f":"\"CREATE INDEX PK_\" & A51& \" ON \" & A51 & CONCATENATE(AC53:AE69) & \" LOCAL (PARTITION BFR_\" & A51 & \"_20221101 TABLESPACE \"&AC74&\") TABLESPACE \"&AC74&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & A51 & \" ADD CONSTRAINT PK_\" & A51 & \" PRIMARY KEY \" & CONCATENATE(AC53:AE70) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$error":"#VALUE!"}]
[{"$nulls":27},"SOIT_D08_T001","SOIT_I08_T001"]
["엣지그룹 내부차선별 집계 테이블 - 배치 -> 종료단계 산출물 후 추가",{"$nulls":37},{"$f":"IF(LEFT(X75, 13) = \"CONSTRAINT PK\", X75, \"\")","v":""},null,null,null,"첨두시간별 집계?"]
["soitcedgegruplanearngtot",{"$nulls":10},{"$f":"LEN(A76)","v":24},{"$nulls":26},""]
["NO","속성명","컬럼명","PK/FK","NULL","형태",null,"TIBERO","길이","비고",{"$nulls":21},"COMMENT ON TABLE",{"$f":"A76&\" \"","v":"soitcedgegruplanearngtot "},null," IS ",{"$f":"\"'\"&SUBSTITUTE(A75,\"테이블\",\"\")&\"'\"","v":"'엣지그룹 내부차선별 집계  - 배치 -> 종료단계 산출물 후 추가'"},";",null,""]
[1,"엣지그룹ID","edge_grup_id","PK/FK","NOT NULL","VARCHAR2(300)",null,"VARCHAR2(300)",20,"엣지그룹ID",{"$nulls":11},"CREATE TABLE ",{"$f":"A76&\" (\"","v":"soitcedgegruplanearngtot ("},{"$f":"C78&\" \"","v":"edge_grup_id "},{"$f":"H78&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(E78=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(D78=\"PK\", D78=\"PK/FK\"), C78, \"\")","v":"edge_grup_id"},{"$f":"IF(OR(D78=\"PK\", D78=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$A$76&\".\"","v":"soitcedgegruplanearngtot."},{"$f":"C78","v":"edge_grup_id"}," IS ",{"$f":"\"'\"&J78&\"'\"","v":"'엣지그룹ID'"},";",null,""]
[2,"집계구분코드","tot_se_cd","PK","NOT NULL","CHAR(1)",null,"VARCHAR2(1)",1,"시간유형(011)","집계구분코드 (1:신호현시, 2:1분단위, 3:5분단위, 4:15분, 5:60분, 6:일별)",{"$nulls":12},"tot_se_cd ","VARCHAR2(1) ","NOT NULL",",",null,null,"tot_se_cd",",","COMMENT ON COLUMN ","soitcedgegruplanearngtot.","tot_se_cd"," IS ","'시간유형(011)'",";",null,""]
[3,"차로번호","lane_no","PK","NOT NULL","NUMBER(2)",null,"NUMBER(2)",2,"차로번호",{"$nulls":13},"lane_no ","NUMBER(2) ","NOT NULL",",",null,null,"lane_no",",","COMMENT ON COLUMN ","soitcedgegruplanearngtot.","lane_no"," IS ","'차로번호'",";",null,""]
[4,"차종코드","kncr_cd","PK","NOT NULL","CHAR(10)",null,"VARCHAR2(10)",3,"차종(008)",{"$nulls":13},"kncr_cd ","VARCHAR2(10) ","NOT NULL",",",null,null,"kncr_cd",",","COMMENT ON COLUMN ","soitcedgegruplanearngtot.","kncr_cd"," IS ","'차종(008)'",";",null,""]
[5,"집계시작유닉스시각","tot_bgng_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"집계시작유닉스시각",{"$nulls":13},"tot_bgng_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"tot_bgng_unix_tm",",","COMMENT ON COLUMN ","soitcedgegruplanearngtot.","tot_bgng_unix_tm"," IS ","'집계시작유닉스시각'",";",null,""]
[6,"집계종료유닉스시각","tot_end_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)"," ","집계종료유닉스시각",{"$nulls":13},"tot_end_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"tot_end_unix_tm",")","COMMENT ON COLUMN ","soitcedgegruplanearngtot.","tot_end_unix_tm"," IS ","'집계종료유닉스시각'",";",null,""]
[7,"교통량","trvl",null,"NULL","NUMBER(10)",null,"NUMBER(10)",10,"기간내 내부교통량",{"$nulls":13},"trvl ","NUMBER(10) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruplanearngtot.","trvl"," IS ","'기간내 내부교통량'",";",null,""]
[8,"구간평균속도","sect_avg_sped",null,"NULL","NUMBER(5,2)",null,"NUMBER(5,2)","5,2","구간평균속도 (기간내 차량당 평균속도)",{"$nulls":13},"sect_avg_sped ","NUMBER(5,2) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruplanearngtot.","sect_avg_sped"," IS ","'구간평균속도 (기간내 차량당 평균속도)'",";",null,""]
[9,"밀도","trfc_dnst",null,"NULL","NUMBER(7,2)",null,"NUMBER(7,2)",5,"교통밀도(단위:대/m)",{"$nulls":13},"trfc_dnst ","NUMBER(7,2) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruplanearngtot.","trfc_dnst"," IS ","'교통밀도(단위:대/m)'",";",null,""]
[10,"포화도","strtn_trst_rt",null,"NULL","NUMBER(12,9)",null,"NUMBER(13,9)","12,9","포화도 (교통량/2200)",{"$nulls":13},"strtn_trst_rt ","NUMBER(13,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruplanearngtot.","strtn_trst_rt"," IS ","'포화도 (교통량/2200)'",";",null,""]
[11,"공간점유율","spae_ocpn_rt",null,"NULL","NUMBER(13,9)",null,"NUMBER(13,9)","12,9","공간점유율 (AVG(차량길이/세그먼트길이))",{"$nulls":13},"spae_ocpn_rt ","NUMBER(13,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruplanearngtot.","spae_ocpn_rt"," IS ","'공간점유율 (AVG(차량길이/세그먼트길이))'",";",null,""]
[12,"최소대기행렬길이","min_queu_lngt",null,"NULL","NUMBER(19,9)",null,"NUMBER(19,9)","19,9","최소대기행렬길이 (meter)",{"$nulls":13},"min_queu_lngt ","NUMBER(19,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruplanearngtot.","min_queu_lngt"," IS ","'최소대기행렬길이 (meter)'",";",null,""]
[13,"최대대기행렬길이","max_queu_lngt",null,"NULL","NUMBER(19,9)",null,"NUMBER(19,9)","19,9","최대대기행렬길이 (meter)",{"$nulls":13},"max_queu_lngt ","NUMBER(19,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruplanearngtot.","max_queu_lngt"," IS ","'최대대기행렬길이 (meter)'",";",null,""]
[14,"구간거리대비 최소대기행렬","min_queu_rt",null,"NULL","NUMBER(19,9)",null,"NUMBER(19,9)","19,9","거리대비 최소대기행렬",{"$nulls":13},"min_queu_rt ","NUMBER(19,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruplanearngtot.","min_queu_rt"," IS ","'거리대비 최소대기행렬'",";"]
[15,"구간거리대비 최대대기행렬","max_queu_rt",null,"NULL","NUMBER(19,9)",null,"NUMBER(19,9)","19,9","거리대비 최대대기행렬",{"$nulls":13},"max_queu_rt ","NUMBER(19,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruplanearngtot.","max_queu_rt"," IS ","'거리대비 최대대기행렬'",";"]
[16,"최소대기행렬대수","min_queu_trcn",null,"NULL","NUMBER(5)",null,"NUMBER(5)",5,"최소대기행렬대수",{"$nulls":13},"min_queu_trcn ","NUMBER(5) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruplanearngtot.","min_queu_trcn"," IS ","'최소대기행렬대수'",";",null,{"$f":"IF(LEFT(X93, 13) = \"CONSTRAINT PK\", X93, \"\")","v":""}]
[17,"최대대기행렬대수","max_queu_trcn",null,"NULL","NUMBER(5)",null,"NUMBER(5)",5,"최대대기행렬대수",{"$nulls":13},"max_queu_trcn ","NUMBER(5) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruplanearngtot.","max_queu_trcn"," IS ","'최대대기행렬대수'",";",null,""]
[18,"정지율","stop_notm_rt",null,"NULL","NUMBER(7,2)",null,"NUMBER(7,2)","5,2","정지율 (소속세그먼트 평균정지율)",{"$nulls":13},"stop_notm_rt ","NUMBER(7,2) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruplanearngtot.","stop_notm_rt"," IS ","'정지율 (소속세그먼트 평균정지율)'",";",null,""]
[19,"지체시간","dely_tm",null,"NULL","NUMBER(7,2)",null,"NUMBER(7,2)","5,2","지체시간 (소속세그먼트 평균지체시간)",{"$nulls":13},"dely_tm ","NUMBER(7,2) ","",{"$f":"\") TABLESPACE \"&AB98&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_T002 NOLOGGING"},{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruplanearngtot.","dely_tm"," IS ","'지체시간 (소속세그먼트 평균지체시간)'",";",null,""]
[{"$nulls":23},{"$f":"CONCATENATE(AB97:AD97)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (tot_bgng_unix_tm) INTERVAL (86400) STORE IN (\"&AB98&\") (PARTITION BFR_\" & A76& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AB98&\");\"","v":"PARTITION BY RANGE (tot_bgng_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_T002) (PARTITION BFR_soitcedgegruplanearngtot_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_T002);"},{"$f":"\"CREATE INDEX PK_\" & A76& \" ON \" & A76 & CONCATENATE(AC78:AE93) & \" LOCAL (PARTITION BFR_\" & A76 & \"_20221101 TABLESPACE \"&AC98&\") TABLESPACE \"&AC98&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & A76 & \" ADD CONSTRAINT PK_\" & A76 & \" PRIMARY KEY \" & CONCATENATE(AC78:AE94) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$error":"#VALUE!"}]
[{"$nulls":27},"SOIT_D08_T002","SOIT_I08_T002"]
["엣지그룹 진입진출 집계 테이블 - 실시간 -> 종료단계 산출물 후 추가",{"$nulls":37},{"$f":"IF(LEFT(X99, 13) = \"CONSTRAINT PK\", X99, \"\")","v":""},null,null,null,"첨두시간별 집계?"]
["soitcedgegrupioutrltmtot",{"$nulls":10},{"$f":"LEN(A100)","v":24},{"$nulls":26},""]
["NO","속성명","컬럼명","PK/FK","NULL","형태",null,"TIBERO","길이","비고",{"$nulls":21},"COMMENT ON TABLE",{"$f":"A100&\" \"","v":"soitcedgegrupioutrltmtot "},null," IS ",{"$f":"\"'\"&SUBSTITUTE(A99,\"테이블\",\"\")&\"'\"","v":"'엣지그룹 진입진출 집계  - 실시간 -> 종료단계 산출물 후 추가'"},";",null,""]
[1,"엣지그룹ID","edge_grup_id","PK/FK","NOT NULL","VARCHAR2(300)",null,"VARCHAR2(300)",20,"엣지그룹ID",{"$nulls":11},"CREATE TABLE ",{"$f":"A100&\" (\"","v":"soitcedgegrupioutrltmtot ("},{"$f":"C102&\" \"","v":"edge_grup_id "},{"$f":"H102&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(E102=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(D102=\"PK\", D102=\"PK/FK\"), C102, \"\")","v":"edge_grup_id"},{"$f":"IF(OR(D102=\"PK\", D102=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$A$100&\".\"","v":"soitcedgegrupioutrltmtot."},{"$f":"C102","v":"edge_grup_id"}," IS ",{"$f":"\"'\"&J102&\"'\"","v":"'엣지그룹ID'"},";",null,""]
[2,"지역구분코드","rgn_prttn_cd","PK/FK","NOT NULL","CHAR(2)",null,"VARCHAR2(2)",null,"지역분할코드(051)",{"$nulls":13},"rgn_prttn_cd ","VARCHAR2(2) ","NOT NULL",",",null,null,"rgn_prttn_cd",",","COMMENT ON COLUMN ","soitcedgegrupioutrltmtot.","rgn_prttn_cd"," IS ","'지역분할코드(051)'",";"]
[3,"실측여부","acsr_yn","PK","NOT NULL","CHAR(1)",null,"VARCHAR2(1)",1,"실측여부 (500) (실시간만 예측있음)",{"$nulls":13},"acsr_yn ","VARCHAR2(1) ","NOT NULL",",",null,null,"acsr_yn",",","COMMENT ON COLUMN ","soitcedgegrupioutrltmtot.","acsr_yn"," IS ","'실측여부 (500) (실시간만 예측있음)'",";",null,{"$f":"IF(LEFT(X104, 13) = \"CONSTRAINT PK\", X104, \"\")","v":""}]
[4,"차로번호","lane_no","PK","NOT NULL","NUMBER(2)",null,"NUMBER(2)",2,"차로번호",{"$nulls":13},"lane_no ","NUMBER(2) ","NOT NULL",",",null,null,"lane_no",",","COMMENT ON COLUMN ","soitcedgegrupioutrltmtot.","lane_no"," IS ","'차로번호'",";",null,""]
[5,"차종코드","kncr_cd","PK","NOT NULL","CHAR(10)",null,"VARCHAR2(10)",3,"차종(008)",{"$nulls":13},"kncr_cd ","VARCHAR2(10) ","NOT NULL",",",null,null,"kncr_cd",",","COMMENT ON COLUMN ","soitcedgegrupioutrltmtot.","kncr_cd"," IS ","'차종(008)'",";",null,""]
[6,"집계시작유닉스시각","tot_bgng_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"집계시작유닉스시각",{"$nulls":13},"tot_bgng_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"tot_bgng_unix_tm",",","COMMENT ON COLUMN ","soitcedgegrupioutrltmtot.","tot_bgng_unix_tm"," IS ","'집계시작유닉스시각'",";",null,""]
[7,"집계종료유닉스시각","tot_end_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"집계종료유닉스시각",{"$nulls":13},"tot_end_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"tot_end_unix_tm",")","COMMENT ON COLUMN ","soitcedgegrupioutrltmtot.","tot_end_unix_tm"," IS ","'집계종료유닉스시각'",";",null,""]
[8,"진입교통량","entr_trvl",null,"NULL","NUMBER(10)",null,"NUMBER(10)",10,"기간내 진입세그먼트 교통량",{"$nulls":13},"entr_trvl ","NUMBER(10) ","",",",null,null,"",{"$f":"IF(OR(D109=\"PK\", D109=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitcedgegrupioutrltmtot.","entr_trvl"," IS ","'기간내 진입세그먼트 교통량'",";",null,""]
[9,"진출교통량","exit_trvl",null,"NULL","NUMBER(10)",null,"NUMBER(10)",10,"기간내 진출세그먼트 교통량",{"$nulls":13},"exit_trvl ","NUMBER(10) ","",",",null,null,"","","COMMENT ON COLUMN ","soitcedgegrupioutrltmtot.","exit_trvl"," IS ","'기간내 진출세그먼트 교통량'",";",null,""]
[10,"시간점유율","hr_ocpn_rt",null,"NULL","NUMBER(13,9)",null,"NUMBER(13,9)","12,9","시간점유율 (SUM(세그먼트길이/기간내 속도))",{"$nulls":9},{"$f":"IF(OR(D111=\"PK\", D111=\"PK/FK\"), C111, \"\")","v":""},{"$f":"IF(OR(D111=\"PK\", D111=\"PK/FK\"), \",\", \"\")","v":""},null,null,"hr_ocpn_rt ","NUMBER(13,9) ","",{"$f":"\") TABLESPACE \"&AB113&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_T001 NOLOGGING"},{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegrupioutrltmtot.","hr_ocpn_rt"," IS ","'시간점유율 (SUM(세그먼트길이/기간내 속도))'",";",null,""]
[{"$nulls":23},{"$f":"CONCATENATE(AB112:AD112)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (tot_bgng_unix_tm) INTERVAL (86400) STORE IN (\"&AB113&\") (PARTITION BFR_\" & A100& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AB113&\");\"","v":"PARTITION BY RANGE (tot_bgng_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_T001) (PARTITION BFR_soitcedgegrupioutrltmtot_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_T001);"},{"$f":"\"CREATE INDEX PK_\" & A100& \" ON \" & A100 & CONCATENATE(AC102:AE108) & \" LOCAL (PARTITION BFR_\" & A93 & \"_20221101 TABLESPACE \"&AC113&\") TABLESPACE \"&AC113&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & A100 & \" ADD CONSTRAINT PK_\" & A100 & \" PRIMARY KEY \" & CONCATENATE(AC102:AE110) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$error":"#VALUE!"}]
[{"$nulls":27},"SOIT_D08_T001","SOIT_I08_T001"]
["엣지그룹 진입진출 집계 테이블 - 배치 -> 종료단계 산출물 후 추가",{"$nulls":37},{"$f":"IF(LEFT(X114, 13) = \"CONSTRAINT PK\", X114, \"\")","v":""},null,null,null,"첨두시간별 집계?"]
["soitcedgegrupioutarngtot",{"$nulls":10},{"$f":"LEN(A115)","v":24},{"$nulls":26},""]
["NO","속성명","컬럼명","PK/FK","NULL","형태",null,"TIBERO","길이","비고",{"$nulls":21},"COMMENT ON TABLE",{"$f":"A115&\" \"","v":"soitcedgegrupioutarngtot "},null," IS ",{"$f":"\"'\"&SUBSTITUTE(A114,\"테이블\",\"\")&\"'\"","v":"'엣지그룹 진입진출 집계  - 배치 -> 종료단계 산출물 후 추가'"},";",null,""]
[1,"엣지그룹ID","edge_grup_id","PK/FK","NOT NULL","VARCHAR2(300)",null,"VARCHAR2(300)",20,"엣지그룹ID",{"$nulls":11},"CREATE TABLE ",{"$f":"A115&\" (\"","v":"soitcedgegrupioutarngtot ("},{"$f":"C117&\" \"","v":"edge_grup_id "},{"$f":"H117&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(E117=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(D117=\"PK\", D117=\"PK/FK\"), C117, \"\")","v":"edge_grup_id"},{"$f":"IF(OR(D117=\"PK\", D117=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$A$115&\".\"","v":"soitcedgegrupioutarngtot."},{"$f":"C117","v":"edge_grup_id"}," IS ",{"$f":"\"'\"&J117&\"'\"","v":"'엣지그룹ID'"},";",null,""]
[2,"집계구분코드","tot_se_cd","PK","NOT NULL","CHAR(1)",null,"VARCHAR2(1)",1,"시간유형(011)","집계구분코드 (1:신호현시, 2:1분단위, 3:5분단위, 4:15분, 5:60분, 6:일별)",{"$nulls":12},"tot_se_cd ","VARCHAR2(1) ","NOT NULL",",",null,null,"tot_se_cd",",","COMMENT ON COLUMN ","soitcedgegrupioutarngtot.","tot_se_cd"," IS ","'시간유형(011)'",";",null,""]
[3,"차로번호","lane_no","PK","NOT NULL","NUMBER(2)",null,"NUMBER(2)",2,"차로번호",{"$nulls":13},"lane_no ","NUMBER(2) ","NOT NULL",",",null,null,"lane_no",",","COMMENT ON COLUMN ","soitcedgegrupioutarngtot.","lane_no"," IS ","'차로번호'",";",null,""]
[4,"차종코드","kncr_cd","PK","NOT NULL","CHAR(10)",null,"VARCHAR2(10)",3,"차종(008)",{"$nulls":13},"kncr_cd ","VARCHAR2(10) ","NOT NULL",",",null,null,"kncr_cd",",","COMMENT ON COLUMN ","soitcedgegrupioutarngtot.","kncr_cd"," IS ","'차종(008)'",";",null,""]
[5,"집계시작유닉스시각","tot_bgng_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"집계시작유닉스시각",{"$nulls":13},"tot_bgng_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"tot_bgng_unix_tm",",","COMMENT ON COLUMN ","soitcedgegrupioutarngtot.","tot_bgng_unix_tm"," IS ","'집계시작유닉스시각'",";",null,""]
[6,"집계종료유닉스시각","tot_end_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"집계종료유닉스시각",{"$nulls":13},"tot_end_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"tot_end_unix_tm",")","COMMENT ON COLUMN ","soitcedgegrupioutarngtot.","tot_end_unix_tm"," IS ","'집계종료유닉스시각'",";",null,""]
[7,"진입교통량","entr_trvl",null,"NULL","NUMBER(10)",null,"NUMBER(10)",10,"기간내 진입세그먼트 교통량",{"$nulls":13},"entr_trvl ","NUMBER(10) ","",",",null,null,"",{"$f":"IF(OR(D123=\"PK\", D123=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitcedgegrupioutarngtot.","entr_trvl"," IS ","'기간내 진입세그먼트 교통량'",";",null,""]
[8,"진출교통량","exit_trvl",null,"NULL","NUMBER(10)",null,"NUMBER(10)",10,"기간내 진출세그먼트 교통량",{"$nulls":13},"exit_trvl ","NUMBER(10) ","",",",null,null,"","","COMMENT ON COLUMN ","soitcedgegrupioutarngtot.","exit_trvl"," IS ","'기간내 진출세그먼트 교통량'",";",null,""]
[9,"시간점유율","hr_ocpn_rt",null,"NULL","NUMBER(13,9)",null,"NUMBER(13,9)","12,9","시간점유율 (SUM(세그먼트길이/기간내 속도))",{"$nulls":9},{"$f":"IF(OR(D125=\"PK\", D125=\"PK/FK\"), C125, \"\")","v":""},{"$f":"IF(OR(D125=\"PK\", D125=\"PK/FK\"), \",\", \"\")","v":""},null,null,"hr_ocpn_rt ","NUMBER(13,9) ","",{"$f":"\") TABLESPACE \"&AB127&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_T002 NOLOGGING"},{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegrupioutarngtot.","hr_ocpn_rt"," IS ","'시간점유율 (SUM(세그먼트길이/기간내 속도))'",";",null,""]
[{"$nulls":23},{"$f":"CONCATENATE(AB126:AD126)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (tot_bgng_unix_tm) INTERVAL (86400) STORE IN (\"&AB127&\") (PARTITION BFR_\" & A115& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AB127&\");\"","v":"PARTITION BY RANGE (tot_bgng_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_T002) (PARTITION BFR_soitcedgegrupioutarngtot_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_T002);"},{"$f":"\"CREATE INDEX PK_\" & A115& \" ON \" & A115 & CONCATENATE(AC117:AE124) & \" LOCAL (PARTITION BFR_\" & A115 & \"_20221101 TABLESPACE \"&AC127&\") TABLESPACE \"&AC127&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & A115 & \" ADD CONSTRAINT PK_\" & A115 & \" PRIMARY KEY \" & CONCATENATE(AC117:AE124) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$error":"#VALUE!"}]
[{"$nulls":27},"SOIT_D08_T002","SOIT_I08_T002"]
["개별차량당 교차로/진입로 통과이력 테이블 - 실시간 (안씀)",{"$nulls":9},"실시간/배치",{"$nulls":27},{"$f":"IF(LEFT(X128, 13) = \"CONSTRAINT PK\", X128, \"\")","v":""}]
["soitcvhclpasintsrltmhstr",{"$nulls":10},{"$f":"LEN(A129)","v":24},{"$nulls":26},""]
["NO","속성명","컬럼명","PK/FK","NULL","형태",null,"TIBERO","길이","비고",{"$nulls":21},"COMMENT ON TABLE",{"$f":"A129&\" \"","v":"soitcvhclpasintsrltmhstr "},null," IS ",{"$f":"\"'\"&SUBSTITUTE(A128,\"테이블\",\"\")&\"'\"","v":"'개별차량당 교차로/진입로 통과이력  - 실시간 (안씀)'"},";",null,""]
[1,"노드ID","node_id","PK/FK","NOT NULL","VARCHAR2(300)",null,"VARCHAR2(300)",20,"진입교차로 노드ID",{"$nulls":11},"CREATE TABLE ",{"$f":"A129&\" (\"","v":"soitcvhclpasintsrltmhstr ("},{"$f":"C131&\" \"","v":"node_id "},{"$f":"H131&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(E131=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(D131=\"PK\", D131=\"PK/FK\"), C131, \"\")","v":"node_id"},{"$f":"IF(OR(D131=\"PK\", D131=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$A$129&\".\"","v":"soitcvhclpasintsrltmhstr."},{"$f":"C131","v":"node_id"}," IS ",{"$f":"\"'\"&J131&\"'\"","v":"'진입교차로 노드ID'"},";",null,""]
[2,"엣지그룹ID","edge_grup_id","PK/FK","NOT NULL","VARCHAR2(300)",null,"VARCHAR2(300)",20,"진입로 엣지그룹ID",{"$nulls":13},"edge_grup_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"edge_grup_id",",","COMMENT ON COLUMN ","soitcvhclpasintsrltmhstr.","edge_grup_id"," IS ","'진입로 엣지그룹ID'",";",null,""]
[3,"지역구분코드","rgn_prttn_cd","PK/FK","NOT NULL","CHAR(2)",null,"VARCHAR2(2)",null,"진입교차로 지역분할코드(051)",{"$nulls":13},"rgn_prttn_cd ","VARCHAR2(2) ","NOT NULL",",",null,null,"rgn_prttn_cd",",","COMMENT ON COLUMN ","soitcvhclpasintsrltmhstr.","rgn_prttn_cd"," IS ","'진입교차로 지역분할코드(051)'",";"]
[4,"차량ID","vhcl_id","PK/FK","NOT NULL","VARCHAR2(150)",null,"VARCHAR2(150)",20,"차량ID",{"$nulls":13},"vhcl_id ","VARCHAR2(150) ","NOT NULL",",",null,null,"vhcl_id",",","COMMENT ON COLUMN ","soitcvhclpasintsrltmhstr.","vhcl_id"," IS ","'차량ID'",";",null,{"$f":"IF(LEFT(X134, 13) = \"CONSTRAINT PK\", X134, \"\")","v":""}]
[5,"실측여부","acsr_yn","PK","NOT NULL","CHAR(1)",null,"VARCHAR2(1)",1,"실측여부 (500) (실시간만 예측있음)",{"$nulls":13},"acsr_yn ","VARCHAR2(1) ","NOT NULL",",",null,null,"acsr_yn",",","COMMENT ON COLUMN ","soitcvhclpasintsrltmhstr.","acsr_yn"," IS ","'실측여부 (500) (실시간만 예측있음)'",";",null,""]
[6,"엣지그룹진입시각","entr_edge_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"엣지그룹진입시각",{"$nulls":13},"entr_edge_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"entr_edge_unix_tm",",","COMMENT ON COLUMN ","soitcvhclpasintsrltmhstr.","entr_edge_unix_tm"," IS ","'엣지그룹진입시각'",";",null,""]
[7,"교차로진입시각","entr_ints_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"교차로진입시각",{"$nulls":13},"entr_ints_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"entr_ints_unix_tm",")","COMMENT ON COLUMN ","soitcvhclpasintsrltmhstr.","entr_ints_unix_tm"," IS ","'교차로진입시각'",";",null,""]
[8,"대기행렬관측유닉스시각","queu_obsrvn_unix_tm",null,"NULL","NUMBER(10)",null,"NUMBER(10)",10,"대기행렬관측유닉스시각",{"$nulls":13},"queu_obsrvn_unix_tm ","NUMBER(10) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcvhclpasintsrltmhstr.","queu_obsrvn_unix_tm"," IS ","'대기행렬관측유닉스시각'",";",null,""]
[9,"최대대기행렬길이","max_queu_lngt",null,"NULL","NUMBER(19,9)",null,"NUMBER(19,9)","19,9","대기행렬길이 (meter)",{"$nulls":13},"max_queu_lngt ","NUMBER(19,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcvhclpasintsrltmhstr.","max_queu_lngt"," IS ","'대기행렬길이 (meter)'",";",null,""]
[10,"회전분류코드","turn_clsf_cd",null,"NULL","CHAR(1)",null,"VARCHAR2(1)",1,"회전(005)","회전정보 (s:직진, r:우회전, l:좌회전, u:유턴)",{"$nulls":12},"turn_clsf_cd ","VARCHAR2(1) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcvhclpasintsrltmhstr.","turn_clsf_cd"," IS ","'회전(005)'",";",null,""]
[11,"차종코드","kncr_cd",null,"NULL","CHAR(10)",null,"VARCHAR2(10)",3,"차종(008)","차종\n( LBUS:대형버스, LTRUCK:대형트럭(4.5T이상), MBUS:미니버스,\nMOTOR:오토바이, MTRUCK:트럭(4.5T미만), PCAR:승용차 )",{"$nulls":12},"kncr_cd ","VARCHAR2(10) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcvhclpasintsrltmhstr.","kncr_cd"," IS ","'차종(008)'",";",null,""]
[12,"진입차로번호","entr_lane_no",null,"NULL","NUMBER(2)",null,"NUMBER(2)",2,"엣지그룹진입차로번호",{"$nulls":13},"entr_lane_no ","NUMBER(2) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcvhclpasintsrltmhstr.","entr_lane_no"," IS ","'엣지그룹진입차로번호'",";",null,""]
[13,"진출차로번호","exit_lane_no",null,"NULL","NUMBER(2)",null,"NUMBER(2)",2,"엣지그룹진출차로번호",{"$nulls":13},"exit_lane_no ","NUMBER(2) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcvhclpasintsrltmhstr.","exit_lane_no"," IS ","'엣지그룹진출차로번호'",";",null,""]
[14,"정지횟수","stop_notm",null,"NULL","NUMBER(5,2)",null,"NUMBER(5,2)","5,2","정지횟수",{"$nulls":13},"stop_notm ","NUMBER(5,2) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcvhclpasintsrltmhstr.","stop_notm"," IS ","'정지횟수'",";",null,""]
[15,"지체시간","dely_tm",null,"NULL","NUMBER(5,2)",null,"NUMBER(5,2)","5,2","지체시간 (SUM(1 - 속도/자유속도))",{"$nulls":13},"dely_tm ","NUMBER(5,2) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcvhclpasintsrltmhstr.","dely_tm"," IS ","'지체시간 (SUM(1 - 속도/자유속도))'",";",null,""]
[16,"구간속도","sect_sped",null,"NULL","NUMBER(5,2)",null,"NUMBER(5,2)","5,2","구간속도 (AVG(속도))",{"$nulls":13},"sect_sped ","NUMBER(5,2) ","",")",{"$nulls":4},"COMMENT ON COLUMN ","soitcvhclpasintsrltmhstr.","sect_sped"," IS ","'구간속도 (AVG(속도))'",";",null,""]
[{"$nulls":23},{"$f":"CONCATENATE(AB147:AD147)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (ENTR_INTS_UNIX_TM) INTERVAL (86400) (PARTITION BFR_\" & A129 & \"_20221101 VALUES LESS THAN (1667228400));\"","v":"PARTITION BY RANGE (ENTR_INTS_UNIX_TM) INTERVAL (86400) (PARTITION BFR_soitcvhclpasintsrltmhstr_20221101 VALUES LESS THAN (1667228400));"},{"$f":"\"CREATE INDEX PK_\" & A129 & \" ON \" & A129 & CONCATENATE(AC131:AE146) & \" LOCAL (PARTITION BFR_\" & A129 & \"_20221101 TABLESPACE SOIT_I08);\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & A129 & \" ADD CONSTRAINT PK_\" & A129 & \" PRIMARY KEY \" & CONCATENATE(AC131:AE146) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$error":"#VALUE!"}]
[]
["개별차량당 교차로/진입로 통과이력 테이블 - 배치 (안씀)",{"$nulls":9},"실시간/배치",{"$nulls":27},{"$f":"IF(LEFT(X149, 13) = \"CONSTRAINT PK\", X149, \"\")","v":""}]
["soitcvhclpasintsarnghstr",{"$nulls":10},{"$f":"LEN(A150)","v":24},{"$nulls":26},""]
["NO","속성명","컬럼명","PK/FK","NULL","형태",null,"TIBERO","길이","비고",{"$nulls":21},"COMMENT ON TABLE",{"$f":"A150&\" \"","v":"soitcvhclpasintsarnghstr "},null," IS ",{"$f":"\"'\"&SUBSTITUTE(A149,\"테이블\",\"\")&\"'\"","v":"'개별차량당 교차로/진입로 통과이력  - 배치 (안씀)'"},";",null,""]
[1,"노드ID","node_id","PK/FK","NOT NULL","VARCHAR2(300)",null,"VARCHAR2(300)",20,"진입교차로 노드ID",{"$nulls":11},"CREATE TABLE ",{"$f":"A150&\" (\"","v":"soitcvhclpasintsarnghstr ("},{"$f":"C152&\" \"","v":"node_id "},{"$f":"H152&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(E152=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(D152=\"PK\", D152=\"PK/FK\"), C152, \"\")","v":"node_id"},{"$f":"IF(OR(D152=\"PK\", D152=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$A$150&\".\"","v":"soitcvhclpasintsarnghstr."},{"$f":"C152","v":"node_id"}," IS ",{"$f":"\"'\"&J152&\"'\"","v":"'진입교차로 노드ID'"},";",null,""]
[2,"엣지그룹ID","edge_grup_id","PK/FK","NOT NULL","VARCHAR2(300)",null,"VARCHAR2(300)",20,"진입로 엣지그룹ID",{"$nulls":13},"edge_grup_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"edge_grup_id",",","COMMENT ON COLUMN ","soitcvhclpasintsarnghstr.","edge_grup_id"," IS ","'진입로 엣지그룹ID'",";",null,""]
[3,"차량ID","vhcl_id","PK/FK","NOT NULL","VARCHAR2(150)",null,"VARCHAR2(150)",20,"차량ID",{"$nulls":13},"vhcl_id ","VARCHAR2(150) ","NOT NULL",",",null,null,"vhcl_id",",","COMMENT ON COLUMN ","soitcvhclpasintsarnghstr.","vhcl_id"," IS ","'차량ID'",";",null,""]
[6,"엣지그룹진입시각","entr_edge_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"엣지그룹진입시각",{"$nulls":13},"entr_edge_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"entr_edge_unix_tm",",","COMMENT ON COLUMN ","soitcvhclpasintsarnghstr.","entr_edge_unix_tm"," IS ","'엣지그룹진입시각'",";",null,""]
[7,"교차로진입시각","entr_ints_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"교차로진입시각",{"$nulls":13},"entr_ints_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"entr_ints_unix_tm",")","COMMENT ON COLUMN ","soitcvhclpasintsarnghstr.","entr_ints_unix_tm"," IS ","'교차로진입시각'",";",null,""]
[8,"대기행렬관측유닉스시각","queu_obsrvn_unix_tm",null,"NULL","NUMBER(10)",null,"NUMBER(10)",10,"대기행렬관측유닉스시각",{"$nulls":13},"queu_obsrvn_unix_tm ","NUMBER(10) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcvhclpasintsarnghstr.","queu_obsrvn_unix_tm"," IS ","'대기행렬관측유닉스시각'",";",null,""]
[9,"회전분류코드","turn_clsf_cd",null,"NULL","CHAR(1)",null,"VARCHAR2(1)",1,"회전(005)","회전정보 (s:직진, r:우회전, l:좌회전, u:유턴)",{"$nulls":12},"turn_clsf_cd ","VARCHAR2(1) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcvhclpasintsarnghstr.","turn_clsf_cd"," IS ","'회전(005)'",";",null,""]
[10,"차종코드","kncr_cd",null,"NULL","CHAR(10)",null,"VARCHAR2(10)",3,"차종(008)","차종\n( LBUS:대형버스, LTRUCK:대형트럭(4.5T이상), MBUS:미니버스,\nMOTOR:오토바이, MTRUCK:트럭(4.5T미만), PCAR:승용차 )",{"$nulls":12},"kncr_cd ","VARCHAR2(10) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcvhclpasintsarnghstr.","kncr_cd"," IS ","'차종(008)'",";",null,""]
[11,"진입차로번호","entr_lane_no",null,"NULL","NUMBER(2)",null,"NUMBER(2)",2,"엣지그룹진입차로번호",{"$nulls":13},"entr_lane_no ","NUMBER(2) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcvhclpasintsarnghstr.","entr_lane_no"," IS ","'엣지그룹진입차로번호'",";",null,""]
[12,"진출차로번호","exit_lane_no",null,"NULL","NUMBER(2)",null,"NUMBER(2)",2,"엣지그룹진출차로번호",{"$nulls":13},"exit_lane_no ","NUMBER(2) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcvhclpasintsarnghstr.","exit_lane_no"," IS ","'엣지그룹진출차로번호'",";",null,""]
[13,"정지횟수","stop_notm",null,"NULL","NUMBER(5,2)",null,"NUMBER(5,2)","5,2","정지횟수",{"$nulls":13},"stop_notm ","NUMBER(5,2) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcvhclpasintsarnghstr.","stop_notm"," IS ","'정지횟수'",";",null,""]
[14,"지체시간","dely_tm",null,"NULL","NUMBER(7,2)",null,"NUMBER(7,2)","5,2","지체시간 (SUM(1 - 속도/자유속도))",{"$nulls":13},"dely_tm ","NUMBER(7,2) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcvhclpasintsarnghstr.","dely_tm"," IS ","'지체시간 (SUM(1 - 속도/자유속도))'",";",null,""]
[15,"구간속도","sect_sped",null,"NULL","NUMBER(5,2)",null,"NUMBER(5,2)","5,2","구간속도 (AVG(속도))",{"$nulls":13},"sect_sped ","NUMBER(5,2) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcvhclpasintsarnghstr.","sect_sped"," IS ","'구간속도 (AVG(속도))'",";",null,""]
[16,"최대대기행렬길이","max_queu_lngt",null,"NULL","NUMBER(19,9)",null,"NUMBER(19,9)","19,9","최대대기행렬길이 (meter)",{"$nulls":13},"max_queu_lngt ","NUMBER(19,9) ","",")",{"$nulls":4},"COMMENT ON COLUMN ","soitcvhclpasintsarnghstr.","max_queu_lngt"," IS ","'최대대기행렬길이 (meter)'",";"]
[{"$nulls":23},{"$f":"CONCATENATE(AB166:AD166)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (ENTR_INTS_UNIX_TM) INTERVAL (86400) (PARTITION BFR_\" & A150 & \"_20221101 VALUES LESS THAN (1667228400));\"","v":"PARTITION BY RANGE (ENTR_INTS_UNIX_TM) INTERVAL (86400) (PARTITION BFR_soitcvhclpasintsarnghstr_20221101 VALUES LESS THAN (1667228400));"},{"$f":"\"CREATE INDEX PK_\" & A150 & \" ON \" & A150 & CONCATENATE(AC152:AE164) & \" LOCAL (PARTITION BFR_\" & A150 & \"_20221101 TABLESPACE SOIT_I08);\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & A150 & \" ADD CONSTRAINT PK_\" & A150 & \" PRIMARY KEY \" & CONCATENATE(AC152:AE164) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$f":"IF(LEFT(X166, 13) = \"CONSTRAINT PK\", X166, \"\")","v":{"$error":"#VALUE!"}}]
[]
["교차로별 집계 테이블 - 실시간",{"$nulls":37},{"$f":"IF(LEFT(X168, 13) = \"CONSTRAINT PK\", X168, \"\")","v":""}]
["soitcintsrltmtot",{"$nulls":10},{"$f":"LEN(A169)","v":16},{"$nulls":26},"",{"$nulls":20},"교통편람 차후 확인",null,null,"교통편람 차후 확인"]
["NO","속성명","컬럼명","PK/FK","NULL","형태",null,"TIBERO","길이","비고",{"$nulls":21},"COMMENT ON TABLE",{"$f":"A169&\" \"","v":"soitcintsrltmtot "},null," IS ",{"$f":"\"'\"&SUBSTITUTE(A168,\"테이블\",\"\")&\"'\"","v":"'교차로별 집계  - 실시간'"},";",null,"",{"$nulls":17},"내부","내부","엣지그룹","엣지그룹","엣지그룹","엣지그룹","엣지그룹","엣지그룹"]
[1,"노드ID","node_id","PK/FK","NOT NULL","VARCHAR2(300)",null,"VARCHAR2(300)",20,"교차로 노드ID",{"$nulls":11},"CREATE TABLE ",{"$f":"A169&\" (\"","v":"soitcintsrltmtot ("},{"$f":"C171&\" \"","v":"node_id "},{"$f":"H171&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(E171=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(D171=\"PK\", D171=\"PK/FK\"), C171, \"\")","v":"node_id"},{"$f":"IF(OR(D171=\"PK\", D171=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$A$169&\".\"","v":"soitcintsrltmtot."},{"$f":"C171","v":"node_id"}," IS ",{"$f":"\"'\"&J171&\"'\"","v":"'교차로 노드ID'"},";",null,"",{"$nulls":5},"교차로ID","진입방향","진입로ID","집계구분","시작시각","종료시각","현시코드","링구분","방향구분","흐름구분","내부연결ID","차종구분","교통량","속도","대기행렬(최대/최소)","공간점유율/밀도","정지횟수","정지율","포화도(V/C)","지체시간"]
[2,"지역구분코드","rgn_prttn_cd","PK/FK","NOT NULL","CHAR(2)",null,"VARCHAR2(2)",null,"진입교차로 지역분할코드(051)",{"$nulls":13},"rgn_prttn_cd ","VARCHAR2(2) ","NOT NULL",",",null,null,"rgn_prttn_cd",",","COMMENT ON COLUMN ","soitcintsrltmtot.","rgn_prttn_cd"," IS ","'진입교차로 지역분할코드(051)'",";"]
[3,"실측여부","acsr_yn","PK","NOT NULL","CHAR(1)",null,"VARCHAR2(1)",1,"실측여부 (500) (실시간만 예측있음)",{"$nulls":13},"acsr_yn ","VARCHAR2(1) ","NOT NULL",",",null,null,"acsr_yn",",","COMMENT ON COLUMN ","soitcintsrltmtot.","acsr_yn"," IS ","'실측여부 (500) (실시간만 예측있음)'",";",null,{"$f":"IF(LEFT(X173, 13) = \"CONSTRAINT PK\", X173, \"\")","v":""},{"$nulls":5},0,"1~16","엣지그룹ID","기간별",20220101000000,20220101123456,"-","-","진입차로별","차로번호","-","1~10","엣지그룹 진출교통량 참조","엣지그룹의 구간속도 참조","조회시 실시간 대기행렬에서 참조, 기간내 최대최소","엣지그룹 공간점유율 참조","기간내 통과차량의 평균정지횟수 참조","기간내 통과차량으로 조회","교통량 컬럼 / 2200","엣지그룹의 지체시간 참조"]
[4,"엣지ID","edge_id","PK/FK","NOT NULL","VARCHAR2(300)",null,"VARCHAR2(300)",20,"진입로 인접 엣지ID/내부 연결엣지ID",{"$nulls":13},"edge_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"edge_id",",","COMMENT ON COLUMN ","soitcintsrltmtot.","edge_id"," IS ","'진입로 인접 엣지ID/내부 연결엣지ID'",";",null,"",{"$nulls":5},0,"1~16","엣지그룹ID","기간별",20220101000000,20220101123456,"-","-","내부회전별","직/좌/우/유","연결엣지ID","1~10","교차로내부 감지교통량 집계","교차로내부 구간속도 집계","-","기간내 통행량/연결엣지길이","기간내 통과차량의 회전별 평균정지횟수 참조","기간내 통과차량으로 조회","교통량 컬럼 / 2200 or 1800","기간내 해당 회전차량의 AVG(지체시간)"]
[5,"집계시작유닉스시각","tot_bgng_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"집계시작유닉스시각",{"$nulls":13},"tot_bgng_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"tot_bgng_unix_tm",",","COMMENT ON COLUMN ","soitcintsrltmtot.","tot_bgng_unix_tm"," IS ","'집계시작유닉스시각'",";",null,"",null,null,"첨두시간별?",null,null,0,"1~16","엣지그룹ID","주기별","현시시작시각","현시종료시각","1~6","A 혹은 B","진입차로별","차로번호","-","1~10","엣지그룹의 진출교통량 집계","엣지그룹의 구간속도 집계","조회시 실시간 대기행렬에서 참조, 기간내 최대최소","엣지그룹 공간점유율 참조","기간내 통과차량의 평균정지횟수 참조","기간내 통과차량으로 조회","교통량 컬럼 / 2200","기간내 해당 회전차량의 AVG(지체시간)"]
[6,"집계종료유닉스시각","tot_end_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"집계종료유닉스시각",{"$nulls":13},"tot_end_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"tot_end_unix_tm",",","COMMENT ON COLUMN ","soitcintsrltmtot.","tot_end_unix_tm"," IS ","'집계종료유닉스시각'",";",null,"",{"$nulls":5},0,"1~16","엣지그룹ID","주기별","현시시작시각","현시종료시각","1~6","A 혹은 B","내부회전별","직/좌/우/유","연결엣지ID","1~10","교차로내부 감지교통량 집계","교차로내부 구간속도 집계","-","기간내 통행량/연결엣지길이","기간내 통과차량의 회전별 평균정지횟수 참조","기간내 통과차량으로 조회","교통량 컬럼 / 2200 or 1800","기간내 해당 회전차량의 AVG(지체시간)"]
[7,"방향구분코드","drct_se_cd","PK","NOT NULL","CHAR(1)",null,"VARCHAR2(1)",1,"집계방향구분(600)","방향구분코드 (1:진입차로별, 2:내부회전별)",{"$nulls":12},"drct_se_cd ","VARCHAR2(1) ","NOT NULL",",",null,null,"drct_se_cd",",","COMMENT ON COLUMN ","soitcintsrltmtot.","drct_se_cd"," IS ","'집계방향구분(600)'",";",null,""]
[8,"흐름구분코드","flow_se_cd","PK","NOT NULL","CHAR(2)",null,"VARCHAR2(2)",1,"진입차로별:진입차로번호, 내부회전별:회전(005)","진입차로별:진입차로번호, 내부회전별:(s:직진, r:우회전, l:좌회전, u:유턴)",{"$nulls":12},"flow_se_cd ","VARCHAR2(2) ","NOT NULL",",",null,null,"flow_se_cd",",","COMMENT ON COLUMN ","soitcintsrltmtot.","flow_se_cd"," IS ","'진입차로별:진입차로번호, 내부회전별:회전(005)'",";",null,""]
[9,"차종코드","kncr_cd","PK","NOT NULL","CHAR(10)",null,"VARCHAR2(10)",3,"차종(008)","차종\n( LBUS:대형버스, LTRUCK:대형트럭(4.5T이상), MBUS:미니버스,\nMOTOR:오토바이, MTRUCK:트럭(4.5T미만), PCAR:승용차 )",{"$nulls":12},"kncr_cd ","VARCHAR2(10) ","NOT NULL",",",null,null,"kncr_cd",")","COMMENT ON COLUMN ","soitcintsrltmtot.","kncr_cd"," IS ","'차종(008)'",";",null,""]
[10,"교통량","trvl",null,"NULL","NUMBER(10)",null,"NUMBER(10)",10,"교통량",{"$nulls":13},"trvl ","NUMBER(10) ","",",",null,null,"",{"$f":"IF(OR(D180=\"PK\", D180=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitcintsrltmtot.","trvl"," IS ","'교통량'",";",null,""]
[11,"속도","sped",null,"NULL","NUMBER(5,2)",null,"NUMBER(5,2)","5,2","속도",{"$nulls":13},"sped ","NUMBER(5,2) ","",",",null,null,"","","COMMENT ON COLUMN ","soitcintsrltmtot.","sped"," IS ","'속도'",";",null,""]
[12,"최소대기행렬길이","min_queu_lngt",null,"NULL","NUMBER(19,9)",null,"NUMBER(19,9)","19,9","최소대기행렬길이 (meter)","진입차로별 집계에서 차선별 합계에만 집계됨",{"$nulls":12},"min_queu_lngt ","NUMBER(19,9) ","",",",null,null,"","","COMMENT ON COLUMN ","soitcintsrltmtot.","min_queu_lngt"," IS ","'최소대기행렬길이 (meter)'",";",null,""]
[13,"최대대기행렬길이","max_queu_lngt",null,"NULL","NUMBER(19,9)",null,"NUMBER(19,9)","19,9","최대대기행렬길이 (meter)","진입차로별 집계에서 차선별 합계에만 집계됨",{"$nulls":12},"max_queu_lngt ","NUMBER(19,9) ","",",",null,null,"","","COMMENT ON COLUMN ","soitcintsrltmtot.","max_queu_lngt"," IS ","'최대대기행렬길이 (meter)'",";",null,""]
[14,"구간거리대비 최소대기행렬","min_queu_rt",null,"NULL","NUMBER(19,9)",null,"NUMBER(19,9)","19,9","거리대비 최소대기행렬",{"$nulls":13},"min_queu_rt ","NUMBER(19,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcintsrltmtot.","min_queu_rt"," IS ","'거리대비 최소대기행렬'",";"]
[15,"구간거리대비 최대대기행렬","max_queu_rt",null,"NULL","NUMBER(19,9)",null,"NUMBER(19,9)","19,9","거리대비 최대대기행렬",{"$nulls":13},"max_queu_rt ","NUMBER(19,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcintsrltmtot.","max_queu_rt"," IS ","'거리대비 최대대기행렬'",";"]
[16,"최소대기행렬대수","min_queu_trcn",null,"NULL","NUMBER(5)",null,"NUMBER(5)",5,"최소대기행렬대수","진입차로별 집계에서 차선별 합계에만 집계됨",{"$nulls":12},"min_queu_trcn ","NUMBER(5) ","",",",null,null,{"$f":"IF(OR(D186=\"PK\", D186=\"PK/FK\"), C186, \"\")","v":""},{"$f":"IF(OR(D186=\"PK\", D186=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitcintsrltmtot.","min_queu_trcn"," IS ","'최소대기행렬대수'",";",null,{"$f":"IF(LEFT(X186, 13) = \"CONSTRAINT PK\", X186, \"\")","v":""}]
[17,"최대대기행렬대수","max_queu_trcn",null,"NULL","NUMBER(5)",null,"NUMBER(5)",5,"최대대기행렬대수","진입차로별 집계에서 차선별 합계에만 집계됨",{"$nulls":12},"max_queu_trcn ","NUMBER(5) ","",",",null,null,"","","COMMENT ON COLUMN ","soitcintsrltmtot.","max_queu_trcn"," IS ","'최대대기행렬대수'",";",null,""]
[18,"공간점유율","spae_ocpn_rt",null,"NULL","NUMBER(13,9)",null,"NUMBER(13,9)","12,9","공간점유율","엣지별 합계에만 집계됨",{"$nulls":12},"spae_ocpn_rt ","NUMBER(13,9) ","",",",null,null,"","","COMMENT ON COLUMN ","soitcintsrltmtot.","spae_ocpn_rt"," IS ","'공간점유율'",";",null,""]
[19,"시간점유율","hr_ocpn_rt",null,"NULL","NUMBER(13,9)",null,"NUMBER(13,9)","12,9","시간점유율 (SUM(세그먼트길이/기간내 속도))","엣지별 합계에만 집계됨",{"$nulls":12},"hr_ocpn_rt ","NUMBER(13,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcintsrltmtot.","hr_ocpn_rt"," IS ","'시간점유율 (SUM(세그먼트길이/기간내 속도))'",";",null,""]
[20,"밀도","trfc_dnst",null,"NULL","NUMBER(7,2)",null,"NUMBER(7,2)",5,"교통밀도(단위:대/m)",{"$nulls":13},"trfc_dnst ","NUMBER(7,2) ","",",",null,null,{"$f":"IF(OR(D190=\"PK\", D190=\"PK/FK\"), C190, \"\")","v":""},{"$f":"IF(OR(D190=\"PK\", D190=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitcintsrltmtot.","trfc_dnst"," IS ","'교통밀도(단위:대/m)'",";",null,""]
[21,"정지율","stop_notm_rt",null,"NULL","NUMBER(7,2)",null,"NUMBER(7,2)","5,2","정지율 (진입차로별 평균 정지율)",{"$nulls":13},"stop_notm_rt ","NUMBER(7,2) ","",",",null,null,"","","COMMENT ON COLUMN ","soitcintsrltmtot.","stop_notm_rt"," IS ","'정지율 (진입차로별 평균 정지율)'",";",null,""]
[22,"포화도","strtn_trst_rt",null,"NULL","NUMBER(12,9)",null,"NUMBER(13,9)","12,9","포화도",{"$nulls":13},"strtn_trst_rt ","NUMBER(13,9) ","",",",null,null,"","","COMMENT ON COLUMN ","soitcintsrltmtot.","strtn_trst_rt"," IS ","'포화도'",";",null,""]
[23,"지체시간","dely_tm",null,"NULL","NUMBER(7,2)",null,"NUMBER(7,2)","5,2","지체시간 (진입차로별 평균지체시간)",{"$nulls":13},"dely_tm ","NUMBER(7,2) ","",{"$f":"\") TABLESPACE \"&AB195&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_T001 NOLOGGING"},{"$nulls":4},"COMMENT ON COLUMN ","soitcintsrltmtot.","dely_tm"," IS ","'지체시간 (진입차로별 평균지체시간)'",";",null,""]
[{"$nulls":23},{"$f":"CONCATENATE(AB194:AD194)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (tot_bgng_unix_tm) INTERVAL (86400) STORE IN (\"&AB195&\") (PARTITION BFR_\" & A169& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AB195&\");\"","v":"PARTITION BY RANGE (tot_bgng_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_T001) (PARTITION BFR_soitcintsrltmtot_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_T001);"},{"$f":"\"CREATE INDEX PK_\" & A169& \" ON \" & A169 & CONCATENATE(AC171:AE182) & \" LOCAL (PARTITION BFR_\" & A169 & \"_20221101 TABLESPACE \"&AC195&\") TABLESPACE \"&AC195&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & A169 & \" ADD CONSTRAINT PK_\" & A169 & \" PRIMARY KEY \" & CONCATENATE(AC171:AE187) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$error":"#VALUE!"}]
[{"$nulls":27},"SOIT_D08_T001","SOIT_I08_T001"]
["교차로별 집계 테이블 - 배치",{"$nulls":37},{"$f":"IF(LEFT(X196, 13) = \"CONSTRAINT PK\", X196, \"\")","v":""}]
["soitcintsarngtot",{"$nulls":10},{"$f":"LEN(A197)","v":16}]
["NO","속성명","컬럼명","PK/FK","NULL","형태",null,"TIBERO","길이","비고",{"$nulls":21},"COMMENT ON TABLE",{"$f":"A197&\" \"","v":"soitcintsarngtot "},null," IS ",{"$f":"\"'\"&SUBSTITUTE(A196,\"테이블\",\"\")&\"'\"","v":"'교차로별 집계  - 배치'"},";",null,{"$f":"IF(LEFT(X198, 13) = \"CONSTRAINT PK\", X198, \"\")","v":""}]
[1,"노드ID","node_id","PK/FK","NOT NULL","VARCHAR2(300)",null,"VARCHAR2(300)",20,"교차로 노드ID",{"$nulls":11},"CREATE TABLE ",{"$f":"A197&\" (\"","v":"soitcintsarngtot ("},{"$f":"C199&\" \"","v":"node_id "},{"$f":"H199&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(E199=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(D199=\"PK\", D199=\"PK/FK\"), C199, \"\")","v":"node_id"},{"$f":"IF(OR(D199=\"PK\", D199=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$A$197&\".\"","v":"soitcintsarngtot."},{"$f":"C199","v":"node_id"}," IS ",{"$f":"\"'\"&J199&\"'\"","v":"'교차로 노드ID'"},";",null,"",{"$nulls":5},"교차로ID","진입방향","진입로ID","집계구분","시작시각","종료시각","현시코드","링구분","방향구분","흐름구분","내부연결ID","차종구분","교통량","속도","대기행렬(최대/최소)","공간점유율/밀도","정지횟수","정지율","포화도(V/C)","지체시간"]
[2,"집계구분코드","tot_se_cd","PK","NOT NULL","CHAR(1)",null,"VARCHAR2(1)",1,"시간유형(011)","집계구분코드 (1:신호현시, 2:1분단위, 3:5분단위, 4:15분, 5:60분, 6:일별)",{"$nulls":12},"tot_se_cd ","VARCHAR2(1) ","NOT NULL",",",null,null,"tot_se_cd",",","COMMENT ON COLUMN ","soitcintsarngtot.","tot_se_cd"," IS ","'시간유형(011)'",";",null,"",{"$nulls":5},0,"1~16","엣지그룹ID","기간별",20220101000000,20220101123456,"-","-","진입차로별","차로번호","-","1~10","엣지그룹 진출교통량 참조","엣지그룹의 구간속도 참조","조회시 실시간 대기행렬에서 참조, 기간내 최대최소","엣지그룹 공간점유율 참조","기간내 통과차량의 평균정지횟수 참조","기간내 통과차량으로 조회","교통량 컬럼 / 2200","엣지그룹의 지체시간 참조"]
[3,"엣지ID","edge_id","PK/FK","NOT NULL","VARCHAR2(300)",null,"VARCHAR2(300)",20,"진입로 인접 엣지ID/내부 연결엣지ID",{"$nulls":13},"edge_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"edge_id",",","COMMENT ON COLUMN ","soitcintsarngtot.","edge_id"," IS ","'진입로 인접 엣지ID/내부 연결엣지ID'",";",null,"",{"$nulls":5},0,"1~16","엣지그룹ID","기간별",20220101000000,20220101123456,"-","-","내부회전별","직/좌/우/유","연결엣지ID","1~10","교차로내부 감지교통량 집계","교차로내부 구간속도 집계","조회시 실시간 대기행렬에서 참조, 기간내 최대최소","기간내 통행량/연결엣지길이","기간내 통과차량의 회전별 평균정지횟수 참조","기간내 통과차량으로 조회","교통량 컬럼 / 2200 or 1800","기간내 해당 회전차량의 AVG(지체시간)"]
[4,"집계시작유닉스시각","tot_bgng_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"집계시작유닉스시각",{"$nulls":13},"tot_bgng_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"tot_bgng_unix_tm",",","COMMENT ON COLUMN ","soitcintsarngtot.","tot_bgng_unix_tm"," IS ","'집계시작유닉스시각'",";",null,"",null,null,"첨두시간별?",null,null,0,"1~16","엣지그룹ID","주기별","현시시작시각","현시종료시각","1~6","A 혹은 B","진입차로별","차로번호","-","1~10","엣지그룹의 진출교통량 집계","엣지그룹의 구간속도 집계","조회시 실시간 대기행렬에서 참조, 기간내 최대최소","기간내 통행량/엣지그룹길이","기간내 통과차량의 평균정지횟수 참조","기간내 통과차량으로 조회","교통량 컬럼 / 2200","기간내 해당 회전차량의 AVG(지체시간)"]
[5,"집계종료유닉스시각","tot_end_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"집계종료유닉스시각",{"$nulls":13},"tot_end_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"tot_end_unix_tm",",","COMMENT ON COLUMN ","soitcintsarngtot.","tot_end_unix_tm"," IS ","'집계종료유닉스시각'",";",null,"",{"$nulls":5},0,"1~16","엣지그룹ID","주기별","현시시작시각","현시종료시각","1~6","A 혹은 B","내부회전별","직/좌/우/유","연결엣지ID","1~10","교차로내부 감지교통량 집계","교차로내부 구간속도 집계","조회시 실시간 대기행렬에서 참조, 기간내 최대최소","기간내 통행량/연결엣지길이","기간내 통과차량의 회전별 평균정지횟수 참조","기간내 통과차량으로 조회","교통량 컬럼 / 2200 or 1800","기간내 해당 회전차량의 AVG(지체시간)"]
[6,"방향구분코드","drct_se_cd","PK","NOT NULL","CHAR(1)",null,"VARCHAR2(1)",1,"집계방향구분(600)","방향구분코드 (1:진입차로별, 2:내부회전별)",{"$nulls":12},"drct_se_cd ","VARCHAR2(1) ","NOT NULL",",",null,null,"drct_se_cd",",","COMMENT ON COLUMN ","soitcintsarngtot.","drct_se_cd"," IS ","'집계방향구분(600)'",";",null,""]
[7,"흐름구분코드","flow_se_cd","PK","NOT NULL","CHAR(2)",null,"VARCHAR2(2)",1,"진입차로별:진입차로번호, 내부회전별:회전(005)","진입차로별:진입차로번호, 내부회전별:(s:직진, r:우회전, l:좌회전, u:유턴)",{"$nulls":12},"flow_se_cd ","VARCHAR2(2) ","NOT NULL",",",null,null,"flow_se_cd",",","COMMENT ON COLUMN ","soitcintsarngtot.","flow_se_cd"," IS ","'진입차로별:진입차로번호, 내부회전별:회전(005)'",";",null,""]
[8,"차종코드","kncr_cd","PK","NOT NULL","CHAR(10)",null,"VARCHAR2(10)",3,"차종(008)","차종",{"$nulls":12},"kncr_cd ","VARCHAR2(10) ","NOT NULL",",",null,null,"kncr_cd",")","COMMENT ON COLUMN ","soitcintsarngtot.","kncr_cd"," IS ","'차종(008)'",";",null,""]
[9,"교통량","trvl",null,"NULL","NUMBER(10)",null,"NUMBER(10)",10,"교통량",{"$nulls":13},"trvl ","NUMBER(10) ","",",",null,null,"",{"$f":"IF(OR(D207=\"PK\", D207=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitcintsarngtot.","trvl"," IS ","'교통량'",";",null,""]
[10,"속도","sped",null,"NULL","NUMBER(5,2)",null,"NUMBER(5,2)","5,2","속도",{"$nulls":13},"sped ","NUMBER(5,2) ","",",",null,null,"","","COMMENT ON COLUMN ","soitcintsarngtot.","sped"," IS ","'속도'",";",null,""]
[11,"최소대기행렬길이","min_queu_lngt",null,"NULL","NUMBER(19,9)",null,"NUMBER(19,9)","19,9","최소대기행렬길이 (meter)","진입차로별 집계에서 차선별 합계에만 집계됨",{"$nulls":12},"min_queu_lngt ","NUMBER(19,9) ","",",",null,null,"","","COMMENT ON COLUMN ","soitcintsarngtot.","min_queu_lngt"," IS ","'최소대기행렬길이 (meter)'",";",null,""]
[12,"최대대기행렬길이","max_queu_lngt",null,"NULL","NUMBER(19,9)",null,"NUMBER(19,9)","19,9","최대대기행렬길이 (meter)","진입차로별 집계에서 차선별 합계에만 집계됨",{"$nulls":12},"max_queu_lngt ","NUMBER(19,9) ","",",",null,null,"","","COMMENT ON COLUMN ","soitcintsarngtot.","max_queu_lngt"," IS ","'최대대기행렬길이 (meter)'",";",null,""]
[13,"구간거리대비 최소대기행렬","min_queu_rt",null,"NULL","NUMBER(19,9)",null,"NUMBER(19,9)","19,9","거리대비 최소대기행렬",{"$nulls":13},"min_queu_rt ","NUMBER(19,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcintsarngtot.","min_queu_rt"," IS ","'거리대비 최소대기행렬'",";"]
[14,"구간거리대비 최대대기행렬","max_queu_rt",null,"NULL","NUMBER(19,9)",null,"NUMBER(19,9)","19,9","거리대비 최대대기행렬",{"$nulls":13},"max_queu_rt ","NUMBER(19,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcintsarngtot.","max_queu_rt"," IS ","'거리대비 최대대기행렬'",";"]
[15,"최소대기행렬대수","min_queu_trcn",null,"NULL","NUMBER(5)",null,"NUMBER(5)",5,"최소대기행렬대수","진입차로별 집계에서 차선별 합계에만 집계됨",{"$nulls":12},"min_queu_trcn ","NUMBER(5) ","",",",null,null,{"$f":"IF(OR(D213=\"PK\", D213=\"PK/FK\"), C213, \"\")","v":""},{"$f":"IF(OR(D213=\"PK\", D213=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitcintsarngtot.","min_queu_trcn"," IS ","'최소대기행렬대수'",";",null,{"$f":"IF(LEFT(X213, 13) = \"CONSTRAINT PK\", X213, \"\")","v":""}]
[16,"최대대기행렬대수","max_queu_trcn",null,"NULL","NUMBER(5)",null,"NUMBER(5)",5,"최대대기행렬대수","진입차로별 집계에서 차선별 합계에만 집계됨",{"$nulls":12},"max_queu_trcn ","NUMBER(5) ","",",",null,null,"","","COMMENT ON COLUMN ","soitcintsarngtot.","max_queu_trcn"," IS ","'최대대기행렬대수'",";",null,""]
[17,"공간점유율","spae_ocpn_rt",null,"NULL","NUMBER(13,9)",null,"NUMBER(13,9)","12,9","공간점유율","엣지별 합계에만 집계됨",{"$nulls":12},"spae_ocpn_rt ","NUMBER(13,9) ","",",",null,null,"","","COMMENT ON COLUMN ","soitcintsarngtot.","spae_ocpn_rt"," IS ","'공간점유율'",";",null,""]
[18,"시간점유율","hr_ocpn_rt",null,"NULL","NUMBER(13,9)",null,"NUMBER(13,9)","12,9","시간점유율 (SUM(세그먼트길이/기간내 속도))",{"$nulls":13},"hr_ocpn_rt ","NUMBER(13,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcintsarngtot.","hr_ocpn_rt"," IS ","'시간점유율 (SUM(세그먼트길이/기간내 속도))'",";"]
[19,"밀도","trfc_dnst",null,"NULL","NUMBER(7,2)",null,"NUMBER(7,2)",5,"교통밀도(단위:대/m)",{"$nulls":13},"trfc_dnst ","NUMBER(7,2) ","",",",null,null,{"$f":"IF(OR(D217=\"PK\", D217=\"PK/FK\"), C217, \"\")","v":""},{"$f":"IF(OR(D217=\"PK\", D217=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitcintsarngtot.","trfc_dnst"," IS ","'교통밀도(단위:대/m)'",";",null,{"$f":"IF(LEFT(X217, 13) = \"CONSTRAINT PK\", X217, \"\")","v":""}]
[20,"정지율","stop_notm_rt",null,"NULL","NUMBER(7,2)",null,"NUMBER(7,2)","5,2","정지율 (진입차로별 평균 정지율)",{"$nulls":13},"stop_notm_rt ","NUMBER(7,2) ","",",",null,null,"","","COMMENT ON COLUMN ","soitcintsarngtot.","stop_notm_rt"," IS ","'정지율 (진입차로별 평균 정지율)'",";",null,""]
[21,"포화도","strtn_trst_rt",null,"NULL","NUMBER(13,9)",null,"NUMBER(13,9)","12,9","포화도",{"$nulls":13},"strtn_trst_rt ","NUMBER(13,9) ","",",",null,null,"","","COMMENT ON COLUMN ","soitcintsarngtot.","strtn_trst_rt"," IS ","'포화도'",";",null,""]
[22,"지체시간","dely_tm",null,"NULL","NUMBER(7,2)",null,"NUMBER(7,2)","5,2","지체시간 (진입차로별 평균지체시간)",{"$nulls":13},"dely_tm ","NUMBER(7,2) ","",{"$f":"\") TABLESPACE \"&AB222&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_T002 NOLOGGING"},{"$nulls":4},"COMMENT ON COLUMN ","soitcintsarngtot.","dely_tm"," IS ","'지체시간 (진입차로별 평균지체시간)'",";",null,""]
[{"$nulls":23},{"$f":"CONCATENATE(AB221:AD221)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (tot_bgng_unix_tm) INTERVAL (86400) STORE IN (\"&AB222&\") (PARTITION BFR_\" & A197& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AB222&\");\"","v":"PARTITION BY RANGE (tot_bgng_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_T002) (PARTITION BFR_soitcintsarngtot_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_T002);"},{"$f":"\"CREATE INDEX PK_\" & A197& \" ON \" & A197 & CONCATENATE(AC199:AE213) & \" LOCAL (PARTITION BFR_\" & A197 & \"_20221101 TABLESPACE \"&AC222&\") TABLESPACE \"&AC222&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & A197 & \" ADD CONSTRAINT PK_\" & A197 & \" PRIMARY KEY \" & CONCATENATE(AC199:AE215) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$error":"#VALUE!"}]
[{"$nulls":27},"SOIT_D08_T002","SOIT_I08_T002"]
["도로구간별 집계 테이블",{"$nulls":9},"배치",{"$nulls":27},{"$f":"IF(LEFT(X223, 13) = \"CONSTRAINT PK\", X223, \"\")","v":""}]
["soitclinkroadtot",{"$nulls":37},""]
["NO","속성명","컬럼명","PK/FK","NULL","형태",null,"TIBERO","길이","비고",{"$nulls":21},"COMMENT ON TABLE",{"$f":"A224&\" \"","v":"soitclinkroadtot "},null," IS ",{"$f":"\"'\"&SUBSTITUTE(A223,\"테이블\",\"\")&\"'\"","v":"'도로구간별 집계 '"},";",null,""]
[1,"대상구분코드","trgt_se_cd","PK","NOT NULL","CHAR(1)",null,"VARCHAR2(1)",1,"대상구분코드 (1:링크, 2:도로)","공간구분코드(601)",{"$nulls":10},"CREATE TABLE ",{"$f":"A224&\" (\"","v":"soitclinkroadtot ("},{"$f":"C226&\" \"","v":"trgt_se_cd "},{"$f":"H226&\" \"","v":"VARCHAR2(1) "},{"$f":"IF(E226=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(D226=\"PK\", D226=\"PK/FK\"), C226, \"\")","v":"trgt_se_cd"},{"$f":"IF(OR(D226=\"PK\", D226=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$A$224&\".\"","v":"soitclinkroadtot."},{"$f":"C226","v":"trgt_se_cd"}," IS ",{"$f":"\"'\"&J226&\"'\"","v":"'대상구분코드 (1:링크, 2:도로)'"},";",null,""]
[2,"대상ID","trgt_id","PK/FK","NOT NULL","VARCHAR2(300)",null,"VARCHAR2(300)",20,"대상ID (링크ID/도로명)",{"$nulls":13},"trgt_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"trgt_id",",","COMMENT ON COLUMN ","soitclinkroadtot.","trgt_id"," IS ","'대상ID (링크ID/도로명)'",";",null,""]
[3,"방향구분코드","drct_se_cd","PK","NOT NULL","CHAR(1)",null,"VARCHAR2(1)",1,"방향(004)","상/하 혹은 좌/우 기준으로 1/2",{"$nulls":12},"drct_se_cd ","VARCHAR2(1) ","NOT NULL",",",null,null,"drct_se_cd",",","COMMENT ON COLUMN ","soitclinkroadtot.","drct_se_cd"," IS ","'방향(004)'",";",null,""]
[4,"집계구분","tot_se_cd","PK","NOT NULL","CHAR(1)",null,"VARCHAR2(1)",1,"시간유형(011)","집계구분코드 (1:신호현시, 2:1분단위, 3:5분단위, 4:15분, 5:60분, 6:일별)",{"$nulls":12},"tot_se_cd ","VARCHAR2(1) ","NOT NULL",",",null,null,"tot_se_cd",",","COMMENT ON COLUMN ","soitclinkroadtot.","tot_se_cd"," IS ","'시간유형(011)'",";",null,""]
[5,"집계시작유닉스시각","tot_bgng_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"집계시작유닉스시각",{"$nulls":13},"tot_bgng_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"tot_bgng_unix_tm",",","COMMENT ON COLUMN ","soitclinkroadtot.","tot_bgng_unix_tm"," IS ","'집계시작유닉스시각'",";",null,""]
[6,"집계종료유닉스시각","tot_end_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"집계종료유닉스시각",{"$nulls":13},"tot_end_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"tot_end_unix_tm",",","COMMENT ON COLUMN ","soitclinkroadtot.","tot_end_unix_tm"," IS ","'집계종료유닉스시각'",";",null,""]
[7,"차로별","lane_no","PK","NOT NULL","NUMBER(2)",null,"NUMBER(2)",2,"차로별",{"$nulls":13},"lane_no ","NUMBER(2) ","NOT NULL",",",null,null,"lane_no",",","COMMENT ON COLUMN ","soitclinkroadtot.","lane_no"," IS ","'차로별'",";",null,""]
[8,"차종코드","kncr_cd","PK","NOT NULL","CHAR(10)",null,"VARCHAR2(10)",3,"차종(008)",{"$nulls":13},"kncr_cd ","VARCHAR2(10) ","NOT NULL",",",null,null,"kncr_cd",")","COMMENT ON COLUMN ","soitclinkroadtot.","kncr_cd"," IS ","'차종(008)'",";",null,""]
[9,"속도","sped",null,"NULL","NUMBER(5,2)",null,"NUMBER(5,2)","5,2","구간평균속도 (기간내 차량당 평균속도)",{"$nulls":13},"sped ","NUMBER(5,2) ","",",",null,null,"",{"$f":"IF(OR(D234=\"PK\", D234=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitclinkroadtot.","sped"," IS ","'구간평균속도 (기간내 차량당 평균속도)'",";",null,""]
[10,"교통량","trvl",null,"NULL","NUMBER(10)",null,"NUMBER(10)",10,"기간내 내부교통량",{"$nulls":13},"trvl ","NUMBER(10) ","",",",null,null,"","","COMMENT ON COLUMN ","soitclinkroadtot.","trvl"," IS ","'기간내 내부교통량'",";",null,""]
[11,"밀도","trfc_dnst",null,"NULL","NUMBER(7,2)",null,"NUMBER(7,2)",5,null,"교통밀도(단위:대/m)","확인후 제외될 수 있음",{"$nulls":11},"trfc_dnst ","NUMBER(7,2) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitclinkroadtot.","trfc_dnst"," IS ",{"$f":"\"'\"&K236&\"'\"","v":"'교통밀도(단위:대/m)'"},";",null,""]
[12,"포화도","strtn_trst_rt",null,"NULL","NUMBER(13,9)",null,"NUMBER(13,9)","12,9",null,"포화도",{"$nulls":12},"strtn_trst_rt ","NUMBER(13,9) ",null,{"$f":"\") TABLESPACE \"&AB239&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_T002 NOLOGGING"},{"$nulls":4},"COMMENT ON COLUMN ","soitclinkroadtot.","strtn_trst_rt"," IS ","'포화도'",";",null,""]
[{"$nulls":23},{"$f":"CONCATENATE(AB238:AD238)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (tot_bgng_unix_tm) INTERVAL (86400) STORE IN (\"&AB239&\") (PARTITION BFR_\" & A225& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AB239&\");\"","v":"PARTITION BY RANGE (tot_bgng_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_T002) (PARTITION BFR_NO_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_T002);"},{"$f":"\"CREATE INDEX PK_\" & A225& \" ON \" & A225 & CONCATENATE(AC227:AE235) & \" LOCAL (PARTITION BFR_\" & A225 & \"_20221101 TABLESPACE \"&AC239&\") TABLESPACE \"&AC239&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & A225 & \" ADD CONSTRAINT PK_\" & A225 & \" PRIMARY KEY \" & CONCATENATE(AC227:AE236) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$error":"#VALUE!"}]
[{"$nulls":27},"SOIT_D08_T002","SOIT_I08_T002"]
["구역별 대표 집계 테이블",{"$nulls":9},"실시간",{"$nulls":27},{"$f":"IF(LEFT(X240, 13) = \"CONSTRAINT PK\", X240, \"\")","v":""}]
["soitcrgntot",{"$nulls":37},""]
["NO","속성명","컬럼명","PK/FK","NULL","형태",null,"TIBERO","길이","비고",{"$nulls":21},"COMMENT ON TABLE",{"$f":"A241&\" \"","v":"soitcrgntot "},null," IS ",{"$f":"\"'\"&SUBSTITUTE(A240,\"테이블\",\"\")&\"'\"","v":"'구역별 대표 집계 '"},";",null,""]
[1,"지역구분코드","rgn_prttn_cd","PK","NOT NULL","CHAR(2)",null,"VARCHAR2(2)",2,"지역분할코드 (051)","0 : 메타버스 POC,1 : 계양구,2 : 남동구_상단,3 : 남동구_하단,4 : 미추홀구,5 : 부평구_상단,6 : 부평구_하단,7 : 서구+동구,8 : 연수구,9 : 중구, 동구:20, 서구:80, 남동구:50, 부평구:60",{"$nulls":10},"CREATE TABLE ",{"$f":"A241&\" (\"","v":"soitcrgntot ("},{"$f":"C243&\" \"","v":"rgn_prttn_cd "},{"$f":"H243&\" \"","v":"VARCHAR2(2) "},{"$f":"IF(E243=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(D243=\"PK\", D243=\"PK/FK\"), C243, \"\")","v":"rgn_prttn_cd"},{"$f":"IF(OR(D243=\"PK\", D243=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$A$241&\".\"","v":"soitcrgntot."},{"$f":"C243","v":"rgn_prttn_cd"}," IS ",{"$f":"\"'\"&J243&\"'\"","v":"'지역분할코드 (051)'"},";",null,""]
[2,"실측여부","acsr_yn","PK","NOT NULL","CHAR(1)",null,"VARCHAR2(1)",1,"실측여부 (500) (실시간만 예측있음)",{"$nulls":13},"acsr_yn ","VARCHAR2(1) ","NOT NULL",",",null,null,"acsr_yn",",","COMMENT ON COLUMN ","soitcrgntot.","acsr_yn"," IS ","'실측여부 (500) (실시간만 예측있음)'",";",null,""]
[3,"집계구분","tot_se_cd","PK","NOT NULL","CHAR(1)",null,"VARCHAR2(1)",1,"시간유형(011)","3:5분단위, 7:일누적",{"$nulls":12},"tot_se_cd ","VARCHAR2(1) ","NOT NULL",",",null,null,"tot_se_cd",",","COMMENT ON COLUMN ","soitcrgntot.","tot_se_cd"," IS ","'시간유형(011)'",";",null,""]
[4,"집계시작유닉스시각","tot_bgng_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"집계시작유닉스시각",{"$nulls":13},"tot_bgng_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"tot_bgng_unix_tm",",","COMMENT ON COLUMN ","soitcrgntot.","tot_bgng_unix_tm"," IS ","'집계시작유닉스시각'",";",null,""]
[5,"집계종료유닉스시각","tot_end_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"집계종료유닉스시각",{"$nulls":13},"tot_end_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"tot_end_unix_tm",")","COMMENT ON COLUMN ","soitcrgntot.","tot_end_unix_tm"," IS ","'집계종료유닉스시각'",";",null,""]
[6,"교통량","trvl",null,"NULL","NUMBER(10)",null,"NUMBER(10)",10,"총교통량",{"$nulls":13},"trvl ","NUMBER(10) ","",",",null,null,"",{"$f":"IF(OR(D248=\"PK\", D248=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitcrgntot.","trvl"," IS ","'총교통량'",";",null,""]
[7,"속도","sped",null,"NULL","NUMBER(5,2)",null,"NUMBER(5,2)","5,2","평균속도",{"$nulls":13},"sped ","NUMBER(5,2) ","",",",null,null,"","","COMMENT ON COLUMN ","soitcrgntot.","sped"," IS ","'평균속도'",";",null,""]
[8,"지체시간","dely_tm",null,"NULL","NUMBER(7,2)",null,"NUMBER(7,2)","5,2","교차로당 평균지체시간",{"$nulls":13},"dely_tm ","NUMBER(7,2) ","",",",null,null,"","","COMMENT ON COLUMN ","soitcrgntot.","dely_tm"," IS ","'교차로당 평균지체시간'",";",null,""]
[9,"대기행렬","queu_lngt",null,"NULL","NUMBER(19,9)",null,"NUMBER(19,9)","19,9","전체 교차로 평균최대대기행렬",{"$nulls":13},"queu_lngt ","NUMBER(19,9) ","",",",null,null,"","","COMMENT ON COLUMN ","soitcrgntot.","queu_lngt"," IS ","'전체 교차로 평균최대대기행렬'",";",null,""]
[10,"구간거리대비 최대대기행렬","queu_rt",null,"NULL","NUMBER(19,9)",null,"NUMBER(19,9)","19,9","거리대비 최대대기행렬",{"$nulls":13},"queu_rt ","NUMBER(19,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcrgntot.","queu_rt"," IS ","'거리대비 최대대기행렬'",";"]
[11,"공간점유율","spae_ocpn_rt",null,"NULL","NUMBER(12,9)",null,"NUMBER(13,9)","12,9","전체 시설물 평균 공간점유율",{"$nulls":13},"spae_ocpn_rt ","NUMBER(13,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcrgntot.","spae_ocpn_rt"," IS ","'전체 시설물 평균 공간점유율'",";",null,{"$f":"IF(LEFT(X253, 13) = \"CONSTRAINT PK\", X253, \"\")","v":""}]
[12,"포화도","strtn_trst_rt",null,"NULL","NUMBER(13,9)",null,"NUMBER(13,9)","12,9","전체 시설물 평균 포화도",{"$nulls":13},"strtn_trst_rt ","NUMBER(13,9) ","",{"$f":"\") TABLESPACE \"&AB256&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_T001 NOLOGGING"},{"$nulls":4},"COMMENT ON COLUMN ","soitcrgntot.","strtn_trst_rt"," IS ","'전체 시설물 평균 포화도'",";",null,""]
[{"$nulls":23},{"$f":"CONCATENATE(AB255:AD255)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (tot_bgng_unix_tm) INTERVAL (86400) STORE IN (\"&AB256&\") (PARTITION BFR_\" & A241& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AB256&\");\"","v":"PARTITION BY RANGE (tot_bgng_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_T001) (PARTITION BFR_soitcrgntot_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_T001);"},{"$f":"\"CREATE INDEX PK_\" & A241& \" ON \" & A241 & CONCATENATE(AC243:AE253) & \" LOCAL (PARTITION BFR_\" & A241 & \"_20221101 TABLESPACE \"&AC256&\") TABLESPACE \"&AC256&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & A241 & \" ADD CONSTRAINT PK_\" & A241 & \" PRIMARY KEY \" & CONCATENATE(AC243:AE253) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$error":"#VALUE!"}]
[{"$nulls":27},"SOIT_D08_T001","SOIT_I08_T001",{"$nulls":9},""]
["시설물 LOS 집계 테이블 - 실시간",{"$nulls":9},"실시간/배치",{"$nulls":27},""]
["soitcfclslosrltmtot",{"$nulls":37},""]
["NO","속성명","컬럼명","PK/FK","NULL","형태",null,"TIBERO","길이","비고",{"$nulls":21},"COMMENT ON TABLE",{"$f":"A258&\" \"","v":"soitcfclslosrltmtot "},null," IS ",{"$f":"\"'\"&SUBSTITUTE(A257,\"테이블\",\"\")&\"'\"","v":"'시설물 LOS 집계  - 실시간'"},";",null,""]
[1,"대상구분코드","trgt_se_cd","PK","NOT NULL","CHAR(2)",null,"VARCHAR2(2)",1,"공간구분코드(601)","3:교차로, 4:엣지그룹, A:전체",{"$nulls":10},"CREATE TABLE ",{"$f":"A258&\" (\"","v":"soitcfclslosrltmtot ("},{"$f":"C260&\" \"","v":"trgt_se_cd "},{"$f":"H260&\" \"","v":"VARCHAR2(2) "},{"$f":"IF(E260=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(D260=\"PK\", D260=\"PK/FK\"), C260, \"\")","v":"trgt_se_cd"},{"$f":"IF(OR(D260=\"PK\", D260=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$A$258&\".\"","v":"soitcfclslosrltmtot."},{"$f":"C260","v":"trgt_se_cd"}," IS ",{"$f":"\"'\"&J260&\"'\"","v":"'공간구분코드(601)'"},";",null,"",{"$nulls":5},"대상ID","지표구분"]
[2,"대상ID","trgt_id","PK/FK","NOT NULL","VARCHAR2(300)",null,"VARCHAR2(300)",20,"대상ID",{"$nulls":13},"trgt_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"trgt_id",",","COMMENT ON COLUMN ","soitcfclslosrltmtot.","trgt_id"," IS ","'대상ID'",";",null,"",{"$nulls":5},"교차로ID","지체시간/대기행렬/정지율"]
[3,"지역구분코드","rgn_prttn_cd","PK","NOT NULL","CHAR(2)",null,"VARCHAR2(2)",2,"지역분할코드 (051)","0 : 메타버스 POC,1 : 계양구,2 : 남동구_상단,3 : 남동구_하단,4 : 미추홀구,5 : 부평구_상단,6 : 부평구_하단,7 : 서구+동구,8 : 연수구,9 : 중구, 동구:20, 서구:80, 남동구:50, 부평구:60",{"$nulls":12},"rgn_prttn_cd ","VARCHAR2(2) ","NOT NULL",",",null,null,"rgn_prttn_cd",",","COMMENT ON COLUMN ","soitcfclslosrltmtot.","rgn_prttn_cd"," IS ","'지역분할코드 (051)'",";"]
[4,"실측여부","acsr_yn","PK","NOT NULL","CHAR(1)",null,"VARCHAR2(1)",1,"실측여부 (500) (실시간만 예측있음)",{"$nulls":13},"acsr_yn ","VARCHAR2(1) ","NOT NULL",",",null,null,"acsr_yn",",","COMMENT ON COLUMN ","soitcfclslosrltmtot.","acsr_yn"," IS ","'실측여부 (500) (실시간만 예측있음)'",";",null,{"$f":"IF(LEFT(X263, 13) = \"CONSTRAINT PK\", X263, \"\")","v":""}]
[5,"지표구분코드","indc_se_cd","PK","NOT NULL","CHAR(2)",null,"VARCHAR2(2)",1," 지표구분코드(508)              ","1:지체시간, 2:(평균)대기행렬, 3:정지율, 4:속도, 5:시간점유율, 6:교통량, \n8:(최대)대기행렬, 9:(최소)대기행렬, 10:밀도, 11:포화도, 12:정지횟수, 13:공간점유율  ",{"$nulls":12},"indc_se_cd ","VARCHAR2(2) ","NOT NULL",",",null,null,"indc_se_cd",",","COMMENT ON COLUMN ","soitcfclslosrltmtot.","indc_se_cd"," IS ","' 지표구분코드(508)              '",";",null,"",{"$nulls":5},"엣지그룹ID","속도/시간점유율/교통량"]
[6,"서비스수준","srvc_levl_cd",null,"NOT NULL","CHAR(2)",null,"VARCHAR2(2)",1,"서비스수준(609)","서비스수준 (A/B/C/D/E/F/FF)",{"$nulls":12},"srvc_levl_cd ","VARCHAR2(2) ","NOT NULL",",",null,null,"","","COMMENT ON COLUMN ","soitcfclslosrltmtot.","srvc_levl_cd"," IS ","'서비스수준(609)'",";",null,"",{"$nulls":5},"행정구역ID","교차로, 엣지그룹 전체지표"]
[7,"실지표값","real_value",null,"NOT NULL","NUMBER(19,9)",null,"NUMBER(19,9)",null,"실지표값",{"$nulls":13},"real_value ","NUMBER(19,9) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcfclslosrltmtot.","real_value"," IS ","'실지표값'",";"]
[8,"집계시작유닉스시각","tot_bgng_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"집계시작유닉스시각",{"$nulls":13},"tot_bgng_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,{"$f":"IF(OR(D267=\"PK\", D267=\"PK/FK\"), C267, \"\")","v":"tot_bgng_unix_tm"},{"$f":"IF(OR(D267=\"PK\", D267=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ","soitcfclslosrltmtot.","tot_bgng_unix_tm"," IS ","'집계시작유닉스시각'",";",null,{"$f":"IF(LEFT(X267, 13) = \"CONSTRAINT PK\", X267, \"\")","v":""},{"$nulls":5},"연동그룹ID","교차로, 엣지그룹 전체지표"]
[9,"집계종료유닉스시각","tot_end_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"집계종료유닉스시각",{"$nulls":13},"tot_end_unix_tm ","NUMBER(10) ","NOT NULL",{"$f":"\") TABLESPACE \"&AB270&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_T001 NOLOGGING"},null,null,"tot_end_unix_tm",")","COMMENT ON COLUMN ","soitcfclslosrltmtot.","tot_end_unix_tm"," IS ","'집계종료유닉스시각'",";",null,"",{"$nulls":5},"전체","교차로, 엣지그룹 전체지표"]
[{"$nulls":23},{"$f":"CONCATENATE(AB269:AD269)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (tot_bgng_unix_tm) INTERVAL (86400) STORE IN (\"&AB270&\") (PARTITION BFR_\" & A258& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AB270&\");\"","v":"PARTITION BY RANGE (tot_bgng_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_T001) (PARTITION BFR_soitcfclslosrltmtot_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_T001);"},{"$f":"\"CREATE INDEX PK_\" & A258& \" ON \" & A258 & CONCATENATE(AC260:AE268) & \" LOCAL (PARTITION BFR_\" & A258 & \"_20221101 TABLESPACE \"&AC270&\") TABLESPACE \"&AC270&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & A258 & \" ADD CONSTRAINT PK_\" & A258 & \" PRIMARY KEY \" & CONCATENATE(AC260:AE268) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$error":"#VALUE!"}]
[{"$nulls":27},"SOIT_D08_T001","SOIT_I08_T001"]
["시설물 LOS 집계 테이블 - 배치",{"$nulls":9},"실시간/배치",{"$nulls":27},{"$f":"IF(LEFT(X271, 13) = \"CONSTRAINT PK\", X271, \"\")","v":""}]
["soitcfclslosarngtot",{"$nulls":37},""]
["NO","속성명","컬럼명","PK/FK","NULL","형태",null,"TIBERO","길이","비고",{"$nulls":21},"COMMENT ON TABLE",{"$f":"A272&\" \"","v":"soitcfclslosarngtot "},null," IS ",{"$f":"\"'\"&SUBSTITUTE(A271,\"테이블\",\"\")&\"'\"","v":"'시설물 LOS 집계  - 배치'"},";",null,""]
[1,"대상구분코드","trgt_se_cd","PK","NOT NULL","CHAR(2)",null,"VARCHAR2(2)",1,"공간구분코드(601)","3:교차로, 4:엣지그룹, 5:행정구역, 6:연동그룹, A:전체, L:링크, 21:도로상행, 22:도로하행",{"$nulls":10},"CREATE TABLE ",{"$f":"A272&\" (\"","v":"soitcfclslosarngtot ("},{"$f":"C274&\" \"","v":"trgt_se_cd "},{"$f":"H274&\" \"","v":"VARCHAR2(2) "},{"$f":"IF(E274=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(D274=\"PK\", D274=\"PK/FK\"), C274, \"\")","v":"trgt_se_cd"},{"$f":"IF(OR(D274=\"PK\", D274=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$A$272&\".\"","v":"soitcfclslosarngtot."},{"$f":"C274","v":"trgt_se_cd"}," IS ",{"$f":"\"'\"&J274&\"'\"","v":"'공간구분코드(601)'"},";",null,"",{"$nulls":5},"대상ID","지표구분"]
[2,"대상ID","trgt_id","PK/FK","NOT NULL","VARCHAR2(300)",null,"VARCHAR2(300)",20,"대상ID",{"$nulls":13},"trgt_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"trgt_id",",","COMMENT ON COLUMN ","soitcfclslosarngtot.","trgt_id"," IS ","'대상ID'",";",null,"",{"$nulls":5},"교차로ID","지체시간/대기행렬/정지율"]
[3,"집계구분코드","tot_se_cd","PK","NOT NULL","CHAR(1)",null,"VARCHAR2(1)",1,"시간유형(011)","집계구분코드 (3:5분단위, 4:15분, 5:60분)",{"$nulls":12},"tot_se_cd ","VARCHAR2(1) ","NOT NULL",",",null,null,"tot_se_cd",",","COMMENT ON COLUMN ","soitcfclslosarngtot.","tot_se_cd"," IS ","'시간유형(011)'",";",null,""]
[4,"지표구분코드","indc_se_cd","PK","NOT NULL","CHAR(2)",null,"VARCHAR2(2)",1," 지표구분코드(508)              ","1:지체시간, 2:(평균)대기행렬, 3:정지율, 4:속도, 5:시간점유율, 6:교통량, \n8:(최대)대기행렬, 9:(최소)대기행렬, 10:밀도, 11:포화도, 12:정지횟수, 13:공간점유율  ",{"$nulls":12},"indc_se_cd ","VARCHAR2(2) ","NOT NULL",",",null,null,"indc_se_cd",",","COMMENT ON COLUMN ","soitcfclslosarngtot.","indc_se_cd"," IS ","' 지표구분코드(508)              '",";",null,"",{"$nulls":5},"엣지그룹ID","속도/시간점유율/교통량"]
[5,"서비스수준","srvc_levl_cd",null,"NOT NULL","CHAR(2)",null,"VARCHAR2(2)",1,"서비스수준(609)","서비스수준 (A/B/C/D/E/F/FF)",{"$nulls":12},"srvc_levl_cd ","VARCHAR2(2) ","NOT NULL",",",null,null,"","","COMMENT ON COLUMN ","soitcfclslosarngtot.","srvc_levl_cd"," IS ","'서비스수준(609)'",";",null,"",{"$nulls":5},"행정구역ID","교차로, 엣지그룹 전체지표"]
[6,"실지표값","real_value",null,"NOT NULL","NUMBER(19,9)",null,"NUMBER(19,9)",null,"실지표값",{"$nulls":13},"real_value ","NUMBER(19,9) ","NOT NULL",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcfclslosarngtot.","real_value"," IS ","'실지표값'",";"]
[7,"집계시작유닉스시각","tot_bgng_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"집계시작유닉스시각",{"$nulls":13},"tot_bgng_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,{"$f":"IF(OR(D280=\"PK\", D280=\"PK/FK\"), C280, \"\")","v":"tot_bgng_unix_tm"},{"$f":"IF(OR(D280=\"PK\", D280=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ","soitcfclslosarngtot.","tot_bgng_unix_tm"," IS ","'집계시작유닉스시각'",";",null,{"$f":"IF(LEFT(X280, 13) = \"CONSTRAINT PK\", X280, \"\")","v":""},{"$nulls":5},"연동그룹ID","교차로, 엣지그룹 전체지표"]
[8,"집계종료유닉스시각","tot_end_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"집계종료유닉스시각",{"$nulls":13},"tot_end_unix_tm ","NUMBER(10) ","NOT NULL",{"$f":"\") TABLESPACE \"&AB283&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_T002 NOLOGGING"},null,null,"tot_end_unix_tm",")","COMMENT ON COLUMN ","soitcfclslosarngtot.","tot_end_unix_tm"," IS ","'집계종료유닉스시각'",";",null,"",{"$nulls":5},"전체","교차로, 엣지그룹 전체지표"]
[{"$nulls":23},{"$f":"CONCATENATE(AB282:AD282)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (tot_bgng_unix_tm) INTERVAL (86400) STORE IN (\"&AB283&\") (PARTITION BFR_\" & A272& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AB283&\");\"","v":"PARTITION BY RANGE (tot_bgng_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_T002) (PARTITION BFR_soitcfclslosarngtot_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_T002);"},{"$f":"\"CREATE INDEX PK_\" & A272& \" ON \" & A272 & CONCATENATE(AC274:AE281) & \" LOCAL (PARTITION BFR_\" & A272 & \"_20221101 TABLESPACE \"&AC283&\") TABLESPACE \"&AC283&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & A272 & \" ADD CONSTRAINT PK_\" & A272 & \" PRIMARY KEY \" & CONCATENATE(AC274:AE281) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$error":"#VALUE!"}]
[{"$nulls":27},"SOIT_D08_T002","SOIT_I08_T002"]
["5분단위 이상/혼잡감지 이력 테이블",{"$nulls":9},"실시간",{"$nulls":27},{"$f":"IF(LEFT(X284, 13) = \"CONSTRAINT PK\", X284, \"\")","v":""}]
["soitcemertrfhstr",{"$nulls":30},"COMMENT ON TABLE",{"$f":"A285&\" \"","v":"soitcemertrfhstr "},null," IS ",{"$f":"\"'\"&SUBSTITUTE(A284,\"테이블\",\"\")&\"'\"","v":"'5분단위 이상/혼잡감지 이력 '"},";",null,""]
["NO","속성명","컬럼명","PK/FK","NULL","형태",null,"TIBERO","길이","비고",{"$nulls":21},"COMMENT ON COLUMN ",{"$f":"$A$285&\".\"","v":"soitcemertrfhstr."},{"$f":"C287","v":"edge_grup_id"}," IS ",{"$f":"\"'\"&J287&\"'\"","v":"'엣지그룹ID'"},";",null,""]
[1,"엣지그룹ID","edge_grup_id","PK/FK","NOT NULL","VARCHAR2(300)",null,"VARCHAR2(300)",20,"엣지그룹ID",{"$nulls":11},"CREATE TABLE ",{"$f":"A285&\" (\"","v":"soitcemertrfhstr ("},{"$f":"C287&\" \"","v":"edge_grup_id "},{"$f":"H287&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(E287=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(D287=\"PK\", D287=\"PK/FK\"), C287, \"\")","v":"edge_grup_id"},{"$f":"IF(OR(D287=\"PK\", D287=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ","soitcemertrfhstr.","rgn_prttn_cd"," IS ","'지역분할코드 (051)'",";",null,""]
[2,"지역구분코드","rgn_prttn_cd","PK","NOT NULL","CHAR(2)",null,"VARCHAR2(2)",2,"지역분할코드 (051)","0 : 메타버스 POC,1 : 계양구,2 : 남동구_상단,3 : 남동구_하단,4 : 미추홀구,5 : 부평구_상단,6 : 부평구_하단,7 : 서구+동구,8 : 연수구,9 : 중구, 동구:20, 서구:80, 남동구:50, 부평구:60",{"$nulls":12},"rgn_prttn_cd ","VARCHAR2(2) ","NOT NULL",",",null,null,"rgn_prttn_cd",",","COMMENT ON COLUMN ","soitcemertrfhstr.","prcs_se_cd"," IS ","'처리구분코드(1:이상감지, 2:혼잡감지)'",";"]
[3,"처리구분코드","prcs_se_cd","PK","NOT NULL","CHAR(1)",null,"VARCHAR2(1)",1,"처리구분코드(1:이상감지, 2:혼잡감지)","집계처리구분(602)",{"$nulls":12},"prcs_se_cd ","VARCHAR2(1) ","NOT NULL",",",null,null,"prcs_se_cd",",","COMMENT ON COLUMN ","soitcemertrfhstr.","tot_bgng_unix_tm"," IS ","'집계시작유닉스시각'",";",null,{"$f":"IF(LEFT(X289, 13) = \"CONSTRAINT PK\", X289, \"\")","v":""}]
[4,"집계시작유닉스시각","tot_bgng_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"집계시작유닉스시각",{"$nulls":13},"tot_bgng_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"tot_bgng_unix_tm",",","COMMENT ON COLUMN ","soitcemertrfhstr.","tot_end_unix_tm"," IS ","'집계종료유닉스시각'",";",null,""]
[5,"집계종료유닉스시각","tot_end_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"집계종료유닉스시각",{"$nulls":13},"tot_end_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"tot_end_unix_tm",")","COMMENT ON COLUMN ","soitcemertrfhstr.","ctrs_clcl_indc_valu"," IS ","'이상감지:대비율, 혼잡감지:한시간전 유닉스시각'",";",null,""]
[6,"대비산출값","ctrs_clcl_indc_valu",null,"NULL","NUMBER(19,9)",null,"NUMBER(19,9)",10,"이상감지:대비율, 혼잡감지:한시간전 유닉스시각",{"$nulls":13},"ctrs_clcl_indc_valu ","NUMBER(19,9) ","",{"$f":"\") TABLESPACE \"&AB294&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_T001 NOLOGGING"},{"$nulls":11},""]
[{"$nulls":23},{"$f":"CONCATENATE(AB293:AD293)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (tot_bgng_unix_tm) INTERVAL (86400) STORE IN (\"&AB294&\") (PARTITION BFR_\" & A285& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AB294&\");\"","v":"PARTITION BY RANGE (tot_bgng_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_T001) (PARTITION BFR_soitcemertrfhstr_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_T001);"},{"$f":"\"CREATE INDEX PK_\" & A285& \" ON \" & A285 & CONCATENATE(AC287:AE291) & \" LOCAL (PARTITION BFR_\" & A285 & \"_20221101 TABLESPACE \"&AC294&\") TABLESPACE \"&AC294&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & A285 & \" ADD CONSTRAINT PK_\" & A285 & \" PRIMARY KEY \" & CONCATENATE(AC287:AE291) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$error":"#VALUE!"}]
[{"$nulls":27},"SOIT_D08_T001","SOIT_I08_T001",{"$nulls":9},""]
[{"$nulls":38},""]
[{"$nulls":38},""]
[{"$nulls":38},""]
[{"$nulls":38},""]
[null,"bi 용 테이블은  화면 기획 나오고  생각하되.  컨셉은   스마트교차로 집계테이블 기준으로   새로  5분 15분..... 집계용 테이블을  진입이동류 별로 집계하는 방향은 어떨지?",{"$nulls":36},"",{"$nulls":5},"교통량 자료.    의미있는           통계치.  데이터.",null,null,null,"hyper데이터에서 불가능하다 그럼 2차 집계까지 고려 필요."]
[null,"bi 공해차량 집계 테이블은 시간별  5분 15분 1시간 일 년  별로  교차로, 카메라id 별로 집계     =>   pl에 등록된 차량의 집입 대수",{"$nulls":36},""]
[{"$nulls":38},""]
[{"$nulls":38},""]
["BI - 진입로 회전별 집계 테이블",{"$nulls":37},""]
["soitcsmrtturntypetot",{"$nulls":37},""]
["NO","속성명","컬럼명","PK/FK","NULL","형태",null,"TIBERO","길이","비고",{"$nulls":21},"COMMENT ON TABLE",{"$f":"A304&\" \"","v":"soitcsmrtturntypetot "},null," IS ",{"$f":"\"'\"&SUBSTITUTE(LEFT(A303,FIND(\"테이블\",A303)-1),\"BI - \",\"\")&\"'\"","v":"'진입로 회전별 집계 '"},";",null,""]
[1,"현장카메라ID","spot_camr_id","PK","NOT NULL","VARCHAR2(10)",null,"VARCHAR2(10)",10,"카메라 ID(교차로 ID + _ + 방향)",{"$nulls":11},"CREATE TABLE ",{"$f":"A304&\" (\"","v":"soitcsmrtturntypetot ("},{"$f":"C306&\" \"","v":"spot_camr_id "},{"$f":"H306&\" \"","v":"VARCHAR2(10) "},{"$f":"IF(E306=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(D306=\"PK\", D306=\"PK/FK\"), C306, \"\")","v":"spot_camr_id"},{"$f":"IF(OR(D306=\"PK\", D306=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$A$304&\".\"","v":"soitcsmrtturntypetot."},{"$f":"C306","v":"spot_camr_id"}," IS ",{"$f":"\"'\"&J306&\"'\"","v":"'카메라 ID(교차로 ID + _ + 방향)'"},";",null,""]
[2,"회전유형코드","turn_type_cd","PK","NOT NULL","CHAR(10)",null,"VARCHAR2(10)",10,"회전 종류 (코드 테이블 참조)",{"$nulls":13},"turn_type_cd ","VARCHAR2(10) ","NOT NULL",",",null,null,"turn_type_cd",",","COMMENT ON COLUMN ","soitcsmrtturntypetot.","turn_type_cd"," IS ","'회전 종류 (코드 테이블 참조)'",";",null,"",null,null,"진입 이동류 번호",null,"용어가 전부 회전으로 통일된건가?"]
[3,"시간유형코드","hr_type_cd","PK","NOT NULL","CHAR(10)",null,"VARCHAR2(10)",10,"시간타입(5분 OR 현시)","집계구분코드 (4:15분)",{"$nulls":12},"hr_type_cd ","VARCHAR2(10) ","NOT NULL",",",null,null,"hr_type_cd",",","COMMENT ON COLUMN ","soitcsmrtturntypetot.","hr_type_cd"," IS ","'시간타입(5분 OR 현시)'",";",null,""]
[4,"통계시작유닉스시각","stats_bgng_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"통계시작일시(unix timestamp)",{"$nulls":13},"stats_bgng_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"stats_bgng_unix_tm",",","COMMENT ON COLUMN ","soitcsmrtturntypetot.","stats_bgng_unix_tm"," IS ","'통계시작일시(unix timestamp)'",";",null,""]
[5,"통계종료유닉스시각","stats_end_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"통계종료일시(unix timestamp)",{"$nulls":13},"stats_end_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"stats_end_unix_tm",")","COMMENT ON COLUMN ","soitcsmrtturntypetot.","stats_end_unix_tm"," IS ","'통계종료일시(unix timestamp)'",";",null,""]
[6,"차종1_교통량","kncr1_trvl",null,"NULL","NUMBER(10)",null,"NUMBER(10)",10,"교통량_차종1","MBUS",{"$nulls":12},"kncr1_trvl ","NUMBER(10) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcsmrtturntypetot.","kncr1_trvl"," IS ","'교통량_차종1'",";",null,""]
[7,"차종2_교통량","kncr2_trvl",null,"NULL","NUMBER(10)",null,"NUMBER(10)",10,"교통량_차종2","LBUS",{"$nulls":12},"kncr2_trvl ","NUMBER(10) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcsmrtturntypetot.","kncr2_trvl"," IS ","'교통량_차종2'",";",null,""]
[8,"차종3_교통량","kncr3_trvl",null,"NULL","NUMBER(10)",null,"NUMBER(10)",10,"교통량_차종3","PCAR",{"$nulls":12},"kncr3_trvl ","NUMBER(10) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcsmrtturntypetot.","kncr3_trvl"," IS ","'교통량_차종3'",";",null,""]
[9,"차종4_교통량","kncr4_trvl",null,"NULL","NUMBER(10)",null,"NUMBER(10)",10,"교통량_차종4","MOTOR",{"$nulls":12},"kncr4_trvl ","NUMBER(10) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcsmrtturntypetot.","kncr4_trvl"," IS ","'교통량_차종4'",";",null,""]
[10,"차종5_교통량","kncr5_trvl",null,"NULL","NUMBER(10)",null,"NUMBER(10)",10,"교통량_차종5","MTRUCK",{"$nulls":12},"kncr5_trvl ","NUMBER(10) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcsmrtturntypetot.","kncr5_trvl"," IS ","'교통량_차종5'",";",null,""]
[11,"차종6_교통량","kncr6_trvl",null,"NULL","NUMBER(10)",null,"NUMBER(10)",10,"교통량_차종6","LTRUCK",{"$nulls":12},"kncr6_trvl ","NUMBER(10) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcsmrtturntypetot.","kncr6_trvl"," IS ","'교통량_차종6'",";",null,""]
[15,"총관측교통량","totl_obsrvn_trvl",null,"NULL","NUMBER(10)",null,"NUMBER(10)",10,"오토바이제외 전교통량",{"$nulls":13},"totl_obsrvn_trvl ","NUMBER(10) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcsmrtturntypetot.","totl_obsrvn_trvl"," IS ","'오토바이제외 전교통량'",";",null,"",null,null,"추가집계"]
[16,"총환산교통량","totl_cvsn_trvl",null,"NULL","NUMBER(19,9)",null,"NUMBER(19,9)","19,9","오토바이제외 대형차는 가중치 1.8 곱한 교통량",{"$nulls":13},"totl_cvsn_trvl ","NUMBER(19,9) ","",{"$f":"\") TABLESPACE \"&AB320&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_T002 NOLOGGING"},{"$nulls":4},"COMMENT ON COLUMN ","soitcsmrtturntypetot.","totl_cvsn_trvl"," IS ","'오토바이제외 대형차는 가중치 1.8 곱한 교통량'",";",null,"",null,null,"추가집계"]
[{"$nulls":23},{"$f":"CONCATENATE(AB319:AD319)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (stats_bgng_unix_tm) INTERVAL (86400) STORE IN (\"&AB320&\") (PARTITION BFR_\" & A304& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AB320&\");\"","v":"PARTITION BY RANGE (stats_bgng_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_T002) (PARTITION BFR_soitcsmrtturntypetot_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_T002);"},{"$f":"\"CREATE INDEX PK_\" & A304& \" ON \" & A304 & CONCATENATE(AC306:AE316) & \" LOCAL (PARTITION BFR_\" & A304 & \"_20221101 TABLESPACE \"&AC320&\") TABLESPACE \"&AC320&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & A304 & \" ADD CONSTRAINT PK_\" & A304 & \" PRIMARY KEY \" & CONCATENATE(AC306:AE315) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$error":"#VALUE!"}]
[{"$nulls":27},"SOIT_D08_T002","SOIT_I08_T002"]
["BI - 보행자통계 테이블",{"$nulls":37},{"$f":"IF(LEFT(X321, 13) = \"CONSTRAINT PK\", X321, \"\")","v":""}]
["soitcsmrtcwdttot",{"$nulls":37},""]
["NO","속성명","컬럼명","PK/FK","NULL","형태",null,"TIBERO","길이","비고",{"$nulls":21},"COMMENT ON TABLE",{"$f":"A322&\" \"","v":"soitcsmrtcwdttot "},null," IS ",{"$f":"\"'\"&SUBSTITUTE(LEFT(A321,FIND(\"테이블\",A321)-1),\"BI - \",\"\")&\"'\"","v":"'보행자통계 '"},";",null,""]
[1,"현장카메라ID","spot_camr_id","PK","NOT NULL","VARCHAR2(10)",null,"VARCHAR2(10)",10,"카메라 ID(교차로 ID + _ + 방향)",{"$nulls":11},"CREATE TABLE ",{"$f":"A322&\" (\"","v":"soitcsmrtcwdttot ("},{"$f":"C324&\" \"","v":"spot_camr_id "},{"$f":"H324&\" \"","v":"VARCHAR2(10) "},{"$f":"IF(E324=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(D324=\"PK\", D324=\"PK/FK\"), C324, \"\")","v":"spot_camr_id"},{"$f":"IF(OR(D324=\"PK\", D324=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$A$322&\".\"","v":"soitcsmrtcwdttot."},{"$f":"C324","v":"spot_camr_id"}," IS ",{"$f":"\"'\"&J324&\"'\"","v":"'카메라 ID(교차로 ID + _ + 방향)'"},";",null,""]
[2,"시간유형코드","hr_type_cd","PK","NOT NULL","CHAR(10)",null,"VARCHAR2(10)",10,"시간유형(011)시간타입(5분, 15분, 60분)","집계구분코드 (3:5분단위, 4:15분)",{"$nulls":12},"hr_type_cd ","VARCHAR2(10) ","NOT NULL",",",null,null,"hr_type_cd",",","COMMENT ON COLUMN ","soitcsmrtcwdttot.","hr_type_cd"," IS ","'시간유형(011)시간타입(5분, 15분, 60분)'",";",null,""]
[3,"통계시작유닉스시각","stats_bgng_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"통계시작일시(unix timestamp)",{"$nulls":13},"stats_bgng_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"stats_bgng_unix_tm",",","COMMENT ON COLUMN ","soitcsmrtcwdttot.","stats_bgng_unix_tm"," IS ","'통계시작일시(unix timestamp)'",";",null,""]
[4,"통계종료유닉스시각","stats_end_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"통계종료일시(unix timestamp)",{"$nulls":13},"stats_end_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"stats_end_unix_tm",")","COMMENT ON COLUMN ","soitcsmrtcwdttot.","stats_end_unix_tm"," IS ","'통계종료일시(unix timestamp)'",";",null,""]
[5,"방향구분코드","drct_se_cd","PK","NOT NULL","CHAR(1)",null,"VARCHAR2(1)",1,"방향(왼쪽,오른쪽)","보행자방향구분(013) (왼쪽:L, 오른쪽:R)",{"$nulls":12},"drct_se_cd ","VARCHAR2(1) ","NOT NULL",",",null,null,"drct_se_cd",{"$f":"IF(OR(D328=\"PK\", D328=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ","soitcsmrtcwdttot.","drct_se_cd"," IS ","'방향(왼쪽,오른쪽)'",";",null,""]
[6,"검지건수","dttn_nocs",null,"NULL","NUMBER(10)",null,"NUMBER(10)",10,"통행감지건수",{"$nulls":13},"dttn_nocs ","NUMBER(10) ","",{"$f":"\") TABLESPACE \"&AB331&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_T002 NOLOGGING"},{"$nulls":4},"COMMENT ON COLUMN ","soitcsmrtcwdttot.","dttn_nocs"," IS ","'통행감지건수'",";",null,""]
[{"$nulls":23},{"$f":"CONCATENATE(AB330:AD330)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (stats_bgng_unix_tm) INTERVAL (86400) STORE IN (\"&AB331&\") (PARTITION BFR_\" & A322& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AB331&\");\"","v":"PARTITION BY RANGE (stats_bgng_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_T002) (PARTITION BFR_soitcsmrtcwdttot_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_T002);"},{"$f":"\"CREATE INDEX PK_\" & A322& \" ON \" & A322 & CONCATENATE(AC323:AE328) & \" LOCAL (PARTITION BFR_\" & A322 & \"_20221101 TABLESPACE \"&AC331&\") TABLESPACE \"&AC331&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & A322 & \" ADD CONSTRAINT PK_\" & A322 & \" PRIMARY KEY \" & CONCATENATE(AC323:AE328) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$error":"#VALUE!"}]
[{"$nulls":27},"SOIT_D08_T002","SOIT_I08_T002"]
["BI - 돌발통계 테이블",{"$nulls":37},{"$f":"IF(LEFT(X332, 13) = \"CONSTRAINT PK\", X332, \"\")","v":""}]
["soitcsmrtunacevettot",{"$nulls":37},""]
["NO","속성명","컬럼명","PK/FK","NULL","형태",null,"TIBERO","길이","비고",{"$nulls":21},"COMMENT ON TABLE",{"$f":"A333&\" \"","v":"soitcsmrtunacevettot "},null," IS ",{"$f":"\"'\"&SUBSTITUTE(LEFT(A332,FIND(\"테이블\",A332)-1),\"BI - \",\"\")&\"'\"","v":"'돌발통계 '"},";",null,""]
[1,"현장카메라ID","spot_camr_id","PK","NOT NULL","VARCHAR2(10)",null,"VARCHAR2(10)",10,"카메라 ID(교차로 ID + _ + 방향)",{"$nulls":11},"CREATE TABLE ",{"$f":"A333&\" (\"","v":"soitcsmrtunacevettot ("},{"$f":"C335&\" \"","v":"spot_camr_id "},{"$f":"H335&\" \"","v":"VARCHAR2(10) "},{"$f":"IF(E335=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(D335=\"PK\", D335=\"PK/FK\"), C335, \"\")","v":"spot_camr_id"},{"$f":"IF(OR(D335=\"PK\", D335=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$A$333&\".\"","v":"soitcsmrtunacevettot."},{"$f":"C335","v":"spot_camr_id"}," IS ",{"$f":"\"'\"&J335&\"'\"","v":"'카메라 ID(교차로 ID + _ + 방향)'"},";",null,""]
[2,"이벤트유형코드","evet_type_cd","PK","NOT NULL","CHAR(1)",null,"VARCHAR2(1)",1,"이벤트 타입(코드테이블참조)","돌발유형(012) (1:차량정지, 2:꼬리물기, 3:보행자횡단;인도이탈, 4:역주행)",{"$nulls":12},"evet_type_cd ","VARCHAR2(1) ","NOT NULL",",",null,null,"evet_type_cd",",","COMMENT ON COLUMN ","soitcsmrtunacevettot.","evet_type_cd"," IS ","'이벤트 타입(코드테이블참조)'",";",null,""]
[3,"시간유형코드","hr_type_cd","PK","NOT NULL","CHAR(10)",null,"VARCHAR2(10)",10,"시간유형(011)시간타입(5분, 15분, 60분)","집계구분코드 (3:5분단위, 4:15분)",{"$nulls":12},"hr_type_cd ","VARCHAR2(10) ","NOT NULL",",",null,null,"hr_type_cd",",","COMMENT ON COLUMN ","soitcsmrtunacevettot.","hr_type_cd"," IS ","'시간유형(011)시간타입(5분, 15분, 60분)'",";",null,""]
[4,"통계시작유닉스시각","stats_bgng_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"통계시작일시(unix timestamp)",{"$nulls":13},"stats_bgng_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"stats_bgng_unix_tm",",","COMMENT ON COLUMN ","soitcsmrtunacevettot.","stats_bgng_unix_tm"," IS ","'통계시작일시(unix timestamp)'",";",null,""]
[5,"통계종료유닉스시각","stats_end_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"통계종료일시(unix timestamp)",{"$nulls":13},"stats_end_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"stats_end_unix_tm",")","COMMENT ON COLUMN ","soitcsmrtunacevettot.","stats_end_unix_tm"," IS ","'통계종료일시(unix timestamp)'",";",null,""]
[6,"검지건수","dttn_nocs",null,"NULL","NUMBER(10)",null,"NUMBER(10)",10,"감지건수",{"$nulls":13},"dttn_nocs ","NUMBER(10) ","",{"$f":"\") TABLESPACE \"&AB342&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_T002 NOLOGGING"},{"$nulls":4},"COMMENT ON COLUMN ","soitcsmrtunacevettot.","dttn_nocs"," IS ","'감지건수'",";",null,""]
[{"$nulls":23},{"$f":"CONCATENATE(AB341:AD341)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (stats_bgng_unix_tm) INTERVAL (86400) STORE IN (\"&AB342&\") (PARTITION BFR_\" & A333& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AB342&\");\"","v":"PARTITION BY RANGE (stats_bgng_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_T002) (PARTITION BFR_soitcsmrtunacevettot_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_T002);"},{"$f":"\"CREATE INDEX PK_\" & A333& \" ON \" & A333 & CONCATENATE(AC334:AE339) & \" LOCAL (PARTITION BFR_\" & A333 & \"_20221101 TABLESPACE \"&AC342&\") TABLESPACE \"&AC342&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & A333 & \" ADD CONSTRAINT PK_\" & A333 & \" PRIMARY KEY \" & CONCATENATE(AC334:AE339) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$error":"#VALUE!"}]
[{"$nulls":27},"SOIT_D08_T002","SOIT_I08_T002"]
["BI - 교차로O/D통계테이블",{"$nulls":37},{"$f":"IF(LEFT(X343, 13) = \"CONSTRAINT PK\", X343, \"\")","v":""},null,null,null,"일단위로만 집계한다"]
["soitcsmrtpltnvhclstats",{"$nulls":37},""]
["NO","속성명","컬럼명","PK/FK","NULL","형태",null,"TIBERO","길이","비고",{"$nulls":21},"COMMENT ON TABLE",{"$f":"A344&\" \"","v":"soitcsmrtpltnvhclstats "},null," IS ",{"$f":"\"'\"&SUBSTITUTE(LEFT(A343,FIND(\"테이블\",A343)-1),\"BI - \",\"\")&\"'\"","v":"'교차로O/D통계'"},";",null,""]
[1,"통계시작유닉스시각","stats_bgng_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"통계시작유닉스시각",{"$nulls":11},"CREATE TABLE ",{"$f":"A344&\" (\"","v":"soitcsmrtpltnvhclstats ("},{"$f":"C346&\" \"","v":"stats_bgng_unix_tm "},{"$f":"H346&\" \"","v":"NUMBER(10) "},{"$f":"IF(E346=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(D346=\"PK\", D346=\"PK/FK\"), C346, \"\")","v":"stats_bgng_unix_tm"},{"$f":"IF(OR(D346=\"PK\", D346=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$A$344&\".\"","v":"soitcsmrtpltnvhclstats."},{"$f":"C346","v":"stats_bgng_unix_tm"}," IS ",{"$f":"\"'\"&J346&\"'\"","v":"'통계시작유닉스시각'"},";",null,""]
[2,"통계종료유닉스시각","stats_end_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"통계종료유닉스시각",{"$nulls":13},"stats_end_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"stats_end_unix_tm",",","COMMENT ON COLUMN ","soitcsmrtpltnvhclstats.","stats_end_unix_tm"," IS ","'통계종료유닉스시각'",";",null,""]
[3,"시작현장교차로ID","bgng_spot_ints_id","PK","NOT NULL","NUMBER(5)",null,"NUMBER(5)",5,"출발현장교차로 ID",{"$nulls":13},"bgng_spot_ints_id ","NUMBER(5) ","NOT NULL",",",null,null,"bgng_spot_ints_id",",","COMMENT ON COLUMN ","soitcsmrtpltnvhclstats.","bgng_spot_ints_id"," IS ","'출발현장교차로 ID'",";",null,""]
[4,"도착현장교차로ID","arvl_spot_ints_id","PK","NOT NULL","NUMBER(5)",null,"NUMBER(5)",5,"도착현장교차로 ID",{"$nulls":13},"arvl_spot_ints_id ","NUMBER(5) ","NOT NULL",",",null,null,"arvl_spot_ints_id",")","COMMENT ON COLUMN ","soitcsmrtpltnvhclstats.","arvl_spot_ints_id"," IS ","'도착현장교차로 ID'",";",null,""]
[5,"총교통량","totl_trvl",null,"NULL","NUMBER(10)",null,"NUMBER(10)",10,"총교통량",{"$nulls":13},"totl_trvl ","NUMBER(10) ","",{"$f":"\") TABLESPACE \"&AB352&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_T002 NOLOGGING"},{"$nulls":4},"COMMENT ON COLUMN ","soitcsmrtpltnvhclstats.","totl_trvl"," IS ","'총교통량'",";",null,""]
[{"$nulls":23},{"$f":"CONCATENATE(AB351:AD351)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (stats_bgng_unix_tm) INTERVAL (86400) STORE IN (\"&AB352&\") (PARTITION BFR_\" & A344& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AB352&\");\"","v":"PARTITION BY RANGE (stats_bgng_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_T002) (PARTITION BFR_soitcsmrtpltnvhclstats_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_T002);"},{"$f":"\"CREATE INDEX PK_\" & A344& \" ON \" & A344 & CONCATENATE(AC346:AE349) & \" LOCAL (PARTITION BFR_\" & A344 & \"_20221101 TABLESPACE \"&AC352&\") TABLESPACE \"&AC352&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & A344 & \" ADD CONSTRAINT PK_\" & A344 & \" PRIMARY KEY \" & CONCATENATE(AC346:AE349) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":8},{"$error":"#VALUE!"}]
[{"$nulls":27},"SOIT_D08_T002","SOIT_I08_T002"]
["BI - 교차로 차종별O/D통계테이블"]
["soitcsmrtpltnvhclkndstats",{"$nulls":37},{"$f":"IF(LEFT(X354, 13) = \"CONSTRAINT PK\", X354, \"\")","v":""}]
["NO","속성명","컬럼명","PK/FK","NULL","형태",null,"TIBERO","길이","비고",{"$nulls":21},"COMMENT ON TABLE",{"$f":"A354&\" \"","v":"soitcsmrtpltnvhclkndstats "},null," IS ",{"$f":"\"'\"&SUBSTITUTE(LEFT(A353,FIND(\"테이블\",A353)-1),\"BI - \",\"\")&\"'\"","v":"'교차로 차종별O/D통계'"},";",null,""]
[1,"통계시작유닉스시각","stats_bgng_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"통계시작유닉스시각",{"$nulls":11},"CREATE TABLE ",{"$f":"A354&\" (\"","v":"soitcsmrtpltnvhclkndstats ("},{"$f":"C356&\" \"","v":"stats_bgng_unix_tm "},{"$f":"H356&\" \"","v":"NUMBER(10) "},{"$f":"IF(E356=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(D356=\"PK\", D356=\"PK/FK\"), C356, \"\")","v":"stats_bgng_unix_tm"},{"$f":"IF(OR(D356=\"PK\", D356=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$A$354&\".\"","v":"soitcsmrtpltnvhclkndstats."},{"$f":"C356","v":"stats_bgng_unix_tm"}," IS ",{"$f":"\"'\"&J356&\"'\"","v":"'통계시작유닉스시각'"},";",null,""]
[2,"통계종료유닉스시각","stats_end_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"통계종료유닉스시각",{"$nulls":13},"stats_end_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"stats_end_unix_tm",",","COMMENT ON COLUMN ","soitcsmrtpltnvhclkndstats.","stats_end_unix_tm"," IS ","'통계종료유닉스시각'",";"]
[3,"시작현장교차로ID","bgng_spot_ints_id","PK","NOT NULL","NUMBER(5)",null,"NUMBER(5)",5,"출발현장교차로 ID",{"$nulls":13},"bgng_spot_ints_id ","NUMBER(5) ","NOT NULL",",",null,null,"bgng_spot_ints_id",",","COMMENT ON COLUMN ","soitcsmrtpltnvhclkndstats.","bgng_spot_ints_id"," IS ","'출발현장교차로 ID'",";"]
[4,"도착현장교차로ID","arvl_spot_ints_id","PK","NOT NULL","NUMBER(5)",null,"NUMBER(5)",5,"도착현장교차로 ID",{"$nulls":13},"arvl_spot_ints_id ","NUMBER(5) ","NOT NULL",",",null,null,"arvl_spot_ints_id",",","COMMENT ON COLUMN ","soitcsmrtpltnvhclkndstats.","arvl_spot_ints_id"," IS ","'도착현장교차로 ID'",";"]
[5,"차종코드","kncr_cd","PK","NOT NULL","CHAR(10)",null,"VARCHAR2(10)",3,"차종(008)",{"$nulls":13},"kncr_cd ","VARCHAR2(10) ","NOT NULL",",",null,null,"kncr_cd",")","COMMENT ON COLUMN ","soitcsmrtpltnvhclkndstats.","kncr_cd"," IS ","'차종(008)'",";"]
[6,"총교통량","totl_trvl",null,"NULL","NUMBER(10)",null,"NUMBER(10)",10,"총교통량",{"$nulls":13},"totl_trvl ","NUMBER(10) ","",{"$f":"\") TABLESPACE \"&AB363&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_T002 NOLOGGING"},{"$nulls":4},"COMMENT ON COLUMN ","soitcsmrtpltnvhclkndstats.","totl_trvl"," IS ","'총교통량'",";"]
[{"$nulls":23},{"$f":"CONCATENATE(AB362:AE362)","v":{"$error":"#VALUE!"}}," ","",null,{"$f":"\"PARTITION BY RANGE (stats_bgng_unix_tm) INTERVAL (86400) STORE IN (\"&AB363&\") (PARTITION BFR_\" & A354& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AB363&\");\"","v":"PARTITION BY RANGE (stats_bgng_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_T002) (PARTITION BFR_soitcsmrtpltnvhclkndstats_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_T002);"},{"$f":"\"CREATE INDEX PK_\" & A354& \" ON \" & A354 & CONCATENATE(AC356:AE360) & \" LOCAL (PARTITION BFR_\" & A354 & \"_20221101 TABLESPACE \"&AC363&\") TABLESPACE \"&AC363&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & A354 & \" ADD CONSTRAINT PK_\" & A354 & \" PRIMARY KEY \" & CONCATENATE(AC356:AE360) & \";\"","v":{"$error":"#VALUE!"}}]
[{"$nulls":23},{"$f":"C363&\" \"","v":" "}," ","",null,"SOIT_D08_T002","SOIT_I08_T002"]
[]
["BI - 진입로 대기행렬 집계 테이블(시간단위)"]
["soitcsmrtaprdqueu"]
["NO","속성명","컬럼명","PK/FK","NULL","형태",null,"TIBERO","길이","비고",{"$nulls":21},"COMMENT ON TABLE",{"$f":"A366&\" \"","v":"soitcsmrtaprdqueu "},null,"IS",{"$f":"\"'\"&SUBSTITUTE(LEFT(A365,FIND(\"테이블\",A365)-1),\"BI - \",\"\")&\"'\"","v":"'진입로 대기행렬 집계 '"},";"]
[1,"현장카메라ID","spot_camr_id","PK","NOT NULL","VARCHAR2(10)",null,"VARCHAR2(10)",10,"카메라 ID(교차로 ID + _ + 방향)",{"$nulls":10},",","CREATE TABLE",{"$f":"A366&\" (\"","v":"soitcsmrtaprdqueu ("},"spot_camr_id","VARCHAR2(10)","NOT NULL",",",null,"(","spot_camr_id",",","COMMENT ON COLUMN",{"$f":"$A$366&\".\"","v":"soitcsmrtaprdqueu."},"spot_camr_id","IS",{"$f":"\"'\"&J368&\"'\"","v":"'카메라 ID(교차로 ID + _ + 방향)'"},";"]
[2,"통계시작유닉스시각","stats_bgng_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"통계시작일시(unix timestamp)",{"$nulls":10},",",null,null,"stats_bgng_unix_tm","NUMBER(10)","NOT NULL",",",null,null,"stats_bgng_unix_tm",",","COMMENT ON COLUMN","soitcsmrtaprdqueu.","stats_bgng_unix_tm","IS","'통계시작일시(unix timestamp)'",";"]
[3,"통계종료유닉스시각","stats_end_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"통계종료일시(unix timestamp)",{"$nulls":10},"));",null,null,"stats_end_unix_tm","NUMBER(10)","NOT NULL",",",null,null,"stats_end_unix_tm",") ","COMMENT ON COLUMN","soitcsmrtaprdqueu.","stats_end_unix_tm","IS","'통계종료일시(unix timestamp)'",";"]
[4,"잔여대기행렬길이","rmnn_queu_lngt",null,"NULL","NUMBER(19,9)",null,"NUMBER(19,9)","19,9","잔여대기행렬(단위:대/km/차선)",{"$nulls":13},"rmnn_queu_lngt","NUMBER(19,9)",null,",",{"$nulls":4},"COMMENT ON COLUMN","soitcsmrtaprdqueu.","rmnn_queu_lngt","IS","'잔여대기행렬(단위:대/km/차선)'",";"]
[5,"최대대기행렬길이","max_queu_lngt",null,"NULL","NUMBER(19,9)",null,"NUMBER(19,9)","19,9","최대대기행렬(단위:대/km/차선)",{"$nulls":13},"max_queu_lngt","NUMBER(19,9)",null,{"$f":"\") TABLESPACE \"&AB374&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_T002 NOLOGGING"},{"$nulls":4},"COMMENT ON COLUMN","soitcsmrtaprdqueu.","max_queu_lngt","IS","'최대대기행렬(단위:대/km/차선)'",";"]
[{"$nulls":23},{"$f":"CONCATENATE(AB373:AD373)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (stats_bgng_unix_tm) INTERVAL (86400) STORE IN (\"&AB374&\") (PARTITION BFR_\" & A366& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AB374&\");\"","v":"PARTITION BY RANGE (stats_bgng_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_T002) (PARTITION BFR_soitcsmrtaprdqueu_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_T002);"},{"$f":"\"CREATE INDEX PK_\" & A366& \" ON \" & A366 & CONCATENATE(AC368:AE371) & \" LOCAL (PARTITION BFR_\" & A366 & \"_20221101 TABLESPACE \"&AC374&\") TABLESPACE \"&AC374&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & A366 & \" ADD CONSTRAINT PK_\" & A366 & \" PRIMARY KEY \" & CONCATENATE(AC368:AE371) & \";\"","v":{"$error":"#VALUE!"}},{"$nulls":8},"CONSTRAINT PK_soitcaprdqueu PRIMARY KEY (spot_camr_id,stats_bgng_unix_tm,stats_end_unix_tm) using index tablespace SOIT_I08);"]
[{"$nulls":27},"SOIT_D08_T002","SOIT_I08_T002"]
["BI - 진입로 차선별 대기행렬 집계 테이블(시간단위)"]
["soitcsmrtlanequeu"]
["NO","속성명","컬럼명","PK/FK","NULL","형태",null,"TIBERO","길이","비고",{"$nulls":21},"COMMENT ON TABLE",{"$f":"A376&\" \"","v":"soitcsmrtlanequeu "},null,"IS",{"$f":"\"'\"&SUBSTITUTE(LEFT(A375,FIND(\"테이블\",A375)-1),\"BI - \",\"\")&\"'\"","v":"'진입로 차선별 대기행렬 집계 '"},";"]
[1,"현장카메라ID","spot_camr_id","PK","NOT NULL","VARCHAR2(10)",null,"VARCHAR2(10)",10,"카메라 ID(교차로 ID + _ + 방향)",{"$nulls":10},",","CREATE TABLE",{"$f":"A376&\" (\"","v":"soitcsmrtlanequeu ("},"spot_camr_id","VARCHAR2(10)","NOT NULL",",",null,"(","spot_camr_id",",","COMMENT ON COLUMN",{"$f":"$A$376&\".\"","v":"soitcsmrtlanequeu."},"spot_camr_id","IS",{"$f":"\"'\"&J378&\"'\"","v":"'카메라 ID(교차로 ID + _ + 방향)'"},";"]
[2,"차로번호","lane_no","PK","NOT NULL","NUMBER(2)",null,"NUMBER(2)",2,"차로 번호",{"$nulls":10},",",null,null,"lane_no","NUMBER(2)","NOT NULL",",",null,null,"lane_no",",","COMMENT ON COLUMN","soitcsmrtlanequeu.","lane_no","IS","'차로 번호'",";"]
[3,"통계시작유닉스시각","stats_bgng_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"통계시작일시(unix timestamp)",{"$nulls":10},",",null,null,"stats_bgng_unix_tm","NUMBER(10)","NOT NULL",",",null,null,"stats_bgng_unix_tm",",","COMMENT ON COLUMN","soitcsmrtlanequeu.","stats_bgng_unix_tm","IS","'통계시작일시(unix timestamp)'",";"]
[4,"통계종료유닉스시각","stats_end_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"통계종료일시(unix timestamp)",{"$nulls":10},"));",null,null,"stats_end_unix_tm","NUMBER(10)","NOT NULL",",",null,null,"stats_end_unix_tm",") ","COMMENT ON COLUMN","soitcsmrtlanequeu.","stats_end_unix_tm","IS","'통계종료일시(unix timestamp)'",";"]
[5,"잔여대기행렬길이","rmnn_queu_lngt",null,"NULL","NUMBER(19,9)",null,"NUMBER(19,9)","19,9","잔여대기행렬(단위:대/km/차선)",{"$nulls":13},"rmnn_queu_lngt","NUMBER(19,9)",null,",",{"$nulls":4},"COMMENT ON COLUMN","soitcsmrtlanequeu.","rmnn_queu_lngt","IS","'잔여대기행렬(단위:대/km/차선)'",";"]
[6,"최대대기행렬길이","max_queu_lngt",null,"NULL","NUMBER(19,9)",null,"NUMBER(19,9)","19,9","최대대기행렬(단위:대/km/차선)",{"$nulls":13},"max_queu_lngt","NUMBER(19,9)",null,{"$f":"\") TABLESPACE \"&AB385&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_T002 NOLOGGING"},{"$nulls":4},"COMMENT ON COLUMN","soitcsmrtlanequeu.","max_queu_lngt","IS","'최대대기행렬(단위:대/km/차선)'",";"]
[{"$nulls":23},{"$f":"CONCATENATE(AB384:AD384)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (stats_bgng_unix_tm) INTERVAL (86400) STORE IN (\"&AB385&\") (PARTITION BFR_\" & A376& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AB385&\");\"","v":"PARTITION BY RANGE (stats_bgng_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_T002) (PARTITION BFR_soitcsmrtlanequeu_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_T002);"},{"$f":"\"CREATE INDEX PK_\" & A376& \" ON \" & A376 & CONCATENATE(AC378:AE382) & \" LOCAL (PARTITION BFR_\" & A376 & \"_20221101 TABLESPACE \"&AC385&\") TABLESPACE \"&AC385&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & A376 & \" ADD CONSTRAINT PK_\" & A376 & \" PRIMARY KEY \" & CONCATENATE(AC378:AE382) & \";\"","v":{"$error":"#VALUE!"}}]
[{"$nulls":27},"SOIT_D08_T002","SOIT_I08_T002"]
["엣지그룹별 실시간 대기행렬/공간점유율 테이블 - 1지역",{"$nulls":37},{"$f":"IF(LEFT(X386, 13) = \"CONSTRAINT PK\", X386, \"\")","v":""}]
["soitcedgegruprltmqueu_1",{"$nulls":10},{"$f":"LEN(A387)","v":23},{"$nulls":26},""]
["NO","속성명","컬럼명","PK/FK","NULL","형태",null,"TIBERO","길이","비고",{"$nulls":21},"COMMENT ON TABLE",{"$f":"A387&\" \"","v":"soitcedgegruprltmqueu_1 "},null," IS ",{"$f":"\"'\"&SUBSTITUTE(A386,\"테이블\",\"\")&\"'\"","v":"'엣지그룹별 실시간 대기행렬/공간점유율  - 1지역'"},";",null,""]
[1,"엣지그룹ID","edge_grup_id","PK/FK","NOT NULL","VARCHAR2(300)",null,"VARCHAR2(300)",20,"엣지그룹ID",{"$nulls":11},"CREATE TABLE ",{"$f":"A387&\" (\"","v":"soitcedgegruprltmqueu_1 ("},{"$f":"C389&\" \"","v":"edge_grup_id "},{"$f":"H389&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(E389=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(D389=\"PK\", D389=\"PK/FK\"), C389, \"\")","v":"edge_grup_id"},{"$f":"IF(OR(D389=\"PK\", D389=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$A$387&\".\"","v":"soitcedgegruprltmqueu_1."},{"$f":"C389","v":"edge_grup_id"}," IS ",{"$f":"\"'\"&J389&\"'\"","v":"'엣지그룹ID'"},";",null,""]
[3,"차로번호","lane_no","PK","NOT NULL","NUMBER(2)",null,"NUMBER(2)",2,"차로번호",{"$nulls":13},"lane_no ","NUMBER(2) ","NOT NULL",",",null,null,"lane_no",",","COMMENT ON COLUMN ","soitcedgegruprltmqueu_1.","lane_no"," IS ","'차로번호'",";",null,""]
[4,"실측여부","acsr_yn","PK","NOT NULL","CHAR(1)",null,"VARCHAR2(1)",1,"실측여부 (500) (실시간만 예측있음)",{"$nulls":13},"acsr_yn ","VARCHAR2(1) ","NOT NULL",",",null,null,"acsr_yn",",","COMMENT ON COLUMN ","soitcedgegruprltmqueu_1.","acsr_yn"," IS ","'실측여부 (500) (실시간만 예측있음)'",";",null,""]
[5,"수집유닉스시각","clct_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"수집유닉스시각",{"$nulls":13},"clct_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"clct_unix_tm",")","COMMENT ON COLUMN ","soitcedgegruprltmqueu_1.","clct_unix_tm"," IS ","'수집유닉스시각'",";",null,""]
[6,"대기행렬길이","queu_lngt",null,"NULL","NUMBER(19,9)",null,"NUMBER(19,9)","19,9","대기행렬길이 (meter)",{"$nulls":13},"queu_lngt ","NUMBER(19,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruprltmqueu_1.","queu_lngt"," IS ","'대기행렬길이 (meter)'",";",null,""]
[7,"대기행렬대수","queu_trcn",null,"NULL","NUMBER(5)",null,"NUMBER(5)",5,"대기행렬대수",{"$nulls":13},"queu_trcn ","NUMBER(5) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruprltmqueu_1.","queu_trcn"," IS ","'대기행렬대수'",";",null,""]
[8,"공간점유율","spae_ocpn_rt",null,"NULL","NUMBER(13,9)",null,"NUMBER(13,9)","12,9","공간점유율 (차량길이/세그먼트길이)",{"$nulls":13},"spae_ocpn_rt ","NUMBER(13,9) ","",{"$f":"\") TABLESPACE \"&AB397&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_T003 NOLOGGING"},{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruprltmqueu_1.","spae_ocpn_rt"," IS ","'공간점유율 (차량길이/세그먼트길이)'",";",null,""]
[{"$nulls":23},{"$f":"CONCATENATE(AB396:AD396)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (clct_unix_tm) INTERVAL (3600) STORE IN (\"&AB397&\") (PARTITION BFR_\" & A387& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AB397&\");\"","v":"PARTITION BY RANGE (clct_unix_tm) INTERVAL (3600) STORE IN (SOIT_D08_T003) (PARTITION BFR_soitcedgegruprltmqueu_1_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_T003);"},{"$f":"\"CREATE INDEX PK_\" & A387& \" ON \" & A387 & CONCATENATE(AC389:AE394) & \" LOCAL (PARTITION BFR_\" & A387 & \"_20221101 TABLESPACE \"&AC397&\") TABLESPACE \"&AC397&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & A387 & \" ADD CONSTRAINT PK_\" & A387 & \" PRIMARY KEY \" & CONCATENATE(AC389:AE394) & \";\"","v":{"$error":"#VALUE!"}}]
["엣지그룹별 실시간 대기행렬/공간점유율 테이블 - 2지역",{"$nulls":26},"SOIT_D08_T003","SOIT_I08_T003",{"$nulls":9},{"$f":"IF(LEFT(X397, 13) = \"CONSTRAINT PK\", X397, \"\")","v":""}]
["soitcedgegruprltmqueu_2",{"$nulls":10},{"$f":"LEN(A398)","v":23},{"$nulls":26},""]
["NO","속성명","컬럼명","PK/FK","NULL","형태",null,"TIBERO","길이","비고",{"$nulls":21},"COMMENT ON TABLE",{"$f":"A398&\" \"","v":"soitcedgegruprltmqueu_2 "},null," IS ",{"$f":"\"'\"&SUBSTITUTE(A397,\"테이블\",\"\")&\"'\"","v":"'엣지그룹별 실시간 대기행렬/공간점유율  - 2지역'"},";",null,""]
[1,"엣지그룹ID","edge_grup_id","PK/FK","NOT NULL","VARCHAR2(300)",null,"VARCHAR2(300)",20,"엣지그룹ID",{"$nulls":11},"CREATE TABLE ",{"$f":"A398&\" (\"","v":"soitcedgegruprltmqueu_2 ("},{"$f":"C400&\" \"","v":"edge_grup_id "},{"$f":"H400&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(E400=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(D400=\"PK\", D400=\"PK/FK\"), C400, \"\")","v":"edge_grup_id"},{"$f":"IF(OR(D400=\"PK\", D400=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$A$398&\".\"","v":"soitcedgegruprltmqueu_2."},{"$f":"C400","v":"edge_grup_id"}," IS ",{"$f":"\"'\"&J400&\"'\"","v":"'엣지그룹ID'"},";",null,""]
[3,"차로번호","lane_no","PK","NOT NULL","NUMBER(2)",null,"NUMBER(2)",2,"차로번호",{"$nulls":13},"lane_no ","NUMBER(2) ","NOT NULL",",",null,null,"lane_no",",","COMMENT ON COLUMN ","soitcedgegruprltmqueu_2.","lane_no"," IS ","'차로번호'",";",null,""]
[4,"실측여부","acsr_yn","PK","NOT NULL","CHAR(1)",null,"VARCHAR2(1)",1,"실측여부 (500) (실시간만 예측있음)",{"$nulls":13},"acsr_yn ","VARCHAR2(1) ","NOT NULL",",",null,null,"acsr_yn",",","COMMENT ON COLUMN ","soitcedgegruprltmqueu_2.","acsr_yn"," IS ","'실측여부 (500) (실시간만 예측있음)'",";",null,""]
[5,"수집유닉스시각","clct_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"수집유닉스시각",{"$nulls":13},"clct_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"clct_unix_tm",")","COMMENT ON COLUMN ","soitcedgegruprltmqueu_2.","clct_unix_tm"," IS ","'수집유닉스시각'",";",null,""]
[6,"대기행렬길이","queu_lngt",null,"NULL","NUMBER(19,9)",null,"NUMBER(19,9)","19,9","대기행렬길이 (meter)",{"$nulls":13},"queu_lngt ","NUMBER(19,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruprltmqueu_2.","queu_lngt"," IS ","'대기행렬길이 (meter)'",";",null,""]
[7,"대기행렬대수","queu_trcn",null,"NULL","NUMBER(5)",null,"NUMBER(5)",5,"대기행렬대수",{"$nulls":13},"queu_trcn ","NUMBER(5) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruprltmqueu_2.","queu_trcn"," IS ","'대기행렬대수'",";",null,""]
[8,"공간점유율","spae_ocpn_rt",null,"NULL","NUMBER(13,9)",null,"NUMBER(13,9)","12,9","공간점유율 (차량길이/세그먼트길이)",{"$nulls":13},"spae_ocpn_rt ","NUMBER(13,9) ","",{"$f":"\") TABLESPACE \"&AB408&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_T003 NOLOGGING"},{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruprltmqueu_2.","spae_ocpn_rt"," IS ","'공간점유율 (차량길이/세그먼트길이)'",";",null,""]
[{"$nulls":23},{"$f":"CONCATENATE(AB407:AD407)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (clct_unix_tm) INTERVAL (3600) STORE IN (\"&AB408&\") (PARTITION BFR_\" & A398& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AB408&\");\"","v":"PARTITION BY RANGE (clct_unix_tm) INTERVAL (3600) STORE IN (SOIT_D08_T003) (PARTITION BFR_soitcedgegruprltmqueu_2_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_T003);"},{"$f":"\"CREATE INDEX PK_\" & A398& \" ON \" & A398 & CONCATENATE(AC400:AE405) & \" LOCAL (PARTITION BFR_\" & A398 & \"_20221101 TABLESPACE \"&AC408&\") TABLESPACE \"&AC408&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & A398 & \" ADD CONSTRAINT PK_\" & A398 & \" PRIMARY KEY \" & CONCATENATE(AC400:AE405) & \";\"","v":{"$error":"#VALUE!"}}]
["엣지그룹별 실시간 대기행렬/공간점유율 테이블 - 1지역",{"$nulls":26},"SOIT_D08_T003","SOIT_I08_T003",{"$nulls":9},{"$f":"IF(LEFT(X408, 13) = \"CONSTRAINT PK\", X408, \"\")","v":""}]
["soitcedgegruprltmqueu_3",{"$nulls":10},{"$f":"LEN(A409)","v":23},{"$nulls":26},""]
["NO","속성명","컬럼명","PK/FK","NULL","형태",null,"TIBERO","길이","비고",{"$nulls":21},"COMMENT ON TABLE",{"$f":"A409&\" \"","v":"soitcedgegruprltmqueu_3 "},null," IS ",{"$f":"\"'\"&SUBSTITUTE(A408,\"테이블\",\"\")&\"'\"","v":"'엣지그룹별 실시간 대기행렬/공간점유율  - 1지역'"},";",null,""]
[1,"엣지그룹ID","edge_grup_id","PK/FK","NOT NULL","VARCHAR2(300)",null,"VARCHAR2(300)",20,"엣지그룹ID",{"$nulls":11},"CREATE TABLE ",{"$f":"A409&\" (\"","v":"soitcedgegruprltmqueu_3 ("},{"$f":"C411&\" \"","v":"edge_grup_id "},{"$f":"H411&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(E411=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(D411=\"PK\", D411=\"PK/FK\"), C411, \"\")","v":"edge_grup_id"},{"$f":"IF(OR(D411=\"PK\", D411=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$A$409&\".\"","v":"soitcedgegruprltmqueu_3."},{"$f":"C411","v":"edge_grup_id"}," IS ",{"$f":"\"'\"&J411&\"'\"","v":"'엣지그룹ID'"},";",null,""]
[3,"차로번호","lane_no","PK","NOT NULL","NUMBER(2)",null,"NUMBER(2)",2,"차로번호",{"$nulls":13},"lane_no ","NUMBER(2) ","NOT NULL",",",null,null,"lane_no",",","COMMENT ON COLUMN ","soitcedgegruprltmqueu_3.","lane_no"," IS ","'차로번호'",";",null,""]
[4,"실측여부","acsr_yn","PK","NOT NULL","CHAR(1)",null,"VARCHAR2(1)",1,"실측여부 (500) (실시간만 예측있음)",{"$nulls":13},"acsr_yn ","VARCHAR2(1) ","NOT NULL",",",null,null,"acsr_yn",",","COMMENT ON COLUMN ","soitcedgegruprltmqueu_3.","acsr_yn"," IS ","'실측여부 (500) (실시간만 예측있음)'",";",null,""]
[5,"수집유닉스시각","clct_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"수집유닉스시각",{"$nulls":13},"clct_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"clct_unix_tm",")","COMMENT ON COLUMN ","soitcedgegruprltmqueu_3.","clct_unix_tm"," IS ","'수집유닉스시각'",";",null,""]
[6,"대기행렬길이","queu_lngt",null,"NULL","NUMBER(19,9)",null,"NUMBER(19,9)","19,9","대기행렬길이 (meter)",{"$nulls":13},"queu_lngt ","NUMBER(19,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruprltmqueu_3.","queu_lngt"," IS ","'대기행렬길이 (meter)'",";",null,""]
[7,"대기행렬대수","queu_trcn",null,"NULL","NUMBER(5)",null,"NUMBER(5)",5,"대기행렬대수",{"$nulls":13},"queu_trcn ","NUMBER(5) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruprltmqueu_3.","queu_trcn"," IS ","'대기행렬대수'",";",null,""]
[8,"공간점유율","spae_ocpn_rt",null,"NULL","NUMBER(13,9)",null,"NUMBER(13,9)","12,9","공간점유율 (차량길이/세그먼트길이)",{"$nulls":13},"spae_ocpn_rt ","NUMBER(13,9) ","",{"$f":"\") TABLESPACE \"&AB419&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_T003 NOLOGGING"},{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruprltmqueu_3.","spae_ocpn_rt"," IS ","'공간점유율 (차량길이/세그먼트길이)'",";",null,""]
[{"$nulls":23},{"$f":"CONCATENATE(AB418:AD418)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (clct_unix_tm) INTERVAL (3600) STORE IN (\"&AB419&\") (PARTITION BFR_\" & A409& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AB419&\");\"","v":"PARTITION BY RANGE (clct_unix_tm) INTERVAL (3600) STORE IN (SOIT_D08_T003) (PARTITION BFR_soitcedgegruprltmqueu_3_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_T003);"},{"$f":"\"CREATE INDEX PK_\" & A409& \" ON \" & A409 & CONCATENATE(AC411:AE416) & \" LOCAL (PARTITION BFR_\" & A409 & \"_20221101 TABLESPACE \"&AC419&\") TABLESPACE \"&AC419&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & A409 & \" ADD CONSTRAINT PK_\" & A409 & \" PRIMARY KEY \" & CONCATENATE(AC411:AE416) & \";\"","v":{"$error":"#VALUE!"}}]
["엣지그룹별 실시간 대기행렬/공간점유율 테이블 - 4지역",{"$nulls":26},"SOIT_D08_T003","SOIT_I08_T003",{"$nulls":9},{"$f":"IF(LEFT(X419, 13) = \"CONSTRAINT PK\", X419, \"\")","v":""}]
["soitcedgegruprltmqueu_4",{"$nulls":10},{"$f":"LEN(A420)","v":23},{"$nulls":26},""]
["NO","속성명","컬럼명","PK/FK","NULL","형태",null,"TIBERO","길이","비고",{"$nulls":21},"COMMENT ON TABLE",{"$f":"A420&\" \"","v":"soitcedgegruprltmqueu_4 "},null," IS ",{"$f":"\"'\"&SUBSTITUTE(A419,\"테이블\",\"\")&\"'\"","v":"'엣지그룹별 실시간 대기행렬/공간점유율  - 4지역'"},";",null,""]
[1,"엣지그룹ID","edge_grup_id","PK/FK","NOT NULL","VARCHAR2(300)",null,"VARCHAR2(300)",20,"엣지그룹ID",{"$nulls":11},"CREATE TABLE ",{"$f":"A420&\" (\"","v":"soitcedgegruprltmqueu_4 ("},{"$f":"C422&\" \"","v":"edge_grup_id "},{"$f":"H422&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(E422=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(D422=\"PK\", D422=\"PK/FK\"), C422, \"\")","v":"edge_grup_id"},{"$f":"IF(OR(D422=\"PK\", D422=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$A$420&\".\"","v":"soitcedgegruprltmqueu_4."},{"$f":"C422","v":"edge_grup_id"}," IS ",{"$f":"\"'\"&J422&\"'\"","v":"'엣지그룹ID'"},";",null,""]
[3,"차로번호","lane_no","PK","NOT NULL","NUMBER(2)",null,"NUMBER(2)",2,"차로번호",{"$nulls":13},"lane_no ","NUMBER(2) ","NOT NULL",",",null,null,"lane_no",",","COMMENT ON COLUMN ","soitcedgegruprltmqueu_4.","lane_no"," IS ","'차로번호'",";",null,""]
[4,"실측여부","acsr_yn","PK","NOT NULL","CHAR(1)",null,"VARCHAR2(1)",1,"실측여부 (500) (실시간만 예측있음)",{"$nulls":13},"acsr_yn ","VARCHAR2(1) ","NOT NULL",",",null,null,"acsr_yn",",","COMMENT ON COLUMN ","soitcedgegruprltmqueu_4.","acsr_yn"," IS ","'실측여부 (500) (실시간만 예측있음)'",";",null,""]
[5,"수집유닉스시각","clct_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"수집유닉스시각",{"$nulls":13},"clct_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"clct_unix_tm",")","COMMENT ON COLUMN ","soitcedgegruprltmqueu_4.","clct_unix_tm"," IS ","'수집유닉스시각'",";",null,""]
[6,"대기행렬길이","queu_lngt",null,"NULL","NUMBER(19,9)",null,"NUMBER(19,9)","19,9","대기행렬길이 (meter)",{"$nulls":13},"queu_lngt ","NUMBER(19,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruprltmqueu_4.","queu_lngt"," IS ","'대기행렬길이 (meter)'",";",null,""]
[7,"대기행렬대수","queu_trcn",null,"NULL","NUMBER(5)",null,"NUMBER(5)",5,"대기행렬대수",{"$nulls":13},"queu_trcn ","NUMBER(5) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruprltmqueu_4.","queu_trcn"," IS ","'대기행렬대수'",";",null,""]
[8,"공간점유율","spae_ocpn_rt",null,"NULL","NUMBER(13,9)",null,"NUMBER(13,9)","12,9","공간점유율 (차량길이/세그먼트길이)",{"$nulls":13},"spae_ocpn_rt ","NUMBER(13,9) ","",{"$f":"\") TABLESPACE \"&AB430&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_T003 NOLOGGING"},{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruprltmqueu_4.","spae_ocpn_rt"," IS ","'공간점유율 (차량길이/세그먼트길이)'",";",null,""]
[{"$nulls":23},{"$f":"CONCATENATE(AB429:AD429)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (clct_unix_tm) INTERVAL (3600) STORE IN (\"&AB430&\") (PARTITION BFR_\" & A420& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AB430&\");\"","v":"PARTITION BY RANGE (clct_unix_tm) INTERVAL (3600) STORE IN (SOIT_D08_T003) (PARTITION BFR_soitcedgegruprltmqueu_4_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_T003);"},{"$f":"\"CREATE INDEX PK_\" & A420& \" ON \" & A420 & CONCATENATE(AC422:AE427) & \" LOCAL (PARTITION BFR_\" & A420 & \"_20221101 TABLESPACE \"&AC430&\") TABLESPACE \"&AC430&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & A420 & \" ADD CONSTRAINT PK_\" & A420 & \" PRIMARY KEY \" & CONCATENATE(AC422:AE427) & \";\"","v":{"$error":"#VALUE!"}}]
["엣지그룹별 실시간 대기행렬/공간점유율 테이블 - 5지역",{"$nulls":26},"SOIT_D08_T003","SOIT_I08_T003",{"$nulls":9},{"$f":"IF(LEFT(X430, 13) = \"CONSTRAINT PK\", X430, \"\")","v":""}]
["soitcedgegruprltmqueu_5",{"$nulls":10},{"$f":"LEN(A431)","v":23},{"$nulls":26},""]
["NO","속성명","컬럼명","PK/FK","NULL","형태",null,"TIBERO","길이","비고",{"$nulls":21},"COMMENT ON TABLE",{"$f":"A431&\" \"","v":"soitcedgegruprltmqueu_5 "},null," IS ",{"$f":"\"'\"&SUBSTITUTE(A430,\"테이블\",\"\")&\"'\"","v":"'엣지그룹별 실시간 대기행렬/공간점유율  - 5지역'"},";",null,""]
[1,"엣지그룹ID","edge_grup_id","PK/FK","NOT NULL","VARCHAR2(300)",null,"VARCHAR2(300)",20,"엣지그룹ID",{"$nulls":11},"CREATE TABLE ",{"$f":"A431&\" (\"","v":"soitcedgegruprltmqueu_5 ("},{"$f":"C433&\" \"","v":"edge_grup_id "},{"$f":"H433&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(E433=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(D433=\"PK\", D433=\"PK/FK\"), C433, \"\")","v":"edge_grup_id"},{"$f":"IF(OR(D433=\"PK\", D433=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$A$431&\".\"","v":"soitcedgegruprltmqueu_5."},{"$f":"C433","v":"edge_grup_id"}," IS ",{"$f":"\"'\"&J433&\"'\"","v":"'엣지그룹ID'"},";",null,""]
[3,"차로번호","lane_no","PK","NOT NULL","NUMBER(2)",null,"NUMBER(2)",2,"차로번호",{"$nulls":13},"lane_no ","NUMBER(2) ","NOT NULL",",",null,null,"lane_no",",","COMMENT ON COLUMN ","soitcedgegruprltmqueu_5.","lane_no"," IS ","'차로번호'",";",null,""]
[4,"실측여부","acsr_yn","PK","NOT NULL","CHAR(1)",null,"VARCHAR2(1)",1,"실측여부 (500) (실시간만 예측있음)",{"$nulls":13},"acsr_yn ","VARCHAR2(1) ","NOT NULL",",",null,null,"acsr_yn",",","COMMENT ON COLUMN ","soitcedgegruprltmqueu_5.","acsr_yn"," IS ","'실측여부 (500) (실시간만 예측있음)'",";",null,""]
[5,"수집유닉스시각","clct_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"수집유닉스시각",{"$nulls":13},"clct_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"clct_unix_tm",")","COMMENT ON COLUMN ","soitcedgegruprltmqueu_5.","clct_unix_tm"," IS ","'수집유닉스시각'",";",null,""]
[6,"대기행렬길이","queu_lngt",null,"NULL","NUMBER(19,9)",null,"NUMBER(19,9)","19,9","대기행렬길이 (meter)",{"$nulls":13},"queu_lngt ","NUMBER(19,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruprltmqueu_5.","queu_lngt"," IS ","'대기행렬길이 (meter)'",";",null,""]
[7,"대기행렬대수","queu_trcn",null,"NULL","NUMBER(5)",null,"NUMBER(5)",5,"대기행렬대수",{"$nulls":13},"queu_trcn ","NUMBER(5) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruprltmqueu_5.","queu_trcn"," IS ","'대기행렬대수'",";",null,""]
[8,"공간점유율","spae_ocpn_rt",null,"NULL","NUMBER(13,9)",null,"NUMBER(13,9)","12,9","공간점유율 (차량길이/세그먼트길이)",{"$nulls":13},"spae_ocpn_rt ","NUMBER(13,9) ","",{"$f":"\") TABLESPACE \"&AB441&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_T003 NOLOGGING"},{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruprltmqueu_5.","spae_ocpn_rt"," IS ","'공간점유율 (차량길이/세그먼트길이)'",";",null,""]
[{"$nulls":23},{"$f":"CONCATENATE(AB440:AD440)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (clct_unix_tm) INTERVAL (3600) STORE IN (\"&AB441&\") (PARTITION BFR_\" & A431& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AB441&\");\"","v":"PARTITION BY RANGE (clct_unix_tm) INTERVAL (3600) STORE IN (SOIT_D08_T003) (PARTITION BFR_soitcedgegruprltmqueu_5_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_T003);"},{"$f":"\"CREATE INDEX PK_\" & A431& \" ON \" & A431 & CONCATENATE(AC433:AE438) & \" LOCAL (PARTITION BFR_\" & A431 & \"_20221101 TABLESPACE \"&AC441&\") TABLESPACE \"&AC441&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & A431 & \" ADD CONSTRAINT PK_\" & A431 & \" PRIMARY KEY \" & CONCATENATE(AC433:AE438) & \";\"","v":{"$error":"#VALUE!"}}]
["엣지그룹별 실시간 대기행렬/공간점유율 테이블 - 6지역",{"$nulls":26},"SOIT_D08_T003","SOIT_I08_T003",{"$nulls":9},{"$f":"IF(LEFT(X441, 13) = \"CONSTRAINT PK\", X441, \"\")","v":""}]
["soitcedgegruprltmqueu_6",{"$nulls":10},{"$f":"LEN(A442)","v":23},{"$nulls":26},""]
["NO","속성명","컬럼명","PK/FK","NULL","형태",null,"TIBERO","길이","비고",{"$nulls":21},"COMMENT ON TABLE",{"$f":"A442&\" \"","v":"soitcedgegruprltmqueu_6 "},null," IS ",{"$f":"\"'\"&SUBSTITUTE(A441,\"테이블\",\"\")&\"'\"","v":"'엣지그룹별 실시간 대기행렬/공간점유율  - 6지역'"},";",null,""]
[1,"엣지그룹ID","edge_grup_id","PK/FK","NOT NULL","VARCHAR2(300)",null,"VARCHAR2(300)",20,"엣지그룹ID",{"$nulls":11},"CREATE TABLE ",{"$f":"A442&\" (\"","v":"soitcedgegruprltmqueu_6 ("},{"$f":"C444&\" \"","v":"edge_grup_id "},{"$f":"H444&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(E444=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(D444=\"PK\", D444=\"PK/FK\"), C444, \"\")","v":"edge_grup_id"},{"$f":"IF(OR(D444=\"PK\", D444=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$A$442&\".\"","v":"soitcedgegruprltmqueu_6."},{"$f":"C444","v":"edge_grup_id"}," IS ",{"$f":"\"'\"&J444&\"'\"","v":"'엣지그룹ID'"},";",null,""]
[3,"차로번호","lane_no","PK","NOT NULL","NUMBER(2)",null,"NUMBER(2)",2,"차로번호",{"$nulls":13},"lane_no ","NUMBER(2) ","NOT NULL",",",null,null,"lane_no",",","COMMENT ON COLUMN ","soitcedgegruprltmqueu_6.","lane_no"," IS ","'차로번호'",";",null,""]
[4,"실측여부","acsr_yn","PK","NOT NULL","CHAR(1)",null,"VARCHAR2(1)",1,"실측여부 (500) (실시간만 예측있음)",{"$nulls":13},"acsr_yn ","VARCHAR2(1) ","NOT NULL",",",null,null,"acsr_yn",",","COMMENT ON COLUMN ","soitcedgegruprltmqueu_6.","acsr_yn"," IS ","'실측여부 (500) (실시간만 예측있음)'",";",null,""]
[5,"수집유닉스시각","clct_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"수집유닉스시각",{"$nulls":13},"clct_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"clct_unix_tm",")","COMMENT ON COLUMN ","soitcedgegruprltmqueu_6.","clct_unix_tm"," IS ","'수집유닉스시각'",";",null,""]
[6,"대기행렬길이","queu_lngt",null,"NULL","NUMBER(19,9)",null,"NUMBER(19,9)","19,9","대기행렬길이 (meter)",{"$nulls":13},"queu_lngt ","NUMBER(19,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruprltmqueu_6.","queu_lngt"," IS ","'대기행렬길이 (meter)'",";",null,""]
[7,"대기행렬대수","queu_trcn",null,"NULL","NUMBER(5)",null,"NUMBER(5)",5,"대기행렬대수",{"$nulls":13},"queu_trcn ","NUMBER(5) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruprltmqueu_6.","queu_trcn"," IS ","'대기행렬대수'",";",null,""]
[8,"공간점유율","spae_ocpn_rt",null,"NULL","NUMBER(13,9)",null,"NUMBER(13,9)","12,9","공간점유율 (차량길이/세그먼트길이)",{"$nulls":13},"spae_ocpn_rt ","NUMBER(13,9) ","",{"$f":"\") TABLESPACE \"&AB452&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_T003 NOLOGGING"},{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruprltmqueu_6.","spae_ocpn_rt"," IS ","'공간점유율 (차량길이/세그먼트길이)'",";",null,""]
[{"$nulls":23},{"$f":"CONCATENATE(AB451:AD451)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (clct_unix_tm) INTERVAL (3600) STORE IN (\"&AB452&\") (PARTITION BFR_\" & A442& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AB452&\");\"","v":"PARTITION BY RANGE (clct_unix_tm) INTERVAL (3600) STORE IN (SOIT_D08_T003) (PARTITION BFR_soitcedgegruprltmqueu_6_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_T003);"},{"$f":"\"CREATE INDEX PK_\" & A442& \" ON \" & A442 & CONCATENATE(AC444:AE449) & \" LOCAL (PARTITION BFR_\" & A442 & \"_20221101 TABLESPACE \"&AC452&\") TABLESPACE \"&AC452&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & A442 & \" ADD CONSTRAINT PK_\" & A442 & \" PRIMARY KEY \" & CONCATENATE(AC444:AE449) & \";\"","v":{"$error":"#VALUE!"}}]
["엣지그룹별 실시간 대기행렬/공간점유율 테이블 - 7지역",{"$nulls":26},"SOIT_D08_T003","SOIT_I08_T003",{"$nulls":9},{"$f":"IF(LEFT(X452, 13) = \"CONSTRAINT PK\", X452, \"\")","v":""}]
["soitcedgegruprltmqueu_7",{"$nulls":10},{"$f":"LEN(A453)","v":23},{"$nulls":26},""]
["NO","속성명","컬럼명","PK/FK","NULL","형태",null,"TIBERO","길이","비고",{"$nulls":21},"COMMENT ON TABLE",{"$f":"A453&\" \"","v":"soitcedgegruprltmqueu_7 "},null," IS ",{"$f":"\"'\"&SUBSTITUTE(A452,\"테이블\",\"\")&\"'\"","v":"'엣지그룹별 실시간 대기행렬/공간점유율  - 7지역'"},";",null,""]
[1,"엣지그룹ID","edge_grup_id","PK/FK","NOT NULL","VARCHAR2(300)",null,"VARCHAR2(300)",20,"엣지그룹ID",{"$nulls":11},"CREATE TABLE ",{"$f":"A453&\" (\"","v":"soitcedgegruprltmqueu_7 ("},{"$f":"C455&\" \"","v":"edge_grup_id "},{"$f":"H455&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(E455=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(D455=\"PK\", D455=\"PK/FK\"), C455, \"\")","v":"edge_grup_id"},{"$f":"IF(OR(D455=\"PK\", D455=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$A$453&\".\"","v":"soitcedgegruprltmqueu_7."},{"$f":"C455","v":"edge_grup_id"}," IS ",{"$f":"\"'\"&J455&\"'\"","v":"'엣지그룹ID'"},";",null,""]
[3,"차로번호","lane_no","PK","NOT NULL","NUMBER(2)",null,"NUMBER(2)",2,"차로번호",{"$nulls":13},"lane_no ","NUMBER(2) ","NOT NULL",",",null,null,"lane_no",",","COMMENT ON COLUMN ","soitcedgegruprltmqueu_7.","lane_no"," IS ","'차로번호'",";",null,""]
[4,"실측여부","acsr_yn","PK","NOT NULL","CHAR(1)",null,"VARCHAR2(1)",1,"실측여부 (500) (실시간만 예측있음)",{"$nulls":13},"acsr_yn ","VARCHAR2(1) ","NOT NULL",",",null,null,"acsr_yn",",","COMMENT ON COLUMN ","soitcedgegruprltmqueu_7.","acsr_yn"," IS ","'실측여부 (500) (실시간만 예측있음)'",";",null,""]
[5,"수집유닉스시각","clct_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"수집유닉스시각",{"$nulls":13},"clct_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"clct_unix_tm",")","COMMENT ON COLUMN ","soitcedgegruprltmqueu_7.","clct_unix_tm"," IS ","'수집유닉스시각'",";",null,""]
[6,"대기행렬길이","queu_lngt",null,"NULL","NUMBER(19,9)",null,"NUMBER(19,9)","19,9","대기행렬길이 (meter)",{"$nulls":13},"queu_lngt ","NUMBER(19,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruprltmqueu_7.","queu_lngt"," IS ","'대기행렬길이 (meter)'",";",null,""]
[7,"대기행렬대수","queu_trcn",null,"NULL","NUMBER(5)",null,"NUMBER(5)",5,"대기행렬대수",{"$nulls":13},"queu_trcn ","NUMBER(5) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruprltmqueu_7.","queu_trcn"," IS ","'대기행렬대수'",";",null,""]
[8,"공간점유율","spae_ocpn_rt",null,"NULL","NUMBER(13,9)",null,"NUMBER(13,9)","12,9","공간점유율 (차량길이/세그먼트길이)",{"$nulls":13},"spae_ocpn_rt ","NUMBER(13,9) ","",{"$f":"\") TABLESPACE \"&AB463&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_T003 NOLOGGING"},{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruprltmqueu_7.","spae_ocpn_rt"," IS ","'공간점유율 (차량길이/세그먼트길이)'",";",null,""]
[{"$nulls":23},{"$f":"CONCATENATE(AB462:AD462)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (clct_unix_tm) INTERVAL (3600) STORE IN (\"&AB463&\") (PARTITION BFR_\" & A453& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AB463&\");\"","v":"PARTITION BY RANGE (clct_unix_tm) INTERVAL (3600) STORE IN (SOIT_D08_T003) (PARTITION BFR_soitcedgegruprltmqueu_7_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_T003);"},{"$f":"\"CREATE INDEX PK_\" & A453& \" ON \" & A453 & CONCATENATE(AC455:AE460) & \" LOCAL (PARTITION BFR_\" & A453 & \"_20221101 TABLESPACE \"&AC463&\") TABLESPACE \"&AC463&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & A453 & \" ADD CONSTRAINT PK_\" & A453 & \" PRIMARY KEY \" & CONCATENATE(AC455:AE460) & \";\"","v":{"$error":"#VALUE!"}}]
["엣지그룹별 실시간 대기행렬/공간점유율 테이블 - 8지역",{"$nulls":26},"SOIT_D08_T003","SOIT_I08_T003",{"$nulls":9},{"$f":"IF(LEFT(X463, 13) = \"CONSTRAINT PK\", X463, \"\")","v":""}]
["soitcedgegruprltmqueu_8",{"$nulls":10},{"$f":"LEN(A464)","v":23},{"$nulls":26},""]
["NO","속성명","컬럼명","PK/FK","NULL","형태",null,"TIBERO","길이","비고",{"$nulls":21},"COMMENT ON TABLE",{"$f":"A464&\" \"","v":"soitcedgegruprltmqueu_8 "},null," IS ",{"$f":"\"'\"&SUBSTITUTE(A463,\"테이블\",\"\")&\"'\"","v":"'엣지그룹별 실시간 대기행렬/공간점유율  - 8지역'"},";",null,""]
[1,"엣지그룹ID","edge_grup_id","PK/FK","NOT NULL","VARCHAR2(300)",null,"VARCHAR2(300)",20,"엣지그룹ID",{"$nulls":11},"CREATE TABLE ",{"$f":"A464&\" (\"","v":"soitcedgegruprltmqueu_8 ("},{"$f":"C466&\" \"","v":"edge_grup_id "},{"$f":"H466&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(E466=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(D466=\"PK\", D466=\"PK/FK\"), C466, \"\")","v":"edge_grup_id"},{"$f":"IF(OR(D466=\"PK\", D466=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$A$464&\".\"","v":"soitcedgegruprltmqueu_8."},{"$f":"C466","v":"edge_grup_id"}," IS ",{"$f":"\"'\"&J466&\"'\"","v":"'엣지그룹ID'"},";",null,""]
[3,"차로번호","lane_no","PK","NOT NULL","NUMBER(2)",null,"NUMBER(2)",2,"차로번호",{"$nulls":13},"lane_no ","NUMBER(2) ","NOT NULL",",",null,null,"lane_no",",","COMMENT ON COLUMN ","soitcedgegruprltmqueu_8.","lane_no"," IS ","'차로번호'",";",null,""]
[4,"실측여부","acsr_yn","PK","NOT NULL","CHAR(1)",null,"VARCHAR2(1)",1,"실측여부 (500) (실시간만 예측있음)",{"$nulls":13},"acsr_yn ","VARCHAR2(1) ","NOT NULL",",",null,null,"acsr_yn",",","COMMENT ON COLUMN ","soitcedgegruprltmqueu_8.","acsr_yn"," IS ","'실측여부 (500) (실시간만 예측있음)'",";",null,""]
[5,"수집유닉스시각","clct_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"수집유닉스시각",{"$nulls":13},"clct_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"clct_unix_tm",")","COMMENT ON COLUMN ","soitcedgegruprltmqueu_8.","clct_unix_tm"," IS ","'수집유닉스시각'",";",null,""]
[6,"대기행렬길이","queu_lngt",null,"NULL","NUMBER(19,9)",null,"NUMBER(19,9)","19,9","대기행렬길이 (meter)",{"$nulls":13},"queu_lngt ","NUMBER(19,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruprltmqueu_8.","queu_lngt"," IS ","'대기행렬길이 (meter)'",";",null,""]
[7,"대기행렬대수","queu_trcn",null,"NULL","NUMBER(5)",null,"NUMBER(5)",5,"대기행렬대수",{"$nulls":13},"queu_trcn ","NUMBER(5) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruprltmqueu_8.","queu_trcn"," IS ","'대기행렬대수'",";",null,""]
[8,"공간점유율","spae_ocpn_rt",null,"NULL","NUMBER(13,9)",null,"NUMBER(13,9)","12,9","공간점유율 (차량길이/세그먼트길이)",{"$nulls":13},"spae_ocpn_rt ","NUMBER(13,9) ","",{"$f":"\") TABLESPACE \"&AB474&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_T003 NOLOGGING"},{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruprltmqueu_8.","spae_ocpn_rt"," IS ","'공간점유율 (차량길이/세그먼트길이)'",";",null,""]
[{"$nulls":23},{"$f":"CONCATENATE(AB473:AD473)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (clct_unix_tm) INTERVAL (3600) STORE IN (\"&AB474&\") (PARTITION BFR_\" & A464& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AB474&\");\"","v":"PARTITION BY RANGE (clct_unix_tm) INTERVAL (3600) STORE IN (SOIT_D08_T003) (PARTITION BFR_soitcedgegruprltmqueu_8_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_T003);"},{"$f":"\"CREATE INDEX PK_\" & A464& \" ON \" & A464 & CONCATENATE(AC466:AE471) & \" LOCAL (PARTITION BFR_\" & A464 & \"_20221101 TABLESPACE \"&AC474&\") TABLESPACE \"&AC474&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & A464 & \" ADD CONSTRAINT PK_\" & A464 & \" PRIMARY KEY \" & CONCATENATE(AC466:AE471) & \";\"","v":{"$error":"#VALUE!"}}]
["엣지그룹별 실시간 대기행렬/공간점유율 테이블 - 9지역",{"$nulls":26},"SOIT_D08_T003","SOIT_I08_T003",{"$nulls":9},{"$f":"IF(LEFT(X474, 13) = \"CONSTRAINT PK\", X474, \"\")","v":""}]
["soitcedgegruprltmqueu_9",{"$nulls":10},{"$f":"LEN(A475)","v":23},{"$nulls":26},""]
["NO","속성명","컬럼명","PK/FK","NULL","형태",null,"TIBERO","길이","비고",{"$nulls":21},"COMMENT ON TABLE",{"$f":"A475&\" \"","v":"soitcedgegruprltmqueu_9 "},null," IS ",{"$f":"\"'\"&SUBSTITUTE(A474,\"테이블\",\"\")&\"'\"","v":"'엣지그룹별 실시간 대기행렬/공간점유율  - 9지역'"},";",null,""]
[1,"엣지그룹ID","edge_grup_id","PK/FK","NOT NULL","VARCHAR2(300)",null,"VARCHAR2(300)",20,"엣지그룹ID",{"$nulls":11},"CREATE TABLE ",{"$f":"A475&\" (\"","v":"soitcedgegruprltmqueu_9 ("},{"$f":"C477&\" \"","v":"edge_grup_id "},{"$f":"H477&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(E477=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(D477=\"PK\", D477=\"PK/FK\"), C477, \"\")","v":"edge_grup_id"},{"$f":"IF(OR(D477=\"PK\", D477=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$A$475&\".\"","v":"soitcedgegruprltmqueu_9."},{"$f":"C477","v":"edge_grup_id"}," IS ",{"$f":"\"'\"&J477&\"'\"","v":"'엣지그룹ID'"},";",null,""]
[3,"차로번호","lane_no","PK","NOT NULL","NUMBER(2)",null,"NUMBER(2)",2,"차로번호",{"$nulls":13},"lane_no ","NUMBER(2) ","NOT NULL",",",null,null,"lane_no",",","COMMENT ON COLUMN ","soitcedgegruprltmqueu_9.","lane_no"," IS ","'차로번호'",";",null,""]
[4,"실측여부","acsr_yn","PK","NOT NULL","CHAR(1)",null,"VARCHAR2(1)",1,"실측여부 (500) (실시간만 예측있음)",{"$nulls":13},"acsr_yn ","VARCHAR2(1) ","NOT NULL",",",null,null,"acsr_yn",",","COMMENT ON COLUMN ","soitcedgegruprltmqueu_9.","acsr_yn"," IS ","'실측여부 (500) (실시간만 예측있음)'",";",null,""]
[5,"수집유닉스시각","clct_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"수집유닉스시각",{"$nulls":13},"clct_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"clct_unix_tm",")","COMMENT ON COLUMN ","soitcedgegruprltmqueu_9.","clct_unix_tm"," IS ","'수집유닉스시각'",";",null,""]
[6,"대기행렬길이","queu_lngt",null,"NULL","NUMBER(19,9)",null,"NUMBER(19,9)","19,9","대기행렬길이 (meter)",{"$nulls":13},"queu_lngt ","NUMBER(19,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruprltmqueu_9.","queu_lngt"," IS ","'대기행렬길이 (meter)'",";",null,""]
[7,"대기행렬대수","queu_trcn",null,"NULL","NUMBER(5)",null,"NUMBER(5)",5,"대기행렬대수",{"$nulls":13},"queu_trcn ","NUMBER(5) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruprltmqueu_9.","queu_trcn"," IS ","'대기행렬대수'",";",null,""]
[8,"공간점유율","spae_ocpn_rt",null,"NULL","NUMBER(13,9)",null,"NUMBER(13,9)","12,9","공간점유율 (차량길이/세그먼트길이)",{"$nulls":13},"spae_ocpn_rt ","NUMBER(13,9) ","",{"$f":"\") TABLESPACE \"&AB485&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_T003 NOLOGGING"},{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegruprltmqueu_9.","spae_ocpn_rt"," IS ","'공간점유율 (차량길이/세그먼트길이)'",";",null,""]
[{"$nulls":23},{"$f":"CONCATENATE(AB484:AD484)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (clct_unix_tm) INTERVAL (3600) STORE IN (\"&AB485&\") (PARTITION BFR_\" & A475& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AB485&\");\"","v":"PARTITION BY RANGE (clct_unix_tm) INTERVAL (3600) STORE IN (SOIT_D08_T003) (PARTITION BFR_soitcedgegruprltmqueu_9_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_T003);"},{"$f":"\"CREATE INDEX PK_\" & A475& \" ON \" & A475 & CONCATENATE(AC477:AE482) & \" LOCAL (PARTITION BFR_\" & A475 & \"_20221101 TABLESPACE \"&AC485&\") TABLESPACE \"&AC485&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & A475 & \" ADD CONSTRAINT PK_\" & A475 & \" PRIMARY KEY \" & CONCATENATE(AC477:AE482) & \";\"","v":{"$error":"#VALUE!"}}]
["BI - 회전별 차종 검지 집계 테이블",{"$nulls":26},"SOIT_D08_T003","SOIT_I08_T003"]
["soitcsmrtturndtrtstats"]
["NO","속성명","컬럼명","PK/FK","NULL","형태",null,"TIBERO","길이","비고",{"$nulls":21},"COMMENT ON TABLE",{"$f":"A486&\" \"","v":"soitcsmrtturndtrtstats "},null," IS ",{"$f":"\"'\"&SUBSTITUTE(A485,\"테이블\",\"\")&\"'\"","v":"'BI - 회전별 차종 검지 집계 '"},";"]
[1,"현장카메라ID","spot_camr_id","PK","NOT NULL","VARCHAR2(10)",null,"VARCHAR2(10)",10,"카메라 ID(교차로 ID + _ + 방향)",{"$nulls":11},"CREATE TABLE ",{"$f":"A486&\" (\"","v":"soitcsmrtturndtrtstats ("},{"$f":"C488&\" \"","v":"spot_camr_id "},{"$f":"H488&\" \"","v":"VARCHAR2(10) "},{"$f":"IF(E488=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(D488=\"PK\", D488=\"PK/FK\"), C488, \"\")","v":"spot_camr_id"},{"$f":"IF(OR(D488=\"PK\", D488=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$A$486&\".\"","v":"soitcsmrtturndtrtstats."},{"$f":"C488","v":"spot_camr_id"}," IS ",{"$f":"\"'\"&J488&\"'\"","v":"'카메라 ID(교차로 ID + _ + 방향)'"},";"]
[2,"차종코드","kncr_cd","PK","NOT NULL","VARCHAR2(10)",null,"VARCHAR2(10)",10,"차종(008)"," LBUS:대형버스, LTRUCK:대형트럭(4.5T이상), MBUS:미니버스,\nMOTOR:오토바이, MTRUCK:트럭(4.5T미만), PCAR:승용차 ",{"$nulls":12},"kncr_cd ","VARCHAR2(10) ","NOT NULL",",",null,null,"kncr_cd",",","COMMENT ON COLUMN ","soitcsmrtturndtrtstats.","kncr_cd"," IS ","'차종(008)'",";"]
[3,"통계시작유닉스시각","stats_bgng_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"통계시작일시(unix timestamp)",{"$nulls":13},"stats_bgng_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"stats_bgng_unix_tm",",","COMMENT ON COLUMN ","soitcsmrtturndtrtstats.","stats_bgng_unix_tm"," IS ","'통계시작일시(unix timestamp)'",";"]
[4,"통계종료유닉스시각","stats_end_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"통계종료일시(unix timestamp)",{"$nulls":13},"stats_end_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"stats_end_unix_tm",",","COMMENT ON COLUMN ","soitcsmrtturndtrtstats.","stats_end_unix_tm"," IS ","'통계종료일시(unix timestamp)'",";"]
[5,"시간유형코드","hr_type_cd","PK","NOT NULL","CHAR(10)",null,"VARCHAR2(10)",10,"집계구분코드(011)"," (3:5분단위, 4:15분)",{"$nulls":12},"hr_type_cd ","VARCHAR2(10) ","NOT NULL",",",null,null,"hr_type_cd",",","COMMENT ON COLUMN ","soitcsmrtturndtrtstats.","hr_type_cd"," IS ","'집계구분코드(011)'",";"]
[6,"회전유형코드","turn_type_cd","PK","NOT NULL","VARCHAR2(10)",null,"VARCHAR2(10)",10,"회전유형(700)","( 11:직진, 21:작은좌회전, 22:큰좌회전, 31:작은우회전, 32:큰우회전, 41:유턴)",{"$nulls":12},"turn_type_cd ","VARCHAR2(10) ","NOT NULL",",",null,null,"turn_type_cd",")","COMMENT ON COLUMN ","soitcsmrtturndtrtstats.","turn_type_cd"," IS ","'회전유형(700)'",";"]
[7,"정검지수","nrdt_cnt",null,"NULL","NUMBER(5)",null,"NUMBER(5)",5,"정검지수",{"$nulls":13},"nrdt_cnt ","NUMBER(5) ","",",",null,null,"",null,"COMMENT ON COLUMN ","soitcsmrtturndtrtstats.","nrdt_cnt"," IS ","'정검지수'",";"]
[8,"오검지수","abdt_cnt",null,"NULL","NUMBER(5)",null,"NUMBER(5)",5,"오검지수",{"$nulls":13},"abdt_cnt ","NUMBER(5) ",null,",",{"$nulls":4},"COMMENT ON COLUMN ","soitcsmrtturndtrtstats.","abdt_cnt"," IS ","'오검지수'",";"]
[9,"미검지수","undt_cnt",null,"NULL","NUMBER(5)",null,"NUMBER(5)",5,"미검지수",{"$nulls":13},"undt_cnt ","NUMBER(5) ",null,{"$f":"\") TABLESPACE \"&AB498&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_T003 NOLOGGING"},{"$nulls":4},"COMMENT ON COLUMN ","soitcsmrtturndtrtstats.","undt_cnt"," IS ","'미검지수'",";"]
[{"$nulls":23},{"$f":"CONCATENATE(AB497:AD497)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (stats_bgng_unix_tm) INTERVAL (86400) STORE IN (\"&AB498&\") (PARTITION BFR_\" & A486& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AB498&\");\"","v":"PARTITION BY RANGE (stats_bgng_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_T003) (PARTITION BFR_soitcsmrtturndtrtstats_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_T003);"},{"$f":"\"CREATE INDEX PK_\" & A486& \" ON \" & A486 & CONCATENATE(AC488:AE495) & \" LOCAL (PARTITION BFR_\" & A486 & \"_20221101 TABLESPACE \"&AC498&\") TABLESPACE \"&AC498&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & A486 & \" ADD CONSTRAINT PK_\" & A486 & \" PRIMARY KEY \" & CONCATENATE(AC488:AE493) & \";\"","v":{"$error":"#VALUE!"}}]
["엣지그룹별 신호현시 집계 테이블",{"$nulls":26},"SOIT_D08_T003","SOIT_I08_T003",{"$nulls":9},{"$f":"IF(LEFT(X498, 13) = \"CONSTRAINT PK\", X498, \"\")","v":""}]
["soitcedgegrupsignaltot",{"$nulls":10},{"$f":"LEN(A499)","v":22},{"$nulls":26},""]
["NO","속성명","컬럼명","PK/FK","NULL","형태",null,"TIBERO","길이","비고",{"$nulls":21},"COMMENT ON TABLE",{"$f":"A499&\" \"","v":"soitcedgegrupsignaltot "},null," IS ",{"$f":"\"'\"&SUBSTITUTE(A498,\"테이블\",\"\")&\"'\"","v":"'엣지그룹별 신호현시 집계 '"},";",null,""]
[1,"엣지그룹ID","edge_grup_id","PK/FK","NOT NULL","VARCHAR2(300)",null,"VARCHAR2(300)",20,"엣지그룹ID",{"$nulls":11},"CREATE TABLE ",{"$f":"A499&\" (\"","v":"soitcedgegrupsignaltot ("},{"$f":"C501&\" \"","v":"edge_grup_id "},{"$f":"H501&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(E501=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(D501=\"PK\", D501=\"PK/FK\"), C501, \"\")","v":"edge_grup_id"},{"$f":"IF(OR(D501=\"PK\", D501=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$A$499&\".\"","v":"soitcedgegrupsignaltot."},{"$f":"C501","v":"edge_grup_id"}," IS ",{"$f":"\"'\"&J501&\"'\"","v":"'엣지그룹ID'"},";",null,""]
[2,"집계시작유닉스시각","tot_bgng_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"집계시작유닉스시각",{"$nulls":13},"tot_bgng_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"tot_bgng_unix_tm",",","COMMENT ON COLUMN ","soitcedgegrupsignaltot.","tot_bgng_unix_tm"," IS ","'집계시작유닉스시각'",";"]
[3,"집계종료유닉스시각","tot_end_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"집계종료유닉스시각",{"$nulls":13},"tot_end_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"tot_end_unix_tm",")","COMMENT ON COLUMN ","soitcedgegrupsignaltot.","tot_end_unix_tm"," IS ","'집계종료유닉스시각'",";"]
[4,"교통량","trvl",null,"NULL","NUMBER(10)",null,"NUMBER(10)",10,"총교통량",{"$nulls":13},"trvl ","NUMBER(10) ","",",",null,null,"",{"$f":"IF(OR(D504=\"PK\", D504=\"PK/FK\"), \",\", \"\")","v":""},"COMMENT ON COLUMN ","soitcedgegrupsignaltot.","trvl"," IS ","'총교통량'",";"]
[5,"속도","sped",null,"NULL","NUMBER(5,2)",null,"NUMBER(5,2)","5,2","평균속도",{"$nulls":13},"sped ","NUMBER(5,2) ","",",",null,null,"","","COMMENT ON COLUMN ","soitcedgegrupsignaltot.","sped"," IS ","'평균속도'",";"]
[6,"지체시간","dely_tm",null,"NULL","NUMBER(7,2)",null,"NUMBER(7,2)","5,2","교차로당 평균지체시간",{"$nulls":13},"dely_tm ","NUMBER(7,2) ","",",",null,null,"","","COMMENT ON COLUMN ","soitcedgegrupsignaltot.","dely_tm"," IS ","'교차로당 평균지체시간'",";"]
[7,"포화도","strtn_trst_rt",null,"NULL","NUMBER(13,9)",null,"NUMBER(13,9)","12,9","전체 시설물 평균 포화도",{"$nulls":13},"strtn_trst_rt ","NUMBER(13,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegrupsignaltot.","strtn_trst_rt"," IS ","'전체 시설물 평균 포화도'",";"]
[8,"밀도","trfc_dnst",null,"NULL","NUMBER(7,2)",null,"NUMBER(7,2)",5,"밀도","교통밀도(단위:대/m)",{"$nulls":12},"trfc_dnst ","NUMBER(7,2) ","",{"$f":"\") TABLESPACE \"&AB510&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_T002 NOLOGGING"},{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegrupsignaltot.","trfc_dnst"," IS ","'밀도'",";"]
[{"$nulls":23},{"$f":"CONCATENATE(AB509:AD509)","v":{"$error":"#VALUE!"}}," ","",null,{"$f":"\"PARTITION BY RANGE (tot_bgng_unix_tm) INTERVAL (86400) STORE IN (\"&AB510&\") (PARTITION BFR_\" & A499& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AB510&\");\"","v":"PARTITION BY RANGE (tot_bgng_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_T002) (PARTITION BFR_soitcedgegrupsignaltot_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_T002);"},{"$f":"\"CREATE INDEX PK_\" & A499& \" ON \" & A499 & CONCATENATE(AC501:AE508) & \" LOCAL (PARTITION BFR_\" & A499 & \"_20221101 TABLESPACE \"&AC510&\") TABLESPACE \"&AC510&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & A499 & \" ADD CONSTRAINT PK_\" & A499 & \" PRIMARY KEY \" & CONCATENATE(AC501:AE508) & \";\"","v":{"$error":"#VALUE!"}}]
["엣지그룹별 신호현시 대기행렬 집계 테이블",{"$nulls":26},"SOIT_D08_T002","SOIT_I08_T002",{"$nulls":9},{"$f":"IF(LEFT(X510, 13) = \"CONSTRAINT PK\", X510, \"\")","v":""}]
["soitcedgegrupsignalqueutot",{"$nulls":10},{"$f":"LEN(A511)","v":26},{"$nulls":26},""]
["NO","속성명","컬럼명","PK/FK","NULL","형태",null,"TIBERO","길이","비고",{"$nulls":21},"COMMENT ON TABLE",{"$f":"A511&\" \"","v":"soitcedgegrupsignalqueutot "},null," IS ",{"$f":"\"'\"&SUBSTITUTE(A510,\"테이블\",\"\")&\"'\"","v":"'엣지그룹별 신호현시 대기행렬 집계 '"},";",null,""]
[1,"엣지그룹ID","edge_grup_id","PK/FK","NOT NULL","VARCHAR2(300)",null,"VARCHAR2(300)",20,"엣지그룹ID",{"$nulls":11},"CREATE TABLE ",{"$f":"A511&\" (\"","v":"soitcedgegrupsignalqueutot ("},{"$f":"C513&\" \"","v":"edge_grup_id "},{"$f":"H513&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(E513=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(D513=\"PK\", D513=\"PK/FK\"), C513, \"\")","v":"edge_grup_id"},{"$f":"IF(OR(D513=\"PK\", D513=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$A$511&\".\"","v":"soitcedgegrupsignalqueutot."},{"$f":"C513","v":"edge_grup_id"}," IS ",{"$f":"\"'\"&J513&\"'\"","v":"'엣지그룹ID'"},";",null,""]
[2,"집계시작유닉스시각","tot_bgng_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"집계시작유닉스시각",{"$nulls":13},"tot_bgng_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"tot_bgng_unix_tm",",","COMMENT ON COLUMN ","soitcedgegrupsignalqueutot.","tot_bgng_unix_tm"," IS ","'집계시작유닉스시각'",";"]
[3,"집계종료유닉스시각","tot_end_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"집계종료유닉스시각",{"$nulls":13},"tot_end_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"tot_end_unix_tm",")","COMMENT ON COLUMN ","soitcedgegrupsignalqueutot.","tot_end_unix_tm"," IS ","'집계종료유닉스시각'",";"]
[4,"최소대기행렬길이","min_queu_lngt",null,"NULL","NUMBER(19,9)",null,"NUMBER(19,9)","19,9","최소대기행렬(단위:대/km/차선)",{"$nulls":13},"min_queu_lngt ","NUMBER(19,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegrupsignalqueutot.","min_queu_lngt"," IS ","'최소대기행렬(단위:대/km/차선)'",";"]
[5,"최대대기행렬길이","max_queu_lngt",null,"NULL","NUMBER(19,9)",null,"NUMBER(19,9)","19,9","최대대기행렬(단위:대/km/차선)",{"$nulls":13},"max_queu_lngt ","NUMBER(19,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegrupsignalqueutot.","max_queu_lngt"," IS ","'최대대기행렬(단위:대/km/차선)'",";"]
[6,"구간거리대비 최소대기행렬","min_queu_rt",null,"NULL","NUMBER(19,9)",null,"NUMBER(19,9)","19,9","거리대비 최소대기행렬",{"$nulls":13},"min_queu_rt ","NUMBER(19,9) ","",",",{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegrupsignalqueutot.","min_queu_rt"," IS ","'거리대비 최소대기행렬'",";"]
[7,"구간거리대비 최대대기행렬","max_queu_rt",null,"NULL","NUMBER(19,9)",null,"NUMBER(19,9)","19,9","거리대비 최대대기행렬",{"$nulls":13},"max_queu_rt ","NUMBER(19,9) ","",{"$f":"\") TABLESPACE \"&AB521&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_T002 NOLOGGING"},{"$nulls":4},"COMMENT ON COLUMN ","soitcedgegrupsignalqueutot.","max_queu_rt"," IS ","'거리대비 최대대기행렬'",";"]
[{"$nulls":23},{"$f":"CONCATENATE(AB520:AD520)","v":{"$error":"#VALUE!"}}," ","",null,{"$f":"\"PARTITION BY RANGE (tot_bgng_unix_tm) INTERVAL (86400) STORE IN (\"&AB521&\") (PARTITION BFR_\" & A511& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AB521&\");\"","v":"PARTITION BY RANGE (tot_bgng_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_T002) (PARTITION BFR_soitcedgegrupsignalqueutot_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_T002);"},{"$f":"\"CREATE INDEX PK_\" & A511& \" ON \" & A511 & CONCATENATE(AC513:AE516) & \" LOCAL (PARTITION BFR_\" & A511 & \"_20221101 TABLESPACE \"&AC521&\") TABLESPACE \"&AC521&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & A511 & \" ADD CONSTRAINT PK_\" & A511 & \" PRIMARY KEY \" & CONCATENATE(AC513:AE516) & \";\"","v":{"$error":"#VALUE!"}}]
["교차로별 인접엣지 교통량 신호현시 집계 테이블",{"$nulls":26},"SOIT_D08_T002","SOIT_I08_T002",{"$nulls":9},{"$f":"IF(LEFT(X521, 13) = \"CONSTRAINT PK\", X521, \"\")","v":""}]
["soitcintssignaltot",{"$nulls":10},{"$f":"LEN(A522)","v":18},{"$nulls":26},""]
["NO","속성명","컬럼명","PK/FK","NULL","형태",null,"TIBERO","길이","비고",{"$nulls":21},"COMMENT ON TABLE",{"$f":"A522&\" \"","v":"soitcintssignaltot "},null," IS ",{"$f":"\"'\"&SUBSTITUTE(A521,\"테이블\",\"\")&\"'\"","v":"'교차로별 인접엣지 교통량 신호현시 집계 '"},";",null,""]
[1,"노드ID","node_id","PK/FK","NOT NULL","VARCHAR2(300)",null,"VARCHAR2(300)",20,"교차로 노드ID",{"$nulls":11},"CREATE TABLE ",{"$f":"A522&\" (\"","v":"soitcintssignaltot ("},{"$f":"C524&\" \"","v":"node_id "},{"$f":"H524&\" \"","v":"VARCHAR2(300) "},{"$f":"IF(E524=\"NOT NULL\", \"NOT NULL\", \"\")","v":"NOT NULL"},",",null,"(",{"$f":"IF(OR(D524=\"PK\", D524=\"PK/FK\"), C524, \"\")","v":"node_id"},{"$f":"IF(OR(D524=\"PK\", D524=\"PK/FK\"), \",\", \"\")","v":","},"COMMENT ON COLUMN ",{"$f":"$A$522&\".\"","v":"soitcintssignaltot."},{"$f":"C524","v":"node_id"}," IS ",{"$f":"\"'\"&J524&\"'\"","v":"'교차로 노드ID'"},";",null,""]
[2,"집계시작유닉스시각","tot_bgng_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"집계시작유닉스시각",{"$nulls":13},"tot_bgng_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"tot_bgng_unix_tm",",","COMMENT ON COLUMN ","soitcintssignaltot.","tot_bgng_unix_tm"," IS ","'집계시작유닉스시각'",";"]
[3,"집계종료유닉스시각","tot_end_unix_tm","PK","NOT NULL","NUMBER(10)",null,"NUMBER(10)",10,"집계종료유닉스시각",{"$nulls":13},"tot_end_unix_tm ","NUMBER(10) ","NOT NULL",",",null,null,"tot_end_unix_tm",",","COMMENT ON COLUMN ","soitcintssignaltot.","tot_end_unix_tm"," IS ","'집계종료유닉스시각'",";"]
[4,"신호상태코드","sgnl_stts_cd","PK","NOT NULL","CHAR(1)",null,"CHAR(1)",1,"신호상태코드 (505)",{"$nulls":13},"sgnl_stts_cd ","CHAR(1) ","NOT NULL",",",null,null,"sgnl_stts_cd",",","COMMENT ON COLUMN ","soitcintssignaltot.","sgnl_stts_cd"," IS ","'신호상태코드 (505)'",";"]
[5,"연결엣지ID","cnct_edge_id","PK","NOT NULL","VARCHAR2(300)",null,"VARCHAR2(300)",null,"연결엣지 ID",{"$nulls":13},"cnct_edge_id ","VARCHAR2(300) ","NOT NULL",",",null,null,"cnct_edge_id",",","COMMENT ON COLUMN ","soitcintssignaltot.","cnct_edge_id"," IS ","'연결엣지 ID'",";"]
[6,"진입진출구분","div_cd","PK","NOT NULL","VARCHAR2(10)",null,"VARCHAR2(10)",null,"인접 진입/진출엣지 구분코드",{"$nulls":13},"div_cd ","VARCHAR2(10) ","NOT NULL",",",null,null,"div_cd",")","COMMENT ON COLUMN ","soitcintssignaltot.","div_cd"," IS ","'인접 진입/진출엣지 구분코드'",";"]
[7,"교통량","trvl",null,"NULL","NUMBER(10)",null,"NUMBER(10)",10,"총교통량",{"$nulls":13},"trvl ","NUMBER(10) ","",{"$f":"\") TABLESPACE \"&AB532&\" NOLOGGING\"","v":") TABLESPACE SOIT_D08_T002 NOLOGGING"},{"$nulls":4},"COMMENT ON COLUMN ","soitcintssignaltot.","trvl"," IS ","'총교통량'",";"]
[{"$nulls":23},{"$f":"CONCATENATE(AB531:AD531)","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"\"PARTITION BY RANGE (tot_bgng_unix_tm) INTERVAL (86400) STORE IN (\"&AB532&\") (PARTITION BFR_\" & A522& \"_20221101 VALUES LESS THAN (1667228400) TABLESPACE \"&AB532&\");\"","v":"PARTITION BY RANGE (tot_bgng_unix_tm) INTERVAL (86400) STORE IN (SOIT_D08_T002) (PARTITION BFR_soitcintssignaltot_20221101 VALUES LESS THAN (1667228400) TABLESPACE SOIT_D08_T002);"},{"$f":"\"CREATE INDEX PK_\" & A522& \" ON \" & A522 & CONCATENATE(AC524:AE529) & \" LOCAL (PARTITION BFR_\" & A522 & \"_20221101 TABLESPACE \"&AC532&\") TABLESPACE \"&AC532&\" NOLOGGING;\"","v":{"$error":"#VALUE!"}},{"$f":"\"ALTER TABLE \" & A522 & \" ADD CONSTRAINT PK_\" & A522 & \" PRIMARY KEY \" & CONCATENATE(AC524:AE529) & \";\"","v":{"$error":"#VALUE!"}}]
[{"$nulls":27},"SOIT_D08_T002","SOIT_I08_T002"]

{"sheet":"글로벌브릿지(백업용)","index":12,"n_rows":216,"n_cols":19,"rows_kept":216,"cut":false,"hidden":false,"merged":[[0,1,0,7],[0,9,0,11],[0,13,0,16],[0,18,0,20],[1,1,1,7],[1,9,1,11],[2,9,2,11],[2,1,2,7],[11,1,11,7],[11,9,11,11],[27,1,27,7],[27,9,27,11],[33,1,33,7],[33,9,33,11],[39,1,39,7],[39,9,39,11],[58,1,58,7],[60,1,60,7],[60,9,60,11],[69,1,69,7],[69,9,69,11],[76,1,76,7],[76,9,76,11],[85,1,85,7],[85,9,85,11],[96,1,96,7],[96,9,96,11],[108,9,108,11],[202,1,202,7],[202,9,202,11],[108,1,108,7],[123,1,123,7],[123,9,123,11],[140,1,140,7],[140,9,140,11],[152,1,152,7],[152,9,152,11],[168,1,168,7],[168,9,168,11],[177,1,177,7],[177,9,177,11],[188,1,188,7],[188,9,188,11]]}
[null,"변경전(글로벌브릿지 정의)",{"$nulls":7},"변경후(센터 도메인 및 용어기준)",null,null,null,"현재까지 확인된 코드값",{"$nulls":4},"전체 코드 최신정보 요청한 상태"]
[]
[null,"crossroad_info",{"$nulls":6},">>","soitgintsinfo"]
[null,"NO","PK","컬럼명","형태","NULL","기본값","설명",null,"논리명","물리명","형태",null,"코드종류","코드종류(용어변경)","코드값","코드 설명","가중치"]
[null,1,"PK","crossroad_id","SMALLINT(5) UNSIGNED","N",0,"교차로 ID (공식 교차로ID)",null,"현장교차로ID","spot_ints_id","NUMBER(5)",null,"car_type","kncr_cd","LBUS","대형버스",1.8]
[null,2,null,"crossroad_name","VARCHAR(25)","N",null,"교차로 명",null,"교차로명","ints_nm","VARCHAR2(40)",null,"car_type","kncr_cd","LTRUCK","대형트럭(4.5T이상)",1.8]
[null,3,null,"district_name","VARCHAR(25)","N",null,"지역(구)",null,"시군구명","sgg_nm","VARCHAR2(40)",null,"car_type","kncr_cd","MBUS","미니버스",1.8]
[null,4,null,"dong_name","VARCHAR(25)","N",null,"지역(동)",null,"행정동명","dong_nm","VARCHAR2(40)",null,"car_type","kncr_cd","MOTOR","오토바이"]
[null,5,null,"actiev_yn","CHAR(1)","N","N","교차로 활성여부(Y/N)",null,"교차로활성여부","ints_vtlt_yn","CHAR(1)",null,"car_type","kncr_cd","MTRUCK","트럭(4.5T미만)",1]
[null,6,null,"comment","VARCHAR(255)","Y",null,"교차로 설명",null,"비고","rmrk","VARCHAR2(2000)",null,"car_type","kncr_cd","PCAR","승용차",1]
[{"$nulls":13},"event_type","evet_type_cd",1,"차량정지"]
[null,"cameras",{"$nulls":6},">>","soitgcamrinfo",null,null,null,"event_type","evet_type_cd",2,"꼬리물기"]
[null,"NO","PK","컬럼명","형태","NULL","기본값","설명",null,"논리명","물리명","형태",null,"event_type","evet_type_cd",3,"보행자횡단(인도이탈)"]
[null,1,"PK","crossroad_id","SMALLINT(5)","N",0,"교차로 ID",null,"현장교차로ID","spot_ints_id","NUMBER(5)",null,"event_type","evet_type_cd",4,"역주행"]
[null,2,"UK","cam_id_hash","VARCHAR(64)","N",null,"cam_id+설치위치의 SHA256값으로 Key 가 된다.",null,"현장카메라위치ID","spot_camr_locn_id","VARCHAR2(64)",null,"time_type","hr_type_cd",1,"신호현시"]
[null,3,"PK","cam_id","VARCHAR(10)","N",null,"카메라 ID(교차로 ID + _ + 방향)",null,"현장카메라ID","spot_camr_id","VARCHAR2(10)",null,"time_type","hr_type_cd",2,"1분 단위"]
[null,4,null,"name","VARCHAR(255)","Y",null,"현장서버 명",null,"현장서버명","spot_srvr_nm","VARCHAR2(256)",null,"time_type","hr_type_cd",3,"5분 단위"]
[null,5,null,"cam_2k_ip","VARCHAR(15)","Y",null,"2K 카메라 IPv4",null,"2K카메라IP","2k_camr_ip","VARCHAR2(15)",null,"turn_type","turn_type_cd",11,"직진"]
[null,6,null,"cam_2k_e_ip","VARCHAR(15)","Y",null,"2K 엣지 IPv4",null,"2K엣지시스템IP","2k_edge_sys_ip","VARCHAR2(15)",null,"turn_type","turn_type_cd",21,"작은좌회전"]
[null,7,null,"cam_4k_ip","VARCHAR(15)","Y",null,"4K 카메라 IPv4",null,"4K카메라IP","4k_camr_ip","VARCHAR2(15)",null,"turn_type","turn_type_cd",22,"큰좌회전"]
[null,8,null,"cam_4k_e_ip","VARCHAR(15)","Y",null,"4K 엣지 IPv4",null,"4K엣지시스템IP","4k_edge_sys_ip","VARCHAR2(15)",null,"turn_type","turn_type_cd",31,"작은우회전"]
[null,9,null,"detection_lan","TINYINT(3)","Y",0,"검지영역 길이(미터)",null,"검지거리","dttn_dstn","NUMBER(19,9)",null,"turn_type","turn_type_cd",32,"큰우회전"]
[null,10,"PK",null,"VARCHAR(2)","Y",null,"설치 위치 코드",null,"설치위치코드","instl_locn_cd","CHAR(2)",null,"turn_type","turn_type_cd",41,"유턴"]
[null,11,null,null,"VARCHAR(50)","Y",null,"일련번호",null,"관리일련번호","mng_sn","VARCHAR2(50)"]
[null,12,null,null,"VARCHAR(1)","N","N","함체 ECU 정보 전송여부",null,"ECU정보전송여부","ecu_info_trsm_yn","CHAR(1)"]
[null,13,null,"active_yn","VARCHAR(1)","N","Y","카메라 활성여부 (Y/N)",null,"카메라활성여부","camr_vtlt_yn","CHAR(1)"]
[]
[null,"lane_num_info",{"$nulls":6},">>","soitglaneinfo"]
[null,"NO","PK","컬럼명","형태","NULL","기본값","설명",null,"논리명","물리명","형태"]
[null,1,"PK","cam_id","VARCHAR(10)","N",null,"카메라 ID(교차로 ID + _ + 방향)",null,"현장카메라ID","spot_camr_id","VARCHAR2(10)"]
[null,2,"PK","lane_num","CHAR(1)","N",1,"차로",null,"차로번호","lane_no","NUMBER(2)"]
[null,3,null,"turn_type","VARCHAR(10)","Y",null,"한글설명",null,"회전유형코드","turn_type_cd","CHAR(10)"]
[]
[null,"codes",{"$nulls":6},">>","soitgspotcdinfo"]
[null,"NO","PK","컬럼명","형태","NULL","기본값","설명",null,"논리명","물리명","형태"]
[null,1,"PK","code_type","VARCHAR(10)","N",null,null,null,"코드유형명","cd_type_nm","VARCHAR2(20)"]
[null,2,"PK","code_key","VARCHAR(10)","N",null,null,null,"식별코드","dstg_cd","CHAR(10)"]
[null,3,null,"comment","VARCHAR(255)","Y",null,null,null,"비고","rmrk","VARCHAR2(2000)"]
[]
[null,"realtime_detections",{"$nulls":6},">>","soitgrtmdtinfo"]
[null,"NO","PK","컬럼명","형태","NULL","기본값","설명",null,"논리명","물리명","형태"]
[null,1,null,"cam_id","VARCHAR(10)","N",null,"카메라 ID(교차로 ID + _ + 방향)",null,"현장카메라ID","spot_camr_id","VARCHAR2(10)"]
[null,2,null,"car_num","VARCHAR(10)","Y",null,"차량 번호 (오검지도 저장)",null,"차량번호명","vhno_nm","VARCHAR2(20)"]
[null,3,null,"validity","VARCHAR(1)","Y",null,"번호판 정검지 여부 (Y : 정검지 N : 미검지 F : 오검지)",null,"차량번호검지여부","vhno_dttn_yn","CHAR(1)"]
[null,4,null,"car_type","VARCHAR(10)","Y",null,"차종(코드테이블 참조)",null,"차종코드","kncr_cd","CHAR(10)"]
[null,5,null,"lane_num","CHAR(1)","Y",null,"진행 차로",null,"차로번호","lane_no","NUMBER(2)"]
[null,6,null,"turn_type","VARCHAR(10)","Y",null,"진행 방향(코드테이블 참조)",null,"회전유형코드","turn_type_cd","CHAR(10)"]
[null,7,null,"turn_sensing_date","INT(10)","Y",0,"방향 ROI 검지 일시 (unix timestamp)",null,"회전검지유닉스시각","turn_dttn_unix_tm","NUMBER(10)"]
[null,8,null,"turn_point_speed","FLOAT","Y",0,"방향 검지 ROI 지점속도",null,"회전검지속도","turn_dttn_sped","NUMBER(5,2)"]
[null,9,null,"stop_sensing_date","INT(10)","Y",0,"정지선 통과 일시 (unix timestamp)",null,"정지선통과유닉스시각","stln_pasg_unix_tm","NUMBER(10)"]
[null,10,null,"stop_point_speed","FLOAT","Y",0,"정지선 검지 지점속도",null,"정지선검지속도","stln_dttn_sped","NUMBER(5,2)"]
[null,11,null,"interval_speed","FLOAT","Y",0,"차량 구간 속도",null,"차량구간속도","vhcl_sect_sped","NUMBER(5,2)"]
[null,12,null,"sensing_date","INT(10)","Y",0,"차량 최초 관측 일시 (unix timestamp)",null,"최초관측유닉스시각","frst_obsrvn_unix_tm","NUMBER(10)"]
[null,13,null,"sensing_time","SMALLINT(5)","Y",1,"차량 관측 시간 합",null,"차량관측시간","vhcl_obsrvn_hr","NUMBER(10)"]
[null,14,null,"img_path","VARCHAR(50)","Y",null,"이미지 저장 경로",null,"이미지경로명","img_path_nm","VARCHAR2(80)"]
[null,15,null,"car_img_name","VARCHAR(50)","Y",null,"차량 이미지 명",null,"차량이미지파일명","vhcl_img_file_nm","VARCHAR2(80)"]
[null,16,null,"car_num_img_name","VARCHAR(50)","Y",null,"번호판 이미지 명",null,"번호판이미지파일명","nopl_img_file_nm","VARCHAR2(80)"]
[null,17,null,"created_date","INT(10)","Y",null,"생성일시(unix timestamp)",null,"생성유닉스시각","crt_unix_tm","NUMBER(10)"]
[null,"유아이 사용 추가 컬럼",{"$nulls":7},"차적조회여부","crrg_inq_yn","CHAR(1)"]
[]
[null,"events",{"$nulls":6},">>","soitgunacevet"]
[null,"NO","PK","컬럼명","형태","NULL","기본값","설명",null,"논리명","물리명","형태"]
[null,1,null,"cam_id","VARCHAR(10)","N",null,"카메라 ID(교차로 ID + _ + 방향)",null,"현장카메라ID","spot_camr_id","VARCHAR2(10)"]
[null,2,null,"event_sensing_date","INT(10)","Y",null,"이벤트 발생 일시",null,"발생유닉스시각","ocrn_unix_tm","NUMBER(10)"]
[null,3,null,"event_type","VARCHAR(10)","Y",null,"이벤트 타입(코드테이블참조)",null,"이벤트유형코드","evet_type_cd","CHAR(1)"]
[null,4,null,"event_img_path","VARCHAR(50)","Y",null,"이미지 경로",null,"이미지경로명","img_path_nm","VARCHAR2(80)"]
[null,5,null,"event_img_name","VARCHAR(50)","Y",null,"이미지 명",null,"이미지파일명","img_file_nm","VARCHAR2(80)"]
[null,6,null,"created_date","INT(10)","Y",0,"생성일시(unix timestamp)",null,"생성유닉스시각","crt_unix_tm","NUMBER(10)"]
[]
[null,"crosswalk_detections",{"$nulls":6},">>","soitgcwdtinfo"]
[null,"NO","PK","컬럼명","형태","NULL","기본값","설명",null,"논리명","물리명","형태"]
[null,1,null,"cam_id","VARCHAR(10)","N",null,"카메라 ID(교차로 ID + _ + 방향)",null,"현장카메라ID","spot_camr_id","VARCHAR2(10)"]
[null,2,null,"sensing_date","INT(10)","N",0,"검지일시",null,"검지유닉스시각","dttn_unix_tm","NUMBER(10)"]
[null,3,null,"walking_type","VARCHAR(1)","N","L","방향(왼쪽,오른쪽)",null,"방향구분코드","drct_se_cd","CHAR(1)"]
[null,4,null,"created_date","INT(10)","Y",0,"생성일시",null,"생성유닉스시각","crt_unix_tm","NUMBER(10)"]
[]
[null,"trackings",{"$nulls":6},">>","soitgvhcltrce"]
[null,"NO","PK","컬럼명","형태","NULL","기본값","설명",null,"논리명","물리명","형태"]
[null,1,"PK","cam_id","VARCHAR(10)","N",null,"카메라 ID(교차로 ID + _ + 방향)",null,"현장카메라ID","spot_camr_id","VARCHAR2(10)"]
[null,2,"PK","tracking_start_date","INT(10)","Y",null,"추적시작일시",null,"추적시작유닉스시각","trce_bgng_unix_tm","NUMBER(10)"]
[null,3,"PK","tracking_end_date","INT(10)","Y",null,"추적종료일시",null,"추적종료유닉스시각","trce_end_unix_tm","NUMBER(10)"]
[null,4,null,"tracking_file_path","VARCHAR(25)","Y",null,"이미지 경로",null,"이미지경로명","img_path_nm","VARCHAR2(80)"]
[null,5,null,"tracking_file_name","VARCHAR(50)","Y",null,"이미지 명",null,"이미지파일명","img_file_nm","VARCHAR2(80)"]
[null,6,null,"created_date","INT(10)","Y",0,"생성일시",null,"생성유닉스시각","crt_unix_tm","NUMBER(10)"]
[]
[null,"validity_stats",{"$nulls":6},">>","soitgvhcldtrtstats"]
[null,"NO","PK","컬럼명","형태","NULL","기본값","설명",null,"논리명","물리명","형태"]
[null,1,"PK","cam_id","VARCHAR(10)","N",null,"카메라 ID(교차로 ID + _ + 방향)",null,"현장카메라ID","spot_camr_id","VARCHAR2(10)"]
[null,2,"PK","stats_start_date","INT(10)","Y",null,"통계시작일시(unix timestamp)",null,"통계시작유닉스시각","stats_bgng_unix_tm","NUMBER(10)"]
[null,3,"PK","stats_end_date","INT(10)","Y",null,"통계종료일시(unix timestamp)",null,"통계종료유닉스시각","stats_end_unix_tm","NUMBER(10)"]
[null,4,null,"validity_y","SMALLINT(5)","Y",0,"정검지 수",null,"정검지수","nrdt_cnt","NUMBER(5)"]
[null,5,null,"validity_n","SMALLINT(5)","Y",0,"오검지 수",null,"오검지수","abdt_cnt","NUMBER(5)"]
[null,6,null,"validity_f","SMALLINT(5)","Y",0,"미검지 수",null,"미검지수","undt_cnt","NUMBER(5)"]
[null,7,null,"validity_m","SMALLINT(5)","Y",0,"오토바이 수",null,"오토바이검지수","mtcl_dttn_cnt","NUMBER(5)"]
[null,8,null,"created_date","INT(10)","Y",0,"생성일시(unix timestamp)",null,"생성유닉스시각","crt_unix_tm","NUMBER(10)"]
[]
[null,"validity_turn_stats",{"$nulls":6},">>","soitgturndtrtstats"]
[null,"NO","PK","컬럼명","형태","NULL","기본값","설명",null,"논리명","물리명","형태"]
[null,1,"PK","cam_id","VARCHAR(10)","N",null,"카메라 ID(교차로 ID + _ + 방향)",null,"현장카메라ID","spot_camr_id","VARCHAR2(10)"]
[null,2,"PK","stats_start_date","INT(10)","Y",null,"통계시작일시(unix timestamp)",null,"통계시작유닉스시각","stats_bgng_unix_tm","NUMBER(10)"]
[null,3,"PK","stats_end_date","INT(10)","Y",null,"통계종료일시(unix timestamp)",null,"통계종료유닉스시각","stats_end_unix_tm","NUMBER(10)"]
[null,4,"PK","trun_type","VARCHAR(10)","N",null,"코드테이블 참조",null,"회전유형코드","turn_type_cd","CHAR(10)"]
[null,5,null,"validity_y","SMALLINT(5)","Y",0,"정검지 수",null,"정검지수","nrdt_cnt","NUMBER(5)"]
[null,6,null,"validity_n","SMALLINT(5)","Y",0,"오검지 수",null,"오검지수","abdt_cnt","NUMBER(5)"]
[null,7,null,"validity_f","SMALLINT(5)","Y",0,"미검지 수",null,"미검지수","undt_cnt","NUMBER(5)"]
[null,8,null,"validity_m","SMALLINT(5)","Y",0,"오토바이 수",null,"오토바이검지수","mtcl_dttn_cnt","NUMBER(5)"]
[null,9,null,"created_date","INT(10)","Y",0,"생성일시(unix timestamp)",null,"생성유닉스시각","crt_unix_tm","NUMBER(10)"]
[]
[null,"access_road_stats",{"$nulls":6},">>","soitgaprdstats"]
[null,"NO","PK","컬럼명","형태","NULL","기본값","설명",null,"논리명","물리명","형태"]
[null,1,"PK","cam_id","VARCHAR(10)","N",null,"카메라 ID(교차로 ID + _ + 방향)",null,"현장카메라ID","spot_camr_id","VARCHAR2(10)"]
[null,2,"PK","time_type","VARCHAR(10)","N",null,"시간타입(5분 OR 현시)",null,"시간유형코드","hr_type_cd","CHAR(10)"]
[null,3,"PK","stats_start_date","INT(10)","N",0,"통계시작일시(unix timestamp)",null,"통계시작유닉스시각","stats_bgng_unix_tm","NUMBER(10)"]
[null,4,"PK","stats_end_date","INT(10)","N",0,"통계종료일시(unix timestamp)",null,"통계종료유닉스시각","stats_end_unix_tm","NUMBER(10)"]
[null,5,null,"traffic","INT(10)","Y",0,"교통량",null,"총교통량","totl_trvl","NUMBER(10)"]
[null,6,null,"point_speed","FLOAT","Y",0,"감지 차량 평균 정지선통과 속도",null,"평균정지선검지속도","avg_stln_dttn_sped","NUMBER(5,2)"]
[null,7,null,"interval_speed","FLOAT","Y",0,"감지 차량 평균 구간속도",null,"평균구간속도","avg_sect_sped","NUMBER(5,2)"]
[null,8,null,"avg_density","SMALLINT(5)","Y",0,"평균 교통밀도(단위:대/km)",null,"평균교통밀도","avg_trfc_dnst","NUMBER(5)"]
[null,9,null,"min_density","SMALLINT(5)","Y",0,"최소 교통밀도(단위:대/km)",null,"최소교통밀도","min_trfc_dnst","NUMBER(5)"]
[null,10,null,"max_density","SMALLINT(5)","Y",0,"최대 교통밀도(단위:대/km)",null,"최대교통밀도","max_trfc_dnst","NUMBER(5)"]
[null,11,null,"traffic_share","TINYINT(3)","Y",0,"점유율(차로별 점유율의 평균값)",null,"평균차로점유율","avg_lane_ocpn_rt","NUMBER(12,9)"]
[null,12,null,"created_date","INT(10)","Y",0,"생성일시(unix timestamp)",null,"생성유닉스시각","crt_unix_tm","NUMBER(10)"]
[]
[null,"turn_type_stats",{"$nulls":6},">>","soitgturntypestats"]
[null,"NO","PK","컬럼명","형태","NULL","기본값","설명",null,"논리명","물리명","형태"]
[null,1,"PK","cam_id","VARCHAR(10)","N",null,"카메라 ID(교차로 ID + _ + 방향)",null,"현장카메라ID","spot_camr_id","VARCHAR2(10)"]
[null,2,"PK","turn_type","VARCHAR(10)","N",null,"회전 종류 (코드 테이블 참조)",null,"회전유형코드","turn_type_cd","CHAR(10)"]
[null,3,"PK","time_type","VARCHAR(10)","N",null,"시간타입(5분 OR 현시)",null,"시간유형코드","hr_type_cd","CHAR(10)"]
[null,4,"PK","stats_start_date","INT(10)","N",0,"통계시작일시(unix timestamp)",null,"통계시작유닉스시각","stats_bgng_unix_tm","NUMBER(10)"]
[null,5,"PK","stats_end_date","INT(10)","N",0,"통계종료일시(unix timestamp)",null,"통계종료유닉스시각","stats_end_unix_tm","NUMBER(10)"]
[null,6,null,"traffic_car_type_1","INT(10)","Y",0,"교통량_차종1",null,"차종1_교통량","1kncr_trvl","NUMBER(10)"]
[null,7,null,"traffic_car_type_2","INT(10)","Y",0,"교통량_차종2",null,"차종2_교통량","2kncr_trvl","NUMBER(10)"]
[null,8,null,"traffic_car_type_3","INT(10)","Y",0,"교통량_차종3",null,"차종3_교통량","3kncr_trvl","NUMBER(10)"]
[null,9,null,"traffic_car_type_4","INT(10)","Y",0,"교통량_차종4",null,"차종4_교통량","4kncr_trvl","NUMBER(10)"]
[null,10,null,"traffic_car_type_5","INT(10)","Y",0,"교통량_차종5",null,"차종5_교통량","5kncr_trvl","NUMBER(10)"]
[null,11,null,"traffic_car_type_6","INT(10)","Y",0,"교통량_차종6",null,"차종6_교통량","6kncr_trvl","NUMBER(10)"]
[null,12,null,"point_speed","FLOAT","Y",0,"감지 차량 평균 정지선통과 속도",null,"평균정지선검지속도","avg_stln_dttn_sped","NUMBER(5,2)"]
[null,13,null,"interval_speed","FLOAT","Y",0,"감지 차량 평균 구간속도",null,"평균구간속도","avg_sect_sped","NUMBER(5,2)"]
[null,14,null,"created_date","INT(10)","Y",0,"생성일시(unix timestamp)",null,"생성유닉스시각","crt_unix_tm","NUMBER(10)"]
[]
[null,"car_type_stats",{"$nulls":6},">>","soitgkncrstats"]
[null,"NO","PK","컬럼명","형태","NULL","기본값","설명",null,"논리명","물리명","형태"]
[null,1,"PK","cam_id","VARCHAR(10)","N",null,"카메라 ID(교차로 ID + _ + 방향)",null,"현장카메라ID","spot_camr_id","VARCHAR2(10)"]
[null,2,"PK","car_type","VARCHAR(10)","N",null,"차종 (코드테이블 참조)",null,"차종코드","kncr_cd","CHAR(10)"]
[null,3,"PK","time_type","VARCHAR(10)","N",null,"시간타입(5분 OR 현시)",null,"시간유형코드","hr_type_cd","CHAR(10)"]
[null,4,"PK","stats_start_date","INT(10)","N",0,"통계시작일시(unix timestamp)",null,"통계시작유닉스시각","stats_bgng_unix_tm","NUMBER(10)"]
[null,5,"PK","stats_end_date","INT(10)","N",0,"통계종료일시(unix timestamp)",null,"통계종료유닉스시각","stats_end_unix_tm","NUMBER(10)"]
[null,6,null,"traffic","INT(10)","Y",0,"교통량",null,"총교통량","totl_trvl","NUMBER(10)"]
[null,7,null,"point_speed","FLOAT","Y",0,"감지 차량 평균 정지선통과 속도",null,"평균정지선검지속도","avg_stln_dttn_sped","NUMBER(5,2)"]
[null,8,null,"interval_speed","FLOAT","Y",0,"감지 차량 평균 구간속도",null,"평균구간속도","avg_sect_sped","NUMBER(5,2)"]
[null,9,null,"created_date","INT(10)","Y",0,"생성일시(unix timestamp)",null,"생성유닉스시각","crt_unix_tm","NUMBER(10)"]
[]
[null,"lane_num_stats",{"$nulls":6},">>","soitglanestats"]
[null,"NO","PK","컬럼명","형태","NULL","기본값","설명",null,"논리명","물리명","형태"]
[null,1,"PK","cam_id","VARCHAR(10)","N",null,"카메라 ID(교차로 ID + _ + 방향)",null,"현장카메라ID","spot_camr_id","VARCHAR2(10)"]
[null,2,"PK","lane_num","VARCHAR(1)","Y",0,"차로",null,"차로번호","lane_no","NUMBER(2)"]
[null,3,"PK","time_type","VARCHAR(10)","N",null,"시간타입(5분 OR 현시)",null,"시간유형코드","hr_type_cd","CHAR(10)"]
[null,4,"PK","stats_start_date","INT(10)","N",0,"통계시작일시(unix timestamp)",null,"통계시작유닉스시각","stats_bgng_unix_tm","NUMBER(10)"]
[null,5,"PK","stats_end_date","INT(10)","N",0,"통계종료일시(unix timestamp)",null,"통계종료유닉스시각","stats_end_unix_tm","NUMBER(10)"]
[null,6,null,"traffic","INT(10)","Y",0,"교통량",null,"총교통량","totl_trvl","NUMBER(10)"]
[null,7,null,"point_speed","FLOAT","Y",0,"감지 차량 평균 정지선통과 속도",null,"평균정지선검지속도","avg_stln_dttn_sped","NUMBER(5,2)"]
[null,8,null,"interval_speed","FLOAT","Y",0,"감지 차량 평균 구간속도",null,"평균구간속도","avg_sect_sped","NUMBER(10)"]
[null,9,null,"avg_density","SMALLINT(5)","Y",0,"평균 교통밀도(단위:대/km/차선)",null,"평균교통밀도","avg_trfc_dnst","NUMBER(5)"]
[null,10,null,"min_density","SMALLINT(5)","Y",0,"최소 교통밀도(단위:대/km/차선)",null,"최소교통밀도","min_trfc_dnst","NUMBER(5)"]
[null,11,null,"max_density","SMALLINT(5)","Y",0,"최대 교통밀도(단위:대/km/차선)",null,"최대교통밀도","max_trfc_dnst","NUMBER(5)"]
[null,12,null,"traffic_share","TINYINT (3)","Y",0,"점유율 (전체차량점유시간/단위시간/차로)",null,"점유율","ocpn_rt","NUMBER(12,9)"]
[null,13,null,"created_date","INT(10)","Y",0,"생성일시(unix timestamp)",null,"생성유닉스시각","crt_unix_tm","NUMBER(10)"]
[]
[null,"access_road_queue",{"$nulls":6},">>","soitgaprdqueu"]
[null,"NO","PK","컬럼명","형태","NULL","기본값","설명",null,"논리명","물리명","형태"]
[null,1,"PK","cam_id","VARCHAR(10)","N",null,"카메라 ID(교차로 ID + _ + 방향)",null,"현장카메라ID","spot_camr_id","VARCHAR2(10)"]
[null,2,"PK","stats_start_date","INT(10)","Y",0,"통계시작일시(unix timestamp)",null,"통계시작유닉스시각","stats_bgng_unix_tm","NUMBER(10)"]
[null,3,"PK","stats_end_date","INT(10)","Y",0,"통계종료일시(unix timestamp)",null,"통계종료유닉스시각","stats_end_unix_tm","NUMBER(10)"]
[null,4,null,"residual_queue","TINYINT(3)","Y",0,"잔여대기행렬(단위:대/km/차선)",null,"잔여대기행렬길이","rmnn_queu_lngt","NUMBER(19,9)"]
[null,5,null,"max_queue","TINYINT(3)","Y",0,"최대대기행렬(단위:대/km/차선)",null,"최대대기행렬길이","max_queu_lngt","NUMBER(19,9)"]
[null,6,null,"created_date","INT(10)","Y",0,"생성일시(unix timestamp)",null,"생성유닉스시각","crt_unix_tm","NUMBER(10)"]
[]
[null,"lane_num_queue",{"$nulls":6},">>","soitglanequeu"]
[null,"NO","PK","컬럼명","형태","NULL","기본값","설명",null,"논리명","물리명","형태"]
[null,1,"PK","cam_id","VARCHAR(10)","N",null,"카메라 ID(교차로 ID + _ + 방향)",null,"현장카메라ID","spot_camr_id","VARCHAR2(10)"]
[null,2,"PK","lane_num","VARCHAR(1)","N",0,"차로 번호",null,"차로번호","lane_no","NUMBER(2)"]
[null,3,"PK","stats_start_date","INT(10)","N",0,"통계시작일시(unix timestamp)",null,"통계시작유닉스시각","stats_bgng_unix_tm","NUMBER(10)"]
[null,4,"PK","stats_end_date","INT(10)","N",0,"통계종료일시(unix timestamp)",null,"통계종료유닉스시각","stats_end_unix_tm","NUMBER(10)"]
[null,5,null,"residual_queue","TINYINT(3)","Y",0,"잔여대기행렬(단위:대/km/차선)",null,"잔여대기행렬길이","rmnn_queu_lngt","NUMBER(19,9)"]
[null,6,null,"max_queue","TINYINT(3)","Y",0,"최대대기행렬(단위:대/km/차선)",null,"최대대기행렬길이","max_queu_lngt","NUMBER(19,9)"]
[null,7,null,"created_date","INT(10)","Y",0,"생성일시(unix timestamp)",null,"생성유닉스시각","crt_unix_tm","NUMBER(10)"]
[]
[]
[null,"함체상태정보(XXXXXX) 5분주기 정보",{"$nulls":6},">>","soitgenclsttsinfo"]
[null,"NO","PK","컬럼명","형태","NULL","기본값","설명",null,"논리명","물리명","형태"]
[null,1,"PK","crossroad_id","SMALLINT(5) UNSIGNED","N",0,"교차로 ID",null,"현장교차로ID","spot_ints_id","NUMBER(5)"]
[null,2,null,"처리일시","INT(10) UNSIGNED","Y",0,"처리 일시 (unix timestamp)",null,"처리유닉스시각","prcs_unix_tm","NUMBER(10)"]
[null,3,null,"통신상태",null,null,0,"0:정상 1:통신두절 2:통신없음",null,"통신상태코드","cmnc_stts_cd","CHAR(1)"]
[null,4,null,"장비상태",null,null,0,"0: 정상 1: 카메라 이상 3:엣지모듈이상 4: 기타오류",null,"장비상태코드","eqpm_stts_cd","CHAR(1)"]
[null,5,null,"장비온도",null,null,0,"-40 ~ +80 ( 온도 숫자 )",null,"장비온도","eqpm_tmpt","NUMBER(3)"]
[null,6,null,"팬상태",null,null,0,"0:정상 1: 이상",null,"팬상태코드","pann_stts_cd","CHAR(1)"]
[null,7,null,"히터상태",null,null,0,"0:가동 1: 중지 3:정보없음",null,"히터상태코드","hetr_stts_cd","CHAR(1)"]
[null,8,null,"함체열림",null,null,0,"0:닫힘 1:열림 3: 정보없음",null,"함체개방여부","encl_open _yn","CHAR(1)"]
[null,9,null,"함체교체여부",null,"N","Y","Y:신규설치 N:기존함체사용",null,"함체교체여부","encl_rplc_yn","CHAR(1)"]
[]
[]
[]
[null,"카메라상태정보 (5분주기)",{"$nulls":6},">>","soitgcamrsttsinfo"]
[null,"NO","PK","컬럼명","형태","NULL","기본값","설명",null,"논리명","물리명","형태"]
[null,1,"PK","crossroad_id","SMALLINT(5)","N",0,"교차로 ID",null,"현장교차로ID","spot_ints_id","NUMBER(5)"]
[null,2,"UK","cam_id_hash","VARCHAR(64)","N",null,"cam_id+설치위치의 SHA256값으로 Key 가 된다.",null,"현장카메라위치ID","spot_camr_locn_id","VARCHAR2(64)"]
[null,3,"PK","cam_id","VARCHAR(10)","N",null,"카메라 ID(교차로 ID + _ + 방향)",null,"현장카메라ID","spot_camr_id","VARCHAR2(10)"]
[null,4,null,"name","VARCHAR(255)","Y",null,"현장서버 명",null,"현장서버명","spot_srvr_nm","VARCHAR2(256)"]
[null,5,null,"cam_2k_상태","VARCHAR(15)","Y",0,"0: 정상 1: 이상 3:정보없음(통신다절) 4: 기타오류",null,"2K카메라 상태코드","2k_camr_stts_cd","CHAR(1)"]
[null,6,null,"cam_2k_e_상태","VARCHAR(15)","Y",0,"0: 정상 1: 이상 3:정보없음(통신다절) 4: 기타오류",null,"2Ke카메라 상태코드","2k_ecamr_stts_cd","CHAR(1)"]
[null,7,null,"cam_4k_상태","VARCHAR(15)","Y",0,"0: 정상 1: 이상 3:정보없음(통신다절) 4: 기타오류",null,"4K카메라 상태코드","4k_camr_stts_cd","CHAR(1)"]
[null,8,null,"cam_4k_e_상태","VARCHAR(15)","Y",0,"0: 정상 1: 이상 3:정보없음(통신다절) 4: 기타오류",null,"4Ke카메라 상태코드","4k_ecamr_stts_cd","CHAR(1)"]
[null,9,"PK",null,"VARCHAR(2)","Y",null,"설치 위치 코드",null,"설치위치코드","instl_locn_cd","CHAR(2)"]
[null,10,null,null,"VARCHAR(50)","Y",null,"일련번호",null,"관리일련번호","mng_sn","VARCHAR2(50)"]
[null,11,null,null,"VARCHAR(1)","N","N","함체 ECU 정보 전송여부",null,"ECU정보전송여부","ecu_info_trsm_yn","CHAR(1)"]
[null,12,null,null,null,"N",null,"처리 일시 (unix timestamp)",null,"처리유닉스시각","prcs_unix_tm","NUMBER(10)"]

{"sheet":"코드테이블 정의","index":13,"n_rows":383,"n_cols":10,"rows_kept":383,"cut":false,"hidden":false,"merged":[]}
[]
[null,"중분류코드","중분류코드명","TRUNCATE TABLE SOITCLRGCLSFCDINFO;",null,"중분류코드","소분류코드","소분류코드명","순서","TRUNCATE TABLE SOITCSMLCLSFCDINFO;"]
[null,"001","여부",{"$f":"\"INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('\"&B3&\"','\"&C3&\"');\"","v":"INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('001','여부');"},null,"001","Y","활성화",0,{"$f":"\"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('\"&F3&\"','\"&G3&\"',\"&I3&\",'\"&H3&\"','');\"","v":"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('001','Y',0,'활성화','');"}]
[null,"002","첨두비첨두","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('002','첨두비첨두');",null,"001","N","비활성화",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('001','N',1,'비활성화','');"]
[null,"003","사용여부","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('003','사용여부');",null,"002","Y","첨두시간",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('002','Y',0,'첨두시간','');"]
[null,"004","방향","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('004','방향');",null,"002","N","비첨두시간",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('002','N',1,'비첨두시간','');"]
[null,"005","회전","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('005','회전');",null,"003","Y","사용",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('003','Y',0,'사용','');"]
[null,"006","방위","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('006','방위');",null,"003","N","미사용",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('003','N',1,'미사용','');"]
[null,"007","링구분코드","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('007','링구분코드');",null,"004",1,"상(좌)",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('004','1',0,'상(좌)','');"]
[null,"008","차종","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('008','차종');",null,"004",2,"하(우)",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('004','2',1,'하(우)','');"]
[null,"009","제어구분코드","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('009','제어구분코드');",null,"005","s","직진",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('005','s',0,'직진','');"]
[null,"010","제어상태코드","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('010','제어상태코드');",null,"005","r","우회전",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('005','r',1,'우회전','');"]
[null,"011","시간구분","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('011','시간구분');",null,"005","l","좌회전",2,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('005','l',2,'좌회전','');"]
[null,"012","돌발유형","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('012','돌발유형');",null,"005","u","유턴",3,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('005','u',3,'유턴','');"]
[null,"013","보행자 방향구분","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('013','보행자 방향구분');",null,"006","2","동",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('006','2',0,'동','');"]
[null,"014","전송여부","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('014','전송여부');",null,"006","4","북",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('006','4',1,'북','');"]
[null,"015","상태코드","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('015','상태코드');",null,"006","6","서",2,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('006','6',2,'서','');"]
[null,"016","함체교체여부","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('016','함체교체여부');",null,"006","8","남",3,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('006','8',3,'남','');"]
[null,"017","등록여부","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('017','등록여부');",null,"006","10","남서",4,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('006','10',4,'남서','');"]
[null,"018","긴급차종","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('018','긴급차종');",null,"006","12","북서",5,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('006','12',5,'북서','');"]
[null,"019","수행여부","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('019','수행여부');",null,"006","14","북동",6,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('006','14',6,'북동','');"]
[null,"020","종료여부","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('020','종료여부');",null,"006","16","남동",7,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('006','16',7,'남동','');"]
[null,"021","검지여부","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('021','검지여부');",null,"007","A","A링",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('007','A',0,'A링','');"]
[null,"022","시간대구분코드","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('022','시간대구분코드');",null,"007","B","B링",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('007','B',1,'B링','');"]
[null,"023","24시구분코드","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('023','24시구분코드');",null,"008","LBUS","대형버스",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('008','LBUS',0,'대형버스','');"]
[null,"024","24시간대구분코드","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('024','24시간대구분코드');",null,"008","LTRUCK","대형트럭(4.5T이상)",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('008','LTRUCK',1,'대형트럭(4.5T이상)','');"]
[null,"025","요일구분코드","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('025','요일구분코드');",null,"008","MBUS","미니버스",2,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('008','MBUS',2,'미니버스','');"]
[null,"026","발생여부","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('026','발생여부');",null,"008","MOTOR","오토바이",3,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('008','MOTOR',3,'오토바이','');"]
[null,"027","요일구분코드2","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('027','요일구분코드2');",null,"008","MTRUCK","트럭(4.5미만)",4,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('008','MTRUCK',4,'트럭(4.5미만)','');"]
[null,"050","교통시간대","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('050','교통시간대');",null,"008","PCAR","승용차",5,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('008','PCAR',5,'승용차','');"]
[null,"051","지역분할코드","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('051','지역분할코드');",null,"009","0","TRC",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('009','0',0,'TRC','');"]
[null,"052","행정구역코드","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('052','행정구역코드');",null,"009","1","TOD",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('009','1',1,'TOD','');"]
[null,"053","구역구분코드","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('053','구역구분코드');",null,"009","2","MAN",2,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('009','2',2,'MAN','');"]
[null,"054","교차로구분코드","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('054','교차로구분코드');",null,"010","0","오프라인",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('010','0',0,'오프라인','');"]
[null,"055","연동그룹구성구분코드","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('055','연동그룹구성구분코드');",null,"010","1","온라인",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('010','1',1,'온라인','');"]
[null,"056","소속구분코드","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('056','소속구분코드');",null,"010","2","트랜스",2,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('010','2',2,'트랜스','');"]
[null,"057","시뮬레이션 구분 코드","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('057','시뮬레이션 구분 코드');",null,"010","3","통신장애",3,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('010','3',3,'통신장애','');"]
[null,"058","엣지그룹구성코드","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('058','엣지그룹구성코드');",null,"011",1,"신호현시",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('011','1',0,'신호현시','');"]
[null,"059","전용차로구분코드","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('059','전용차로구분코드');",null,"011",2,"1분단위",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('011','2',1,'1분단위','');"]
[null,"060","도로등급코드","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('060','도로등급코드');",null,"011",3,"5분단위",2,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('011','3',2,'5분단위','');"]
[null,"061","도로형태구분코드","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('061','도로형태구분코드');",null,"011",4,"15분단위",3,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('011','4',3,'15분단위','');"]
[null,"062","주교차로구분","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('062','주교차로구분');",null,"011",5,"60분단위",4,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('011','5',4,'60분단위','');"]
[null,"063","주도로구분","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('063','주도로구분');",null,"011",6,"일단위",5,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('011','6',5,'일단위','');"]
[null,"064","간선도로구분코드","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('064','간선도로구분코드');",null,"011",7,"일누적",6,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('011','7',6,'일누적','');"]
[null,"065","도로축구분","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('065','도로축구분');",null,"011","8","첨두시간",7,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('011','8',7,'첨두시간','');"]
[null,"066","이동류코드","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('066','이동류코드');",null,"012","1","차량정지",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('012','1',0,'차량정지','');"]
[null,"500","실측여부","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('500','실측여부');",null,"012","2","꼬리물기",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('012','2',1,'꼬리물기','');"]
[null,"501","진행상태","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('501','진행상태');",null,"012","3","보행자횡단, 인도 이탈",2,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('012','3',2,'보행자횡단, 인도 이탈','');"]
[null,"502","현시제어코드","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('502','현시제어코드');",null,"012","4","역주행",3,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('012','4',3,'역주행','');"]
[null,"503","대기행렬관측여부","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('503','대기행렬관측여부');",null,"013","L","왼쪽",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('013','L',0,'왼쪽','');"]
[null,"504","참조정보구분코드","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('504','참조정보구분코드');",null,"013","R","오른쪽",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('013','R',1,'오른쪽','');"]
[null,"505","신호구분코드","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('505','신호구분코드');",null,"014","Y","전송",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('014','Y',0,'전송','');"]
[null,"506","진행상태코드","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('506','진행상태코드');",null,"014","N","미전송",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('014','N',1,'미전송','');"]
[null,"507","정검지 여부","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('507','정검지 여부');",null,"015",0,"정상",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('015','0',0,'정상','');"]
[null,"508","지표구분","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('508','지표구분');",null,"015",1,"이상",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('015','1',1,'이상','');"]
[null,"509","대상여부","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('509','대상여부');",null,"016","Y","교체",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('016','Y',0,'교체','');"]
[null,"600","집계방향구분코드","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('600','집계방향구분코드');",null,"016","N","미교체",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('016','N',1,'미교체','');"]
[null,"601","공간구분코드","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('601','공간구분코드');",null,"017","Y","등록",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('017','Y',0,'등록','');"]
[null,"602","집계처리구분코드","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('602','집계처리구분코드');",null,"017","N","미등록",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('017','N',1,'미등록','');"]
[null,"603","서비스수준","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('603','서비스수준');",null,"018","0","엠블란스",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('018','0',0,'엠블란스','');"]
[null,"700","회전유형코드","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('700','회전유형코드');",null,"018","1","소방차",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('018','1',1,'소방차','');"]
[null,"701","통신상태코드","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('701','통신상태코드');",null,"018","2","경찰차",2,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('018','2',2,'경찰차','');"]
[null,"702","장비상태코드","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('702','장비상태코드');",null,"019","Y","수행",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('019','Y',0,'수행','');"]
[null,"703","히터상태코드","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('703','히터상태코드');",null,"019","N","미수행",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('019','N',1,'미수행','');"]
[null,"704","함체개방여부","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('704','함체개방여부');",null,"020","Y","종료",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('020','Y',0,'종료','');"]
[null,"705","카메라상태코드","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('705','카메라상태코드');",null,"020","N","진행",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('020','N',1,'진행','');"]
[null,"800","교차로연도구분","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('800','교차로연도구분');",null,"021","Y","검지",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('021','Y',0,'검지','');"]
[null,801,"운영구분코드","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('801','운영구분코드');",null,"021","N","미검지",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('021','N',1,'미검지','');"]
[null,802,"특수제어코드","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('802','특수제어코드');",null,"022","1","지정시간",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('022','1',0,'지정시간','');"]
[null,803,"제어모드코드","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('803','제어모드코드');",null,"022","2","첨두시간",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('022','2',1,'첨두시간','');"]
[null,"804","예약명령코드","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('804','예약명령코드');",null,"022","3","주기별",2,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('022','3',2,'주기별','');"]
[null,"805","신호출력방향","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('805','신호출력방향');",null,"023","00","00시",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('023','00',0,'00시','');"]
[null,"806","보행 LSU","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('806','보행 LSU');",null,"023","01","01시",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('023','01',1,'01시','');"]
[null,"807","보행 출력 신호","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('807','보행 출력 신호');",null,"023","02","02시",2,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('023','02',2,'02시','');"]
[null,901,"운영구분코드","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('901','운영구분코드');",null,"023","03","03시",3,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('023','03',3,'03시','');"]
[null,902,"분석구분코드","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('902','분석구분코드');",null,"023","04","04시",4,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('023','04',4,'04시','');"]
[null,903,"분석진행코드","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('903','분석진행코드');",null,"023","05","05시",5,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('023','05',5,'05시','');"]
[null,904,"최적화진행코드","INSERT INTO SOITCLRGCLSFCDINFO (LRG_CLSF_CD, CD_NM) VALUES ('904','최적화진행코드');",null,"023","06","06시",6,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('023','06',6,'06시','');"]
[{"$nulls":5},"023","07","07시",7,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('023','07',7,'07시','');"]
[{"$nulls":5},"023","08","08시",8,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('023','08',8,'08시','');"]
[{"$nulls":5},"023","09","09시",9,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('023','09',9,'09시','');"]
[{"$nulls":5},"023","10","10시",10,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('023','10',10,'10시','');"]
[{"$nulls":5},"023","11","11시",11,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('023','11',11,'11시','');"]
[{"$nulls":5},"023","12","12시",12,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('023','12',12,'12시','');"]
[{"$nulls":5},"023","13","13시",13,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('023','13',13,'13시','');"]
[{"$nulls":5},"023","14","14시",14,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('023','14',14,'14시','');"]
[{"$nulls":5},"023","15","15시",15,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('023','15',15,'15시','');"]
[{"$nulls":5},"023","16","16시",16,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('023','16',16,'16시','');"]
[{"$nulls":5},"023","17","17시",17,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('023','17',17,'17시','');"]
[{"$nulls":5},"023","18","18시",18,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('023','18',18,'18시','');"]
[{"$nulls":5},"023","19","19시",19,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('023','19',19,'19시','');"]
[{"$nulls":5},"023","20","20시",20,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('023','20',20,'20시','');"]
[{"$nulls":5},"023","21","21시",21,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('023','21',21,'21시','');"]
[{"$nulls":5},"023","22","22시",22,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('023','22',22,'22시','');"]
[{"$nulls":5},"023","23","23시",23,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('023','23',23,'23시','');"]
[{"$nulls":5},"024","00","00:00 ~ 01:00",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('024','00',0,'00:00 ~ 01:00','');"]
[{"$nulls":5},"024","01","01:00 ~ 02:00",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('024','01',1,'01:00 ~ 02:00','');"]
[{"$nulls":5},"024","02","02:00 ~ 03:00",2,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('024','02',2,'02:00 ~ 03:00','');"]
[{"$nulls":5},"024","03","03:00 ~ 04:00",3,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('024','03',3,'03:00 ~ 04:00','');"]
[{"$nulls":5},"024","04","04:00 ~ 05:00",4,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('024','04',4,'04:00 ~ 05:00','');"]
[{"$nulls":5},"024","05","05:00 ~ 06:00",5,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('024','05',5,'05:00 ~ 06:00','');"]
[{"$nulls":5},"024","06","06:00 ~ 07:00",6,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('024','06',6,'06:00 ~ 07:00','');"]
[{"$nulls":5},"024","07","07:00 ~ 08:00",7,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('024','07',7,'07:00 ~ 08:00','');"]
[{"$nulls":5},"024","08","08:00 ~ 09:00",8,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('024','08',8,'08:00 ~ 09:00','');"]
[{"$nulls":5},"024","09","09:00 ~ 10:00",9,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('024','09',9,'09:00 ~ 10:00','');"]
[{"$nulls":5},"024","10","10:00 ~ 11:00",10,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('024','10',10,'10:00 ~ 11:00','');"]
[{"$nulls":5},"024","11","11:00 ~ 12:00",11,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('024','11',11,'11:00 ~ 12:00','');"]
[{"$nulls":5},"024","12","12:00 ~ 13:00",12,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('024','12',12,'12:00 ~ 13:00','');"]
[{"$nulls":5},"024","13","13:00 ~ 14:00",13,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('024','13',13,'13:00 ~ 14:00','');"]
[{"$nulls":5},"024","14","14:00 ~ 15:00",14,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('024','14',14,'14:00 ~ 15:00','');"]
[{"$nulls":5},"024","15","15:00 ~ 16:00",15,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('024','15',15,'15:00 ~ 16:00','');"]
[{"$nulls":5},"024","16","16:00 ~ 17:00",16,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('024','16',16,'16:00 ~ 17:00','');"]
[{"$nulls":5},"024","17","17:00 ~ 18:00",17,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('024','17',17,'17:00 ~ 18:00','');"]
[{"$nulls":5},"024","18","18:00 ~ 19:00",18,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('024','18',18,'18:00 ~ 19:00','');"]
[{"$nulls":5},"024","19","19:00 ~ 20:00",19,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('024','19',19,'19:00 ~ 20:00','');"]
[{"$nulls":5},"024","20","20:00 ~ 21:00",20,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('024','20',20,'20:00 ~ 21:00','');"]
[{"$nulls":5},"024","21","21:00 ~ 22:00",21,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('024','21',21,'21:00 ~ 22:00','');"]
[{"$nulls":5},"024","22","22:00 ~ 23:00",22,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('024','22',22,'22:00 ~ 23:00','');"]
[{"$nulls":5},"024","23","23:00 ~ 00:00",23,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('024','23',23,'23:00 ~ 00:00','');"]
[{"$nulls":5},"025","1","일요일",6,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('025','1',6,'일요일','');"]
[{"$nulls":5},"025","2","월요일",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('025','2',0,'월요일','');"]
[{"$nulls":5},"025","3","화요일",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('025','3',1,'화요일','');"]
[{"$nulls":5},"025","4","수요일",2,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('025','4',2,'수요일','');"]
[{"$nulls":5},"025","5","목요일",3,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('025','5',3,'목요일','');"]
[{"$nulls":5},"025","6","금요일",4,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('025','6',4,'금요일','');"]
[{"$nulls":5},"025","7","토요일",5,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('025','7',5,'토요일','');"]
[{"$nulls":5},"025","8","화요일~금요일",7,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('025','8',7,'화요일~금요일','');"]
[{"$nulls":5},"026","Y","발생",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('026','Y',0,'발생','');"]
[{"$nulls":5},"026","N","미발생",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('026','N',1,'미발생','');"]
[{"$nulls":5},"027","1","평일",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('027','1',0,'평일','');"]
[{"$nulls":5},"027","2","일주일",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('027','2',1,'일주일','');"]
[{"$nulls":5},"050","01","심야시간",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('050','01',0,'심야시간','');"]
[{"$nulls":5},"050","02","오전비첨두",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('050','02',1,'오전비첨두','');"]
[{"$nulls":5},"050","03","오전첨두",2,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('050','03',2,'오전첨두','');"]
[{"$nulls":5},"050","04","오전시간",3,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('050','04',3,'오전시간','');"]
[{"$nulls":5},"050","05","낮시간",4,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('050','05',4,'낮시간','');"]
[{"$nulls":5},"050","06","오후시간",5,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('050','06',5,'오후시간','');"]
[{"$nulls":5},"050","07","오후첨두",6,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('050','07',6,'오후첨두','');"]
[{"$nulls":5},"050","08","오후비첨두",7,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('050','08',7,'오후비첨두','');"]
[{"$nulls":5},"051","0","메타버스 POC",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('051','0',0,'메타버스 POC','');"]
["000",{"$nulls":4},"051","1","계양구",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('051','1',1,'계양구','');"]
["공통 운영관리",{"$nulls":4},"051","2","부평구 상단",2,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('051','2',2,'부평구 상단','');"]
["050",{"$nulls":4},"051","3","부평구 하단",3,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('051','3',3,'부평구 하단','');"]
["네트워크/신호",{"$nulls":4},"051","4","남동구 상단",4,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('051','4',4,'남동구 상단','');"]
[{"$nulls":5},"051","5","남동구 하단",5,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('051','5',5,'남동구 하단','');"]
["500",{"$nulls":4},"051","6","미추홀구",6,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('051','6',6,'미추홀구','');"]
["지표",{"$nulls":4},"051","7","연수구",7,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('051','7',7,'연수구','');"]
["600",{"$nulls":4},"051","8","중구",8,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('051','8',8,'중구','');"]
["집계",{"$nulls":4},"051","9","서구+동구",9,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('051','9',9,'서구+동구','');"]
["700",{"$nulls":4},"051","20","동구",10,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('051','20',10,'동구','');"]
["글로벌",{"$nulls":4},"051","80","서구",11,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('051','80',11,'서구','');"]
["800",{"$nulls":4},"051","50","남동구",12,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('051','50',12,'남동구','');"]
["동인",{"$nulls":4},"051","60","부평구",13,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('051','60',13,'부평구','');"]
["900",{"$nulls":4},"051","99","인천전체",14,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('051','99',14,'인천전체','');"]
["최적화",{"$nulls":4},"052","23010","중구",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('052','23010',0,'중구','');"]
[{"$nulls":5},"052","23020","동구",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('052','23020',1,'동구','');"]
[{"$nulls":5},"052","23040","연수구",2,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('052','23040',2,'연수구','');"]
[{"$nulls":5},"052","23050","남동구",3,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('052','23050',3,'남동구','');"]
[{"$nulls":5},"052","23060","부평구",4,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('052','23060',4,'부평구','');"]
[{"$nulls":5},"052","23070","계양구",5,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('052','23070',5,'계양구','');"]
[{"$nulls":5},"052","23080","서구",6,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('052','23080',6,'서구','');"]
[{"$nulls":5},"052","23090","미추홀구",7,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('052','23090',7,'미추홀구','');"]
[{"$nulls":5},"053","1","시뮬레이션용",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('053','1',0,'시뮬레이션용','');"]
[{"$nulls":5},"053","2","최적화분석용",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('053','2',1,'최적화분석용','');"]
[{"$nulls":5},"053","3","사업구역전체",2,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('053','3',2,'사업구역전체','');"]
[{"$nulls":5},"054","1","일반노드",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('054','1',0,'일반노드','');"]
[{"$nulls":5},"054","2","신호교차로",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('054','2',1,'신호교차로','');"]
[{"$nulls":5},"054","3","스마트교차로",2,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('054','3',2,'스마트교차로','');"]
[{"$nulls":5},"054","4","차선변경노드",3,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('054','4',3,'차선변경노드','');"]
[{"$nulls":5},"054","5","골목길노드",4,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('054','5',4,'골목길노드','');"]
[{"$nulls":5},"055","1","교차로(중간)",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('055','1',0,'교차로(중간)','');"]
[{"$nulls":5},"055","2","CI",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('055','2',1,'CI','');"]
[{"$nulls":5},"055","3","SCI",2,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('055','3',2,'SCI','');"]
[{"$nulls":5},"055","4","MI",3,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('055','4',3,'MI','');"]
[{"$nulls":5},"056",1,"대상지역",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('056','1',0,'대상지역','');"]
[{"$nulls":5},"056",2,"주변지역",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('056','2',1,'주변지역','');"]
[{"$nulls":5},"057","1","실시간",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('057','1',0,'실시간','');"]
[{"$nulls":5},"057","2","메타버스",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('057','2',1,'메타버스','');"]
[{"$nulls":5},"057","3","배치",2,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('057','3',2,'배치','');"]
[{"$nulls":5},"057","4","모델학습",2,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('057','4',2,'모델학습','');"]
[{"$nulls":5},"058","1","외부진입엣지그룹",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('058','1',0,'외부진입엣지그룹','');"]
[{"$nulls":5},"058","2","그룹내부엣지그룹",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('058','2',1,'그룹내부엣지그룹','');"]
[{"$nulls":5},"059","AA","모든차량허용",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('059','AA',0,'모든차량허용','');"]
[{"$nulls":5},"059","BA","버스전용차로-전일제",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('059','BA',1,'버스전용차로-전일제','');"]
[{"$nulls":5},"059","BB","버스전용차로-시간제",2,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('059','BB',2,'버스전용차로-시간제','');"]
[{"$nulls":5},"059","BC","버스전용차로-중앙차로(24시간)",3,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('059','BC',3,'버스전용차로-중앙차로(24시간)','');"]
[{"$nulls":5},"059","FF","모든차량이용불가",4,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('059','FF',4,'모든차량이용불가','');"]
[{"$nulls":5},"060","101","고속국도",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('060','101',0,'고속국도','');"]
[{"$nulls":5},"060","102","도시고속화국도",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('060','102',1,'도시고속화국도','');"]
[{"$nulls":5},"060","103","일반국도",2,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('060','103',2,'일반국도','');"]
[{"$nulls":5},"060","104","특별/광역시도",3,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('060','104',3,'특별/광역시도','');"]
[{"$nulls":5},"060","105","국가지원지방도",4,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('060','105',4,'국가지원지방도','');"]
[{"$nulls":5},"060","106","지방도",5,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('060','106',5,'지방도','');"]
[{"$nulls":5},"060","107","시/군도",6,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('060','107',6,'시/군도','');"]
[{"$nulls":5},"060","108","고속도로 연결램프",7,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('060','108',7,'고속도로 연결램프','');"]
[{"$nulls":5},"061","01","일반도로",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('061','01',0,'일반도로','');"]
[{"$nulls":5},"061","02","교량",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('061','02',1,'교량','');"]
[{"$nulls":5},"061","03","터널",2,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('061','03',2,'터널','');"]
[{"$nulls":5},"061","04","고가도로",3,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('061','04',3,'고가도로','');"]
[{"$nulls":5},"061","05","지하차도",4,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('061','05',4,'지하차도','');"]
[{"$nulls":5},"062","1","주교차로",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('062','1',0,'주교차로','');"]
[{"$nulls":5},"062","2","연등교차로",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('062','2',1,'연등교차로','');"]
[{"$nulls":5},"063","10","부도로",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('063','10',0,'부도로','');"]
[{"$nulls":5},"063","20","주도로",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('063','20',1,'주도로','');"]
[{"$nulls":5},"064",1,"주간선도로 ",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('064','1',0,'주간선도로 ','');"]
[{"$nulls":5},"064",2,"보조간선도로",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('064','2',1,'보조간선도로','');"]
[{"$nulls":5},"065",1,"동서축",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('065','1',0,'동서축','');"]
[{"$nulls":5},"065",2,"남북축",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('065','2',1,'남북축','');"]
[{"$nulls":5},"066","01","동좌",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('066','01',0,'동좌','');"]
[{"$nulls":5},"066","02","서",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('066','02',1,'서','');"]
[{"$nulls":5},"066","03","남좌",2,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('066','03',2,'남좌','');"]
[{"$nulls":5},"066","04","북",3,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('066','04',3,'북','');"]
[{"$nulls":5},"066","05","서좌",4,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('066','05',4,'서좌','');"]
[{"$nulls":5},"066","06","동",5,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('066','06',5,'동','');"]
[{"$nulls":5},"066","07","북좌",6,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('066','07',6,'북좌','');"]
[{"$nulls":5},"066","08","남",7,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('066','08',7,'남','');"]
[{"$nulls":5},"066","09","북동좌",8,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('066','09',8,'북동좌','');"]
[{"$nulls":5},"066","10","남서",9,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('066','10',9,'남서','');"]
[{"$nulls":5},"066","11","남동좌",10,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('066','11',10,'남동좌','');"]
[{"$nulls":5},"066","12","북서",11,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('066','12',11,'북서','');"]
[{"$nulls":5},"066","13","남서좌",12,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('066','13',12,'남서좌','');"]
[{"$nulls":5},"066","14","북동",13,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('066','14',13,'북동','');"]
[{"$nulls":5},"066","15","북서좌",14,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('066','15',14,'북서좌','');"]
[{"$nulls":5},"066","16","남",15,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('066','16',15,'남','');"]
[{"$nulls":5},"066","17","보행",16,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('066','17',16,'보행','');"]
[{"$nulls":5},"066","18","무신호",17,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('066','18',17,'무신호','');"]
[{"$nulls":4},"08/08추가","500","Y","실측",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('500','Y',0,'실측','');"]
[{"$nulls":5},"500","N","예측",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('500','N',1,'예측','');"]
[{"$nulls":5},"501","1","시뮬레이션진행중",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('501','1',0,'시뮬레이션진행중','');"]
[{"$nulls":5},"501","2","시뮬레이션완료",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('501','2',1,'시뮬레이션완료','');"]
[{"$nulls":5},"501","3","처리진행중",2,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('501','3',2,'처리진행중','');"]
[{"$nulls":5},"501","4","처리진행완료",3,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('501','4',3,'처리진행완료','');"]
[{"$nulls":5},"501","6","집계완료",4,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('501','6',4,'집계완료','');"]
[{"$nulls":5},"501","9","에러",5,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('501','9',5,'에러','');"]
[{"$nulls":5},"502","1","일반",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('502','1',0,'일반','');"]
[{"$nulls":5},"502","2","시차",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('502','2',1,'시차','');"]
[{"$nulls":5},"503","Y","관측",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('503','Y',0,'관측','');"]
[{"$nulls":5},"503","N","미 관측",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('503','N',1,'미 관측','');"]
[{"$nulls":5},"504",1,"이력정보",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('504','1',0,'이력정보','');"]
[{"$nulls":5},"504","2","LC_카운터",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('504','2',1,'LC_카운터','');"]
[{"$nulls":5},"504","3","TOD",2,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('504','3',2,'TOD','');"]
[{"$nulls":5},"505","G","녹색",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('505','G',0,'녹색','');"]
[{"$nulls":5},"505","g","녹색",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('505','g',1,'녹색','');"]
[{"$nulls":5},"505","r","적색",2,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('505','r',2,'적색','');"]
[{"$nulls":5},"505","y","황색",3,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('505','y',3,'황색','');"]
[{"$nulls":5},"506","0","초기셋팅",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('506','0',0,'초기셋팅','');"]
[{"$nulls":5},"506","1","신호이력insert",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('506','1',1,'신호이력insert','');"]
[{"$nulls":5},"506","2","종료시각update",2,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('506','2',2,'종료시각update','');"]
[{"$nulls":5},"506","3","황색시간insert",3,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('506','3',3,'황색시간insert','');"]
[{"$nulls":5},"506","11","신호이력insert",4,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('506','11',4,'신호이력insert','');"]
[{"$nulls":5},"506","12","종료시각update",5,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('506','12',5,'종료시각update','');"]
[{"$nulls":5},"506","13","황색시간insert",6,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('506','13',6,'황색시간insert','');"]
[{"$nulls":5},"507","Y","정검지",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('507','Y',0,'정검지','');"]
[{"$nulls":5},"507","N","미검지",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('507','N',1,'미검지','');"]
[{"$nulls":5},"507","F","오검지",2,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('507','F',2,'오검지','');"]
[{"$nulls":5},"508","1","제어지체시간(초)",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('508','1',0,'제어지체시간(초)','');"]
[{"$nulls":5},"508","2","대기행렬(m)",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('508','2',1,'대기행렬(m)','');"]
[{"$nulls":5},"508","3","정지율(%)",2,{"$f":"\"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('\"&F258&\"','\"&G258&\"',\"&I258&\",'\"&H258&\"','');\"","v":"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('508','3',2,'정지율(%)','');"}]
[{"$nulls":5},"508","4","속도(km/h)",3,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('508','4',3,'속도(km/h)','');"]
[{"$nulls":5},"508","5","시간점유율(%)",4,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('508','5',4,'시간점유율(%)','');"]
[{"$nulls":5},"508","6","교통량(대)",5,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('508','6',5,'교통량(대)','');"]
[{"$nulls":5},"508","7","전체지표",6,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('508','7',6,'전체지표','');"]
[{"$nulls":5},"508","8","최대 대기행렬(m)",7,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('508','8',7,'최대 대기행렬(m)','');"]
[{"$nulls":5},"508","9","최소 대기행렬(m)",8,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('508','9',8,'최소 대기행렬(m)','');"]
[{"$nulls":5},"508","10","밀도(대/km/초)",9,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('508','10',9,'밀도(대/km/초)','');"]
[{"$nulls":5},"508","11","포화도(%)",10,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('508','11',10,'포화도(%)','');"]
[{"$nulls":5},"508","13","공간점유율(%)",11,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('508','13',11,'공간점유율(%)','');"]
[{"$nulls":5},"509","Y","대상",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('509','Y',0,'대상','');"]
[{"$nulls":5},"509","N","미대상",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('509','N',1,'미대상','');"]
[{"$nulls":5},"600","1","진입차로별",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('600','1',0,'진입차로별','');"]
[{"$nulls":5},"600","2","내부회전별",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('600','2',1,'내부회전별','');"]
[{"$nulls":5},"601","1","링크",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('601','1',0,'링크','');"]
[{"$nulls":5},"601","2","도로",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('601','2',1,'도로','');"]
[{"$nulls":5},"601","3","교차로",2,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('601','3',2,'교차로','');"]
[{"$nulls":5},"601","4","구간",3,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('601','4',3,'구간','');"]
[{"$nulls":5},"601","5","행정구역(네트워크)",4,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('601','5',4,'행정구역(네트워크)','');"]
[{"$nulls":5},"601","6","연동그룹",5,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('601','6',5,'연동그룹','');"]
[{"$nulls":5},"601","A","전체",6,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('601','A',6,'전체','');"]
[{"$nulls":5},"601","L","링크",7,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('601','L',7,'링크','');"]
[{"$nulls":5},"602","1","이상감지",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('602','1',0,'이상감지','');"]
[{"$nulls":5},"602","2","혼잡감지",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('602','2',1,'혼잡감지','');"]
[{"$nulls":5},"603","A","A",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('603','A',0,'A','');"]
[{"$nulls":5},"603","B","B",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('603','B',1,'B','');"]
[{"$nulls":5},"603","C","C",2,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('603','C',2,'C','');"]
[{"$nulls":5},"603","D","D",3,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('603','D',3,'D','');"]
[{"$nulls":5},"603","E","E",4,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('603','E',4,'E','');"]
[{"$nulls":5},"603","F","F",5,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('603','F',5,'F','');"]
[{"$nulls":5},"700","11","직진",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('700','11',0,'직진','');"]
[{"$nulls":5},"700","21","작은좌회전",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('700','21',1,'작은좌회전','');"]
[{"$nulls":5},"700","22","큰좌회전",2,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('700','22',2,'큰좌회전','');"]
[{"$nulls":5},"700","31","작은우회전",3,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('700','31',3,'작은우회전','');"]
[{"$nulls":5},"700","32","큰우회전",4,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('700','32',4,'큰우회전','');"]
[{"$nulls":5},"700","41","유턴",5,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('700','41',5,'유턴','');"]
[{"$nulls":5},"701","0","정상",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('701','0',0,'정상','');"]
[{"$nulls":5},"701","1","통신두절",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('701','1',1,'통신두절','');"]
[{"$nulls":5},"701","2","통신없음",2,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('701','2',2,'통신없음','');"]
[{"$nulls":5},"702","0","정상",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('702','0',0,'정상','');"]
[{"$nulls":5},"702","1","카메라이상",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('702','1',1,'카메라이상','');"]
[{"$nulls":5},"702","3","엣지모듈이상",2,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('702','3',2,'엣지모듈이상','');"]
[{"$nulls":5},"702","4","기타오류",3,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('702','4',3,'기타오류','');"]
[{"$nulls":5},"703","0","가동",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('703','0',0,'가동','');"]
[{"$nulls":5},"703","1","중지",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('703','1',1,'중지','');"]
[{"$nulls":5},"703","3","정보없음",2,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('703','3',2,'정보없음','');"]
[{"$nulls":5},"704","0","닫힘",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('704','0',0,'닫힘','');"]
[{"$nulls":5},"704","1","열림",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('704','1',1,'열림','');"]
[{"$nulls":5},"704","3","정보없음",2,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('704','3',2,'정보없음','');"]
[{"$nulls":5},"705","0","정상",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('705','0',0,'정상','');"]
[{"$nulls":5},"705","1","이상",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('705','1',1,'이상','');"]
[{"$nulls":5},"705","3","통신단절",2,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('705','3',2,'통신단절','');"]
[{"$nulls":5},"705","4","기타오류",3,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('705','4',3,'기타오류','');"]
[{"$nulls":5},"800","0","2004년",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('800','0',0,'2004년','');"]
[{"$nulls":5},"800","1","2011년",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('800','1',1,'2011년','');"]
[{"$nulls":5},"801","0","일반",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('801','0',0,'일반','');"]
[{"$nulls":5},"801","1","시차1",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('801','1',1,'시차1','');"]
[{"$nulls":5},"801","2","시차2",2,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('801','2',2,'시차2','');"]
[{"$nulls":5},"801","3","시차3",3,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('801','3',3,'시차3','');"]
[{"$nulls":5},"801","4","시차4",4,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('801','4',4,'시차4','');"]
[{"$nulls":5},"801","5","시차5",5,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('801','5',5,'시차5','');"]
[{"$nulls":5},"801","6","보행맵",6,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('801','6',6,'보행맵','');"]
[{"$nulls":5},"802","0","없음",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('802','0',0,'없음','');"]
[{"$nulls":5},"802","1","점멸",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('802','1',1,'점멸','');"]
[{"$nulls":5},"802","2","소등",2,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('802','2',2,'소등','');"]
[{"$nulls":5},"802","3","수종",3,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('802','3',3,'수종','');"]
[{"$nulls":5},"802","4","감응",4,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('802','4',4,'감응','');"]
[{"$nulls":5},"803","0","비감응 지역제어",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('803','0',0,'비감응 지역제어','');"]
[{"$nulls":5},"803","1","감응 지역제어",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('803','1',1,'감응 지역제어','');"]
[{"$nulls":5},"803","2","감응 중앙제어",2,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('803','2',2,'감응 중앙제어','');"]
[{"$nulls":5},"803","3","비감응 중앙제어",3,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('803','3',3,'비감응 중앙제어','');"]
[{"$nulls":5},"804","0","없음",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('804','0',0,'없음','');"]
[{"$nulls":5},"804","1","조광제어",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('804','1',1,'조광제어','');"]
[{"$nulls":5},"804","2","점멸제어",2,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('804','2',2,'점멸제어','');"]
[{"$nulls":5},"804","3","소등제어",3,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('804','3',3,'소등제어','');"]
[{"$nulls":5},"804","4","시차제어",4,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('804','4',4,'시차제어','');"]
[{"$nulls":5},"804","5","감응제어",5,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('804','5',5,'감응제어','');"]
[{"$nulls":5},"804","6","보행자버튼활성",6,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('804','6',6,'보행자버튼활성','');"]
[{"$nulls":5},"805","0","북",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('805','0',0,'북','');"]
[{"$nulls":5},"805","1","동",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('805','1',1,'동','');"]
[{"$nulls":5},"805","2","남",2,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('805','2',2,'남','');"]
[{"$nulls":5},"805","3","서",3,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('805','3',3,'서','');"]
[{"$nulls":5},"805","4","북동",4,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('805','4',4,'북동','');"]
[{"$nulls":5},"805","5","남동",5,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('805','5',5,'남동','');"]
[{"$nulls":5},"805","6","남서",6,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('805','6',6,'남서','');"]
[{"$nulls":5},"805","7","북서",7,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('805','7',7,'북서','');"]
[{"$nulls":5},"805","8","예비1",8,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('805','8',8,'예비1','');"]
[{"$nulls":5},"805","9","예비2",9,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('805','9',9,'예비2','');"]
[{"$nulls":5},"806","0","없음",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('806','0',0,'없음','');"]
[{"$nulls":5},"806","1","LSU1",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('806','1',1,'LSU1','');"]
[{"$nulls":5},"806","2","LSU2",2,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('806','2',2,'LSU2','');"]
[{"$nulls":5},"806","3","LSU3",3,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('806','3',3,'LSU3','');"]
[{"$nulls":5},"806","4","LSU4",4,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('806','4',4,'LSU4','');"]
[{"$nulls":5},"806","5","LSU5",5,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('806','5',5,'LSU5','');"]
[{"$nulls":5},"806","6","LSU6",6,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('806','6',6,'LSU6','');"]
[{"$nulls":5},"806","7","LSU7",7,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('806','7',7,'LSU7','');"]
[{"$nulls":5},"806","8","LSU8",8,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('806','8',8,'LSU8','');"]
[{"$nulls":5},"806","9","LSU9",9,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('806','9',9,'LSU9','');"]
[{"$nulls":5},"806","10","LSU10",10,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('806','10',10,'LSU10','');"]
[{"$nulls":5},"806","11","LSU11",11,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('806','11',11,'LSU11','');"]
[{"$nulls":5},"806","12","LSU12",12,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('806','12',12,'LSU12','');"]
[{"$nulls":5},"806","13","LSU13",13,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('806','13',13,'LSU13','');"]
[{"$nulls":5},"806","14","LSU14",14,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('806','14',14,'LSU14','');"]
[{"$nulls":5},"806","15","LSU15",15,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('806','15',15,'LSU15','');"]
[{"$nulls":5},"806","16","LSU16",16,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('806','16',16,'LSU16','');"]
[{"$nulls":5},"807","0","없음",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('807','0',0,'없음','');"]
[{"$nulls":5},"807","1","G1",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('807','1',1,'G1','');"]
[{"$nulls":5},"807","2","G2",2,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('807','2',2,'G2','');"]
[{"$nulls":5},"807","3","Y1",3,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('807','3',3,'Y1','');"]
[{"$nulls":5},"901","1","실운영",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('901','1',0,'실운영','');"]
[{"$nulls":5},"901","2","시범운영",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('901','2',1,'시범운영','');"]
[{"$nulls":5},"902","1","현황",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('902','1',0,'현황','');"]
[{"$nulls":5},"902","2","최적화",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('902','2',1,'최적화','');"]
[{"$nulls":5},"903","1","시뮬레이션 준비중",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('903','1',0,'시뮬레이션 준비중','');"]
[{"$nulls":5},"903","11","분석데이터 로딩중",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('903','11',1,'분석데이터 로딩중','');"]
[{"$nulls":5},"903","12","데이터 전처리중",2,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('903','12',2,'데이터 전처리중','');"]
[{"$nulls":5},"903","13","현황분석 결과 산출중",3,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('903','13',3,'현황분석 결과 산출중','');"]
[{"$nulls":5},"903","2","시뮬레이션 완료",4,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('903','2',4,'시뮬레이션 완료','');"]
[{"$nulls":5},"903","3","결과 저장중",5,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('903','3',5,'결과 저장중','');"]
[{"$nulls":5},"903","4","완료",6,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('903','4',6,'완료','');"]
[{"$nulls":5},"904","1","시뮬레이션 준비중",0,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('904','1',0,'시뮬레이션 준비중','');"]
[{"$nulls":5},"904","16","강화학습 진행중",1,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('904','16',1,'강화학습 진행중','');"]
[{"$nulls":5},"904","17","최적화 결과 산출중",2,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('904','17',2,'최적화 결과 산출중','');"]
[{"$nulls":5},"904","2","시뮬레이션 완료",3,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('904','2',3,'시뮬레이션 완료','');"]
[{"$nulls":5},"904","3","결과 저장중",4,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('904','3',4,'결과 저장중','');"]
[{"$nulls":5},"904","4","완료",5,"INSERT INTO SOITCSMLCLSFCDINFO (LRG_CLSF_CD, SML_CLSF_CD, SEQ, CD_NM, RMRK) VALUES ('904','4',5,'완료','');"]

{"sheet":"센터(SUMO) 질의","index":14,"n_rows":9,"n_cols":6,"rows_kept":9,"cut":false,"hidden":false,"merged":[]}
["등록시각","등록자","화면명","내용","해결","해결일자"]
["2022-06-27","김종성","센터(SUMO관련)","전체적인 최적화 기능에 대하여 설명 부탁드립니다.\n - 분석타입 각각이 목표하는 최적화결과가 무엇인지 설명 요청\n   (구체적인 어떤 수치를 최적화한다 는지...)\n - 각 설계하신 테이블의 목적 등 상세 설명 요청\n   (도메인 작업에 참고가 매우 많이 됩니다)"]
["2022-06-27","김종성","센터(SUMO관련)","tb_train_history\n - 요청이력테이블? 공간분석단위에서 실제 값을 받는 부분?\n - 행정구ID나 도로명, 연동그룹ID를 저장할 컬럼 추가 필요할 듯 합니다\n - 일전 안양처럼 유닉스 방식의 시작 종료시각 값이 SUMO에서 필요하지 않나요? 지금 구성으로도 갠찮나요?"," - 요청이력테이블 맞음\n - 추가 완료\n - 추가 요청 완료","2022-06-27"]
["2022-06-27","김종성","센터(SUMO관련)","tb_time_plan, tb_program, tb_phase_config\n - 최적화된 TOD 결과에 대한 테이블은 어떤 테이블을 보아야 하나요?\n - TIME 스케줄을 무조건 하나만 산출?"," - 해당 테이블 참조\n - 시간대별로 추가됨\n  -> tb_time_plan 테이블을 기준으로 program과 phase 테이블에 데이터가 추가 생성되는 구조","2022-06-27"]
["2022-06-27","김종성","센터(SUMO관련)","현황 분석 결과에 대한 테이블은 별도 없음?   \n차량이력, 각종지표, 최적화 수치에 대한 현황분석의 대표 수치값 / 현황분석에서 tod 도 만들었었는데 이번에 빠진이유가?\n - 현황분석의 차량이력, 최적화 기준수치 유무 확인 요청\n - 최적화분석과 비료하기 위한 현황분석의 최적화수치값 확인"," - 현황분석은 기존 모니터링 테이블 참조로 변경\n - 영향권내 히트맵과 종합평가, TOD 정보를 호출\n  -> 프론트 화면 설계 변경 불가피","2022-06-27"]
["2022-06-27","김한빈","센터(SUMO관련)","tb_phase_config 테이블의 신호상태와 녹색시간 컬럼이 별도로 구분된 이유"," - 신호변경이력 테이블이 아니므로 녹색시간이 맞음\n  -> 해당 Phase의 녹색시간 의미\n  -> 신호상태는 전체 신호 상태의 문자열 정보임 개별정보가 아님","2022-06-27"]
["2022-06-27","김한빈","센터(SUMO관련)","개별교차로의 이동류코드 혹은 회전방향 확인은 어디서 하나요?"," - tb_phase_config에 컬럼 추가","2022-06-27"]
["2022-06-27","황인규","센터(SUMO관련)","몇가지 속성정보에 대해서 문의드립니다.\n\n1. 도로등급, 도로시설물(지하도로,일반도로), 최고속도 : 기존데이터가 아니라 새롭게 생성된 데이터의 경우 속성정보가 없는 상태입니다. 기본값을 임의로 정해서 넣어도 괜찮을까요??\n2. 최고속도 : 많은 링크들의 값이 0인 경우가 많습니다. 그대로 두면 될까요?","1. 도로등급, 도로시설물 : 없는대로 두기\n2. 최고속도 : '0'값이거나 NA값은 60km/h로 변경","2022-06-27"]
["2022-07-18","오효섭","센터(SUMO관련)","- 샘플에서는 속도가 소수점으로 나오는데 테이블 설계에는 그냥 정수형으로 되어 있네요. 어떻게 넣어야하는건가요?","정수형으로 반올림하도록 하겠습니다!"]

{"sheet":"데이터 구성참조 설문자료","index":15,"n_rows":35,"n_cols":23,"rows_kept":35,"cut":false,"hidden":false,"merged":[[2,1,2,2],[34,4,53,10],[0,1,1,2],[0,4,0,10],[0,12,0,19],[1,4,1,6],[1,7,1,10],[1,12,1,19]]}
[{"$nulls":4},"데이터 생성 정보",{"$nulls":7},"데이터 사용처정보"]
[{"$nulls":4},"데이터 생성/반영하는 파트에서 담당자명 기입",null,null,"생성하는 파트에서 데이터 속성 구분 입력",{"$nulls":4},"데이터 참조하는 파트에서 담당자명 기입",{"$nulls":7},"기입된 양보다 많이 필요하면 입력"]
[null,"테이블명",null,null,"시뮬레이선 전처리","시뮬레이션 수행","WEB_API PRONT","입력DB - VOLT","입력DB - TIBERO","데이터 구분","갱신 구분",null,"시뮬레이선 전처리","참조DB","시뮬레이션 수행","참조DB","WEB_API PRONT","참조DB","최적화","참조DB","최대 필요데이터량",null,"비고"]
[null,"soitsspotintstmdiff","시차제 교차로 정보",null,"김규리","-","-","김규리","김한빈","마스터","기반정보(1번만 입력)",null,null,null,"전정재/한별","V+T","-","-",null,null,"ALL"]
[null,"soitsphasinfo","현시정보",null,"박산하","-",null,"김규리","김한빈","마스터","기반정보(1번만 입력)",null,null,null,"전정재/한별","V+T","-","-",null,null,"ALL"]
[null,"soitsphasinfotmdiff","현시정보(시차제)",null,"박산하","-","-","김규리","김한빈","마스터","기반정보(1번만 입력)",null,null,null,"전정재/한별","V+T","-","-",null,null,"ALL"]
[null,"soitsintscnctlaneinfo","연결차로 신호상태순서",null,"박산하","-","-","김규리","김한빈","마스터","기반정보(1번만 입력)",null,null,null,"전정재/한별","V+T","-","-",null,null,"ALL"]
[null,"soitsphassgnlinfo","현시신호정보",null,"전정재","-","-","전정재","EXPORT","이력성","주기 누적",null,null,null,"전정재","V+T","-","-",null,null,"최소 1일치",null,"5분/1시간 시뮬레이션의 신호이력 입력에 참조하며 실시간으로 1분에 한번씩 데이터 생성"]
[null,"soitsphastodinfo","현시TOD정보",null,"전정재","-","-","전정재","EXPORT","이력성","주기 누적",null,null,null,"-",null,"-","-","?","TIBERO","최소 2주일치",null,"신호최적화 학습데이터 생성에 사용"]
[null,"soitsdummy","더미",null,"최명훈","-","-","최명훈","-","마스터","기반정보(1번만 입력)",null,null,"VOLT",null,"VOLT","-","-","-",null,"ALL",null,"DUAL 테이블 처리를 위한 VOLT전용 테이블"]
[null,"soitsrgnprttninfo","지역 분할정보",null,"최명훈",null,null,"김규리","김한빈","마스터","기반정보(1번만 입력)",null,null,null,"한별","V+T","-","-",null,null,"ALL",null,"지역구 소속 노드 기반정보 5분/1시간 시뮬레이션에 필요"]
[null,"soitspbadmsprttninfo","지역 분할정보 공간",null,"최명훈","-","김한빈","-","김한빈 (가공)","마스터","기반정보(1번만 입력)",{"$nulls":5},"김한빈","TIBERO",null,null,"ALL",null,"최위원님이 주신 데이터로 김한빈차장이 가공하여 입력, 공간정보라 티베로 전용임"]
[null,"soitssmlnflfmthstr","시뮬레이션수행이력",null,null,"이정섭/한별","-","이정섭/한별","이정섭/한별","마스터","불규칙 갱신",{"$nulls":5},"김한빈","TIBERO",null,null,"최소 7일",null,"시뮬레이션 후 이력내용을 시뮬레이션 종료 후 DB에 자동입력"]
[null,"soitsedgegrup","엣지그룹",null,"박산하","-","김한빈","김규리","김한빈 (가공)","마스터","기반정보(1번만 입력)",{"$nulls":5},"김한빈","TIBERO",null,null,"ALL",null,"기초정보는 박산하과장이 생성하여 김한빈차장이 최종결과물 가공하여 입력"]
[null,"soitsedgegrupcnfg","엣지그룹 구성",null,"박산하","-","김한빈","김규리","김한빈 (가공)","마스터","기반정보(1번만 입력)",{"$nulls":5},"김한빈","TIBERO",null,null,"ALL",null,"기초정보는 박산하과장이 생성하여 김한빈차장이 최종결과물 가공하여 입력"]
[null,"soitscnctedge","연결엣지",null,"김규리","-","-","김규리","김한빈 (가공)","마스터","기반정보(1번만 입력)",{"$nulls":5},"김한빈","TIBERO",null,null,"ALL",null,"TIBERO는 김한빈차장이 1차네트워크가공 거쳐서 입력"]
[null,"soitscnctlane","연결차로",null,"김규리","-","-","김규리","김한빈 (가공)","마스터","기반정보(1번만 입력)",{"$nulls":5},"김한빈","TIBERO",null,null,"ALL",null,"TIBERO는 김한빈차장이 1차네트워크가공 거쳐서 입력"]
[null,"soitsnode","노드",null,"김규리","-","-","김규리","김한빈 (가공)","마스터","기반정보(1번만 입력)",null,null,null,"전정재/한별","V+T","김한빈","TIBERO","박산하","TIBERO","ALL",null,"TIBERO는 김한빈차장이 1차네트워크가공 거쳐서 입력"]
[null,"soitsedge","엣지",null,"김규리","-","-","김규리","김한빈 (가공)","마스터","기반정보(1번만 입력)",{"$nulls":5},"김한빈","TIBERO","박산하","TIBERO","ALL",null,"TIBERO는 김한빈차장이 1차네트워크가공 거쳐서 입력"]
[null,"soitslane","차로",null,"김규리","이정섭/한별","-","김규리","김한빈 (가공)","마스터","기반정보(1번만 입력)",null,null,null,"이정섭","V+T","김한빈","TIBERO",null,null,"ALL",null,"TIBERO는 김한빈차장이 1차네트워크가공 거쳐서 입력"]
[null,"soitssgmn","세그먼트",null,"박산하","이정섭/한별","-","김규리","김한빈 (가공)","마스터","기반정보(1번만 입력)",null,null,null,"이정섭","V+T","김한빈","TIBERO",null,null,"ALL",null,"TIBERO는 김한빈차장이 1차네트워크가공 거쳐서 입력"]
[null,"soitsstdlinkcnfg","표준노드링크 구성",{"$nulls":4},"-","김한빈","마스터","기반정보(1번만 입력)",{"$nulls":5},"김한빈","TIBERO",null,null,"ALL",null,"BI의 링크별집계에 필요함. 매칭자료 구성 대기중"]
[null,"soitsroadinfo","도로 정보",null,"-","-","김한빈","-","김한빈","마스터","기반정보(1번만 입력)",{"$nulls":5},"김한빈","TIBERO",null,null,"ALL"]
[null,"soitsroadintsinfo","도로 소속 교차로 정보",null,"-","-","김한빈","-","김한빈","마스터","기반정보(1번만 입력)",{"$nulls":5},"김한빈","TIBERO","박산하","TIBERO","ALL"]
[null,"soitscnctlanesgnlinfo","연결차로 스마트카메라정보",null,"김규리","-","-","김규리","김한빈","마스터","기반정보(1번만 입력)",null,null,null,"전정재/한별","V+T","김한빈","TIBERO",null,null,"ALL"]
[null,"soitsnodemtv","메타버스 노드 매핑",null,"김규리","-","-","김규리",null,"마스터","기반정보(1번만 입력)",{"$nulls":5},"-","-"]
[null,"soitsedgemtv","메타버스 엣지 매핑",null,"김규리","-","-","김규리",null,"마스터","기반정보(1번만 입력)",{"$nulls":5},"-","-"]
[null,"soitsintssgnlcnfginfo","교차로 신호구성정보",null,"김규리","-","-","김규리","김한빈","마스터","기반정보(1번만 입력)",{"$nulls":5},"-","-","박산하","TIBERO","ALL"]
[null,"soitsintssgnlcnfginfotmdiff","교차로 신호구성정보(시차제)",null,"김규리","-","-","김규리","김한빈","마스터","기반정보(1번만 입력)",{"$nulls":5},"-","-","박산하","TIBERO","ALL"]
[{"$nulls":14},"5분:VOLT, 1시간:TIBERO"]
[]
[]
[]
[]
[{"$nulls":4},"내용 입력 안내\n\n1. 데이터 구분 항목 입력\n - 마스터 : 이력성 누적 테이블이 아닌 고정 정보 테이블 \n ex) 교차로 정보 테이블, 현시 구성 테이블\n - 이력성 : 변경내역이 시간대 혹은 순번에 따라 누적 입력되는 테이블\n ex) 현시변경이력 테이블 등\n\n2. 갱신 구분 입력\n - 기반정보 : 시스템이 구동을 시작하면 내용이 변동되지 않는 테이블\n ex) 노드 테이블, 엣지 테이블 등...\n - 주기 갱신 : 특정주기시마다 데이터가 UPDATE되는 테이블\n ex) 최신 하루치 교통량 집계 테이블 등\n - 불규칙 갱신 : 불특정 시마다 데이터가 UPDATE되는 테이블\n ex) 실시간 장비 상태정보 테이블 등\n - 주기 누적 : 특정주기시마다 데이터가 INSERT 되는 테이블\n ex) 교차로 현시 변경이력 테이블\n - 불규칙 누적 : 특정주기시마다 데이터가 INSERT 되는 테이블\n ex) 돌발 이벤트 이력 테이블\n - 기타\n\n3. 최대 필요데이터량 : 시스템 구동 시 오늘기준 며칠치 데이터가 필요한지 입력해주세요. 더 많은 양이 기입되어 있다면 따로 입력하지 않아도 됩니다."]

{"sheet":"테이블 보관주기동기화","index":16,"n_rows":170,"n_cols":20,"rows_kept":170,"cut":false,"hidden":false,"merged":[[155,1,155,9],[163,1,163,9],[0,13,0,14],[2,1,2,9],[23,1,23,9],[47,1,47,9],[86,1,86,9],[109,1,109,9],[121,1,121,9]]}
[{"$nulls":13},"DDL 생성"]
[null,"테이블명","COMMENT","데이터 생성\nDB","VOLT\n보관주기","VOLT >>> TIBERO\n이관테이블","VOLT <<< TIBERO\n이관테이블","TIBERO\n보관주기","TIBERO <-> VOLT\n동기화여부","사용처","EXPORT\n방법","최신\n버전","TIBERO\n갱신일자","CREATE\nTABLE","TIBERO\nPARTITION 설정\n(KEY COLUMN)\n","TIBERO\n파티션 단위","TIBERO\n보관주기 설정","DB테이블\n생성"]
[null,"글로벌 스마트교차로 테이블 (VOLT)",{"$nulls":10},"OK","OK",null,null,"이전 삭제"]
["export 설정 X","soitgintsinfo","교차로정보","VOLT / TIBERO","영구"," - "," - ","영구","-","통합운영참조",null,null,null,"OK","-",null,null,"OK","초기 한번만 밀어넣고 동기화 X"]
["export 설정 X","soitgcamrinfo","현장서버정보","VOLT / TIBERO","영구"," - "," - ","영구","-","통합운영참조",null,null,null,"OK","-",null,null,"OK","초기 한번만 밀어넣고 동기화 X"]
["export 설정 X","soitglaneinfo","차로정보","VOLT / TIBERO","영구"," - "," - ","영구","-","통합운영참조",null,null,null,"OK","-",null,null,"OK","초기 한번만 밀어넣고 동기화 X"]
["export 설정 X","soitgspotcdinfo","코드정보","VOLT","영구"," - "," - "," - ","-",{"$nulls":4},"OK","-",null,null,"VOLT만","신호쪽 코드테이블에 내용이 있음 동기화 X"]
["nifi 설정 완료","soitgrtmdtinfo","실시간 차량검지 정보","VOLT","4시간","O"," - ","6개월+@","-","BI 추가집계 시 필요",null,null,null,"OK","STLN_PASG_UNIX_TM","86400sec","840H","OK",null,{"$f":"\"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('\" &UPPER(B8)&\"',\"& SUBSTITUTE(Q8,\"H\",\"\") & \",0,'HANBIN');\"","v":"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITGRTMDTINFO',840,0,'HANBIN');"}]
["nifi 설정 완료","soitgunacevet","돌발 이벤트","VOLT","4시간","O"," - ","6개월+@","-","BI 추가집계 시 필요",null,null,null,"OK","ocrn_unix_tm","3600sec","840H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITGUNACEVET',840,0,'HANBIN');"]
["nifi 설정 완료","soitgcwdtinfo","실시간 보행자 검지 정보","VOLT","4시간","O"," - ","6개월+@","-","BI 추가집계 시 필요",null,null,null,"OK","dttn_unix_tm","3600sec","24H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITGCWDTINFO',24,0,'HANBIN');"]
["export 설정 완료","soitgvhcltrce","차량 트래킹 정보","VOLT","4시간","O"," - ","6개월+@","-","BI 추가집계 시 필요",null,null,null,"OK","trce_bgng_unix_tm","3600sec","24H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITGVHCLTRCE',24,0,'HANBIN');"]
["export 설정 완료","soitgvhcldtrtstats","번호판 검지 통계","VOLT","4시간","O"," - ","6개월+@","-","BI",null,null,null,"OK","stats_bgng_unix_tm","86400sec","840H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITGVHCLDTRTSTATS',840,0,'HANBIN');"]
["export 설정 완료","soitgturndtrtstats","회전별 번호판 검지 통계","VOLT","4시간","O"," - ","6개월+@","-","BI",null,null,null,"OK","stats_bgng_unix_tm","86400sec","840H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITGTURNDTRTSTATS',840,0,'HANBIN');"]
["nifi 설정 완료","soitgaprdstats","접근로별 통계","VOLT","4시간","O"," - ","6개월+@","-","BI",null,null,null,"OK","stats_bgng_unix_tm","86400sec","840H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITGAPRDSTATS',840,0,'HANBIN');"]
["nifi 설정 완료","soitgturntypestats","회전별 통계","VOLT","4시간","O"," - ","6개월+@","-","BI",null,null,null,"OK","stats_bgng_unix_tm","86400sec","840H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITGTURNTYPESTATS',840,0,'HANBIN');"]
["nifi 설정 완료","soitgkncrstats","차종별 통계","VOLT","4시간","O"," - ","6개월+@","-","BI",null,null,null,"OK","stats_bgng_unix_tm","86400sec","840H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITGKNCRSTATS',840,0,'HANBIN');"]
["nifi 설정 완료","soitglanestats","차로별 통계","VOLT","4시간","O"," - ","6개월+@","-","BI",null,null,null,"OK","stats_bgng_unix_tm","86400sec","840H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITGLANESTATS',840,0,'HANBIN');"]
["nifi 설정 완료","soitgaprdqueu","접근로별 대기행렬(신호 1주기)","VOLT","4시간","O"," - ","6개월+@","-","BI",null,null,null,"OK","stats_bgng_unix_tm","86400sec","840H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITGAPRDQUEU',840,0,'HANBIN');"]
["nifi 설정 완료","soitglanequeu","차로별 대기행렬(신호 1주기)","VOLT","4시간","O"," - ","6개월+@","-","BI",null,null,null,"OK","stats_bgng_unix_tm","86400sec","840H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITGLANEQUEU',840,0,'HANBIN');"]
["nifi 설정 완료","soitgenclsttsinfo","함체 상태정보","VOLT","4시간","O"," - ","6개월+@","-","상황판시스템 참조",null,null,null,"OK","prcs_unix_tm","3600sec","24H","OK","마스터성 상태 테이블","INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITGENCLSTTSINFO',24,0,'HANBIN');"]
["nifi 설정 완료","soitgcamrsttsinfo","카메라 상태 정보","VOLT","4시간","O"," - ","6개월+@","-","상황판시스템 참조",null,null,null,"OK","prcs_unix_tm","3600sec","24H","OK","마스터성 상태 테이블","INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITGCAMRSTTSINFO',24,0,'HANBIN');"]
["nifi 설정 완료","soitgrtmdtinfo_2K","2K 실시간 차량검지 정보","VOLT","?","X"," - "," - ","-","글로벌에서 VOLT 참조",null,null,null,"OK","STLN_PASG_UNIX_TM","86400sec","840H","OK"]
["nifi 설정 완료","soitgrtmdtinfo_4K","4K 실시간 차량검지 정보","VOLT","?","X"," - "," - ","-","글로벌에서 VOLT 참조",null,null,null,"OK","STLN_PASG_UNIX_TM","86400sec","840H","OK"]
[null,"동인 교차로/현시/긴급차량 테이블 (VOLT)",{"$nulls":10},"OK","OK"]
["export 설정 완료","soitdspotintsinfo","신호교차로관리","VOLT","최신정보만","O"," - ","6개월+@","-","TOD테이블조회 참조",null,null,null,"OK","CLCT_UNIX_TM","86400sec","48H","OK","신호교차로 마스터정보",{"$f":"\"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('\" &UPPER(B25)&\"',\"& SUBSTITUTE(Q25,\"H\",\"\") & \",0,'HANBIN');\"","v":"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITDSPOTINTSINFO',48,0,'HANBIN');"}]
["export 설정 완료","soitdtodcnfg","TOD구성","VOLT","1일(매일 4시)","-"," - ","6개월+@","-","TOD테이블조회 참조",null,null,null,"OK","CLCT_UNIX_TM","86400sec","48H","OK","신호교차로 마스터정보","INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITDTODCNFG',48,0,'HANBIN');"]
["export 설정 완료","soitdtodplan","시각계획","VOLT","1일(매일 4시)","O"," - ","6개월+@"," - ","TOD테이블조회 참조",null,null,null,"OK","CLCT_UNIX_TM","86400sec","48H","OK","신호교차로 마스터정보","INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITDTODPLAN',48,0,'HANBIN');"]
["export 설정 완료","soitdtimeplan","시간계획","VOLT","1일(매일 4시)","O"," - ","6개월+@"," - ","TOD테이블조회 참조",null,null,null,"OK","CLCT_UNIX_TM","86400sec","48H","OK","신호교차로 마스터정보","INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITDTIMEPLAN',48,0,'HANBIN');"]
["export 설정 완료","soitdintsphasinfo","교차로현시","VOLT","1일(매일 4시)","O"," - ","6개월+@"," - ","TOD테이블조회 참조",null,null,null,"OK","CLCT_UNIX_TM","86400sec","48H","OK","신호교차로 마스터정보","INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITDINTSPHASINFO',48,0,'HANBIN');"]
["export 설정 X","soitdintsgrp","교차로그룹관리","VOLT","1일(매일 4시)","O"," - ","6개월+@"," - ","TOD테이블조회 참조",null,null,null,"OK","CLCT_UNIX_TM","86400sec","48H","OK","신호교차로 마스터정보 VOLT 참조","INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITDINTSGRP',48,0,'HANBIN');"]
["export 설정 완료","soitdspdydayplan","특수일시각제어","VOLT","1일(매일 4시)","O"," - ","6개월+@"," - ","TOD테이블조회 참조",null,null,null,"OK","CLCT_UNIX_TM","86400sec","48H","OK","신호교차로 마스터정보","INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITDSPDYDAYPLAN',48,0,'HANBIN');"]
["export 설정 완료","soitdwklyplan","주간시각제어","VOLT","1일(매일 4시)","O"," - ","6개월+@"," - ","TOD테이블조회 참조",null,null,null,"OK","CLCT_UNIX_TM","86400sec","48H","OK","신호교차로 마스터정보","INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITDWKLYPLAN',48,0,'HANBIN');"]
["export 설정 X","soitdspotintsstts","신호교차로상태","VOLT / TIBERO","-"," - "," - ","6개월+@"," - ","글로벌/상황판 신호정보참조함",null,null,null,"OK",null,null,null,"OK","이력테이블, 볼트 티베로 모두 INSERT됨"]
["export 설정 완료","soitdspotintsoperhstr","신호교차로운영이력","VOLT","1일(매일 4시)","O"," - ","일주일치만","-","전략본부에서 신호정보참조함",null,null,null,"OK","CLCT_UNIX_TM","3600sec","24H","OK","이력테이블",{"$f":"\"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('\" &UPPER(B34)&\"',\"& SUBSTITUTE(Q34,\"H\",\"\") & \",0,'HANBIN');\"","v":"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITDSPOTINTSOPERHSTR',24,0,'HANBIN');"}]
["export 설정 X","soitdintsgrpinfo","소속교차로관리","VOLT","1일(매일 4시)","O"," - ","6개월+@","-",{"$nulls":4},"OK","CLCT_UNIX_TM","86400sec","48H","OK","신호교차로 마스터정보 VOLT 참조","INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITDINTSGRPINFO',48,0,'HANBIN');"]
["export 설정 완료","soitdphasrevt","교차로예약","VOLT","1일(매일 4시)","O"," - ","6개월+@","-",{"$nulls":4},"OK","CLCT_UNIX_TM","86400sec","48H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITDPHASREVT',48,0,'HANBIN');"]
["export 설정 X","soitdsgnlctrr","신호제어기","VOLT","1일(매일 4시)","O"," - ","6개월+@","-",{"$nulls":4},"OK","CLCT_UNIX_TM","86400sec","48H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITDSGNLCTRR',48,0,'HANBIN');"]
["export 설정 X","soitdopermap3","신호 운영 맵3","VOLT","1일(매일 4시)"," - "," - ","일주일치만","-","횡단보도이력",null,null,null,"OK","CLCT_UNIX_TM","86400sec","48H","OK","사용처가 없어 현재 데이터 입력 안함","INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITDOPERMAP3',48,0,'HANBIN');"]
["export 설정 X","soitdopermap4","신호 운영 맵4","VOLT","1일(매일 4시)"," - "," - ","일주일치만","-","횡단보도이력",null,null,null,"OK","CLCT_UNIX_TM","86400sec","48H","OK","사용처가 없어 현재 데이터 입력 안함","INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITDOPERMAP4',48,0,'HANBIN');"]
["export 설정 X","soitdsgnlotptdrct","신호출력","VOLT","1일(매일 4시)"," - "," - ","6개월+@","-",{"$nulls":4},"OK","CLCT_UNIX_TM","86400sec","48H","OK","사용처가 없어 현재 데이터 입력 안함","INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITDSGNLOTPTDRCT',48,0,'HANBIN');"]
["nifi 설정 완료","soitdemrgvhcloperhstr","긴급차량운영이력","VOLT","1일(매일 4시)","O"," - ","6개월+@","-","신호최적화에서 참조",null,null,null,"OK","CLCT_UNIX_TM","3600sec","720H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITDEMRGVHCLOPERHSTR',720,0,'HANBIN');"]
["nifi 설정 완료","soitdemrgsgnlinfo","우선신호요청정보","VOLT","1일(매일 4시)","O"," - ","6개월+@","-","신호최적화에서 참조",null,null,null,"OK","CLCT_UNIX_TM","86400sec","720H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITDEMRGSGNLINFO',720,0,'HANBIN');"]
["nifi 설정 완료","soitdemrgvhclinfo","긴급차량정보","VOLT","최신정보만","O"," - ","최신정보만","O","신호최적화에서 참조",null,null,null,"OK","CLCT_UNIX_TM","86400sec","720H","OK","마스터성 테이블","INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITDEMRGVHCLINFO',720,0,'HANBIN');"]
["nifi 설정 완료","soitdemrgsgnlpasghstr","우선신호 운영교차로","VOLT","1일(매일 4시)","O"," - ","6개월+@","-","신호최적화에서 참조",null,null,null,"OK","CLCT_UNIX_TM","86400sec","720H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITDEMRGSGNLPASGHSTR',720,0,'HANBIN');"]
["nifi 설정 완료","soitdemrgdestinfo","긴급차량 목적지 마스터 정보","TIBERO"," - "," - ",null,"6개월+@","-","상황판시스템 참조",null,null,null,"OK","CLCT_UNIX_TM","86400sec","720H","OK","마스터성 테이블","INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITDEMRGDESTINFO',720,0,'HANBIN');"]
["export 설정 X","soitdemrgvhclpathinfo","우선신호 안내경로 정보","TIBERO"," - "," - "," - ","6개월+@","-","상황판시스템 참조",null,null,null,"OK","CLCT_UNIX_TM","86400sec","720H","OK","CLOB 타입 데이터로 인하여 TIBERO INSERT 처리함","INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITDEMRGVHCLPATHINFO',720,0,'HANBIN');"]
["nifi 설정 완료","soitdemrgintninfo","긴급차량 기관정보","TIBERO"," - "," - ",null,"6개월+@","-","상황판시스템 참조",null,null,null,"OK","CLCT_UNIX_TM","86400sec","720H","OK","마스터성 테이블","INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITDEMRGINTNINFO',720,0,'HANBIN');"]
[null,"SUMO 네트워크/신호정보",{"$nulls":8},"EXPORT\n방법","최신\n버전","TIBERO\n갱신일자","OK"]
["export 설정 X","soitsspotintstmdiff","시차제 교차로 정보 테이블","VOLT","영구","-","-","영구","HUMAN",{"$nulls":4},"OK",null,null,null,"OK"]
["export 설정 X","mtvsspotintstmdiff","시차제 교차로 정보 테이블 (메타버스)","VOLT","영구","-","-","영구","HUMAN",{"$nulls":4},"OK",null,null,null,"OK"]
["export 설정 X","soitsphasinfo","현시정보 테이블","VOLT / TIBERO","영구","-","-","영구","HUMAN",null,"DBEAVER","2023-01-26","2023-02-08","OK",null,null,null,"OK"]
["export 설정 X","mtvsphasinfo","현시정보 테이블 (메타버스)","VOLT","영구","-","-","영구","HUMAN",{"$nulls":4},"OK",null,null,null,"OK"]
["export 설정 X","soitsphasinfotmdiff","현시정보(시차제) 테이블","VOLT / TIBERO","영구","-","-","영구","HUMAN",null,"DBEAVER","2023-01-26","2023-02-08","OK",null,null,null,"OK"]
["export 설정 X","mtvsphasinfotmdiff","현시정보(시차제) 테이블 (메타버스)","VOLT","영구","-","-","영구","HUMAN",{"$nulls":4},"OK"]
["export 설정 X","soitsintscnctlaneinfo","연결차로 신호상태순서","VOLT / TIBERO","영구","-","-","영구","HUMAN",null,"DBEAVER","2023-01-26","2023-02-08","OK",null,null,null,"OK","티베로 저장하지 않기로 함"]
["export 설정 X","mtvsintscnctlaneinfo","연결차로 신호상태순서 (메타버스)","VOLT / TIBERO","영구","-","-",{"$nulls":6},"OK"]
["export 설정 X","soitsphassgnlinfo","현시신호정보 테이블","TIBERO","4시간","O"," - ","1개월+@","-",null,"-","-","-","OK","CLCT_UNIX_TM","3600sec","24H","OK","티베로로 직접 입력중임",{"$f":"\"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('\" &UPPER(B57)&\"',\"& SUBSTITUTE(Q57,\"H\",\"\") & \",0,'HANBIN');\"","v":"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITSPHASSGNLINFO',24,0,'HANBIN');"}]
["export 설정 X","mtvsphassgnlinfo","현시신호정보 테이블 (메타버스)","VOLT","4시간","O"," - ",null,null,null,"-","-","-","OK","CLCT_UNIX_TM"]
["export 설정 X","soitsphastodinfo","현시TOD정보 테이블","TIBERO","4시간","O"," - ","1개월+@","-",null,"-","-","-","OK","CLCT_UNIX_TM","3600sec","340H","OK","티베로로 직접 입력중임",{"$f":"\"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('\" &UPPER(B59)&\"',\"& SUBSTITUTE(Q59,\"H\",\"\") & \",0,'HANBIN');\"","v":"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITSPHASTODINFO',340,0,'HANBIN');"}]
["export 설정 X","mtvsphastodinfo","현시TOD정보 테이블 (메타버스)","VOLT","4시간","O"," - ",null,null,null,"-","-","-","OK","CLCT_UNIX_TM"]
["export 설정 X","soitsdummy","더미","VOLT","영구","-","-","-","-","DUAL 가상테이블","-","-","-",{"$nulls":4},"VOLT만"]
["export 설정 X","soitsrgnprttninfo","지역 분할정보","VOLT / TIBERO","영구","-","-","영구","HUMAN",null,"DBEAVER","2023-01-13","2023-01-13","OK",null,null,null,"OK"]
["export 설정 X","soitspbadmsprttninfo","지역 분할정보 공간","TIBERO","-","-","-","영구","HUMAN",null,"-","-","-","OK",null,null,null,"OK"]
["export 설정 X","soitssmlnflfmthstr","시뮬레이션수행이력","VOLT / TIBERO","영구","-","-","영구","-",null,"-","-","-","OK",null,null,null,"OK","동기화하면 안됨 실시간/배치 시뮬레이션 별도로 들어감"]
["export 설정 X","soitsedgegrup","엣지그룹 ","VOLT / TIBERO","영구","-","-","영구","HUMAN",null,"API","2023-01-26","2023-02-14","OK",null,null,null,"OK"]
["export 설정 X","soitsedgegrupcnfg","엣지그룹 구성 테이블","VOLT / TIBERO","영구","-","-","영구","HUMAN",null,"API","2023-01-26","2023-02-14","OK",null,null,null,"OK"]
["export 설정 X","soitscnctedge","연결엣지 ","VOLT / TIBERO","영구","-","-","영구","HUMAN",null,"SHP-LOADER","2023-01-26","2023-02-08","OK",null,null,null,"OK"]
["export 설정 X","soitscnctlane","연결차로 ","VOLT / TIBERO","영구","-","-","영구","HUMAN",null,"SHP-LOADER","2023-01-26","2023-02-08","OK",null,null,null,"OK"]
["export 설정 X","soitsnode","노드 ","VOLT / TIBERO","영구","-","-","영구","HUMAN",null,"API","2023-04-18","2023-04-18","OK",null,null,null,"OK"]
["export 설정 X","mtvsnode","노드 (메타버스)","VOLT / TIBERO","영구","-","-",{"$nulls":6},"OK"]
["export 설정 X","soitsedge\n","엣지 ","VOLT / TIBERO","영구","-","-","영구","HUMAN",null,"SHP-LOADER","2023-01-26","2023-02-08","OK",null,null,null,"OK"]
["export 설정 X","soitslane","차로","VOLT / TIBERO","영구","-","-","영구","HUMAN",null,"SHP-LOADER","2023-01-26","2023-02-08","OK",null,null,null,"OK"]
["export 설정 X","mtvslane","차로 (메타버스)","VOLT / TIBERO","영구","-","-","영구","HUMAN",{"$nulls":4},"OK"]
["export 설정 X","soitssgmn","세그먼트","VOLT / TIBERO","영구","-","-","영구","HUMAN",null,"SHP-LOADER","2023-01-26","2023-02-08","OK",null,null,null,"OK"]
["export 설정 X","mtvssgmn","세그먼트 (메타버스)",null,null,"-","-",{"$nulls":6},"OK"]
["export 설정 X","soitsstdlinkcnfg","표준노드링크 구성","TIBERO","-","-","-","영구","HUMAN",{"$nulls":4},"OK",null,null,null,"OK"]
["export 설정 X","soitsroadinfo","도로 정보","TIBERO","-","-","-","영구","HUMAN",null,"SHP-LOADER","2023-01-26","2023-02-08","OK",null,null,null,"OK"]
["export 설정 X","SOITSSGLGINFO","교차로 신호등 위치정보","TIBERO","-","-","-","영구",null,null,"API","2023-01-26","2023-02-08","OK",null,null,null,"OK"]
["export 설정 X","soitsroadintsinfo","도로 소속 교차로 정보","TIBERO","-","-","-","영구","HUMAN",null,"API","2023-01-26","2023-02-08","OK",null,null,null,"OK"]
["export 설정 X","soitsroadedgegrupinfo","도로 소속 엣지그룹 정보","TIBERO","-","-","-","영구","HUMAN",null,"API","2023-01-26","2023-02-08","OK"]
["export 설정 X","soitscnctlanesgnlinfo","연결차로 스마트카메라정보","VOLT / TIBERO","영구","-","-","영구","HUMAN",null,"DBEAVER","2023-04-18","2023-04-18","OK",null,null,null,"OK"]
["export 설정 X","mtvscnctlanesgnlinfo","연결차로 스마트카메라정보 (메타버스)",null,null,"-","-",{"$nulls":6},"OK"]
["export 설정 X","soitsnodemtv","메타버스 노드 매핑 테이블","VOLT","영구","-","-","-","-",null,"-","-","-","OK",null,null,null,"VOLT만"]
["export 설정 X","soitsedgemtv","메타버스 엣지 매핑 테이블","VOLT","영구","-","-","-","-",null,"-","-","-","OK",null,null,null,"VOLT만"]
["export 설정 X","soitsintssgnlcnfginfo","교차로 신호구성정보 테이블","VOLT","영구","-","-",null,null,"티베로 구현 안하기로함",null,null,null,"OK",null,null,null,"OK","티베로 저장하지 않기로 함"]
["export 설정 X","soitsintssgnlcnfginfotmdiff","교차로 신호구성정보(시차제)","VOLT ","영구","-","-",null,null,"티베로 구현 안하기로함",null,null,null,"OK",null,null,null,"OK","티베로 저장하지 않기로 함"]
[null,"SUMO 실시간시뮬레이션결과",{"$nulls":10},"OK","OK"]
["export 설정 X","soitsrltmacsrvhclmvmntowh_1","실시간 차량이동궤적 (실측)","TIBERO","-","-","-","6개월+@","-","9개권역 나눔",null,null,null,"OK","locn_clct_unix_tm","3600sec","168H","OK",null,{"$f":"\"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('\" &UPPER(B88)&\"',\"& SUBSTITUTE(Q88,\"H\",\"\") & \",0,'HANBIN');\"","v":"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITSRLTMACSRVHCLMVMNTOWH_1',168,0,'HANBIN');"}]
["export 설정 X","soitsrltmacsrvhclmvmntowh_2","실시간 차량이동궤적 (실측)","TIBERO",{"$nulls":9},"OK","locn_clct_unix_tm","3600sec","168H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITSRLTMACSRVHCLMVMNTOWH_2',168,0,'HANBIN');"]
["export 설정 X","soitsrltmacsrvhclmvmntowh_3","실시간 차량이동궤적 (실측)","TIBERO",{"$nulls":9},"OK","locn_clct_unix_tm","3600sec","168H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITSRLTMACSRVHCLMVMNTOWH_3',168,0,'HANBIN');"]
["export 설정 X","soitsrltmacsrvhclmvmntowh_4","실시간 차량이동궤적 (실측)","TIBERO",{"$nulls":9},"OK","locn_clct_unix_tm","3600sec","168H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITSRLTMACSRVHCLMVMNTOWH_4',168,0,'HANBIN');"]
["export 설정 X","soitsrltmacsrvhclmvmntowh_5","실시간 차량이동궤적 (실측)","TIBERO",{"$nulls":9},"OK","locn_clct_unix_tm","3600sec","168H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITSRLTMACSRVHCLMVMNTOWH_5',168,0,'HANBIN');"]
["export 설정 X","soitsrltmacsrvhclmvmntowh_6","실시간 차량이동궤적 (실측)","TIBERO",{"$nulls":9},"OK","locn_clct_unix_tm","3600sec","168H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITSRLTMACSRVHCLMVMNTOWH_6',168,0,'HANBIN');"]
["export 설정 X","soitsrltmacsrvhclmvmntowh_7","실시간 차량이동궤적 (실측)","TIBERO",{"$nulls":9},"OK","locn_clct_unix_tm","3600sec","168H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITSRLTMACSRVHCLMVMNTOWH_7',168,0,'HANBIN');"]
["export 설정 X","soitsrltmacsrvhclmvmntowh_8","실시간 차량이동궤적 (실측)","TIBERO",{"$nulls":9},"OK","locn_clct_unix_tm","3600sec","168H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITSRLTMACSRVHCLMVMNTOWH_8',168,0,'HANBIN');"]
["export 설정 X","soitsrltmacsrvhclmvmntowh_9","실시간 차량이동궤적 (실측)","TIBERO",{"$nulls":9},"OK","locn_clct_unix_tm","3600sec","168H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITSRLTMACSRVHCLMVMNTOWH_9',168,0,'HANBIN');"]
["export 설정 X","soitsrltmprdtvhclmvmntowh_1","실시간 차량이동궤적 (예측)","TIBERO","-","-","-","6개월+@","-","9개권역 나눔",null,null,null,"OK","locn_clct_unix_tm","3600sec","168H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITSRLTMPRDTVHCLMVMNTOWH_1',168,0,'HANBIN');"]
["export 설정 X","soitsrltmprdtvhclmvmntowh_2","실시간 차량이동궤적 (예측)","TIBERO","-","-","-","6개월+@","-","9개권역 나눔",null,null,null,"OK","locn_clct_unix_tm","3600sec","168H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITSRLTMPRDTVHCLMVMNTOWH_2',168,0,'HANBIN');"]
["export 설정 X","soitsrltmprdtvhclmvmntowh_3","실시간 차량이동궤적 (예측)","TIBERO","-","-","-","6개월+@","-","9개권역 나눔",null,null,null,"OK","locn_clct_unix_tm","3600sec","168H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITSRLTMPRDTVHCLMVMNTOWH_3',168,0,'HANBIN');"]
["export 설정 X","soitsrltmprdtvhclmvmntowh_4","실시간 차량이동궤적 (예측)","TIBERO","-","-","-","6개월+@","-","9개권역 나눔",null,null,null,"OK","locn_clct_unix_tm","3600sec","168H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITSRLTMPRDTVHCLMVMNTOWH_4',168,0,'HANBIN');"]
["export 설정 X","soitsrltmprdtvhclmvmntowh_5","실시간 차량이동궤적 (예측)","TIBERO","-","-","-","6개월+@","-","9개권역 나눔",null,null,null,"OK","locn_clct_unix_tm","3600sec","168H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITSRLTMPRDTVHCLMVMNTOWH_5',168,0,'HANBIN');"]
["export 설정 X","soitsrltmprdtvhclmvmntowh_6","실시간 차량이동궤적 (예측)","TIBERO","-","-","-","6개월+@","-","9개권역 나눔",null,null,null,"OK","locn_clct_unix_tm","3600sec","168H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITSRLTMPRDTVHCLMVMNTOWH_6',168,0,'HANBIN');"]
["export 설정 X","soitsrltmprdtvhclmvmntowh_7","실시간 차량이동궤적 (예측)","TIBERO","-","-","-","6개월+@","-","9개권역 나눔",null,null,null,"OK","locn_clct_unix_tm","3600sec","168H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITSRLTMPRDTVHCLMVMNTOWH_7',168,0,'HANBIN');"]
["export 설정 X","soitsrltmprdtvhclmvmntowh_8","실시간 차량이동궤적 (예측)","TIBERO","-","-","-","6개월+@","-","9개권역 나눔",null,null,null,"OK","locn_clct_unix_tm","3600sec","168H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITSRLTMPRDTVHCLMVMNTOWH_8',168,0,'HANBIN');"]
["export 설정 X","soitsrltmprdtvhclmvmntowh_9","실시간 차량이동궤적 (예측)","TIBERO","-","-","-","6개월+@","-","9개권역 나눔",null,null,null,"OK","locn_clct_unix_tm","3600sec","168H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITSRLTMPRDTVHCLMVMNTOWH_9',168,0,'HANBIN');"]
["export 설정 X","soitsrltmvhclnoinfo","실시간 차량번호정보","TIBERO","-","-","-","6개월+@","-","신호최적화 모니터링 참조",null,null,null,"OK","anls_unix_tm","3600sec","168H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITSRLTMVHCLNOINFO',168,0,'HANBIN');"]
["export 설정 X","soitsrltmacsrsgnlchghstr","실시간 신호변경이력 (실측)","TIBERO","4시간","O","-","6개월+@","-","신호최적화 모니터링 참조",null,null,null,"OK","phas_bgng_unix_tm","3600sec","4H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITSRLTMACSRSGNLCHGHSTR',4,0,'HANBIN');"]
["export 설정 X","soitsrltmprdtsgnlchghstr","실시간 신호변경이력 (예측)","TIBERO","4시간","O","-","6개월+@","-","신호최적화 모니터링 참조",null,null,null,"OK","phas_bgng_unix_tm","3600sec","4H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITSRLTMPRDTSGNLCHGHSTR',4,0,'HANBIN');"]
["export 설정 X","mtvsrltmsgnlchghstr","실시간 신호변경이력 (메타버스)","VOLT","4시간","O","-","6개월+@","-",{"$nulls":4},"OK","phas_bgng_unix_tm"]
[null,"SUMO 최적화",{"$nulls":10},"OK","OK"]
[null,"soitsanlshrplancnfg","시간계획분석구성 테이블","TIBERO","-","-","-","무제한","-",{"$nulls":4},"OK","-",null,"-","OK"]
[null,"soitsanlshrplanrslt","최적시간계획결과 테이블","TIBERO","-","-","-","무제한","-",{"$nulls":4},"OK","-",null,"-","OK"]
[null,"soitsanlsphasrslt","최적현시결과 테이블","TIBERO","-","-","-","무제한","-",{"$nulls":4},"OK","-",null,"-","OK"]
[null,"soitsanlsrcrnhstr","반복분석이력 테이블","TIBERO","-","-","-","무제한","-",{"$nulls":4},"OK","-",null,"-","OK"]
[null,"soitsanls5minvalue","5분 대상지역 종합지표","TIBERO","-","-","-","무제한",{"$nulls":5},"OK","-",null,"-","OK"]
[null,"soitsanlsallvalue","전체지역 종합지표","TIBERO","-","-","-","무제한",{"$nulls":5},"OK","-",null,"-","OK"]
[null,"soitsanlsintsvalue","교차로별 평균지표","TIBERO","-","-","-","무제한",{"$nulls":5},"OK","-",null,"-","OK"]
[null,"soitsanlsvhclmvmntowh","분석 차량이동궤적 테이블","TIBERO","-","-","-","무제한",{"$nulls":5},"OK","-",null,"-","OK"]
[null,"soitsanlslnkggrupinfo","최적 연동그룹 테이블","TIBERO","-","-","-","무제한",{"$nulls":5},"OK","-",null,"-","OK"]
[null,"soitsanlsedgegrupinfo","최적연동그룹 구성 엣지그룹 테이블","TIBERO","-","-","-","무제한",{"$nulls":5},"OK","-",null,"-","OK"]
[null,"soitsanlsedgeinfo","최적연동그룹 구성 엣지 테이블","TIBERO","-","-","-","무제한",{"$nulls":5},"OK","-",null,"-","OK"]
[null,"센터배치집계 (5/15/60/하루) + 실시간집계 (TIBERO)",{"$nulls":10},"OK","OK"]
[null,"SOITCSGMNRLTMTOT","실시간 세그먼트별 집계 테이블","TIBERO","-","-","-","5년+@","-","신호최적화 분석/현황조회사용",null,null,null,"OK","TOT_BGNG_UNIX_TM","86400sec","720H","OK",null,{"$f":"\"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('\" &UPPER(B123)&\"',\"& SUBSTITUTE(Q123,\"H\",\"\") & \",0,'HANBIN');\"","v":"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITCSGMNRLTMTOT',720,0,'HANBIN');"}]
[null,"SOITCSGMNARNGTOT","배치 세그먼트별 집계 테이블","TIBERO","-","-","-","5년+@","-","신호최적화 분석/현황조회사용",null,null,null,"OK","TOT_BGNG_UNIX_TM","86400sec","720H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITCSGMNARNGTOT',720,0,'HANBIN');"]
[null,"SOITCEDGEGRUPRLTMQUEU_1","실시간 초당 대기행렬 테이블","TIBERO","-","-","-","5년+@","-","신호최적화 분석/현황조회사용",null,null,null,"OK","CLCT_UNIX_TM","3600sec","168H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITCEDGEGRUPRLTMQUEU_1',168,0,'HANBIN');"]
[null,"SOITCEDGEGRUPRLTMQUEU_2","실시간 초당 대기행렬 테이블","TIBERO","-","-","-","5년+@","-","신호최적화 분석/현황조회사용",null,null,null,"OK","CLCT_UNIX_TM","3600sec","168H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITCEDGEGRUPRLTMQUEU_2',168,0,'HANBIN');"]
[null,"SOITCEDGEGRUPRLTMQUEU_3","실시간 초당 대기행렬 테이블","TIBERO","-","-","-","5년+@","-","신호최적화 분석/현황조회사용",null,null,null,"OK","CLCT_UNIX_TM","3600sec","168H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITCEDGEGRUPRLTMQUEU_3',168,0,'HANBIN');"]
[null,"SOITCEDGEGRUPRLTMQUEU_4","실시간 초당 대기행렬 테이블","TIBERO","-","-","-","5년+@","-","신호최적화 분석/현황조회사용",null,null,null,"OK","CLCT_UNIX_TM","3600sec","168H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITCEDGEGRUPRLTMQUEU_4',168,0,'HANBIN');"]
[null,"SOITCEDGEGRUPRLTMQUEU_5","실시간 초당 대기행렬 테이블","TIBERO","-","-","-","5년+@","-","신호최적화 분석/현황조회사용",null,null,null,"OK","CLCT_UNIX_TM","3600sec","168H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITCEDGEGRUPRLTMQUEU_5',168,0,'HANBIN');"]
[null,"SOITCEDGEGRUPRLTMQUEU_6","실시간 초당 대기행렬 테이블","TIBERO","-","-","-","5년+@","-","신호최적화 분석/현황조회사용",null,null,null,"OK","CLCT_UNIX_TM","3600sec","168H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITCEDGEGRUPRLTMQUEU_6',168,0,'HANBIN');"]
[null,"SOITCEDGEGRUPRLTMQUEU_7","실시간 초당 대기행렬 테이블","TIBERO","-","-","-","5년+@","-","신호최적화 분석/현황조회사용",null,null,null,"OK","CLCT_UNIX_TM","3600sec","168H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITCEDGEGRUPRLTMQUEU_7',168,0,'HANBIN');"]
[null,"SOITCEDGEGRUPRLTMQUEU_8","실시간 초당 대기행렬 테이블","TIBERO","-","-","-","5년+@","-","신호최적화 분석/현황조회사용",null,null,null,"OK","CLCT_UNIX_TM","3600sec","168H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITCEDGEGRUPRLTMQUEU_8',168,0,'HANBIN');"]
[null,"SOITCEDGEGRUPRLTMQUEU_9","실시간 초당 대기행렬 테이블","TIBERO","-","-","-","5년+@","-","신호최적화 분석/현황조회사용",null,null,null,"OK","CLCT_UNIX_TM","3600sec","168H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITCEDGEGRUPRLTMQUEU_9',168,0,'HANBIN');"]
[null,"SOITCEDGEGRUPLANERLTMTOT","실시간 차선별 엣지그룹 집계 테이블","TIBERO","-","-","-","5년+@","-","신호최적화 분석/현황조회사용",null,null,null,"OK","TOT_BGNG_UNIX_TM","86400sec","720H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITCEDGEGRUPLANERLTMTOT',720,0,'HANBIN');"]
[null,"SOITCEDGEGRUPIOUTRLTMTOT","실시간 진입진출별 엣지그룹 집계 테이블","TIBERO","-","-","-","5년+@","-","신호최적화 분석/현황조회사용",null,null,null,"OK","TOT_BGNG_UNIX_TM","86400sec","720H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITCEDGEGRUPIOUTRLTMTOT',720,0,'HANBIN');"]
[null,"SOITCEDGEGRUPLANEARNGTOT","배치 차선별 엣지그룹 집계 테이블","TIBERO","-","-","-","5년+@","-","신호최적화 분석/현황조회사용",null,null,null,"OK","TOT_BGNG_UNIX_TM","86400sec","720H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITCEDGEGRUPLANEARNGTOT',720,0,'HANBIN');"]
[null,"SOITCEDGEGRUPIOUTARNGTOT","배치 진입진출별 엣지그룹 집계 테이블","TIBERO","-","-","-","5년+@","-","신호최적화 분석/현황조회사용",null,null,null,"OK","TOT_BGNG_UNIX_TM","86400sec","720H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITCEDGEGRUPIOUTARNGTOT',720,0,'HANBIN');"]
[null,"SOITCEDGEGRUPSIGNALQUEUTOT","엣지그룹 대기행렬 현시별 집계 테이블",{"$nulls":10},"OK","TOT_BGNG_UNIX_TM","86400sec","720H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITCEDGEGRUPSIGNALQUEUTOT',720,0,'HANBIN');"]
[null,"SOITCEDGEGRUPSIGNALTOT","엣지그룹 현시별 집계 테이블",{"$nulls":10},"OK","TOT_BGNG_UNIX_TM","86400sec","720H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITCEDGEGRUPSIGNALTOT',720,0,'HANBIN');"]
[null,"SOITCINTSRLTMTOT","실시간 교차로별 집계 테이블","TIBERO","-","-","-","5년+@","-","신호최적화 분석/현황조회사용",null,null,null,"OK","TOT_BGNG_UNIX_TM","86400sec","720H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITCINTSRLTMTOT',720,0,'HANBIN');"]
[null,"SOITCINTSARNGTOT","배치 교차로별 집계 테이블","TIBERO","-","-","-","5년+@","-","신호최적화 분석/현황조회사용",null,null,null,"OK","TOT_BGNG_UNIX_TM","86400sec","720H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITCINTSARNGTOT',720,0,'HANBIN');"]
[null,"SOITCINTSSIGNALTOT","교차로 현시별 인접엣지 교통량 집계 테이블",{"$nulls":10},"OK","TOT_BGNG_UNIX_TM","86400sec","720H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITCINTSSIGNALTOT',720,0,'HANBIN');"]
[null,"soitclinkroadtot","구간별 집계 테이블","TIBERO","-","-","-","5년+@","-","신호최적화 분석/현황조회사용",null,null,null,"OK","TOT_BGNG_UNIX_TM","86400sec","720H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITCLINKROADTOT',720,0,'HANBIN');"]
[null,"SOITCFCLSLOSRLTMTOT","실시간 시설물 LOS 집계 테이블","TIBERO","-","-","-","5년+@","-","신호최적화 분석/현황조회사용",null,null,null,"OK","TOT_BGNG_UNIX_TM","86400sec","720H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITCFCLSLOSRLTMTOT',720,0,'HANBIN');"]
[null,"SOITCFCLSLOSARNGTOT","배치 시설물 LOS 집계 테이블","TIBERO","-","-","-","5년+@","-","신호최적화 분석/현황조회사용",null,null,null,"OK","TOT_BGNG_UNIX_TM","86400sec","720H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITCFCLSLOSARNGTOT',720,0,'HANBIN');"]
[null,"SOITCRGNTOT","구역별 대표 집계 (실시간) 테이블","TIBERO","-","-","-","5년+@",null,"신호최적화 분석/현황조회사용",null,null,null,"OK","TOT_BGNG_UNIX_TM","86400sec","720H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITCRGNTOT',720,0,'HANBIN');"]
[null,"soitcemertrfhstr","5분단위 이상/혼잡감지 이력 테이블","TIBERO","-","-","-","5년+@","-","신호최적화 분석/현황조회사용",null,null,null,"OK","TOT_BGNG_UNIX_TM","86400sec","720H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITCEMERTRFHSTR',720,0,'HANBIN');"]
[null,"SOITCSMRTAPRDQUEU","스마트교차로 - 진입로 대기행렬 집계",{"$nulls":10},"OK","STATS_BGNG_UNIX_TM","86400sec","720H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITCSMRTAPRDQUEU',720,0,'HANBIN');"]
[null,"SOITCSMRTCWDTTOT","스마트교차로 - 보행자통계",{"$nulls":10},"OK","STATS_BGNG_UNIX_TM","86400sec","720H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITCSMRTCWDTTOT',720,0,'HANBIN');"]
[null,"SOITCSMRTLANEQUEU","스마트교차로 - 진입로차선별 대기행렬 집계",{"$nulls":10},"OK","STATS_BGNG_UNIX_TM","86400sec","720H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITCSMRTLANEQUEU',720,0,'HANBIN');"]
[null,"SOITCSMRTPLTNVHCLKNDSTATS","스마트교차로 차종별O/D통계",{"$nulls":10},"OK","STATS_BGNG_UNIX_TM","86400sec","720H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITCSMRTPLTNVHCLKNDSTATS',720,0,'HANBIN');"]
[null,"SOITCSMRTPLTNVHCLSTATS","스마트교차로 O/D 통계",{"$nulls":10},"OK","STATS_BGNG_UNIX_TM","86400sec","720H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITCSMRTPLTNVHCLSTATS',720,0,'HANBIN');"]
[null,"SOITCSMRTTURNDTRTSTATS","스마트교차로 - 회전별 차종 검지 집계",{"$nulls":10},"OK","STATS_BGNG_UNIX_TM","86400sec","720H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITCSMRTTURNDTRTSTATS',720,0,'HANBIN');"]
[null,"SOITCSMRTTURNTYPETOT","스마트교차로 - 진입로 회전별 집계",{"$nulls":10},"OK","STATS_BGNG_UNIX_TM","86400sec","720H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITCSMRTTURNTYPETOT',720,0,'HANBIN');"]
[null,"SOITCSMRTUNACEVETTOT","스마트교차로 - 돌발통계",{"$nulls":10},"OK","STATS_BGNG_UNIX_TM","86400sec","720H","OK",null,"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITCSMRTUNACEVETTOT',720,0,'HANBIN');"]
[null,"센터운영(공통) (TIBERO)",{"$nulls":10},"OK","OK"]
[null,"soitcpltnvhclcrdnints","공해차량 단속지점 정보 ","TIBERO","-","-","-","영구","-",{"$nulls":8},"OK"]
[null,"soitasmrtintscnctinfo","스마트교차로연결정보","TIBERO","-","-","-","영구","-",{"$nulls":8},"OK"]
[null,"soitctrfctmslinfo","교통시간대정보(첨두비첨두)","TIBERO","-","-","-","영구","-","첨두비첨두 집계 및 화면 표출용",{"$nulls":7},"OK"]
[null,"soitctrfctmslhstr","교통시간대이력(첨두비첨두)","TIBERO","-","-","-","영구","-","첨두비첨두 집계 및 화면 표출용",{"$nulls":7},"OK"]
[null,"soitclrgclsfcdinfo","코드테이블 - 대분류","TIBERO","-","-","-","영구","-","코드명표현시 참조",{"$nulls":7},"OK","마스터성 테이블"]
[null,"soitcsmlclsfcdinfo","코드테이블 - 소분류","TIBERO","-","-","-","영구","-","코드명표현시 참조",{"$nulls":7},"OK","마스터성 테이블"]
[null,"soitatodrprthstr","TOD보고서 변경이력 테이블","TIBERO","-","-","-","영구","-",{"$nulls":8},"OK"]
[null,"네트워크가공 (TIBERO)",{"$nulls":10},"OK","OK"]
[null,"soitsedgegrupsgmninfo","엣지그룹 구성세그먼트 정보","TIBERO","-","-","-","영구","-",null,"SCRIPT","2023-02-14","2023-02-14","OK",null,null,null,"OK"]
[null,"SOITSINTSSGMNINFO","교차로 연결세그먼트 정보","TIBERO","-","-","-","영구","-",null,"SCRIPT","2023-02-14","2023-02-14","OK",null,null,null,"OK"]
[null,"SOITSINTSCNCTINFO","교차로 연결정보","TIBERO","-","-","-","영구","-",null,"API","2023-01-26","2023-02-14","OK",null,null,null,"OK"]
[null,"SOITSINTSGRUPINFO","교차로군 정보","TIBERO","-","-","-","영구","-",{"$nulls":4},"OK",null,null,null,"OK"]
[null,"SOITSPHASSGNLCHGHSTR","현시구간이력 정보","TIBERO","-","-","-","6개월+@","-",{"$nulls":4},"OK","bgng_unix_tm","3600sec","720H","OK",null,{"$f":"\"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('\" &UPPER(B169)&\"',\"& SUBSTITUTE(Q169,\"H\",\"\") & \",0,'HANBIN');\"","v":"INSERT INTO SOITATABLEAGIGINFO (TB_NM, MTNM_HOUR, MDFCN_UNIX_TM, MDFCN_USID) VALUES ('SOITSPHASSGNLCHGHSTR',720,0,'HANBIN');"}]
[null,"SOITSINTSSTOPLOCINFO","교차로 차선별 정지선 정보","TIBERO","-","-","-","영구","-",{"$nulls":4},"OK",null,null,null,"OK"]

{"sheet":"물리타입 변환 안내","index":17,"n_rows":8,"n_cols":5,"rows_kept":8,"cut":false,"hidden":false,"merged":[]}
[]
[null,null,"VOLT DB","TIBERO","비고"]
[null,"정수형(4바이트)","INTEGER","NUMBER(10)","기본 정수형"]
[null,"정수형(8바이트)","LONG","NUMBER(20)","INTEGER타입의 오버플로우 이외에는 가급적 쓰지 않을 것."]
[null,"실수형","FLOAT","NUMBER(n, m)","각 컬럼의 논리자료형 그대로 자릿수 정의하여 사용"]
[null,"문자형","VARCHAR(n)","VARCHAR2(n)","각 컬럼의 논리자료형 그대로 자릿수 정의하여 사용"]
[null,"시각","INTEGER","NUMBER(10)","EPOCH 타임 처리, Second 기준으로 처리함"]
[null,"지리정보","geography, VARCHAR(2000)","geometry","VOLT DB에서 LineString 지원하지 않아 타입을 이원화하여 관리 (LineString 타입은 WKT String으로 저장)"]

{"sheet":"VOLT DB","index":18,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[null,"from_unixtime()","from_unixtime(INTEGER)","https://www.epochconverter.com/"]
[null,"TO_TIMESTAMP()","Converts an integer value to a VoltDB timestamp based on the time unit specified.","https://docs.voltdb.com/UsingVoltDB/sqlfunctotimestamp.php"]
[null,"CURRENT_TIMESTAMP()","NOW()"]
[null,"SINCE_EPOCH( )","SELECT SINCE_EPOCH( SECOND, CURRENT_TIMESTAMP() )\n FROM SOITDUMMY"]
["공간함수","POLYGONFROMTEXT()","POLYGONFROMTEXT(WKT String)","https://docs.voltdb.com/PerfGuide/GeoWorkWith.php","WKT로 표현한 POLYGON 정보를 VOLT DB의 Geography 타입으로 변환해주는 함수\n - POLYGON 정보의 시작점과 끝점이 같은 점이어야 한다.\n - POLYGON 이외 WKT 정보는 변환하지 못한다."]
[null,null,"INSERT INTO TEST_TABLE2 (GEOINFO, TEST) VALUES ( POINTFROMTEXT('POINT(-74.0059 40.7127)', '1');"]
["테이블 수정으로 인한\n스냅샷 갱신",null,"1. voltadmin save 명령 을 사용하여 데이터베이스를 저장합니다 .\n2. 각 노드에서 데이터베이스 루트 디렉토리를 종료하고 다시 초기화하십시오.\n3. voltdb start 명령 으로 클러스터를 시작합니다 .\n4. sqlcmd를 사용하여 수정된 스키마 및 저장 프로시저를 로드합니다.\n5. voltadmin restore 명령 을 사용하여 데이터베이스 내용을 복원합니다 .","https://docs.voltdb.com/UsingVoltDB/ChapSaveRestore.php#SaveModSchema","스냅샷을 복원하기 전에 데이터베이스 구조를 수정할 때 주의해야 할 두 가지 사항은 다음과 같습니다.\n1. 기존 행이 새 열이 추가된 테이블에 복원되면 새 열이 기본값(스키마에서 정의한 경우) 또는 null로 채워집니다.\n2. 열의 데이터 유형을 변경할 때 데이터 유형 크기를 줄일 수 있습니다(예: INT에서 TINYINT로 이동). 그러나 기존 값이 새 데이터 유형의 용량을 초과하는 경우(예: 데이터 유형이 TINYINT로 변경된 정수 값 5,000) 전체 복원이 실패합니다.\n\n저장 프로시저를 제거하거나 수정하는 경우(특히 매개변수의 수 및/또는 데이터 유형을 변경하는 경우) 클라이언트 응용 프로그램에도 해당 변경 사항이 적용되었는지 확인해야 합니다."]
[null,null,"형 타입이 다를 경우 WHERE equal 조건 안 먹음 (ex. varchar = integer... 오라클은 자동 형변환 되는데, volt는 안됨)"]
[null,null,"Inline view (인라인 뷰) 사용 시 table alias 반드시 지정. 미지정시 에러"]

{"sheet":"테이블 인덱스 목록","index":19,"n_rows":120,"n_cols":7,"rows_kept":120,"cut":false,"hidden":false,"merged":[[73,1,73,6],[76,1,76,6],[79,1,79,6],[89,1,89,6],[111,1,111,6],[48,1,48,6],[68,1,68,6],[5,1,5,2],[6,1,6,6],[7,1,9,1],[7,2,9,2],[27,1,27,6]]}
[]
[null,"1.  PK로 자동 정의되는 인덱스는 기입하지 않는다."]
[null,"2. 인덱스 명칭은 IDX_테이블명_순번 으로 규칙한다."]
[null,"3. 같은 테이블끼리 모아서 순번에 맞춰 추가해주세요.",null,null,null,"추후 PK로 잡혀 있으면, INDEX 삭제 예정 - 최명훈"]
[]
[null,"테이블명",null,"순번","VOLT/TIBERO","INDEX QUERY","입력자명"]
[null,"글로벌 스마트교차로 테이블 (VOLT)"]
["예시","soitgintsinfo","교차로정보",1,"VOLT"]
["예시",null,null,2,"TIBERO"]
["예시",null,null,3,"VOLT"]
[null,"soitgcamrinfo","현장서버정보",1]
[null,"soitglaneinfo","차로정보",1]
[null,"soitgspotcdinfo","코드정보",1]
[null,"soitgrtmdtinfo","실시간 차량검지 정보",1]
[null,"soitgunacevet","돌발 이벤트",1]
[null,"soitgcwdtinfo","실시간 보행자 검지 정보",1]
[null,"soitgvhcltrce","차량 트래킹 정보",1]
[null,"soitgvhcldtrtstats","번호판 검지 통계",1]
[null,"soitgturndtrtstats","회전별 번호판 검지 통계",1]
[null,"soitgaprdstats","접근로별 통계",1]
[null,"soitgturntypestats","회전별 통계",1]
[null,"soitgkncrstats","차종별 통계",1]
[null,"soitglanestats","차로별 통계",1]
[null,"soitgaprdqueu","접근로별 대기행렬(신호 1주기)",1]
[null,"soitglanequeu","차로별 대기행렬(신호 1주기)",1]
[null,"soitgenclsttsinfo","함체 상태정보",1]
[null,"soitgcamrsttsinfo","카메라 상태 정보",1]
[null,"동인 교차로/현시/긴급차량 테이블 (VOLT)"]
[null,"soitdspotintsinfo","신호교차로관리",1]
[null,"soitdtodcnfg","TOD구성",1,null,"CREATE INDEX IDX_SOITDTODCNFG_01 ON SOITDTODCNFG (SPOT_INTS_ID, TM_PLAN_NO);","최명훈"]
[null,"soitdtodplan","시각계획",1]
[null,"soitdtimeplan","시간계획",1]
[null,"soitdintsphasinfo","교차로현시",1]
[null,"soitdintsgrp","교차로그룹관리",1]
[null,"soitdspdydayplan","특수일시각제어",1]
[null,"soitdwklyplan","주간시각제어",1,null,"CREATE INDEX IDX_SOITDWKLYPLAN_01 ON SOITDWKLYPLAN (SPOT_INTS_ID);","최명훈"]
[null,"soitdspotintsstts","신호교차로상태",1]
[null,"soitdspotintsoperhstr","신호교차로운영이력",1,null,"CREATE INDEX IDX_SOITDSPOTINTSOPERHSTR_01 ON SOITDSPOTINTSOPERHSTR (SPOT_INTS_ID, CLCT_UNIX_TM);","최명훈"]
[null,"soitdintsgrpinfo","소속교차로관리",1]
[null,"soitdphasrevt","교차로예약",1]
[null,"soitdsgnlctrr","신호제어기",1]
[null,"soitdopermap3","신호 운영 맵3",1]
[null,"soitdopermap4","신호 운영 맵4",1]
[null,"soitdsgnlotptdrct","신호출력",1]
[null,"soitdemrgvhcloperhstr","긴급차량운영이력",1]
[null,"soitdemrgsgnlinfo","우선신호요청정보",1]
[null,"soitdemrgvhclinfo","긴급차량정보",1]
[null,"soitdemrgsgnlpasghstr","우선신호 운영교차로",1]
[null,"SUMO 네트워크/신호정보"]
[null,"soitsdummy","더미",1]
[null,"soitsrgnprttninfo","지역 분할정보",1,null,"CREATE INDEX IDX_SOITSRGNPRTTNINFO_01 ON SOITSRGNPRTTNINFO (SPOT_INTS_ID, RGN_PRTTN_CD);","최명훈"]
[null,"soitspbadmsprttninfo","행정구 분할정보",1]
[null,"soitssmlnflfmthstr","시뮬레이션수행이력",1]
[null,"soitslnkggrupcnfg","연동그룹구성 ",1]
[null,"soitslnkggrupinfo","연동그룹정보 ",1]
[null,"soitsedgegrup","엣지그룹 ",1,null,"CREATE INDEX IDX_SOITSEDGEGRUP_01 ON SOITSEDGEGRUP (ROAD_NM, BGNG_NODE_ID, END_NODE_ID);","최명훈"]
[null,"soitscnctedge","연결엣지 ",1,null,"CREATE INDEX IDX_SOITSCNCTEDGE_01 ON SOITSCNCTEDGE (CNCT_EDGE_ID, NODE_ID, ENTR_EDGE_ID, EXIT_EDGE_ID);","최명훈"]
[null,"soitscnctlane","연결차로 ",1,null,"CREATE INDEX IDX_SOITSCNCTLANE_01 ON SOITSCNCTLANE (CNCT_EDGE_ID, NODE_ID);","최명훈"]
[null,"soitsnode","노드 ",1,null,"CREATE INDEX IDX_SOITSNODE_01 ON SOITSNODE (SPOT_INTS_ID, NODE_ID, INTS_SE_CD, LNKG_GRUP_ID, PBADMS_DSTT_CD);","최명훈"]
[null,"soitsedge\n","엣지 ",1]
[null,"soitslane","차로",1]
[null,"soitssgmn","세그먼트",1]
[null,"soitsstdlinkcnfg","표준노드링크 구성",1]
[null,null,"세그먼트 구성 (설계중)",1]
[null,"soitscnctlanesgnlinfo"," 연결차로 신호정보",1,null,"CREATE INDEX IDX_SOITSCNCTLANESGNLINFO_01 ON SOITSCNCTLANESGNLINFO (SPOT_INTS_ID, SPOT_CAMR_ID, RING_SE_CD, TURN_CLSF_CD);","최명훈"]
[null,"soitsintssgnlcnfginfo","교차로 신호구성정보",1,null,"CREATE INDEX IDX_SOITSINTSSGNLCNFGINFO_01 ON SOITSINTSSGNLCNFGINFO (SPOT_INTS_ID, ENTR_EDGE_ID, EXIT_EDGE_ID);","최명훈"]
[null,"SOITSPHASSGNLINFO","현시신호정보 테이블",1,null,"CREATE INDEX IDX_SOITSPHASSGNLINFO_01 ON SOITSPHASSGNLINFO (SPOT_INTS_ID, CLCT_UNIX_TM, PRGRS_STTS_CD);","최명훈"]
[null,"SOITSPHASINFO","현시정보 테이블",1,null,"CREATE INDEX IDX_SOITSPHASINFO_01 ON SOITSPHASINFO (SPOT_INTS_ID, PHAS_NO);","최명훈"]
[null,"SUMO 실시간시뮬레이션결과"]
[null,"soitsrltmvhclmvmntowh","실시간 차량이동궤적",1]
[null,"soitsrltmsgnlchghstr","실시간 신호변경이력",1,null,"CREATE INDEX IDX_SOITSRLTMSGNLCHGHSTR_01 ON SOITSRLTMSGNLCHGHSTR (SPOT_INTS_ID, CLCT_UNIX_TM, PRGRS_STTS_CD, ACSR_YN, PHAS_NO, RING_SE_CD);","최명훈"]
[null,"mtvssrltmvhclmvmntowh","메타버스 차량이동궤적",1]
[null,"mtvssrltmsgnlchghstr","메타버스 신호변경이력",1]
[null,"SUMO 배치시뮬레이션결과"]
[null,"soitsarngvhclmvmntowh"," 배치 차량이동궤적",1]
[null,"soitsarngsgnlchghstr","배치 신호변경이력",1]
[null,"SUMO 최적화"]
[null,"설계중",null,1]
[null,null,null,1]
[null,"실시간집계 (5분) (TIBERO)"]
[null,"soitssgmntot","세그먼트별 집계 테이블",1]
[null,"soitsedgegruprltmqueu","엣지그룹별 실시간 대기행렬 테이블",1]
[null,"soitsedgegruptot","엣지그룹별 집계 테이블",1]
[null,"soitsvhclpasintshstr","개별차량당 교차로/진입로 통과이력 테이블",1]
[null,"soitsintstot","교차로별 집계 테이블",1]
[null,"soitslinkroadtot","구간별 집계 테이블",1]
[null,"soitsfclslostot                                                                        ","5분단위 시설물 LOS 테이블",1]
[null,"soitslnkggruptot                                                                        ","5분단위 연동그룹 집계 테이블",1]
[null,"soitsemertrfhstr","5분단위 이상/혼잡감지 이력 테이블",1]
[null,"센터배치집계 (5/15/60/하루) (TIBERO)"]
[null,"soitcsgmntot","세그먼트별 집계 테이블",1]
[null,"soitcedgegruprltmqueu","엣지그룹별 실시간 대기행렬 테이블",1]
[null,"soitcedgegruptot","엣지그룹별 집계 테이블",1]
[null,"soitcvhclpasintshstr","개별차량당 교차로/진입로 통과이력 테이블",1]
[null,"soitcintstot","교차로별 집계 테이블",1]
[null,"soitclinkroadtot","구간별 집계 테이블",1]
[null,"soitcfclslostot\t\t\t\t\t\t\t\t\t","5분단위 시설물 LOS 테이블",1]
[null,"soitclnkggruptot\t\t\t\t\t\t\t\t\t","5분단위 연동그룹 집계 테이블",1]
[null,"soitcemertrfhstr","5분단위 이상/혼잡감지 이력 테이블",1]
[null,"soitcaprdstats","진입로별 집계 테이블",1]
[null,"soitcaprdstats","진입로 회전별 집계 테이블",1]
[null,"soitcturntypestats","진입로 회전별 집계 테이블",1]
[null,"soitckncrstats","진입로 차종별 집계 테이블",1]
[null,"soitclanestats","진입로 차선별 집계 테이블",1]
[null,"soitcaprdqueu","진입로 대기행렬 집계 테이블",1]
[null,"soitclanequeu","진입로 차선별 대기행렬 집계 테이블",1]
[null,"soitccwdtstats","보행자통계 테이블",1]
[null,"soitcunacevetstats","돌발통계 테이블",1]
[null,"soitcpltnvhclstats","공해차량통계 테이블",1]
[null,"soitcintsodstats","교차로O/D통계테이블",1]
[null,"soitcprttnrgnodstats","분할지역O/D통계테이블",1]
[null,"센터운영(공통) (TIBERO)"]
[null,"pltnvhclcrdnints","공해차량 단속지점 정보 ",1]
[null,"soitasmrtintscnctinfo","스마트교차로연결정보",1]
[null,"soitctrfctmslinfo","교통시간대정보(첨두비첨두)",1]
[null,"soitctrfctmslhstr","교통시간대이력(첨두비첨두)",1]
[null,"soitclrgclsfcdinfo","코드테이블 - 대분류",1]
[null,"soitcsmlclsfcdinfo","코드테이블 - 소분류",1]
[null,"soitatodrprthstr","TOD보고서 변경이력 테이블",1]
[null,"soitaroadintsinfo","도로 별 교차로 정보",1]